Consulta: creatorFacets:"Lemoine, Jean-philippe"
Registros recuperados: 2
Data/hora: 10/06/2024 10:14:55

In situ high frequency long term measurements of suspended sediment concentration in turbid estuarine system (Seine Estuary, France): Optical turbidity sensors response to suspended sediment characteristics
Provedor de dados: 5
Autores: Druine, Flavie; Verney, Romaric; Deloffre, Julien; Lemoine, Jean-philippe; Chapalain, Marion; Landemaine, Valentin; Lafite, Robert.
The aim of this study is to investigate the complex response of optical turbidity sensors (side- and back-scattering sensors) to Suspended Particle Matter (SPM) characteristics and the consequences when investigating SPM dynamics from long-term high frequency monitoring networks. Our investigation is based on the analysis of a unique dataset of monthly 12 h cycle measurements of SPM characteristics such as turbidity, concentration, floc size distribution, floc density and organic matter content in the macrotidal Seine Estuary (France) between February 2015 and June 2016. Results reveal that despite calibration to a Formazin standard, turbidity sensor response to SPM concentrations (in the range of 7–7000 mg L−1) are strongly variable, from the tidal scale...
Tipo: Text
Palavras-chave: Turbidity; Suspended sediment concentration; Optical sensor; Flocs; Long term monitoring.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00431/54227/55550.pdf

Modélisation environnementale de l'estuaire de la Seine
Provedor de dados: 5
Autores: Bacq, Nicolas; Cugier, Philippe; Grasso, Florent; Le Gendre, Romain; Le Hir, Pierre; Lemoine, Jean-philippe; Riou, Philippe; Schulz, Elisabeth; Thouvenin, Benedicte; Verney, Romaric.
Dans le cadre du programme de recherche Seine-Aval 5, différentes stratégies de modélisation numérique sont mises en place pour aider à répondre aux questionnements scientifiques et sociétaux associés au fonctionnement physique, biologique, chimique et écologique de l'estuaire de la Seine (ex. projets RESET et HYMOSED). Les forçages météo-marins (vent, vague, marée) et hydrologique (débit) contrôlent le fonctionnement hydro-morpho-sédimentaire et biogéochimique de l'estuaire, modifiant ainsi les paramètres environnementaux de l’estuaire amont jusqu’à la baie de Seine (ex. nature des fonds, courant, turbidité, salinité, température, oxygène dissous, chlorophylle-a). La modélisation de ces paramètres, ainsi que leur évolution face à différents scénarios...
Tipo: Text
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00284/39480/37966.pdf