Consulta: creatorFacets:"Mamann,Ângela T. W De"
Registros recuperados: 2
Data/hora: 13/06/2024 08:13:46

Nitrogen efficiency in wheat yield through the biopolymer hydrogel
Provedor de dados: 91
Autores: Mamann,Ângela T. W De; Silva,José A. G. da; Scremin,Osmar B.; Mantai,Rubia D.; Scremin,Ari H.; Dornelles,Eldair F.
ABSTRACT Nitrogen use efficiency in wheat biomass and grain yields can be favored by the biopolymer hydrogel. The objective of the study was to analyze the use of the biopolymer hydrogel applied to the seed in the optimization of fertilizer-N on wheat biomass and grain yields, under different conditions of agricultural year and succession systems of high and reduced release of residual-N. In the study, two experiments were conducted, with different farming systems, soybean/wheat and maize/wheat, one to quantify the biomass yield rate and the other to determine grain yield. The experiments were conducted in the years 2014 and 2015, in a randomized block design with four replicates in a 4 x 4 factorial scheme, corresponding to hydrogel doses (0, 30, 60 and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Triticum aestivum; Simulation; Farming systems; Water stress.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017001000697

Simulation of wheat biomass yield by thermal time, rainfall and nitrogen
Provedor de dados: 91
Autores: Trautmann,Ana P. B.; Silva,José A. G. da; Binelo,Manuel O.; Scremin,Osmar B.; Mamann,Ângela T. W De; Bandeira,Luiz M.
ABSTRACT Wheat biomass yield focused on the production of quality silage is dependent on rainfall, temperature and nitrogen (N). The objective of the study was to validate the use of rainfall, thermal time and N as potential variables for the composition of the multiple linear regression model and simulation of wheat biomass yield for silage production under N supply conditions during the cycle, in the systems of succession. The study was conducted in 2012, 2013 and 2014, in randomized blocks with four replicates in 4 x 3 factorial, for N-fertilizer doses (0, 30, 60, 120 kg ha-1) and forms of N supply [single application (100%) in the stage V3 (third expanded leaf); split application (70%/30%) in the stages V3/V6 (third and sixth expanded leaves); split...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Triticum aestivum; N dose; Split N application; Residual N; Silage.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017001100763