Consulta: creatorFacets:"Osmari, Milene Puntel"
Registros recuperados: 2
Data/hora: 09/06/2024 17:12:01

Intake, digestibility, performance and carcass characteristics of ewes fed crambe replacing soybean meal in the diet
Provedor de dados: 2
Autores: Goes, Rafael Henrique de Tonissi e Buschinelli de; Yoshihara Carneiro, Mayara Mitiko; Osmari, Milene Puntel; Souza, Kennyson Alves de; Oliveira, Raquel Tenório de; Souza, Charles Jhonnatan dos Santos.
 The use of alternative sources of protein for ruminant can alter productivity and reduce costs in animal production. The aim of this study was to evaluate the performance, apparent digestibility and quantitative characteristics of carcass components of ewes fed increasing levels (0, 50, 100 and 150 g kg-1 dry matter) of crambe crushed in the diets. Twenty-four culling ewes were distributed in a completely randomized design. All animals were kept in a shed, with individual stalls equipped with feeder, drinker and concrete floor covered with rice hulls. The animals received corn silage as roughage and diets were isoenergetic with 700 g kg-1 of TDN. Animals were slaughtered when reached a body condition score of 3.5 points. The dry matter intake (948.53 g...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: 5.04.03.02-8 byproduct; Ether extract; Oilseeds; Crambe abyssinica.
Ano: 2018
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAnimSci/article/view/37171

Corn grain processing improves chemical composition and fermentative profile of rehydrated silage
Provedor de dados: 2
Autores: Silva, Marlon Richard Hilário da; Jobim, Clóves Cabreira; Neumann, Mikael; Osmari, Milene Puntel.
This study evaluated the effects of the rehydration and ensiling of corn grain with two geometric mean diameters (GMD) of 0.55 and 1.83 mm obtained by the diameter of the sieved used on the fermentation characteristics and chemical composition of the silage. The experimental design was completely randomized with two treatments and six replications, as follows: rehydrated fine-corn grain silage (RFS) and rehydrated coarse-corn grain silage (RCS). Ground corn was rehydrated with water to achieve moisture levels close to 350 g kg-1. There was no effect on the dry matter recovery, though the recovery rate was high, with values greater than 97% in both silages. The particle size influenced the fiber content, with lower values in the RFS. The acetic and lactic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Organic acids; Particle size; Processing grain; Storage losses.
Ano: 2018
URL: http://periodicos.uem.br/ojs/index.php/ActaSciAnimSci/article/view/42564