Consulta: creatorFacets:"Paillard, Michel"
Registros recuperados: 3
Data/hora: 15/06/2024 10:54:59

Spatio-temporal variations in intertidal mudflat erodability: Marennes-Oleron Bay, western France
Provedor de dados: 5
Autores: Orvain, Francis; Sauriau, Pierre-guy; Le Hir, Pierre; Guillou, Gael; Cann, Philippe; Paillard, Michel.
A portable erosion device (ERIS) was deployed in November 2000 and May 2001 to investigate the spatio-temporal variation of fine-grained sediment erosion over a transect on the intertidal mudflats of Marennes-Oleron Bay, western France. The objective was to relate changes in bed erodability over diurnal emersion periods to bioturbation, rapid changes in sediment characteristics, and microphytobenthos biomass.   Macrofaunal assemblages were dominated by the bivalve, Scrobicularia plana, on the upper mudflat, and by the gastropod, Hydrobia ulvae. on the middle mudflat. A power relationship was obtained where tau(cr) was plotted as a function of sediment density. Results from the upper part of the mudflat deviated from this relationship due to bioturbation by...
Tipo: Text
Palavras-chave: EPS; Microphytobenthos; Erodability; Intertidal mudflat; Sediment; Scrobicularia plana; Hydrobia ulvae; Bioturbation; Resuspension; Eris.
Ano: 2007
URL: http://archimer.ifremer.fr/doc/2007/publication-3779.pdf

Field measurements of coastal waves and currents in Portugal and Greece
Provedor de dados: 5
Autores: Paillard, Michel; Prevosto, Marc; Barstow, Sf; Soares, Cg.
The MAST II WAVEMOD Project aimed at improving stochastic modelling of ocean waves and currents in coastal waters. In order to supplement existing data, two measurement campaigns were carried our, one on the Atlantic coast of Portugal, and, secondly, on the northern coast of Crete in the Mediterranean. The Portuguese measurements covered 7 months during winter 1993-1994, while off Crete, measurements started early in February 1994 and continued for 10 months, In both sites, two directional Waveriders and one non-directional Waverider were deployed along a transect our from the coast in water depths between 10 and 100 m. In addition, the Mediterranean site also incorporated measurements of mean current velocities. Available satellite data were analysed to...
Tipo: Text
Palavras-chave: Waves; Currents; Portugal; Greece.
Ano: 2000
URL: https://archimer.ifremer.fr/doc/00000/10506/66722.pdf

Synthèse du Colloque SHF « Energies Marines Renouvelables » ‑ EMR 2013 Brest, 9 et 10 octobre 2013
Provedor de dados: 5
Autores: Aelbrecht, Denis; Paillard, Michel.
Tipo: Text
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00260/37084/35585.pdf