Consulta: creatorFacets:"Regnault, Jean-pierre"
Registros recuperados: 3
Data/hora: 07/06/2024 08:18:07

First results of a geophysical survey on the northern flank of the Storegga. slides (Norway).
Provedor de dados: 5
Autores: Nouze, Herve; Contrucci, Isabelle; Foucher, Jean-paul; Marsset, Bruno; Thomas, Yannick; Thereau, Estelle; Normand, Alain; Le Drezen, Eliane; Didailler, Stephane; Regnault, Jean-pierre; Le Conte, Sandie; Guidart, Stéphanie; Lekens, Win; Dean, Simon; Throo, Alexandre.
The Storegga slides, off Norway, are among the largest submarine slides ever known on a continental slope. The HYDRATECH cruise on N/O Le Suro (i) over capt aimed at a high-resolution survey of an area at the northern boundary of the slides. This survey images in great detail the bottom simulating reflector (BSR) extent and properties, the various fluid escape structures and the sediment deformations. The combination and the quality of the data help to understand the still poorly constrained relationships between fluid escapes, gas hydrates and slope stability in the survey area.
Tipo: Text
Palavras-chave: Slope stability; Fluid escapes; Gas hydrates; Storegga.
Ano: 2004
URL: http://archimer.ifremer.fr/doc/2004/publication-511.pdf

Deep-towed High Resolution multichannel seismic imaging
Provedor de dados: 5
Autores: Marsset, Bruno; Menut, Eric; Ker, Stephan; Thomas, Yannick; Regnault, Jean-pierre; Leon, Pierre; Martinossi, Henri; Artzner, Laurent; Chenot, Damien; Dentrecolas, Stephane; Spychalski, B.; Mellier, G.; Sultan, Nabil.
High Resolution (220–1050 Hz) seismic acquisition performed in deep water using deep-towed systems provides unrivalled lateral resolution when compared to conventional surface seismic. The lateral resolution of these acquisitions is controlled by the width of the first Fresnel zone, taking advantage of their positions close to the sea bottom. No current existing deep towed equipment can benefit from seismic imaging processing techniques to improve this resolution as a consequence of positioning inaccuracies. The technological developments of a digital deep-towed multichannel streamer are presented with a particular attention to positioning: each hydrophone incorporates a pitch, roll and heading sensor in order to monitor the constant deformation of the...
Tipo: Text
Palavras-chave: Deep-towed seismics; Multichannel streamer; Seismic imaging.
Ano: 2014
URL: https://archimer.ifremer.fr/doc/00206/31745/35690.pdf

PREVIMER: A contribution to in situ coastal observing systems
Provedor de dados: 5
Autores: Charria, Guillaume; Repecaud, Michel; Quemener, Loic; Menesguen, Alain; Rimmelin-maury, Peggy; L'Helguen, Stephane; Beaumont, Laurence; Jolivet, Aurelie; Morin, Pascal; Mace, E; Lazure, Pascal; Le Gendre, Romain; Jacqueline, Franck; Verney, Romaric; Marie, Louis; Jegou, Paul; Le Reste, Serge; Andre, Xavier; Dutreuil, Vincent; Regnault, Jean-pierre; Jestin, Herve; Lintanf, Herve; Pichavant, Pascal; Retho, Michael; Allenou, Jean-pierre; Stanisiere, Jean-yves; Bonnat, Armel; Nonnotte, Lidwine; Duros, Wenceslas; Tarot, Stephane; Carval, Thierry; Le Hir, Pierre; Dumas, Franck; Vandermeirsch, Frederic; Lecornu, Fabrice.
To design a prototype for an Integrated Ocean Observing System (IOOS), at least three components are mandatory: a modeling platform, an in situ observing system and a structure to collect and to disseminate the information (e.g. database, website). The PREVIMER project followed this approach and in order to sustain model applications, PREVIMER has developed, funded and organized part of in situ observing networks in the Bay of Biscay and the Channel. For a comprehensive system, focus was addressed on fi xed platforms (MAREL MOLIT, MAREL Iroise, Island network and D4 for sediment dynamics), ships of opportunity (RECOPESCA program and FerryBoxes), and coastal profi lers (ARVOR-C/Cm). Each system is briefl y described and examples of scientifi c results...
Tipo: Text
Ano: 2014
URL: http://archimer.ifremer.fr/doc/00197/30785/29143.pdf