Consulta: creatorFacets:"Rodrigues,Juliana Ferraz Huback"
Registros recuperados: 2
Data/hora: 06/06/2024 02:50:39

Bromatological and microbiological characteristics of sugarcane silages treated with calcium oxide
Provedor de dados: 96
Autores: Cavali,Jucilene; Pereira,Odilon Gomes; Valadares Filho,Sebastião de Campos; Santos,Edson Mauro; Carvalho,Gleidson Giordano Pinto de; Santos,Márcia Vitória; Porto,Marlos Oliveira; Rodrigues,Juliana Ferraz Huback.
It was evaluated the addition of calcium oxide (0; 0.5; 1.0; 1.5; and 2.0% of dry matter) effect on the chemical composition and ruminal degradability of the dry matter and neutral detergent fiber, on the losses of dry matter, and on the microbial population in sugar cane silages. A design with five levels of calcium oxide and three replications was used. All the variables were influenced by the addition of calcium oxide in the silages, except the composition in acid detergent insoluble protein, water soluble carbohydrates and lignin. The dry matter content and pH linearly increased while the contents of organic matter, hemicellulose and crude protein linearly decreased with the levels of calcium oxide. Neutral detergent fiber corrected for ashes and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Effluent; Ensilage; Microbial population; Nutritional value; Whitewash.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-35982010000700002

Microbiological profile and aerobic stability of Tifton 85 bermudagrass silage with different additives
Provedor de dados: 96
Autores: Neres,Marcela Abbado; Zambom,Maximiliane Alavarse; Fernandes,Tatiane; Castagnara,Deise Dalazen; Rodrigues,Juliana Ferraz Huback; Taffarel,Loreno Egidio; Javorski,Cleovani Rossi; Pozza,Magali Soares dos Santos.
The objective of this study was to evaluate the microbiological profile and aerobic stability of silage with Tifton 85 bermudagrass and different additives and wilting. The studied treatments were: pre-drying in the sun for two hours before ensiling; use of bacterial-enzymatic inoculant; addition of soybean peel; addition of corn grits and use of salt in the surface layer of the silo. The experimental design was completely randomized with six treatments and four replications. Plants of Tifton 85 bermudagrass with 38 days were ensiled in experimental silos with Bunsen valves, with compacting density of 236 kg silage per m³ for Tifton 85 bermudagrass, which was pre-dried in the sun; the average silage was 294 kg m-3 for the other treatments. The ratios...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Clostridium; Enterobacteria; PH silage; Temperature silage; Yeasts.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-35982013000600001