Consulta: creatorFacets:"Rosalen,David Luciano"
Registros recuperados: 2
Data/hora: 09/06/2024 10:21:18

Influence of distance, geometry and number of control stations on quality of local geodetic networks for the purpose of georeferencing of rural properties
Provedor de dados: 70
Autores: Rosalen,David Luciano.
The implementation of local geodetic networks for georeferencing of rural properties has become a requirement after publication of the Georeferencing Technical Standard by INCRA. According to this standard, the maximum distance of baselines to GNSS L1 receivers is of 20 km. Besides the length of the baseline, the geometry and the number of geodetic control stations are other factors to be considered in the implementation of geodetic networks. Thus, this research aimed to examine the influence of baseline lengths higher than the regulated limit of 20 km, the geometry and the number of control stations on quality of local geodetic networks for georeferencing, and also to demonstrate the importance of using specific tests to evaluate the solution of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: GNSS baseline Law 10; 267/2001.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200012

Agronomic performance of white oats cultivated under fertigation with treated sewage effluent and definition of critical limits of Normalized Difference Vegetation Index
Provedor de dados: 53
Autores: Coelho,Anderson Prates; Faria,Rogério Teixeira de; Barbosa,Aline Michelle da Silva; Dalri,Alexandre Barcellos; Rosalen,David Luciano.
ABSTRACT One of the benefits of irrigation with wastewater in agriculture is the reduction in the use of mineral fertilizers and the increase in crop yield. For wastewater application, the use of remote sensing can help to define specific management areas. The aim of this study was to evaluate the yield and the growth of irrigated white oats (Avena sativa L.) with varying treated sewage effluent (TSE) levels. These attributes were then correlated with Normalized Difference Vegetation Index (NDVI) values obtained at four phenological stages of the crop and used to define critical limits of NDVI. The experiment consisted of five TSE treatments differing in irrigation depths (11, 31, 60, 87, and 100%). Mean NDVI values in the crop were determined with an...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avena sativa L.; Biomass; Modeling; NDVI; Remote sensing.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0006-87052019000400553