Consulta: creatorFacets:"Santos,Tânia M. B. dos"
Registros recuperados: 2
Data/hora: 10/06/2024 05:36:18

Anaerobic biodigestion of manure from finishing pig supplemented with ractopamine over different periods
Provedor de dados: 70
Autores: Santos,Tânia M. B. dos; Trevizan,Paula S. F.; Xavier,Cristiane A. N.; Kiefer,Charles; Ferraz,André L. J.
ABSTRACT This study aimed to evaluate the efficiency of anaerobic digestion and biogas production by manure from pig supplemented with ractopamine over different periods. We used manure of 50 finishing pigs according to the following diets: without supplementation and supplemented with 20-ppm ractopamine during 7, 14, 21, 28 and 35 days pre-slaughter. Continuous bench biodigesters were used in the experiment. We measured biogas production and made analyses of total (TS) and volatile solids (VS), pH, total phosphorus (total P), total nitrogen (total N) and ammoniacal nitrogen (ammoniacal N) in samples of manure, affluent and effluent from biodigesters. The pH and ammoniacal N as indicator parameters of the process balance and stability were satisfactory....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Β-adrenergic; Biogas; Ractopamine hydrochloride; Environmental impact and nutrient partitioning.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300399

RESPONSE FROM ANAEROBIC DIGESTION OF LAYING HEN MANURE WITH BIOCHAR ADDITION
Provedor de dados: 70
Autores: Andrade,Willian R.; Ferreira,Cecilia de F. S.; Gates,Richard S.; Borges,Alisson C.; Santos,Tânia M. B. dos.
ABSTRACT This study aimed to assess the anaerobic digestion response of laying hen manure with different inclusion levels of biochar in batch reactors as measured by physicochemical parameters, biogas production and digestate quality. Four levels of biochar inclusions (0, 2.5, 5.0 and 7.5%) were tested with 3 replicates each. Twelve two-liter anaerobic batch reactors were used for 86 days at 35°C. Substrate and digestate of each treatment were assessed for monitored parameters, biogas production and digestate quality. Increased levels (0, 2.5, 5.0 and 7.5%) of biochar were found to gradually reduce total ammonia nitrogen (1794.33, 140.84, 950.81 and 509.32 mg.L-1, respectively). Despite the positive effect of biochar to accelerate initial biogas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogas yield; Total ammonia nitrogen; Volatile solids.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300315