Consulta: creatorFacets:"Silva,Wilton P. da"
Registros recuperados: 9
Data/hora: 13/06/2024 02:18:23

Influência da temperatura do ar de secagem no calor latente de vaporização de água em feijão macassar (Vigna unguiculata (L.) Walp.), variedade sempre-verde
Provedor de dados: 70
Autores: Silva,Wilton P. da; Silva,Cleide M. D. P. S. e; Precker,Jürgen W.; Silva,Diogo D. P. S. e.
Em cálculos da quantidade de energia requerida em processos de secagem artificial de um produto agrícola, é necessário o conhecimento de uma expressão para a determinação do calor latente de vaporização (H) de água no produto. Normalmente, as expressões para H, encontradas na literatura, são dadas pelo calor latente de vaporização (h) de água livre multiplicado por funções que dependem apenas do teor de água do produto. Isso significa que a relação H/h, para um dado produto, só depende do teor de água, o que é uma simplificação, pois se sabe que tal relação depende também da temperatura. Neste artigo, é apresentada uma expressão para o cálculo de H para feijão macassar, variedade sempre-verde, levando em consideração a dependência de H/h com a temperatura....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energia; Produtos agrícolas; Secagem.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200012

Effective diffusivity and convective mass transfer coefficient during the drying of bananas
Provedor de dados: 70
Autores: Silva,Cleide M. D. P. da S. e; Silva,Wilton P. da; Farias,Vera S. de O.; Gomes,Josivanda P.
In this article, a methodology is used for the simultaneous determination of the effective diffusivity and the convective mass transfer coefficient in porous solids, which can be considered as an infinite cylinder during drying. Two models are used for optimization and drying simulation: model 1 (constant volume and diffusivity, with equilibrium boundary condition), and model 2 (constant volume and diffusivity with convective boundary condition). Optimization algorithms based on the inverse method were coupled to the analytical solutions, and these solutions can be adjusted to experimental data of the drying kinetics. An application of optimization methodology was made to describe the drying kinetics of whole bananas, using experimental data available in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drying kinetics; Algorithm optimization; Diffusion; Porous media.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200014

Comparison of diffusion models for description of osmotic dehydration of radish slices dipped in brine
Provedor de dados: 70
Autores: Silva,Wilton P. da; Silva,Cleide M. D. P. da S. E; Gomes,Josivanda P.
ABSTRACT This paper aims at describing the osmotic dehydration of radish cut into cylindrical pieces, using one- and two-dimensional analytical solutions of diffusion equation with boundary conditions of the first and third kind. These solutions were coupled with an optimizer to determine the process parameters, using experimental data. Three models were proposed to describe the osmotic dehydration of radish slices in brine at low temperature. The two-dimensional model with boundary condition of the third kind well described the kinetics of mass transfers, and it enabled prediction of moisture and solid distributions at any given time.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Inverse method; Analytical models; Cylindrical geometry.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500894

Determinação da difusividade e da energia de ativação para feijão macassar (Vigna unguiculata (L.) Walp.), variedade sempre-verde, com base no comportamento da secagem
Provedor de dados: 70
Autores: Silva,Wilton P. da; Mata,Mário E. R. M. C.; Silva,Cleiton D. P. S. e; Guedes,Manoel A.; Lima,Antonio G. B.
Neste artigo, teve-se o objetivo de determinar curvas de secagem em camada fina para grãos de feijão macassar, variedade sempre-verde. Visou-se, também, à determinação da difusividade efetiva da água no interior do produto, bem como a energia de ativação. Para tal, foram utilizadas amostras com 150 g de feijão com teor inicial de água de 37% (bu), nas temperaturas de 40; 50 e 60 ºC. A velocidade do ar do secador convectivo foi mantida em 1,0 m s-1 e, durante todo o processo, os valores médios da temperatura e da umidade relativa do ar ambiente foram, respectivamente, 29 ºC e 58%. A difusividade efetiva da água no produto foi determinada, em cada temperatura, por meio da lei de Fick, pressupondo um modelo esférico para os grãos. Uma expressão para a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelo de Page; Segunda lei de Fick; Teor de água; Grãos esféricos.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200013

Empirical models in the description of prickly pear shoot (Nopal) drying kinetics
Provedor de dados: 91
Autores: Pereira,Emmanuel M.; Silva,Wilton P. da; Gomes,Josivanda P.; Silva,Cleide M. D. P. da S. e; Formiga,Anderson dos S.; Costa,Franciscleudo B. da.
ABSTRACT The objective of this study was to describe the technological process involved in the drying kinetics of fresh-cut prickly pear shoots through numerical and analytical solutions. Shoots of two different prickly pear species were used, ‘Gigante’ and ‘Miúda’. Drying was performed at different temperatures (50, 60, 70 and 80 °C) and weighing procedures were made continuously. The experimental data were expressed as moisture ratio. The Page model showed the best fit to the drying kinetics of minimally processed ‘Gigante’ and ‘Miúda’ prickly pear shoots, with the best coefficients of determination and Chi-square. Peleg and Wang &amp; Singh models can not be used to simulate the drying of ‘Gigante’ and ‘Miúda’ prickly pear shoots within the evaluated...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mathematical modeling; Opuntia; Nopalea; Minimal processing.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017001100798

Estabilidade de geleias convencionais de umbu-cajá durante o armazenamento em condições ambientais
Provedor de dados: 91
Autores: Oliveira,Emanuel N. A. de; Santos,Dyego da C.; Rocha,Ana P. T.; Gomes,Josivanda P.; Silva,Wilton P. da.
Neste trabalho propôs-se estudar a estabilidade física e química de geleias convencionais de umbu-cajá durante o armazenamento por 180 dias em condições ambientais. As geleias foram formuladas por meio de planejamento experimental fatorial 22 com 2 experimentos no ponto central resultando em 6 experimentos, variando-se as concentrações de açúcar cristal (50, 55 e 60%) e pectina de alto teor de metoxilação (0,5; 1,0 e 1,5%). As formulações foram aquecidas e concentradas em tacho aberto até atingir teor de sólidos solúveis totais de â‰ˆ65 ºBrix, envasadas em recipientes de vidro transparente e estocadas em temperatura e umidade relativa médias de 23,25 ºC e 81%, respectivamente, com análises físicas e químicas a cada 30 dias de armazenamento. De acordo com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spondias spp; Estocagem; Vida-de-prateleira.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662014000300013

Solar drying of cowpea bean combined with drying in a heat accumulator dryer
Provedor de dados: 91
Autores: Alves,Ronaldo A.; Queiroz,Alexandre J. de M.; Figueirêdo,Rossana M. F. de; Silva,Wilton P. da; Gomes,Josivanda P.
ABSTRACT As solar radiation is abundant in Brazil during most of the year and this source of energy is renewable and non-polluting par excellence, solar drying of agricultural products is a promising methodology. The objective of this study was to dry cowpea [Vigna unguiculata (L.) Walp.] bean grains using solar energy in different exposure times, adjusting the mathematical models and calculation of the effective diffusivity. Drying was performed during the day with samples exposed to the sun; during the night, half of the samples were put to dry in a heat accumulator dryer for nighttime drying and the other half was left on a laboratory bench as control. Cowpea bean grains had initial and final moisture contents of 65.42 and 6.73% d.b. (after drying in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vigna unguiculata; Renewable energy; Mathematical models.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662019000900709

Convective drying kinetics of osmotically pretreated papaya cubes
Provedor de dados: 91
Autores: Ferreira,João P. de L.; Castro,Deise S. de; Moreira,Inacia dos S.; Silva,Wilton P. da; Figueirêdo,Rossana M. F. de; Queiroz,Alexandre J. de M.
ABSTRACT This study assessed the fitting of mathematical models to the convective drying kinetics of osmotically pre-dehydrated papaya cubes. Papaya cubes were subjected to osmotic dehydration in sucrose solutions at 40 and 50 ºBrix, at temperatures of 50 and 60 ºC, followed by complementary convective drying in forced air circulation oven under three temperatures (50, 60 and 70 °C) and constant air velocity of 1.0 m s-1. Ten thin-layer drying mathematical models were fitted to the experimental data. The increase in air temperature and the decrease in osmotic solution concentration resulted in increased water removal rate. Based on the statistical indices, the Two Terms model was the one that best described the drying kinetics of the samples for all...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carica papaya; Osmotic dehydration; Effective diffusivity.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662020000300200

Physico-chemical characteristics of passion fruit flour under removal of flavedo and of maceration
Provedor de dados: 91
Autores: Silva,Elaine C. O. da; Silva,Wilton P. da; Gomes,Josivanda P.; Silva,Cleide D. P. da S. e; Souto,Leidjane M. de; Costa,Zanelli R. T.
ABSTRACT Passion fruit has the peel (albedo and flavedo) as its major component and it can be used in the production of flour as source of nutrients and enrichment of food products. Thus, this study aimed to evaluate the production of flours from passion fruit albedo and whole peel, verifying the influences of flavedo removal and maceration, as well as the variation in drying temperature (70 and 80 °C) on the physical and chemical characteristics of the flours. The flours has a light color with slight trend to red and stronger trend to yellow. Moisture content is within the limits established by the current norms of ANVISA (a maximum of 15%). The flavedo removal contributed to the increase of water, crude fiber, neutral detergent fiber and acid detergent...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Passiflora edulis; Albedo; Waste management; Yellow passion fruit.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662019001100869