Consulta: creatorFacets:"Streck,E. V."
Registros recuperados: 3
Data/hora: 02/06/2024 13:15:27

Reconsolidation of the soil surface after tillage discontinuity, with and without cultivation, related to erosion and its prediction with RUSLE
Provedor de dados: 90
Autores: Streck,E. V.; Cogo,N. P.
Site-specific regression coefficient values are essential for erosion prediction with empirical models. With the objective to investigate the surface-soilconsolidation factor, Cf, linked to the RUSLE's prior-land-use subfactor, PLU, an erosion experiment using simulated rainfall on a 0.075 m m-1 slope, sandy loam Paleudult soil, was conducted at the Agriculture Experimental Station of the Federal University of Rio Grande do Sul (EEA/UFRGS), in Eldorado do Sul, State of Rio Grande do Sul, Brazil. Firstly, a row-cropped area was excluded from cultivation (March 1995), the existing crop residue removed from the field, and the soil kept clean-tilled the rest of the year (to get a degraded soil condition for the intended purpose of this research). The soil was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water erosion; Simulated rainfall; Soil consolidation; RUSLE equation.
Ano: 2003
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832003000100015

Surface and subsurface decomposition of a desiccated grass pasture biomass related to erosion and its prediction with RUSLE
Provedor de dados: 90
Autores: Cogo,N. P.; Streck,E. V.
Erosion is deleterious because it reduces the soil's productivity capacity for growing crops and causes sedimentation and water pollution problems. Surface and buried crop residue, as well as live and dead plant roots, play an important role in erosion control. An efficient way to assess the effectiveness of such materials in erosion reduction is by means of decomposition constants as used within the Revised Universal Soil Loss Equation - RUSLE's prior-land-use subfactor - PLU. This was investigated using simulated rainfall on a 0.12 m m-1 slope, sandy loam Paleudult soil, at the Agriculture Experimental Station of the Federal University of Rio Grande do Sul, in Eldorado do Sul, State of Rio Grande do Sul, Brazil. The study area had been covered by native...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water erosion; Simulated rainfall; Crop biomass decomposition; RUSLE equation.
Ano: 2003
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832003000100016

Erosão hídrica influenciada por condições físicas de superfície e subsuperfície do solo resultantes do seu manejo, na ausência de cobertura vegetal
Provedor de dados: 90
Autores: Volk,L. B. S.; Cogo,N. P.; Streck,E. V.
Práticas diferenciadas de manejo resultam em condições físicas de superfície e subsuperfície do solo distintas, as quais, por sua vez, resultam em níveis de erosão hídrica variados. Com isto em mente, realizou-se um estudo a campo com o objetivo de avaliar o efeito de formas de preparo e cultivo do solo e de manejo dos resíduos culturais em algumas de suas condições físicas de superfície e subsuperfície, em relação à erosão hídrica, durante 5,5 anos. Para tal, utilizou-se chuva simulada sobre um Argissolo Vermelho distrófico típico, bastante degradado pelo manejo anterior, com declividade de 0,08 m m-1. Os tratamentos consistiram dos cultivos de milho e aveia preta, em semeadura direta e em preparo convencional de solo (este com incorporação e com remoção...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Perda de solo; Perda de água; Chuva simulada; Preparo do solo; Consolidação do solo; Rugosidade superficial do solo; Manejo do resíduo cultural.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832004000400016