Consulta: creatorFacets:"Sunada,Natália da Silva"
Registros recuperados: 10
Data/hora: 05/06/2024 01:20:55

Effects of biofertilizer rates on the structural, morphogenetic and productive characteristics of Piatã grass
Provedor de dados: 96
Autores: Orrico Junior,Marco Antonio Previdelli; Centurion,Stanley Ribeiro; Orrico,Ana Carolina Amorim; Sunada,Natália da Silva.
The objective of this study was to investigate the influence of different levels of biofertilizers from cattle and swine manure on the structural, morphogenetic and productive characteristics of Brachiaria brizantha cv. Piatã. The experiment was arranged in a completely randomized factorial design with split plots. The plots were defined by eight treatments: two biofertilizers (cattle and swine), four levels (0, 100, 200 and 300 kg N.ha-1) and subplots by four different cutting periods. The cutting for plant uniformity was performed at 45 days after sowing at 15 cm above the soil surface. The biofertilizeres were applied in a single level, after the cutting of plants, in rates of 0, 0.23 and 0.19, 0.45 and 0.38, 0.68 and 0.57 liters pot-1 for the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brachiaria brizantha; Forage production; Organic fertilizer; Phyllochron.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-35982012000600009

Potential of biogas and methane production from anaerobic digestion of poultry slaughterhouse effluent
Provedor de dados: 96
Autores: Sunada,Natália da Silva; Orrico,Ana Carolina Amorim; Orrico Júnior,Marco Antônio Previdelli; Vargas Junior,Fernando Miranda de; Garcia,Rodrigo Garófallo; Fernandes,Alexandre Rodrigo Mendes.
The objective of this study was to evaluate the efficiency of anaerobic digestion on the treatment of effluent from poultry slaughterhouse. The experiment was conducted at the Laboratory of Waste Recycling from Animal Production/FCA/UFGD. During four weeks, eight experimental digesters, semi-continuous models, were loaded and set according to the hydraulic retention time (HRT) of 7, 14, 21 and 28 days, and according to the solid fraction treatment, separated with 1 mm sieve or without separation. The average weekly production of biogas and methane as well as the methane concentrations, the potential production per amount of chemical oxygen demand (COD) added and reduced, the concentrations of N, P and K at the beginning and end of process, and the most...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chemical oxygen demand; Total solids; Volatile solids.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-35982012001100013

Crude glycerin in anaerobic co-digestion of dairy cattle manure increases methane production
Provedor de dados: 63
Autores: Simm,Silvana; Orrico,Ana Carolina Amorim; Orrico Junior,Marco Antonio Previdelli; Sunada,Natália da Silva; Schwingel,Alice Watte; Mendonça Costa,Mônica Sarolli Silva de.
ABSTRACT Anaerobic digestion of crude glycerin (CG) along with animal waste has been an excellent option for increasing the production of biogas and methane to achieve efficiency in the treatment of both residues. This study aimed to evaluate improvements in specific productions of biogas and methane, reductions in solid and fibrous components in substrates prepared with dairy cattle manure and CG (containing 14 % glycerol). With these residues, experimental substrates were prepared and placed in 25 batch digesters. Initial content of the TS in the influent was 4 % and CG was added in increasing doses (0, 5, 10, 15 and 20 % relative to total solids (TS) of the influent). Results were submitted to ANOVA and orthogonal contrasts to assess the effects of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycerol; Biogas; Anaerobic digestion; Solids.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162017000300175

Crude glycerin in co-composting with laying hen manure reduces N losses
Provedor de dados: 63
Autores: Orrico Junior,Marco Antonio Previdelli; Orrico,Ana Carolina Amorim; Fava,Aldo Felipe; Sunada,Natália da Silva; Schwingel,Alice Watte; Garcia,Rodrigo Garófallo; Borquis,Rusbel Raul Aspilcueta.
ABSTRACT: The composting of laying hen manure is an efficient way of treating waste and producing an organic fertilizer with excellent characteristics; however, the high N losses reduce its concentration in the resulting fertilizer. Associating this residue with crude glycerin (CG) promotes a better C:N ratio and contributes to higher N retention during composting, with improvements in solids reduction and production of organic fertilizer with higher concentration of this nutrient. We carried out this research considering the hypothesis that adding CG – a byproduct of biodiesel production – to laying hen waste composting provides better N retention in the fertilizer generated. Increasing CG doses (0, 3, 6, 9, and 12 % in relation to the fresh mass in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Windrows; Total solids; Volatile solids.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162018000500361

Biogas production: litter from broilers receiving direct-fed microbials and an enzyme blend
Provedor de dados: 63
Autores: Praes,Maria Fernanda Ferreira Menegucci; Lucas Junior,Jorge de; Orrico,Ana Carolina Amorim; Orrico Junior,Marco Antonio Previdelli; Hermes,Rafael Gustavo; Sorbara,José Otávio Berti; Duarte,Karina Ferreira; Schwingel,Alice Watte; Sgavioli,Sarah; Domingues,Carla Heloisa de Faria; Sunada,Natália da Silva.
ABSTRACT The effect of additives used in the feed of broilers on anaerobic bio-digestion of poultry litter was evaluated. Four diets were used: NC: negative control; DFM: NC + 500 ppm direct-fed microbials (DFM) containing Bacillus subtilis and Bacillus licheniformis; ENZ: diet formulated with an enzyme blend (20 ppm phytase, 200 ppm protease and 200 ppm xylanase); DFM+E: ENZ + DFM. Substrates for the anaerobic bio-digestion were prepared with litter from each treatment, containing 4 % total solids (TS). These were used in 16 continuous bio-digesters with a 2 kg d−1 load, to determine the production and potential biogas production and composition during an 85-day period. Influent and effluent samples were collected for the amounts of TS and volatile solids...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Additives; Bio-digestion; Bio-digester; Methane; Livestock residues.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162016000500406

Características produtivas, morfogênicas e estruturais do capim Piatã submetido à adubação orgânica
Provedor de dados: 65
Autores: Orrico Junior,Marco Antonio Previdelli; Centurion,Stanley Ribeiro; Orrico,Ana Carolina Amorim; Oliveira,Arley Borges de Morais; Sunada,Natália da Silva.
A adubação orgânica pode ser uma alternativa viável na produção de gramíneas forrageiras, no entanto poucas são as informações referentes às doses e à composição dos principais adubos orgânicos. O objetivo do trabalho foi verificar a influência das diferentes doses de composto orgânico produzido com dois tipos de cama de frango sobre as características produtivas, morfogênicas e estruturais de Brachiaria brizantha, cv 'Piatã'. O experimento foi conduzido em casa de vegetação em delineamento inteiramente casualizado, em esquema fatorial com parcela subdividida no tempo. As parcelas foram compostas por seis tratamentos: dois tipos compostos (cama de frango a base de cana de açúcar ou napier) em três doses (100, 200 e 300kg ha-1 equivalente N) e as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brachiaria brizantha; Filocrono; Matéria seca; Nitrogênio.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782013000700015

Adição de óleo e lipase sobre a biodigestão anaeróbia de dejetos suínos
Provedor de dados: 65
Autores: Rodrigues,João Paulo; Orrico,Ana Carolina Amorim; Orrico Junior,Marco Antonio Previdelli; Seno,Leonardo de Oliveira; Araújo,Laura Costa de; Sunada,Natália da Silva.
O objetivo do trabalho foi verificar a eficiência da co-digestão anaeróbia dos dejetos suínos com crescentes níveis de adição de óleo de descarte e lipase. Foram testadas quatro doses de óleos (8, 12, 16 e 20g kg-1 de substrato) e 3 doses de lipase (1, 2 e 3g kg-1 de substrato). Os parâmetros avaliados foram: redução de sólidos totais (ST), sólidos voláteis (SV) e número mais provável (NMP) de coliformes totais (CT) e termotolerantes (CTT), além do pH, demanda química de oxigênio (DQO), produção e potenciais de produção de biogás. Os resultados demonstraram que houve influência das adições de óleo e lipase sobre as reduções de ST SV e pH do efluente, seguindo um modelo de predição linear e decrescente. As reduções do NMP de CT e CTT foram mais elevadas nos...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Biogás; Enzima; Lipídeo; Resíduo; Suíno.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782014000300025

Características morfogênicas do capim-piatã submetido à adubação com efluentes de abatedouro avícola
Provedor de dados: 65
Autores: Orrico Junior,Marco Antonio Previdelli; Orrico,Ana Carolina Amorim; Centurion,Stanley Ribeiro; Sunada,Natália da Silva; Vargas Junior,Fernando Miranda de.
O objetivo do trabalho foi avaliar diferentes doses de efluente de abatedouro avícola para proporcionar melhorias nas características produtivas, morfogênicas e estruturais do capim-piatã. O experimento foi conduzido em casa de vegetação, adotando-se delineamento inteiramente casualizado, em que foram testadas cinco doses de efluentes: 324, 648, 972, 1.296 e 1620m³ ha-1 ou equivalente a 50, 100, 150, 200 e 250kg ha-1 de N. As variáveis mensuradas foram: produção de matéria seca (MS), taxa de aparecimento de folha (TApF), taxa de alongamento de folha (TAlF), filocrono, taxa de alongamento de pseudocolmo (TAlC), comprimento final de folha (CFF) e números de folhas verdes (NFV). A produção de MS seguiu um modelo linear de predição em função das doses efluente...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adubação orgânica; Brachiaria brizantha; Filocrono; Matéria seca.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782013000100026

Compostagem de resíduo sólido de abatedouro avícola
Provedor de dados: 65
Autores: Sunada,Natália da Silva; Orrico,Ana Carolina Amorim; Orrico Junior,Marco Antônio Previdelli; Centurion,Stanley Ribeiro; Oliveira,Arley Borges de Morais; Fernandes,Alexandre Rodrigo Mendes; Lucas Junior,Jorge de; Seno,Leonardo de Oliveira.
Em virtude da grande demanda por proteína de origem animal, tem-se aumentado a produção de frangos de corte e consequentemente a geração de resíduos provenientes do abate de aves, sendo necessário o desenvolvimento de técnicas que permitam o aproveitamento e reciclagem desses materiais. Objetivou-se com a execução deste trabalho avaliar a eficiência da compostagem no tratamento e reciclagem do resíduo sólido de abatedouro avícola. Utilizou-se resíduo sólido de abatedouro avícola comercial composto por fragmentos de vísceras, tecido muscular, adiposo e ósseo, sangue coagulado e penas e, como fonte de carbono, a casca de arroz. Montou-se uma leira com 1,5m3 de volume inicial, na qual foram monitorados os parâmetros: temperatura, teores de sólidos totais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Matéria orgânica compostável; Matéria orgânica resistente à compostagem; Reciclagem de nutrientes; Tratamento aeróbio.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782015000100178

Anaerobic co-digestion of animal manure at different waste cooking oil concentrations
Provedor de dados: 65
Autores: Sunada,Natália da Silva; Orrico,Ana Carolina Amorim; Orrico Junior,Marco Antonio Previdelli; Lucas Junior,Jorge de; Lopes,Walter Renato Teixeira; Schwingel,Alice Watte.
ABSTRACT: This study aimed to obtain the best dose of waste cooking oil inclusion for the co-digestion of substrates prepared with dairy cattle and swine manure in order to maximize solids reductions and biogas yield. Analyses of total solids (TS), volatile solids (VS), and neutral detergent fiber (NDF) were performed during the loading and unloading of digesters, while biogas yield was measured twice a week. The maximum reduction in VS (51.4%) was reached with the inclusion of up to 54.6g waste cooking oil.kg manure-1. Maximum NDF degradation occurred with inclusions of up to 69.4g waste cooking oil.kg manure-1. Inclusions of up to 64g of waste cooking oil.kg manure-1 provided specific biogas yield of 291.4 and 251.0L biogas.kg VS-1 added to substrates...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digestion; Biogas; Energy recycling.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782018000700351