Consulta: creatorFacets:"Van Eck, B.T.M."
Registros recuperados: 3
Data/hora: 17/06/2024 18:11:24

General description of the Scheldt estuary
Provedor de dados: 27
Autores: Baeyens, W.F.J.; Van Eck, B.T.M.; Lambert, C.; Wollast, R.; Goeyens, L.
A general description of the Scheldt estuary, including the hydrology, the sediment transport, the productivity and the biodegradation with respect to their influence on the trace metal behaviour in the Scheldt estuary, is given. The river basin can be divided in several sections according to their morphological, hydrodynamical and sedimentary properties. The zone from km 78 to 55, which corresponds roughly with the salinity zone from 2 to 10 psu, is the zone of high turbidity, high sedimentation and of oxygen depletion, especially in the summer period. That area is called the geochemical filter because the solid/dissolved distribution of the trace metals is controlled by redox, adsorption/desorption, complexation and precipitation/coprecipitation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: ANE; Netherlands; Westerschelde.
Ano: 1998
URL: http://www.vliz.be/nl/open-marien-archief?module=ref&refid=7040

Water quality modelling of the western Scheldt estuary
Provedor de dados: 27
Autores: Ouboter, M.R.L.; Van Eck, B.T.M.; Van Gils, J.A.G.; Sweerts, J.P.; Villars, M.T.
1n 1987 the National Institute for Coastal and Marine Management (the Netherlands) initiated the SAWES project (Systems Analysis WEstern Scheldt). The main goals of the project were to acquire knowledge with respect to the pollution problems in the Scheldt estuary and to apply this knowledge to management issues of the Scheldt on an operational level. The main interest was to understand quantitatively the relation between inputs of polluting substances and effects on the ecosystem. In the framework of the project, a water quality model for the Scheldt estuary was made. In 1995, the model area was expanded to include the Belgian coastal region at the mouth of the estuary. The model calculates the fate of discharged substances and establishes the relation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Heavy metals Modelling Pollution Water quality ANE; Netherlands; Westerschelde.
Ano: 1998
URL: http://www.vliz.be/nl/open-marien-archief?module=ref&refid=7062

De Scheldeatlas: een beeld van een estuarium
Provedor de dados: 27
Autores: Van Eck, B.T.M.
Tipo: Info:eu-repo/semantics/book
Palavras-chave: Atlases ANE; Netherlands; Westerschelde Belgium; Zeeschelde.
Ano: 1999
URL: http://www.vliz.be/nl/open-marien-archief?module=ref&refid=4896