Consulta: creatorFacets:"Vellame,Lucas Melo"
Registros recuperados: 7
Data/hora: 11/06/2024 09:47:31

Transpiração de plantas jovens de laranjeira 'valência' sob porta-enxerto limão'cravo' e citrumelo 'swingle' em dois tipos de solo
Provedor de dados: 94
Autores: Vellame,Lucas Melo; Coelho,Rubens Duarte; Tolentino,João Batista.
A área total irrigada em pomares cítricos no Brasil tem aumentado ao longo das décadas. A principal causa desse aumento deve-se ao uso de porta-enxertos tolerantes à Morte Súbita dos Citros, porém menos tolerantes à seca que o limão Cravo. Este trabalho tem como objetivo estudar a influência do porta-enxerto e do tipo de solo na transpiração de plantas jovens de laranjeira Valência. O experimento foi conduzido em estufa, nas dependências do Departamento de Engenharia de Biossistemas da ESALQ/USP. Mudas de laranjeira foram plantadas em caixas de 500 L. Determinou-se, simultaneamente, a transpiração de 20 plantas por meio de sondas de dissipação térmica (fluxo de seiva). Foram medidas a radiação solar global, a umidade relativa e a temperatura do ar com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiração; Método Granier; Sonda de dissipação térmica.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-29452012000100006

Transpiration of young cocoa trees under soil water restriction
Provedor de dados: 63
Autores: Fraga Junior,Luciano Sobral; Vellame,Lucas Melo; Oliveira,Aureo Silva de; Paz,Vital Pedro da Silva.
ABSTRACT: Cocoa plantations in Brazil have been expanding beyond the borders of traditional regions by implementing a strategy based on irrigation and the establishment of crops exposed to full sunlight. The quantification of transpiration is essential to the establishment and management of crops, and is the main factor in the determination of water demand. This study had as its objective the estimating of transpiration of young cocoa trees as a function of reference evapotranspiration (ETo) and soil matric potential (Ψw). Two experiments were conducted, one in a greenhouse and the other in the field, using clones and seminal plants. Soil water content, plant transpiration and reference evapotranspiration were monitored. Cocoa trees were subjected to soil...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Theobroma cacao L.; Sapflow; Evapotranspiration; Water deficit.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162021000200301

Transpiration of young cocoa trees under soil water restriction
Provedor de dados: 63
Autores: Fraga Junior,Luciano Sobral; Vellame,Lucas Melo; Oliveira,Aureo Silva de; Paz,Vital Pedro da Silva.
ABSTRACT: Cocoa plantations in Brazil have been expanding beyond the borders of traditional regions by implementing a strategy based on irrigation and the establishment of crops exposed to full sunlight. The quantification of transpiration is essential to the establishment and management of crops, and is the main factor in the determination of water demand. This study had as its objective the estimating of transpiration of young cocoa trees as a function of reference evapotranspiration (ETo) and soil matric potential (Ψw). Two experiments were conducted, one in a greenhouse and the other in the field, using clones and seminal plants. Soil water content, plant transpiration and reference evapotranspiration were monitored. Cocoa trees were subjected to soil...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Theobroma cacao L.; Sapflow; Evapotranspiration; Water deficit.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162021000200503

Load cell adoption in an electronic drag force flowmeter
Provedor de dados: 63
Autores: Camargo,Antonio Pires de; Botrel,Tarlei Arriel; Vieira,Ricardo Godoi; Pinto,Marinaldo Ferreira; Vellame,Lucas Melo.
This research introduces the development of an electronic flowmeter based on the drag force that a body experiences when immersed in a fluid stream. Its main goal was the development of an Electronic Drag Force Flowmeter (EDFF) using a load cell, as well as the evaluation of its performance parameters. The developed flowmeter should not require specialized labor, equipments, computers or any sophisticated and complex method, providing an easy and accurate way of flow estimation. This research was carried out in the following stages: (i) EDFF mechanical structure development; (ii) data acquisition system and embedded software design; and (iii) evaluation of EDFF performance parameters. EDFF has routines for instantaneous flow rate measurement, interactive...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Technology innovation; Flow measurement; Electronics on agriculture.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162011000300002

Effect of partial soil wetting on transpiration, vegetative growth and root system of young orange trees
Provedor de dados: 63
Autores: Vellame,Lucas Melo; Fraga Júnior,Eusímio Felisbino; Coelho,Rubens Duarte.
The wetted area fraction is a factor critical to the success of drip irrigation. This study aimed to evaluate the effect of partial soil wetting on transpiration, vegetative growth and root system of young orange trees. The experiment was carried out in a greenhouse where plants were grown in 0.5 m3boxes internally divided into compartments. The wetting of 12 % of soil area was tested on two types of soil cultivated with ‘Valencia’ orange trees grafted onto Rangpur lime and ‘Swingle’ citrumelo rootstocks. Transpiration was determined in 40 plants. Water extraction and root density were evaluated in the compartments. Transpiration is reduced by restriction in wetted soil area, and such reduction is influenced by the number of days after the beginning of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drip irrigation; Sap flow; Wetted bulb; Root length density.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162015000500377

Análise estatística exploratória e variabilidade da densidade do solo em um perfil de latossolo amarelo coeso do tabuleiros costeiros da Bahia
Provedor de dados: 64
Autores: Melo Filho,José Fernandes de; Oliveira,Aureo Silva de; Lopes,Leonardo da Costa; Vellame,Lucas Melo.
Com o objetivo de realizar a análise estatística exploratória e verificar a distribuição espacial vertical da densidade do solo de um LATOSSOLO AMARELO Coeso dos Tabuleiros Costeiros da Bahia, visando examinar a possibilidade de uso deste atributo na identificação do horizonte coeso em um perfil, coletaram-se 30 amostras indeformadas em cada face de uma trincheira de 1,0 m de largura x 5,0 m de comprimento x 1,5 m de profundidade. Para tanto, foram definidos cinco perfis eqüidistantes de 1,0 m em cada lado da trincheira e divididos arbitrariamente em camadas de 0,20 m de espessura. As profundidades de amostragem variaram de 0,10 a 1,10 m. A caracterização da variabilidade dos resultados foi realizada segundo o resumo estatístico com a determinação das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Densidade do solo; Solo coeso; Propriedades do solo.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542006000200002

Montagem e acurácia de um sistema experimental de pesagem para calibração de sensores de umidade do solo
Provedor de dados: 64
Autores: Santos,Ricardo Martins; Oliveira,Aureo Silva de; Vellame,Lucas Melo; Brandão,Flávia Janaína Carvalho.
O presente trabalho descreve os procedimentos de desenvolvimento e teste de um sistema de pesagem de grande capacidade para utilização em gravimetria como método padrão de calibração de sensores de umidade do solo. O trabalho foi desenvolvido no Laboratório de Irrigação e Drenagem, Centro de Ciências Agrárias e Ambientais da Universidade Federal da Bahia, campus de Cruz das Almas (12º40'S, 39º30'W), BA. O princípio de funcionamento do sistema de pesagem baseia-se no seu componente principal, a célula de carga. Utilizou-se uma célula de carga do tipo flexão, de capacidade 60 kg e sensibilidade de 2 mV/V, quando submetida à carga máxima. A calibração foi realizada por meio de massas-padrão de 1, 5, 10 e 20 kg em sete ciclos de carregamento e descarregamento....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gravimetria; Célula de carga; Instrumentação agrícola.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1413-70542006000600019