Consulta: creatorFacets:"Weirich Neto,Pedro H."
Registros recuperados: 19
Data/hora: 03/06/2024 07:36:24

PERFORMANCE OF FERTILIZER METERING MECHANISMS OF PLANTERS AS A FUNCTION OF LONGITUDINAL INCLINATION
Provedor de dados: 70
Autores: Garcia,Luiz C.; Diniz,Renan N.; Rocha,Carlos H.; Souza,Nátali M.; Weirich Neto,Pedro H.
ABSTRACT: Sowing occurs in agricultural areas with irregular relief, influencing the quality of seed and fertilizer distribution. The aim of this study was to analyze the performance of different fertilizer metering mechanisms of planters as a function of longitudinal inclination. The experimental design was a completely randomized design with five treatments and six replications. Treatments consisted of five longitudinal inclinations to the metering mechanism (−10, −5, 0, 5, and 10 degrees). The mass of fertilizer collected per minute was considered as a replication. We worked with two types of fertilizers: a mixture of granules and powder. Metering mechanisms used were a horizontal toothed rotor, helical without flow restrictor, helical with lateral...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Powder fertilizer; Operational efficiency; Granule mixtures; Variation in dosage.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601155

MANOBRAS DE SEMEADURA COM SISTEMA DE NAVEGAÇÃO
Provedor de dados: 70
Autores: Garcia,Luiz C.; Meer,Roderik W. Van Der; Souza,Nátali M. de; Justino,Altair; Weirich Neto,Pedro H.
Resumo Os sistemas de navegação por posicionamento global (GPS) estão cada vez mais presentes no campo, prometendo diminuir os custos operacionais do agricultor. O objetivo deste trabalho foi avaliar o tempo de manobra durante a operação de semeadura da soja sem e com sistema de navegação. O delineamento experimental foi inteiramente aleatorizado, com dois tratamentos e doze repetições. Os tratamentos consistiram no tempo das manobras feitas de modo convencional e utilizando-se do sistema de navegação por GPS acoplado num piloto automático. Avaliaram-se o tempo de manobra e o retorno econômico. As manobras realizadas com auxílio do sistema de navegação foram, em média, 49% mais rápidas do que as manobras realizadas de forma convencional. Houve economia de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Piloto automático; Viabilidade econômica.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200361

Semeadura do milho em sistema de plantio direto sem e com manejo mecânico da matéria seca
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Justino,Altair; Antunes,Rodolfo K.; Fornari,Allison J.; Garcia,Luiz C.
O objetivo deste trabalho foi verificar se a cultura do milho é influenciada pelo manejo mecânico da aveia-preta dessecada antes de sua semeadura, pela utilização de rolo destorroador. Os tratamentos consistiram na semeadura do milho sob a matéria seca de aveia-preta dessecada sem manejo mecânico e rolada. O experimento foi realizado em quatro propriedades, duas na safra de 2007/2008 e as outras duas na safra de 2008/2009. O delineamento experimental adotado foi em blocos ao acaso, com 11 repetições, cujas parcelas possuíam 80 m² cada. Avaliaram-se a qualidade da semeadura e os componentes de rendimento. Conclui-se que o manejo mecânico da palha de aveia-preta antes da semeadura do milho pode elevar significativamente os espaçamentos falhos e reduzir...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aveia-preta; Rolo destorroador; Componentes de rendimento.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400019

Fungicide application using a trailing boom in soybean fields
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Fornari,Allison J.; Bauer,Fernando C.; Justino,Altair; Garcia,Luiz C.
The objective of this study was to determine the effects in the yield of soybean crop utilizing a trailing boom sprayer for chemical control of late season diseases. The experimental design was randomized blocks with 04 treatments, which consisted of applying fungicides with a traditional sprayer, trailing boom, the traditional sprayer plus the trailing boom simultaneously and control (without fungicide aerial application) in 05 repetitions per treatment. The variables evaluated were: final plant population, pods per plant, grains per pod, weight of one thousand grains and yield. It was concluded that the control of foliar diseases with fungicides presented weight of one thousand grains and yield significantly higher than the average of plots without...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Late season diseases; Spray boom; Yield components.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400026

ADJUVANTS IN FUNGICIDE SPRAYING IN WHEAT AND SOYBEAN CROPS
Provedor de dados: 70
Autores: Garcia,Luiz C.; Machado Júnior,Carlos R.; Bochnia,Giovana P.; Weirich Neto,Pedro H.; Raetano,Carlos G.
ABSTRACT The objective of this study was to determine whether the combination of adjuvants to fungicides significantly alters the spray physicochemical characteristics, and potentiates the chemical control of foliar diseases, in that it may affect yield components in wheat (Triticum aestivum) and soybean (Glycine max). The experimental design was completely randomized for the spray physicochemical characteristics, and randomized blocks for the culture variables analyzed, with four treatments and five replications. Treatments consisted of control (no fungicide spraying in the shoot), with fungicides only in plant shoots, fungicides + 0.25% of the spray with adjuvant of methyl ester base of soybean oil, and fungicides + 0.05% of the spray with adjuvant...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Disease; Glycine max; Application technology; Triticum aestivum.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601110

Profundidade de deposição de semente de milho na região dos Campos Gerais, Paraná
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Schimandeiro,Adriana; Gimenez,Leandro M.; Colet,Marcelo J.; Garbuio,Paulo W.
O sistema plantio direto encontra-se hoje plenamente incorporado à região dos Campos Gerais no Paraná. A acurácia e a precisão no processo de semeadura são itens de grande importância para que tal sistema alcance sucesso. Sendo assim, foram selecionadas 50 propriedades e, em 38, determinou-se a profundidade de deposição da semente de milho. A área experimental era formada por quatro ou cinco linhas de semeadura, onde se avaliaram dez plântulas por linha. A profundidade ficou em torno de 46 mm, observando-se diferenças significativas entre as linhas, em 21 áreas. O coeficiente de variação médio ficou em torno de 20%, limite estatístico entre médio e alto. Conforme análise de outros parâmetros, tais coeficientes podem representar diferentes tipos de erro no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantio direto; Processo de semeadura; Mecanização agrícola.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400022

Comparison of metering mechanisms of corn seed
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Justino,Altair; Namur,Rodrigo T.; Domingues,José; Garcia,Luiz C.
It was compared the performance of the metering mechanism of corn seeds (Zea mays) in direct seeding in an area of ​​200 ha, a property in Piraí do Sul, State of Paraná - PR, in Brazil. It was seeded 4 maize hybrids, 50 ha of each, with seeds of different sieves. The experiment was conducted in a randomized block design (RBD), with 3 treatments and 9 repetitions for each corn hybrid. The treatments were the pneumatic seed of metering mechanisms, horizontal perforated disc with and without ramp®. The plots were 40 m² and were distributed at the early, middle and late sowing. The variables analyzed in each corn hybrid were initial population, faulty spacing, multiple spacing, acceptable spacing, and yield components. As there were no significant differences...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pneumatic system; Horizontal seed plate; Disc with ramp®.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500017

Positioning of fertilizer in corn sowing
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Justino,Altair; Frare,Ivo; Gomes,Jorge N.; Garcia,Luiz C.
The aim of this study was to determine whether the form of placing the fertilizer by the planter during the sowing under mulch in the no till system affects the yield of corn. The treatments consisted of placing the fertilizer during the seeding 0.05 m below and beside the seed, in front of the cutting blade and without fertilizer, in 03 farms during 03 cropping years. The experimental design at each farm was the randomized block, with 08 repetitions, whose plots had 30 m² each. The initial population and yield components were evaluated. Under the experimental conditions it is concluded that base fertilization can affect the yield. Fertilizer placement can affect the initial stand, but not the yield.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tillage; Seeding fertilizer; Yield components.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600010

Management zones in agriculture acording to the soil and landscape variables
Provedor de dados: 70
Autores: Delalibera,Hevandro C.; Weirich Neto,Pedro H.; Nagata,Noemi.
The study of spatial variability of soil and plants attributes, or precision agriculture, a technique that aims the rational use of natural resources, is expanding commercially in Brazil. Nevertheless, there is a lack of mathematical analysis that supports the correlation of these independent variables and their interactions with the productivity, identifying scientific standards technologically applicable. The aim of this study was to identify patterns of soil variability according to the eleven physical and seven chemical indicators in an agricultural area. It was used two multivariate techniques: the hierarchical cluster analysis (HCA) and the principal component analysis (PCA). According to the HCA, the area was divided into five management zones: zone...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Multivariate analysis; Precision agriculture; Spatial variability.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600021

Automatic and manual spray bar sections control
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Meer,Roderik W. V. D.; Vink,Peter; Justino,Altair; Garcia,Luiz C.
The use of precision farming tools in pesticide application technology can improve the techniques effectiveness during the spraying. Thus, this study aimed to compare automatic and manual systems to interrupt the syrup flow in the spray bar sections when applied in overlapped areas. The sprayings were carried out in eight places in completely randomized design. It was compared the spray consumption and the sprayed area in relation to the total area. The results indicated that in sprays performed with the automatic system there was an average savings of 17.2% of the sprayed volume. The sprayed area using the bar section's automatic control was an average 6.1% lower than the sprayed area with manual control.
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Precision farming and pesticide application technology.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600015

Performance of a diesel engine fueled with a preheated blend of soybean oil and petrodiesel
Provedor de dados: 70
Autores: Delalibera,Hevandro C.; Campolina,Nilson; Weirich Neto,Pedro H.; Ralisch,Ricardo.
Brazil is doing a major effort to find alternatives to diesel oil as combustible. Some study lines are oriented to the development of vegetable oils used as fuel, as a source of getting cheaper and have higher energy density than the converted vegetable oils, and less risk of environmental contamination. The aim of this study was to evaluate the performance, the useful life of the lubricant and some components of a Diesel Cycle engine, with an electronic injection system, in a long-term test operating with a preheated blend (65°C) of 50% (v v-1) of soybean oil in petrodiesel. There was a reduction of the useful life of the injectors which presented failure because of high wear with 264 hours of operation and showed an increase in emissions of particulate...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Electronic injection; Opacity; Lubricant.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600007

PERFORMANCE OF DIESEL ENGINE FUELLED WITH FOUR VEGETABLE OILS, PREHEATED AND AT ENGINE WORKING TEMPERATURE
Provedor de dados: 70
Autores: Delalibera,Hevandro C.; Johann,André L.; Figueiredo,Paulo R. A. de; Toledo,Anderson de; Weirich Neto,Pedro H.; Ralisch,Ricardo.
ABSTRACT With the rise of restrictions imposed by law for gases emission, several technologies both for petrodiesel (PD) or diesel engines are been applied, such as the sulfur reduction and the injection electronic command, followed of gases recirculation and/or after-treatment. The utilization of biofuels is considered as an interesting option for pollutants reduction. In this study was evaluated the performance on short duration tests (minor period than the factory indication of the lubricant lifespan) of the Diesel engine fueled with four vegetable oils. With the aim to select the most interesting oils for future evaluations in long duration tests. The analyzed variables were fuel consumption, power relative loss and opacity, for oils of linseed,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Consumption; Brake power; Opacity.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200302

QUALITY OF SEED DISTRIBUTION AT DIFFERENT SPACES BETWEEN BASE AND INTERMEDIATE BASE
Provedor de dados: 70
Autores: Garcia,Luiz C.; Weirich Neto,Pedro H.; Justino,Altair; Eurich,Joelcio; Souza,Nátali M.
ABSTRACT The aim of this study was to analyze the influence of space between the base and intermediate base on quality of seed distribution with a horizontal seed plate. The experiment was carried out in 2012 at the Laboratory of Agricultural Mechanization of the State University of Ponta Grossa - PR, Brazil, using a sowing simulation device. The experimental design was completely randomized design with four treatments and seven replications. Treatments consisted of spaces (0, 1, 2, and 3 mm) between the base and intermediate base. Replications were defined by 250 spacing between seeds. Corn (Zea mays L.), soybean (Glycine max L. Merrill), and sorghum (Sorghum bicolor Moench) seeds were tested. The analyzed variables were faulty, multiple and acceptable...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Horizontal seed plate; Glycine max; Seeder-fertilizer machine; Sorghum bicolor; Zea mays.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100128

Fragment size of corn silage according to the dry matter and forage harvester adjustments
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Garbuio,Paulo W.; Souza,Nátali M. de; Delalibera,Hevandro C.; Leitão,Khetlen.
In Brazil, the best results in milk production are found in the state of Paraná. Such results are reached through genetic selection of the animals and management of their diets, in which whole plant corn silage is widely used. Aiming the silage quality, it was evaluated the influence of dry matter content of the corn culture as forage and the harvester adjustments on the fragment size of whole plant corn silage. The fragment size of two corn hybrids silage (SPEED and 2B688) was evaluated using a 5x3 factorial, with 4 repetitions. The first factor was the harvest time of the plants (105, 108, 112, 118, and 123 days after sowing (DAS)), which determines the forage dry matter (DM) content. The second factor was the harvester adjustments (2, 6.5 and 11mm of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ensilage; Whole plant silage; Harvest time.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400016

Suscetibilidade de dois tipos de solo à compactação
Provedor de dados: 91
Autores: Weirich Neto,Pedro H.; Rosa,André L. T. da; Gomes,Jaime A.
Com vistas ao aumento da produção agrícola, optou-se no Brasil, pelo acréscimo de área cultivada; para tal o uso indiscriminado da motomecanização mostrou-se eficiente em um primeiro momento, porém acarretando problemas à física do solo no decorrer dos anos. Paralelamente, práticas conservacionistas se fazem presentes, vide semeadura sob a palha (Plantio Direto), uma realidade no sul do Brasil. Sendo assim, avaliou-se a suscetibilidade de compactação de dois tipos de solo, ambos com sistema de semeadura sob a palha. Para dimensionar a suscetibilidade a compactação, utilizou-se ensaio de Proctor. Os solos foram ensaiados com e sem a presença de matéria orgânica livre. Os resultados demonstraram que para o Cambissolo, textura média, não houve diferença nos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ensaio de Proctor; Plantio direto; Matéria orgânica.
Ano: 2002
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662002000200027

Adequação de propriedades rurais ao Código Florestal Brasileiro: estudo de caso no estado do Paraná
Provedor de dados: 91
Autores: Okuyama,Kássio K.; Rocha,Carlos H.; Weirich Neto,Pedro H.; Almeida,Dayana; Ribeiro,Diogenes R. S.
O Código Florestal Brasileiro de 1965 conceitua e regulamenta as Áreas de Preservação Permanente (APP) e Reserva Legal (RL). Para regulamentar a adequação das propriedades agrícolas ao código florestal, o estado do Paraná instituiu o SISLEG - Sistema de Manutenção, Recuperação e Proteção da Reserva Legal e Áreas de Preservação Permanente. Neste estudo foram quantificadas, com auxílio do sistema de posicionamento global (GPS) e programas de Sistemas de Informações Geográficas (SIG), as APPs e RLs de 147 propriedades em oito municípios das regiões centro-oriental e sudeste do Paraná, visando analisá-las frente ao Código Florestal vigente. Observou-se expressiva cobertura florestal formada por fragmentos de Floresta Ombrófila Mista; as superfícies disponíveis...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reserva legal; Área de preservação permanente; Agricultura familiar.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662012000900013

Variáveis dimensionais de sementes de soja que influenciam o processo de semeadura
Provedor de dados: 91
Autores: Santos,Sérgio R. dos; Weirich Neto,Pedro H.; Fey,Emerson; Wobeto,Celso.
No processo de semeadura de soja (Glycine max (L.) Merrill), as semeadoras de precisão comumente utilizadas são as dotadas de mecanismo dosador tipo disco perfurado horizontal. Com vistas a um processo de semeadura eficiente, deve-se levar em consideração a velocidade e a homogeneidade das sementes entre outros. O objetivo deste trabalho foi estudar a influência das variáveis dimensionais das sementes de soja sobre a qualidade de semeadura. Para isto, foram usados uma semeadora de precisão, três cultivares de soja e quatro discos dosadores de náilon, submetidos a cinco velocidades de deslocamento. Como variáveis dependentes, analisou-se a porcentagem de enchimento do disco dosador e a porcentagem de danos físicos perceptíveis visualmente nas sementes. Com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycine max; Sementes de soja; Semeadora de precisão; Discos dosadores.
Ano: 2003
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662003000100029

Necessidade de fertilizante e calcário em área sob sistema plantio direto considerando variabilidade espacial
Provedor de dados: 91
Autores: Weirich Neto,Pedro H.; Sverzut,Cláudio B.; Schimandeiro,Adriana.
A região dos Campos Gerais do Paraná é pioneira no sistema plantio direto, apresentando rendimentos elevados e alta tecnificação. Neste sentido, surgem técnicas para auxiliar na otimização desses processos, a exemplo da agricultura de precisão ou manejo localizado de solo e culturas. Com este trabalho, objetivou-se avaliar as necessidades localizadas de fertilizante e calcário em lavoura comercial sob sistema plantio direto e comparar os resultados com a recomendação tradicional. As amostras de solo foram coletadas em malha retangular, formada por quatro linhas de quinze pontos eqüidistantes 40 m, totalizando 60 pontos (9,6 ha). Os dados de capacidade de troca catiônica (CTC), saturação por bases (V%), fósforo (P) e potássio (K) foram analisados pela...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Taxa variável de reposição; Fertilidade do solo.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662006000200013

Alocação de reserva legal em propriedades rurais: do cartesiano ao holístico
Provedor de dados: 91
Autores: Delalibera,Hevandro C.; Weirich Neto,Pedro H.; Lopes,Angelo R. C.; Rocha,Carlos H.
Ao exigir áreas de Preservação Permanente (APP) e Reserva Legal (RL) em todos os imóveis rurais do Brasil, o Código Florestal Brasileiro (Lei Federal 4771/1965) se reverte em um dos instrumentos mais importantes com o propósito de mitigar impactos ambientais das atividades agrícolas. Como em outros estados, no Paraná esta legislação também foi ignorada; para cumprir o disposto no Código Florestal e estipular prazo para as adequações necessárias, foi instituído o Sistema de Manutenção, Recuperação e Proteção da Reserva Legal e Áreas de Preservação Permanente - SISLEG (Decreto Estadual 387/1999). Com o objetivo de se analisar essas normativas, elaborou-se um estudo de imóvel rural típico dos Campos Gerais do Paraná e, com base em técnicas de sensoriamento...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Código florestal; Área de preservação permanente; SISLEG; Geoprocessamento.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662008000300010