Consulta: creatorFacets:"Yolsal-cevikbilen, S."
Registros recuperados: 1
Data/hora: 05/06/2024 13:21:09

3-D sediment-basement tomography of the Northern Marmara trough by a dense OBS network at the nodes of a grid of controlled source profiles along the North Anatolian fault
Provedor de dados: 5
Autores: Bayrakci, Gaye; Laigle, Mireille; Becel, A.; Hirn, A.; Taymaz, T.; Yolsal-cevikbilen, S.
A 3-D tomographic inversion of first arrival times of shot profiles recorded by a dense 2-D OBS network provides an unprecedented constraint on the P-wave velocities heterogeneity of the upper-crustal part of the North Marmara Trough (NMT), over a region of 180 km long by 50 km wide. One of the specific aims of this controlled source tomography is to provide a 3-D initial model for the local earthquake tomography (LET). Hence, in an original way, the controlled source inversion has been performed by using a code dedicated to LET. After several tests to check the results trade-off with the inversion parameters, we build up a 3-D a priori velocity model, in which the sea-bottom topography, the acoustic and the crystalline basements and the Moho interfaces...
Tipo: Text
Palavras-chave: Body waves; Seismic tomography; Continental tectonics: strike-slip and transform; Crustal structure.
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00185/29601/28033.pdf