Consulta: creatorFacets:"Yusuf, Kamorudeen Olaniyi"
Registros recuperados: 2
Data/hora: 13/06/2024 02:12:11

Effects of magnetized water on the vegetative growth and yield of tomato
Provedor de dados: 111
Autores: Yusuf, Kamorudeen Olaniyi.
This study was conducted to determine the effect of magnetized water on the vegetative growth and yield of tomato.  The values of magnetic flux densities used for treating the irrigation water varied from 124 to 719 G (T2 to T10) were produced from electromagnet and T1 was the control experiment which was not treated with magnetic field.  The water after passing through (treated with) magnetic field (T2 to T10) was called magnetized water while the control experiment (T1) was called non-magnetized water.  The experimental layout for the study was a 10 by 10 Latin Square Design.  The tomato (variety UC82B) was planted in 100 buckets in a transparent garden shed for 130 d and irrigated with magnetized and non-magnetized water, respectively.  The heights of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural Engineering and Soil and Water Option magnetized water; Tomato yield; Vegetative growth; Irrigation; Electromagnet; Magnetic field.
Ano: 2017
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/3258

Effect of Magnetized Water on Water Use Efficiency, Yield and Nutritional Qualities of Watermelon under Deficit Irrigation
Provedor de dados: 111
Autores: Yusuf, Kamorudeen Olaniyi; Ogunbamowo, Tolulope Ruth; Obalowu, Rasheed Olarewaju.
Magnetized water (MW) is a non-chemical method and new technology for crop production. It is environmentally-friendly which improves water use efficiency (WUE) and enhances high crop yield. The study was conducted to determine the effect of MW on WUE, yield and nutritional qualities of watermelon under deficit irrigation in a garden shed. A Completely Randomized Design was used for the experimental layout. Irrigation water was treated using magnetic flux density of 319 gauss. Water applied as the treatments were 100%, 80%, 60% and 50% water requirement and each treatment was replicated four times. Watermelon seed (variety: Kaolack with LOT number: VG-PV-0519-KA) was planted in 15 litres/pot (285 mm diameter and 255 mm depth) with 16 pots for MW and 16 pots...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Magnetized water; Water use efficiency; Watermelon; Paired t-test.
Ano: 2020
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/5833