Consulta: subjectFacets:"Bio-ethanol"
Registros recuperados: 5
Data/hora: 11/06/2024 09:00:39

The Role of Systems Modeling for Sustainable Development Policy Analysis: the Case of Bio-Ethanol
Provedor de dados: 7
Autores: Chan, Albert W; National Research Council of Canada; albert.chan@nrc.ca; Hoffman, Robert T; ;; McInnis, Bert; ;.
A dynamic systems modeling technique has been developed to assess technologies according to the criterion of sustainability. In a case study, the potential contribution of bio-ethanol toward achieving Canada&amp;#8217;s commitment to the Kyoto targets for greenhouse gas reductions is analyzed. The analysis concludes that, although bio-ethanol may help reduce greenhouse gas emissions, the technology by itself is insufficient to meet the Kyoto target. Applying the systems modeling approach to analyze sustainability helps highlight those policy issues that warrant more in-depth study. Although the systems model may not provide definitive answers, it raises relevant questions about physical constraints that might be encountered and estimates the extent to...
Tipo: Peer-Reviewed Reports
Palavras-chave: Bio-ethanol; Biofuels; Dynamic systems modeling; Emission targets; Energy crops; Light-duty vehicles; Policy analysis; Sustainability analysis.
Ano: 2004

Efficient use of unexploited agricultural and fishery resources in the Tokachi district- Focusing on research, development and commercialization
Provedor de dados: 19
Autores: Ohba, Kiyoshi.
2005年8月4日とかちプラザ・レインボーホールで開催､日本ユネスコ国内委員会主催の帯広農村開発教育国際セミナー(OASERD)国際連合ユネスコアジア太平洋地域教育開発計画事業(APEID)シンポジウム「地球にやさしい農業をめざして :　資源リサイクルを利用した持続可能な食糧生産－」講演資料
Palavras-chave: Dried salmon; Potato peptide; Pumpkin fiber and seed; Adzuki bean; Polyphenol; Bio-ethanol.
Ano: 2005
URL: http://ir.obihiro.ac.jp/dspace/handle/10322/1898

BIOHAJTÓANYAGOK HELYZETE MAGYARORSZÁGON
Provedor de dados: 31
Autores: Taralik,   Krisztina.
Ha a Magyarországon jelenleg tervezett összes bioetanol- és biodízel-üzem felépül, akkor kb. 2,6-3 millió tonna bioetanol és 400 ezer tonna biodízel előállítása válik lehetővé. Ez a mennyiség amellett, hogy jelentősen meghaladja a hazai 2010-es 5,75%-os bekeverési arányhoz szükséges mennyiséget, inputigényét tekintve már középtávon is jelent_s importot tehet szükségessé. Ennek árfelhajtó hatása befolyásolhatja egyrészt a biohajtóanyag-előállítás gazdaságosságát, másrészt az állattenyésztésben és az élelmiszeriparban feszültségeket eredményezhet. Érdemes tehát megvizsgálni, hogy milyenek a lehetőségek és a korlátok a biohajtóanyagok inputjában.              -             If all planned bio-ethanol and bio-diesel plants are built, Hungary will be able to...
Tipo: Journal Article
Palavras-chave: Bioetanol; Biodízel; Tervezett feldolgozó kapacitások; Inputhiány; Bio-ethanol; Bio-diesel; Planned processing capacities; Lack of inputs; Agricultural and Food Policy; Land Economics/Use.
Ano: 2007
URL: http://purl.umn.edu/57721

Magyarország régióinak értékelése a bioüzemanyagok kisüzemi előállításának szempontjából
Provedor de dados: 31
Autores: Vida,   Adrienn.
Az elmúlt években több elemzés látott napvilágot azzal kapcsolatban, hogy Magyarország adottságai melyik megújítható energiaforrás hangsúlyozott felhasználására alkalmasak. A korábban jellemző mezőgazdasági túltermelés, klímaváltozás, a fosszilis energiahordozók drasztikus és tartós áremelkedése azonban hazánkban is a bioüzemanyagok irányába terelte a figyelmet. A fokozott érdeklődést indokolja továbbá, hogy a biomassza ilyen irányú felhasználása komplex megoldást kínál nem csupán a fenti problémákra, de a gazdálkodók számára is lehetőséget nyújt az optimális és az életszínvonal emelésére is alkalmas termelési szerkezet kialakítására. A kutatás során a szakirodalomban fellelhető módszertan kiegészítésével és részbeni átalakításával olyan elemzés készült,...
Tipo: Journal Article
Palavras-chave: Bioetanol; Biodízel; BtL; Fenntartható mezőgazdaság; Kisüzemi rendszer.; Bio-ethanol; Bio-diesel; BtL; Sustainable agriculture; Small scale production.; Agricultural and Food Policy; Crop Production/Industries; Environmental Economics and Policy.
Ano: 2009
URL: http://purl.umn.edu/92420

Ethanol fermentation of sugarcane molasses by Zymomonas mobilis MTCC 92 immobilized in Luffa cylindrica L. sponge discs and Ca-alginate matrices
Provedor de dados: 58
Autores: Behera,Shuvashish; Mohanty,Rama C.; Ray,Ramesh C.
Bio-ethanol production from cane molasses (diluted to 15 % sugar w/v) was studied using the bacterium, Zymomonas mobilis MTCC 92 entrapped in luffa (Luffa cylindrica L.) sponge discs and Ca-alginate gel beads as the immobilizing matrices. At the end of 96 h fermentation, the final ethanol concentrations were 58.7 ± 0.09 and 59.1 ± 0.08 g/l molasses with luffa and Ca-alginate entrapped Z. mobilis cells, respectively exhibiting 83.25 ± 0.03 and 84.6 ± 0.02 % sugar conversion. There was no statistical significant difference (Fischer's LSD) in sugar utilization (t = 0.254, p &lt;0.801) and ethanol production (t =-0.663, p &lt;0.513) between the two immobilization matrices used. Further, the immobilized cells in both the matrices were physiologically active for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bio-ethanol; Cell immobilization; Fermentation; Molasses; Zymomonas mobilis MTCC 92.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1517-83822012000400034