Consulta: subjectFacets:"Corn stover"
Registros recuperados: 8
Data/hora: 11/06/2024 08:10:28

Xylanolytic enzymes production by Aspergillus niger GS1 from solid-state fermentation on corn stover and their effect on ruminal digestibility
Provedor de dados: 69
Autores: Regalado,Carlos; Vázquez-Obregón,Immer; García-Almendárez,Blanca Estela; Domínguez-Domínguez,Jorge; Aguilera-Barreyro,Araceli; Amaro-Reyes,Aldo.
Hemicellulosic agricultural by-products such as corn stover (CS) are highly available materials which represent an opportunity to develop value added products. Native Aspergillus niger GS1 was used for solid-state fermentation (SSF) on alkali pre-treated CS (ACS) aimed to optimize xylanolytic enzymes production, and their effect on in vitro ruminal and true digestibility of ACS. Enzyme production was empirically modelled using a fractional factorial design 2(9-5), and the resulting significant factors were glucose, yeast extract and two mineral salts, which were arranged in a Draper-Lin optimization design at two levels. Predicted optimum xylanolytic activity of 33.6 U (mg protein)-1 was achieved at 48 hrs of SSF, and was validated by confirmatory...
Tipo: Journal article
Palavras-chave: Aspergillus niger GS1; Corn stover; Digestibility; Solid-state fermentation; Xylanolytic activity.
Ano: 2011
URL: http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0717-34582011000200009

Land Use Implications of Expanding Biofuel Demand
Provedor de dados: 31
Autores: Dicks,   Michael R.; Campiche,   Jody L.; Torre Ugarte,   Daniel de la; Hellwinckel,   Chad M.; Bryant,   Henry L.; Richardson,   James W.
The Renewable Fuel Standard mandates in the Energy Independence and Security Act of 2007 will require 36 billion gallons of ethanol to be produced in 2022. The mandates require that 16 of the 36 billion gallons must be produced from cellulosic feedstocks. The potential land use implications resulting from these mandates were examined using two methods, the POLYSYS model and a general equilibrium model. Results of the POLYSYS analysis indicated that 72.1 million tons of corn stover, 23.5 million tons of wheat straw, and 24.7 million acres would be used to produce 109 million tons of switchgrass in 2025 to meet the mandate. Results of the CGE analysis indicated that 10.9 billion bushels of corn grain, 71 million tons of corn stover, and 56,200 tons of...
Tipo: Journal Article
Palavras-chave: Cellulosic ethanol; Corn stover; Grain ethanol; Renewable fuel standard; Switchgrass; Crop Production/Industries; Demand and Price Analysis; Environmental Economics and Policy; Land Economics/Use; Resource /Energy Economics and Policy; Q15; Q42.
Ano: 2009
URL: http://purl.umn.edu/53091

Choice of optimum feedstock portfolio for a cellulosic ethanol plant  – A dynamic linear programming solution
Provedor de dados: 31
Autores: Kumarappan,   Subbu; Ivanic,   Rasto.
When the lignocellulosic biofuels industry reaches maturity and many types of biomass sources become economically viable, management of multiple feedstock supplies – that vary in their yields, density (tons per unit area), harvest window, storage and seasonal costs, storage losses, transport distance to the production plant – will become increasingly important for the success of individual enterprises. The manager’s feedstock procurement problem is modeled as a multi-period sequence problem to account for dynamic management over time. The case is illustrated with a hypothetical 53 million annual US gallon cellulosic ethanol plant located in south west Kansas that requires approximately 700,000 metric dry tons of biomass. The problem is framed over 40...
Tipo: Conference Paper or Presentation
Palavras-chave: Cellulosic ethanol; Feedstock; Switchgrass; Miscanthus; Corn stover; Optimization; Biofuels; Biomass; Energy; Renewable; Agribusiness.
Ano: 2009
URL: http://purl.umn.edu/49407

The Economics of Harvesting and Transporting Corn Stover for Conversion to Fuel Ethanol: A Case Study for Minnesota
Provedor de dados: 31
Autores: Petrolia,   Daniel R.
Corn stover harvest and transport cost functions were estimated for two harvest operations for a proposed biomass-to-ethanol conversion facility located in southern Minnesota, USA.  This work presents an alternative methodology to estimating corn stover quantities and harvest costs at the county level, taking into account county-specific yields, transportation distances, erosion constraints, machinery specifications, and other key variables.  Monte Carlo simulation was also used to estimate the probability distribution of costs under alternative assumption on key parameters whose values vary widely in the literature.  Marginal stover cost for 50MM gal/year of ethanol output was estimated at $54/dt ($0.77/gal ethanol) for the more intensive harvest method...
Tipo: Working or Discussion Paper
Palavras-chave: Biomass; Corn stover; Economics; Ethanol; Lignocellulose; Monte Carlo; Crop Production/Industries; Resource /Energy Economics and Policy.
Ano: 2006
URL: http://purl.umn.edu/14213

Impact of a corn stover market on corn and soybean production: empirical estimation
Provedor de dados: 31
Autores: Kurkalova,   Lyubov A.
We quantify empirically the shifts in corn and soybean production possibilities frontier under alternative corn stover prices.
Tipo: Conference Paper or Presentation
Palavras-chave: Corn stover; Production possibilities frontier; Production Economics; Q11; Q42.
Ano: 2011
URL: http://purl.umn.edu/103582

A Corn Stover Supply Logistics System
Provedor de dados: 31
Autores: Morey,   R. Vance; Kaliyan,   Nalladurai; Tiffany,   Douglas G.; Schmidt,   David R.
Published in Applied Engineering in Agriculture, Vol. 26(3): 455‐461, 2010.  American Society of Agricultural and Biological Engineers
Tipo: Journal Article
Palavras-chave: Corn stover; Economics; GHG emission; Logistics; Roll press compaction; Tub grinding; Agribusiness; Crop Production/Industries.
Ano: 2010
URL: http://purl.umn.edu/91342

Modeling Cellulosic Bioenergy Feedstock Supply
Provedor de dados: 31
Autores: Archer,   David W.
Tipo: Conference Paper or Presentation
Palavras-chave: Bioenergy; Feedstock; GIS; Corn stover; Wheat straw; Environmental Economics and Policy; Production Economics; Resource /Energy Economics and Policy.
Ano: 2010
URL: http://purl.umn.edu/61372

Enhanced alkaline cellulases production by the thermohalophilic Aspergillus terreus AUMC 10138 mutated by physical and chemical mutagens using corn stover as substrate
Provedor de dados: 58
Autores: Isaac,George Saad; Abu-Tahon,Medhat Ahmed.
Abstract A thermohalophilic fungus, Aspergillus terreus AUMC 10138, isolated from the Wadi El-Natrun soda lakes in northern Egypt was exposed successively to gamma and UV-radiation (physical mutagens) and ethyl methan-sulfonate (EMS; chemical mutagen) to enhance alkaline cellulase production under solid state fermentation (SSF) conditions. The effects of different carbon sources, initial moisture, incubation temperature, initial pH, incubation period, inoculum levels and different concentrations of NaCl on production of alkaline filter paper activity (FPase), carboxymethyl cellulase (CMCase) and β-glucosidase by the wild-type and mutant strains of A. terreus were evaluated under SSF. The optimum conditions for maximum production of FPase, CMCase and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermohalophilic fungus; Aspergillus terreus; Alkaline cellulase; Solid state fermentation; Corn stover.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1517-83822015000401269