Consulta: subjectFacets:"Diafiltration"
Registros recuperados: 1
Data/hora: 08/06/2024 17:40:53

Concentration and purification of Porphyridium cruentum exopolysaccharides by membrane filtration at various cross-flow velocities
Provedor de dados: 5
Autores: Balti, Rafik; Le Balc'H, Romain; Brodu, Nicolas; Gilbert, Marthe; Le Gouic, Benjamin; Le Gall, Sophie; Sinquin, Corinne; Masse, Anthony.
Exopolysaccharides (EPS) from cell-free Porphyridium cruentum media were concentrated then purified (diafiltration) on a 0.14 µm ceramic membrane. The influence of cross-flow velocities on filtration performances was investigated. Mean permeate fluxes equal to 49.8, 68.9 and 81.9 L.h-1. m-2 were obtained during the concentration at 4 bar for respectively cross-flow velocities inside the membrane lumen equal to 2.5, 3.3 and 4.2 m.s-1; 49.7 L.h-1. m-2 for the diafiltration at 3.3 m.s-1. Permeate fluxes were correctly predicted from polysaccharide concentrations (10 % deviation). Volume reduction factors higher than 7.8 were reached. Rejection rates of polysaccharides and proteins varied according to the cross-flow velocities. Thus, the EPS recovery rate or...
Tipo: Text
Palavras-chave: Membrane filtration; Exopolysaccharides; Microalga; Concentration; Diafiltration.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00445/55694/57360.pdf