Consulta: subjectFacets:"Drying  biomass fuel"
Registros recuperados: 1
Data/hora: 11/06/2024 06:36:20

DRYING KINETICS OF UNRIPE PLANTAIN CHIPS USING CHARCOAL FUELLED CABINET DRYER.
Provedor de dados: 111
Autores: Famurewa, John Alaba Victor.
This study presents the thin layer drying behavior of unripe plantain slices (Musa paradisiaca) in a developed biomass cabinet dryer. The developed dryer provided an environment with an optimum operating temperature between 50 - 700C meant for drying agricultural materials. The use of thin layer drying mechanisms and equations contribute to better understanding of drying food materials. The thin layer drying behaviour of agricultural products was identified based on the mathematical models which describe the heat and mass transfer phenomena of the products. In order to select a suitable drying model, fourteen different thin layer drying models were fitted to experimental data. Fick’s second law was used to calculate the moisture diffusivity with some...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Food Engineering Thin layer; Mathematical modelling; Diffusion; Drying  biomass fuel.
Ano: 2015
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/3028