Consulta: subjectFacets:"Drying characteristics"
Registros recuperados: 2
Data/hora: 12/06/2024 10:36:26

A comparative study on drying of basil leaves
Provedor de dados: 111
Autores: Parmar, Mansukhlal Ramjibhai; Kumpavat, Mahendrasinh T.; Doshi, Jayesh Sevantilal; Kapdi, Shyamsundar S.
Basil is a popular aromatic and annual herb growing in many regions of the world.  Immediately after its harvesting, the highly perishable raw material, i.e. leaves, have to be preserved against deterioration and spoilage.  More often, during peak period, most of the crop is lost/wasted due to lack of proper post-harvest processing techniques.  Drying is by far the most widely used treatment, which needs to be performed very carefully and preciously so as to preserve the aroma and color of the leaves.  Various drying treatments and experimental methods viz., solar drying, tray drying, vacuum drying and fluidized bed drying were carried out at the temperatures of45°C,55°Cand65°Cto find and suggest the optimum drying condition for acquiring quality dried...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural Engineering; Post Harvest Process and Food Engineering drying; Drying characteristics; Basil leaves; Solar drying; Tray drying; Vacuum drying and fluidized bed drying.
Ano: 2017
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/3867

Solar Tunnel Drying: Pretreatment on drying kinetic of plum tomatoes
Provedor de dados: 65
Autores: Karaaslan,Sevil; Ekinci,Kamil; Kumbul,Barbaros Salih.
ABSTRACT:  Drying of thin layer tomato was studied using a solar tunnel dryer under the ecological conditions of Isparta, Turkey. During drying process, solar irradiation, drying air temperature, relative humidity, and air velocity were measured constantly in different parts of the dryer. Drying runs were performed using plum tomatoes, characterized by an oval shape, intense red color. The change of tomatoes mass was measured daily. The color measurements of dried products were determined at the beginning and end of experiment. In this study, the fresh tomato samples were sorted, graded, washed in water and then sliced into quarters and halves before pretreated. Sun drying behavior of half and quarter sliced tomatoes pretreated with 10% NaCl solution and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drying characteristics; Tomato slices; Tunnel dryer; Mathematical modeling.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782019000700203