Consulta: subjectFacets:"Egoma leaf"
Registros recuperados: 1
Data/hora: 02/06/2024 07:31:38

Optimization of functional egoma (Perilla flutescens var. flutescens) leaf snack production
Provedor de dados: 106
Autores: Nipat Limsangouan; Chulaluck Charunuch; Seiichiro Isobe.
Optimization condition for egoma leaf snack production was investigated using response surface methodology. A central composite  design with four independent variables: screw speed; feed rate; moisture content and egoma leaf content was use to study the response variables. A second-degree equation for independent and response variables was computed and used to create the contour and surface plot graphs. The screw speed at 215 rpm, feed rate of 43.1 g/min, moisture content at 14.1 % and egoma leaf content of 3.0 % were suitable to make egoma leaf snack with the responses as 2.20 ± 0.08 (expansion ratio);  0.48 ± 0.01 g/ml (bulk density);  3451 ± 207 g (hardness); 9.80 ± 3.90 (crispness); 0.25 ± 0.02 mmol Trolox/g  (antioxidant activity); 3.02  ± 0.25 mg...
Tipo: PhysicalObject
Palavras-chave: Egoma leaf; Snack; Optimization; Functional food; Extrusion; ผลิตภัณฑ์อาหารเสริมเพื่อสุขภาพ; อาหารขบเคี้ยว; การกดอัดเป็นรูป; งาขี้ม้อน; ใบ; คุณสมบัติทางกายภาพ; คุณสมบัติเชิงหน้าที่.
Ano: 2009
URL: http://anchan.lib.ku.ac.th/agnet/handle/001/5260