Consulta: subjectFacets:"Electrocoagulation"
Registros recuperados: 1
Data/hora: 06/06/2024 10:16:44

The efficiency of electrocoagulation using aluminum electrodesin treating wastewater from a dairy industry
Provedor de dados: 65
Autores: Valente,Gerson de Freitas Silva; Mendonça,Regina Célia Santos; Pereira,José Antônio Marques.
This research deals with the investigation of electrocoagulation (EC) treatment of wastewater from a dairy plant using aluminum electrodes. Electrolysis time, pH, current density and distance between electrodes were considered to assess the removal efficiency of chemical oxygen demand (COD), total solids (TS) and their fractions and turbidity. Samples were collected from the effluent of a dairy plant using a sampling methodology proportional to the flow. The treatments were applied according to design factorial of half fraction with two levels of treatments and 3 repetitions at the central point. The optimization of parameters for treating dairy industry effluent by electrocoagulation using aluminum electrodes showed that electric current application for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Electrolysis; Dairy industry; Electrocoagulation.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782015000901713