Consulta: subjectFacets:"Flow injection"
Registros recuperados: 1
Data/hora: 14/06/2024 21:27:56

Determination of iron-porphyrin-like complexes at nanomolar levels in seawater
Provedor de dados: 5
Autores: Vong, Lilita; Laes, Agathe; Blain, Stéphane.
A new method for the non-specific determination of iron-porphyrin-like complexes in natural waters has been developed. It is based on the chemiluminescent oxidation of the luminol in the presence of dioxygen (O-2) at pH 13. The method has been implemented in a FIA manifold that allowed the direct injection of seawater. The limit of detection is 0.11 nM of equivalent hemin (Fe-protoporphyrin IX). Fe2+, Fe3+, H2O2, siderophore (deferoxamin mesylate), humic acid and phytic acid did not interfere when the), were present at the concentrations expected in seawater. Metal free porphyrin and Mg, Cu, Co porphyrin complexes did not induce a significant chemiluminescent signal. Poisoned unfiltered samples could be stored for several weeks before analyses. The new...
Tipo: Text
Palavras-chave: Chemiluminescence; Complexation; Flow injection; Seawater; Porphyrin; Iron.
Ano: 2007
URL: http://archimer.ifremer.fr/doc/2007/publication-3298.pdf