Consulta: subjectFacets:"GR4H"
Registros recuperados: 2
Data/hora: 14/06/2024 12:34:02

Vers une modélisation déterministe des écoulements de surface en Nouvelle-Calédonie. Implémentation du code GR4H sur quatre bassins versants du Grand Nouméa
Provedor de dados: 5
Autores: Desclaux, Terence; Pischedda, Marine; Lemonnier, Hugues; Soulard, Benoit; Le Gendre, Romain.
Ce rapport fait suite au stage de Marine Pischedda (Master 2 La Rochelle) réalisé au sein de l’unité de recherche "Lagons, Ecosystèmes et Aquaculture Durable en Nouvelle-Calédonie" (LEAD/NC) de l’Ifremer entre février et juillet 2016. Cette étude a été conduite sur quatre bassins versants du Grand Nouméa : la Coulée, la Dumbéa Est, la Dumbéa Nord et la Couvelée. L’objectif principal était de démontrer la pertinence de l’utilisation de modèle pluie-débit au pas de temps horaire (GR4H en l’occurrence) sur les bassins versants calédoniens. Le cadre plus général de ce travail était d’aboutir à une représentation affinée du continuum terre-mer par le couplage des modèles GR4H et MARS3D développés pour simuler la circulation côtière. Les périodes d’étiages ayant...
Tipo: Text
Palavras-chave: Continuum Terre-Lagon; Nouvelle-Calédonie; Rivières; GR4H; Bassins versants; Grand Nouméa; Modélisation; Débits; Land-lagoon continuum; New Caledonia; River; GR4H; Watershed; Nouméa; Model; River Flow.
Ano: 2017
URL: http://archimer.ifremer.fr/doc/00388/49969/50545.pdf

Suitability of a lumped rainfall–runoff model for flashy tropical watersheds in New Caledonia
Provedor de dados: 5
Autores: Desclaux, Terence; Lemonnier, Hugues; Genthon, Pierre; Soulard, Benoit; Le Gendre, Romain.
The GR4H lumped hourly rainfall–runoff model was assessed for its integration in a ridge-to-reef modelling framework. Particular attention was paid to rainfall representation, robustness of parameter estimates and ability to reproduce main runoff features. The study was conducted in four tropical mountainous watersheds in New Caledonia, exposed to intense rainfall events, large annual climatic variations triggered by El Niño oscillation, and wildfires. The inverse distance and elevation weighting algorithm outperformed other classical rainfall interpolation methods under data-limited conditions. The time-span of data needed for robust calibration was site-specific and varied from 6–7 years to 10 years, which may be linked to El Niño events and to...
Tipo: Text
Palavras-chave: Hydrological model; Ridge-to-reef; GR4H; Rainfall-runoff model; Integrated modelling; New Caledonia; Lagoon; Wildfire.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00455/56681/58466.pdf