Consulta: subjectFacets:"Impact penetrometer"
Registros recuperados: 2
Data/hora: 11/06/2024 15:22:57

Measuring mechanical impedance in clayey gravelly soils
Provedor de dados: 90
Autores: Stolf,R.; Cassel,D. K.; King,L. D.; Reichardt,K.
Mechanical impedance of clayey and gravelly soils is often needed to interpret experimental results from tillage and other field experiments. Its measurement is difficult with manual and hydraulic penetrometers, which often bend or break in such soils. The purpose of this study was to evaluate the feasibility of a hand-operated "Stolf" impact penetrometer to measure mechanical impedance (soil resistance). The research was conducted in Raleigh, North Carolina, USA (35º 45'N, 78º 42'W, elevation 75 m). Corn was planted on April 19, 1991. Penetrometer measurements were taken on May 10, 1991, in 5 cm intervals to 60 cm at 33 locations on a transect perpendicular to the corn rows in each of four tillage treatments. The data permitted three-dimensional displays...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Impact penetrometer; Soil resistance; Hard clayey and gravelly soils; Spatial distribution.
Ano: 1998
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06831998000200003

Correction of resistance to penetration by pedofunctions and a reference soil water content
Provedor de dados: 90
Autores: Moraes,Moacir Tuzzin de; Debiasi,Henrique; Franchini,Julio Cezar; Silva,Vanderlei Rodrigues da.
The soil penetration resistance is an important indicator of soil compaction and is strongly influenced by soil water content. The objective of this study was to develop mathematical models to normalize soil penetration resistance (SPR), using a reference value of gravimetric soil water content (U). For this purpose, SPR was determined with an impact penetrometer, in an experiment on a Dystroferric Red Latossol (Rhodic Eutrudox), at six levels of soil compaction, induced by mechanical chiseling and additional compaction by the traffic of a harvester (four, eight, 10, and 20 passes); in addition to a control treatment under no-tillage, without chiseling or additional compaction. To broaden the range of U values, SPR was evaluated in different periods....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pedotransfer functions; Oxisol; Impact penetrometer; Soil compaction.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832012000600004