Consulta: subjectFacets:"Magnetized water"
Registros recuperados: 2
Data/hora: 01/06/2024 00:44:40

Water magnetization and phosphorus transport parameters in the soil
Provedor de dados: 91
Autores: Generoso,Tarcila N.; Martinez,Mauro A.; Rocha,Genelício C.; Hamakawa,Paulo J.
ABSTRACT There are scientific studies describing changes in properties of the water when subjected to the action of a magnetic field, which may favor the availability of some nutrients in the soil solution. Some nutrients, although they are essential to the process of crop development, can be sources of pollution for watercourses and soil. The aim of this study was to evaluate the effect of water magnetization on transport parameters of the phosphate ion in a Red Latosol (RL) and in a Quartzarenic Neosol (QN). Saturated leaching columns were connected to bottles containing KH2PO4 solutions. In RL, there were significant differences in phosphorus (P) transport parameters, related to the retardation factor (R) and distribution coefficient (Kd). For the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Magnetized water; Ion movement; Nutrient availability; Fertigation.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000100009

Effect of Magnetized Water on Water Use Efficiency, Yield and Nutritional Qualities of Watermelon under Deficit Irrigation
Provedor de dados: 111
Autores: Yusuf, Kamorudeen Olaniyi; Ogunbamowo, Tolulope Ruth; Obalowu, Rasheed Olarewaju.
Magnetized water (MW) is a non-chemical method and new technology for crop production. It is environmentally-friendly which improves water use efficiency (WUE) and enhances high crop yield. The study was conducted to determine the effect of MW on WUE, yield and nutritional qualities of watermelon under deficit irrigation in a garden shed. A Completely Randomized Design was used for the experimental layout. Irrigation water was treated using magnetic flux density of 319 gauss. Water applied as the treatments were 100%, 80%, 60% and 50% water requirement and each treatment was replicated four times. Watermelon seed (variety: Kaolack with LOT number: VG-PV-0519-KA) was planted in 15 litres/pot (285 mm diameter and 255 mm depth) with 16 pots for MW and 16 pots...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Magnetized water; Water use efficiency; Watermelon; Paired t-test.
Ano: 2020
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/5833