Consulta: subjectFacets:"Sensor."
Registros recuperados: 2
Data/hora: 01/06/2024 09:38:17

Sensores móveis e autônomos de temperatura de baixo custo.
Provedor de dados: 14
Autores: NERY, R. N.; LANDAU, E. C.; GUIMARAES, D. P.; SANTOS, A. H. dos; FERREIRA, R. V. M.
A verificação da temperatura foi iniciada no final do século XVI e até hoje continua evoluindo. Há várias aplicações para as medições de temperatura, mas seu registro automático nem sempre é possível. O registro de temperatura automático ainda pode representar um desafio, pois os equipamentos capazes de armazenar essas informações são caros, tornandose inatingíveis para grande parte da população. Neste trabalho, são aplicadas tecnologias livres, para desenvolvimento de um amostrador de temperatura autônomo utilizando sensores de baixo custo. A conexão entre os sensores e o armazenamento de dados se dá em um microcontrolador, difundido por também apresentar baixo custo e ser de hardware livre. Neste trabalho, foi desenvolvido e testado um amostrador...
Tipo: Documentos (INFOTECA-E)
Palavras-chave: Armazenamento de dados; Sensor.; Clima; Temperatura.
Ano: 2016
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1063417

Développement et essais d’un salinomètre optique pour l’océanographie
Provedor de dados: 5
Autores: Le Menn, Monique; Malardé, Damien; David, Arnaud; Brault, Patrice; Grosso, Philippe; De Bougrenet De La Tocnaye, Jean-louis; Le Reste, Serge; Podeur, Christian.
Salinity is the essential parameter for ocean dynamics studies. Its definition and using in the equations used to calculate the thermodynamic properties of seawater, were revised in 2010, opening the possibility of new sensors developments. In this context, NOSS (NKE Optical Salinity Sensor) has emerged as one of the first underwater instrument for in situ refractive index measurement in the past years open up the scope of possibilities to access to density parameter. This achievement is the fruit of the cooperation between several institutions and the fruit of several years of developments and trials. NOSS sensor is designed to be deployed in coastal environment and open-ocean waters up to 2000m, especially on profiling floats of the Argo network.
Tipo: Text
Palavras-chave: Salinity; Density; Ocean; Seawater; Refractive index; Sensor.
Ano: 2016
URL: https://archimer.ifremer.fr/doc/00664/77601/79616.pdf