Consulta: subjectFacets:"Sprinkler"
Registros recuperados: 3
Data/hora: 12/06/2024 00:42:41

Resposta da abobora hibrida tipo Tetsukabuto a diferentes laminas de agua e doses de nitrogenio.
Provedor de dados: 14
Autores: MAROUELLI, W. A.; PEREIRA, W.; SILVA, H. R.; SILVA, W. L. C.; SOUZA, A. F.
bitstream/item/103125/1/pa-26.pdf
Tipo: Séries anteriores (INFOTECA-E)
Palavras-chave: Hibrido Tetsukabuto; Lamina de agua; Brasilia; Distrito Federal; Brasil; Pumpkim; Hybrid; Sprinkler; Fertilization.; Adubação; Abóbora; Cucúrbita Máxima; Cucúrbita Moschata; Cerrado; Irrigação por Aspersão; Nitrogênio.; Brazil; Irrigation; Nitrogen.
Ano: 1999
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/766624

Artificial neural network model for simulation of water distribution in sprinkle irrigation
Provedor de dados: 91
Autores: Menezes,Paulo L. de; Azevedo,Carlos A. V. de; Eyng,Eduardo; Dantas Neto,José; Lima,Vera L. A. de.
ABSTRACTDetermining uniformity coefficients of sprinkle irrigation systems, in general, depends on field trials, which require time and financial resources. One alternative to reduce time and expense is the use of simulations. The objective of this study was to develop an artificial neural network (ANN) to simulate sprinkler precipitation, using the values ​​of operating pressure, wind speed, wind direction and sprinkler nozzle diameter as the input parameters. Field trials were performed with one sprinkler operating in a grid of 16 x 16, collectors with spacing of 1.5 m and different combinations of nozzles, pressures, and wind conditions. The ANN model showed good results in the simulation of precipitation, with Spearman's correlation coefficient (rs)...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sprinkler; Water distribution uniformity; Artificial intelligence; Computational model.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662015000900817

Influence of the wind on water application uniformity of a mechanical lateral move irrigation equipment using rotating plate sprinklers
Provedor de dados: 65
Autores: Faria,Lessandro Coll; Beskow,Samuel; Colombo,Alberto; Nörenberg,Bernardo Gomes; Rettore Neto,Osvaldo; Simões,Matheus Chagas.
ABSTRACT: Investigations demonstrate that the wind is the factor that causes the biggest negative influence on water application of sprinkler irrigation systems. Therefore, this paper aims to evaluate, in in-field conditions, the influence of wind on the water distribution uniformity of a mechanical lateral move sprinkler system used for irrigation in rice crop in the South of Rio Grande do Sul State, Brazil. The equipment is located at the Campo Experimental de Terras Baixas (ETB) of EMBRAPA/CPACT and operates with water emitters model I-Wob installed in drop tubes in a distance of 2.8m above the soil surface, having a uniform space of 2.3m between each other and pressure regulators of 68.9kPa. Sixteen in-field evaluations were done and they permitted to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigated rice; Sprinkler; In-field tests; Irrigation uniformity.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782016000100083