Consulta: subjectFacets:"Submersible chemical analyser"
Registros recuperados: 1
Data/hora: 09/06/2024 11:56:43

Impact of environmental factors on in situ determination of iron in seawater by flow injection analysis
Provedor de dados: 5
Autores: Laes, Agathe; Vuillemin, Renaud; Leilde, Bernard; Sarthou, Géraldine; Bournot Marec, Claudie; Blain, Stéphane.
A sensitive method for iron determination in seawater has been adapted on a submersible chemical analyser for in situ measurements. The technique is based on flow injection analysis (FIA) coupled with spectrophotometric detection. When direct injection of seawater was used, the detection limit was 1.6 nM, and the precision 7%, for a triplicate injection of a 4 nM standard. At low iron concentrations, on line preconcentration using a column filled with 8-hydroxyquinoline (8HQ) resin was used. The detection limit was 0.15 nM (time of preconcentration = 240 s), and the precision 6%, for a triplicate determination of a I nM standard, allowing the determination of Fe in most of the oceanic regimes, except the most depleted surface waters. The effect of...
Tipo: Text
Palavras-chave: Temperature and pressure effects; Submersible chemical analyser; Seawater; In situ measurements; Iron; Flow injection analysis.
Ano: 2005
URL: http://archimer.ifremer.fr/doc/2005/publication-1209.pdf