Consulta: country:"Brazil"
Registros recuperados: 148.874
Máximo de registros impressos: 2500
Data/hora: 05/06/2024 19:07:20

Azospirillum brasilense AND COMPOUND OF PHYTOHORMONES AS BIOSTIMULANTS IN JALO PRECOCE BEANS
Provedor de dados: 196
Autores: Moreira, Allisson Sousa; Contardi, Lucymara Merquides; Camilo, Lucas Jandrey; Andrade, Maria Gabriela Oliveira; Lima, Sebastião Ferreira; Vendruscolo, Eduardo Pradi; Simon, Cátia Aparecida.
Beans are one of the most important crops in Brazil but still have a low yield. The use of technologies such as the application of biostimulants can provide greater yield for the crop. Thus, the work aimed to evaluate the effect of using Azospirillum brasilense and phytohormones on Jalo Precoce beans. The experiment was carried out in randomized blocks with nine treatments and four replications. The treatments consisted of a control, Stimulate (compound of phytohormones), and A. brasilense applied isolated or associated to the seeds or in a furrow. The plant height, stem diameter, shoot dry matter, number of pods per plant, number of grains per pod, the weight of grains per pod, and 100-grain weight were favored by A. brasilense and compound of...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5974

CARBON, NITROGEN, AND ORGANIC MATTER OF SOIL IN AN INTEGRATED CROP-LIVESTOCK SYSTEM
Provedor de dados: 196
Autores: Mattei, Eloisa; Rabello de Oliveira, Paulo Sérgio; Rampim, Leandro; Rocha de Moraes Rego, Carlos Augusto; Piano, Jeferson Tiago; Carpiski Sampaio, Marinez.
This study aimed to evaluate the effect of the integrated crop-livestock system on the contents and stocks of total organic carbon, total nitrogen, and soil organic matter. The experiment was carried out between April 2016 and February 2017, in a randomized block design in a strip-block scheme, with additional control treatment (fallow) and four repetitions. The treatments consisted of two densities of oat sowing (40 and 60 kg ha-1) in strips A and different grazing frequencies (without grazing - WG, one grazing - 1G, and two grazing - 2G) in strips B, besides fallow as a control treatment. The determinations of the contents of total organic carbon (TOC), total nitrogen (TN), and organic matter (SOM) were carried out in the soil layers of 0-5, 5-10, and...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4526

ALLEVIATION OF SOIL SALINITY ON PHYSIOLOGICAL AND AGRONOMIC TRAITS OF RICE CULTIVARS USING Arbuscular mycorrhizal fungi AND Pseudomonas STRAINS UNDER FIELD CONDITIONS
Provedor de dados: 196
Autores: Norouzinia, Firouz; Ansari, Mohammad Hossein; Aminpanah, Hashem; Firozi, Saeed.
Rice cultivation in Iran has a special place and its cultivation area is about 640,000 ha. Soil salinization is one of the most factor in reducing of grain yields and cultivation of paddy rice. Currently, half of Iran's cultivated lands (9.5 million ha) are affected by salinity, which has a major impact on crop yields. For this purpose, an field experiment conducted with the use of microorganisms (Pseudomonas putida strain S34, Pseudomonas fluorescens strain R167, Arbuscular mycorrhizal fungi (AMF) (Rhizophagus irregularis), co-inoculation of P.putida + P.fluorescens + AMF, and a non-inoculated treatment as control) on two rice cultivars (Hashemi and Gilane) in saline and normal soil in north of Iran during the 2018 and 2019. The results showed...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4042

AVALIAÇÃO DE GENÓTIPOS DE MAMONA EM DIFERENTES NÍVEIS DE ADUBAÇÃO
Provedor de dados: 196
Autores: Pivetta, Laerte Gustavo; Zanotto, Maurício Dutra; Tomaz, Camila de Aquino; Pivetta, Laércio Augusto; Lara Fioreze, Ana Carolina da Costa; Zoz, Tiago.
O estudo teve como objetivo avaliar a resposta de híbridos do Programa de Melhoramento de Mamona da UNESP-FCA e de cultivares de mamona em diferentes níveis de adubação. O delineamento experimental utilizado foi de blocos ao acaso, em esquema fatorial 4x4, com quatro repetições. O primeiro fator correspondeu aos quatro genótipos de mamona (dois híbridos experimentais A e B e duas cultivares FCA-PB e IAC 2028) e o segundo fator correspondeu aos quatro níveis de adubação (0, 50, 100 e 150% da dose recomendada com base na análise de solo). A cultivar IAC 2028 apresentou o menor número de racemos, mas obteve maior número de grãos por racemo, massa de cem grãos e produtividade. O aumento da dose de adubo aumentou todos os componentes de produção e a...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/256

QUALIDADE FISIOLÓGICA E COMPOSIÇÃO QUÍMICA DE SEMENTES DE BRACHIARIA BRIZANTHA EM FUNÇÃO DO CONDICIONAMENTO OSMÓTICO
Provedor de dados: 196
Autores: Cardoso, Eliana Duarte; de Sá, Marco Eustáquio; Haga, Kuniko Iwamoto; Binotti, Flávio Ferreira da Silva; Costa, Edilson.
O condicionamento fisiológico em sementes tem se mostrado benéfico, entretanto há necessidade de estudos para cada espécie de interesse. Objetivou-se com este trabalho avaliar o efeito do condicionamento osmótico (CO) com diferentes soluções na qualidade fisiológica e composição química das sementes de Brachiaria brizantha cv. MG-5. O trabalho foi conduzido no Laboratório de Análises de Sementes da FEIS/UNESP, em 2009. Utilizou-se delineamento inteiramente casualizados e o estudo foi constituído por soluções mistas (1:1) formadas por PEG 8000 (potencial de -1,5 MPa a 25ºC) junto a soluções com nutrientes (KNO3 0,2%, Ca(NO3)2 0,2%), com reguladores de crescimento/bioestimulante (Citocinina – CIN 1,62 mg L-1, Giberelina - GA3 0,5 mg L-1, Auxina – IBA 0,5 mg...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fisiologia de Sementes.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/264

AGRICULTURA DE PRECISÃO: UM ALERTA À IMPRECISÃO – ESTUDO DE CASO NA CAFEICULTURA
Provedor de dados: 196
Autores: Almeida, Leandro da Silva; Guimarães, Ednaldo Carvalho.
O objetivo deste trabalho foi avaliar a discrepância existente entre mapas gerados a partir da utilização da configuração padrão fornecidos por softwares de agricultura de precisão (default) comparando com os mapas nos quais se realiza criteriosamente os procedimentos necessários para o ajuste dos mapas. Para estudo foi utilizado o programa Gamma Design Software (GS+®) versão 7.0. O experimento foi conduzido em propriedade cafeeira que possui 65 ha de cafeeiro arábica (Coffea arabica L.), cultivado em um Latossolo Vermelho Distrófico (LVd), localizada no município de Araguari-MG. Foi utilizada uma malha não sistemática de um ponto para cada hectare. Os dados a principio foram submetidos, a análise fatorial exploratória, gerando três fatores. Os fatores...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1469

DENSIDADE DE PLANTIO E SUBSTÂNCIAS HÚMICAS NO CULTIVO DO TOMATEIRO (Solanum lycopersicum L.)
Provedor de dados: 196
Autores: Benetti, Rafael; Benett, Katiane Santiago Silva; Arruda, Natália; Benett, Cleiton Gredson Sabin; Seleguini, Alexsander.
O tomate é uma das hortaliças tipo fruto mais populares do Brasil. Desta forma, torna-se de suma importância realizar pesquisas para garantir produtividade e frutos de alta qualidade. Objetivo do trabalho foi avaliar diferentes doses de ácidos húmicos e fúlvicos sobre o crescimento e produtividade do tomateiro cultivado com diferentes densidades de plantio. O experimento foi realizado na fazenda da Universidade Estadual de Goiás (UEG), Campus de Ipameri. Foi adotado os espaçamentos de 0,30 e 0,50 m entre plantas, correspondendo, respectivamente, às populações de 33.333 e 20.000 plantas ha-1; com as diferentes doses (0, 20, 40, 60 e 80 L ha-1) de ácidos húmicos e fúlvicos. O delineamento experimental utilizado foi de blocos casualizados em esquema fatorial...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2136

GROWTH AND DEVELOPMENT OF BELL PEPPER CROP IRRIGATED WITH MAGNETICALLY-TREATED WATER
Provedor de dados: 196
Autores: Lorenzoni, Marcelo Zolin; Rezende, Roberto; Souza, Alvaro Henrique Cândido de; Seron, Cassio de Castro; Gonçalves, Antônio Carlos Andrade; Saath, Reni.
This study aimed to evaluate the benefits of irrigation with magnetically-treated water and replacement depths based on ETc, in plant growth and development of bell pepper grown in a protected environment in two cultivation seasons. The experiment was carried out in a protected environment, in the Centro Técnico de Irrigação (CTI), at Universidade Estadual de Maringá (UEM), in Maringá - PR. Two experiments were performed: summer (2017-2018) and winter-spring (2018). The experimental design adopted was randomized blocks in factorial scheme 3 x 2 (six treatments) with four replications in the summer season and 2 x 2 (four treatments) with six replications in the winter-spring season. The first factor consisted of water replacement depths (50, 75 and 100% of...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4173

Aplicação foliar de doses de bioestimulante em duas épocas na cultura do feijoeiro
Provedor de dados: 196
Autores: Lopes, Wytalo Oliveira; Varão, Lorenna Correia; Buso, Wilian Henrique Diniz.
Salinity is one of the environmental stresses that most affects plants' vital processes, especially germination. Brassinosteroids, including 24-epibrassinolide (EBL), have multiple actions in essential processes in plants. Thus, this research's objective was to evaluate the effects of EBL on tomato seeds' physiological conditioning on germination, growth, and production of dry seedling mass under salinity conditions. The experiment was carried out in a 2x5 factorial scheme, as follows: two concentrations of EBL (0 and 10-6 M) and five levels of salinity (0.5 control; 1.5; 3.0; 4.5 and 6.0 dS m-1), consisting of ten treatments, with four replications of 50 seeds. In isolation, the salt stress reduced the percentage of germination and germination speed index...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus vulgaris; Biostimulant; Phytohormones; Phaseolus vulgaris; Bioestimulante; Fitohormônios.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6981

CHEMICAL PROPERTIES AND PHYSICAL FRACTIONS OF ORGANIC MATTER IN OXISOLS UNDER INTEGRATED AGRICULTURAL PRODUCTION SYSTEMS
Provedor de dados: 196
Autores: de Moraes Rego, Carlos Augusto Rocha; Oliveira, Paulo Sérgio Rabello de; Piano, Jeferson Tiago; Egewarth, Jonas Francisco; Egewarth, Vanessa Aline; López de Herrera, Juan; Gonçalves Junior, Affonso Celso.
The main cause of decreased soil fertility and soil organic matter content is intensive crop farming with inadequate management. This study aimed to evaluate soil chemical properties, total organic carbon content, physical granulometric fractions (particulate organic carbon and mineral-associated organic carbon), carbon stocks, and carbon management indices of oxisols in different integrated agricultural production systems (IAPSs) with reference to values in a haymaking area and native forest. The experiments were performed using completely randomized design, considering nine differently managed areas, including seven IAPSs and two reference areas (haymaking area and native forest); four soil samples from the 0.00-0.05, 0.05-0.10, and 0.10-0.20 m layers...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4747

BIQUINHO PEPPER CULTIVATED ON THE REFLECTIVE BENCH IN PROTECTED ENVIRONMENTS
Provedor de dados: 196
Autores: Moreira, Loryelle de Jesus; Mello, Bruna Finotti Fonseca Reis de; Silva, Abimael Gomes; Costa, Edilson; Binotti, Flávio Ferreira da Silva; Vieira, Gustavo Haralampidou da Costa.
The choice of the cultivation environment interferes with the whole vegetable development because of the micro-meteorological conditions in which the plants are cultivated, and the use of technologies with reflective material aims to complement the production in both quantity and quality. In this sense, the objective was to analyze the growth and productivity of Biquinho pepper (Capsicum chinese) plants cultivated in two types of protected environments and benches with reflective material. The experiment was conducted in a completely randomized design, with five repetitions. A plastic greenhouse with 42% shading and agricultural screen with 30% shading, inside these environments, there were benches with and without reflective material of the type Aluminet®...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5921

CONTROL OF WEEDS IN THE JAPANESE PUMPKIN HYBRIDS
Provedor de dados: 196
Autores: Guerra, Antonia Mirian Nogueira de Moura; Silva, Maria Gabriela Magalhães; Evangelista, Régila Santos; Santos, Edeilton Borges dos; Rodrigues, Ítalo José da Silva.
The Japanese pumpkin known as "Tetsukabuto" is the result of crossing selected lines of squash. Squashes are highly susceptible to weed interference due to slow initial growth, requiring more considerable attention as to their control. Studies focusing on the losses caused by weeds to Japanese pumpkin hybrids are scarce. Thus, this study aimed to evaluate the influence of weed control on the fruit yield of Japanese pumpkin hybrid cultivars. A randomized block design with four replications in a 3x4 factorial scheme was used. Three cultivars (Corina F1, Triunfo F1, and Takayama F1) and four weed control periods, without weed control, weed control from 0 to 30 and from 0 to 60 days after transplanting (DAT), and weed control throughout the crop cycle...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4290

DESEMPENHO PRODUTIVO E QUALIDADE DE CULTIVARES DE RÚCULA EM SISTEMA SEMI-HIDROPÔNICO
Provedor de dados: 196
Autores: Jardina, Lucimara Lima; Cordeiro, Carlos Alberto Martins; Silva, Marcelo Cléon de Castro; Sanches, Alex Guimarães; Araújo Júnior, Pedro Vitorino de.
O sistema semi-hidropônico é uma alternativa para a produção de hortaliças; combina substrato inerte e solução nutritiva, requer menor quantidade de água e funciona por nível, não há uso de energia elétrica. Nesse contexto, objetivou-se avaliar o desempenho produtivo e a qualidade de cultivares de rúcula em sistema semi-hidropônico. A pesquisa foi desenvolvida em hidroponia comercial localizada no município de Altamira-PA, no período de dezembro de 2014 a fevereiro de 2015. As cultivares avaliadas foram: Apreciatta, Cultivada, Donatella, Gigante e Rococó. Aos 28 dias após o transplante foram avaliados a altura das plantas, número de folhas, massa fresca das raízes e produtividade; a qualidade foi determinada mediante análises de pH, sólidos solúveis totais...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1399

INFESTAÇÃO DE PLANTAS DANINHAS DE DIFÍCIL CONTROLE EM FUNÇÃO DE ANOS DE CONSÓRCIO MILHO-BRAQUIÁRIA
Provedor de dados: 196
Autores: Mechi, Ivan Arcanjo; Santos, Anna Luiza Farias dos; Ribeiro, Luan Marlon; Ceccon, Gessí.
Objetivou-se com esse trabalho avaliar a infestação de plantas daninhas após cinco anos de cultivo com milho solteiro ou consorciado com Brachiaria ruziziensis no outono-inverno. Os tratamentos foram estabelecidos em áreas com diferentes períodos de consórcio (milho+braquiária) e cultivos do milho solteiro entre 2011 a 2015, sendo milho solteiro de 2011 a 2015, consórcio em 2011 + milho solteiro de 2012 a 2015, consórcio em 2011 e 2012 + milho solteiro de 2013 a 2015, consórcio de 2011 a 2013 + milho solteiro em 2014 e 2015, consórcio de 2011 a 2014 + milho solteiro em 2015, consórcio de 2011 a 2015, milho solteiro em 2011 + consórcio de 2012 a 2015, milho solteiro em 2011 e 2012 + consórcio de 2013 a 2015, milho solteiro de 2011 a 2013 + consórcio em 2014...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1642

INFLUENCE OF COVERAGE BASED ON BIOPOLYMERS ON THE MATURATION OF CAGAITA (Eugenia dysenterica DC.)
Provedor de dados: 196
Autores: Braz, Aline Jordane; Nascente, Letícia de Paula; Corrêa, Nayara Canedo; Rocha, Rodrigo de Almeida; Barbosa de Souza, Eli Regina; Siqueira, Ana Paula Silva.
The cagaita is a native fruit of the cerrado, of high perishability, and for postharvest conservation of the fresh fruit, methods are used to increase its life cycle. In the present study, edible coatings are used, a technique that aims to control the loss of mass through transpiration reduces gas exchange, increases the shelf-life, improves the appearance, preserves the structural integrity and mechanical properties. The study aims to evaluate the influence of coatings based on biopolymers on the maturation of cagaita during storage. The factorial scheme 3 x 4 was used, with three treatments - without coating, polysaccharide coating and protein coating, four evaluation points - with an interval of 2 days, stored at 25 ºC. The fruits were submitted to...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3334

REARING DENSITY IN THE PERFORMANCE AND PROFITABILITY OF ROSS 308 BROILERS
Provedor de dados: 196
Autores: Silva, Higor Jonathan de Oliveira; Souza, Andréia Fróes Galuci Oliveira de; Garcia, Elis Regina de Moraes; Leite, Meiby Carneiro de Paula; Cassuci, Leticia Gabriela Talhaferro; Domingues, Elyan Carlos da Silva; Marques, Ana Letícia Ribeiro; Santos, João Paulo Gomes dos; Costa, Gabriela da Silva da; Machado, Dayane Camargo; Silva, Maria Vitória.
The objective was to evaluate the effect of stocking density on productive performance, carcass characteristics, productivity, bone development, and profitability of Ross 308 broilers. A completely randomized experimental design with four stocking densities (10, 12, 14, and 16 birds m-2) and four replicates, and the subplots the bone collection ages (7, 14, 21, 28, 35, and 42 days old). The variables analyzed were live weight at 21 and 42 days, weight gain, feed intake, and conversion in the accumulated periods from 1 to 21 and 1 to 42 days. Weights of carcasses, commercial cuts, edible viscera, abdominal fat, productivity, production efficiency index, viability, and profitability were evaluated. The length, thickness, weight, and Seedor index of long...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5856

ALTERNATIVES FOR SPRING FORAGE EMPTINESS IN PAMPA, BRAZIL
Provedor de dados: 196
Autores: Malaguez, Edgard Gonçalves; Dinarte, Gabriella Valduga; Tadielo, Leonardo Ereno; Dos Santos, Nathaly Lopes Toledo; Castagnara, Deise Dalazen.
The spring forage emptiness is an obstacle to the development of Brazilian livestock, including in the Bioma Pampa region. Feed strategies for this period contributed to the development of livestock and to the conservation of the biome. The objective of this work was to know the nutritional potential of forages during spring forage for use as strategies in the forage planning. The experiment had a completely randomized design, with ten forages and four replicates. The chemical composition, in vitro dry matter digestibility (IVDMD) and the total digestible nutrient content (NTD) of elephant grass, brachiaria cultivars Convert and Marandu, Tifton 68; diploid and tetraploid ryegrass; red, white and arrowleaf clover; and bird’s-foot trefoil. The grasses had a...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1590

EFFECTS OF METHYL JASMONATE AND CADMIUM ON GROWTH TRAITS, CADMIUM TRANSPORT AND ACCUMULATION, AND ALLENE-OXIDE CYCLASE GENE EXPRESSION IN WHEAT SEEDLINGS
Provedor de dados: 196
Autores: Alikhani, Ozra; Abbaspour, Hossein.
 This research investigated the toxicity effects of cadmium chloride (0, 100, 200 and 300 μM) and its interactive effects with methyl jasmonate (MeJA) (0, 0.01 and 0.1 mM) on growth parameters, cadmium (Cd) accumulation, and Allene-Oxide Cyclase (AOC) gene expression in wheat seedling (Sivand cultivar). According to the results, Cd at concentrations of 200 μM and 300 μM reduced the growth traits of the wheat. Under exposure to 300 μM Cd, root and shoot cadmium content was 30 and 17 times greater than the base level, respectively. Under 100 μM Cd exposures, bioaccumulation factor (BCF) for root and shoot increased by 46 and 25 times respectively. The spraying of MeJA on Cd-stressed plants showed a positive effect on growth parameters, increasing them by...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3322

QUALITY OF CAMBUCI PEPPER SEEDLINGS IN RESPONSE TO THE APPLICATION OF NUTRIENT SOLUTIONS
Provedor de dados: 196
Autores: Nordi, Nicholas Taborda; Aires, Eduardo Santana; Alves, Thatiane Nepomuceno; Perisato, Samara Moreira; Cardoso, Antonio Ismael Inácio.
One of the main stages in the production system of a crop is the production of quality seedlings since it influences the plants' final performance in the field and their production. The study aimed to evaluate different nutrient solutions in the production of Cambuci pepper seedlings. The design used was a complete randomized design, with six treatments corresponding to the nutrient solutions proposed for the pepper crop by Castellane and Araújo, Claudio Roberto, Hoagland, and Arnon, besides the commercial products Plenan® and Biobokashi®, and a control treatment without fertilization, with six replications. The final evaluation was carried out 45 days after sowing. The following variables were analyzed: stem diameter, plant height, leaf dry matter, shoot...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4880

SUBSTRATE VOLUMES AND APPLICATION OF PACLOBUTRAZOL FOR ORNAMENTAL PEPPER PRODUCTION
Provedor de dados: 196
Autores: Parladore, Naine; Silva, Abimael Gomes da; Costa, Edilson; Binotti, Flávio Ferreira da Silva; Silva, Laura Araújo; Vieira, Gustavo Haralampidou da Costa; Souza, Andreia Froes Galuci Oliveiva de.
The objective was to evaluate the quality of ornamental pepper seedlings, cultivar Pyramid, in different substrate volumes, with foliar application of paclobutrazol (PBZ).The experiment was carried out at the Mato Grosso do Sul State University - UEMS, in Cassilândia - MS. The experimental design was completely randomized, in a 2 x 2 factorial scheme (growth container x foliar application of PBZ) with four replicates of 36 seedlings each. Plastic trays (cells with a volume of 50 mL) and polystyrene trays (Isopor®, 100 mL cells) were used as containers. The treatments were: polystyrene tray with PBZ application; polystyrene tray without PBZ application; plastic tray with PBZ application and plastic tray without the application of PBZ. Plant height, root...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3342

INITIAL DEVELOPMENT OF COFFEE SEEDLINGS IN THE PRESENCE OF PLANT EXTRACTS
Provedor de dados: 196
Autores: Costa, Bruna Penha; Duarte Júnior, José Barbosa; Rinaldi, Luanna Karoline; de Moraes Rego, Carlos Augusto Rocha; Stangarlin, José Renato.
The coffee plant can grow together with different plants, but the presence of allelochemicals can affect the crop post-planting. This study aimed to evaluate the early growth of coffee seedlings following treatment with plant extracts from different botanical families. The experimental design used randomized blocks with four trials, in a 7 × 2 factorial scheme; the first factor consisted of aqueous extracts from six species: canola, crotalaria, brachiaria, sunflower, wheat, and lupine; water was used as the control. The second factor comprised of different botanical parts of the aforementioned six species of plant. The extracts were diluted to 5% concentration and were applied at a dose of 20 mL per plant. The agronomic variables analyzed were plant height...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4500

EMERGÊNCIA DE PICÃO-PRETO EM DIFERENTES PROFUNDIDADES DE SEMEADURA E DIFERENTES AMBIENTES
Provedor de dados: 196
Autores: de Sousa Almeida, André Cirilo; de Oliveira, Fernando Castro; Netto, Maurilio de Sousa; Vieira, Bruna do Carmo; Sabin Benett, Cleiton Gredson.
Entender a dinâmica da semente de planta daninha em função da profundidade é fundamental para promover atividade de controle. O objetivo deste trabalho foi avaliar a emergência de sementes de picão-preto submetidas a diferentes profundidades de semeadura, em dois ambientes. O delineamento experimental empregado foi o de blocos casualizados, em esquema fatorial 2 x 5, com quatro repetições. Os tratamentos foram constituídos de dois ambientes (condições de campo e ambiente controlado) e cinco profundidades de semeadura (0, 2, 4, 6 e 8 cm). As sementes foram semeadas em vasos plásticos com capacidade de 5 L preenchidos com um Latossolo Vermelho, sendo semeadas 20 sementes por vaso. Avaliou-se o índice de velocidade de emergência e a porcentagem de emergência...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantas Daninhas.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/250

INTERFERÊNCIA DE CULTURAS ANUAIS NO CRESCIMENTO INICIAL DE Brachiaria ruziziensis
Provedor de dados: 196
Autores: Ribeiro, Luan Marlon; Leite, Ericksson Martins; Ceccon, Gessí.
Objetivou-se avaliar o crescimento inicial da B. ruziziensis consorciada com espécies anuais. O experimento foi conduzido na Embrapa Agropecuária Oeste, em Dourados-MS. Em 18/05/2014 semeou-se a B. ruziziensis solteira e consorciada com aveia branca, trigo, canola, girassol, crambe e Crotalaria ochroleuca, com seis plantas por vaso; e milheto, feijão-caupi, feijão-comum, sorgo sacarino e milho com quatro plantas por vaso, contendo 30 kg de solo seco. O arranjo experimental foi em esquema fatorial 2x12 (Solos (argiloso e arenoso) e Culturas), em blocos casualizados, com três repetições. Aos 55 dias após a semeadura das culturas avaliou-se o crescimento, massa seca de plantas, número de perfilho e altura da braquiária; área foliar e massa seca das culturas...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2077

MANEJO COM INSETICIDAS VISANDO O CONTROLE DE PERCEVEJO MARROM NA SOJA INTACTA
Provedor de dados: 196
Autores: Ribeiro, Francisco de Carvalho; Rocha, Francileia de Sousa; Lemus Erasmo, Eduardo Andrea; de Matos, Edilson Pereira; da Costa, Sergio José.
Ao longo dos anos, verificaram-se grandes mudanças no sistema de produção de soja no Brasil. O percevejo marrom (Euschistus heros) é uma praga‑chave da cultura de soja. É a espécie mais abundante do complexo de percevejos apresentando-se em predominância no estado do Tocantins e em grande parte das regiões dos cerrados produtoras de soja. Objetivou-se com esse trabalho avaliar a eficiência de diferentes inseticidas utilizados no manejo de Euschistus heros na cultura da soja intacta. O experimento foi conduzido no ano agrícola 2014/2015 em condições de campo na Fazenda Pedrinha, situada no município de Porto Nacional – TO. O delineamento experimental foi de blocos casualizados, constituído de seis tratamentos com quatro repetições. Realizou-se amostragens...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1132

DENSIDADE POPULACIONAL DO NEMATOIDES-DAS-LESÕES-RADICULARES EM CANA-DE-AÇÚCAR EM FUNÇÃO DE CULTIVARES, MANEJO DO PALHIÇO E ESCARIFICAÇÃO DO SOLO
Provedor de dados: 196
Autores: Barbosa, Gabrielle Regina Miguel; Asmus, Guilherme Lafourcade.
A expansão do setor sucroalcooleiro suscitou preocupação quanto a questões que afetam a produtividade, tais como a presença de fitonematoides e as práticas de manejo cultural. O objetivo deste trabalho foi analisar a comunidade de nematoides do gênero Pratylenchus em cultivares de cana-de-açúcar plantados em solo submetido ou não à escarificação e ao aleiramento do palhiço residual da colheita. Foi conduzido experimento de campo em duas áreas, com e sem escarificação, nas quais foram plantadas 15 cultivares de cana-de-açúcar em subparcelas com e sem aleiramento do palhiço sobre as linhas de plantio. Anualmente, foram quantificados os nematoides do gênero Pratylenchus, no solo e nas raízes das plantas. Houve diferenças na densidade populacional do...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2715

AGRONOMIC PERFORMANCE AND PHYSIOLOGICAL QUALITY OF PEPPER SEEDS UNDER DIFFERENT PLANTING SYSTEM
Provedor de dados: 196
Autores: Beloti, Igor Forigo; Nunes Rodrigues de Azevedo, Breno; Maciel, Gabriel Mascarenhas; Peres, Hugo Gabriel; Pivetta Momesso, Mauricio; Alves, Igor Matheus.
The pepper crop is cultivated in all Brazilian regions,and the planting system with the arrangement of plants in the single-row prevails. Therefore, this work aimed to evaluate the agronomic performance and physiological quality of the seeds of different pepper genotypes according to the planting systems. The experiment was carried out at the Federal University of Uberlândia, in Monte Carmelo, in a randomized blocks experimental design, in a 4 x 2 factorial scheme, four genotypes (UFU-62-5M; UFU-28-1M; UFU-58-6D and UFU-5-3BD) under two planting systems (Single-row planting - SRP and Double-row planting - DRP), with four repetitions. The spacing of 0.6 m between plants and rows was used in the SRP. In the DRP, the spacing of 0.6 m between rows and 1.20 m...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3432

CARACTERIZAÇÃO MICROMETEOROLÓGICA DE AMBIENTES PROTEGIDOS PARA A PRODUÇÃO VEGETAL
Provedor de dados: 196
Autores: Silva, Abimael Gomes da; Costa, Edilson; Zoz, Tiago; Binotti, Flávio Ferreira da Silva.
This study evaluates the influence of the four seasons and twelve months of the year on the micrometeorological variables of global solar radiation, air temperature, and relative air humidity in different protected environments for plant production. The protected environment types and the characteristics of the shade screen modify the indoor air temperature. This environment provides greater relative humidity. The global solar radiation percentages in the environments were: full sun (100%); black screen with 30% shading (47.3%); greenhouse with LDPE + 22-30% shading screen under the film (38.1%); aluminized screen with 35% shading (36.9%) and greenhouse with LDPE + 42-50% shading screen under the film (26.9%). The micrometeorological conditions of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solar radiation; Temperature; Relative humidity; Radiação solar; Temperatura; Umidade Relativa.
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6177

Características agronômicas e produtivas de diferentes híbridos de milho no norte goiano
Provedor de dados: 196
Autores: Borges Silva, Luciana; Diniz Buso, Wilian Henrique.
Objetivou-se com a pesquisa avaliar os caracteres agronômicos e produtivos de híbridos de milho em dois locais. O delineamento experimental utilizado foi de blocos casualizados em esquema fatorial 11x2 (11 híbridos e dois locais) com quatro repetições. Cada parcela foi constituída por quatro linhas de cinco metros. As avaliações ocorreram nas duas linhas deixando 0,50 m de bordadura nas extremidades. As variáveis analisadas foram: altura de planta, altura da primeira espiga, diâmetro da espiga, número de fileira de grãos, número de grãos por fileira, comprimento da espiga, massa de mil grãos e produtividade. Os híbridos de milho se adaptaram melhor no município de Santa Isabel. Em relação a produtividade, no município de Santa Isabel os híbridos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays Genotype by environment interaction Yield Zea mays; Genótipo x Ambiente; Produtividade.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6849

FENOLOGIA DE QUALEA PARVIFLORA MART. (VOCHYSIACEAE) EM UM REMANESCENTE DE CERRADO SENSU STRICTO
Provedor de dados: 196
Autores: Ferreira, Kleyton Rezende; Fina, Bruna Gardenal; Rêgo, Norton Hayd; da Rui, Ricardo Fernando; Kusano, Daniel Makoto.
O objetivo desse estudo foi avaliar as fenofases vegetativas (queda de folhas e brotamento) e reprodutivas (floração e frutificação) de dezoito indivíduos de Q. parviflora localizados em uma área de cerrado sensu stricto na fazenda da Universidade Estadual de Mato Grosso do Sul, no município de Aquidauana, MS. As observações foram realizadas quinzenalmente, no período de agosto de 2010 a julho de 2012. Para o cálculo das porcentagens de cada fenofase seguimos a metodologia proposta por Fournier (1974). Utilizamos a correlação de Spearman (P&amp;lt;0,05) para verificar relação entre variáveis climáticas e as fenofases da espécie. A população mostrou elevada sincronia dentro de cada fenofase e apresentou um padrão fenológico sazonal. O brotamento teve...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1534

INIBIÇÃO DO CRESCIMENTO MICELIAL DE FUSARIUM SOLANI F. SP. GLYCINES COM O USO DE ÓLEOS ESSENCIAIS
Provedor de dados: 196
Autores: Nascimento, Daniele Maria; Vieira, Gustavo Haralampidou da Costa; Kronka, Adriana Zanin.
A síndrome da morte súbita da soja tem causado sérios problemas na cultura. Objetivou-se avaliar o efeito dos óleos essenciais de copaíba, nim, manjericão, menta e palma rosa no crescimento micelial de Fusarium solani f. sp. glycines, agente causal desta doença. Foram testadas quatro concentrações dos óleos essenciais, 4000, 6000, 8000 e 1000 µL/L de meio BDA (batata-dextrose-ágar). Discos miceliais de 3 mm de diâmetro foram inoculados no centro das placas de Petri contendo o meio BDA com os tratamentos, medindo se o crescimento micelial sete dias após a incubação das placas. Com exceção dos óleos essenciais de nim e copaíba, os demais inibiram completamente o desenvolvimento micelial. Esses resultados demonstram o potencial antifúngico destes óleos...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1195

EMBALAGEM E TRATAMENTO HIDROTÉRMICO NA MANUTENÇÃO DA QUALIDADE PÓS-COLHEITA DE JAMBU
Provedor de dados: 196
Autores: Oliveira, Olganeth Moreira de; Menezes, Keren Railka Paiva; Santos, Guilherme Celestino de Souza; Sanches, Alex Guimarães; Cordeiro, Carlos Alberto Martins.
O jambu também conhecido como agrião bravo e jambu pequeno é uma hortaliça folhosa que apresenta elevada perecibilidade após a colheita, observada pela rápida deterioração e intensa perda de água. Desta forma, o presente trabalho tem por objetivo avaliar a conservação pós-colheita do jambu pelo uso do hidroresfriamento e do acondicionamento em diferentes embalagens. O experimento foi conduzido em um delineamento experimental inteiramente casualizado em arranjo fatorial 5x5, sendo cinco tratamentos e cinco tempos de armazenamento com quatro repetições. A unidade experimental foi formada por amostras de 50 g. Houve efeito significativo ao nível de 1% e 5% pelo teste F para todas as variáveis avaliadas tanto na interação entre os fatores dias de armazenamento...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1611

RADIAÇÃO UV-C SOB A QUALIDADE PÓS-COLHEITA DE JABUTICABA
Provedor de dados: 196
Autores: Evangelista, Zeuxis Rosa; Campos, André José de; Silva, Danilo Corrêa; Araújo, Kari Katiele Souza; Campos, Luiz Fernandes Cardoso.
O objetivo desse trabalho foi avaliar o efeito do tempo de exposição da radiação UV-C, na qualidade pós-colheita da jabuticaba ‘Sabará’. O delineamento experimental foi inteiramente casualizado, com arranjo fatorial 5x5, sendo: tempo de exposição à UV-C (0, 2, 4, 6 e 8 minutos) x dias de análise (0, 2, 4, 6 e 8 dias de armazenamento), em três repetições. Após aplicação dos tratamentos, os frutos foram acondicionados em embalagens de polipropileno e armazenados a 12º C, com 85-90% de UR. Foram avaliados perda de massa fresca, conservação pós-colheita, firmeza, sólidos solúveis, acidez titulável e pH. A utilização da radiação UV-C não interferiu positivamente na conservação da jabuticaba ‘Sabará’.
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2222

COINOCULAÇÃO DE Bradyrhizobium japonicum e Azospirillum brasilense EM SEMENTES DE AMENDOIM DE DIFERENTES TAMANHOS
Provedor de dados: 196
Autores: Silva, Elijanara Raissa da; Salles, Josiane Souza; Zuffo, Alan Mario; Steiner, Fábio.
O tamanho da semente é um importante indicador físico da qualidade fisiológica das sementes, pois pode afetar a taxa de germinação e o crescimento inicial das plântulas. Neste contexto, o presente estudo teve como objetivo avaliar os efeitos do tamanho das sementes e da inoculação de Bradyrhizobium japonicum e Azospirillum brasilense de forma isolada ou combinada na emergência das plântulas, nodulação das raízes e no crescimento inicial das plantas de amendoim (Arachis hypogaea L., cv. IAC Tatu ST). As plantas foram cultivadas em vasos plásticos de 8,0 L preenchidos com um solo arenoso do Cerrado e mantidas sob condições de casa-de-vegetação. O delineamento experimental utilizado foi o de blocos ao acaso em esquema fatorial 3 × 4 com quatro repetições. Os...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2192

ENERGY CULTURES AND SUSTAINABILITY IN BIOFUEL PRODUCTION
Provedor de dados: 196
Autores: Mascarenhas Santos, Maria do Socorro; Silva, Cesar José da; Cruz, Sandra Helena da; Batistote, Margareth; Cardoso, Claudia Andrea Lima.
Energy cultures are emerging as viable renewable energy sources because they satisfy sustainability requirements. The present study involves a survey regarding the technological characteristics for sugarcane and sweet sorghum energy crops, in addition to their potential for bioethanol production. An exploratory survey was conducted regarding the agronomic and technological characteristics of cane and sorghum. Pre-inmates were produced with YPSAC 5% liquid medium, sterilized and 0.10 grams of yeasts FT858 and Pedra-2 were inoculated and incubated at 30 °C for 10 h at 250 rpm. After the production, the cells were recovered by centrifugation, at 105 rpm, resulting in a 10 mg mg-1 concentration of moist dough. This dough was subsequently inoculated in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biomass; Saccharomyces cerevisiae; Bioethanol.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6719

UTILIZAÇÃO DE RADIAÇÃO GAMA E AMIDO DE MILHO NO ARMAZENAMENTO PÓS-COLHEITA DAS FOLHAS DE COUVE MANTEIGA
Provedor de dados: 196
Autores: Sanches, Alex Guimarães; Costa, Jaqueline Macedo; Silva, Maryelle Barros da; Moreira, Elaine Gleice Silva.
Devido à alta perecibilidade apresentada pelas folhas de couve-manteiga após a colheita, o presente trabalho teve por objetivo avaliar o efeito isolado e combinado da radiação gama e amido de milho visando o prolongamento de sua vida útil. O delineamento experimental utilizado foi o inteiramente casualizado em esquema fatorial 4 x 9 com cinco repetições e os parâmetros teor de clorofila, atividade das enzimas POD e PPO, sólidos solúveis, pH, acidez titulável, perda de massa fresca, murchamento, sabor e qualidade geral foram avaliados a cada dois dias. De acordo com os resultados observou-se interação significativa a nível de 5% de probabilidade pelo teste F em todos os parâmetros avaliados. A utilização do amido de milho na forma isolada apresentou...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1186

INITIAL DEVELOPMENT OF CORN SUBJECTED TO INCREASING NITROGEN DOSES
Provedor de dados: 196
Autores: Neto, Dhiego César Oliveira Riva; Barros, Leonardo Rodrigues; Sousa, Vinicius Silva; Brasil, Eliana Paula Fernandes; Ribon, Adriana Aparecida; Smaniotto, Alex Oliveira.
Corn (Zea mays L.) is one of the most important cereals grown and consumed in the world not only for its economic value but also due to its importance in human and animal nutrition. This study aimed to assess the initial development of corn as a function of increasing nitrogen doses. The study was carried out in a greenhouse on the Sipal Farm, Confresa, MT, Brazil. The experiment was set up in a completely randomized design, consisting of five treatments (0, 100, 200, 300, and 400 mg N dm−3 soil), with four replications, conducted from April to June 2020. Four seeds of the hybrid K 9606 VIP 3 were sown per 8-L polyethylene pot. The plants were thinned at 7 days after emergence (DAE), leaving only one plant per pot. Morphological components were assessed. A...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5226

HIDRATAÇÃO CONTROLADA DE SEMENTES DE SOJA: POTENCIAL FISIOLÓGICO E EMERGÊNCIA EM SOLO COM RHIZOCTONIA SOLANI
Provedor de dados: 196
Autores: Costa, Denis Santiago da; Rocha, Cartiane Rubishirley de Macedo; Yagushi, Juliana Tieme; Menten, José Otávio Machado; Cruz, Ananias Alves.
A hidratação controlada é uma técnica que favorece a germinação rápida e uniforme diminuindo o tempo de contato entre fungos responsáveis pelo tombamento de plântulas e os tecidos suscetíveis. Assim, objetivou-se avaliar diferentes métodos de hidratação controlada de sementes de soja, seus efeitos sobre o potencial fisiológico das sementes e sobre emergência em solo infestado por Rhizoctonia solani. Três lotes de sementes de soja do cultivar BRS 232 foram avaliados e classificados quanto à germinação e ao vigor e, em seguida, submetidas à procedimentos de hidratação controlada (controle, entre papéis com água destilada, entre papéis com água destilada com PEG 6000 e por imersão direta em solução aquosa de PEG 6000). A eficiência dos tratamentos foi...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1363

Azospirillum brasilense INTERACTION EFFECTS WITH CAPTAN AND THIODICARB ON THE INITIAL GROWTH OF CORN PLANTS
Provedor de dados: 196
Autores: Vogel, Gabriel Felipe; Fey, Rubens.
The application of biological products containing diazotrophic bacteria in the seed has been highlighted as an alternative to reduce the use of nitrogen fertilizers; however, the chemical treatment of the seeds may negatively affect the survival rate of these microorganisms in the soil. The effects of the application of captan (fungicide) and thiodicarb (insecticide) in association with the inoculation of Azospirillum brasilense were investigated in this study for the corn crop. The research was conducted under greenhouse conditions at Universidade Estadual do Centro-Oeste (UNICENTRO), in Guarapuava, Paraná, Brazil, and under laboratory conditions at the Universidade Federal da Fronteira Sul (UFFS), in Laranjeiras do Sul, Paraná, Brazil. A completely...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3133

HYDRATION LEVELS ON CONIDIAL PRODUCTION OF Metarhizium rileyi (Ascomycota) IN SOLID GROWING MEDIUM
Provedor de dados: 196
Autores: Loureiro, Elisângela de Souza; Pessoa, Luis Gustavo Amorim; Dias, Pamella Mingotti; Ribeiro, Muller De Paula; Tosta, Ricardo Alexandre De Souza; Teodoro, Paulo Eduardo.
This study aimed to evaluate the conidial production of Metarhizium rileyi in rice with different water volumes. The bioassay was composed by completely randomized design (CRD), with four treatments (20, 30, 40 and 50 mL of distilled water), being added 100 g of rice thin and long, making a total of 10 plastic bags per treatment, which were autoclaved for 15 minutes at 1.0 atm pressure, to 120 ºC. After the cooling of the rice, were added in each plastic bag, 2.0 mL of suspension containing 1 × 108 conidia mL-1. Then the bags were incubated for ten days in a germination chamber (BOD type) at 25 °C (±1 °C), 80% (±10%) relative humidity and 12h photoperiod to promote conidial germination and growth of the fungus, being performed a mild agitation every two...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2899

EFEITO DO SEXO SOBRE DESEMPENHO PRODUTIVO E CARACTERÍSTICAS DE CARCAÇA DE FRANGOS DE CORTE
Provedor de dados: 196
Autores: Fernandes de Freitas Gottardi, Camila Priscila; Fróes Galuci Oliveira, Andréia; Ricardo Queiroz de Souza, Aurélio; Reis Ferreira, Bruno; Silva Ferreira, Thales; Pereira Abaker, João Eduardo.
Objetivou-se com o presente estudo avaliar o efeito do sexo sobre o desempenho produtivo e características de carcaça de uma linhagem comercial de frangos de corte, em região de clima quente. Foram utilizados 360 pintinhos de um dia, da linhagem comercial Cobb 500®, distribuídos em delineamento experimental inteiramente casualizado, com três tratamentos (macho, fêmea e misto) e quatro repetições. Para o desempenho, avaliou-se o peso vivo, consumo de ração, ganho de peso e conversão alimentar nos períodos de 1-7, 1-14, 1-21, 1-28, 1-35 e 1-42 dias, e para as características de carcaça avaliou-se o peso e rendimento de carcaça, peso e rendimento de cortes comerciais e de miúdos comestíveis e peso da gordura abdominal aos 42 dias. Para o período de 1-42 dias,...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1738

DESEMPENHO AGRONÔMICO DE HÍBRIDOS DE MILHO EM TRÊS ÉPOCAS DE SEMEADURA NO CERRADO GOIANO
Provedor de dados: 196
Autores: Buso, Wilian Henrique Diniz; Silva, Luciana Borges e; Silva, Sandra Máscimo da Costa e; Leão Junior, Laidson Alves.
Avaliou-se o desempenho agronômico de híbridos de milho em três épocas de semeadura no município de Ceres-GO. O experimento foi desenvolvido na Fazenda Experimental do IF Goiano Campus Ceres. O delineamento experimental foi o de blocos completos casualizados em esquema fatorial 10x3, dez híbridos de milho (Truck, Fórmula, P30F53, P3646H, P30F35H, AGN 30A91H, AGN 30A37H, AG 8088VTPRO, DKB 390 e DKB bi 9438) semeados em três épocas (30/11/2011, 01/02/2012 e 20/02/2012), com três repetições. Os híbridos que apresentaram maior número de fileira de grãos foram Truck, Formula, P30F35H, AG8088PRO. Para altura de planta e da primeira espiga e o diâmetro do colmo houve diferença estatística nas épocas de semeadura. O híbrido DKB Bi 9438 diferiu estatisticamente dos...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1826

COMPORTAMENTO REOLÓGICO DE NÉCTAR DE CAGAITA DESCRITO PELO MODELO LEI DE POTÊNCIA
Provedor de dados: 196
Autores: Oliveira, Fernando Luiz; de Oliveira, Camila Fernanda Dias; Pinto, Ellen Godinho.
Neste trabalho, foi determinado o comportamento reológico do néctar de cagaita sob a pasteurização lenta e rápida mediante um reômetro, nos intervalos de temperatura de 5, 15 e 25°C. Foi realizado o ajuste pelo modelo Lei de Potência, o modelo se demonstrou adequado para descrever o comportamento reológico do néctar de cagaita. O néctar de cagaita sob os dois tipos de pasteurização demonstrou comportamento não newtoniano e demostrando característica de fluido pseudoplástico. Os índices de comportamento de consistência decresceram com o aumento da temperatura
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1202

DINÂMICA POPULACIONAL DE Bemisia Tabaci  BIÓTIPO B (GENNADIUS, 1889) EM CULTIVARES DE SOJA TRANSGÊNICA
Provedor de dados: 196
Autores: da Silva Oliveira, Carlos Eduardo; Flóride Carneiro, Danilo Emanuel; Toscano, Luciana Cláudia; Ferreira dos Santos, Renan Marcelo.
A ocorrência de pragas é apontada como um dos principais fatores que causam perdas de produtividade na cultura da soja. A mosca-branca Bemisia tabaci biótipo B tem preocupado os sojicultores da região Centro-Oeste devido aos diversos danos causados. Com o uso cada vez maior de plantas com tecnologia Bt sendo implantadas nessas áreas, ainda são escassos estudos do impacto dessa tecnologia em pragas não-alvo. Objetivou-se, neste trabalho, avaliar a dinâmica populacional de B. tabaci biótipo B, em diferentes cultivares de soja transgênica e relacioná-las com cultivares de soja convencional, verificando o impacto do uso da tecnologia Bt sobre a sua população. O experimento foi realizado em blocos ao acaso, com quatro tratamentos e cinco repetições. Os...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1425

CULTIVO DE SOJA SOB DIFERENTES DENSIDADES DE SEMEADURA E ARRANJOS ESPACIAIS
Provedor de dados: 196
Autores: Cruz, Simério Carlos Silva; Sena Junior, Darly Geraldo; Aires dos Santos, Danilo Marcelo; Lunezzo, Leandro Oliveira; Machado, Carla Gomes.
A produtividade é definida pela interação entre a planta, ambiente e manejo. Dentre as práticas de manejo destacam-se a densidade de semeadura e o espaçamento entrelinhas. Objetivou-se com este trabalho avaliar o efeito de densidades e arranjos de plantas no desenvolvimento vegetativo e produtividade de grãos de soja. O delineamento experimental foi de blocos casualizados com quatro repetições em esquema de parcelas subdivididas. Nas parcelas foram alocados dois arranjos espaciais: convencional (45 cm entre fileiras) e fileira duplas (65 cm entre uma fileira dupla e outra e 25 cm entre as linhas dentro da fileira dupla). Nas subparcelas foram alocadas cinco densidades de semeadura (7, 10, 15, 19 e 22 sementes m-1). Cada subparcela foi composta por oito...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/431

Qualidade da pimenta-do-reino produzida no nordeste do Pará
Provedor de dados: 196
Autores: Nunes Pinto Paracampo, Nádia Elígia; Figueiredo Abreu, Laura; Filgueira de Lemos, Oriel; Castanheira Lima Both, João Paulo.
Black pepper (Piper nigrum L.) is the most widely used spice in the world. This crop has great economic importance in Brazil, especially in the North and Southeast regions. However, the variability in quality between cultivars is high. The objective of this study was to characterize black pepper from northeastern Pará available on the market and obtain an overview of its quality parameters. A total of 23 samples from black pepper cultivars/clones were evaluated for impurities and foreign matter, empty grains, density, moisture and ether extract, as established by Brazilian legislation. Additionally, the contents of total ash, protein, crude fiber and piperine were determined. Among the samples, one was outside the standard for density. The moisture...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Piper nigrum L.; Physical characterization Chemical characterization Piperine Piper nigrum L. Caracterização física Caracterização química Piperina.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/7020

DESEMPENHO AGRONÔMICO DA COUVE-FLOR (Brassica oleracea var. botrytis) EM FUNÇÃO DA ADUBAÇÃO SILICATADA
Provedor de dados: 196
Autores: Curvelo, Carmen Rosa da Silva; Fernandes, Érika Faleiro; Diniz, Layane Hyasmin Bernardes; Pereira, Alexandre Igor de Azevedo.
A couve-flor (Brassica oleracea var botrytis) está entre as hortaliças mais cultivadas e consumidas no Brasil, sendo uma das principais brássicas cultivadas. Dessa forma, objetivou-se avaliar os efeitos da adubação silicatada na qualidade e rendimento pós-colheita da couve-flor cultivar Sharon. O delineamento experimental adotado foi em blocos casualizados (DBC), com quatro tratamentos e sete repetições. Foram utilizadas oito mudas por parcela, com o critério de plantio uniformidade de tamanho. Os tratamentos corresponderam às seguintes doses de silício: 0 mg L-1 (T1), 20,0 mg L-1 (T2), 30,0 mg L-1 (T3) e 40,0 mg L-1 (T4). Os parâmetros avaliados foram: número de folhas (NF), comprimento e diâmetro do caule (cm), diâmetro da inflorescência (cm), massa da...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2556

1–METILCICLOPROPENO NA MANUTENÇÃO DA QUALIDADE PÓS-COLHEITA DE TAPEREBÁ (SPONDIA MOMBIN L.)
Provedor de dados: 196
Autores: Sanches, Alex Guimarães; Silva, Maryelle Barros da; Moreira, Elaine Gleice Silva; Costa, Jaqueline Macedo.
A vida útil pós-colheita do taperebá é muito curta mesmo em condições de refrigeração, assim o presente trabalho tem por objetivo avaliar a influência de diferentes concentrações de 1–metilciclopropeno (MCP) sobre a conservação e preservação da qualidade deste fruto visando maior tempo de comercialização na forma in natura. Adotou-se um delineamento experimental inteiramente casualizado em arranjo fatorial 4x5 com cinco repetições. A cada três dias os frutos de cada tratamento foram avaliados quanto à perda de massa fresca, firmeza da polpa, pH, o conteúdo de sólidos solúveis, teor de vitamina C, acidez titulável, índice de maturação e taxa respiratória. Os resultados demonstraram efeito significativo em todas as características avaliadas tanto no tempo de...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1398

PRIMEIRO REGISTRO DE Psyllaephagus bliteus PARASITANDO Glycaspis brimblecombei EM CHAPADÃO DO SUL, MS
Provedor de dados: 196
Autores: Vieira, Ricardo De Lima; Pessoa, Luis Gustavo Amorim; Costa, Valmir Antônio; Loureiro, Elisângela De Souza; Poersch, Nerison Luís.
Psyllaephagus bliteus Riek, 1962 (Hymenoptera: Encyrtidae) é uma vespa de origem australiana que parasita ninfas de Glycaspis brimblecombei Moore, 1964 (Hemiptera: Psyllidae). No Brasil, a presença de ambos foi registrada pela primeira vez no Estado de São Paulo em 2003 e, posteriormente, sua ocorrência foi registrada nos estados do Paraná, Goiás, Minas Gerais, Santa Catarina, Rio Grande do Sul e Mato Grosso. No manejo dessa praga, P. bliteus é uma das formas mais promissoras de controle biológico clássico, uma vez que G. brimblecombei tem causando danos significativos na produção florestal. A ocorrência destes insetos na região nordeste de Mato Grosso do Sul foi constatada no Município de Chapadão do Sul, em povoamento de Eucalyptus camaldulensis,...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2538

CORRELAÇÃO DOS COMPONENTES VEGETATIVOS DA CULTURA DA PUPUNHA E DOS ATRIBUTOS QUÍMICOS DO SOLO
Provedor de dados: 196
Autores: Montanari, Rafael; Lima, Elizeu de Souza; Lovera, Lenon Henrique; Ferrari, Samuel; Queiroz, Hernandes Andrade.
A pupunha (Bactris gasipaes) tem se mostrado uma excelente opção econômica para os produtores rurais, pois sua produção de palmito permite precocidade de corte, rusticidade, perfilhamento abundante, boa palatabilidade, ausência de oxidação do palmito, alta produtividade e facilidade nos tratos culturais. Objetivou-se selecionar, entre os atributos do solo pesquisado, aquele com a melhor correlação, linear e espacial, para explicar a variabilidade da planta da pupunha. O experimento foi conduzido na fazenda de pesquisa e extensão da Faculdade de Engenharia de Registro (SP), foi avaliada a variabilidade espacial dos componentes vegetativos da pupunha e dos atributos químicos de um Cambissolo Eutrófico. Uma malha contendo 54 pontos foi georreferenciada de...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/857

PRODUTIVIDADE DE CULTIVARES DE SORGO SACARINO EM DIFERENTES ÉPOCAS DE SEMEADURA E TIPOS DE SOLO
Provedor de dados: 196
Autores: Ceccon, Gessi; Makino, Priscila Akemi; Alves, Valdecir Batista; Fachinelli, Ricardo; da Luz, Renato Albuquerque.
Objetivou-se avaliar o desempenho agronômico de cultivares de sorgo sacarino (BRS 506, BRS 508, BRS 509 e BRS 511), em diferentes épocas de semeadura (dezembro, janeiro, fevereiro, março e abril) e distintos tipos de solo (arenoso e argiloso). O experimento foi realizado em casa telada com cobertura de vidro. Utilizou-se o delineamento inteiramente casualizado, em esquema fatorial 4x5x2, com três repetições. Na fase de “grão leitoso” foram avaliados a altura da planta, diâmetro de colmo, produção de biomassa, oBrix, volume de calda e massa seca da rebrota dos cultivares. Os cultivares semeados nos meses de dezembro e janeiro, independentemente do tipo de solo, apresentaram maior produção de biomassa e açúcares totais.  Nas semeaduras realizadas em março e...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1729

EXOGENOUS APPLICATION OF VITAMINS IN UPLAND RICE
Provedor de dados: 196
Autores: Vendruscolo, Eduardo Pradi; Rodrigues, Aliny Heloísa Alcântara; Oliveira, Paulo Ricardo; Leitão, Rodrigo Andrade; Campos, Luiz Fernandes Cardoso; Seleguini, Alexander; de Lima, Sebastião Ferreira.
Vitamin application can optimize plant growth and grain yield of rice crop due to its beneficial effect on many plant physiological characteristics. The present study was conducted to evaluate the effects of niacin and thiamin applied as seed soaking or foliar spray on the morphological and productive characteristics of upland rice crop (Oryza sativa L., cv. Primavera), grown under greenhouse conditions. The experiment was arranged in a randomized block design in a 4 x 2 factorial scheme, with four replicates. The treatments consisted of the application of vitamins (control; 200 mg L-1 thiamin; 200 mg L-1 niacin; and 100 mg L-1 thiamin + 100 mg L-1 niacin) and two application methods (seed soaking and foliar spraying). Morphological and productive...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3241

MORPHOLOGICAL ANALYSIS AND ACCUMULATION OF NUTRIENTS IN Peltophorum dubium (Spreng.) Taub. SEEDLINGS PRODUCED IN ORGANIC SUBSTRATES WITH DIFFERENT PROPORTIONS
Provedor de dados: 196
Autores: Melo Nunes Astolfi, Angelica Christina; da Silva Mota, Lucas Junior; Pontes, Montcharles da Silva; Clemente, Leyzinara Zenteno; Santiago, Etenaldo Felipe; de Carvalho, Laércio Alves; Motta, Ivo de Sá.
Environmental conservation and regeneration actions must consider plant species that add value by restoring structural and functional aspects of the ecosystem. The forest species, Peltophorum dubium, has several characteristics that make its use viable in projects of restoration of degraded areas, making it necessary to study the species' responses to different cultivation environments. Thus, 500 seeds were selected and sown in vermicompost substrates prepared with different proportions of cattle rumen content (CR) and sugarcane bagasse (SB) (V1 - 60% CR x 40% SB / V2 - 50% CR x 50 % SB / V3 - 40% CR x 60% SB / V4 - 70% CR x 30% SB) and in an commercial substrate (Plantmax®). At 79 days after sowing, 20 seedlings per treatment were removed; they were...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4093

MATURAÇÃO DE GRAVIOLAS APÓS ARMAZENAMENTO EM ATMOSFERA CONTROLADA
Provedor de dados: 196
Autores: Sanches, Alex Guimarães; Silva, Maryelle Barros da; Moreira, Elaine Gleice Silva; Costa, Jaqueline Macedo; Cordeiro, Carlos Alberto Martins.
Por se tratar de um fruto climatérico a graviola apresenta vida útil relativamente curta principalmente pela perda de firmeza provocada pelo amadurecimento comprometendo assim sua expansão para mercados distantes. Diante disso, o presente trabalho tem por objetivo avaliar o efeito de diferentes condições de atmosfera controlada no prolongamento da vida útil deste fruto. O delineamento experimental adotado foi inteiramente casualizado em arranjo fatorial 5x3 sendo cinco variações de gás carbônico (CO2) sob atmosfera controlada e três tempos de armazenamento após a saída das câmaras, com cinco repetições e a parcela experimental composta por dois frutos. Após quinze dias em atmosfera controlada e mais oito dias em temperatura ambiente avaliou-se: coloração...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1101

PRODUÇÃO DE MUDAS DE MARACUJÁ AMARELO COM DIFERENTES MATERIAIS REFLETORES SOBRE BANCADA
Provedor de dados: 196
Autores: Santos, Tiago Vilela; Lopes, Thamíris Campaneli; Silva, Abimael Gomes; de Paula, Rita de Cássia Mariano; Costa, Edilson; Binotti, Flávio Ferreira da Silva.
O maracujá amarelo (Passiflora edulis Sims. f. flavicarpa Deg) é uma das espécies frutíferas mais cultivadas no Brasil, mais vigorosa e mais adaptada aos dias quentes. Objetivou-se avaliar a utilização de diferentes materiais refletores em bancadas de cultivo, visando melhor aproveitamento da luz no interior do ambiente protegido, para obtenção de mudas de maracujazeiro vigorosas e de elevada qualidade. O experimento foi conduzido em delineamento inteiramente casualizado, com 5 tratamentos e 6 repetições. Foram testados os seguintes tratamentos: T1: testemunha (bancada metálica de cor cinza, sem material refletor); T2: bancada metálica coberta com papel alumínio; T3: bancada metálica coberta com tecido “falso paetê”; T4: bancada metálica coberta com...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1781

QUALIDADE FISIOLÓGICA DE SEMENTES DE SOJA ESVERDEADAS EM DIFERENTES TAMANHOS
Provedor de dados: 196
Autores: Pardo, Fábio Faustini; Binotti, Flávio Ferreira da Silva; Cardoso, Eliana Duarte; Costa, Edilson.
O tamanho da semente e o estágio de maturação podem influenciar a qualidade fisiológica das sementes. O objetivo foi avaliar a influência da semente esverdeada e tamanho das sementes na qualidade fisiológica de sementes de soja. O presente trabalho foi desenvolvido na Universidade Estadual do Mato Grosso do Sul na Unidade Universitária de Cassilândia, localizada no município de Cassilândia – MS. O delineamento experimental foi inteiramente casualizado em esquema fatorial 2x2, constituído por tamanhos (peneiras 5,75 mm e 6,5 mm) e tipos de sementes (normais e esverdeadas), com cinco repetições cada. Realizaram-se avaliações de vigor e germinação. Sementes de soja esverdeadas apresentam menor potencial fisiológico e na mesma quanto menor o tamanho menor será...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/275

PLANT PHYSIOLOGICAL PERFORMANCE AND SEED CHEMICAL COMPOSITION OF SOYBEAN UNDER DIFFERENT SPATIAL ARRANGEMENT
Provedor de dados: 196
Autores: Nobre, Danubia Aparecida Costa; Silva, Rodrigo Rocha; Guimarães Nasser, Vinicius; Silva, Geraldo Humberto; Aquino, Leonardo Angelo; Macedo, Willian.
Poucos estudos apresentam interações entre a fisiologia das plantas e sua posterior composição química, quando cultivadas em diferentes arranjos. Esta pesquisa buscou compreender a relação entre o espaço de cultivo da soja e sua influência sobre a qualidade da semente. Foram estudadas duas cultivares de soja (Tec 7849 Ipro e Monsoy 6972 Ipro) em quatro arranjos espaciais distintos (50,0 x 7,1; 40,0 x 8,9; 30,0 x 11,9 e 18,9 x 18,9 ou 16,2 x 16,2 cm, respectivamente). Durante os estádios fenológicos V4 e R2, foram analisadas trocas gasosas e na colheita, foram constituídos 2 grupos, um de sementes frescas e outro de sementes envelhecidas, para ambos os grupos se analisaram: teste de germinação, vigor, índice de velocidade de germinação, massa fresca das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gas exchange; Germination; Lipids; Gas chromatography; Trocas gasosas; Germinação; Lipídeos; Cromatografia gasosa.
Ano: 2023
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6850

CONSÓRCIO GUANDU-MILHO-BRAQUIÁRIA PARA INTEGRAÇÃO LAVOURA-PECUÁRIA
Provedor de dados: 196
Autores: Guimarães, Frederico da Silva; Ciappina, Angelina Luzia; Anjos, Rosane Angélica Reis dos; da Silva, Alex; Pelá, Adilson.
A Integração Lavoura-Pecuária (ILP) é uma alternativa para melhor exploração da terra durante o ano. Uma possível melhoria para este sistema é a inserção do feijão guandu anão (Cajanus cajan) visando o aumento no teor de proteína da pastagem durante o período de seca. O presente trabalho objetivou analisar a produtividade de biomassa de milho para silagem (Zea mays) em consórcio com braquiária (Urochloa ruziziensis) e diferentes densidades de feijão guandu. O delineamento experimental foi em blocos casualizados com sete tratamentos e quatro repetições, sendo eles: milho + braquiária + cinco densidades de feijão guandu (50 mil, 100 mil, 150 mil, 200 mil e 300 mil plantas por hectare), milho + braquiária e milho solteiro. A maior produtividade de massa seca...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2218

INSECT RICHNESS IN DUNG PATCHES OF CATTLE RAISED IN TWO LIVESTOCK SYSTEMS
Provedor de dados: 196
Autores: Gusmão, Marcos Rafael; Oliveira, Marcia Cristina de Sena; Nicodemo, Maria Luiza Franceschi; Pezzopane, Jose Ricardo Macedo.
The negative impact of livestock breeding on the environment has been mitigated through the combination of pastures and trees, characterizing the silvopastoral systems (SPS), an alternative to conventional pasture systems (CPS). The SPS provides environmental services, particularly the recovery of degraded areas and carbon sequestration. Furthermore, the complexity of the SPS can improve other environmental services, for example, enhance biodiversity and reduce pests through biological control. However, it is not clear the relationship between microclimate, pasture, trees, cattle, and invertebrate present in this environment. The purpose of this research was to characterize the macrofauna and determine the richness and abundance of invertebrates associated...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4033

REFLECTIVE MATERIALS AND SEEDS FROM DIFFERENT PLANT POSITIONS FOR PRODUCTION OF ACHACHAIRU SEEDLINGS
Provedor de dados: 196
Autores: Silva, Bruna Luzia Barbosa da; Souza, Vitória Cristina Di Matheus e; Costa, Edilson; Silva, Abimael Gomes; Binotti, Flavio Ferreira da Silva; Cavalcante, Daniele Ferreira; Benett, Cleiton Gredson Sabin; Zoz, Tiago.
The plant environment in the production of Achachairu (Garcinia humilis) seedlings aims to obtain quality plants for orchards' formation. The present study aimed to evaluate reflective materials on benches and fruit seeds harvested from different plant positions to produce Achachairu seedlings. The reflective materials used under the cultivation benches were aluminum foil, "fake sequin" fabric, mirror, and tetra pak®. The fruit collection positions in the plants were at the top, median and bottom. The largest seedlings were obtained on the bench with reflective material of Tetra Pak®; however, in this material, there was a greater relationship between the height and diameter of the seedlings' neck, which is not desired for quality seedlings. The largest...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5709

CULTURE MEDIA EVALUATION ON THE Leucoagaricus gongylophorus AND Escovopsis sp. FUNGI DEVELOPMENT
Provedor de dados: 196
Autores: Sousa, Maria Lucidalva Ribeiro de; Nogueira, Janaína da Costa; Freitas, Adriana Dantas Gonzaga.
This study aimed to evaluate the in vitro interference of different culture media, Czapek Dox Agar, Nutrient Agar, Starch Casein agar, Malt Extract Broth Base, Nutrient Broth, and the medium containing Peptone, Malt, Agar and crushed peach palm pulp (Bactris gasipaes) and tucumã (Astrocaryum aculeatum) on the fungus Leucoagaricus gongylophorus and the parasitic fungus Escovopsis sp. growth. The fungi were inoculated in different culture media and then kept in acclimatized chambers at 28 ºC in the dark for 42 days, being analyzed at weekly intervals, totaling six evaluations. Fungal colonies were evaluated considering the factor "f" (cm), obtained from the product between the width (W) and length (L) of the diameter of the colonies (f = W x L). The results...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5869

APLICAÇÃO DE ACYBENZOLAR-S-METHYL EM ALGODOEIRO PARA CONTROLE DE Aphis gossypii (GLOVER) E Ramularia areola (ATKINSON)
Provedor de dados: 196
Autores: Martins, Gustavo Luís Mamoré; Tomquelski, Germison Vital; Papa, Geraldo.
O acibenzolar-S-methyl funciona como um ativador na resistência das plantas contra pragas e doenças. O objetivo do trabalho foi avaliar a atividade de acybenzolar-S-methyl sobre Aphis gossypii (Glover) e Ramularia areola (Atkinson) em algodoeiro. O experimento foi conduzido no município de Selvíria, MS. O delineamento experimental foi de blocos casualizados no esquema de parcelas subdivididas (2x6), constituídos pela combinação de duas cultivares de algodão (Acala-90 e DeltaOpal) e seis indutores de resistência. Os tratamentos foram: 1) testemunha; 2) acybenzolar-s-methyl (20 g i.a. ha-1); 3) acybenzolar-s-methyl + azoxystrobin (20 + 40 g i.a. ha-1); 4) acybenzolar-s-methyl + tiofanato metílico (20 + 350 g i.a. ha-1); 5) azoxystrobin (40 g i.a. ha-1) e 6)...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fitossanidade.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/245

NITROGEN FERTILIZATION OF PAIAGUÁS GRASS: PRODUCTION AND NUTRITION
Provedor de dados: 196
Autores: Domingues, Alexandre Alves; Santos, Alessandro José Marques; Backes, Clarice; Rodrigues, Lucas Matheus; Teodoro, Arthur Gabriel; Bessa, Stephanie Vicente; Ribon, Adriana Aparecida; Giongo, Pedro Rogério; Godoy, Leandro José Grava de; Resende, Cinthya Cristina Fernandes de.
Nitrogen (N) is a nutrient associated with the development of plant shoots, which makes it a vitally important element for the maintenance and sustainability of pasture. The goal of this study was to evaluate the effects of nitrogen fertilization on the productive and nutritional traits of Urochloa brizantha Paiaguás, as well as the efficiency of digital imaging and the use of a chlorophyll meter in obtaining green color indices. The experiment was conducted in the field on the Escola farm at the State University of Goiás, located in São Luís de Montes Belos, GO. A randomized-block design with five treatments and four replicates was adopted. Treatments consisted of four N rates (0, 75, 150, 300, and 600 kg ha‒1) in the form of ammonium sulfate. The grass...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5918

PRODUTIVIDADE E QUALIDADE DE FRUTOS DE VIDEIRA 'ISABEL' EM FUNÇÃO DAS DOSES DE ETEFON E ÉPOCAS DE PODA
Provedor de dados: 196
Autores: Abreu, Camila Meira; Campos, Luiz Fernandes Cardoso; Ascheri, Diego Palmiro Ramirez; Seleguini, Alexsander.
A videira em região tropical necessita de cuidados diferenciados, quando comparada às regiões de clima temperado, principalmente em relação ao manejo da copa. Objetivou-se com este trabalho avaliar a produtividade e a qualidade dos frutos, influenciados por diferentes épocas de poda aliadas a doses de Ethephon, em duas safras da videira Isabel. O delineamento foi inteiramente casualizado, com dezesseis tratamentos no esquema fatorial 4 x 4, com quatro repetições. O primeiro fator foi composto pelas épocas de poda: na safra de inverno (08/março, 22/março, 05/abril e 19/abril de 2013); na safra de verão (25/agosto, 08/setembro, 22/setembro e 06/outubro de 2013). O segundo fator consistiu em quatro concentrações de Ethephon (0, 720, 1440, 2160 mg i.a. L-1)....
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1170

APLICAÇÃO DE FILMES BIODEGRADÁVEIS DE PROTEÍNAS DO SORO DE LEITE
Provedor de dados: 196
Autores: Soares, Dayana Silva Batista; Silva, Estéfani Alves do Nascimento; de Oliveira, Taysa Martins.
A embalagem tem como função principal manter a integridade do produto, protegendo-o contra danos mecânicos, perda e ganho de umidade. A maior parte das embalagens é fabricada com materiais não biodegradáveis e de fonte não renovável promovendo grande impacto ambiental. Já os filmes biodegradáveis vêm surgindo como alternativa viável a este problema. Os filmes biodegradáveis não apresentam a mesma resistência apresentada pelos filmes sintéticos logo, muitos tratamentos estão sendo aplicados aos filmes na tentativa de melhorar as propriedades mecânicas. Assim, foram desenvolvidos a partir do concentrado proteico de soro do leite aplicando duas variações de tratamento de pH: 5,5 e 8,5 no método de casting. Para a avaliação da embalagem avaliou-se espessura,...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1196

DESEMPENHO DE TRÊS TRATORES AGRÍCOLAS EM ENSAIOS DE TRAÇÃO
Provedor de dados: 196
Autores: Fiorese, Diego Augusto; Marasca, Indiamara; Fernandes, Bárbara Barreto; Sandi, Jefferson; Morelli-Ferreira, Francielle; Lanças, Kléber Pereira.
A avaliação de desempenho de tratores agrícolas, levando-se em consideração a condição do solo, é importante para identificar a máxima capacidade de tração e o consumo de combustível de acordo com os níveis de esforços exigidos. Neste sentido, o objetivo do trabalho foi realizar ensaios de tração para determinação do desempenho de tratores agrícolas sobre pista de solo firme sem cobertura vegetal. Foram avaliados três modelos de tratores 4x2 TDA, e seis níveis de esforços (força de tração) na barra de tração (5, 10, 15, 20, 25 e 27 kN). Para o fator trator, as médias foram comparadas pelo teste de Tukey, e para o fator força de tração, as médias foram ajustadas por equações de regressão. Observou-se que o menor desempenho energético representado pelo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Máquinas e mecanização agrícola.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/258

TETRAZOLIUM AND INTERACTION OF TEMPERATURE AND LIGHT UNDER SEED GERMINATION IN Ormosia arborea (FABACEAE)
Provedor de dados: 196
Autores: Silva, Aparecida Leonir da; Carlos, Halisson César Vinci; Rivaben, Rodrigo Cyrino; Silva, Laércio Junio; Dias, Denise Cunha Fernandes dos Santos; Morais, Glaucia Almeida de; Lima, Liana Baptista de.
The study aimed to define the best conditions to conduct germination tests for Ormosia arborea seeds and assess the viability of seeds using the tetrazolium test. The germination tests were conducted at temperatures of 10, 15, 20, 25, 30, and 35 °C and alternating temperatures of 20-30 °C, in the presence or absence of light. For the tetrazolium test, seeds were immersed in tetrazolium solution 0.075%, at 35 °C for three hours, and then the viability was evaluated. It was verified that the seeds did not present absolute photosensitivity. The tetrazolium test was effective in separating the seeds into two categories concerning seed viability, viable and nonviable. It was concluded that O. arborea seeds germinate in the presence or absence of light in a wide...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5206

DESENVOLVIMENTO DA CULTURA DO MILHO SOB EFEITOS DE DIFERENTES PROFUNDIDADES DE COMPACTAÇÃO DO SOLO
Provedor de dados: 196
Autores: Labegalini, Nayara Spricigo; Buchelt, Antonio Carlos; Andrade, Lurian; Oliveira, Samieli Camargo de; Campos, Luana Marques.
A compactação do solo determina, de certa maneira, as relações entre ar, água e temperatura, e estas influenciam praticamente em todas as fases do desenvolvimento vegetal. Nesse sentido, o objetivo do trabalho foi avaliar o efeito de diferentes profundidades de compactação, no desenvolvimento da cultura do milho. O delineamento experimental utilizado foi o de blocos inteiramente casualizados, com cinco tratamentos (0, 25, 50, 75 e 100% de compactação) e quatro repetições totalizando 20 unidades experimentais. Essas unidades experimentais foram representadas por vasos de polipropileno com 18 cm de altura e volume de 6,7 dm3. As características avaliadas foram: Altura de plantas, massa verde da parte aérea, massa seca da parte aérea, massa verde de raízes...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1102

GERMINAÇÃO E EMERGÊNCIA DE SEMENTES DE MILHO DE DIFERENTES TAMANHOS SUBMETIDAS À TRATAMENTOS QUÍMICOS
Provedor de dados: 196
Autores: Bulegon, Lucas Guilherme; Castagnara, Deise Dalazen; Tsutsumi, Claudio Yuji; Erig, Marcos Cristiano; Zoz, Tiago.
Com o atual sistema de cultivo intensivo cresce a necessidade de práticas culturais que possibilitem uma emergência e um desenvolvimento inicial adequado de plântulas. Assim, no presente trabalho objetivou-se estudar os efeitos de diferentes tratamentos de sementes sobre diferentes peneiras na germinação e emergência de plântulas de milho. O delineamento experimental utilizado foi em blocos casualizados em esquema fatorial 2 x 4, com dois tamanhos das sementes (C2 e R3) e quatro tratamentos das sementes: testemunha; tratamento com tiametoxam; tiametoxam + fertilizante misto; tiametoxam + fertilizante misto + carbendazim + thiram, e quatro repetições. Avaliou-se a germinação e vigor de sementes. Uma menor germinação de sementes foi encontrada quando...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/263

CHANGES IN LAND USE IN MATO GROSSO DO SUL
Provedor de dados: 196
Autores: Lamas, Fernando Mendes; Richetti, Alceu.
Among the species cultivated in Mato Grosso do Sul, the area with soybeans is larger than that only for pasture cultivation. This work was developed in fourteen municipalities of the state. Based on information from the Brazilian Institute of Geography and Statistics (IBGE), the evolution of the area occupied by soybean, pasture and sugarcane in these municipalities was analysed. In particular, the area cultivated with soybeans has shown constant and significant growth. On the other hand, the pasture area has been continuously decreasing, especially in Ponta Porã, Maracaju and Rio Brilhante. The areas previously occupied with pastures are giving way to soy and sugarcane cultivation.
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3827

THERMAL VARIATION FOR GROWTH OF ZOOSPORES OF Albugo spp.
Provedor de dados: 196
Autores: Fonseca, Rafaela Souza Alves; Neves, Paula Rodrigues; Lemes, Natanael Marcos; Decloquement, Jennifer; Lima, Milton Luiz da Paz.
The objective of this work was to identify the time of the thermal shock that promotes the greater release of zoospores/sporangia. The experiments were carried out with five treatments, varying the thermal variation time (20', 30', 40', 50' and 60') of sporangia suspension of 7.105 sporangia mL-1 under 5 °C temperature. The incidence of sporangia germinated by 20 times whose It was evaluated100 units at random, using an optical microscope at 40 times magnification. The F and Tukey test were used to compare the means. The sexual phase (presence of oospores) was identified in the isolate derived from purslane. In purslane leaves (infected by Albugo portulacae) the time of 20-30' promoted a greater number of zoospores released, whereas for the isolate from...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1634

DENDROMETRIC CHARACTERISTICS AND BASIC WOOD DENSITY OF EUCALYPTUS CLONES IN DIFFERENT SPACING
Provedor de dados: 196
Autores: Tavares, Ana Paula Cardoso; Soares, Thelma Shirlen; Cruz, Edmilson Santos.
This study aimed to analyze the effect of two planting spacing on dendrometric characteristics and basic wood density of eucalyptus clones. The experiment in the municipality of Jataí-GO, Brazil, used a randomized complete block design with three replications, in which the spacing (3.0 m x 2.0 m and 3.0 m x 3.0 m) were allocated to the plots and the clones (3335, 3336 and 3487) in the subplots. Diameter at breast height (dbh), total height (HT), total volume (VT), basic density (db), stem biomass (BS), leaf and branch biomass (BLB) and total biomass (BT) were evaluated. The data were submitted to analysis of variance, followed by the Tukey test for comparison of means at the 5% probability level. It was found that the dbh and VT characteristics were not...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4355

EFEITO DE EXTRATOS DE FOLHAS E RAMOS DE TRICHILIA SILVATICA  SOBRE SPODOPTERA FRUGIPERDA
Provedor de dados: 196
Autores: Teixeira, Felipe Ferlini; Rodrigues, Sérgio Roberto; Garcez, Walmir Silva; Garcez, Fernanda Rodrigues; Soares, Aloízio de Oliveira.
Espécies vegetais da família Meliaceae apresentam grande interesse nos estudos de controle de pragas devido a sua atividade inseticida. Para o presente trabalho, verificou-se a atividade inseticida de Trichilia silvatica, sobre o desenvolvimento de Spodoptera frugiperda. A partir de folhas e ramos de T. silvatica, foram preparados extratos etanólicos a 1%, e verificado o efeito inseticida sobre larvas, em seguida foi realizado o fracionamento das fases hidrometanólica, hexânica e acetato de etila de folhas e das fases hidrometanólica e hexânica de ramos, os quais foram aplicados em folhas de milho e oferecidas para alimentação de larvas recém eclodidas. Nos ensaios conduzidos, as variáveis biológicas avaliadas foram: peso de larvas ao 10º dia de idade,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantas inseticidas.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/239

UNIFORMIDADE DE DISTRIBUIÇÃO DE UM SISTEMA DE IRRIGAÇÃO POR ASPERSÃO VIA PIVÔ CENTRAL
Provedor de dados: 196
Autores: Nascimento, Valderir Facundo; Feitosa, Erialdo Oliveira; Soares, José Ivo.
A inadequada uniformidade de aplicação da água em sistemas de irrigação proporciona excesso em parte da área de cultivo e carência em outra, diminuindo a disponibilidade de água à cultura e aumentando o custo de produção. Nesse sentido, objetivou-se avaliar a uniformidade de aplicação de água por aspersão em pivôs centrais. Foram determinados os seguintes parâmetros: coeficientes de uniformidade (CUC, CUD e CUE) e a eficiência de aplicação. As vazões e pressões dos sistemas foram obtidos de acordo com a metodologia. No pivô central 04 os valores de CUC, CUD encontrados no teste estavam inadequados, abaixo do mínimo recomendado (85%); o CUE foi classificado como razoável e a eficiência de irrigação baixa. No pivô central 05 os valores de CUC e CUE...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1643

Compostagem de cama de aviário e seus efeitos na ocorrência da hérnia das crucíferas
Provedor de dados: 196
Autores: de Oliveira Lima, Jéssica; dos Santos, Carlos Antônio; da Costa Barros de Souza, Camila; Luiza Batalha Xavier, Cíntia; Moura Brasil do Amaral Sobrinho, Nelson; Goréte Ferreira do Carmo, Margarida Goréte Ferreira.
This study aimed to evaluate the effects of the application of poultry litter with different composting times on the occurrence of clubroot and the development of cauliflower plants. Plots inoculated with Plasmodiophora brassicae (Pb) and fertilized with non-composted poultry litter (PL-0 + Pb) and with poultry litter composted for 15 (PL-15 + Pb) and 30 days (PL-30 + Pb), were tested. As control treatments, we used inoculated plots without poultry litter (Control + Pb), non-inoculated plots (NI) and treated with composted poultry litter for 30 days (PL-30 - NI), and without poultry litter (Control - NI). The degree of stabilization and maturation of the poultry litter affected the severity of the clubroot, the volume and mass of healthy roots and galls,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brassica oleracea var. botrytis; Plasmodiophora brassicae; Compost; Organic matter; Suppressiveness; Brassica oleracea var. botrytis; Plasmodiophora brassicae; Composto; Matéria orgânica; Supressividade.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6806

APLICAÇÃO DE NITROGÊNIO, POTÁSSIO E CÁLCIO NA CULTURA DA CENOURA
Provedor de dados: 196
Autores: Silva, Luciana Maria da; Basílio, Scarlet de Aguiar; Silva Junior, Rogério Lamim; Benett, Katiane Santiago Silva; Benett, Cleiton Gredson Sabin.
O presente trabalho teve como objetivo avaliar de forma isolada a aplicação de fontes e doses de nitrogênio, modos de aplicação e doses de potássio e doses e modos de aplicação de nitrocálcio, nas características produtivas da cultura da cenoura. Os experimentos foram realizados em campo na Universidade Estadual de Goiás, Câmpus de Ipameri. O delineamento experimental utilizado em ambos foi o de blocos casualizados em esquema fatorial 2 x 5, com quatro repetições. Os dados foram submetidos à análise de variância (teste F) e as médias comparadas pelo teste de Tukey a 5% de probabilidade e foram realizadas análise de regressão. As fontes de nitrogênio e épocas não influenciaram nas características produtivas da cultura da cenoura em nenhuma das variáveis...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1412

ANÁLISE DE TRILHA DE ATRIBUTOS FÍSICOS NA RESISTÊNCIA À PENETRAÇÃO DE UM LATOSSOLO AMARELO
Provedor de dados: 196
Autores: Lima, Renato Paiva; Silva, Anderson Rodrigo; Oliveira, Dener Márcio da Silva.
O estudo das rela&amp;ccedil;&amp;otilde;es entre os atributos f&amp;iacute;sicos do solo &amp;eacute; mecanismo importante no monitoramento da compacta&amp;ccedil;&amp;atilde;o. O objetivo do trabalho foi estudar o desdobramento das correla&amp;ccedil;&amp;otilde;es em efeitos diretos e indiretos, por meio da an&amp;aacute;lise de trilha, de atributos f&amp;iacute;sicos sobre a resist&amp;ecirc;ncia &amp;agrave; penetra&amp;ccedil;&amp;atilde;o de um Latossolo Amarelo. O trabalho foi realizado na Fazenda Experimental Ch&amp;atilde;-de-Jardim, Areia, PB. As amostras, total de 24, foram coletadas na camada de 0,0-0,2 m, em uma parcela experimental de 35 &amp;times; 35 m. Os atributos f&amp;iacute;sicos analisados foram: densidade do solo, umidade, textura,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Física do Solo.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/216

RESISTÊNCIA MECÂNICA À PENETRAÇÃO EM DIFERENTES SISTEMAS DE USO DO SOLO
Provedor de dados: 196
Autores: Vogel, Gabriel Felipe; Fey, Rubens.
O objetivo deste trabalho foi avaliar a resistência do solo à penetração sob quatro diferentes sistemas de manejo do solo (café; amoreira; pastagem; silvipastoril) em três profundidades (0,0-0,20 m; 0,20-0,40 m; 0,40-0,60 m). O presente estudo foi realizado em Jardim Alegre–PR, em um Latossolo Vermelho. Os manejos foram: 1 - Cafezal cultivado manualmente; 2 - Área com amoreira para produção de bicho-da-seda, com tráfego de máquinas; 3 - Pastagem de braquiária (Urochloa decumbens) em sistema rotacionado, com taxa de lotação variada; 4 - Sistema silvipastoril com U. decumbens e eucalipto, com taxa de lotação variada. Houve interação significativa entre os diferentes tipos de manejo do solo e as profundidades. Na profundidade de 0,0-0,20 m as menores...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/812

RESPOSTA DO MILHO (Zea Mays L.) À ADUBAÇÃO FOLIAR E VIA SOLO DE NITROGÊNIO
Provedor de dados: 196
Autores: Mortate, Roberto Kennedy; Nascimento, Eduarda Fernanda; Gonçalves, Edmar Gustavo de Souza; Lima, Max Wendell de Paula.
O presente trabalho teve por objetivo avaliar a resposta de plantas de milho submetidas a diferentes fontes de adubos nitrogenados. O experimento foi conduzido em um delineamento em blocos casualizados (DBC), com quatro tratamentos e cinco repetições, totalizando 20 parcelas. Os tratamentos usados foram: T1= controle (sem aplicação de N), T2= 300 kg ha-1 de sulfato de amônio (18% de N), T3= 200 kg ha-1 de ureia (45% de N) e T4= 2 L ha-1 de Fortune® (20% de N), os quais foram aplicados em adubação de cobertura via solo e via foliar, conforme especificidade de cada produto, entre os estádios fenológicos V6 e V8. Os parâmetros avaliados foram: clorofila total (SPAD), diâmetro de espigas (cm), número de fileiras de grãos por espiga, massa de grãos por espiga...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2202

SPATIAL VARIABILITY OF HYDRAULIC CONDUCTIVITY OF SATURATED SOIL IN CONSERVATION UNIT
Provedor de dados: 196
Autores: Mesquita, Glaucia Machado; Santos, Felipe Corrêa Veloso dos; Dores, Anne Louise; Correchel, Vladia.
The study aimed to evaluate the hydraulic conductivity using soil samples with undisturbed structure in the soil layers of 0-5, 5-10, 10-20, and 20-40 cm; 120 soil samples were collected. For the determination of hydraulic conductivity, the constant load permeameter was used. For geostatistical analysis, exploratory data analysis was performed using frequency histograms, determining the main measures of position and dispersion, verifying the trends for the construction of boxplot graphics, which allows the identification of discrepant points. The lowest and highest hydraulic conductivity values were found in the 20-40 cm and 0-5 cm soil layers, respectively; values commonly found in soils under forest conditions. Based on the results, we conclude when the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil physical quality indicator; Permanent preservation areas; Soil water; Permeability.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6532

OCORRÊNCIA DE NEMATÓIDES FITOPARASITOS EM SOLO CULTIVADO COM ALGODÃO E SOJA
Provedor de dados: 196
Autores: Pereira, Amanda Casagrande; Toscano, Luciana Claudia; Abreu, Alexandra Botelho; Vieira, Noemi Souza; Dias, Pamella Mingotti.
O objetivo da pesquisa foi identificar a dinâmica populacional das espécies de nematóides nas culturas de algodão e soja em Cassilândia-MS. O experimento foi instalado na Universidade Estadual de Mato Grosso do Sul (UEMS), em duas áreas com 500 m² para cada cultura. As coletas de solo e raiz foram realizadas a cada 15 dias desde o início até o término das culturas, totalizando oito coletas. As amostras coletadas foram encaminhadas para o laboratório da Fundação Chapadão, em Chapadão do Sul-MS. Os nematóides identificados nas culturas foram dos gêneros Pratylenchus, Meloidogyne, Heterodera, Helicotylenchus, Mesocriconema, sendo a maior população encontrada para o gênero Pratylenchus, variando de 10 a 100 indivíduos/100 cm3 de solo para nos cultivos de soja...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/276

MANEJO DA ADUBAÇÃO POTÁSSICA PARA A CULTURA DO RABANETE
Provedor de dados: 196
Autores: Souza, Gabriel Pereira de; Lima, Luiza Gabriela Fulgêncio de; Borges, Isa Anastácia; Benett, Cleiton Gredson Sabin; Benett, Katiane Santiago Silva.
Estudos que visam avaliar se as quantidades de potássico aplicadas estão sendo aproveitadas para melhorar a fertilidade do solo e se têm influência na produtividade das hortaliças são de extrema importância para o adequado manejo da adubação potássica. Neste sentido, objetivou avaliar os efeitos da época de aplicação e de doses de fertilizantes potássicos na produtividade da cultura do rabanete. O delineamento experimental utilizado foi o de blocos casualizados em esquema fatorial 2 x 5 com quatro repetições. Os tratamentos resultaram da combinação de duas épocas de aplicação (semeadura e cobertura) e cinco doses de potássio (0, 30, 60, 90 e 120 kg ha-1), na forma de cloreto de potássio. A colheita foi realizada 20 dias após a semeadura do rabanete. As...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/287

QUALITY OF Genipa Spruceana STEYERM SEEDLINGS SUBMITTED TO FERTIGATION
Provedor de dados: 196
Autores: de Souza, Luciano Maria; Saragosa Rossi, Fernando; Caione, Gustavo; Gomes Oliveira, Pedro Paulo; Bertolino, Nayara.
Jenipapo (Genipa spruceana) é uma espécie nativa da Amazônia que possui grande potencial na produção de mudas para reflorestamento. O objetivo desse estudo foi avaliar o efeito de doses de nutrientes aplicadas por meio de fertirrigação na qualidade de mudas de Genipa spruceana. O delineamento experimental foi inteiramente casualizado com cinco repetições, totalizando sete tratamentos. Os tratamentos foram: testemunha (sem fertilização); 900 mg N   L-1 e 750 mg K L-1 com e sem micronutrientes; 1800 mg N L-1 e 1500 mg K L-1 com e sem micronutrientes, 3600 mg N L-1 e 3000 mg K L-1 com e sem micronutrientes. O experimento foi conduzido em casa de vegetação por 35 dias. Em seguida, foram avaliadas as seguintes variáveis: diâmetro do caule, altura da parte...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Amazon; Dickson Quality Index; Forest essences; Amazonas; Essência da floresta; Produção de mudas.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6815

NUTRIENTES E GIBERELINA NO CONDICIONAMENTO FISIOLÓGICO SOB A QUALIDADE DE SEMENTES DE BRAQUIÁRIA
Provedor de dados: 196
Autores: Barbosa Batista, Thiago; Duarte Cardoso, Eliana; Ferreira da Silva Binotti, Flávio; Eustáquio de Sá, Marco; Iwamoto Haga, Kuniko.
A aplicação de agentes químicos em sementes via condicionamento fisiológico, pode incrementar a produção e melhorar a qualidade fisiológica das mesmas. Objetivou – se avaliar a influencia de ciclos de condicionamento fisiológico com diferentes nutrientes e giberelina na qualidade fisiológica de sementes de Brachiaria brizantha cv. MG-5. O trabalho foi conduzido no Laboratório de Análise de Sementes da Universidade Estadual de Mato Grosso do Sul/Unidade Universitária de Cassilândia, de março a abril de 2013. O delineamento experimental foi o inteiramente casualizado, em esquema fatorial 3x3, constituído por primeiro ciclo de hidratação (controle – água, nitrato de potássio (KNO3) e Giberelina (GA3)), e segundo ciclo de hidratação [água, nitrato de cálcio...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Produção e Tecnologia de Sementes.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/253

SUBSTRATO À BASE DE PEQUI (Caryocar coriaceum) NA PRODUÇÃO DE MUDAS DE TOMATE E PIMENTÃO
Provedor de dados: 196
Autores: Maciel, Tamires Coelho Matias; da Silva, Toshik Iarley; Alcantara, Francisca Dayanne de Oliveira; Marco, Cláudia Araújo; Ness, Ricardo Luiz Lange.
Em meio à riqueza vegetal da Chapada do Araripe ocorre o extrativismo do pequi (Caryocar coriaceum) como importante atividade econômica e social das principais cidades do Cariri Cearense. Assim, o presente trabalho teve como objetivo a utilização dos resíduos dessa atividade como substrato na produção de mudas de tomate (Solanum licopersicum) e pimentão (Capsicum annuum). O experimento foi conduzido na área experimental do Centro de Ciências Agrárias e Biodiversidade da Universidade Federal do Cariri. O delineamento experimental foi inteiramente casualizado com cinco tratamentos e seis repetições, com dezesseis células (plantas) para cada repetição. Os dados obtidos foram submetidos à análise de variância e as médias comparadas pelo teste de Tukey a 5% de...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1551

INTERFERÊNCIA DE PLANTAS DANINHAS NA QUALIDADE E PRODUTIVIDADE DO GRÃO-DE-BICO
Provedor de dados: 196
Autores: Teixeira, Matheus Ferreira França; Biesdorf, Evandro Marcos; Pinheiro, Daniel Teixeira; Barros, Tiago Teixeira Viana; Iglesias, Erick.
O cultivo de grão-de-bico (Cicer arietinum L.) tem sido dificultado devido às interferências das plantas daninhas. Objetivou-se verificar o efeito da interferência de seis diferentes espécies invasoras (Bidens pilosa, Commelina benghalensis, Eleusine indica, Ipomoea grandifolia, Uruchloa brizantha e Uruchloa ruziziensis) na qualidade e produtividade de dois cultivares de grão-de-bico (BRS Aleppo e FLIP 86-77c). A interferência das plantas daninhas reduziu o período vegetativo de ambos os cultivares. A espécie Uruchloa ruziziensis influenciou negativamente o número de vagens do cultivar BRS Aleppo sugerindo ser prejudicial ao cultivo. Além disso, os resultados indicaram que há relação entre o período de convivência e o nível de infestação no número de grãos...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1598

MÉTODOS DE APLICAÇÃO DE NITROGÊNIO NA CULTURA DO MILHO EM SOLO DE CERRADO
Provedor de dados: 196
Autores: Biesdorf, Evandro Marcos; Biesdorf, Elivelton Maciel; Teixeira, Matheus Ferreira França; Dietrich, Otto Herbert; Pimentel, Leonardo Duarte; de Araujo, Charles.
O nitrogênio (N) é o nutriente mais limitante à produtividade do milho, sendo requerido em grandes quantidades para suprir a demanda da cultura. Além disso, o N aplicado via fertilizante mineral é muito susceptível a perdas por volatilização e/ou lixiviação, o que sugere a necessidade de estudos sobre métodos de aplicação visando otimizar o uso deste insumo. Objetivou-se com este estudo avaliar os efeitos de métodos de aplicação de N na cultura do milho nas condições do Cerrado Mato-grossense. Foram testadas duas formas de aplicação do N, na forma de ureia: aplicação a lanço em área total e incorporação ao solo na linha de plantio as quais foram parceladas em duas aplicações (semeadura e estádio vegetativo V6). O delineamento experimental utilizado foi o...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/805

COMPOSIÇÃO FLORÍSTICA E FITOSSOCIOLÓGICA DE UM REMANESCENTE DE FLORESTA OMBRÓFILA MISTA
Provedor de dados: 196
Autores: Bambolim, Amauri; Wojciechowski, Júlio César.
O estudo da composição florística e fitossociológica das florestas naturais são essenciais para a compreensão do funcionamento das comunidades vegetais. O presente estudo teve como objetivo conhecer, analisar e descrever a composição florística e a estrutura do componente arbóreo de um remanescente de Floresta Ombrófila Mista, na Floresta Nacional do município de São Francisco de Paula no estado do Rio Grande do Sul. Foram instaladas 100 parcelas de 10 x 10 demarcadas em um hectare no interior da floresta onde foram medidos e identificados todos os indivíduos com CAP ≥ 30 cm. A densidade total foi de 835 indivíduos/ha, pertencentes a 42 espécies, 29 gêneros e 17 famílias botânicas. As famílias Myrtaceae, Lauraceae e Euphorbiaceae apresentaram o maior...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1173

ADUBAÇÃO NITROGENADA EM COBERTURA EM DOIS CULTIVARES DE MILHO NO CARIRI-CE
Provedor de dados: 196
Autores: Máximo, Paulo José de Morais; Pinto, Antônio Alves; Camara, Felipe Thomaz da; Mota, Antônio Marcos Duarte; Nicolau, Francisca Edcarla de Araújo.
O milho tem importante destaque para a produção de forragem na alimentação animal, com a adubação nitrogenada sendo fundamental para garantir elevados níveis de produtividade. Portanto, o presente trabalho teve por objetivo avaliar a produtividade de massa verde de dois cultivares de milho em função da adubação nitrogenada em cobertura na região do Cariri-CE. O experimento foi conduzido no assentamento Malhada, no distrito de Ponta da Serra, distante 19 km da sede do município de Crato – CE. Foi utilizado o delineamento em blocos casualizados em esquema fatorial 2x4, com três repetições, totalizando 24 observações. O primeiro fator foi dois cultivares de milho híbrido (AG 1051 e FTH 960), e, o segundo, as doses de adubo nitrogenado em cobertura (0%, 50%,...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2561

COVER CROPS CHANGE THE PHYTOSOCIOLOGY OF WEEDS AND THE BANANA YIELD
Provedor de dados: 196
Autores: Ávila, Jorgiani; Andrade, Maria Gabriela Oliveira; Vendruscolo, Eduardo Pradi; Martins, Jordana Dias; Lima, Sebastião Ferreira.
This work aimed to evaluate the phytosociology of weeds and the fruit yield of banana (cv. Tropical) in different soil coverings. The experimental design used was randomized blocks, with eight treatments and three replications. The treatments consisted of sowing of Canavalia ensiformis, Cajanus cajan, Crotalaria juncea, Stylosanthes 'Campo Grande', Crotalaria spectabilis, Sorghum bicolor, and Phaseolus lunatus between the rows of the banana trees. A control treatment was also used without cover crops. Weed phytosociology was evaluated in four treatments. The number of hands per bunch, the number of fruits per hand, the number of fruits per bunch, and the fruit yield were estimated in all treatments. In the phytosociological survey, 23 species were...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3349

DESENVOLVIMENTO E CARACTERIZAÇÃO FÍSICO-QUÍMICA DE GELEIA COMUM E EXTRA DE GRAVIOLA COM PIMENTA
Provedor de dados: 196
Autores: Teles, Ana Claudia Martins; Pinto, Ellen Godinho; dos Santos, Janyne Ribeiro; de Oliveira, Camila Fernanda Dias; Soares, Dayana Silva Batista.
A produção de geleias é um processo bastante utilizado, porém algumas frutas com grande quantidade de nutrientes, como é o caso da graviola, são ainda pouco exploradas comercialmente nesses processos. Neste trabalho teve-se como objetivo o desenvolvimento e caracterização de geleia de graviola (Annona muricata) com pimenta “dedo de moça” tipo extra e comum em três concentrações de pectina 0,5; 1,0 e 1,5%. As análises físicas e químicas foram analisadas quanto ao seu teor de sólidos solúveis totais, umidade, vitamina C, Aw (atividade de água), acidez e pH, teste de sinérese e coloração expressa com valores de L*, a*, b*,croma e hue. A acidez e umidade foram influenciadas pela concentração de pectina e também pela concentração de açúcar na geleia extra e...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1341

PRODUÇÃO DE MUDAS DE BATATA-DOCE DE BAIXO CUSTO EM DIFERENTES SUBSTRATOS E NÍVEIS DE ENFOLHAMENTO DE ESTACAS
Provedor de dados: 196
Autores: Vendruscolo, Eduardo Pradi; Martins, Angélica Pires Batista; Campos, Luiz Fernandes Cardoso; Brandão, Daniel Cardoso; Nascimento, Lucas Marquezan; Seleguini, Alexsander.
A batata-doce é um alimento que se destaca como importante fonte de energia e fonte alternativa de carboidratos em substituição à grãos e outros tubérculos. O cultivo rudimentar, através da utilização de ramos para propagação diretamente a campo, é usual e pode, no entanto, ser responsável por um baixo índice de sobrevivência das brotações. Neste aspecto, objetivou-se definir a melhor técnica para obtenção de mudas em ambiente protegido através da utilização de diferentes substratos e níveis de enfolhamento das estacas de batata-doce. Foi empregado o delineamento experimental inteiramente casualizado, em esquema fatorial 4 x 2, sendo quatro substratos (água, solução nutritiva, substrato turfoso saturado com água e substrato turfoso saturado com solução...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1429

ENRICHMENT OF CASING SOIL WITH FE AND SOY-FLOUR UNDER Pseudomonas INOCULATION ON YIELD AND QUALITY OF BUTTON MUSHROOM
Provedor de dados: 196
Autores: Maknali, Fereshteh; Kashi, Abdolkarim; Salehi Mohammadi, Reza; Khalighi, Ahmad.
Effects of casing soil enrichment with soybean flour (SF) and iron (Fe) were explored on yield and quality of edible mushrooms inoculated with plant growth-promoting bacteria in a factorial experiment with four replications. Fe from Fe chelate source was applied at two levels of 0 (Fe0) and 500 mg L-1 (Fe500), SF at three levels of 0% (SF0), 1.5% (SF1.5), and 3% (SF3) of compost dry weight, and bacteria inoculation at two levels (non-inoculation and inoculation of mycelia with P. putida). The maximum fresh yield (20.3 kg m-2), mushroom number (1041), biological efficiency (95.0%), vitamin C (3.74 mg 100 g-1 FW), and yield of protein (6.48 kg m-2) were obtained from SF1.5 + P. putida. But, the maximum tryptophan (1.37 mg g-1 DW), methionine (2.29 mg g-1...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5111

ARMAZENAMENTO DE VARIEDADES DE BANANAS EM CONDIÇÕES DE ATMOSFERA MODIFICADA COM PERMANGANATO DE POTÁSSIO
Provedor de dados: 196
Autores: Falcão, Heloisa Alves de Sousa; Fonseca, Andreia Oliveira; Oliveira Filho, Josemar Gonçalves de; Pires, Marcio de Carvalho; Peixoto, José Ricardo.
A banana (Musa spp.) representa uma das principais frutas brasileiras com relação a produção e comercialização. Entretanto, as perdas pós-colheita têm sido bastante significativas. Assim, o presente trabalho teve por objetivo avaliar a qualidade de duas variedades de bananas armazenadas em sistema de atmosfera modificada com a utilização de absorvedor de etileno impregnado com solução de KMnO4, com e sem refrigeração. O delineamento experimental adotado foi em blocos casualizados em arranjo fatorial 2×2×2 com três repetições e seis períodos de armazenamento. Avaliou-se a qualidade dos frutos quanto à perda de massa fresca, teor de sólidos solúveis (SS), acidez titulável (AT) e relação SS/AT. Os resultados indicaram que a combinação do uso da embalagem com...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1734

INFLUÊNCIA DE SISTEMAS DE PREPARO NA MANUTENÇÃO DA PALHADA E RESISTÊNCIA DO SOLO À PENETRAÇÃO
Provedor de dados: 196
Autores: Theodoro, Gustavo de Faria; Golin, Henrique de Oliveira; da Silva, Marcio Santos; Rezende, Rafael Padilha; Abreu, Victor Luan Silva de.
O preparo do solo favorece o desenvolvimento do sistema radicular e cria condições adequadas para o desenvolvimento das plantas. Todavia, o intenso uso de máquinas e implementos pode afetar a resistência do solo à penetração (RP) e a manutenção da cobertura vegetal morta na superfície do solo. O objetivo deste trabalho foi avaliar a influência dos sistemas de preparo convencional e reduzido sobre a RP e a cobertura vegetal morta em um Latossolo vermelho de textura muito argilosa, em condições de baixa umidade, além de comparar três métodos na estimativa da palhada. A RP foi avaliada por meio do uso de um penetrômetro de impacto modelo IAA/Planalsucar – Stolf na profundidade de 0,0-0,6m e a cobertura vegetal morta por meio da captura e análise de imagens....
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2220

DIAGNOSE FOLIAR E PRODUÇÃO DE SOJA APÓS APLICAÇÃO DE RESÍDUOS EM UM LATOSSOLO SOB SISTEMA PLANTIO DIRETO
Provedor de dados: 196
Autores: Cardoso dos Santos, Susiane Moura; Antonangelo, João Arthur; Deus, Angélica Cristina Fernandes; Büll, Leonardo Theodoro.
A aplicação superficial de resíduos e o não revolvimento do solo decorrente do sistema plantio direto (SPD) favorecem os atributos químicos, físicos e biológicos do solo, afetando também a dinâmica de nutrientes ao longo do seu perfil. Além de atenuadores da acidez do solo, alguns resíduos ainda são excelentes fontes de nutrientes às plantas, dentre eles os macronutrientes, como o fósforo, o nitrogênio e o cálcio, e os micronutrientes, como o manganês e o zinco. Neste contexto, objetivou-se avaliar o estado nutricional e a produtividade de grãos da cultura da soja (Glycine max) cultivada sob SPD em um Latossolo Vermelho Distrófico submetido à aplicação superficial de resíduos industriais e urbanos. O delineamento experimental utilizado foi o de blocos...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2725

PERFORMANCE OF Metarhizium rileyi APPLIED ON Helicoverpa armigera (Hubner) (Lepidoptera: Noctuidae)
Provedor de dados: 196
Autores: de Souza Loureiro, Elisângela; de Souza Tosta, Ricardo Alexandre; Mingotti Dias, Pamella; Amorim Pessoa, Luis Gustavo; Mendes de Oliveira Neto, Francisco; Reis Devoz, Gabriel Luiz; Muchalak, Franciele.
This study aimed to evaluate the efficiency of different strains of the entomopathogenic fungus Metarhizium rileyi in the control of Helicoverpa armigera caterpillars in laboratory conditions. Caterpillars between the 2nd and 3rd instar were used, ranging in size from 0.7 to 1.2 cm length. The experimental design used was completely randomized, composed of five treatments and five replications, each one consisting of 50 insects. The treatments T1 - Control (sterile distilled water), T2 - M. rileyi UFMS 02 strain, T3 - M. rileyi UFMS 03 strain, T4 - M. rileyi UFMS 06 strain, and T5 - M. rileyi UFMS 07 strain were evaluated. All treatments were applied (2 mL/insect) in suspensions of the order of 1.0 × 109 conidia mL-1, and Tween 80® was added in all...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4208

ACÚMULO DE MATÉRIA SECA E NUTRIENTES NO CAPIM-MOMBAÇA EM FUNÇÃO DO MANEJO DA ADUBAÇÃO NITROGENADA
Provedor de dados: 196
Autores: Galindo, Fernando Shintate; Buzetti, Salatiér; Teixeira Filho, Marcelo Carvalho Minhoto; Dupas, Elisângela; Ludkiewicz, Mariana Gaioto Ziolkowski.
O nitrogênio é um elemento de extrema importância na cultura de forrageiras, sendo o nutriente que mais influencia na produtividade e na qualidade das pastagens. Objetivou-se estudar a condução de uma pastagem com alto potencial produtivo utilizando fontes e doses de nitrogênio. As fontes de N foram nitrato de amônio (N.A.) e ureia aplicadas nas doses de N: 0, 50, 100, 150 e 200 kg ha-1 por corte, na espécie forrageira Panicum maximum cv. Mombaça, avaliando o acúmulo de nitrogênio (N), fósforo (P) e potássio (K) e a taxa de acúmulo de matéria seca (MS). As fontes de N não influenciaram o acúmulo de N, P e K e taxa de acúmulo de MS. As doses influenciaram positivamente no acúmulo de N, K e a taxa de acúmulo de MS, ocorrendo incremento com o aumento das...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2132

BAGAÇO DE MALTE COMO SUBSTRATO PARA PRODUÇÃO DE BIOPIGMENTOS PRODUZIDOS POR MONASCUS RUBER CCT 3802
Provedor de dados: 196
Autores: Oliveira, Camila Fernanda Dias de; Vendruscolo, Francielo; da Costa, Jaquelinne Pires Vital; de Araújo, Welker Denner Bernardes.
O presente estudo busca, evidenciar o reaproveitamento do resíduo agroindustrial bagaço de malte, na fabricação de pigmentos naturais produzidos por Monascus, determinando a velocidade de crescimento radial pelo fungo filamentoso Monascus ruber CCT 3802, em cultivo sólido sob diferentes concentrações de bagaço de malte. A determinação da velocidade de crescimento radial foi realizada em meio ágar dextrose batata (PDA) sob diferentes concentrações de substrato bagaço de malte (5, 10, 20 e 40 g.L-1), além da placa padrão contendo apenas PDA. A maior velocidade de crescimento radial do Monascus. ruber foi obtida da placa contendo 40 g.L-1 de bagaço de malte 0,1383 mm h-1, o que corresponde a um crescimento de 3,32 mm dia-1, ou seja, um aumento de 54,95%...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1200

ESTABILIDADE DE AGREGADOS E TEOR DE MATÉRIA ORGÂNICA EM UM LATOSSOLO VERMELHO SOB UROCHLOA BRIZANTHA APÓS A APLICAÇÃO DE CAMA DE PERU
Provedor de dados: 196
Autores: Betiolo Troleis, Maria Julia; Roque, Cassiano Garcia; Rezende Zuffo Borges, Monica Cristina; Noguerira, Kenio Batista; Gouveia, Natalia Amanda.
O aumento da produção de aves na região Centro-Oeste do Brasil tem produzido um considerável montante de esterco animal para produção em potencial de adubos orgânicos. Objetivou-se com este estudo avaliar os efeitos da aplicação de cama de peru nos teores de matéria orgânica e na estabilidade dos agregados de um Latossolo Vermelho distrófico cultivado com Urochloa brizantha. O delineamento experimental foi em blocos casualizados, com três repetições. Os tratamentos foram constituídos dos seguintes manejos da fertilidade do solo: i) controle; ii) aplicação de 2,5 Mg ha-1 cama de peru; iii) 5 Mg ha-1 cama de peru; iv) 7,0 Mg ha-1 cama de peru; v) 2,5 Mg ha-1 cama de peru + 1,0 Mg ha-1 calcário; vi) 5,0 Mg ha-1 de cama de peru + 1,0 Mg ha-1 calcário, vii) 7,0...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1267

EXTRACTS OF CINNAMON (Cinnamomum cassia) AND MINT (Mentha arvensis) FOR THE FUNGI CONTROL OF Sclerotinia sclerotiorum
Provedor de dados: 196
Autores: Ferreira, Laura Martins; Xavier, Murilo Gustavo Andrade; Dias, Paulo Ricardo Resende; Vieira, Gustavo Haralampidou da Costa.
Studies regarding vegetal extracts and essential oils from native plants have demonstrated efficiency in controlling phytopathogens of fungitoxic action, hampering the development of phytopathogenic fungi. This study aims to determine the fungicide effect of vegetal extracts during the mycelial growth of the fungus Sclerotinia sclerotiorum (Lib.) de Bary. The experiment was conducted in the phytosanitary laboratory of the UEMS in the unit of Cassilândia-MS, Brazil. A completely randomized design was used with a factorial scheme 4 x 5, comprising leaves, bark, and branches of cinnamon and mint leaves in the concentrations of 0, 2.5, 5.0, 10, and 20%, with six repetitions per treatment. The evaluations were made 24, 48, and 96 hours after the transplant,...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6161

MINERAL, PROTEIN, AND ENERGY SUPPLEMENTATION IN HEIFERS IN A NATIVE PAMPA BIOME PASTURE DURING WINTER
Provedor de dados: 196
Autores: Malaguez, Edgard Gonçalves; Gonçalves, Thaís Lopes; Giudice, Bibiana Bastos; Oaigen, Ricardo Pedroso; Castagnara, Deise Dalazen; de Azevedo, Eduardo Bohrer.
This study evaluated the effect of different supplements during winter on the performance of heifers in a native Pampa biome field using deferred grazing and evaluated the economic viability of each treatment. A total of 124 heifers from Brangus and Angus breeds, 18 months old, and with an average weight of 301.6 kg were included in this experiment. The treatments applied were: control with only native grassland, native grassland + 80P mineral salt treatment (MS), native grassland + protein salt treatment (PS), and native grassland + protein/energy salt treatment (PES). Besides the productive, botanical, and bromatological characteristics of the pasture, the average daily gain and the live weight gain per hectare were evaluated. The economic viability of...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3519

ASPECTOS CULTURAIS, MORFOLÓGICOS E MORFOMÉTRICOS DE Sordaria fimicola INCIDENTE EM FOLHAS DE CAPIM-MASSAMBARÁ (Sorghum arundinaceum)
Provedor de dados: 196
Autores: Almeida, Andressa de Souza; Costa, Marcos Antônio Garcia Caetano da; Estrela, Lucinete Martins Barbosa; Lima, Milton Luiz da Paz.
O capim-massambará (Sorghum arundinaceum) pode servir de fonte de inóculo de agentes de biocontrole como Sordaria spp. O objetivo deste trabalho foi avaliar o crescimento in vitro, a patogenicidade, caracterizar e identificar um isolado de Sordaria sp. incidente em capim-massambará. Amostras de folhas apresentando sintomas foram submetidas a isolamento em meio de cultura. A partir deste foram aplicados os seguintes testes: a) teste fisiológico – análise do crescimento micelial em meio de cultura. b) teste biológico – discos de micélio e solução de ascósporos foram inoculados em folhas; e c) identificação – caracterização morfológica das estruturas reprodutivas. O maior crescimento micelial foi observado nos meios BDA e ST. O isolado em condições...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1423

PRODUCCIÓN BABY LEAF DE BERRO DE TIERRA CULTIVADO EN DIFERENTES AMBIENTES Y MARCOS DE PLANTACIÓN
Provedor de dados: 196
Autores: Espíndola, Jhone Souza; Otto, Rosana Fernandes; Beruski, Gustavo Castilho; Ohse, Silvana.
Baby leaf es un tipo de hortícola que llama la atención de los consumidores por el pequeño tamaño de las hojas y la posibilidad de ser comercializada con una mezcla de hojas para ensalada. El trabajo se realizó en Ponta Grossa– PR (Brasil) y tuvo como objetivo evaluar los ambientes de cultivo y la densidad plantas en la producción de baby leaf de berros de tierra. Los tratamientos fueron 03 ambientes de cultivo (TA - túnel agrotextil; TP - túnel plástico; AL– Aire Libre) y 03 marcos de plantación (E1- 15 x 10 cm; E2- 15 x 7 cm; E3- 10 x 7 cm).Los ambientes TP y TA, de manera independiente, proporcionaron altura y número de hojas de plantas superiores al cultivo en AL, así como valores mayores de biomasas fresca (BF) y seca (BS) y del índice de área foliar...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2569

ESTERCO BOVINO E FIBRA DE COCO NA FORMAÇÃO DE MUDAS DE BARUZEIRO
Provedor de dados: 196
Autores: Oliveira, Letícia Carolina de; Costa, Edilson; Oliveira Sobrinho, Marcos Fidêncio de; Binotti, Flávio Ferreira da Silva; Maruyama, Wilson Itamar; Alves, Ana Carolina.
A utilização de subprodutos da agropecuária na formação de mudas frutíferas do Cerrado auxilia a gestão ambiental e pode reduzir custos de produção. Desta forma, o presente trabalho avaliou a formação de mudas de baruzeiro, Dipteryx alata, em diferentes substratos orgânicos, constituídos de: 80% esterco bovino + 20% fibra de coco; 60% esterco bovino + 40% fibra de coco; 40% esterco bovino + 60% fibra de coco e 20% esterco bovino + 80% fibra de coco. Foram avaliados dados de emergência, altura, diâmetro do colo, biomassas e relações envolvendo estas variáveis. O esterco utilizado foi apenas curtido e seco e não compostado. Foi adotado o delineamento experimental inteiramente casualizado com sete repetições de três plantas cada. Utilizando esterco não...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/240

MODELOS DE AFILAMENTO E OTIMIZAÇÃO DE MULTIPRODUTOS DE UM POVOAMENTO DE Eucalyptus NÃO DESBASTADO
Provedor de dados: 196
Autores: Lustosa Junior, Ilvan Medeiros; Lima, Mirella Basileu de Oliveira; Nascimento, Beatriz Garcia; Meira Junior, Milton Serpa de; Castro, Renato Vinícius Oliveira.
Este trabalho consiste na seleção de um modelo de taper para descrever o afilamento de fustes das árvores de um povoamento não desbastado, a fim de ser aplicado em um sistema de otimização de corte das árvores para multiprodutos da madeira. O trabalho foi realizado no município de Martinho Campos, Minas Gerais, tendo com área de estudo um povoamento do híbrido Eucalyptus grandis W. Hill X Eucalyptus urophylla S. T. Blake, implantado em janeiro de 2007. Dentre os modelos de taper ajustados, o modelo de Garay foi o que melhor representou o afilamento dos fustes das árvores quando verificou as estatísticas de precisão e as análises gráficas dos resíduos. Posterior ao ajuste desse modelo obteve-se a seguinte equação para estimativa dos diâmetros ao longo do...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2216

PERDAS DE ÁGUA, SOLO E NUTRIENTES POR ESCOAMENTO SUPERFICIAL APÓS APLICAÇÃO DE DEJETOS LÍQUIDOS DE SUÍNOS NA CULTURA DO MILHO
Provedor de dados: 196
Autores: Scherrer Menezes, June Faria; da Silva, Mariana Pina; Benett, Cleiton Gredson Sabin; Benites, Vinicius de Melo; Cantão, Veridiana Cardoso Garcia.
O objetivo do trabalho foi avaliar a perda de solo, água e nutrientes em um Latossolo Vermelho distroférrico submetido a aplicação de dejetos líquido de suínos (DLS) e adubação mineral. O experimento foi conduzido em área experimental da Universidade de Rio Verde no período de outubro de 2005 a março de 2006 em área de sistema de plantio direto desde 2000. O experimento foi constituído por três tratamentos (50 e 200 m3 ha-1 de DLS e 570 kg ha-1 da fórmula 04-14-08 (N-P2O5-K2O) para o cultivo de milho), estabelecidos em um delineamento experimental de blocos casualizados, com três repetições. O tratamento com a aplicação de 50 m3 ha-1 de DLS resultou em maior perda de água e solo. Sendo que no tratamento com 200 m3 ha-1 de DLS foi detectado menores perdas...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1747

DOSES DE NPK EM TOMATEIRO CV. MARMANDE E SEU DESEMPENHO A CAMPO NO CERRADO
Provedor de dados: 196
Autores: Silva, Valéria Lima da; de oliveira, Alessandra Conceição; Farias, Geyci Aires; Silva, WESLIAN Vilanova da; Sllva, Lucely Pereira da.
 Atender as necessidades nutricionais das mudas é fundamental para o desempenho da planta no campo. Nesse sentido, objetivou-se com esse trabalho avaliar o efeito de doses de NPK na fertirrigação de mudas de tomate e seu desempenho a campo. O delineamento experimental utilizado foi em blocos ao acaso com cinco tratamentos e quatro repetições. Os tratamentos foram doses de NPK (0; 1,5; 3,0; 4,5 e 6,0 mg dm-3) na fertirrigação das mudas. Estas, quando foram a campo, tiveram maior desempenho, acima de 4,5 mg dm-3. Conclui-se que a cv. Marmande obteve o melhor desenvolvimento e as mudas quando foram a campo tiveram maior desempenho com doses a partir de 4,5 mg dm-3, mostrando que o tomateiro responde a adubação NPK de forma positiva.
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2090

DIVERGÊNCIA GENÉTICA ENTRE CULTIVARES DE FEIJÃO COMUM CULTIVADOS NO ESTADO DO TOCANTINS
Provedor de dados: 196
Autores: Tavares, Taynar Coelho de Oliveira; Sousa, Sérgio Alves de; Lopes, Marilia Barcelos Souza; Veloso, Danilo Alves; Fidelis, Rodrigo Ribeiro.
A escolha e seleção de genitores podem ser auxiliadas por várias análises multivariadas que orientam os melhoristas na tomada de decisão em um programa de melhoramento, dentre elas, podendo destacar as análises de dissimilaridade genética. Diante disso, objetivou-se com este trabalho avaliar a divergência genética de dezenove cultivares de feijão comum cultivado no Estado do Tocantins. O delineamento estatístico adotado foi o de blocos casualizados com quatro repetições. Para identificar a dissimilaridade das cultivares estudada, avaliou-se altura de planta, inserção de primeira vagem, diâmetro de caule, número de vagem por planta, número de grãos por vagem, massa de 100 grãos e produtividade de grãos. Conclui-se que existe variabilidade genética entre as...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1892

TAMARIND TREE SEEDLINGS IN PROTECTED ENVIRONMENTS AND SUBSTRATE
Provedor de dados: 196
Autores: Silva, Anne Karoline da; Costa, Edilson; Curi, Thayla Morandi Ridolfi de Carvalho; Salles, Josiane Souza; Binotti, Flávio Ferreira da Silva; Binotti, Eliana Duarte Cardoso; Vieira, Gustavo Haralampidou da Costa; Zoz, Tiago.
This study aimed to evaluate the formation of tamarind tree seedlings in different protected environments and substrates. Five protected environments were used and substrates using combinations of different proportions of humus, cattle manure, vermiculite, and cassava stems. The environments with screens and the environments with polyethylene films were conducive to the emergence of the tamarind seedlings. All the substrates presented adequate conditions for the emergence of seedlings in these environments. The environment covered with bacuri straw was not favorable to the emergence of the tamarind seedlings. The substrates containing cattle manure provided the best conditions for emergence in the environment covered with bacuri straw. The greenhouses and...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4838

MUDAS DE JAMBOLÃO SOB NÍVEIS DE SOMBREAMENTO, BANCADAS REFLETORAS E PROFUNDIDADE DE SEMEADURA
Provedor de dados: 196
Autores: Salles, Josiane Souza; Lima, Alexandre Henrique Freitas de; Costa, Edilson.
A fase de formação de mudas frutíferas é muito importante para implantação ou renovação de pomares. O trabalho avaliou níveis de sombreamento, material refletor em bancadas de cultivo e profundidade de semeadura para mudas de jambolão, na Universidade Estadual de Mato Grosso do Sul, Unidade Universitária de Cassilândia – MS. Foram avaliados quatro níveis de sombreamento 0, 18, 30 e 50%, dois tipos de bancadas (com e sem material refletor de papel alumínio) e duas profundidades de semeadura (2 e 4 cm). Nos ambientes o experimento foi conduzido em delineamento experimental inteiramente casualizado, em esquema fatorial 2 x 2 com 5 repetições. Os ambientes foram comparados pela análise conjunta. Foram avaliados os parâmetros de crescimento e razões...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2181

MUFFINS ISENTOS DE GLÚTEN E LACTOSE DESENVOLVIDOS COM RESÍDUO DE POLPA DE GRAVIOLA (ANNONA MURICATA)
Provedor de dados: 196
Autores: dos Santos, Janyne Ribeiro; Boêno, Josianny Alves.
Apesar do acréscimo na produção nos últimos anos, atualmente ainda são escassos os produtos no mercado destinados à indivíduos com restrições alimentares. O presente estudo visou desenvolver “muffins” (bolinhos) isentos de glúten e lactose, utilizando farinha de arroz e resíduo da filtragem da polpa de graviola (Annona muricata), e avaliar a influencia do resíduo nas características da massa. Os muffins elaborados com 0 % (padrão), 10, 20 e 30 % de resíduo da polpa de graviola em substituição a farinha de arroz, foram submetidos a análises físicas de peso, diâmetro e espessura antes e depois do forneamento, cálculo da expansão de massa, análise de pH, cinzas e umidade. Valores obtidos nas análises físicas dos muffins demostraram que as amostras com maior...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1207

PERFORMANCE OF LETTUCE UNDER INFLUENCE OF DIFFERENT SOIL COVERS AND PLANTING SPACING
Provedor de dados: 196
Autores: Vendruscolo, Eduardo Pradi; Campos, Luiz Fernandes Cardoso; Rodrigues, Aliny Heloísa Alcântara; Correia, Sávio Rosa; Oliveira, Paulo Ricardo; Freitas, Murillo Ribeiro; Seleguini, Alexsander.
Lettuce cultivation is an activity of great economic importance; therefore, the use of techniques for better use of space and better-growing conditions should be evaluated. The objective of this study was to evaluate the development and yield of garden lettuce grown under different soil coverings and plant spacing. The study was conducted in an experimental area located at the School of Agronomy of the Federal University of Goiás, in the city of Goiânia, Goiás. The experiment was conducted in a randomized block design with subdivided plots in four replications. The plots consisted of three soil coverings (soil without cover, straw, and plastic cover) and the subplots in three planting spacing (PS1 = 25 x 20; PS2 = 25 x 25; PS3 = 25 x 30 cm), totaling nine...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5850

ADUBAÇÃO COM BORO NO CRESCIMENTO DE MUDAS DE MOGNO-AFRICANO
Provedor de dados: 196
Autores: Araújo, Matheus da Silva; Melo, Marcela Amaral de; Hodecker, Bárbara Elias Reis; Barretto, Vitor Corrêa de Mattos; Rocha, Ednaldo Cândido.
Em razão da escassez de informações sobre adubação em mogno-africano, no presente estudo, objetivou-se avaliar a adubação com boro (B) no crescimento inicial de mudas de mogno-africano (Khaya senegalensis A. Juss). O experimento foi realizado em estufa, em recipientes de plástico com capacidade de 7 dm3 e utilizado como substrato solo Latossolo Vermelho-Amarelo distrófico. O delineamento experimental utilizado foi inteiramente casualizado, com cinco tratamentos e seis repetições. Os tratamentos foram constituídos de cinco doses de B (0; 0,5;1,0; 2,0 e 4,0 mg dm-3), utilizando-se o ácido bórico como fonte. Aos 150 dias após o transplantio foram analisados a altura da planta, o diâmetro do coleto, o número de folíolos e a matéria seca de folhas, caule e...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2183

EFEITO DE SILICATO DE CÁLCIO E MAGNÉSIO NO CRESCIMENTO INICIAL DE MILHO TRANSGÊNICO
Provedor de dados: 196
Autores: de Souza, João Paulo Freitas; Martins, Gustavo Luís Mamoré; Pereira, Amanda Casagrande; Binotti, Flávio Ferreira da Silva; Maruyama, Wilson Itamar.
O fornecimento do silício pode estimular o desenvolvimento vegetativo e a produção vegetal. Desse modo, o objetivo do trabalho foi avaliar o efeito da aplicação de silicato de cálcio e magnésio no crescimento inicial de plântulas de milho transgênico. O experimento foi conduzido em casa de vegetação na área experimental da Universidade Estadual de Mato Grosso do Sul (UEMS), Unidade Universitária de Cassilândia-MS. O delineamento experimental utilizado foi o inteiramente casualizado (DIC) com cinco tratamentos e cinco repetições. Os tratamentos foram constituídos por cinco doses de silicato de cálcio e magnésio: 0, 18, 24, 30 e 36 g dm-3. Após seis meses da aplicação do silicato de cálcio e magnésio foi realizado a semeadura do híbrido Dekalb 310 PRO 2. Foi...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/280

WEEDS IN SOYBEAN CROP AFTER ANNUAL CROPS AND PASTURE
Provedor de dados: 196
Autores: Fachinelli, Ricardo; Stradioto Melo, Thais; Prevedel Capristo, Denise; Antunes de Abreu, Hadassa Kathyuci; Ceccon, Gessí.
The use of crop practices to reduce the weed community is an ally to integrated weed management. Given this, the study aimed to identify a composition and weed infestation in a soybean area under different predecessor crops implanted in different years. The experiment was carried out in the 2019/2020 harvest in Dourados, MS. The experimental design was a randomized block with nine treatments. The treatments were composed of autumn-winter crops. The area with predecessor cultivation: corn-Brachiaria intercropping; cowpea beans; single corn; an area with predecessor cultivation of Brachiaria as pasture for one year; two years; three years; four years; five years, and six years. All treatments were followed by soybean cultivation in the 2018/2019 harvest and...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5563

Rendimentos de larvas de moscas em diferentes colheitas com três proporções de farelo de trigo e esterco suíno
Provedor de dados: 196
Autores: Casanovas Cosío, Enrique; Reyes Reyes, Reina; Suárez del Villar Labastida, Alexis; Álvarez Sánchez, Ana; Padilla Morales, Raúl.
The aim of the research was to compare the yields of house fly larvae using different proportions of wheat bran and swine feces as larval development medium, in a randomized block experimental design with five replications: A-100 % wheat bran; B- 50% wheat bran and 50% swine feces; C- 100% swine feces. Measurements of the temperature of the substrates, as well as the temperature and relative humidity of the place where the flies were developing were made every 24 hours. The larval yield per m2 and kg of substrate, (including the water used to moisten the larval media) were also registered. The wheat bran substrate presented the highest temperature values (36.78 oC), with values above the ambient temperature. The relative humidity varied between 44 and 68%....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water; Insects; Alternative protein; Organic residues; Substrates; Água; Insetos; Proteína alternativa; Resíduos orgánicos; Sustratos.
Ano: 2023
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6997

Semeadura de soja com disco dosador agrupado pneumático sob diferentes velocidades operacionais
Provedor de dados: 196
Autores: Lopes, Arthur Gabriel Caldas; Correia, Tiago Pereira da Silva; Taveira, Wesley Matheus Cordeiro Fulgêncio; Pereira, Gabriela Greice; de Souza, Alyne Ayla Rodrigues.
Convencionalmente a semeadura da soja é realizada distribuindo as sementes de forma individualizada e equidistante ao longo do sulco de semeadura. uma possível alternativa é a dosagem e distribuição agrupada de sementes, apenas rearranjando-as. Sendo assim, o objetivo do trabalho foi avaliar as características agronômicas da soja semeada com disco dosador de sementes convencional e agrupado sob diferentes velocidades operacionais. O delineamento experimental adotado foi o inteiramente casualizado em esquema fatorial 2 x 3, sendo dois arranjos de semeadura, agrupado e convencional, e três velocidades de semeadura 4,5; 5,2 e 6 km h-1, com quatro repetições cada. Os resultados evidenciam incremento produtivo entre 20,7% e 39,9% para o arranjo agrupado nas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycine max; Spatial arrangement; Agronomic characteristics; Agronomic characteristics.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6721

DESENVOLVIMENTO E AVALIAÇÃO DE UM PULVERIZADOR HIDRÁULICO DE BARRAS RÍGIDAS HORIZONTAIS DE BAIXO CUSTO
Provedor de dados: 196
Autores: França, Jorge Alfredo Luiz; Gonçalves, Wagner Santos; Romeiro, Bruno Peres; Benett, Cleiton Gredson Sabin; Silva, Anderson Rodrigo da.
Encontram-se no mercado diversos modelos de pulverizador costal manual que nem sempre atendem a necessidade do pequeno produtor, pois o uso destes equipamentos demandam excessivo tempo e mão-de-obra. Objetivou-senessetrabalho desenvolver um pulverizador hidráulico de barras rígidas horizontais de baixo custo e avaliar a uniformidade de vazão (L min-1)dos bicos de pulverização ao longo das barras. O trabalho foi realizado no Instituto Federal Goiano - Câmpus Urutaí. O experimento foi realizado em blocos casualizados em esquema fatorial 2 x 12 (duas rotações na tomada de potência do trator e 12 bicos de pulverização). Foram utilizadas as rotações de 540 e 750 RPM na tomada de potência do trator, as quais proporcionaram pressões de serviço de 118 e 211 kPa...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Engenharia Agrícola.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/246

CARACTERIZAÇÃO MORFOLÓGICA DE Alternaria alternata ASSOCIADO A SEMENTES DE ALFACE AMERICANA CV. ‘ASTRA’
Provedor de dados: 196
Autores: Muniz, Paulo Henrique Pereira Costa; Marques, Marina Gabriela; Silva Peixoto, Gustavo Henrique; Simão, Kamila Gabriela; Carvalho, Daniel Diego Costa.
A mancha de alternaria, cujo agente causal é o fungo, Alternaria spp., encontra-se distribuída pelas áreas de plantio de hortaliças no Brasil onde frequentemente a doença é veiculada por sementes contaminadas. Neste sentido, a qualidade sanitária e fisiológica de sementes é fundamental para o estabelecimento uniforme das culturas em campo, sendo um dos fatores que garantem o sucesso da produção da olerícola. O objetivo deste trabalho foi caracterizar o fungo Alternaria associado a sementes de alface americana cv. ‘Astra’. A análise de incidência foi realizada pelo método blotter test, empregando-se o delineamento inteiramente casualizado (DIC), com quatro repetições (50 sementes gerbox-1). Após sete dias a 20 ºC (± 2 ºC) e foto período de 12 h, a avaliação...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1799

RECIPIENTE BIODEGRADÁVEL E SUBSTRATOS PARA MUDAS DE MARACUJAZEIRO
Provedor de dados: 196
Autores: Guerra, Mariana Santana; Barbosa, Marcelo Sousa; Costa, Edilson; Costa Vieira, Gustavo Haralampidou.
O descarte incorreto dos recipientes plásticos usados na produção de mudas causa impactos ao ambiente. O maracujazeiro amarelo é produzido em grande escala, tendo importância fármaco-terapêutico, além de ser uma frutífera de produção rápida, sendo para isso imprescindível a obtenção de mudas de qualidade. O objetivo deste trabalho foi avaliar recipientes e substratos na formação de mudas de maracujazeiro. O experimento foi conduzido num delineamento inteiramente casualizado, em esquema fatorial 2 x 4, sendo 2 recipientes e 4 substratos. Como recipientes foram utilizados bucha vegetal e sacos plásticos. Em cada recipiente foram testados os seguintes substratos: 30% de esterco bovino + 70% de vermiculita; 30% de Bioplant + 70% vermiculita; 30% de esterco...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1641

EVALUATION OF THE EFFECTS OF THE INFUSION OF Ocimum selloi LEAVES USING THE Allium cepa MODEL
Provedor de dados: 196
Autores: Mascarenhas Santos, Maria do Socorro; Verdan, Maria Helena; Piva, Raul Cremonezi; Viana, Lucilene Finoto; Cardoso, Claudia Andrea Lima.
Ocimum selloi is a plant used in traditional medicine as a tea; however, no studies have reported the biological activity of the aqueous extract of this plant. This study aimed to evaluate the cytotoxicity, genotoxicity, and mutagenicity of two concentrations of an aqueous extract prepared by infusion of leaves from O. selloi using the Allium cepa model. The O. selloi infusion contained 107.1 ± 1.27 mg GAE g-1. In the A. cepa test, the concentration of the extract influenced the germination index; for 1.0 mg mL-1, it was 60.78% and for 5.0 mg mL-1, it was 51.14%. The evaluation of root development also showed differences between the two concentrations and the negative control, and differences in mitotic index were observed between the concentrations and...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5647

ESTRESSE HÍDRICO SIMULADO EM GENÓTIPOS DE FEIJÃO, MILHO E SOJA
Provedor de dados: 196
Autores: Viçosi, Karen Andreon; Ferreira, Aparecido Alves Serafim; Oliveira, Luis Augusto Batista de; Rodrigues, Fabrício.
O trabalho teve como objetivo simular condições de déficit hídrico, em laboratório, por meio do manitol, para avaliação do desempenho fisiológico de sementes de cultivares de feijão, milho e soja. As sementes foram submetidas à germinação sob condições de estresse hídrico, com os níveis 0, -0,6, -1,2, -1,8 e -2,4 MPa de potencial osmótico, simulados com soluções de manitol (C6H14O6), nas doses: 0; 44; 58; 89,17; 133,75 g L-1. Para cada espécie, foi utilizada quatro repetições por tratamento, composta de 50 sementes colocadas em três folhas de papel Germitest, umedecida com solução de manitol correspondente a 2,5 sua massa, e levadas a uma câmara de germinação por 10 dias. O feijão foi a cultura com maior sensibilidade ao déficit hídrico, com redução da...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2194

YIELD AND QUALITY OF BELL PEPPER FRUITS IRRIGATED WITH MAGNETICALLY TREATED WATER
Provedor de dados: 196
Autores: Lorenzoni, Marcelo Zolin; Rezende, Roberto; Seron, Cássio de Castro; Souza, Álvaro Henrique Cândido de.
The application of magnetically treated water is a valuable technique for crop irrigation to enhance the yield and quality of agricultural products. This study aims to evaluate the effect of irrigation water depths and the application of water with and without magnetic treatment on the yield and quality of bell pepper fruits in a controlled environment, verifying the effect of magnetically treated water on soil water retention. Two experiments were conducted in the Irrigation Technical Center of the Universidade Estadual de Maringá, Maringá/PR; the first on Summer 2017-2018, and the second on Winter-Spring 2018. A randomized block design with a factorial scheme 3 x 2 with four repetitions was used for the first experiment and a 2 x 2 scheme with six...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6153

SYMPTOMATOLOGY, HOSTS, AND PATHOGENICITY OF Corynespora cassiicola
Provedor de dados: 196
Autores: Caetano, Alicionon de Oliveira; Diniz, Rayane Louise Candida; Lemes, Natanael Marcos; Rietjens, Anderson Rodrigues; Lima, Milton Luiz da Paz.
Many diseases are affecting tomato fruits in the field and greenhouse. The objective of this work was to identify, to verify the symptomatology, pathogenicity and hosts of C. cassiicola causal agent of tomato fruit rot. Symptomatic tomato fruit were isolated in medium agar-water (AW). After 48 hours, the mycelia were replicated on potato-dextrose-agar (PDA) medium. The inoculation was used mycelia discs, for treatments with and without injury, in fruits of tomato, okra, bell pepper, eggplant, zucchini, and noni were present. Both treatments, confirming the aggressiveness and pathogenicity on the original host. Among the other hosts, pathogenicity was confirmed only in okra, bell pepper, and tomato, in treatments with injury only. The comparative analysis,...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1410

EMERGÊNCIA DO BARUZEIRO SOB AMBIENTES PROTEGIDOS E SUBSTRATOS
Provedor de dados: 196
Autores: Oliveira, Letícia Carolina de; Costa, Edilson; Oliveira, Anair Diniz de; Jorge, Marçal Henrique Amici.
O baruzeiro (Dipteryx alata Vog.), esp&amp;eacute;cie arb&amp;oacute;rea de distribui&amp;ccedil;&amp;atilde;o irregular na paisagem do Cerrado, apresenta diversos usos, tanto a planta como os frutos. O trabalho teve como objetivo a avalia&amp;ccedil;&amp;atilde;o de ambientes protegidos e substratos na emerg&amp;ecirc;ncia de pl&amp;acirc;ntulas de Baru, na Universidade Estadual de Mato Grosso do Sul, Aquidauana-MS. Foram utilizados dois ambientes protegidos: estufa agr&amp;iacute;cola com tela termo-refletora sob o filme de polietileno e telado agr&amp;iacute;cola de tela preta (Sombrite&amp;reg;). Foram utilizados 15 diferentes substratos das misturas de esterco bovino, h&amp;uacute;mus, ramas de mandioca e vermiculita. Cada ambiente foi considerado um...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/218

ADIÇÃO DE MOINHA DE CARVÃO E DE STIMULATE® NA FORMAÇÃO DE MUDAS DE Acacia mangium
Provedor de dados: 196
Autores: Carvalho, João Henrique do Nascimento; Lima, Ana Paula Leite; Lima, Sebastião Ferreira.
Considerando que a Acacia mangium é uma importante espécie florestal e a moinha de carvão associada a bioestimulantes tem potencial para melhorar o crescimento e qualidade de mudas, o objetivo deste trabalho foi avaliar o uso da moinha de carvão e de Stimulate® na produção de mudas de Acacia mangium. O experimento foi instalado em esquema fatorial, combinando proporções de moinha de carvão de 0,0, 0,5, 1,0, 1,5 e 2,0 em mistura com 3 partes de solo para 2 partes de areia na composição do substrato, na presença ou não de Stimulate® (15 mL L-1 de água) no tratamento da semente, com 4 repetições, constituída por 12 tubetes cada. Noventa dias após a semeadura, foram avaliados: índice de velocidade de emergência (IVE), massa seca de raiz (MSR), de parte aérea...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2126

FERTILIZANTE FOLIAR EM FEIJOEIRO DE INVERNO E SUA INFLUÊNCIA NA PRODUTIVIDADE E QUALIDADE FISIOLÓGICA DAS SEMENTES
Provedor de dados: 196
Autores: Oliveira, Ítalo Bazzo de; Mendonça, Gabriel Wanderley de; Binotti, Flávio Ferreira da Silva; Ascoli, Alexandre de Araújo; Costa, Edilson.
Aplicação de nutrientes via foliar pode propiciar efeito direto no crescimento do feijoeiro e consequentemente na produtividade e qualidade das sementes. O objetivo foi avaliar nas cultivares BRS pontal e pérola a resposta da aplicação de nutrientes via foliar no crescimento, na produtividade do feijoeiro, além da qualidade fisiológica das sementes produzidas nesses tratamentos. O experimento foi realizado a campo da área experimental da Unidade Universitária de Cassilândia/Universidade Estadual de Mato Grosso do Sul. O delineamento experimental utilizado foi o de blocos casualizados em esquema fatorial 2x4, constituído por cultivares (BRS Pontal e Pérola) e aplicação de fertilizantes via foliar (Testemunha, Adubo foliar 1, Adubo foliar 2 e Adubo foliar 1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nutrição vegetal.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/262

CARACTERIZAÇÃO TÉCNICO-PRODUTIVA DO SISTEMA DE CULTIVO DE PALMA FORRAGEIRA NO CARIRI PARAIBANO
Provedor de dados: 196
Autores: Aires Souza, José Thyago; Nascimento, Maria das Graças Rodrigues do; de Figueredo, Janailson Pereira; Nápoles, Fábio Agra de Medeiros; Andrade, Francisco Hélio Alves de.
Objetivou-se analisar o sistema técnico-produtivo da cultura da palma forrageira (Opuntia ficus-indica Mill) em Taperoá, estado da Paraíba, Brasil. Foi realizada uma pesquisa qualitativa e quantitativa através de questionários no segundo semestre de 2013, envolvendo 50 produtores rurais. 80% dos produtores produzem suas próprias mudas, 66% fazem a primeira colheita após quatro anos de cultivo, 60% não utilizam consórcio, não recebem assistência técnica e não comercializam palma forrageira. O esterco bovino é a fonte de adubação orgânica mais utilizada (54%), 100% não utilizam análise de solo, 74% dos solos cultivados com palma forrageira são argilosos.
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1683

RECUPERAÇÃO DE PASTAGEM DEGRADADA PELO CONSÓRCIO DE MILHO, Urochloa brizantha cv. MARANDU E GUANDU
Provedor de dados: 196
Autores: da Silva, Alex; Santos, Fenelon Lourenço de Sousa; Barretto, Vitor Corrêa de Mattos; Freitas, Roberto José de; Kluthcouski, João.
Objetivou-se com esse trabalho avaliar a viabilidade da recuperação de pastagens degradadas através do banco de sementes presente na área, com a utilização do sistema de consórcio de milho com pastagem com feijão guandu. O delineamento experimental foi em blocos ao acaso, em esquema fatorial 2x3 composto pela utilização ou não do guandu e 3 densidades de semeadura da forrageira (banco de semente – 0 kg ha-1; 2 kg ha-1 e 4 kg ha-1), com 4 repetições. Foram avaliados: o número de espigas por planta, altura de inserção da primeira espiga, altura de plantas, número de fileiras de grãos por espiga, número de grãos por fileira, peso de cem grãos, produtividade do milho, rendimento de biomassa verde do milho, rendimento de biomassa seca do milho, biomassa seca da...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1382

AGRONOMIC PERFORMANCE AND PHOTOSYNTHETICALLY ACTIVE RADIATION INTERCEPTED BY MAIZE INTERCROPPED WITH BRACHIARIA
Provedor de dados: 196
Autores: Makino, Priscila Akemi; Ceccon, Gessi; Ribeiro, Luan Marlon; Ceccon, Felipe.
Maize and soybean are the main crops used for crop yield on Brazilian Cerrado biome. The off-season maize intercropped with ruzigrass [Urochloa ruziziensis (R. Germ. &amp;amp; C.M. Evrard) Crins (Syn. Brachiaria ruziziensis Germ. &amp;amp; Evrard)] increases soil cover and yield for crops in succession. However, the benefits on maize yield depend on the distribution and radiation-use efficiency (RUE) and its conversion to biomass. This study aimed to evaluate maize and ruzigrass yield in different cultivation systems. The experiment was carried out at Embrapa Agropecuária Oeste, in Dourados, MS, Brazil. The experiment design was randomized blocks, with seven treatments constituted by the combination of spacing between maize rows, single and intercropped,...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3624

PRECISION POULTRY FARMING: MAPPING ATTRIBUTES THAT INFLUENCE LAYING BIRDS IN NOVA ANDRADINA/MS
Provedor de dados: 196
Autores: Sorano, Leticia Almeida; Lima, Maycom Dias de; Suszek, Grazieli; Royer, Ana Flávia Basso.
Precision poultry farming is related to effective monitoring of production stages and product quality. This work evaluated the influence of temperature, air humidity, and luminosity variables on chicken egg production and quality (internal and external), under uncontrolled environment and natural lighting, using precision poultry techniques. One hundred and sixty birds of Embrapa 51 line, reared in cages, were assessed with 24, 30, 50, and 70 weeks of life. Values of temperature, relative humidity, luminosity, and the samples for productivity and egg quality determination were collected in predefined locations in a poultry house belonging to IFMS, Nova Andradina/MS Campus. Spatial maps were generated using the inverse distance weighted interpolation (IDW)....
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4961

EFICIÊNCIA FOTOSSINTÉTICA E PRODUTIVA DE MILHO SAFRINHA EM FUNÇÃO DE ÉPOCAS DE SEMEADURA E POPULAÇÕES DE PLANTAS
Provedor de dados: 196
Autores: Santos, Anna Luiza Farias dos; Mechi, Ivan Arcanjo; Ribeiro, Luan Marlon; Ceccon, Gessí.
A pesquisa foi realizada com o objetivo de avaliar os componentes produtivos e variáveis fotossintéticas de plantas de milho cultivadas em quatro épocas de semeadura e quatro populações de plantas. O delineamento experimental foi em blocos casualizados, com parcelas subdivididas e quatro repetições. Nas parcelas foram alocadas as épocas de semeadura do milho safrinha (01 e 15 de fevereiro e 01 e 15 de março) e, nas subparcelas, as populações de plantas (50, 60, 70 e 80 mil plantas ha-1). As maiores taxas fotossintéticas e eficiência de carboxilação da Rubisco foram observadas nas plantas das semeaduras de 15/02 e 15/03. A semeadura realizada em 15/02 e 01/03 resultou na maior massa de 100 grãos e grãos por espiga. Em relação à produtividade de grãos, a...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1631

PRODUTIVIDADE DE FEIJÃO CAUPI CRIOULO EM FUNÇÃO DO ESPAÇAMENTO ENTRE LINHAS E NÚMERO DE PLANTAS POR COVA
Provedor de dados: 196
Autores: Camara, Felipe Thomaz da; Mota, Antônio Marcos Duarte; Nicolau, Francisca Edcarla de Araújo; Pinto, Antônio Alves; Silva, Josefa Maria Franciele da.
O feijão caupi é uma das principais culturas na região nordeste tendo seu cultivo voltado para a produção de grãos ou em vagens verdes. Desta forma, objetivou-se avaliar o desenvolvimento e a produtividade do feijão caupi em grãos e em vagens verdes em função do espaçamento entre plantas e da prática de desbaste na região do Cariri cearense. O experimento foi conduzido no Sitio Pintado, Missão Velha-CE, delineamento em blocos casualizados, em esquema fatorial 2x3, com quatro repetições. O primeiro fator foi o espaçamento entre plantas (0,5; 0,33 e 0,25 m) e o segundo a prática (ou não) do desbaste Quanto ao desenvolvimento e produtividade do feijão verde, avaliou-se a população de plantas, número de vagens por planta, massa de vagens verdes por planta,...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2282

APLICAÇÃO DE BIOESTIMULANTES E Bacillus subtilis NA GERMINAÇÃO E DESENVOLVIMENTO INICIAL DA CULTURA DO MILHO
Provedor de dados: 196
Autores: Buchelt, Antonio Carlos; Metzler, Carlos Renato; Castiglioni, José Lucas; Dassoller, Tiago Ferrarezi; Lubian, Matheus Sergio.
O presente trabalho teve como objetivo avaliar a germinação e o crescimento inicial da cultura do milho em sementes submetidas à aplicação de bioestimulantes (ProGibb 400® e Stimulate®) e de Bacillus subtilis. O experimento foi realizado no laboratório de tecnologia e sementes da Universidade do Estado de Mato Grosso, Campus de Alta Floresta. O delineamento utilizado foi o inteiramente casualizado, com dez tratamentos com quatro repetições de 25 sementes cada. Os tratamentos utilizados foram: Testemunha, ProGibb 400® 1, 2 e 3 com doses respectivas de 25, 50 e 75 mg kg-1 de sementes, Stimulate® 1, 2 e 3 com doses respectivas de 5, 10 e 15 mL kg-1 de sementes e Bacillus subtilis 1, 2 e 3 com doses respectivas de 4, 6 e 8 mL kg-1 de sementes. Os parâmetros...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2762

DETERMINAÇÃO DA UMIDADE DO SOLO POR MICRO-ONDAS E ESTUFA EM TRÊS TEXTURAS DE UM LATOSSOLO VERMELHO-AMARELO DO CERRADO
Provedor de dados: 196
Autores: de Oliveira, Luis Fernando Cunha; Roque, Cassiano Garcia.
O objetivo do trabalho foi estudar a equivalência de tempos de secagem para determinação de umidade do solo em forno micro-ondas comparada ao método padrão (estufa). Tal estudo foi realizado em um Latossolo Vermelho-Amarelo de Cerrado nas classes texturais de 20, 35 e 50% de argila. As amostras de solo foram submetidas a cinco tempos de secagem no micro-ondas (2; 4; 6; 8 e 10 minutos) em comparação com o método padrão (110 ºC/24 h), em um experimento inteiramente casualizado. As análises de regressão dos dados quantitativos apresentaram altos coeficientes de determinação, demonstrando a possibilidade do uso do micro-ondas na determinação da umidade do solo (%) pela rapidez e confiabilidade de resultados em relação ao padrão de estufa.
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1163

EFEITO DE FONTES E DOSES DE NITROGÊNIO NA CULTURA DO RABANETE
Provedor de dados: 196
Autores: Caetano, Alicionon de Oliveira; Diniz, Rayane Louise Candida; Benett, Cleiton Gredson Sabin; Salomão, Leandro Caixeta.
O rabanete é uma Brassicaceae de período curto de cultivo que possui raiz globular comestível, possui vitaminas, nutrientes, fibras e baixa caloria. A cultura apresenta deficiência nutricional, principalmente, de nitrogênio (N) causando menor rendimento de raízes. O objetivo foi avaliar o efeito de fontes e doses de N na cultura do rabanete. O experimento foi realizado em ambiente protegido no Instituto Federal Goiano, campus de Urutaí-GO. O delineamento experimental utilizado foi blocos casualizados, arranjados em esquema fatorial 2 x 5, sendo duas fontes de N (ureia convencional e ureia revestida), cinco doses de N (0, 40, 80, 120 e 160 kg ha-1) e quatro repetições. Cada parcela foi constituída de um vaso com capacidade de 8 L de solo com cinco plantas...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/286

EFEITO RESIDUAL DA GESSAGEM E CALAGEM NA RESISTÊNCIA À PENETRAÇÃO OBTIDA COM DOIS PENETRÔMETROS
Provedor de dados: 196
Autores: Oliveira, Marcela Pacola; Roque, Cassiano Garcia; Borges, Monica Cristina Rezende Zuffo; Oliveira, Roberta Pacola; Nogueira, Kenio Batista.
A resistência do solo à penetração é um dos fatores limitantes para o desenvolvimento das culturas. O objetivo foi avaliar o efeito residual de gessagem e calagem na resistência à penetração medida com o penetrômetro de impacto e o eletrônico em sistema de semeadura direta e convencional, em diferentes sistemas de condicionamento do solo. O delineamento utilizado foi de blocos casualizados com os fatores arranjados em parcelas subdivididas. As parcelas receberam as aplicações de calcário e gesso agrícola (Controle, Calcário (3,563 Mg ha-1), Gesso (2 Mg ha-1), Calcário dose recomendada + Gesso (3,563 Mg ha-1 + 2 Mg ha-1), Calcário metade da dose recomendada + Gesso (1,781 Mg ha-1 + 2 Mg ha-1) e Calcário dobro da dose recomendada + Gesso (7,126 Mg ha-1 + 2...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1208

PRODUCTION OF ORNAMENTAL PYRAMID PEPPER WITH REFLECTIVE MATERIAL ON BENCHES IN DIFFERENT ENVIRONMENTS
Provedor de dados: 196
Autores: Silva, Laura Araújo; Salles, Josiane Souza; Cambui Neto, Luiz Martins; Costa, Edilson; Silva, Abimael Gomes; Cavalcante, Daniele Ferreira; Binotti, Flávio Ferreira da Silva; Zoz, Tiago.
Pepper trees have great ornamental value due to the varied colors of their fruits. Thus, the objective was to evaluate the Pyramid cultivar's production in different cultivation environments using benches with reflective material. The experiment was carried out in two protected environments: a) agricultural greenhouse with 42-50% shade screen under the plastic film and b) agricultural screen with black monofilament screen with 18% shade. Inside the environments, the production system was tested with and without reflective material on the cultivation bench. The experiments were conducted in a completely randomized design, with four replicates and six plants per plot. Joint analysis was used to compare environments. At 45, 60, and 75 days after...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5698

DURAÇÃO DA LUMINOSIDADE E TAMANHO DE RECIPIENTES PARA A PRODUÇÃO DE ALFACE EM HORTAS URBANAS
Provedor de dados: 196
Autores: Pinto, Antônio Alves; Santana, Laudeline Dantas; Camara, Felipe Thomaz da; Rodrigues, Wíctor Állyson Dias; da Silva, Francisco Edson.
A necessidade de consumo de alimentos de melhor qualidade tem conduzido à produção de hortaliças em ambientes domésticos, prática que tem sido denominada de hortas urbanas. Neste estudo foram avaliados os efeitos do volume do recipiente e da duração da luminosidade direta no crescimento e no rendimento das plantas de alface. O trabalho foi realizado no Centro de Ciências Agrárias e da Biodiversidade (CCAB) da Universidade Federal do Cariri (UFCA). O delineamento experimental utilizado foi inteiramente casualizado, em esquema fatorial 2 x 4, com três repetições. Os tratamentos constituíram de dois tempos da duração da luminosidade (4 e 7 horas de sol) e de três tamanhos de recipientes (0,6; 1,2; 1,8 e 3,4 dm³). Foram conduzidos dois experimentos e duas...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1607

COMPATIBILIDADE DE INSETICIDAS UTILIZADOS NA CULTURA DO EUCALIPTO COM Metarhizium rileyi (FARLOW) (=Nomuraea rileyi)
Provedor de dados: 196
Autores: Da Costa, Maiara Amaral; Loureiro, Elisângela De Souza; Pessoa, Luis Gustavo Amorim; Dias, Pamella Mingotti.
Objetivou-se avaliar a compatibilidade dos inseticidas químicos (Orthene® 750 BR, Mospilan®, Imidacloprid® NORTOX e Evidence® 700 WG), sobre o desenvolvimento de Metarhizium rileyi. Os experimentos foram realizados “in vitro”, avaliando os efeitos sobre o crescimento vegetativo, produção de conídios (esporulação) e germinação do fungo M. rileyi (isolado UFMS 03) na presença de diferentes inseticidas. Após a obtenção dos dados de diâmetro de colônias, produção de conídios e germinação foram calculados o fator de compatibilidade. Os inseticidas Mospilan®, Imidacloprid® NORTOX e Evidence® 700 WG proporcionaram crescimento vegetativo semelhante a testemunha, considerados compatíveis com M. rileyi enquanto que Orthene® 750 BR foi considerado moderadamente...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2149

COTTON CULTIVARS X PLANT POPULATION IN MONTIVIDIU, GOIÁS, BRAZIL
Provedor de dados: 196
Autores: Rodríguez de la Torre, Elio de Jesús; Lamas, Fernando Mendes.
This study aimed to evaluate the quantitative and qualitative aspects of production in different populations of cotton cultivars. Ten cultivars were evaluated annually in four plant populations. A randomized block design with split plots and three replicates was used. The cultivars were placed in plots, and the plant populations were placed in the subplots. The following characteristics were evaluated: fiber percentage, fiber yield (kg ha-1), fiber length (mm), the micronaire index, the short fiber index (%), and fiber resistance (gf tex-1). In general, the effect of cultivar was much more important than that of the plant population. These results agree with those obtained by several other authors who have claimed that cotton has a high capacity to adapt...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5451

APLICAÇÃO DE ÁCIDO GIBERÉLICO E PACLOBUTRAZOL NA CULTURA DA SOJA
Provedor de dados: 196
Autores: Cruciol, Giovana Carolina Dourado; Tieme Koyanagui, Marli; Barbosa Batista, Thiago; Ferreira da Silva Binotti, Flávio; Luiza Nunes Costa, Maria.
As giberelinas são associadas à promoção do crescimento do caule e sua aplicação na planta pode induzir a um aumento significativo na sua altura. O paclobutrazol é considerado regulador de crescimento utilizado na agricultura com finalidade de controlar o crescimento vegetativo, estimulando a capacidade reprodutiva das plantas. O objetivo foi avaliar o crescimento, mudanças morfológicas e teor de clorofila foliar A, B e total em plantas de soja, mediante a aplicação de ácido giberélico via foliar e de paclobutrazol via solo. O experimento foi desenvolvido na Universidade Estadual de Mato Grosso do Sul, unidade Universitária de Cassilândia, num delineamento inteiramente casualizado em esquema fatorial de 2 x 2, com aplicação de paclobutrazol via solo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Produção Vgetal.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/234

RELAÇÃO ENTRE VELOCIDADE DE DESLOCAMENTO, RENDIMENTO DA CANA-DE-AÇÚCAR E O CONSUMO DE COMBUSTÍVEL DA COLHEDORA
Provedor de dados: 196
Autores: Martins, Murilo Battistuzzi; Ramos, Carlos Renato Guedes; Souza, Fábio Lopes de; Sartori, Maria Márcia Pereira; Lanças, Kléber Pereira.
A colheita mecanizada de cana-de-açúcar apresenta diversos fatores que imprimem à essa atividade um custo elevado; dentre os principais fatores ressalta-se o consumo de combustível. O presente estudo teve como objetivo avaliar o consumo de combustível de uma colhedora de cana-de-açúcar em função da velocidade de deslocamento e do rendimento da cultura. O trabalho foi realizado em canaviais com produtividade de colmos de 65 e 80 t ha–1, sem a despalha prévia por fogo, com espaçamento entrelinhas de 1,5 m. Utilizou-se uma colhedora de cana-de-açúcar de uma linha, onde foi instalado dois fluxometros, para a medição do consumo instantâneo de combustível. Para aquisição dos dados foi usado um controlador lógico programável (CLP). O delineamento foi inteiramente...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1264

CONTROLE QUIMICO DE CONYZA BONARIENSIS EM DESSECAÇÃO
Provedor de dados: 196
Autores: Leite, Rafael da Costa; Tomquelski, Germison Vital; Guazina, Renato Anastacio; Leal, Aguinaldo Jose Freitas.
A buva (Conyza bonariensis) é uma das principais plantas infestantes no agroecossistema brasileiro, demandando novas alternativas de manejo a cada safra. O objetivo desse trabalho foi avaliar o desempenho de diferentes programas de aplicação de herbicidas na dessecação de área experimental infestada com buva. O experimento foi conduzido em condições de campo, no município de Chapadão do Sul, MS. O delineamento experimental foi em blocos casualizados com 26 tratamentos e quatro repetições. A eficiência de controle dos tratamentos foi determinada pelo método de avaliação visual, atribuindo-se notas em porcentagem de controle. Glufosinato-Sal de Amônio + Óleo Mineral (T21) apresentou a maior eficiência no controle da buva. Os tratamentos, 2,4 D + Glifosato...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantas Daninhas.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/238

COMPARISON OF DIFFERENT MEDIA TO PRODUCE CYMBIDIUM ORCHIDS BY PSEUDOBULBS
Provedor de dados: 196
Autores: Sedaghathoor, Shahram; Golzari Dehno, Gholamreza; Naderi, Rohangiz; Kalatehjari, Sepideh; Kaviani, Behzad.
Nowadays, Orchids are one of the most commercial products in flower markets. One of the propagation methods for Cymbidium is using old pseudobulbs that are thrown out after flowering period. This research carried out using standard Cymbidium back-bulbs based on randomized complete block design with 5 treatments in 3 replications. The trial traits were leaf length, root length, leaf number and root number that were studied for 180 days. The results show that minimum length of root was significant under different growth beds. The minimum percent of rooting was observed in pure sand treatment. The maximum length was observed in pure perlite. The shortest of leaves were gained in perlite + sand treatment and the maximum leaf length was observed in pure perlite...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1701

Impacto de diferentes sistemas de uso no carbono orgânico total e mineralizável do solo sob solo arenoso
Provedor de dados: 196
Autores: Lopes , Giovana Tetsuya; Rosset, Jean Sérgio; Ozório, Jefferson Matheus Barros; Maiane Mendes da Silva, Ozielly; Vieira dos Santos, Wesley; Victor Hugo dos Santos, José; dos Santos Gonçalves, Andrea; Marra, Leandro Marciano.
O objetivo deste trabalho foi avaliar o impacto de diferentes sistemas de uso nos teores e estoques de carbono orgânico total (COT) e a evolução diária e total do carbono mineralizável (C-CO2) em um Argissolo Vermelho Amarelo de textura arenosa. O estudo foi realizado no município de Eldorado, MS, em uma área de referência de Mata Nativa (MN), e em três áreas manejadas: pastagem permanente (PP), semeadura direta (SD) e área de Reserva Particular de Patrimônio Natural em processo de regeneração natural (RPPN). Amostras de solo das camadas 0,0-0,05, 0,05-0,10 e 0,10-0,20 m foram coletadas para avaliação de densidade do solo (Ds), teores de COT, com posteriores cálculos do índice de estratificação (IE), estoque de carbono (EstC) e variação do estoque de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil organic matter; Private Natural Heritage Reserve (PNHR); Conservation unit; Matéria orgânica do solo; Reserva Particular do Patrimônio Natural (RPPN); Unidade de conservação.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6991

EFEITO DO PREPARO DO SOLO COM DIFERENTES IMPLEMENTOS SOBRE A RESISTÊNCIA DO SOLO À PENETRAÇÃO
Provedor de dados: 196
Autores: Monteiro, Mario Augusto Chaves; Zoz, Andre; Limede, Arnaldo Cintra; Oliveira, Carlos Eduardo da Silva; Zoz, Tiago.
O preparo de solo é condição essencial para receber a cultura. A resistência do solo à penetração tem sido um dos parâmetros mais utilizados na avaliação de sua estrutura física. O objetivo deste trabalho foi determinar a resistência do solo à penetração mediante o preparo com diferentes implementos agrícolas. O ensaio foi composto pelo preparo do solo com cinco implementos (grade leve, grade intermediária, subsolador, arado de discos e arado de aiveca). Cada implemento foi utilizado para preparar uma faixa de 10 metros de comprimento por 5 metros de largura. Para a realização das avaliações foi descartado 1,0 metro em cada extremidade da faixa preparada. Foi realizada avaliação de resistência do solo à penetração antes de realizar o preparo do solo e...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1468

PRODUÇÃO E QUALIDADE DE INFLORESCÊNCIAS DE COUVE-FLOR EM FUNÇÃO DA DENSIDADE DE PLANTIO
Provedor de dados: 196
Autores: Ferreira, Nozimary Carneiro; Seleguini, Alexsander; Seno, Shizuo; Faria Júnior, Max José de Araújo.
A couve-flor é uma das hortaliças mais plantadas em todo o Brasil, sendo uma cultura bastante rentável. A utilização de plantios mais adensados pode incrementar a produtividade da cultura e aumentar o retorno financeiro aos produtores. Assim este trabalho objetivou verificar o efeito da combinação de diferentes espaçamentos entre linhas e entre plantas sobre a produtividade e a qualidade de inflorescências de couve-flor ‘Piracicaba Precoce’. Utilizou-se delineamento experimental em blocos casualizados e os tratamentos consistiram na combinação de três distancias entre linhas (70, 80 e 90 cm) com três distancias entre plantas na linha (50, 60 e 70 cm), e quatro repetições. Foi avaliada a produtividade total e por classes de tamanho das inflorescências, bem...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manejo e tratos culturais.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/241

EFFECT OF THE PEEL EXTRACTS FROM TWO CAMPOMANESIA (MYRTACEAE) SPECIES ON ALLIUM CEPA L. (AMARYLLIDACEAE)
Provedor de dados: 196
Autores: Silva, Bruno Araújo; Castro, Thiago Luis Aguayo de; Viana, Lucilene Finoto; Mascarenhas Santos, Maria do Socorro; Cardoso, Claudia Andrea Lima.
Species from the genus Campomanesia have been studied due to their biological activity and low toxicity. However, studies on the fruit peel of these species are scarce. In this context, the effects of ethanol extract from the fruit peel of Campomanesia sessiliflora (O. Berg) Mattos (CS) and Campomanesia guazumifolia (Cambess) O. Berg (CG) were evaluated concerning the effect on germination and meristem cells of roots of Allium cepa. The CG ethanolic extract showed flavonoid compounds higher than CS ethanolic extract. The CS extract showed no antioxidant activity. CS showed greater antiproliferative activity with reduced root size in A. cepa seeds. The two extracts did not induce mutagenicity and cell death at the studied concentration of 1 mg mL-1....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Germination; Allelopathy; Ethanolic extract.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6831

PRODUCTION OF 'FORMOSA' PAPAYA SEEDLINGS IN DIFFERENT PROTECTED ENVIRONMENTS AND ORGANIC SUBSTRATES
Provedor de dados: 196
Autores: Santos, Érica Letícia Leal dos; Silva, Anne Karolyne da; Curi, Thayla Morandi Ridolfi de Carvalho; Costa, Edilson; Jorge, Marçal Henrique Amici.
It is aimed to evaluate the effect of cattle manure, and ground crushed cassava branches based substrates in the growth of 'Formosa' papaya seedlings under different environmental conditions. Four protected environments were tested: greenhouse in arched, covered with polyethylene film with a thermo reflective screen underneath it; similar greenhouse but without the reflective screen; monofilament nursery with 50% shade screen and thermo reflective nursery with 50% shade screen. In the protected environments, seedlings were accomodated in polyethylene bags (15.0 x 25.0 cm) were filled with cattle manure, and ground cassava branches based substrates in the following proportions: 100% cassava branches; 80% cassava branches and 20% cattle manure; 60% cassava...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1107

RESPONSES OF COWPEA CULTIVARS TO SALINE STRESS
Provedor de dados: 196
Autores: Romanoski, Vanessa; de Moura Souza Filho, Paulo Roberto; Badaró Pimentel, Adérico Júnior.
The cowpea [Vigna unguiculata (L.) Walp] is widely cultivated in Northeast Brazil and stands out for its economic and social importance. Part of the cultivation area is affected by salt stress, which affects the performance of the crop. The effects of salinity can be mitigated with the development of tolerant cultivars. The objective of this work was to evaluate the behavior of cowpea cultivars under different levels of saline stress in the germination and emergence phases of the crop. Two trials evaluating the germination and emergence phases were conducted, under controlled conditions, in a factorial scheme with 11 cultivars and five solution of NaCl with concentrations ranging from 0 to 120 mM. There was a marked difference in the response of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vigna unguiculata; Melhoramento genético; Estresse abiótico; Germinação; Emergência; Vigna unguiculata; Genetic improvement; Abiotic stress; Germination; Emergency.
Ano: 2023
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/7230

ALLELOPATHIC EFFECT OF Sorghum bicolor AND Digitaria insularis ON GERMINATION AND INITIAL DEVELOPMENT OF CANOLA
Provedor de dados: 196
Autores: Campos, Thiago Souza; Sousa, Ane Gabriele Vaz; Rego Junior, Jaime Santos do; Sousa, Westefann dos Santos; Benett, Cleiton Gredson Sabin; Arruda, Natália.
Agriculture depends on biotic and abiotic factors, and one of them is allelopathy, defined as the chemical interference that one plant has on others, which can negatively affect germination. The objective of this work is to evaluate the allelopathic effects of Sorghum bicolor and Digitaria insularis on seed germination and initial development of canola seedlings (Brassica napus L.). A completely randomized design was used in a 2x5 factorial scheme (two extracts: D. insularis and S. bicolor) and five concentrations (0, 25, 50, 75, and 100%), with four replicates of fifty seeds, the plot being constituted by a 'gerbox' box containing 50 seeds evenly distributed. The variable analyzed were germination percentage (G), abnormal seedlings (AS), dead seeds (DS),...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4230

DO EXOGENOUS APPLICATION OF THIAMINE MITIGATES LOW SOIL BASE SATURATION EFFECTS ON BELL PEPPER PLANTS?
Provedor de dados: 196
Autores: Vendruscolo, Eduardo Pradi; Dantas Alves, Vitória; Rodrigues Sant'Ana, Gabriela; Pacheco de Almeida Prado Bortolheiro, Fernanda; Battistuzzi Martins, Murilo; de Castro Seron, Cássio; de Souza, Maria Ingrid; Dantas, Thaise.
O uso intensivo do solo para a produção de hortaliças resulta em elevada degradação do solo e da área de cultivo. A utilização de técnicas e recursos que viabilizem a produção sob condições desfavoráveis pode ser decisiva para agricultura. Desta maneira, o objetivo deste trabalho foi avaliar os efeitos isolados e conjuntos da correção do solo e da aplicação de tiamina sobre o desenvolvimento das plantas de pimentão. Os tratamentos foram compostos por três diferentes saturações de base do solo (36, 60 e 80%), combinadas à aplicação de tiamina via foliar (com e sem) na concentração de 100 mg L-1. Verificou-se que a tiamina ameniza os efeitos da baixa saturação por base do solo sobre as características fisiológicas das plantas de pimentão. Os incrementos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carbon fixation; Biostimulants; Soil management; Plant protection; Fixação de carbono; Bioestimulantes; Manejo do solo; Proteção vegetal.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6803

OPERATIONAL PERFORMANCE OF AN AGRICULTURAL TRACTOR UNDER DIFFERENT TIRE INFLATION PRESSURES IN THE SUBSOILING OPERATION
Provedor de dados: 196
Autores: Lopes, Arthur Gabriel Caldas; Correia, Tiago Pereira da Silva; Lima, Gabriel Pastor de Barros; Souza, Isabela Dias de; Taveira, Wesley Matheus Cordeiro Fulgêncio; Pereira, Gabriela Greice.
For the agricultural tractor's best performance, it must be correctly adapted to the job. Among other factors, the adequacy of tire inflation pressure is one of the most important and may influence the operation's efficiency and productivity. This study aimed to evaluate an agricultural tractor's operational performance with different tire inflation pressures in the subsoiling operation. The study was carried out in an experimental area of the Agricultural Machinery and Mechanization Laboratory of the experimental farm “Água Limpa,” belonging to the University of Brasília. The experimental design used was in randomized blocks with the following values, 206.8 kPa (30 psi), 137.9 kPa (20 psi), and 68.9 kPa (10 psi), of inflation pressure for agricultural...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4878

INCIDÊNCIA E CARACTERIZAÇÃO MORFOLÓGICA DE Alternaria alternata EM SEMENTES DE SALSA
Provedor de dados: 196
Autores: Magalhães Barroso, Franciely; Pereira Costa Muniz, Paulo Henrique; Silva Peixoto, Gustavo Henrique; Milan, Mariany Dalila; Costa Carvalho, Daniel Diego.
A queima de alternaria, cujo agente causal é o fungo Alternaria spp., é uma doença ocorrente em áreas de produção de hortaliças da família Apiaceae, devido, principalmente, ao fato de sua veiculação ser por sementes contaminadas. Neste sentido, a qualidade sanitária e fisiológica de sementes é fundamental para o estabelecimento uniforme das culturas em campo, fator que garante o sucesso da produção. O objetivo deste trabalho foi estimar a incidência e caracterizar o fungo Alternaria ocorrente em sementes de salsa cv. ‘Graúda Portuguesa’. A análise de incidência foi realizada pelo método blotter test, empregando-se oito repetições (50 sementes por caixa gerbox). Após 10 dias a 25 ºC e fotoperíodo de 12 h de luz, a avaliação foi realizada examinando-se...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2552

DESENVOLVIMENTO INICIAL E QUANTIFICAÇÃO DE PROTEÍNAS DO MILHO APÓS INOCULAÇÃO COM NOVAS ESTIRPES DE Azospirillum brasilense
Provedor de dados: 196
Autores: Galeano, Rodrigo Mattos Silva; Campelo, Analice Paula de Souza; Mackert, Aline; Brasil, Marivaine da Silva.
O uso indiscriminado de fertilizantes nitrogenados na cultura do milho ocasiona poluição ambiental. A fixação biológica do nitrogênio (FBN) é uma alternativa para a redução desses químicos em campo. Bactérias do gênero Azospirillum estão entre as mais importantes envolvidas na FBN em gramíneas. Portanto, o objetivo do trabalho foi analisar a germinação e o desenvolvimento inicial, bem como quantificar as proteínas totais do milho após a inoculação com diferentes estirpes de Azospirillum brasilense isoladas de gramíneas do Pantanal Sul-Mato-Grossense. O experimento foi inteiramente casualizado com três repetições de 50 sementes para os seguintes tratamentos: testemunha sem inoculação; inoculação com estirpes MAY1, MAY12 e BR-11001; e inoculante comercial...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2613

EFEITO DE FERTILIZANTE FOLIAR SOBRE ISOLADOS DE Sclerotinia sclerotiorum
Provedor de dados: 196
Autores: Putrick, Thayla Christiane; Costa, Maria Luiza Nunes; Theodoro, Gustavo de Faria.
O mofo branco, causado por Sclerotinia sclerotiorum, é uma doença muito importante para muitas culturas agrícolas e seu controle tem sido feito por meio da adoção de medidas de forma integrada. Foi avaliada a ação antifúngica de um fertilizante foliar preparado com óleo essencial da casca de laranja (Orobor N1®: nitrogênio 1%, boro 0,22 %) sobre o crescimento micelial e germinação carpogênica de S. sclerotiorum. Os experimentos foram conduzidos em delineamento inteiramente casualizados, em esquema fatorial, utilizando-se cinco isolados do patógeno e seis concentrações do fertilizante foliar. Na avaliação do crescimento micelial, discos de BDA (6 mm) com micélio fúngico, foram depositados em placas de Petri contendo a mistura de BDA com o produto nas...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1453

CRESCIMENTO E PRODUTIVIDADE DE DOIS CULTIVARES DE SOJA EM FUNÇÃO DE DOSES DE SILÍCIO
Provedor de dados: 196
Autores: Coelho, Paulo Henrique Moreira; Benett, Katiane Santiago Silva; Arruda, Natália; Benett, Cleiton Gredson Sabin; Nascimento, Mariana Vieira.
A utilização de silício na agricultura tem se tornado cada vez mais comum, pois se evidencia a melhoria de funções fisiológicas e sanitárias das plantas cultivadas. O objetivo do trabalho foi avaliar a influência do silício no crescimento e na produtividade de dois cultivares de soja. O experimento foi conduzido na área experimental da Universidade Estadual de Goiás (UEG), Campus Ipameri. O delineamento utilizado foi em blocos casualizados, no esquema fatorial 2 x 6 (cultivares x doses) com quatro repetições. Os cultivares de soja utilizados foram AS 3730 RR2 IPRO (Intacta) e NA 7490 RR. A aplicação das doses de silício (0, 125, 250, 500, 625 e 750 Kg ha-1 de Si) foi realizada no sulco de plantio e a fonte utilizada foi o silicato de cálcio e magnésio em...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2602

ENVELHECIMENTO ACELERADO TRADICIONAL E ALTERNATIVO EM SEMENTES DE MELANCIA
Provedor de dados: 196
Autores: Ribeiro Duarte, Rafaelle; Silva Borges, Renato; Silva  da Costa, Geany Giovana; da Silva, Eliamara Marques; dos Santos, Jessica Morgana.
Este trabalho teve por objetivo avaliar a qualidade inicial das sementes de melancia submetidas aos testes de envelhecimento acelerado tradicional e alternativo. Foram empregados dois procedimentos para o envelhecimento acelerado: tradicional (40 ml de água destilada) e método alternativo [solução saturada de NaCl (40 g do sal/100 mL de água)], sob temperatura de 42 ºC durante 24, 48, 72, e 96 horas. O delineamento utilizado foi inteiramente casualizado, em esquema fatorial (2x4) com quatro repetições. Ao término de cada período, as sementes foram submetidas ao teste de germinação e a avaliação da porcentagem de plântulas normais foi realizada aos cinco dias após a semeadura. Os dados da contagem de germinação foram submetidos à análise de variância e as...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2207

RELAÇÃO ENTRE O ESTÁDIO DE ABERTURA FLORAL E PULSING NA VIDA ÚTIL DO COPO DE LEITE
Provedor de dados: 196
Autores: Sanches, Alex Guimarães; Costa, Jaqueline Macedo; Silva, Maryelle Barros da; Moreira, Elaine Gleice Silva; Cosme, Shirley Silva.
O copo de leite é muito apreciado tanto como flor para uso em arranjos florais bem como em jardins, contudo, os aspectos relacionados à determinação do ponto de colheita e o prolongamento da sua vida útil pós-colheita ainda são bem escassos na literatura. Diante disso o presente trabalho tem por objetivo avaliar a relação entre o estádio de abertura floral das espatas de copo de leite e a sua conservação em solução de pulsing a base de ácido cítrico. Para tanto adotou-se um delineamento experimental inteiramente casualizado em esquema fatorial 3 x 4 x 6; três estádios de abertura floral, quatro concentrações de ácido cítrico e seis tempos de armazenamento com cinco repetições e três hastes por parcela experimental. As análises de qualidade e perda de massa...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1400

INTERFERENCE OF ALDICARB IN INFECTIVE FORMS OF Meloidogyne incognita AND ITS EFFECTS ON REPRODUCTION IN SOYBEAN
Provedor de dados: 196
Autores: da Silva, Esdras Henrique; Campos, Vicente Paulo; Rocha, Fernando da Silva; Zeviani, Walmes Marques; Terra, Willian César; Rigitano, Renê Luís de Oliveira.
The effect of aldicarb on mortality, motility, and reproduction of M. incognita in soybean was studied. The mortality of second-stage juveniles (J2) in aldicarb solution (5 and 50 μg mL-1) was only high at 20 days of exposure, being higher in the concentration of 50 μg mL-1 and lower in control (water). Motility was inversely proportional to the exposure time, and at 20 days of incubation, the number of J2 mobiles was statistically equal for both concentrations evaluated. There was a reduction inversely proportional to the number of galls and eggs per gram of root according to the J2 incubation time in water and aldicarb (5, 10, and 20 days). J2, when incubated in 50 μg mL-1 aldicarb for 5 and 10 days, always provided the same values regarding the number...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4367

PERFORMANCE OF LETTUCE SUBMITTED TO THE ROCK DUST REMINERALIZER AND DOSES OF EFFICIENT MICROORGANISMS
Provedor de dados: 196
Autores: Sousa, Westefann dos Santos; Campos, Thiago Souza; Souza, Ane Gabriele Vaz; Cintra, Pedro Henrique Nascimento; Faria, Layanara Oliveira; Santos, Talles Eduardo Borges dos.
The use of soil remineralizers with efficient microorganisms (EM) can represent an effective and sustainable alternative to improve the growth, development, and yield of cultivated plants. Thus, the present study aimed to evaluate the effect of different doses of EM, in the presence or absence of rock dust (RD), on the development of iceberg lettuce, cultivar Lucy Brown. The design used was completely randomized, arranged in a 2 x 5 factorial scheme, with four replications. The treatments consisted of the presence and absence of RD in the substrate composition, combined with five commercial product doses based on EM (0, 2, 4, 6, and 8 L ha-1). At 30 days after transplanting, root and stem length, head circumference, the number of leaves, stem diameter,...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5526

ESTRUTURA FITOSSOCIOLÓGICA DE UMA ÁREA DE CERRADO NA ESTAÇÃO ECOLÓGICA DE ITAPEVA, SÃO PAULO, BRASIL
Provedor de dados: 196
Autores: Garcia, Celso Augusto; dos Santos, Arnaldo Gonçalves; Barreira, Sybelle.
A Estação Ecológica de Itapeva, SP é uma unidade de conservação administrada pelo Instituto Florestal do Estado de São Paulo e está instalada em uma área de 106,77 hectares. Com o objetivo fornecer subsídios para futuros projetos de manejo do local, bem como conhecer a estrutura da vegetação, foram calculados alguns parâmetros fitossociológicos, utilizando-se a metodologia de pontos quadrantes. Foram amostrados 800 indivíduos, pertencentes a 18 famílias botânicas totalizando 30 espécies. A distância média geral de ponto-planta foi de 1,81 m fornecendo uma área média geral de 3,85 m², sendo a densidade total por área de 2.870 árvores/ha. A família Fabaceae teve o maior número de espécies amostradas (cinco espécies) seguida por Lauraceae (três),...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/261

MUDAS DE CULTIVARES DE PEPINEIRO EM DIFERENTES SUBSTRATOS
Provedor de dados: 196
Autores: Luqui, Laís de Lima; Costa, Edilson; Alves, Ana Carolina; Binotti, Flávio Ferreira da Silva; Cardoso, Eliana Duarte.
A produção de mudas é uma importante fase do processo produtivo, onde plântulas de elevada qualidade podem incrementar a produção. Neste trabalho objetivou-se o estudo de formação de mudas de cultivares de pepineiro em diferentes combinações de substratos. Quatro cultivares, “Verde comprido”, “Aodai”, “Caipira” e “Marketer” foram produzidas em quatro combinações de substratos: “1/3 vermiculita + 1/3 esterco bovino + 1/3 esterco de aviário”; “1/3 ramas de mandioca + 1/3 esterco bovino + 1/3 esterco de aviário”; “1/3 vermiculita + 1/3 ramas de mandioca + 1/3 esterco bovino” e “1/3 vermiculita + 1/3 ramas de mandioca + 1/3 esterco de aviário”. O delineamento experimental utilizado foi o inteiramente casualizado, em esquema fatorial 4x4 com 5 repetições de 5...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/252

PRODUTIVIDADE DE REPOLHO EM FUNÇÃO DE DOSES DE BOKASHI
Provedor de dados: 196
Autores: Xavier, Mariana Caroline Guimarães; dos Santos, Carlos Antônio; Costa, Evandro Silva Pereira; do Carmo, Margarida Goréte Ferreira.
Devido às poucas informações sobre a resposta da cultura do repolho (Brassica oleracea var. capitata) a compostos orgânicos do tipo bokashi, desenvolveu-se o presente trabalho, que teve como objetivo avaliar o efeito de diferentes doses de bokashi (0,0; 5,0; 7,5; 10,0 e 12,5 t ha-1)sobre o seu desenvolvimento e produtividade. Realizou-se ensaio de campo nas condições de Seropédica, RJ, no período de maio a agosto de 2017. Utilizou-se o híbrido Sekai I F1. O composto foi aplicado nas covas de plantio (50%) e em uma adubação de cobertura (50%), aos 38 dias após o transplantio (DAT). Adotou-se o delineamento de blocos ao acaso, com quatro repetições. Colheram-se as plantas aos 75 DAT, onde foram obtidas as seguintes variáveis: diâmetro longitudinal (DL) e...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2372

Controle biológico de Corynespora cassicola e Drechslera triticirepentis
Provedor de dados: 196
Autores: Avozani, Aveline; Tumelero, Andréia Iraci; Baldiga Tonin , Rosane; Denardin, Norimar; Gomes Silva, Abimael; Garcés-Fiallos, Felipe Rafael.
O controle químico é o método mais usado no manejo de doenças em grandes culturas como soja e trigo. No entanto, a alguns anos o controle biológico tem ganhado destaque. Assim, avaliou-se o antagonismo das bactérias Pseudomonas fluorencens, Pantoea aglomerans e Bacillus sp. sobre os fitopatógenos Corynespora cassiicola e Drechslera tritici-repentis, isolados previamente de folhas de soja e trigo, respectivamente. O experimento foi realizado em condições controladas, no Laboratório de Fitobacteriologia da Faculdade de Agronomia e Medicina Veterinária (FAMV), Universidade de Passo Fundo (UPF), Rio Grande do Sul, Brasil. Os tratamentos foram: T1: P. fluorencens + patógeno; T2: P. aglomerans + patógeno; T3: Bacillus spp. + patógeno e T4: patógeno (controle)....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pseudomonas fluorencens; Pantoea aglomerans; Bacillus sp.; Mycelial growth inhibition; Pseudomonas fluorencens; Pantoea aglomerans; Bacillus sp.; Inibição do crescimento micelial.
Ano: 2023
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/7111

DIVERGÊNCIA GENÉTICA ENTRE HÍBRIDOS DE MILHO EM CONDIÇÕES DE DEFICIÊNCIA HÍDRICA
Provedor de dados: 196
Autores: Melo, Aurélio Vaz de; Santos, Valdere Martins dos; Lopes, Tiago Mateus; Dias, Marilene Alves Ramos; Nunes, Helber Veras.
Na obtenção de cultivares adaptados às condições edafoclimáticas de uma determinada região ou estresse específico, é importante que as diferenças entre os cultivares estejam sob controle genético. Diante disso, objetivou-se determinar a divergência genética entre híbridos experimentais de milho (Zea mays) quanto à resistência a condições de seca. Para tal, realizou-se um ensaio em ambiente protegido no delineamento experimental em blocos casualizados, com quatro repetições, sendo os tratamentos dispostos em um arranjo fatorial 28 x 2, em que 28 híbridos experimentais de milho, oriundos do Programa de melhoramento da UFT, foram avaliados em duas condições hídricas (a 20% e a 80% da CC) utilizando metodologia adaptada do lisímetro. Decorridos 20 dias da...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2339

SILVOPASTORAL SYSTEM: A REVIEW REGARDING THE FAMILY AGRICULTURE
Provedor de dados: 196
Autores: Fey, Rubens; Malavasi, Ubirajara Contro; Malavasi, Marlene de Matos.
The Silvopastoral System (SPS) is understood as an interaction between trees, animals and pasture. The knowledge about the component action potentialities and limitations determines the system success or failure. The potentialities that can be highlighted are the heat reduction for animals and the improvement of the forage quality provided by the trees shadows. The reduction of pasture production at degraded systems is a limitation. The SPS is a sustainable option for family properties that produce meat and milk. The economical, social and cultural limitations are a problematic issue for the SPS adoption and it slows down the number of producers implementing it, specially the called family agriculture. The public policy deficiency to improve it, the lack...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistema Silvipastoril.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/265

USO DA PRÓPOLIS E ÓLEO DE NIM NO CONTROLE DOS FUNGOS Lasiodiplodia theobromae E Colletotrichum gloesporioides: PRINCIPAIS PATÓGENOS QUE ACOMETEM OS FRUTOS DA MANGA
Provedor de dados: 196
Autores: Machado, Patricia Pereira; Vieira, Gustavo Haralampidou da Costa; Machado, Rafael Alves.
O estudo foi desenvolvido com o objetivo de determinar a eficácia do extrato etanólico de própolis (EEP) e óleo de nim (Azadirachta indica L.) no controle dos fungos Lasiodiplodia theobromae e Colletotrichum gloesporioides, principais patógenos que acometem os frutos da manga (Mangifera indica L.). O método compreendeu o desenvolvimento colonial desses fungos em meio de cultura batata-dextrose-ágar (BDA), acrescido das referidas substâncias, em diferentes concentrações. O delineamento experimental foi inteiramente casualizado (DIC) em esquema fatorial 2 x 6: dois extratos (própolis e óleo de nim) e seis concentrações de aplicação (0, 4, 8, 16, 32 e 64 mL L-1), com cinco repetições. Paralelo aos testes, foi estabelecido um tratamento com fungicida para...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/653

PLANTABILITY AND INFLUENCE OF THE APPLICATION OF GRAPHITE ASSOCIATED WITH THE CHEMICAL TREATMENT OF SOYBEAN SEEDS
Provedor de dados: 196
Autores: Pereira, Julio César; Marques Filho, Aldir Carpes; Pereira de Souza, Flávia Luize; Arbex Silva, Paulo Roberto.
Brazil stands out among the world's largest soy producers. The uniformity in the deposition of seeds and the correct distribution of plants are important factors for the crop to express its maximum productive potential. The present study aimed to evaluate the influence of the lubricant agent “graphite”, applied during and after the chemical treatment of soybean seeds in function of its longitudinal distribution at different operating speeds. For this purpose, a seeder with mechanical type feeder was used, at three working speeds: 4, 6 and 8 km h-1 and conducted in a strip design, organized in a 2x3 factorial scheme, with two different modes of application of graphite and 3 operating speeds. The results presented showed that the addition of graphite...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5997

ADUBAÇÃO NITROGENADA E POTÁSSICA EM SOJA SOB SISTEMAS DE SEMEADURA
Provedor de dados: 196
Autores: Korber, Angelo Henrique Canan; Pinto, Luana Patricia; Pivetta, Laércio Augusto; Albrecht, Leandro Paiola; Frigo, Késia Damaris de Azevedo.
Atualmente, práticas agrícolas sustentáveis que contribuam para maximizar a produtividade da soja nos diversos sistemas de produção são de extrema importância para o agronegócio da cultura no Brasil. O objetivo deste trabalho foi avaliar o desempenho agronômico da soja em função da adubação nitrogenada e potássica em cobertura, em sistema de semeadura cruzada e simples. Em cada sistema de semeadura foram testadas doses de potássio (K2O) aplicadas de forma isolada ou combinada com nitrogênio (N). Os experimentos foram instalados na safra de 2013/2014 e receberam a aplicação de 0, 20, 40, 60 e 80 kg ha-1 de K2O e/ou N, totalizando quatro experimentos. Todos os experimentos foram delineados em blocos casualizados com quatro repetições. Na colheita foram...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1653

CONTROLE DE Spodoptera frugiperda (Smith, 1797) EM DIFERENTES TECNOLOGIAS Bts (Bacillus thuringienses) NA CULTURA DO MILHO
Provedor de dados: 196
Autores: Barcelos, Paulo Henrique Soares; Angelini, Marina Robles.
O milho geneticamente modificado contendo o gene bt é usado no controle de lepidópteros na cultura do milho. Esse método de controle é bastante eficaz colaborando na preservação do meio ambiente visto que implica na redução da aplicação de inseticidas. Dessa forma, o objetivo do presente trabalho foi estudar o comportamento de diferentes tecnologias de milho geneticamente modificado frente ao ataque de Spodoptera frugiperda, em condições de campo, além de verificar a necessidade de aplicações de inseticidas nos diferentes materiais testados. O delineamento experimental adotado foi em blocos casualizados com 6 tratamentos e quatro repetições. Aos 7, 14, 21 e 28 dias após a emergência (DAE), avaliou-se danos causados por S. frugiperda nas folhas de 25...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1824

MULCHING É UMA OPÇÃO PARA O AUMENTO DE PRODUTIVIDADE DA MELANCIA
Provedor de dados: 196
Autores: Lambert, Ricardo Alexandre; Barro, Leonardo Silva; Carmo, Karoeynne Silva Gomes do; Oliveira, Aldaisa Martins da Silva de; Borges, Andréia Aparecida.
A cobertura do solo com filme plástico (“mulching”) é uma prática agrícola que visa principalmente reduzir a evaporação da água e o aparecimento de plantas daninhas, além de diminuir o uso de herbicida, impedir o contato de frutos e folhas com o solo. Estes benefícios no sistema de produção de melancia podem resultar em menor custo, maior produtividade e qualidade dos frutos produzidos. Neste contexto, objetivou-se com este trabalho avaliar o desenvolvimento, a produtividade e a viabilidade econômica do cultivo de melancia com e sem mulching. O experimento foi conduzido na Estação Experimental do ILES/ULBRA em Itumbiara-GO, utilizando-se a cultivar “Crimson Sweet”. O delineamento experimental utilizado foi o inteiramente casualizado, com dois tratamentos e...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1184

COMBINATION OF Azospirillum brasilense AND Bradyrhizobium japonicum IN THE PROMOTION OF INITIAL CORN GROWTH
Provedor de dados: 196
Autores: Pereira, Gabriel Monteiro Aguiar; Menezes, Renato de Carvalho; Cunha, Marcos Gomes da; Carrer Filho, Renato.
Biological formulations used as inoculants are increasingly present in grasses, especially in corn. Positive results in promoting plant growth, with different associations with diazotrophic bacteria, show these capacities of interaction to act as plant growth regulators, making it a promising alternative with a low environmental impact. Thus, this study aimed to evaluate the efficiency of inoculation and co-inoculation of nodulating and non-nodulating diazotrophic bacteria as promoters of initial growth in corn plants. Therefore, the bacteria Azospirillum brasilense (UFG21 strain), Bradyrhizobium japonicum (commercial product), and their co-inoculation were used in seed treatment. The evaluations consisted of growth measuring of the root system and shoot...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5360

ESPALHAMENTO E TENSÃO SUPERFICIAL DE GOTAS DE SOLUÇÕES COM HERBICIDAS E ADJUVANTES EM FOLHAS DE Digitaria insularis
Provedor de dados: 196
Autores: Cologni Salvalaggio, Adriana; Vilanova da Costa, Neumárcio; Cazzo, Victor Natan; Conradi Junior, Elio; Eckert, Alesson Felipe.
Objetivou-se avaliar a tensão superficial e eficiência do espalhamento de gotas de soluções com herbicidas e adjuvantes em diferentes concentrações em folhas de Digitaria insularis. O delineamento experimental utilizado foi inteiramente casualizado, com quatro repetições. Os tratamentos utilizados foram glyphosate (Roundup Original®, 360 g L-1) na dose de 960 g L-1 e glufosinato-sal de amônio (Finale®, 200 g L-1), na dose de 400 g L-1 com adição dos adjuvantes: óleo mineral (Nimbus®), óleo vegetal (Aureo®) e glicerina (Hygrogem®, subproduto do biodiesel de soja), nas concentrações de: 0,00; 0,08; 0,16; 0,31; 0,63; 1,25; 2,50 e 5,00% (v/v), em folhas de Digitaria insularis. O espalhamento das gotas das soluções foram avaliadas nas faces foliares adaxial e...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1721

HETEROTIC ESTIMATION AND ADAPTABILITY OF TOMATO HYBRIDS FOR FRUIT YIELD AND ITS RELATED TRAITS IN PAKISTAN.
Provedor de dados: 196
Autores: Javed, Ahsan; Akram, Atif; Tabassum, Muhammad Ijaz; Ahmad, Nadeem; Sarwar, Muhammad; Atif, Muhammad Jawaad.
Current study is emphasizing on the estimation of heterosis for different yield attributing traits and adaptability of tomato hybrids. It was performed in the research area of VCRP, HRI, NARC Islamabad during 2018-2019. Crossing was completed among six parents followed by line × tester. The analyzed data depicted significant differences (P ≤ 0.01) among all the characters.Due to desirable high negative heterotic values hybrids Peto-86 × Nagina and Riograndi × Roma were found suitable for breeding early maturing hybrids. For plant height maximum positive heterosis was observed in Riograndi × Nagina, for no. of cluster/plant in Naqeeb × Roma, for traits like flower cluster-1, fruit cluster-1, fruit length &amp;amp; width and single fruit weight in Naqeeb ×...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Heterosis; Heterobeltiosis; Hybrid vigor.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6582

INOCULAÇÃO COM Rhizobium tropici E ADUBAÇÃO FOLIAR COM MOLIBDÊNIO NA CULTURA DO FEIJÃO COMUM
Provedor de dados: 196
Autores: Oliveira, Carlos Alberto Bispo de; Pelá, Gláucia de Mello; Pelá, Adilson.
O feijão comum, em simbiose com a rizobactéria Rhizobium tropici, é capaz de ter a sua exigência de nitrogênio (N) satisfeita com a fixação biológica de nitrogênio (FBN) que por sua vez é afetada pela deficiência de molibdênio (Mo) visto que este nutriente faz parte da enzima nitrogenase, responsável pelo processo. O objetivo deste trabalho foi avaliar a resposta do feijão comum e seus componentes: teor de clorofila, teor de nitrogênio, produtividade de grãos, número de vagens por planta, número de grãos por vagem, peso de mil sementes, matéria fresca da parte aérea (MFPA), matéria seca da parte aérea (MSPA), matéria fresca das raízes (MFR), matéria seca das raízes (MSR), e produção de biomassa da cultura ao uso da inoculação das sementes combinadas com a...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2193

CRESCIMENTO INICIAL DE ESPÉCIES DE UROCHLOA EM FUNÇÃO DA PROFUNDIDADE DE SEMEADURA
Provedor de dados: 196
Autores: Santos, Fenelon Lourenço de Sousa; Melo, Willany Rayany Formiga; Coelho, Paulo Henrique Moreira; Benett, Cleiton Gredson Sabin; Dotto, Marciane Cristina.
A utilização de plantas de cobertura é uma prática cada vez mais adotada por produtores que utilizam o sistema plantio direto (SPD). No entanto, a profundidade de semeadura tem grande importância na implantação de consórcios de culturas anuais de grãos com gramíneas forrageiras, por influenciar diretamente a emergência das plântulas, podendo ser um fator decisivo para o sucesso do sistema de integração lavoura-pecuária (ILP). Objetivou-se, com esse trabalho, avaliar o crescimento inicial de plântulas de Urochloa brizantha cv. BRS Piatã, U. brizantha cv. BRS Paiaguás e U. ruziziensis em razão da profundidade de semeadura. O delineamento experimental utilizado foi inteiramente casualizado, em esquema fatorial 3x5, sendo três espécies e cinco profundidades...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/685

FITOSSOCIOLOGIA DE PLANTAS DANINHAS NA CULTURA DO MILHO SUBMETIDA À APLICAÇÃO DE DOSES DE NITROGÊNIO
Provedor de dados: 196
Autores: Ferreira, Evander Alves; Paiva, Maria Carolina Gomes; Pereira, Gustavo Antônio Mendes; Oliveira, Maxwel Coura; Silva, Enilson de Barros.
O nitrogênio aplicado às culturas pode alterar o comportamento das plantas daninhas. Assim, algumas espécies são favorecidas pela presença de adubos nitrogenados em doses elevadas, e outras se mostram indiferentes. A finalidade deste estudo foi verificar os efeitos de diferentes doses de nitrogênio na dinâmica de plantas daninhas da lavoura durante o ciclo da cultura do milho. Foi testada a influência de doses de nitrogênio sobre o crescimento do híbrido de milho AG8088 YGRR e na dinâmica das plantas daninhas. A comunidade de espécies infestantes da lavoura sofreu alterações na sua dinâmica em função do tempo de amostragem e inserção de técnicas de plantio, assim como o aumento da disponibilidade de nitrogênio na área. A similaridade foi menor quando se...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2710

PHOTOSYNTHETIC EFFICIENCY OF TOMATO PLANTS SUBMITTED TO CALCIUM SILICATE APPLICATION
Provedor de dados: 196
Autores: Coutinho, Pablo Wenderson Ribeiro; Echer, Márcia de Moraes; Guimarães, Vandeir Francisco; Lana, Maria do Carmo; Inagaki, Adriano Mitio; Brito, Tauane Santos; Alves, Thatiane Nepomuceno.
The objective was to evaluate the effect of calcium silicate on the chlorophyll content and gas exchange of two tomato hybrids. The design used was in randomized blocks in a 2x5 factorial scheme, with four replications. The first factor was composed of two tomato hybrids: Ivety and Natália, and the second factor was composed of five doses of calcium silicate (0, 150, 300, 450, and 600 kg ha-1), applied to the substrate before planting the seedlings. Gas exchange: net CO2 assimilation rate (A), leaf transpiration rate (E), stomatal conductance (gs), internal CO2 concentration (Ci), water-use efficiency (WUE), intrinsic efficiency water use (iWUE), and instant carboxylation efficiency (ACi); SPAD index and the levels of chlorophylls a, b, and total were...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4495

BACTÉRIAS FIXADORAS DE NITROGÊNIO E MOLIBDÊNIO NO CULTIVO DO AMENDOIM EM SOLO DO CERRADO
Provedor de dados: 196
Autores: Santos, Diego Muniz da Silva; Bush, Aécio; Silva, Elijanara Raissa da; Zuffo, Alan Mario; Steiner, Fábio.
O uso de práticas agrícolas sustentáveis que otimizem a fixação biológica de nitrogênio (FBN) pela cultura do amendoim são importantes para assegurar elevados níveis de produtividade. Portanto, neste estudo objetivou-se avaliar a eficiência da aplicação de molibdênio e da coinoculação das sementes com Bradyrhizobium japonicum e/ou Azospirillum brasilense na nodulação, no crescimento e na partição de matéria seca das plantas de amendoim (Arachis hypogaea L., cv. IAC Tatu ST). As plantas foram cultivadas em vasos de 5,5 L preenchidos com um solo arenoso do Cerrado e mantidas em casa de vegetação.O experimento foi disposto no delineamento de blocos casualizados em um esquema fatorial 2 × 4, com quatro repetições. Os tratamentos constituíram da aplicação (+Mo)...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2165

ÁCIDO GIBERÉLICO AUXILIA NA SUPERAÇÃO DA DORMÊNCIA FISIOLÓGICA E EXPRESSÃO DE VIGOR DAS SEMENTES DE GRAVIOLA
Provedor de dados: 196
Autores: Rego, Carlos Henrique Queiroz; Cardoso, Fernanda Brito; Cotrim, Mayara Fávero; Cândido, Ana Carina da Silva; Alves, Charline Zaratin.
As sementes de graviola (Annona muricata) apresentam tegumento resistente e impermeável, além de substâncias inibidoras que dificultam a germinação das sementes. Assim, objetivou-se avaliar a contribuição da embebição em ácido giberélico para a superação da dormência e aumento da germinação das sementes de graviola. O delineamento experimental foi inteiramente casualizado, com cinco tratamentos e quatro repetições. As sementes foram escarificadas e em seguida embebidas por 24 horas a 25 ºC em soluções contendo 0; 50; 100; 150 e 200 mg L-1 (ppm) de ácido giberélico. Após este período de embebição as sementes foram submetidas ao teste de germinação, sendo avaliados a porcentagem de germinação, o índice de velocidade e o tempo médio de germinação. As...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2354

AVALIAÇÃO SENSORIAL E ACEITAÇÃO COMERCIAL DO COGUMELO COMESTÍVEL PLEUROTUS FLORIDA
Provedor de dados: 196
Autores: Gonçalves, Andriele de Oliveira Soares; David, Grace Queiroz; da Silva, Mariana Pina; Peres, Walmor Moya; Yamashita, Oscar Mitsuo.
O cogumelo comestível Pleurotus florida, possui características sensoriais que atraem consumidores de todo o mundo. A região de Alta Floresta apresenta características fisiológicas de natureza ideais para o cultivo desse fungo, o que na prática proporciona emprego para comunidade e oferta comercial do produto com custo inferior ao atual. O objetivo dessa pesquisa foi realizar a avaliação sensorial do cogumelo comestível Pleurotus florida e a verificação da aceitação comercial do mesmo. O método utilizado para levantamento de dados foi aplicação de questionário utilizando escala hedônica de 9 pontos para avaliação sensorial do hiratake in natura e cozido, escala de atitude para teste de aceitação e questão direta para intenção de compra. A tabulação dos...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1614

Efeitos do cobre no desenvolvimento e produção de grãos de feijão-caupi em Latossolo Amarelo
Provedor de dados: 196
Autores: dos Santos de Lima, Silvia Kalini; Viégas, Ismael de Jesus Matos; Oliveira da Silva, Alasse; da Silva Conceição, Elane Cristina; Silva, Aline Oliveira da; Albuquerque Gomes, Jhonatah.
This study aimed to evaluate the effects of Cu doses on the development and yield of cowpea bean grains, cultivars BR3 Tracuateua and Canapu, in terms of fertility in a medium texture Oxisol in the eastern Amazon, Brazil. The experiment was carried out in a greenhouse at the Universidade Federal Rural (UFRA), on the Capanema Campus, Pará. The experimental design was a completely randomized arrangement of 5x2 factorial, with five repetitions, where the first factor is the use of five doses (0, 10, 20, 30 and 60 mg dm-3 of Cu) having copper sulfate as a source, while the second factor is the use of cultivars BR3 Tracuateua and Canapu. Cowpea bean cultivars have different behaviors in terms of Cu requirement and cultivar BR3 Tracuateua, in general, is more...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vigna unguiculata (L.); Growth; Micronutriente; Grains; Vigna unguiculata (L.); Crescimento; Micronutriente; Grãos.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6845

SEEDLINGS PRODUCTION AND FRUIT YIELD OF CUCUMBER ON DIFFERENT ORGANIC SUBSTRATES
Provedor de dados: 196
Autores: Luqui, Laís de Lima; Salles, Josiane Souza; Costa, Edilson; Alves, Vitória Carolina Dantas; Souza, Larissa Gabriela Pereira de; Vieira, Mariane Tavares; Salles, Jussara Souza; Souza, Vitória Cristina Di Matheus e.
Demand for agricultural products with zero or reduced amounts of agrochemicals leads to increasingly healthy production alternatives. Thus, seedling formation and fruit yield of three cucumber cultivars were evaluated on different organic substrates in a protected environment. Marketer, Caipira and Verde Comprido cultivars were grown on five substrates: 100% cassava stems + 0% cattle manure; 75% cassava stems + 25% cattle manure; 50% cassava stems + 50% cattle manure; 25% cassava stems + 75% cattle manure and 0% cassava stems + 100% cattle manure. A completely randomized design in a 5 x 3 factorial scheme (5 substrates X 3 cultivars) was used, with six replications of four seedlings in the seedling formation phase and five replications of two plants in the...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3544

Fontes e doses de potássio sobre os componentes da produção na cultura da soja e do sorgo
Provedor de dados: 196
Autores: de Oliveira, Lucas Robson; Fonseca Filho, Marcos Cesar; Montes, Rafael Marangoni; Benett, Katiane Santiago Silva; Benett, Cleiton Gredson Sabin.
Para uma boa produtividade agrícola é fundamental que o solo possua a fertilidade adequada, para disponibilizar os nutrientes exigidos pelas culturas. O objetivo do trabalho foi avaliar o efeito das diferentes fontes e doses de potássio sobre os componentes da produção e produtividades na cultura da soja e na safrinha com a cultura do sorgo. O experimento foi instalado na safra 2018/2019 no campo experimental da Universidade Estadual de Goiás, Unidade Universitária de Ipameri, Campus Sul, no município de Ipameri-GO. O delineamento experimental utilizado foi o de blocos casualizados, arranjados em esquema fatorial 2 x 6, sendo duas fontes de potássio (cloreto de potássio e fonolito) e seis doses de potássio (0; 60; 120; 180; 240 e 300 kg ha-1), com quatro...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertilization; Phonolite; KCl; Yield; Adubação; Fonolito; KCl; Produtividade.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/7016

Tetranychus mexicanus (Acari: Tetranychidae) IN SOURSOP SEEDLINGS IN THE STATE OF MATO GROSSO DO SUL, BRAZIL
Provedor de dados: 196
Autores: Silva, Eliamara Marques; Toscano, Luciana Cláudia; Steiner, Fábio; Maruyama, Wilson Itamar.
Phytophagous mites belonging to the family Tetranychidae are considered pests of a wide range of plant species of agricultural importance in the Annonaceae family. This study aimed to reports the occurrence and attack symptoms of the mite Tetranychus mexicanus (McGregor) (Acari: Tetranychidae) on soursop seedlings (Anonna muricata L.). High mite infestation on the leaves of soursop seedlings was reported in a seedling production nursery made of black Sombrite® screen with 35% restriction of full daylight, located at the State University of Mato Grosso do Sul (UEMS), in Cassilândia, MS, Brazil, during the month of October 2015. Attack symptoms were on the adaxial side of the leaves, whereas mite colonies were located on the abaxial face of the leaves. The...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3579

DIFERENTES DOSES E ÉPOCAS DE APLICAÇÃO DE ZINCO NA CULTURA DA SOJA
Provedor de dados: 196
Autores: Oliveira, Fernando Castro de; Benett, Cleiton Gredson Sabin; Benett, Katiane Santiago Silva; Silva, Luciana Maria da; Vieira, Bruna do Carmo.
A soja é uma das culturas mais importantes do mundo sendo sua produtividade afetada pela deficiência do micronutriente zinco. O presente trabalho teve como objetivo avaliar o efeito de doses e épocas de aplicação de zinco nas características agronômicas da soja, cultivada em solo da região do Cerrado. O delineamento experimental utilizado foi o de blocos casualizados em esquema fatorial 2 x 5, sendo, duas épocas de aplicação (estádio V9 e R1) e cinco doses (0, 3, 6, 9 e 12 kg ha-1 de zinco), com quatro repetições. Avaliou-se teor de zinco foliar, teor relativo de clorofila, altura de planta, diâmetro do caule, altura de inserção da primeira vagem, número de vagens por planta, número de grãos por vagem, número de nós reprodutivos por planta, massa de 100...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2188

YIELD AND DEVELOPMENT OF MUNG BEAN ACCORDING TO THE PLANT DENSITY
Provedor de dados: 196
Autores: Silva, Edvan Costa da; Peixoto, Nei; Arruda, Natália; Ferreira, Natália Cássia de Faria; Oliveira, Luís Augusto Batista de.
The study aimed to determine the optimal population density for mung bean crop by defining row spacing, and number of plants per meter. The experimental design was a randomized block with treatments arranged in a split-plot scheme with four replications. Two row spacings (25 and 50 cm) were allocated in the plots, and six number of plants per meter (4, 8, 12, 16, 20, and 24 plants) were allocated in the subplots. The experimental units had 4.0 m long, and 2.5 m wide, with 4.0 m2 of useful area. In the useful area of plot, plant height, stem diameter, number of pods per plot, pod length, pod width, number of grains per pod, 100-pods weight, 100-grains weight, final plant population, and grain yield were evaluated. Plant height, pod length, pod width, number...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3572

ANÁLISE TEMPORAL DA MICROBACIA MARIANA NO MUNICÍPIO DE ALTA FLORESTA, MATO GROSSO
Provedor de dados: 196
Autores: Bambolim, Amauri; Donde, Abilene Rodrigues.
O uso do sensoriamento remoto tem sido amplamente utilizado por pesquisadores a fim de obter melhores resultados sobre a constante dinâmica da cobertura vegetal. O presente trabalho teve como objetivo realizar uma análise temporal utilizando técnicas de sensoriamento remoto da Microbacia Mariana, localizada no município de Alta Floresta – MT. Foram utilizadas 3 imagens do satélite Landsat 5 sensor TM dos anos de 1990, 2000 e 2010 e uma imagem do satélite Landsat 8 sensor OLI do ano de 2016. Para a classificação das imagens foi utilizado o classificador não supervisionado máxima verossimilhança para a obtenção da classe Floresta e a classe Uso Alternativo do Solo. A análise demonstrou que os anos de 1990, 2000, 2010 e 2016 apresentaram 54%, 25,5%, 27,25% e...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1613

SAMPLE SIZE AND LINEAR RELATIONS IN SLENDER LEAF RATTLEBOX
Provedor de dados: 196
Autores: Cargnelutti Filho, Alberto; Silveira, Daniela Lixinski; Bubans, Valéria Escaio; Osmari, Bruno Fillipin; Somavilla, Felipe Manfio; Ortiz, Vithória Morena; Osmari, Lucas Fillipin.
Objectives of this work were to determine the sample size (number of plants) to estimate the mean of slender leaf rattlebox (Crotalaria ochroleuca) traits and investigate the relations among traits. In an experimental area of 8 m × 20 m (160 m2), at 147 days after sowing, 110 plants were randomly selected. The following traits were evaluated for each plant: plant height, stem diameter, number of nodes, number of leaves, leaf fresh matter, stem fresh matter, shoot fresh matter, leaf dry matter, stem dry matter and shoot dry matter. Measures of central tendency, variability, skewness and kurtosis were calculated. Normality was verified using the Kolmogorov-Smirnov test and the sample size was calculated to estimate the mean of the traits, assuming estimation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Crotalaria ochroleuca; Sample sizing; Experimental precision; Correlation; Path analysis; Crotalaria ochroleuca; Dimensionamento amostral; Precisão experimental; Correlação; Aanálise de trilha.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6834

BIOECONOMIC PERFORMANCE OF A FEEDLOT BULL WITH DIFFERENT GENETIC GROUPS
Provedor de dados: 196
Autores: da Silva Maia, Janaína Teles; Gonçalves, Thaís Lopes; David, Guilherme De; Domingues, Felipe Nogueira; Oaigen, Ricardo Pedroso.
Livestock systems require a thorough analysis of zootechnical and financial indicators. In this sense, the objective of this study was to evaluate the bioeconomic performance of feedlot bulls with different genetic groups in 2012 and 2013. The experiment was carried out on a farm in Paragominas, State of Pará. The confined animals belonged to the Nellore (NE), ½ Angus ½ Nellore (AN) and ½ Charolais ½ Nellore (CH) breeds. The indicators analyzed were the cost of production and economic indicators. Additionally, zootechnical indicators were evaluated, being considered NE, AN, and CH as treatments in a completely randomized design. The financial results of the total production cost were R$ 118,493.21 in 2012, and R$ 111,166.35 in 2013, and the profitability...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4578

EFEITO DE DOSES DE SILÍCIO NA RESISTÊNCIA DO FEIJOEIRO A Spodoptera frugiperda
Provedor de dados: 196
Autores: Rodrigues, João Hermes Vilela; Angelini, Marina Robles; Oliveira, Reinaldo Silva de; Queiroz, Angélica Araújo.
O presente trabalho objetivou verificar os efeitos das diferentes doses de silício na resistência do feijoeiro à Spodoptera frugiperda. O delineamento adotado foi inteiramente casualizado com quatro tratamentos e cinco repetições. Os tratamentos foram representados pelos níveis de silício: 0 kg ha-1; 50 kg ha-1; 100 kg ha-1 e 200 kg ha-1, sendo o silicato de potássio aplicado ao solo com a adubação de plantio. Avaliou-se o desenvolvimento larval, o período pupal, a biomassa de pupas e a não preferência alimentar de larvas do primeiro ínstar. O maior acúmulo de silício foliar no feijoeiro foi observado para a dose de 111.1 kg ha-1 de silício. A sobrevivência larval de S. frugiperda não foi afetada pela adubação de plantas de feijoeiro com silício. Porém, o...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2496

RELATIVE CHLOROPHYLL INDEX OF MAIZE AND SOYBEAN ACCORDING TO WEATHER CONDITIONS AT DIFFERENT TIMES OF DAY
Provedor de dados: 196
Autores: Silva, Luciana Maria da; Oliveira, Lucas Robson; Rodrigues, Fabrício; Benett, Katiane Santiago Silva; Benett, Cleiton Gredson Sabin.
The present study aimed to identify the best day time to evaluate the relative chlorophyll index in maize and soybean crops as a function of weather conditions. The experiments were conducted in the 2018/2019 harvest, in January and February, in the experimental area of the State University of Goiás, Ipameri University Unit, in Ipameri-GO. A completely randomized design with three replications and 40 plants per plot was used. The measurements of relative chlorophyll index at 7:00, 10:00, 13:00, 16:00, and 19:00, at the maize stage R1 (silking) and soy stage R2 (full bloom), were evaluated. The replications consisted of alternating days over seven days. The relative chlorophyll index, leaf temperature, air temperature, and relative humidity, and light...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5058

AGROCLIMATIC RISK ZONING FOR GUAVA (Psidium guajava L.) IN PARANÁ RIVER BASIN 3
Provedor de dados: 196
Autores: Caldana, Nathan Felipe da Silva; Nitsche, Pablo Ricardo; Martelócio, Alan Carlos; Ferreira, Luiz Gustavo Batista; Caramori, Paulo Henrique; Martins, Jorge Alberto.
Fruticulture constitutes an important sector of the Brazilian agricultural industry. Despite technological and scientific advances, climate is still the most important variable defining crop productivity. Because of this, agroclimatic zoning should be one of the first factors to consider when starting to plant a particular crop. The objective of this work was to conduct climate risk zoning for guava (Psidium guajava L.) in Paraná river basin 3, Paraná, Brazil, using meteorological data from 43 stations collected between 1976 and 2018. The climate risk analysis was based on the climatic factors that impact the species, such as rainfall, annual water deficit, average annual temperature, coldest month temperature, and risk of frost. The findings of this study...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4025

EFFECTS OF 24-EPIBRASSINOLIDE ON GERMINATION AND GROWTH OF TOMATO SEEDLINGS UNDER SALT STRESS
Provedor de dados: 196
Autores: Maia Júnior, Sebastião de Oliveira; Andrade, Jailma Ribeiro de; Lima, Robson Felipe de; Guimarães, Rafaela Félix Basílio; Souza, Allesson Ramos de; Nascimento, Ronaldo do.
Salinity is one of the environmental stresses that most affects plants' vital processes, especially germination. Brassinosteroids, including 24-epibrassinolide (EBL), have multiple actions in essential processes in plants. Thus, this research's objective was to evaluate the effects of EBL on tomato seeds' physiological conditioning on germination, growth, and production of dry seedling mass under salinity conditions. The experiment was carried out in a 2x5 factorial scheme, as follows: two concentrations of EBL (0 and 10-6 M) and five levels of salinity (0.5 control; 1.5; 3.0; 4.5 and 6.0 dS m-1), consisting of ten treatments, with four replications of 50 seeds. In isolation, the salt stress reduced the percentage of germination and germination speed index...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4842

DIVERSIDADE GENÉTICA EM GENÓTIPOS DE MILHO DE PLANTIO TARDIO SOB DIFERENTES NÍVEIS DE NITROGÊNIO NO TOCANTINS
Provedor de dados: 196
Autores: Leite Silva, Karen Cristina; Ferreira dos Santos, Weder; Sérgio Afférri, Flávio; Mucci Peluzio, Joenes; Ferreira Sodré, Layanni.
O estudo da diversidade genética é importante para os programas de melhoramento genético, pois a variabilidade existente entre os genótipos é uma estratégia para obter ganhos de seleção nos cruzamentos. Objetivou-se com este trabalho avaliar a divergência genética de genótipos de milho com uso de dados de seis ensaios na Região Central do Estado do Tocantins, distribuídos em duas épocas de semeadura (21/01/2014 e 19/02/2014). Em cada época, os ensaios foram realizados sob condições de alto, médio e baixo fornecimento de adubação nitrogenada de cobertura. Na aplicação da técnica de agrupamento dos genótipos, foi adotada a distância generalizada de Mahalanobis (D2) como medida de dissimilaridade. Os genótipos 7 e 10 foram produtivos e apresentaram maior...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2327

ANALISE FÍSICO-QUÍMICA DE FRUTOS DE ACHACHAIRU COLETADOS EM DIFERENTES PARTES DA PLANTA
Provedor de dados: 196
Autores: Melo, Márcio Silva; Benett, Cleiton Gredson Sabin; Melo, Bruno Silva; Lourenço, Samara Leticia Oliveira; Barboza, Frederico Severino.
O achachairu, também conhecido como mangostinho, é originária da Bolívia cujo nome científico é Garcinia humilis, pertence à família Clusiaceae. O presente trabalho teve como propósito avaliar a qualidade físico-química de frutos de achachairu em diferentes partes da planta. O experimento foi conduzido no laboratório da Universidade Estadual de Goiás, Câmpus Ipameri, localizado no município de Ipameri-GO. O delineamento experimental utilizado foi o inteiramente casualizado, com três partes de coleta de frutos na planta (superior, mediana e base), sendo cada repetição constituída de três plantas. Os frutos de mangostinho foram utilizados de árvores provenientes do pomar da própria área experimental do Câmpus. Foram realizadas as seguintes avaliações físicas...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2189

Editorial v. 3, n. 3, jul-set. 2016
Provedor de dados: 196
Autores: Costa, Edilson.
Editorial v. 3, n. 3, jul-set. 2016
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1215

INFLUENCE OF SOYBEAN SEED MOISTURE CONTENT IN THE RESPONSE TO SEED TREATMENT IN SOYBEAN
Provedor de dados: 196
Autores: Dias, Marcos Altomani Neves; Urano, André Kitaro Mocelin; da Silva, Deborah Bueno; Cicero, Silvio Moure.
Seed treatment (ST) is an important practice for soybean crop. This research had the objective to evaluate the influence of seed moisture content in the response to different spray volumes (SV) used for seed treatment in soybean, considering effects on seed physiological quality. Three seed lots with distinct moistures were used: 7.2%, 10.1% and 13.0%. Untreated seeds (control) and three SV were tested: 8, 13 and 18 mL kg-1. All lots received the same treatment combination, containing insecticide, fungicide, fertilizer and biostimulant. This combination represented 8 mL kg-1 of SV; the doses of 13 and 18 mL kg-1 were obtained by adding 5 and 10 mL kg-1 of water, respectively. Evaluations of seed physiological quality consisted of electrical conductivity,...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1415

QUALITY OF CUCUMBER SEEDLINGS GROWN IN DIFFERENT CONTAINERS
Provedor de dados: 196
Autores: Mello, Bruna Finotii Fonseca Reis de; Trevisan, Mateus Vieira; Steiner, Fábio.
The use of high quality seedlings is a key factor for the success of vegetable production, and the container size and design characteristics of the containers are important determinants of seedling quality. A experiment was conducted to investigate the effects of different container types on quality of cucumber seedlings (Cucumis sativus L., cv. Aodai Melhorado). Seedlings were grown in a seedling nursery with shadow protection at 50% in different containers: (i) 128-cell trays; (ii) 64-cell trays; (iii) tubes of 120 cm3; and (iv) plastic cups of 180 cm3. The plant height, diameter, root length, shoot dry matter, root dry matter, sturdiness quotient (SQ), shoot:root dry matter ratio (SRR) and Dickson quality index (DQI) were measured at 21st days after...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/820

ELABORAÇÃO E AVALIAÇÃO SENSORIAL DE SORVETE DIET E SEM LACTOSE DE MANGABA ENDÊMICA DO CERRADO
Provedor de dados: 196
Autores: Almeida, Ana Beatriz da Silva; Ferreira, Monica Aparecida Campos; Barbosa, Thaís Alves; Siqueira, Ana Paula Silva; de Souza, Eli Regina Barboza.
A mangaba é um fruto do cerrado, rica em ferro e fonte de vitamina C mas com alta perecibilidade. Com o objetivo de reduzir os desperdícios e aumentar o processamento desse fruto, foi elaborado um sorvete a partir da polpa do fruto, em uma formulação integral e em outra sem lactose e diet, para atender a consumidores com restrições alimentares. Os sorvetes foram analisados quanto ao pH, sólidos solúveis, acidez titulável e derretimento. E submetidos a análise sensorial por 30 provadores, que mostraram aceitação de ambos, mesmo sendo possível detectar diferença entre eles.  A produção de sorvetes é viável para aumentar o processamento de mangaba e evitar desperdícios
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1206

PERDAS OCORRIDAS NA COLHEITA DO MILHO EM FUNÇÃO DO TEOR DE ÁGUA DOS GRÃOS NA COLHEITA
Provedor de dados: 196
Autores: Galindo, Fernando Shintate; Zocoler, João; Teixeira Filho, Marcelo; Buzetti, Salatier; Alves, Cleiton; Santini, José.
A utilização de métodos de fácil aplicação e com resultados rápidos na determinação do teor de água nos grãos é importante para que os produtores de milho possam decidir o momento correto para realização da colheita, com redução das perdas na produtividade de grãos com a secagem natural a campo. Objetivou-se estudar o teor de água dos grãos na colheita da cultura do milho, para a melhor produtividade e os melhores componentes produtivos, bem como para as menores perdas com a secagem natural a campo. O delineamento experimental foi o de blocos ao acaso com quatro repetições, e os tratamentos consistiram na colheita nos seguintes teores de água em base úmida (b.u.) dos grãos: 28,9 (ponto de maturidade fisiológica plena); 23,5; 21,9; 18,9; 16,1; e 13,8%....
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2742

DEPENDÊNCIA ESPACIAL DO RUÍDO DE TRATORES AGRÍCOLAS EM DIFERENTES ROTAÇÕES DO MOTOR
Provedor de dados: 196
Autores: Spadim, Emanuel Rangel; Marasca, Indiamara; Batistuzzi, Murilo Martins; Denadai, Marcelo Scantaburlo; Guerra, Saulo P. Sebastião.
Diversos elementos afetam a saúde do trabalhador, sendo o ruído um importante fator causador de estresse e prejudicial aos operadores expostos por muitas horas à tais ruídos elevados. O objetivo do trabalho foi de quantificar e dimensionar a amplitude dos valores de ruído em diferentes rotações de dois tratores agrícolas. O ensaio foi realizado nas dependências do Núcleo de Ensaio de Máquinas e Pneus Agroflorestais, Faculdade de Ciências Agronômicas, UNESP de Botucatu/SP. O ruído foi mensurado com um decibelímetro marca Icel modelo DL-4200. Utilizou-se dois tratores de 78 cv de potência. As rotações escolhidas foram a rotação de 2200 rpm e a de 2400 rpm. Os valores de ruído foram analisados por geoestatística. Para a construção dos mapas temáticos,...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/270

HYDROCOOLING EFFICIENCY ON POSTHARVEST CONSERVATION AND QUALITY OF ARUGULA
Provedor de dados: 196
Autores: Moreira, Elaine Gleice Silva; Basílio, Scarlet Aguiar; Milan, Mariany Dalila; Arruda, Natália; Benett, Katiane Santiago Silva.
Arugula is mainly cultivated by small producers, being a leafy vegetable susceptible to water loss and wilting after harvest, which may result in changes in appearance, texture, color (yellowing), and nutritional value of the product. Hydrocooling is a cooling method that stands out for being simple, practical and efficient. Its use is to reduce the temperature and respiratory rate of vegetables after harvesting by immersion in ice or cold water, so they can be packed and stored. This study was conducted to evaluate the hydrocooling efficiency when associated with the storage period in the postharvest shelf life of arugula leaves. Arugula leaves were subjected to ten days of storage, and measurements were taken at 0, 2, 4, 6, 8 and 10 days. The...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3457

ÓLEO ESSENCIAL DE Mentha spicata REDUZ O CRESCIMENTO INICIAL DE Corynespora cassiicola in vitro
Provedor de dados: 196
Autores: Silva, Abimael Gomes; Souza, Ana Caroline de; Lopes, Beatriz Garcia; Silva, Eliamara Marques da; Vieira, Gustavo Haralampidou da Costa.
O uso de fungicidas sintéticos é uma das estratégias de manejo de doenças mais utilizadas na agricultura, porém, busca-se manejos que sejam mais sustentáveis. Dessa forma, objetivou-se avaliar o potencial de óleos essenciais de Cedrela fissilis e Mentha spicata no controle, in vitro, do crescimento micelial do patógeno Corynespora cassiicola. O trabalho foi desenvolvido no Laboratório de Fitossanidade da Universidade Estadual do Mato Grosso do Sul (UEMS), Unidade Universitária de Cassilândia-MS. Os óleos essenciais, Cedro (Cedrela fissilis) e Hortelã (Mentha spicata) foram adquiridos comercialmente. O delineamento experimental utilizado foi inteiramente casualizado, em esquema fatorial 2 categorias de óleos essenciais (hortelã e cedro) x 5 concentrações...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phytopathology; Fungicide resistance; Alternative control; Fitopatologia; Resistência a fungicidas; Controle alternativo.
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6375

CONSERVAÇÃO DOS RESÍDUOS DA PODA DE OLIVEIRAS NA FORMA DE SILAGEM
Provedor de dados: 196
Autores: Echeverria, Antônio Dias; Bremm, Tainara; Tadielo, Leonardo Ereno; Altermann, Othon Dalla Colleta; Castagnara, Deise Dalazen.
Por meio de um delineamento inteiramente casualizado procedeu-se a caracterização nutricional de resíduos da poda de oliveiras mantidos in natura ou conservados na forma de silagens durante 110 e 150 dias. Estudou-se o perfil fermentativo por meio da determinação do conteúdo de matéria seca (MS), pH e nitrogênio amoniacal (N-NH3). A MS elevou-se de 487 para 535 g kg-1 com a ensilagem, enquanto o pH não foi afetado pela ensilagem (4,77) e o N-NH3 elevou-se de 5,24 para 6,09% do nitrogênio total. No perfil microbiológico estudaram-se as populações de fungos filamentosos, Lactobacillus, enterobactérias e Clostridium, que apresentaram aumento com a ensilagem. No perfil bromatológico determinou-se os conteúdos de cinzas, matéria orgânica (MO), proteína bruta...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/271

PROPRIEDADES FÍSICAS DE SEMENTES DE BARU EM FUNÇÃO DA SECAGEM
Provedor de dados: 196
Autores: Oliveira, Letícia Carolina; Costa, Edilson; Cardoso, Eliana Duarte; Binotti, Flávio Ferreira da Silva; Jorge, Marçal Henrique  Amici.
O conhecimento das propriedades f&amp;iacute;sicas das sementes s&amp;atilde;o informa&amp;ccedil;&amp;otilde;es que auxiliam o dimensionamento de m&amp;aacute;quinas de pr&amp;eacute;-processamento, processamento e classifica&amp;ccedil;&amp;atilde;o das mesmas. O experimento teve o objetivo de efetuar a caracteriza&amp;ccedil;&amp;atilde;o das propriedades f&amp;iacute;sicas de sementes de Baru (Dipteryx alata. Vog.), provenientes da regi&amp;atilde;o de Sidrol&amp;acirc;ndia-MS. Foram avaliados 4 tratamentos: T1 = sementes n&amp;atilde;o secadas; T2 = sementes secadas em estufa de circula&amp;ccedil;&amp;atilde;o for&amp;ccedil;ada de ar por 48 horas &amp;agrave; 40 &amp;deg;C; T3 =&amp;nbsp; sementes secadas em estufa de...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/223

ELECTRICAL CONDUCTIVITY TEST IN Melanoxylon brauna SCHOTT. SEEDS (FABACEAE-CAESALPINIOIDEAE)
Provedor de dados: 196
Autores: Ataíde, Glauciana da Mata; Borges, Eduardo Euclydes de Lima; Flores, Andressa Vasconcelos.
The electrical conductivity test is a simple and rapid method for evaluating seed vigor. The aim of the present study was to optimize the electrical conductivity test for assessing the vigor of Melanoxylon brauna seeds by investigating the effects of seed number (25, 50, or 75), water volume (25, 50, or 75 mL), and soaking duration (24, 48, or 72 h). The seeds belonged to two lots (I and II) that were collected in 2010 and 2012, respectively, and were incubated in a germination chamber at 25 ºC. Electrical conductivity was determined using a conductivity meter Micronal model B220. The Lot II seeds performed better, in terms of vigor and germination, than the Lot I seeds, regardless of other parameters. In addition, electrical conductivity decreased with...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1878

QUALIDADE MICROBIOLÓGICA E FÍSICO-QUÍMICA DE QUEIJO MINAS FRESCAL ARTESANAL E INDUSTRIAL
Provedor de dados: 196
Autores: Dias, Bruna Ferreira; Ferreira, Suzane Martins; Carvalho, Vania Silva; Soares, Dayana Silva Batista.
A produção de queijos é uma forma apropriada de conservar o leite, transformando-o em produto mais estável, cujas qualidades são mantidas. No comércio são encontrados queijos Minas frescal nas comercializados industrial e artesanal, e fazem parte da tradição alimentar de todo país, atingindo todas as classes sociais. O presente trabalho avaliou as características físico-químicas, analisou a rotulagem e verificou as condições higiênico sanitárias quanto presença de Salmonella spp; contagem de Staphylococcus aureus, de coliformes termotolerantes e totais de queijos Minas frescal, produzidos industrialmente e artesanalmente na região Sul do estado de Goiás. Foram utilizadas 5 amostras de queijos industrializados, 5 de queijos artesanais comercializados em...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1211

EFFECT OF SILVER NANOPARTICLES, SPERMINE, SALICYLIC ACID AND ESSENTIAL OILS ON VASE LIFE OF Alstroemeria
Provedor de dados: 196
Autores: Langroudi, Motahareh Ershad; Hashemabadi, Davood; Kalatejari, Sepideh; Asadpour, Leila.
In this study, effects of different concentrations of silver nanoparticles (NS), salicylic acid (SA), spermine (SP), dill (AN), and cumin (CM) essential oils are investigated on physiological and microbiological traits of alstroemeria (Alstroemeria hybrida) cut flowers during a preharvest and postharvest application. The study was performed as a factorial experiment based on a randomized completely design with three replications. During the experiment the vase life of cut flower was evaluated in terms of chlorophylls a, b and total, SOD, MDA, stem end bacterial colonies and bacterial identification. The results showed that using high concentrations of nanosilver (NS2) increased significantly the vase life of cut Alstroemeria in preharvest and postharvest....
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2366

CINÉTICA DE SECAGEM E AVALIAÇÃO FÍSICO-QUÍMICA DE FRUTA-PÃO (Artocarpus altilis) VARIEDADE SEMINÍFERA
Provedor de dados: 196
Autores: Resende, Kalline Kelly Oliveira; Silva, Sumária Sousa e; Guedes, Sumaya Ferreira; Loss, Raquel Aparecida.
O presente trabalho teve como objetivo realizar a secagem da fruta-pão variedade Seminífera e avaliar os parâmetros físico-químicos da fruta in natura e desidratada (farinha). As frutas foram separadas em partes (polpa, semente, caroço e casca) e submetidas às análises de umidade, pH, acidez, cinzas, e também foi determinado o teor de amido. Para realização da cinética de secagem, utilizou-se estufa com circulação forçada de ar e os dados foram analisados com modelos matemáticos. Os resultados mostraram que na fruta in natura o maior teor de umidade e cinzas foi encontrado no caroço, com 89% e 9,33%, respectivamente. Já na forma de farinha, a parte que apresentou o maior teor de umidade e cinzas foi a polpa. No geral, a fruta apresentou pH ácido, tanto in...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2665

SCARABAEIDAE PRAGAS EM SUCESSÃO DE SOJA E ALGODÃO EM CAMPO NOVO DOS PARECIS, MT
Provedor de dados: 196
Autores: Rodrigues, Sérgio Roberto; Pereira, Alex Furquim.
O Estado de Mato Grosso possui as maiores &amp;aacute;reas cultivadas com soja e algod&amp;atilde;o e face &amp;agrave;s extensas &amp;aacute;reas cultivadas v&amp;aacute;rias s&amp;atilde;o as esp&amp;eacute;cies de pragas que ocorrem, incluindo os cole&amp;oacute;pteros fit&amp;oacute;fagos da fam&amp;iacute;lia Scarabaeidae. Assim, foram desenvolvidos estudos para conhecer as esp&amp;eacute;cies de Scarabaeidae ocorrentes no sistema de sucess&amp;atilde;o de cultura de soja e algod&amp;atilde;o em Campo Novo dos Parecis, MT. Para obten&amp;ccedil;&amp;atilde;o dos imaturos foram realizadas amostragens em janeiro de 2011, na cultura da soja, em abril na cultura do algod&amp;atilde;o, em julho quando a &amp;aacute;rea estava em pousio e na cultura da soja...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/220

TESTE DE CONDUTIVIDADE ELÉTRICA PARA DIFERENCIAÇÃO DOS NÍVEIS DE DETERIORAÇÃO DE SEMENTES DE FORRAGEIRAS
Provedor de dados: 196
Autores: Pinto, Adriana Hernandes; Binotti, Flávio Ferreira da Silva; Souza, Hugo Manoel; Batista, Thiago Barbosa; Gouveia, Geraldo Candido Cabral.
O teste de condutividade elétrica destaca-se por gerar respostas rápidas para diferenciação de lotes em diferentes níveis de deterioração. No entanto, necessita-se de novos estudos visando o aprimoramento desta prática para espécies forrageiras, como Brachiaria brizantha e Panicum maximum. O objetivo foi adequar o teste de condutividade elétrica para determinação do nível de deterioração de sementes de B. brizantha cv. MG-5 e de P. maximum cv. Tanzânia. O delineamento experimental foi inteiramente casualizado e os tratamentos dispostos em esquema fatorial 3 x 3, sendo três níveis de deterioração e três períodos de embebição (8, 16 e 24 horas) à 25 ºC, com 6 repetições. Avaliou-se a condutividade elétrica em três volumes de água da solução de embebição (25,...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1070

PRODUÇÃO DE MANDIOQUINHA-SALSA (Arracacia xanthorrhiza Bancroft) SUBMETIDAS A QUATRO ÉPOCAS DE PLANTIO
Provedor de dados: 196
Autores: Biesdorf, Elivelton Maciel; Biesdorf, Evandro Marcos; de Araújo, Eliezer Melisário; Costa, Eunápio José Oliveira; de Oliveira, Osvaldo José.
O presente trabalho objetivou avaliar o efeito de diferentes épocas de plantio de mandioquinha-salsa Arracacia xanthorrhiza Bancroft, nas condições da região sul Mato-grossense. Testaram-se quatro épocas de plantio a campo, em canteiros, de mudas pré-brotadas: plantio na data 0 (na primavera (22/09/2014)), 90 dias após a data 0 (no verão (22/12/2014)), 180 dias após a data 0 (no outono (21/03/2015)) e 270 dias após a data 0 (no inverno (22/06/2015)). O delineamento utilizado foi o de blocos casualizados com quatro tratamentos e seis repetições. Foi efetuada a colheita aos 270 dias após o plantio. Foram avaliados, na colheita, o número de folhas (NF), matéria seca da planta inteira (MSPI), altura das plantas (AP), massa seca da parte aérea (MSPA) e...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1366

BUSH SNAP BEAN GENOTYPES UNDER CONVENTIONAL AND ORGANIC CULTIVATION
Provedor de dados: 196
Autores: Vidal, Valdivina Lúcia; Assunção , Aracelle; Coelho, Marcos; Nascimento Sales, Raimunda; Peixoto, Nei.
Snap bean is a species widely cultivated in Goiás, in which cultivars of indeterminate growth are used in a staking system. Considering the high cost of staking and the unavailability of a workforce, there has been a demand for bush cultivars, but little is available on the market. In this sense, the present study was developed to evaluate, in 2016, under the conventional and organic cultivation systems, in Anápolis-GO, the behavior of 20 bush snap bean genotypes. The experimental design was randomized blocks, with 20 treatments and three replications. There was a significant interaction between genotypes and cultivation systems for vigor, average pod mass, number of pods per plant, and pod yield, evidencing that the types of cultivation, organic and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus vulgaris L.; Production system; Organic agriculture; Phaseolus vulgaris L.; Sistema de produção; Agricultura orgânica.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6827

HÍBRIDOS DE MILHO FRENTE AO ATAQUE DE Spodoptera frugiperda EM ASSOCIAÇÃO COM ADUBAÇÃO SILICATADA E O EFEITO SOBRE O PREDADOR Doru luteipes
Provedor de dados: 196
Autores: Toscano, Luciana Cláudia; Fernandes, Mariano Antunes; Rota, Murilo; Maruyama, Wilson Itamar; Andrade, Jessica Velasco.
O objetivo deste trabalho foi avaliar diferentes híbridos de milho frente ao ataque de S. frugiperda em associação com adubação silicatada e o efeito sobre o predador D. luteipes. O experimento foi realizado durante a safra 2008/09, com três híbridos de milho, Impacto (Syngenta), AS1575 (Agroeste) e o transgênico AG7000YG (Agroceres), em diferentes épocas de aplicação do produto comercial (Sili-K®), contendo silício na concentração 12,2% (SIO2) e 15% de K2O, via foliar na dosagem de 3 L ha-1. O delineamento experimental utilizado foi em blocos casualizados, em parcelas subdivididas com quatro repetições. As parcelas foram constituídas por 3 cultivares de milho e as subparcelas constituídas por 3 épocas diferentes de aplicação foliar de silício (aos 10 e 30...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/680

DEFICIT IN STATIC GRAIN STORAGE CAPACITY IN THE STATE OF GOIÁS IN THE 2016/17 HARVEST
Provedor de dados: 196
Autores: da Silva Berti, Mariana Pina; guimaraes, André Felippe Monteiro; Arruda, Natalia; Berti, Christian Luis Ferreira.
The Central-West region has been highlighted as the largest agricultural center in the country, accounting for 42% of national grain production. Goiás State represented an amount of 18.9 million tons in the last harvest. Despite the large production, a problem which affects the negotiations and the quality of the harvested grains is storage. A static capacity of 20% higher than grain production is recommended. The objective of this work was to evaluate the storage capacity of grains in the State of Goiás and their respective mesoregions using a comparison with the agricultural production of the Center-West region. The deficit in the static storage capacity of grain in Goiás for the 2016/17 harvest was 25.17% in relation to grain production, since the...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3124

GROWTH AND QUALITY OF ‘PÉROLA’ PINEAPPLE AS A FUNCTION OF LEVELS OF GIBBERELLIC ACID
Provedor de dados: 196
Autores: Moura da Silva, Juanderson; Barbosa da Silva, João Henrique; Eraldo Souza Araújo, José Rayan; Marinho Gomes, Eduardo; Manoel Ferreira de Lima Cruz, José; Veimar da Silva, Antônio; Gledson da Silva, Francisco; de Oliveira Santos, João Paulo; Esfrain Pereira, Walter.
Gibberellin is a plant hormone capable of enhancing the productivity of plant’s productivity rants, due to its action in plant physiology, mainly in fruit formation. In this sense, this study aimed to evaluate gibberellic acid levels and application times on the growth and quality of ‘Pérola’ pineapple. The experiment was conducted under field conditions in the municipality of Pedras de Fogo, state of Paraíba, Brazil. The treatments consisted of five levels of gibberellic acid (0.0, 1.5, 3.0, 6.0, and 12.0 mg/plant), distributed in a randomized block experimental design, with four repetitions, in which three applications were made at 50, 80, and 110 days after flower induction. The soluble solids content, fruit height, fruit diameter, and weight were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ananas comosus L.; Gibberellin; Plant Hormones; Ananas comosus L.; Gibberellin; Plant Hormones.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6731

EFEITO DO ALDICARBE NO CICLO DE VIDA DE Meloidogyne incognita
Provedor de dados: 196
Autores: Silva, Esdras Henrique da; Campos, Vicente Paulo; Rocha, Fernando da Silva; Zeviani, Walmes Marques; Terra, Willian César; Rigitano, Renê Luís de Oliveira.
Ovos, juvenis de segundo estádio (J2) e fêmeas de Meloidogyne incognita foram inseridos em solução contendo o princípio ativo aldicarbe com ação nematicida. A exposição ao nematicida ocasionou: (1) redução na eclosão, (2) redução na mobilidade, (3) mortalidade de J2, e (4) redução na penetração. A aplicação do nematicida após a infecção com J2 saudáveis foi mais eficiente em reduzir a reprodução do nematoide. A aplicação feita mais próxima da inoculação causou maiores reduções de galhas e de ovos/g de raiz de planta de soja, com maior efeito na reprodução. Enquanto os J2 incubados por 24 h em aldicarbe 50 μg mL-1 e inoculados em soja tiveram o número de ovos/g raiz reduzido em 2,5%, em comparação à testemunha, a aplicação da mesma concentração após a...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2164

MANEJO DA ADUBAÇÃO NITROGENADA NA CULTURA DA CANOLA
Provedor de dados: 196
Autores: Webber Puhl, Roberto; Rasche, Jimmy Walter.
Atualmente não existe recomendação de fertilização nitrogenada na canola no Paraguai. O objetivo foi verificar o efeito do manejo da adubação nitrogenada na cultura de canola. Foi implantado um experimento com 5 tratamentos que consistiram em diferentes doses e épocas de aplicação de N na cultura da canola T1: 0 kg de N ha-1; T2: 15 kg de N ha-1na semeadura; T3: 15 kg de N ha-1na semeadura, 46 kg de N ha-1 no início da roseta; T4: 15 kg de N ha-1 na semeadura e 46 kg de N ha-1na roseta e; T5: 15 kg de N ha-1na semeadura, 23 kg de N ha-1 no inicio de roseta  e 23 kg de N ha-1 na floração, com quatro repetições. Foi determinada altura de planta aos 60 dias após a semeadura e no final de ciclo, o número de síliquas por planta, rendimento de grãos e massa de...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/251

REAÇÃO DE CULTIVARES DE SORGO SACARINO A Meloidogyne javanica, Rotylenchulus reniformis E Pratylenchus brachyurus
Provedor de dados: 196
Autores: Oliveira, Cibelle da Silva; Asmus, Guilherme Lafourcade.
O objetivo do presente trabalho foi avaliar a reprodução de Meloidogyne javanica, Rotylenchulus reniformis e Pratylenchus brachyurus em raízes das cultivares de sorgo sacarino ‘BRS 506’, ‘BRS 508’, ‘BRS 509’ e ‘BRS 511’ em três experimentos conduzidos em casa de vegetação. As cultivares de sorgo foram semeadas em vasos de polietileno de 3 L, preenchidos com substrato desinfestado, composto da mistura de solo e areia (2:1). Doze dias após a emergência, cada planta foi inoculada com populações puras de M. javanica, R. reniformis ou P. brachyurus, nos respectivos experimentos. Os padrões de susceptibilidade foram soja ‘BRS 360RR’ para M. javanica, algodão ‘BRS Cedro’ para R. reniformis e milho ‘BRS 1010’ para P. brachyurus. Crotalária (Crotalaria spectabilis)...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2705

SINGLE-HEAD BROCCOLI PRODUCTION UNDER DIFFERENT SPACING AND CONDITIONS OF BAIXADA FLUMINENSE
Provedor de dados: 196
Autores: Macedo, Taísa Gonçalves; dos Santos, Carlos Antônio; Brandão, Antônio de Amorim; Silva Pereira Costa, Evandro; Goréte Ferreira do Carmo, Margarida.
This study aimed to evaluate different spacings between rows on the development and yield of single-head broccoli under the soil and climate conditions of Seropédica, in the Baixada Fluminense region, the State of Rio de Janeiro (Brazil). Tests were carried out under field conditions using the Avenger hybrid. The experimental design adopted was randomized blocks with four treatments and four replications per treatment. Four spacings between rows were tested: 0.6 m, 0.7 m, 0.8 m, and 1.0 m. The spacing between plants in the rows was 0.6 m in all treatments. The number of leaves (NL), plant height (PHT), fresh leaf mass (FLM), stem fresh mass (SFM), inflorescence fresh mass (IFM), inflorescence longitudinal diameter (ILD), and estimated yield (YLD) were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brassica oleracea var. italica; Brassicaceae; Population density; Brassica oleracea var. italica; Brassicaceae; Densidade populacional.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6908

EFEITO DA ADUBAÇÃO NITROGENADA EM COBERTURA NA SEVERIDADE DA FERRUGEM COMUM DO MILHO
Provedor de dados: 196
Autores: Pereira, Igor Souza; Pereira, Márcia Toyota.
A adubação nitrogenada pode interferir positivamente ou negativamente na intensidade de diversas doenças das plantas. Neste contexto, este estudo objetivou avaliar o efeito da aplicação de doses de nitrogênio em cobertura na severidade da ferrugem comum do milho (Puccinia sorghi). O experimento foi instalado na Fazenda Experimental da EPAMIG, em Prudente de Morais (MG), utilizando-se o híbrido de milho-verde AG 4051. O delineamento experimental adotado foi de blocos ao acaso com cinco tratamentos e três repetições. Os tratamentos constituíram da aplicação de cinco doses de N (0, 60, 120, 180 e 240 kg ha-1) na forma de ureia em cobertura. Foram realizadas cinco avaliações (em intervalo semanal) da severidade da doença em 3 folhas marcadas (2 acima e 1...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1688

INCREASING DOSES OF CATTLE MANURE FOR ORGANIC CHILI PEPPER PRODUCTION
Provedor de dados: 196
Autores: Ribeiro, João Victor Silva; Semensato, Leandra Regina; Vendruscolo, Eduardo Pradi.
There is a contemporary trend of change in the agricultural sector, aiming at the use of ecologically friendly inputs. This trend can be seen by the constant increase in the demand for organic products. However, as with other technologies, there is a need for studies to evaluate the effectiveness of its use. The present study aimed to evaluate the effects of the application of increasing doses of cattle manure on the development and productivity of chili peppers. The treatments consisted of increasing doses of cattle manure (0; 5; 10; 15; 20 Mg ha-1). The variables plant height, stem diameter, number of plant leaves and length, diameter, and fruit yield were evaluated. It was found that, with the maximum amount of cattle manure, there was an increase of...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5158

CAN DOSING MECHANISMS AFFECT THE PHYSICAL QUALITY OF CORN SEEDS AT DIFFERENT SEEDING SPEEDS?
Provedor de dados: 196
Autores: Parizotto, Nayara Francieli; Carpes Marques Filho, Aldir; Munhoz  Venâncio de Oliveira, Marcelo; Pereira de Souza, Flavia Luize; Arbex Silva, Paulo Roberto.
Corn (Zea mays L.) is one of the main commodities of Brazilian agribusiness, however, the sowing operation of this crop still presents challenges related to the performance of the metering mechanisms and operational speed, since these can affect the physical quality of the seeds and impair germination. The aim of this study was to evaluate the physical quality of maize seeds as a function of different metering mechanisms and operational speeds in a controlled sowing trial. The experiment was carried out at the State University, UNESP/Botucatu-SP, using five commercial models of seed dosers at four operational sowing speeds. The results showed that the metering model and the operational speed directly affected the physical quality of the corn seeds,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantability; Mechanical damage; Distribution systems; Seeding; Plantabilidade; Dano mecânico; Sistemas de distribuição; Semeadura.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6823

AMBIENTES PROTEGIDOS E SUBSTRATOS PARA MUDAS DE BOCAIÚVA ORIUNDAS DO CAMPO
Provedor de dados: 196
Autores: Ascoli, Alexandre de Araújo; Pereira, Amanda Casagrande; Costa, Edilson; Jorge, Marçal Henrique Amici; Maruyama, Wilson Itamar.
A bocaiuva é espécie promissora para produção de alimentos e biodiesel; tecnologias de formação de mudas ajudam toda a cadeia produtiva desta espécie. O objetivo foi avaliar  o pegamento e o crescimento de mudas de bocaiuva oriundas do campo, em diferentes substratos e ambientes protegidos. Foram avaliados dois ambientes: telado agrícola com tela aluminizada na cobertura e laterais com tela preta; telado agrícola com tela preta em toda sua extensão. Foram testados os substratos Bioplant®; 0% de esterco bovino + 70% de solo + 30% de areia; 10% de esterco bovino + 60% de solo + 30% de areia; 20% de esterco bovino + 50% de solo + 30% de areia; 30% de esterco bovino + 40% de solo + 30% de areia. Foi adotado o delineamento inteiramente casualizado com 4...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/274

CARACTERÍSTICAS BROMATOLÓGICAS EM HÍBRIDOS DE MILHO PARA PRODUÇÃO DE SILAGEM NO ESTADO DE MINAS GERAIS
Provedor de dados: 196
Autores: Silva, Michele Jorge da; Balbino, Lucas Coelho; Cardoso, Dimas Antônio Del Bosco; Miranda, Lucas Mattos; Pimentel, Leonardo Duarte.
Embora existam várias plantas forrageiras, anuais e perenes, o milho é uma das culturas mais utilizadas neste processo no Brasil, sendo considerada a cultura padrão. Pesquisas de comparação entre híbridos para produção de silagem de milho são fundamentais para o avanço dos programas de melhoramento genético e importantes na recomendação a técnicos e produtores sobre o híbrido destinado à produção de silagem. O objetivo deste trabalho foi avaliar as características bromatológicas de híbridos de milho para o cultivo na região da Zona da Mata Mineira. O experimento foi conduzido na Fazenda Nô da Silva, localizada no município de Cajuri, Minas Gerais. Os tratamentos foram constituídos por 24 híbridos com aptidão para silagem. Utilizou-se o delineamento...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1584

GRAIN SORGHUM GROWN AS SECOND CROP AND INOCULATED WITH Azospirillum brasilense ASSOCIATED WITH NITROGEN FERTILIZATION
Provedor de dados: 196
Autores: Soares, Deyvison de Asevedo; Andreotti, Marcelo; Vicentini, Maria Elisa; Freitas, Leandro Alves; Modesto, Viviane Cristina; Nakao, Allan Hisashi; Dickmann, Lourdes; Teixeira Filho, Marcelo Carvalho Minhoto.
Nitrogen fertilization in off-season sorghum may have lower cost-benefit ratios than expected due to the residual effect of previous crops. However, the use of growth-promoting bacteria can be an economical alternative to increase crop yields in Cerrado. The objective was to evaluate the response of grain sorghum to nitrogen fertilization and its inoculation by Azospirillum brasilense. This study aims to evaluate grain sorghum responses to nitrogen fertilization and A. brasilense inoculation. The experiment was carried out in a fully randomized block design and 5 x 2 factorial scheme, with five replications. Treatments consisted of applying N recommendation (120 kg N-urea ha-1) split as follows: 100% at sowing, 100% as topdressing, 25% at sowing and 75% as...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5117

INITIAL DEVELOPMENT OF GABIROBA (Campomanesia adamantium) ACCORDING TO FERTILIZATION WITH NITROGEN AND PHOSPHORUS
Provedor de dados: 196
Autores: Mello Duarte, Jéssica Rodrigues de; Basílio, Scarlet de Aguiar; Peixoto, Nei; Berti, Mariana Pina da Silva.
Campomanesia adamantium (Cambess.) Berg O. is a native of Savanna, popularly known as gabiroba, guavira, or gabiroba-do-campo, and has many uses, with its fruit being consumed fresh or processed. This study aimed to evaluate different doses of phosphorus and nitrogen in the initial development of gabiroba (Campomanesia adamantium) cultivated in pots. Five doses of phosphorus (0, 100, 200, 300, and 400kg ha-1 of P2O5) and three doses of nitrogen (0, 100, and 200 kg ha-1of N) were tested. The experimental design used was completely randomized in a 5x3 factorial scheme with six replications. The evaluations were carried out 120 days after plant emergence, and the variables analyzed were stem diameter, plant height, and number of leaves. Data were subjected to...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5825

HYDRO-MICROBIOLOGICAL ATTRIBUTES OF THE SOIL IN EDGE OF SEASONAL SEMIDECIDUOUS FOREST FRAGMENT
Provedor de dados: 196
Autores: D'Abadia, Karolayne Lemes; Souza, Ane Gabriele Vaz; Silva, Gabriela Gomes da Silva Gomes da; Machado, Murilo Silva; Vale, Vagner Santiago do Vale Santiago do; Santos, Talles Eduardo Borges dos.
Native forests have been suffering changes, such as fragmentation and edge effect, and these have implications for the dynamics of carbon within the same fragment, differentiating vegetation and soil. In this way, the work aimed to evaluate the hydro-microbiological attributes of the soil in rainy and dry periods, as well as to indicate if there is an edge effect in a seasonal semideciduous forest fragment. The study was carried out in a forest fragment in the area of the State University of Goiás, Ipameri Campus, consisting of three transects divided into three blocks from the edge. Sampling was performed in two periods of the year, rainy and dry, to determine the gravimetric soil water content (UG), microbial biomass carbon (MBC), basal respiration (BR),...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3919

ENCAPSULATED BAITS CONTAINING ZINC SULFATE AND Trichoderma harzianum REDUCE FUNGAL GARDEN IN Atta sexdens COLONIES
Provedor de dados: 196
Autores: da Silva, Daniella Gonçalves; Lucena Júnior, Aldemir; Sarmento, Renato de Almeida; Santos Silva, Cynthia Lhourrana; Teles Tenório, Amanda Caroline; de Souza, Danival José; Melo, Márcio Silva.
The aim of the study was to test the effects of various concentrations of zinc sulfate (ZnSO4) on the radial growth of Trichoderma harzianum and Leucoagaricus gongylophorus in Petri dishes. In addition, we investigated the acceptance of baits containing live propagules of the encapsulated T. harzianum fungus and baits containing ZnSO4 by foraging leafcutter worker ants, A. sexdens, as well as their effects on the colonies of these ants. For the in vitro test, the design was completely randomized using ten replicates of a 2 × 7 factorial scheme: two species of fungi (T. harzianum and L. gongylophorus) and seven concentrations of ZnSO4. For bait acceptance tests, four treatments were used: baits without the mycelium and ZnSO4 (T1, control), baits containing...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5064

ATIVIDADE RESPIRATÓRIA E QUALIDADE DE BETERRABA INTEIRA E MINIMAMENTE PROCESSADA
Provedor de dados: 196
Autores: Sanches, Alex Guimarães; Silva, Maryelle Barros da; Moreira, Elaine Gleice Silva; Costa, Jaqueline Macedo; Cordeiro, Carlos Alberto Martins.
A beterraba (Beta vulgaris L.) é uma raiz tuberosa de grande importância agrícola e que vem ganhando espaço na linha de produtos minimamente processados. Todavia, o comportamento respiratório e a avaliação da qualidade pós-colheita dessa olerícola ainda é restrito principalmente quanto a melhor forma de processamento sendo este o principal objetivo desta pesquisa. As raízes foram armazenadas durante sete dias em refrigerador com temperatura de 5°C e avaliados diariamente quanto a taxa respiratória, a produção de etileno, o conteúdo de sólidos solúveis, acidez titulável, teor de ácido ascórbico e de betaleínas. A taxa respiratória e os teores de betalaínas foram afetados, independente do armazenamento, inteiro ou processado. De modo geral o armazenamento...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1182

SOIL CARBON STOCK IN DIFFERENT USES IN THE SOUTHERN CONE OF MATO GROSSO DO SUL
Provedor de dados: 196
Autores: Martins, Luis Felipe Batista Nandi; Troian, Douglas; Rosset, Jean Sérgio; Souza, Camila Beatriz da Silva; Farias, Paulo Guilherme da Silva; Ozório, Jefferson Matheus Barros; Marra, Leandro Marciano; Castilho, Selene Cristina de Pierri.
This study aimed to assess the soil density (Sd) and the total organic carbon contents and stocks in different management systems and implementation times in the municipality of Iguatemi, MS, Brazil. A completely randomized design with four replications was applied to four areas: conventional tillage (CT), reformed pasture (RP), and degraded pasture (DP), in addition to a native forest (NF) area with no anthropic action. Disturbed and undisturbed soil samples were collected at depths of 0–0.05, 0.05–0.1, and 0.1–0.2 m. The determination of Sd and total organic carbon content (TOC) allowed calculating the carbon stock (Cstock), the stratification index (SI), and the carbon stock variation (ΔCstock), with subsequent multivariate analysis. The NF area...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5351

EFEITO DO SAL DE ÁCIDO CARBOXÍLICO SOBRE NINFAS DE Aphis gossypii GLOVER (1877) (Hemiptera: Aphididae)
Provedor de dados: 196
Autores: Pessoa, Luis Gustavo Amorim; Silva, Willyam Eduardo Bonafede da; Ribeiro, Muller de Paula; Loureiro, Elisângela de Souza; Dias, Pamella Mingotti.
Objetivou-se avaliar o efeito do sal de ácido carboxílico no controle de Aphis gossypi.Para instalação dos experimentos, adultos em fase reprodutiva foram coletados em plantas de algodão cultivadas em casa de vegetação e levados ao laboratório, sendo acondicionados em placas de Petri (6 cm de diâmetro) contendo discos foliares de algodão fixadas em uma fina camada solidificada de ágar-água. Os adultos permaneceram nos discos por 24 horas, sendo as ninfas produzidas utilizadas para aplicação dos tratamentos. Foram utilizadas ninfas de primeiro e terceiro ínstares. Os tratamentos foram aplicados com auxílio de torre de Potter sendo compostos por diferentes concentrações do sal de ácido carboxílico BIO ADD (0,25%; 0,5% e 0,75%), além do tratamento testemunha...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2197

RECUPERAÇÃO DE UM SOLO DE CERRADO APÓS 19 ANOS: OCORRÊNCIA ESPONTÂNEA DE ESPÉCIES ARBÓREAS
Provedor de dados: 196
Autores: Rosa, Poliana Aparecida Leonel; Alves, Marlene Cristina; Videira, Ligia Maria Lucas; Bonini, Carolina Batista dos Santos.
A interven&amp;ccedil;&amp;atilde;o humana com a retirada das camadas superficiais do solo para obras civis, tem resultado em extensas &amp;aacute;reas degradadas. Atrav&amp;eacute;s deste trabalho objetivou-se avaliar o grau de recupera&amp;ccedil;&amp;atilde;o de um solo, ap&amp;oacute;s 19 anos, sob diferentes interven&amp;ccedil;&amp;otilde;es para sua recupera&amp;ccedil;&amp;atilde;o e a ocorr&amp;ecirc;ncia espont&amp;acirc;nea de esp&amp;eacute;cies arb&amp;oacute;reas. Os tratamentos foram instalados em 1992. Utilizou-se o delineamento experimental em blocos casualizados com sete tratamentos e quatro repeti&amp;ccedil;&amp;otilde;es, sendo os tratamentos compostos por diferentes m&amp;eacute;todos de regenera&amp;ccedil;&amp;atilde;o. Em 1999...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recuperação do Solo.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/221

EFFICIENCY AND UNIFORMITY OF AN SUBSURFACE DRIP IRRIGATION SYSTEM IN SUGARCANE CROP
Provedor de dados: 196
Autores: Ferreira dos Santos, José Wibison; Sampaio Reis, Lígia; Dos Santos Dias, Mirandy; Silva dos Santos, Rilbson Henrique; de Assis da Silva, Francisco; de Oliveira Santos, João Paulo.
Agricultural productivity in irrigated areas depends on several factors, including the design and maintenance of irrigation systems. Excessive or insufficient applications of water affect plant growth and development, hence agricultural productivity. For this reason, the evaluation of the irrigation system is essential to avoid water loss during application. This study aimed to evaluate the efficiency and uniformity of a subsurface drip irrigation system in sugarcane crops in an area of the company Usina Coruripe, Alagoas, Brazil. For data collection, the flow rates were obtained in four points along the lateral line, in the first dripper, in the drippers located at 1/3 and 2/3 of the lateral line length, and in the last dripper of each operational unit of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum officinarum L.; Irrigation management; Localized irrigation.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6829

AGRONOMIC PERFORMANCE AND YIELD OF RADISH CULTIVARS
Provedor de dados: 196
Autores: Moreira, Romário da Silva; Santos, Marlei Rosa dos; Sousa, Ronildo Almeida de; Almeida, Rubenalto da Silva; Gomes Junior, Francisco de Assis; Coelho, Warlington Aquilis Araujo.
The radish is a Brassicaceae with small size, adapted to regions with mild temperatures between 13 and 20 °C and short days. However, there are cultivars adapted to high-temperature conditions, which has allowed the cultivation of this tuberous vegetable throughout the year, even in tropical regions. The present work had as objective evaluate the agronomic performance and yield of six cultivars of radish, in Uruçuí - PI. The experimental design was in randomized blocks, with four replicates and six cultivars. Harvest was performed according to the cycle of each cultivar. Number of leaves per plant, fresh and dry mass of shoot and root, diameter, and root length and yield were evaluated. The cultivars Margaret Queen and Crimson Gigante presented better root...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3345

POTENTIAL OF F3:4 SEGREGATING WHEAT POPULATIONS FOR TOLERANCE TO HEAT STRESS
Provedor de dados: 196
Autores: Ribeiro, Guilherme; Pimentel, Adérico Júnior Badaró; Rocha, João Romero do Amaral Santos de Carvalho; Oliveira, Isadora Cristina Martins; Souza, Moacil Alves de.
Heat is one of the major abiotic stresses that affect wheat yield and quality in many parts of the world. To overcome this problem, the development of heat tolerant cultivars has been shown to be one of the main targets of breeding programs, especially for the conditions of Central Brazil. The present study was developed with objective of identifying promising populations for tolerance to heat stress, in order to obtain lines adapted to the conditions of Central Brazil. The experiment was carried out in the summer of 2011 in Coimbra/MG where 36 segregating populations with different numbers of families per population were evaluated in an augmented block design, determining the cycle, plant height and grain yield. Genetic variability for heat tolerance was...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3314

POTENCIAL FISIOLÓGICO DE SEMENTES DE FEIJÃO-CAUPI SUBMETIDAS À PRÉ-HIDRATAÇÃO
Provedor de dados: 196
Autores: Nunes, Luma Rayane de Lima; Pinheiro, Paloma Rayane; Dutra, Alek Sandro.
A utilização de sementes de boa qualidade é fundamental para o estabelecimento adequado de uma lavoura. Para uma análise mais precisa da qualidade de sementes, faz-se necessária a complementação das informações fornecidas pelo teste de germinação com os testes de vigor, que dentre eles se destaca o de condutividade elétrica, por ser considerado rápido, simples e confiável. O presente trabalho objetivou avaliar a influência da pré-hidratação na eficiência do teste de condutividade elétrica na avaliação do potencial fisiológico em seis lotes de sementes de feijão-caupi cv. Setentão. Inicialmente, procedeu-se à caracterização dos lotes pela determinação do teor de água e pelos testes de germinação e vigor (primeira contagem, índice de velocidade de...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2646

UTILIZAÇÃO DE MÉTODOS FÍSICOS E DE FITORREGULADORES PARA SUPERAÇÃO DE DORMÊNCIA EM SEMENTES DE PINHA
Provedor de dados: 196
Autores: Vasconcelos, Luís Henrique Costa; Vendruscolo, Eduardo Pradi; Vasconcelos, Rebeca Freitas; Santos, Marivone Moreira dos; Seleguini, Alexsander.
A pinha é uma fruta muito apreciada devido ao sabor, e pode ser propagada por sementes ou de forma vegetativa por enxertia. No entanto, a produção de mudas por propagação seminal é dificultada pela dormência acentuada das sementes. Neste aspecto, objetivou-se determinar o melhor tratamento para a superação de dormência de sementes de pinha (Annona squamosa L.), submetendo-as à associação de tratamento pré-germinativo mecânico e não mecânico. Foi empregado o delineamento experimental inteiramente casualizado em esquema fatorial 4 × 2, com quatro repetições. Os tratamentos foram caracterizados por quatros tratamentos pré-germinativos não mecânicos em associação a tratamento pré-germinativo mecânico (presença ou ausência) com escarificação mecânica com lixa...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/267

USO DA PRÓPOLIS NO CONTROLE “IN VITRO” DO FUNGO Colletotrichum gloeosporioides CAUSADOR DA ANTRACNOSE EM FRUTOS DE BERINJELA
Provedor de dados: 196
Autores: Pastana, Rubens Felippe; Costa Vieira, Gustavo Haralampidou; Machado, Patricia Pereira.
O trabalho foi desenvolvido com o objetivo de determinar o efeito da própolis no controle “in vitro” do fungo Colletotrichum gloeosporioides. A atividade antifúngica da própolis foi determinada através do desenvolvimento do fungo em meio de cultura BDA (batata-dextrose-ágar) acrescido da referida substância em diferentes concentrações, conforme os seguintes tratamentos: 1) testemunha absoluta (sem aplicação); 2) testemunha com aplicação de 4 mL L–1 de fungicida (Cupravit Azul BR - oxicloreto de cobre inorgânico); 3) 4 mL L–1 de própolis; 4) 8 mL L–1 de própolis; 5) 16 mL L–1 de própolis; e, 6) 32 mL L–1 de própolis. O crescimento micelial do fungo foram avaliados após 48, 72 e 96 h de inoculação. Os resultados indicaram que o uso de própolis na maior...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/654

WEEDS IN SOYBEAN CULTIVATION WITH DIFFERENT PREDECESSOR COVER CROPS
Provedor de dados: 196
Autores: Pinto, Pedro Henrique Gomes; Lima, Sebastião Ferreira; Andrade, Maria Gabriela Oliveira; Contardi, Lucymara Merquides; Ávila, Jorgiani; Reis, Breno Oliveira; Bernardo, Vitória Fátima; Vendruscolo, Eduardo Pradi.
The competition between soybean and weeds affects crop development due to reduced resources such as water, light, and nutrients, leading to yield losses. Thus, the study aimed to evaluate quantitatively and qualitatively, through phytosociology and seed bank, the weed presence in a soybean cultivation area with different predecessor cover crops. The experiment was installed under no-till system conditions using a randomized block design with nine treatments and three replications. The treatments were composed of the following cover crops, sorghum (Sorghum bicolor), crotalaria (Crotalaria ochroleuca), millet (Pennisetum americanum), Urochloa ruziziensis, U. brizantha cv. Piatã, fodder radish (Raphanus sativus L.), U. brizantha cv. Xaraés, millet + fodder...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5890

EFFECTS OF THE PROPAGULE SIZE ON THE TUBEROUS RHIZOME PRODUCTION AND PHYSICOCHEMICAL CHARACTERISTICS OF JERUSALEM ARTICHOKE
Provedor de dados: 196
Autores: Li, Meiling; Solano Mendoza, Juan David; Ming, Lin Chau.
As a crop that is rich in oligosaccharides, Jerusalem artichoke is considered one of the most promising plants for production because of its ability to survive in marginal lands, strong resistance to biotic and abiotic stresses, ease of conversion into biofuels, and use for food consumption. In the present study, the effects of propagule size on tuberous rhizome production and the physicochemical characteristics of Jerusalem artichoke were evaluated. Five propagule sizes of tuberous rhizome, 10 g (T1), 30 g (T2), 50 g (T3), 70 g (T4), and 90 g (T5), were used in a completely randomized experiment with 5 replicates and 11 plants per replicate. Harvesting was carried out 164 days after planting. The results showed that T1 resulted in the lowest emergence...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4231

DEVELOPMENT AND QUALITY OF SWEET MAIZE INOCULATED WITH DIAZOTROPHIC BACTERIA AND TREATED THIAMINE
Provedor de dados: 196
Autores: Vendruscolo, Eduardo Pradi; Siqueira, Ana Paula Silva; Furtado, João Paulo Marques; Campos, Luiz Fernandes Cardoso; Seleguini, Alexsander.
The insertion of technologies that help to maintain or increase the productivity and quality of agricultural products is highly important in the face of the challenges for the generation of more sustainable farming systems. Thus, the objective of this work was to evaluate the biometric and post-harvest characteristics of sweet maize under inoculation with Azospirillum brasilense and different doses of thiamine applied by seed treatment. The experiment was conducted in a factorial scheme (2 x 4) and the composition of the treatments was the combination of the presence or absence of the Azospirillum brasilense and different doses of thiamine (0, 15, 30 and 45 mg kg-1). Were evaluated the grain yield, ear weight with and without the straw, straw weight, straw...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2766

SISTEMA PLANTIO DIRETO E CONVENCIONAL: EFEITO NA PRODUTIVIDADE DE FIBRA DE TRÊS CULTIVARES DE ALGODOEIRO
Provedor de dados: 196
Autores: Lamas, Fernando Mendes; de Barcellos Ferreira, Alexandre Cunha; Rodrigues de La Torre, Elio de Jesus; Staut, Luiz Alberto.
O sistema de produção predominante na cultura do algodoeiro é o sistema convencional de manejo do solo, que tem proporcionado degradação dos atributos físicos, químicos e biológicos do solo. Com o objetivo de avaliar o efeito do Sistema Plantio Direto (SPD) e do Sistema Convencional de Manejo do Solo (SC) sobre a produtividade de fibra das cultivares BRS Cedro, BRS Jatobá e BRS Araçá, foram conduzidos experimentos em Primavera do Leste, MT, no período de 2006/2007 a 2012/2013. O algodoeiro foi cultivado em SPD, obedecendo à seguinte sequência para os períodos de verão e outono-inverno, respectivamente: ano 1) soja/Urochloa ruziziensis; ano 2) milho + U. ruziziensis/U. ruziziensis; ano 3) algodão/pousio; ano 4) soja/U. ruziziensis e em SC, com mobilização...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/846

EXTRACTION METHODS AND POTASSIUM AVAILABILITY FOR SOYBEAN IN THE PARANA STATE’S SOILS, BRAZIL
Provedor de dados: 196
Autores: Steiner, Fábio; Lana, Maria do Carmo; Zoz, Tiago; Frandoloso, Jucenei Fernando; Fey, Rubens.
Evaluating the potassium (K) availability to the plants can be performed by different methods. In general, multielement methods are employed and they are used for K due to increase operational of soil testing laboratory. The efficacy of ammonium acetate, Mehlich-1, Mehlich-3 and ion exchange resin soil K extractantsin determining the K availability for soybean [Glycine max L. (Merrill)], in different Parana’s soils, were investigated in this study. Twelve soil samples, collected from the upper layer 0–0.20 m, were cultivated with soybean for 42 days in greenhouse conditions. The average amount of available soil K extracted in test soils was found, displayed in decreasing order: ammonium acetate &amp;gt; Mehlich-3 &amp;gt; Mehlich-1 = ion exchange resin....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Extratores; Disponibilidade de Nutrientes.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/232

DIFERENTES SUBSTRATOS E AMBIENTES PROTEGIDOS PARA O CRESCIMENTO DE MUDAS DE MARACUJAZEIRO AMARELO DOCE
Provedor de dados: 196
Autores: Lima, Isabela Machado de Oliveira; Silva Júnior, Joaquim Souto; Costa, Edilson; Cardoso, Eliana Duarte; Binotti, Flávio Ferreira da Silva; Jorge, Marçal Henrique Amici.
A muda de alta qualidade, com vigor superior e equilíbrio de crescimento em altura e diâmetro, possui condições de melhor pegamento e sobrevivência no local definitivo de plantio. Objetivou-se estudar vários substratos contendo diferentes mistura de esterco bovino, solo de barranco, Bioplant®, vermiculita super fina e areia fina em ambientes telados na formação de mudas de maracujá. Foram utilizados o (A1) telado agrícola (dimensões: 8,0 m x 18,0 m x 3,5 m), fechamento em 45º de inclinação, com tela preta de monofilamento em toda sua extensão, malha para 50% de sombreamento (Sombrite®) e (A2) telado agrícola (dimensões: 8,0 m x 18,0 m x 4,0 m), com tela aluminizada termorrefletora na cobertura a 3,30 m, malha para 50% de sombreamento (Aluminet®),...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1240

NUTRIENTES NO SOLO E PRODUÇÃO DE QUIABO CONFORME DOSES DE SILICATO DE CÁLCIO E MAGNÉSIO
Provedor de dados: 196
Autores: Moraes, Emmerson Rodrigues de; Reis, Aysha Cristinne dos; Silva, Nikson Elias Pinto da; Ferreira, Mateus; Menezes, Felipe Garcia de.
A acidez do solo é fator limitante na agricultura, pelo fato da mesma indisponibilizar o fósforo na solução do solo e influenciar na dinâmica dos demais nutrientes no solo. A utilização de silicato de cálcio (Ca) e magnésio (Mg) fornece silício (Si) e corrige a acidez do solo aumentando a produtividade. O objetivo do estudo foi observar a produção do quiabeiro e as características químicas do solo em função da aplicação de diferentes doses de silicato de cálcio e magnésio. Utilizou-se o delineamento em blocos casualizados com cinco tratamentos e cinco repetições cultivado em 2014 e 2016. O silicato de cálcio e magnésio foi aplicado ao solo nas seguintes doses: 0; 0,5; 1,0; 2,0 e 4,0 t ha-1. Foram avaliados o peso de fruto por planta, peso médio de frutos,...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2097

DIVERSIDADE DE INSETOS EM PLANTAS HOSPEDEIRAS PRÓXIMAS ÀS ÁREAS DE CULTIVO DE MILHO E ALGODÃO
Provedor de dados: 196
Autores: Oliveira, Rafael Alvim G.; Rando, Jael Simões Santos.
As plantas hospedeiras servem como refúgios para os insetos no período de entressafra, onde se alimentam, acasalam ou ficam em diapausa aguardando novo plantio para que os indivíduos sobreviventes se dirijam à lavoura. Este estudo teve como objetivo avaliar a diversidade de insetos em treze espécies de plantas espontâneas próximas a áreas de cultivo de algodão e milho no período de entressafra. Foram selecionadas quatro plantas hospedeiras e realizadas avaliações mensais por observação direta e identificados os insetos. Foi realizada a análise faunística determinando-se a riqueza, índice de diversidade de Margalef e Shannon-Wiener e índice de equitabilidade. Foram coletados indivíduos pertencentes às ordens Coleoptera, Hemiptera, Hymenoptera, Diptera,...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1602

PRODUÇÃO DE BRÓCOLIS EM FUNÇÃO DAS DOSES DE NITROGÊNIO E POTÁSSIO NA FERTIRRIGAÇÃO DAS MUDAS
Provedor de dados: 196
Autores: Silva, Priscilla Nátaly de Lima; Souza, Luis Gustavo de; Redigolo, Mateus Vinicius Narciso; Cardoso, Antonio Ismael Inacio.
Frente à existência de poucos estudos relacionados à aplicação de nitrogênio e potássio na produção de mudas de Brassicáceas, objetivou-se avaliar os efeitos de doses destes nutrientes na fertirrigação de mudas produzidas em substrato à base de fibra da casca de coco sobre a produção de brócolis. Foi utilizado o delineamento experimental em blocos casualizados, em esquema fatorial com quatro doses de N (0, 80, 160 e 240 mg L-1) e quatro doses de K (0, 100, 200 e 300 mg L-1) na fertirrigação das mudas, com quatro repetições. Foram avaliadas a quantidade de macronutrientes e características vegetativas das mudas, como: número de folhas, altura, diâmetro do caule, massa fresca e seca da parte aérea e, na colheita, o número de folhas, diâmetro e massa fresca e...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2448

VIDA ÚTIL DE VARIEDADES  DE MANGABA  ENDÊMICAS DO CERRADO  EM DIFERENTES ESTÁDIOS DE MATURAÇÃO
Provedor de dados: 196
Autores: Siqueira, Ana Paula Silva; Morgado, Cristiane Maria Ascari; Cavalcante, Karina Athaide; Cunha Júnior, Luís Carlos; Souza, Eli Regina Barboza.
A mangabeira é uma frutífera nativa do Cerrado de grande potencial produtivo. Os frutos são globosos, de coloração verde amarelada e agridoces, são também muito perecíveis e explorados por comunidades que vivem do extrativismo de frutíferas desse bioma. Diante da importância desse fruto e de sua alta perecibilidade, objetivou-se com este estudo avaliar a vida útil de duas variedades de mangaba endêmicas do cerrado (Harconia speciosa var. gardineri e var. cuiabenses) colhidas em diferentes estádios de maturação, armazenadas em temperatura média de 20 ºC. Após armazenamento os frutos foram avaliados físico-quimicamente em relação ao teor de sólidos solúveis, acidez titulável, ratio, firmeza e teor de ácido ascórbico diariamente até sua senescência, detectada...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1927

EFEITO DO TRATAMENTO HIDROTÉRMICO ASSOCIADO AO ETANOL NA QUALIDADE DE MANGA TOMMY ATKINS
Provedor de dados: 196
Autores: Oliveira Vilar, Silvana Belém de; Castro, Maria Fernanda Pontes Penteado Moretzsohn de; Sigrist, José Maria Monteiro; Araújo, Ana Julia Brito; Schmidt, Flavio Luis.
A manga é uma fruta de grande expressão nas exportações brasileiras, porém, como barreira fitossanitária alguns países importadores exigem que as mesmas recebam um tratamento hidrotérmico  para o controle de moscas-das-frutas. Alternativas do uso do etanol no controle de microrganismos e fitopatógenos em vegetais têm sido estudadas. Este trabalho avaliou a influência do tratamento hidrotérmico e sua associação com 1% de etanol na qualidade de mangas cv. Tommy Atkins armazenadas a 10ºC/90%UR. Foram realizados experimentos com 200 frutos em estágio de maturação 2, comparando-se o tratamento controle (mangas lavadas, secas e armazenadas), o tratamento hidrotérmico sem etanol e o tratamento combinando o banho hidrotérmico com 1% de etanol. Concluiu-se que os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pós colheita de frutas.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/260

INFLUÊNCIA DO SUBSTRATO E DO TEOR DE ÁGUA SOBRE A GERMINAÇÃO DE SEMENTES DE SOJA
Provedor de dados: 196
Autores: Jacinto, Júlia Terra Dourado; Benett, Katiane Santiago Silva; Benett, Cleiton Gredson Sabin.
&amp;nbsp; Na cultura da soja, nos per&amp;iacute;odos de germina&amp;ccedil;&amp;atilde;o-emerg&amp;ecirc;ncia, bem como na fase de flora&amp;ccedil;&amp;atilde;o-enchimento de gr&amp;atilde;os a disponibilidade de &amp;aacute;gua &amp;eacute; de extrema import&amp;acirc;ncia para a cultura. O objetivo foi avaliar a influ&amp;ecirc;ncia de diferentes teores de &amp;aacute;gua em diferentes substratos sobre a germina&amp;ccedil;&amp;atilde;o de sementes de soja. O trabalho foi realizado no laborat&amp;oacute;rio da Universidade Estadual de Goi&amp;aacute;s, C&amp;acirc;mpus de Ipameri, utilizando-se sementes de soja variedade BRS 8160. O delineamento utilizado foi o inteiramente casualizado em esquema fatorial 2x6, com dois substratos para...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/219

DIFERENTES SOLUÇÕES E MÉTODOS DE HIDRATAÇÃO DAS SEMENTES DE SOJA NO POTENCIAL FISIOLÓGICO
Provedor de dados: 196
Autores: Rodrigues, Tiago da Silva; de Souza, Hugo Manoel; Dias, Thais Santos; Osório, Christian Rones Wruck de Souza; Binotti, Flávio Ferreira da Silva.
O experimento teve o intuito de estudar a qualidade fisiológica de sementes de soja utilizando extrato aquoso de Cyperus rotundus e biorreguladores sintéticos, sob diferentes métodos de hidratação. O estudo foi realizado na Universidade Estadual de Mato Grosso do Sul, Cassilândia-MS, utilizando o delineamento inteiramente casualizado, sendo realizado em duas etapas. Na primeira etapa avaliou-se o desempenho do extrato aquoso de C. rotundus a 3%, comparando-o com: testemunha (sem condicionamento); controle - água; Auxina (IBA) a 0,2%; Stimulate® a 0,2%; Nitrato de Cálcio Ca (NO3)2 a 0,2%. Na segunda etapa aferiu-se o melhor método de condicionamento, utilizando-se de extrato aquoso de C. rotundus 3%, em quatro processos de hidratação: testemunha, submersão,...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1232

EVALUATION OF CORN HYBRIDS PERFORMANCE IN TWO LOCATIONS OF GOIÁS
Provedor de dados: 196
Autores: Gomes, Leandro Lopes; Buso, Wilian Henrique Diniz; Lima, Janaina Batista; Matos, Helber Garcez; Leão Junior, Laidson Alves.
The objective of this study was to evaluate the agronomic traits and grain yield of corn hybrids in two locations of the North Central region of Goiás. The experimental design was a randomized block, in the 17x2 factorial scheme (17 hybrids and two locations) with four replications. The locations were Itapaci and Ceres. Each plot consisted of two rows of five meters, spaced 0.50 m and rows were sown on the sides, which served as a border. The evaluations occurred in the two central rows, excluding 0.50 m at the extremities. The variables analyzed were: first ear height, plant height, stem, number of ears per plant, number of grain rows, number of grains per row, 1000 grain weight and grain yield (kg ha-1). The hybrids that showed the best conditions for...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2362

OCORRÊNCIA DE PUCCINIA DICHONDRAE - AGENTE CAUSAL DA FERRUGEM - EM ORELHA-DE-RATO (DICHONDRA REPENS)
Provedor de dados: 196
Autores: Diniz, Rayane Louise Candida; Lima, Milton Luiz da Paz; Caetano, Alicionon de Oliveira; Decloquement, Jennifer; Silva, Jakelinny Martins.
Orelha-de-rato (Dichondra repens – Convolvulaceae) é uma planta perene de baixo crescimento, considerada como forrageira. O trabalho teve como objetivo a identificação da ferrugem da orelha-de-rato causada por Puccinia sp. Amostras de folhas de orelha-de-rato foram coletadas no município de Bento Gonçalves, RS, exsicatadas e depositadas na coleção micológica de referência do IF Goiano Câmpus Urutaí e, posteriormente, analisadas em microscópio estereoscópico. Lâminas semi-permanentes e cortes histológicos foram realizados. Para registro dos sintomas e sinais do patógeno fez-se macro e microfotografias. A morfometria das estruturas reprodutivas foi realizada utilizando microscópio óptico. O fitopatógeno apresentou télia de coloração marrom avermelhado,...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1164

ATRIBUTOS QUÍMICOS DE UM NEOSSOLO QUARTZARÊNICO DE CERRADO SOB DIFERENTES SISTEMAS DE USO E MANEJO
Provedor de dados: 196
Autores: de Oliveira, Taine Pereira; Ensinas, Simone Cândido; Barbosa, Giselle Feliciani; Nanzer, Marina Chiquito; Barreta, Paulo Gabriel Vechetin.
Os Neossolos são solos com baixa fertilidade natural, porém, as formas de uso e manejo do solo podem alterar seus atributos químicos do solo, com isso objetivou-se quantificar os teores de pH, H+Al, Al, Ca, Mg, P e K e calcular a SB, CTC, m% e V% num Neossolo Quartzarênico sob vegetação nativa, seringueira solteira, seringueira consorciada com abacaxi, pastagem de Brachiaria sp. com 30 anos, pastagem de Brachiaria brizanta cv. Marandu com 3 anos e área de plantio convencional. As amostras de solo foram coletadas em Cassilândia-MS nas camadas de 0-10, 10-20 e 20-30 cm. Os resultados foram submetidos à análise de variância e quando significativa, as médias dos tratamentos foram agrupadas pelo teste de Scott-Knott (p≤0,05). O sistema de pastagem com 3 anos...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2182

DOSES DE BOKASHI EM COBERTURA NA PRODUÇÃO DE BETERRABA
Provedor de dados: 196
Autores: Silva, Priscilla Nátaly de Lima; Lanna, Natália de Brito Lima; Cardoso, Antonio Ismael Inácio.
A produção orgânica de hortaliças tem apresentado crescimento constante. Porém, ainda há necessidade de pesquisas em algumas etapas da produção, como a adubação. Na cultura da beterraba, são escassas as informações sobre a adubação orgânica em cobertura. Desta forma, objetivou-se com este trabalho avaliar a influência de doses de bokashi aplicadas em cobertura na produção de beterraba. Foram realizados dois experimentos na Fazenda Experimental São Manuel (FCA/UNESP) e estudadas cinco doses de bokashi em cobertura (0, 150, 300, 450 e 600 g m-2) e uma testemunha com cobertura inorgânica, utilizando-se um delineamento experimental de blocos ao acaso, com quatro repetições. No primeiro experimento, a adubação de plantio constou apenas de composto orgânico e no...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1818

COMPATIBILIDADE DE INSETICIDAS UTILIZADOS NO CONTROLE DA MOSCA BRANCA EM SOJA COM Beauveria bassiana
Provedor de dados: 196
Autores: Oliveira, Roberta Pacola; Pessoa, Luis Gustavo Amorim; Loureiro, Elisângela de Souza; oliveira, Marcela Pacola.
Objetivou-se avaliar o efeito de inseticidas utilizados no manejo da mosca branca sobre o fungo entomopatogênico Beauveria bassiana. Os bioensaios foram realizados in vitro, utilizando inseticidas em doses mínima, máxima e média, quando possível. Avaliou-se o crescimento vegetativo, a produção de conídios e a compatibilidade dos produtos com o fungo. Apenas o inseticida contendo piriproxifem na dose máxima não interferiu negativamente na produção de conídios. Todos os inseticidas e doses testadas reduziram significativamente a germinação dos conídios. Somente o inseticida contendo espiromesifeno, na dose média, proporcionou crescimento vegetativo significativamente superior à testemunha, possibilitando sua classificação como compatível com o fungo B....
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2416

CARACTERIZAÇÃO E ESTUDO DA ESTABILIDADE FÍSICA DE SUCO MISTO ADOÇADO DE MANGABA E CAGAITA
Provedor de dados: 196
Autores: Martins da Silva, Herberth Diego; Perfeito, Danielle Godinho de Araújo; da Silva, Anderson Rodrigo; Peixoto, Nei.
O objetivo do trabalho consistiu em desenvolver e avaliar as características físico-químicas e sensoriais do suco tropical misto de mangaba e cagaita e verificar sua estabilidade física. Para isso, foram desenvolvidas três formulações padronizadas em 40% de polpa com as seguintes proporções: Formulação 1) 20% mangaba e 20% cagaita; Formulação 2) 10% mangaba e 30% cagaita; e, Formulação 3) 30% mangaba e 10% cagaita. A caracterização físico-química dos sucos foi avaliada pelo teor de sólidos totais, acidez titulável, pH, sólidos solúveis e ratio. Para avaliação sensorial, cinquenta consumidores não treinados avaliaram aparência, aroma, sabor, textura e impressão global. Após a avaliação sensorial, a formulação de melhor aceitação foi analisada quanto à...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1542

RATES OF APPLICATION OF Azospirillum brasilense IN TOMATO CROP
Provedor de dados: 196
Autores: de Lima, Neberson de Souza Antunes; Vogel, Gabriel Felipe; Fey, Rubens.
The use of plant growth-promoting bacteria (PGPB) may be a promising agronomic practice to improve the growth and productivity of vegetables. The objective of this work was to evaluate the effect of inoculation of Azospirillum brasilense on plant growth and tomato fruit production. Two experiments were carried out: the first one evaluating the growth of the plants in a greenhouse and the second one evaluating the production of fruits under field conditions. The experimental design used in two experiments was the completely randomized 2 x 5 factorial scheme, with four replications. The treatments resulted from the combination of two tomato cultivars (Gaúcho Melhorado and San Marzano) and four inoculant doses (0; 2; 4; 6 e 8 mL kg-1 of seed) containing the...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3142

PHYSICOCHEMICAL EVALUATION AND ANTIFUNGAL ACTIVITY OF ESSENTIAL OIL FROM Bauhinia forficata FLOWER Link (Fabaceae)
Provedor de dados: 196
Autores: Menezes Filho, Antonio Carlos Pereira de; Santos, Douglas Braga; Nascimento, Ronaldo Cezar; Oliveira, Marilene Silva; Castro, Carlos Frederico de Souza.
The essential oil of Bauhinia forficata collected in three locations, Rio Verde, Acreúna and Montividiu – GO, Brazil, had a satisfactory extraction with a yield of 0.038; 0.043 and 0.046%, and the relative density was 0.903; 0.901 and 0.903 g mL-1, respectively, and the positive solubility in ethanol. The percentage of mycelial inhibition in vitro of the essential oil mix was more efficient for the strains of S. sclerotiorum and A. flavus. Slight growth inhibition was observed for C gloeosporioides, which proved to be more resistant to essential oil concentrations used. The essential oil mix of Bauhinia forficata flowers proved to be a great option as an antifungal agent.
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4264

OCORRÊNCIA DE CYCLOCEPHALA MELANOCEPHALA (COLEOPTERA: SCARABAEIDAE) EM SERINGUEIRA
Provedor de dados: 196
Autores: Taira, Tiago Ledesma; Assunção, Paulo Cezar Gomes; Silva, Gilmar Modesto da; Rodrigues, Sérgio Roberto.
Os adultos de Cyclocephala Dejean, 1821 são conhecidos principalmente por sua associação com flores de várias espécies vegetais. Em uma área comercial de seringueira em Inocência, MS, foram observados adultos de C. melanocephala (Fabr., 1775) causando danos. Em plantas de seringueira com 1,0 a 1,20 m de altura, foram quantificados no ponteiro e ápice de trinta plantas, entre 40 a 120 adultos em cada planta, sendo que em sua maioria já estavam mortos e unidos uns aos outros. Os ponteiros e ápices das plantas não apresentavam folhas ou brotações, pois haviam sido consumidos. Devido à produção de látex por essa espécie vegetal, os insetos ao se alimentarem da planta proporcionaram o extravasamento do látex, o que levou ao aprisionamento dos insetos na própria...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/231

VARIABILIDADE ESPACIAL DA RESISTÊNCIA DO SOLO À PENETRAÇÃO E DA PRODUTIVIDADE DO MILHO
Provedor de dados: 196
Autores: da Silva, Fabricio Justino; Oliveira, Carlos Alberto Alves de; Almeida, Leandro da Silva; de Lima, Leomar Paulo; Guimarães, Ednaldo Carvalho.
O presente trabalho teve como objetivo estudar a variabilidade espacial da resistência do solo à penetração (RP), teor de água no solo (U) e a produtividade na cultura do milho. O experimento foi conduzido no ano agrícola de 2015/2016, na fazenda Sobradinho, da propriedade do Instituto Federal do Triângulo Mineiro, Campus Uberlândia. A resistência à penetração foi determinada através do penetrômetro de impacto (modelo IAA/Planasulcar-Stolf) nas profundidades de 0-10, 10-20 e 20-30, Para analisar as variáveis, utilizou-se cálculos da estatística descritiva e técnicas de geoestatística. Para avaliar a dependência espacial das variáveis empregou-se o cálculo da semivariância e do ajuste dos dados ao semivariograma experimental. Para calcular a produtividade,...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1625

SOIL MULCHING AND DEFICIT IRRIGATION WITH WASTEWATER IN THE QUALITY OF ITALIAN ZUCCHINI
Provedor de dados: 196
Autores: Sena, Carolina Carvalho Rocha; Ferreira, Anamaria Achtschin; Evangelista, Zeuxis Rosa; Araujo, Kari Katiele Souza.
Conscious agricultural management, which aims to conserve natural resources, has been the target of contemporary agriculture. In this context, the reuse of water in deficit water depth in agricultural irrigation becomes a viable technique, and this work aimed to evaluate the effect of different irrigation depths with wastewater and soil mulching on the microbiological and postharvest characteristics of the Italian zucchini. The experiment was conducted in the field conditions with a randomized block design in a split-plot arrangement. Four irrigation depths (100%, 85%, 70%, and 55% of the estimated ETc from the Class A Evaporation Pan) and three types of soil mulching (rice husk, double-sided black and white polyethylene film, and uncovered soil) were...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4411

DO EXOGENOUS APPLICATION OF THIAMINE MITIGATES LOW SOIL BASE SATURATION EFFECTS ON BELL PEPPER PLANTS?
Provedor de dados: 196
Autores: Vendruscolo, Eduardo Pradi; Dantas Alves, Vitória; Rodrigues Sant'Ana, Gabriela; Pacheco de Almeida Prado Bortolheiro, Fernanda; Battistuzzi Martins, Murilo; de Castro Seron, Cássio; de Souza, Maria Ingrid; Dantas, Thaise.
O uso intensivo do solo para a produção de hortaliças resulta em elevada degradação do solo e da área de cultivo. A utilização de técnicas e recursos que viabilizem a produção sob condições desfavoráveis pode ser decisiva para agricultura. Desta maneira, o objetivo deste trabalho foi avaliar os efeitos isolados e conjuntos da correção do solo e da aplicação de tiamina sobre o desenvolvimento das plantas de pimentão. Os tratamentos foram compostos por três diferentes saturações de base do solo (36, 60 e 80%), combinadas à aplicação de tiamina via foliar (com e sem) na concentração de 100 mg L-1. Verificou-se que a tiamina ameniza os efeitos da baixa saturação por base do solo sobre as características fisiológicas das plantas de pimentão. Os incrementos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carbon fixation; Biostimulants; Soil management; Plant protection; Fixação de carbono; Bioestimulantes; Manejo do solo; Proteção vegetal.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6803

BIOESTIMULANTE VIA FOLIAR EM ALFACE APÓS O TRANSPLANTIO DAS MUDAS
Provedor de dados: 196
Autores: Izidório, Tarcel Henrique Correia; de Lima, Sebastião Ferreira; Vendruscolo, Eduardo Pradi; de Ávila, Jorgiani; Alvarez, Rita de Cássia Félix.
A alface é considerada a hortaliça folhosa de maior importância nacional. O aumento da demanda e exigência sobre a qualidade do produto estimula a utilização de novas tecnologias, como os bioestimulantes, na etapa produtiva. O objetivo, neste trabalho, foi o de avaliar o efeito da aplicação do bioestimulante comercial Stimulate® via foliar em época de transplantio, sobre as características agronômicas da cultura da alface, cultivar Amanda. O delineamento experimental foi em blocos casualizados com seis tratamentos, compostos por seis doses de bioestimulante (0,0; 3,0; 6,0; 9,0; 12,0; 15,0 mL L-1), aplicadas sobre as mudas de alface transplantadas para a área experimental em quatros repetições. O experimento foi instalado em julho de 2013, na horta...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/257

INORGANIC PHOSPHORUS FORMS IN AN OXISOL UNDER NO-TILL AFTER INDUSTRIAL AND MUNICIPAL RESIDUES APPLICATION
Provedor de dados: 196
Autores: Cardoso dos Santos, Susiane Moura; Antonangelo, João Arthur; Deus, Angélica Cristina Fernandes; Büll, Leonardo Theodoro.
Industrial and municipal residues applied to agricultural crops under no-till (NT) can promote benefits to many soil properties. The reuse of such materials reduces the supply of mineral fertilizers and provides greater economic and environmental sustainability. Besides being attenuators of soil acidity, some of these residues are excellent sources of plant nutrients such as phosphorus (P). Understanding the dynamics of P arising from residues applied in tropical soils is important to assist in crops fertilization management. In this context, the objective was to quantify the inorganic P forms (Pi) through the P fractionation in an Oxisol that received application of municipal and industrial residues. Four residues composed treatments: LC - centrifuged...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2772

FUNGICIDAS PROTETORES E SISTÊMICOS NO CONTROLE DE Corynespora cassiicola EM SOJA
Provedor de dados: 196
Autores: Souza, Matheus Bravo; Vidal, Roberta Luiza.
A mancha alvo da soja vem ganhando notoriedade no Brasil, sendo poucos os estudos que visaram identificar controles químicos eficientes. O objetivo deste trabalho foi avaliar o efeito de fungicidas protetores, sistêmicos e associação entre ambos no controle desta doença, em casa de vegetação. O experimento foi conduzido em delineamento inteiramente casualizado, com sete repetições, utilizando plantas de soja da cultivar M6410 IPRO. O fungicida Oxicloreto de cobre SC foi previamente aplicado nas plantas no estádio V4 e, os fungicidas Trifloxistrobina + Protioconazol, Azoxistrobina + Ciproconazol e Fluxapiroxade + Piraclostrobina, isolados e em associação, foram aplicados após a inoculação dos conídios. As avaliações foram realizadas semanalmente, baseadas...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2032

EFFECTIVENESS REDUCTION OF NUCLEOPOLYHEDROVIRUS AGAINST Chrysodeixis includens DAYS AFTER APPLICATION IN SOYBEAN PLANTS
Provedor de dados: 196
Autores: Botelho, Ana Beatriz Riguetti Zanardo; da Silva, Ivana Fernandes; Ávila, Crébio José.
The use of nucleopolyhedroviruses (NPVs) can provide an effective and environmentally benign alternative to synthetic chemicals. The efficacy and persistence of their occlusion bodies may be affected by several factors. The present study investigated the efficacy of isolate Chin-IA (I-A) (ChinSNPV) on third-instar Chrysodeixis includens larvae after 10 days of its application in soybean plants under semi-field conditions. Two concentrations of virus (2x1011 and 10x1011 PIB ha-1) and water (control treatment) were applied in soybean plants. Leaves were collected 0, 2, 4, 6, 8 and 10 days after application of treatments, and then used as disc format to feed the soybean looper larvae in the lab. It was considered a split plot scheme with a randomized complete...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2901

DIFFERENT PACKAGES IN THE POST-HARVEST QUALITY OF STRAWBERRY (cv. Camarosa)
Provedor de dados: 196
Autores: Sena, Carolina Carvalho Rocha; Camilo, Yanuzi Mara Vargas; Evangelista, Zeuxis Rosa; Araujo, Kari Katiele Souza; Semensato, Leandra Regina.
The method and temperature of storage of a product are the basic agents that make it possible to prolong the post-harvest life of strawberries. In this context, this study aimed to evaluate the use of different packages with the passive modified atmosphere in the post-harvest quality of strawberry (cv. Camarosa). The strawberries were harvested and subsequently transported to the Laboratory of Drying and Post-harvest Storage of Agricultural Products, where they were stored in BOD, at 0ºC, and 90±5% relative air humidity. A completely randomized design was used, in a 3 x 5 factorial scheme (three packages: expanded polystyrene (EPS) packaging + polyvinyl chloride (PVC) film at 0 °C; polyethylene terephthalate (PET) packaging at 0 °C; and without packaging...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3307

DESENVOLVIMENTO INICIAL DO AMENDOINZEIRO SOB DIFERENTES DENSIDADES DE MATOCOMPETIÇÃO COM Urochloa
Provedor de dados: 196
Autores: Lisboa, Lucas Aparecido Manzani; Viana, Ronaldo da Silva; Ribeiro, Filipe Virgílio; de Figueiredo, Paulo Alexandre Monteiro; Ramos, Sérgio Bispo.
Gramíneas e leguminosas competem nos sistemas produtivos, sendo que esta competição depende de suas habilidades específicas para a sua sobrevivência. O objetivo desse trabalho foi avaliar o desenvolvimento inicial de amendoinzeiro sob diferentes densidades de matocompetição com Urochloa. Foi realizado um experimento com delineamento inteiramente casualizado, em esquema fatorial 4 x 5. O primeiro fator foi composto por quatro tipos de gramíneas, ou seja, Urochloa brizantha cv. Paiaguás, Marandu, Piatã e Urochloa ruziziensis; o segundo, por cinco densidades de matocompetição e cinco repetições, totalizando 100 parcelas ou vasos. Após 30 dias da semeadura, foram determinados os seguintes parâmetros: ISPADA – índice spad do amendoim; CEA – condutância...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1670

HETEROSE EM HÍBRIDOS DE MELANCIA
Provedor de dados: 196
Autores: Tavares, Aline Torquato; Lopes, Danilo Alves Porto da Silva; Alves, Francielly Quiteria Guimaraes; Santos, Gil Rodrigues; Nascimento, Ildon Rodrigues.
A melancia é uma curcubitácea bastante difundida no mundo, predominando nos cultivos comerciais o uso de híbridos. Apesar desse cenário, poucos são os trabalhos que relatam a magnitude e efeito da heterose em caracteres de interesse nesta cultura. O objetivo desse trabalho foi estimar a heterose em híbridos de melancia para características agronômicas e qualidade dos frutos. Os tratamentos foram constituídos de 22 genótipos, sendo 15 híbridos experimentais obtidos do cruzamento de seis genitores: quatro cultivares comerciais, duas linhagens experimentais e um híbrido comercial, usado como testemunha. O experimento foi realizado em delineamento de blocos casualizados com três repetições. Os cruzamentos e a análise estatística dos dados foram realizados...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2658

IDENTIFICAÇÃO DE GENÓTIPOS DE FEIJOEIRO COMUM TOLERANTES AO ALUMÍNIO
Provedor de dados: 196
Autores: Fidelis, Rodrigo Ribeiro; Fernandes, Patricia Sumara Moreira; Moreira, Erica Rodrigues; Tavares, Taynar Coelho de Oliveira.
Este trabalho teve como objetivo identificar genótipos de feijão comum tolerantes ao alumínio, em solução nutritiva. O experimento foi conduzido em condições de casa de vegetação, na Universidade Federal do Tocantins – Campus Universitário de Gurupi – TO, em blocos inteiramente casualizados, com seis repetições e tratamentos dispostos em esquema fatorial constituído por 15 genótipos e quatro tratamentos: 0, 3 e 6 mg L-1 de alumínio em pH 4,0 ± 0,2 e 0 mg L-1 de alumínio em pH 6,5 ± 0,2. Foram avaliadas as seguintes características: comprimento da parte aérea, comprimento radicular, massa seca da parte aérea e massa seca radicular. Concluiu-se que existe variabilidade genética entre os genótipos de feijão comum quanto à tolerância ao alumínio. Os cultivares...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1894

ADUBAÇÃO FOSFATADA NO CULTIVO DE HORTALIÇAS PRODUTORAS DE RAÍZES
Provedor de dados: 196
Autores: Nascimento, Mariana Vieira; Fernandes, Luiz Roberto Silva Guimarães; Xavier, Ricardo Caldas; Benett, Katiane Santiago Silva; Silva, Luciana Maria da.
Objetivou-se avaliar os efeitos de fontes e doses de fertilizantes fosfatados sobre o desenvolvimento e a produtividade de hortaliças produtoras de raízes tuberosas. Foram realizados três experimentos distintos, na Universidade Estadual de Goiás - UEG, Câmpus Ipameri-GO, sendo estudado apenas uma espécie em cada um deles. O delineamento utilizado, para cada experimento, foi o de blocos ao acaso, em esquema fatorial 2 x 5, sendo utilizado cinco doses de fósforo (P) e duas fontes de P com quatro repetições. As espécies estudadas foram: cenoura, beterraba e rabanete, as fontes de P utilizadas foram o Superfosfato simples e o Superfosfato triplo. Foram avaliados a altura de planta; diâmetro e comprimento de raiz; número de folhas; teor de P foliar e de raízes;...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2209

DESEMPENHO DE HÍBRIDOS DE DENDEZEIRO (Elaeis guineenses Jacq.) NAS FASES DE PRÉ-VIVEIRO E VIVEIRO
Provedor de dados: 196
Autores: Costa, Sérgio José da; Erasmo, Eduardo Andrea Lemus; Silva, Joedna; Oliveira, Taynar Coelho.
A palma do dendezeiro (Elaeis guineensis) é uma cultura que produz maior quantidade de óleo por unidade de área cultivada entre todas as outras plantas oleaginosas, com ciclo produtivo de 25 a 30 anos, e apresenta elevada capacidade de realizar o sequestro de carbono. Para a produção de mudas é necessário desenvolver cuidados para garantir plantas aptas a serem cultivadas em campo. Diante desse contexto, a presente pesquisa buscou estudar as fases inciais desta planta (pré-viveiro e viveiro) em região de fronteira agrícola no cerrado do Tocantins. Os materiais avaliados foram BRS 2301, BRS 7201, BRS 2528, BRS 2001 e BRS 2501. As variáveis avaliadas foram altura de planta, número de folhas, volume radicular, comprimento de raiz, diâmetro do caule, massa...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1435

EFFECTS OF ALUMINUM ON SEED GERMINATION AND INITIAL GROWTH OF PHYSIC NUT SEEDLINGS
Provedor de dados: 196
Autores: Machado, Juan Sotta; Steiner, Fábio; Zoz, Tiago; Honda, Guilherme Bento; Oliveira, Bruno Leminski Neto de.
Aluminum (Al3+) toxicity is one of the major factors that limit plant growth and crop yield in acid soils. The phytotoxic effects of aluminum on seed germination and initial growth of physic nut (Jatropha curcas L.) seedlings were investigated in the present study. Physic nut seeds were subjected to five levels of aluminum [0 (control), 20, 40, 60 and 80 mg L–1], using the solution-paper method, with eight replications. The experimental unit consisted in a germitest paper roll with 25 physic nut seeds.Treatments were evaluated based on the following tests: first count of germination test (7 days), total germination (12 days) and initial growth of physic nut seedlings (12 days). The addition of 80 mg L–1of Al reduced the first count of germination test...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fisiologia de Sementes.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/248

DESEMPENHO AGRONÔMICO DE CULTIVARES DE ALHO VERNALIZADO E NÃO VERNALIZADO NA REGIÃO SUDESTE DE MATO GROSSO
Provedor de dados: 196
Autores: Biesdorf, Evandro Marcos; Silva, Jefferson Santana; Biesdorf, Elivelton Maciel; de Oliveira, Osvaldo José; Del Conte, Murilo Viotto.
Nos últimos anos, o uso da vernalização tem possibilitado o cultivo de alho nobre (Allium sativum L.) em regiões nas quais as condições de fotoperíodo e temperatura não satisfazem as exigências da cultura. Neste contexto, este estudo teve como objetivo avaliar o desempenho agronômico de 13 cultivares de alho vernalizados e não vernalizados na região sudeste de Mato Grosso. O experimento foi realizado em Santo Antônio do Leverger, MT, de maio a outubro de 2012. Os cultivares de alho não vernalizados testadas foram: Hozan L.V, Hozan, Amarante L.V, Chinês Real, Gigante do Núcleo, Amarante, Caturra, Curitibanos Gigante Roxo. Os cultivares de alho Quitéria L.V, Caçador, Quitéria, e Jonas foram submetidos a um período de vernalização de pré-plantio à 5 oC, por...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/281

EFFECT OF SALINITY ON PHOTOSYNTHETIC AND ENZYMATIC ACTIVITIES AND TUBERIZATION YIELD IN THE GENOTYPE OF POTATO CULTIVAR AGRIA UNDER IN VITRO CONDITIONS
Provedor de dados: 196
Autores: Mousavi, Seyyed Nosrat; Ebadi, Mostafa; Khorshidi, Mahdi; Hokmabadi, Hossein; Masoudian, Nahid.
The aim of this study aimed to investigate the effect of salinity levels on physiological and biochemical properties and tuberization yield of potato, cultivar Agria, in MS culture medium. After preparation and cultivation of tuber, the lateral aerial buds were removed after a few months and cultured in MS medium. After that, healthy samples were prepared and induced at the above-mentioned salinity stress level and transferred to the culture medium. Two weeks later, an air sample was taken, and the physiological and biochemical properties studied in this study (photosynthetic pigments, proline, soluble sugars, anthocyanins, phenolic compounds, and the activity of some antioxidant enzymes) were measured. Finally, salinity stress assessment was evaluated and...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4028

ADUBAÇÃO NITROGENADA NO DESENVOLVIMENTO INICIAL DE UVAIA
Provedor de dados: 196
Autores: Viçosi, Karen Andreon; Costa da Silva, Edvan; Magalhães Barroso, Franciely; Costa, João Paulo; Pina da Silva Berti, Mariana.
A uvaia é uma espécie arbórea nativa utilizada tanto na indústria, quanto no paisagismo e reflorestamento, porém, pouco estudada em relação ao seu manejo, principalmente quando se refere à adubação. Objetivou-se avaliar o efeito de diferentes doses de nitrogênio no transplantio de mudas de Eugenia pyriformis. O experimento foi desenvolvido em casa de vegetação na Universidade Estadual de Goiás, Câmpus Ipameri-GO. Foi utilizado o delineamento inteiramente casualizado, com seis doses de nitrogênio na ocasião do transplantio (0, 50, 100, 150, 200 e 250 kg ha-1), na forma de ureia, com cinco repetições por tratamento. As plantas foram avaliadas aos 30 e 60 dias após o transplantio, obtendo as variáveis altura; diâmetro do caule; número de galhos; massa seca da...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2612

VOLATILIZAÇÃO DE AMÔNIA EM PASTAGEM ADUBADA COM FONTES NITROGENADAS
Provedor de dados: 196
Autores: Chagas, Paulo Henrique Menezes das; Gouveia, Geraldo Candido Cabral; Costa, Geany Giovana Silva da; Barbosa, Willams Ferreira Sousa; Alves, Ana Carolina.
A adubação nitrogenada é essencial para o aumento de produção de forrageiras, porém a fonte de nitrogênio (N) e fatores como o manejo podem ocasionar elevadas perdas de amônia (NH3) por volatilização. O presente trabalho foi conduzido com objetivo de quantificar as perdas de N por volatilização de NH3 em fontes nitrogenadas em pastagem. O experimento foi desenvolvido na Universidade Estadual de Mato Grosso do Sul (UEMS), Unidade Universitária de Cassilândia-MS, utilizando o delineamento experimental em blocos ao acaso com quatro tratamentos (ureia; ureia revestida com polímero; ureia com inibidor de urease; e nitrato de amônia) e cinco repetições. Em todos os tratamentos foi aplicada a dose equivalente a 100 kg ha-1 de N. Para a quantificação da...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1301

DISTRIBUIÇÃO DE GOTAS DE UM PULVERIZADOR HIDRÁULICO DE BARRAS DE BAIXO CUSTO
Provedor de dados: 196
Autores: Romeiro, Bruno Peres; França, Jorge Alfredo luiz; Gonçalves, Wagner Santos; Benett, Cleiton Gredson Sabin.
Em meio à diversidade de componentes do processo de produção agrícola, destaca-se a tecnologia de aplicação de produtos fitossanitários, que é a responsável pela colocação correta dos produtos no alvo. Assim, objetivou-se nesse trabalho avaliar a uniformidade na distribuição das gotas cm-2 em solo descoberto e na parte superior, média e inferior da planta, utilizando um pulverizador hidráulico de barras de baixo custo, para tratores com baixa demanda de potência e de baixo investimento financeiro. O trabalho foi conduzido em área experimental do Instituto Federal Goiano - Câmpus Urutaí, na cidade de Urutaí-GO. Foram realizados quatro experimentos para avaliação do número de gotas cm-2, realizados em delineamento inteiramente casualizado, com dois...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/259

MANEJO DO NITROGÊNIO EM COBERTURA DO FEIJOEIRO DE INVERNO NO SISTEMA PLANTIO DIRETO
Provedor de dados: 196
Autores: Binotti, Flávio Ferreira da Silva; Arf, Orivaldo; Cardoso, Eliana Duarte; Sá, Marco Eustáquio de; Buzetti, Salatier.
O nitrog&amp;ecirc;nio &amp;eacute; o nutriente absorvido em maior quantidade pela cultura do feijoeiro e v&amp;aacute;rios trabalhos t&amp;ecirc;m evidenciado seu efeito positivo na produtividade. O manejo da aduba&amp;ccedil;&amp;atilde;o nitrogenada de cobertura &amp;eacute; de vital import&amp;acirc;ncia para aumentar a efici&amp;ecirc;ncia da planta na utiliza&amp;ccedil;&amp;atilde;o do N e aumentar produtividade. O objetivo foi avaliar o efeito da &amp;eacute;poca de aplica&amp;ccedil;&amp;atilde;o e fontes de nitrog&amp;ecirc;nio em cobertura no crescimento e produtividade do feijoeiro de inverno. O projeto foi instalado no munic&amp;iacute;pio de Selv&amp;iacute;ria (MS), no per&amp;iacute;odo de outono-inverno (2003) em solo classificado como...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/226

CARACTERIZAÇÃO FÍSICO-QUÍMICA DE MÉIS PRODUZIDOS NO ESTADO DE MATO GROSSO DO SUL, BRASIL
Provedor de dados: 196
Autores: Vieira, Gustavo Haralampidou da Costa; Gomes, Maria de Fátima Falcão; Moraes, Atila Norberto; Oliveira, Antônio Franscisco.
O trabalho foi desenvolvido com o objetivo de caracterizar, através de análises físico-químicas, nove amostras de méis oriundas de apiários localizados nos municípios de Cassilândia, Aquidauana e Campo Grande, MS. As amostras foram levadas ao laboratório de análises de alimento da UFMS para determinação dos índices de umidade, sólidos solúveis, cinzas, sólidos insolúveis, reação de Fiehe e reação de Lund, conforme as normas analíticas do Instituto Adolfo Lutz. Todas as amostras foram analisadas em triplicata. Para a umidade foram obtidos valores de 18,6% a 23%. Para os sólidos solúveis foram obtidos valores de 75º a 80 ºBrix. Cinzas apresentaram valores de 0,06% a 0,55%. Sólidos insolúveis variaram de 0,002 a 0,05%. Para a reação de Fiehe apenas uma...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1597

SOJA ASSOCIADA À INOCULAÇÃO E COINOCULAÇÃO DE Bradyrhizobium E Azospirillum APÓS CULTIVOS DE OUTONO-INVERNO
Provedor de dados: 196
Autores: Flauzino, Darlan Souza; Ribeiro, Luan Marlon; Ceccon, Gessí.
Objetivou-se avaliar o desenvolvimento e os componentes de produção da cultura da soja com e sem inoculação de Bradyrhizobium japonicum, e a coinoculação de B. japonicum mais Azospirillum brasilense após cultivos de outono-inverno. O delineamento experimental foi em blocos casualizados, com parcelas subdivididas. As parcelas principais foram os cultivos de outono-inverno (feijão-caupi, Brachiaria ruziziensis, milho solteiro e consórcio de milho-B. ruziziensis), e nas subparcelas a soja BRS 360 RR, sem inoculação (BRS 360-0), inoculada com B. japonicum (BRS 360-CB) e a coinoculação com B. japonicum + A. brasilense (BRS 360-CB+A), em quatro repetições. Os dados foram submetidos à análise de variância e as médias comparadas pelo teste de Tukey...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2001

IN VITRO COMPATIBILITY BETWEEN INSECTICIDES AND THE COMMERCIAL BIOINSECTICIDE AGREE® WG
Provedor de dados: 196
Autores: Loureiro, Elisângela de Souza; Pessoa, Luis Gustavo Amorim; Putrick, Thayla Christiane; Pantaleão, Ariane de Andréa; Dias, Pamella Mingotti.
Compatibility studies are essential for the integration and simultaneous use of chemical and biological pest control methods since they are necessary for an Integrated Pest Management (IPM) program. In this work, the aim was to evaluate the compatibility of insecticides used in soybean and cotton crops for pest control with Bacillus thuringiensis (Bt). The in vitro inoculation technique was used with B. thuringiensis var. kurstaki and B. thuringiensis var. aizawai, in culture medium containing the following insecticides: beta-cyfluthrin (Bulldock®), methomyl (Bazuka®), thiamethoxam + lambda-cialotrina (Engeo Pleno®), zeta-cypermethrin (Fury 200®), acetamiprid (Saurus®), bifenthrin + carbosulfano (Talisman®) and bifenthrin (Talstar®), in Petri dishes. The...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3597

GENERATING GENETIC DIVERSITY THROUGH DIALLEL CROSSES OF PROMISING POTATO CULTIVARS (Solanum tuberosum L.) AND STUDYING CULTIVAR HYBRIDS UNDER WATER DEFICIT STRESS
Provedor de dados: 196
Autores: Vesali, Mohammad Reza; Baradaran, Reza; Hassanpanah, Davoud; Seghatoleslami, Mohammad Javad.
This research was conducted from 2017 to 2018 to produce genetic diversity and examine selected suitable hybrids concerning certain agricultural traits under normal and water-deficit stress conditions in a Zarghostar-Arta company. In 2017, four potato cultivars, namely, Luca, Banba, Esprit, and Agria, were crossed as parents via mutual hybridization based on the diallel method guided by Griffing’s method III. About 8550 true potato seeds were produced, among which 3944 seeds were germinated, and 151 hybrids were selected for culturing on a split-plot with a randomized complete block design involving three replications. The main factors of interest in the design were three irrigation levels (100%, 85%, and 70% water supply requirements), and the sub-factors...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4511

EFICIÊNCIA DE UTILIZAÇÃO DE ADUBAÇÃO ORGÂNICA EM FORRAGEIRAS TROPICAIS
Provedor de dados: 196
Autores: Castro, Camila da Silva; Lobo, Ulisses Gabriel Moraes; Rodrigues, Lucas Matheus; Backes, Clarice; Santos, Alessandro José Marques.
A adubação orgânica pode influenciar de forma positiva e significativa o desenvolvimento de gramíneas forrageiras. Dois experimentos foram instalados em vasos, em casa de vegetação, com o objetivo de avaliar o efeito de doses de esterco bovino no desenvolvimento dos capins Brachiaria brizantha (Syn. Uroclhoa brizantha) cv. Marandu e Panicun maximum cv. Mombaça. O delineamento utilizado para cada experimento foi em blocos ao acaso com quatro repetições. Para o capim-marandu foram utilizados cinco tratamentos constituídos por quatro doses de esterco de bovino curtido: 0; 9; 18 e 27 Mg ha-1 (base seca) e mais um tratamento com adubação inorgânica (AI), na dose recomendada. O experimento com o capim-mombaça consistiu de seis tratamentos: 0, 4,5; 9; 18; 36 Mg...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1144

DIFERENTES TÉCNICAS DE PULVERIZAÇÃO SOBRE O DEPÓSITO DE GOTAS NA CULTURA DO TRIGO
Provedor de dados: 196
Autores: Christovam, Rafael de Souza; Raetano, Carlos Gilberto; Leite, Leonardo Aparecido Inacio; Prado, Evandro Pereira; do Amaral Dal Pogetto, Mário Henrique Ferreira.
A cultura do trigo (Triticum aestivum L.), tem relevante importância no mundo. Ao longo dos tempos, com o surgimento de doenças, foram desenvolvidas pesquisas para buscar a melhor eficiência no controle desses patógenos. Para obter resultados de melhor eficiência em aplicação curativa de fungicidas, o presente trabalho objetivou avaliar técnicas de pulverização sobre o depósito de gotas nas folhas da cultura. Foram realizados dois experimentos na área experimental da FCA/UNESP – Campus de Botucatu, sendo divididos em duas áreas: área de agricultura e área cascalheira. No Experimento I utilizou-se o esquema fatorial 3 x 2, com quatro repetições; foram dispostos três níveis de ar (0; 15; 29 km h-1), dois volumes de pulverização (100 L ha-1 e 200 L ha-1). No...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1914

CARACTERIZAÇÃO DE FRUTOS DE MANGABAS (Hancornia speciosa GOMES) E ESTUDO DE PROCESSOS DE EXTRAÇÃO DA POLPA
Provedor de dados: 196
Autores: Perfeito, Danielle Godinho Araújo; Carvalho, Natália; Lopes, Milene Cristina Mendes; Schmidt, Flávio Luís.
Estudos visando aprimorar a tecnologia de pós-colheita da mangaba se fazem necessários em função da alta perecibilidade da fruta e falta de tecnologias de transformação adaptáveis às condições de microempresas. Nesse estudo frutos de mangaba com três estágios de maturação foram caracterizados quanto a suas propriedades físicas e químicas, além disso foram avaliadas diferentes formas de despolpamento dos frutos em função do rendimento e características da polpa. As características físicas dos frutos determinadas foram o comprimento, diâmetro, massa específica aparente, volume e massa específica. Determinou-se o uso de prévia redução de tamanho dos frutos em multiprocessador sob aquecimento e dois tipos de peneiras em extrator, tipo escovas: com 0,8 e 0,5 mm...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/269

OCORRÊNCIA DE LAGARTAS EM FUNÇÃO DO MANEJO DE INSETICIDAS E UTILIZAÇÃO DE CULTIVARES DE ALGODOEIRO
Provedor de dados: 196
Autores: Pereira, Amanda Casagrande; Martins, Gustavo Luís Mamoré; Tomquelski, Germison Vital.
O objetivo do trabalho foi avaliar a ocorrência de lagartas em função do manejo de inseticidas e modos de utilização de cultivares de algodoeiro. O delineamento foi em blocos casualisados, em esquema fatorial 2 x 3, com seis tratamentos e cinco repetições, totalizando 30 parcelas. Os tratamentos foram: 1) Cultivar Nuopal (com inseticida) (100% Bt); 2) Cultivar Deltaopal (com inseticida) (100% não Bt); 3) Cultivar Nuopal centro (80%) e bordadura Deltaopal (20%) (com inseticida) (80% Bt + 20% não Bt); 4) Cultivar Nuopal (sem inseticida) (100% Bt); 5) Cultivar Deltaopal (sem inseticida) (100% não Bt) e 6) Cultivar Nuopal centro (80%) e bordadura deltaopal (sem inseticida) (80% Bt + 20% não Bt). Realizaram-se amostragens semanais em 10 plantas por parcela de...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1125

BIOLOGICAL EFFECTIVENESS OF ONION PLANT PROTECTION SCHEME
Provedor de dados: 196
Autores: Bondarenko, Anastasia; Tyutyuma, Natalya.
The average yield of bulb onions is still quite low. The purpose of this study was to improve the techniques and methods of cultivating onions using new generation preparations against the background of N180P60K60 in a drip irrigation method. To achieve the objective of this study, field surveys, observations and measurements were carried out using generally accepted methods. The experimental data obtained from the studies were processed using analysis of variance in Excel, which is part of the Microsoft Office installation package. Field experience included both background application of mineral fertilizers, as well as integrated nutrition of plants with Aminofol Plus and Novosil bulb onion growth stimulants and its biological protection with drugs...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bulb onions; Processing; Herbicide; Trips; Weeds; Yield; Bulbo de cebolas; Processamento; Herbicida; Viagens; Ervas daninhas.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6930

PHYSICAL CHARACTERIZATION OF FRUITS AND SEEDS Inga laurina (Sw.) Willd. (Fabaceae - Mimosaceae)
Provedor de dados: 196
Autores: da Silva Oliveira, Carlos Eduardo; Zuffo, Alan Mário; Fonseca, Wéverson Lima; Steiner, Fábio.
The main physical and morphological characteristics of Inga laurina (Sw.) Willd. (Fabaceae –Mimosaceae) fruits and seeds, and correlation estimates between these characteristics were investigate in this study. Mature fruits of I. laurina were collected from matrices trees established in a savannah area located at the municipality of Cassilândia, Mato Grosso do Sul, Brazil. The length, width, and thickness of 100 fruits and 100 seeds were measured. The fresh mass of fruits, pulp and seeds, and seed number per fruit were quantified. Data were analyzed by using descriptive statistics, adjustment of statistical distributions, and Spearman's rank correlation analysis (rS). The I. laurina presents variation in the size and weight of fruits, pulp, and seeds,...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3006

PIGEON PEA INITIAL GROWTH UNDER DIFFERENT CONCENTRATIONS OF ALUMINUM AND COMMERCIAL SUBSTRATE
Provedor de dados: 196
Autores: Rodrigues, Gustavo Araújo; Pereira, Breno de Jesus; Santos, Anacleto Ranulfo dos; Costa, Francielle Medeiros; Anjos, Gilvanda Leão dos.
The incorporation of organic substrate into the soil can reduce aluminum toxicity in pigeon pea (Cajanus cajan (L.) Millsp.) plants, making it a viable alternative for use by small farmers in acidic soil regions such as the northeast semi-arid regions of Brazil that contain toxic aluminum in the soil. The aim of this study was to evaluate the effect of increasing aluminum doses and different commercial substrate concentrations on the initial growth of the pigeon pea. The experiment was undertaken in a greenhouse using a completely randomized design with a 5 × 3 factorial scheme. The first factor consisted of five doses of aluminum (0, 13.5, 27, 54, and 108 mg L-1) and the second factor consisted of three percentages of commercial substrate Vivato Slim Pro®...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5046

APLICAÇÃO FOLIAR DE EXTRATO DE ALGA NA CULTURA DA BATATA
Provedor de dados: 196
Autores: Backes, Clarice; Lyra Villas Bôas, Roberto; Marques dos Santos, Alessandro José; Ribon, Adriana Aparecida; Bardiviesso, Diógenes Martins.
No presente trabalho, objetivou-se avaliar os efeitos da aplicação foliar do extrato da alga Ascophyllum nodosum no crescimento e produtividade da cultura da batata. O experimento foi conduzido dentro de uma área de plantio comercial de batata no município de Itapetininga-SP. Utilizou-se a variedade Asterix, em um delineamento de blocos ao acaso, com cinco tratamentos e cinco repetições. Os tratamentos foram constituídos de cinco doses de extrato de alga Ascophyllun nodosum, 0; 0,5; 1; 2; e 4 L ha-1, aplicado às plantas via foliar. Ao longo do ciclo foram avaliadas as variáveis: altura da planta; número de hastes por planta; intensidade de coloração verde da folha (ICV); concentração de nutrientes nas folhas e área foliar da quarta folha. Ao final...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1567

EFICIÊNCIA DA APLICAÇÃO DE NUTRIENTES VIA SEMENTE E FOLIAR NA CULTURA DO AMENDOIM
Provedor de dados: 196
Autores: Silva, Raphaela Maceió; Viana, Jeandson Silva; Gonçalves, Edilma Pereira; Moraes, Guilherme Souza de.
O adequado suprimento de nutrientes é essencial para promover o crescimento e desenvolvimento das plantas e assegurar elevados níveis de produtividade das culturas. Este estudo teve como objetivo avaliar a eficiência da aplicação de cálcio (Ca), boro (B), cobalto (Co) e molibdênio (Mo) nas sementes associado à aplicação foliar de Ca + B em diferentes épocas na cultura do amendoim. O ensaio constituiu das seguintes aplicações de nutrientes: aplicação de Co, Mo, Ca, e B nas sementes associado a aplicação foliar de Ca e B aos 0, 17, 23, 29, 35 e 41 dias após a semeadura (DAS) e um tratamento adicional sem aplicação de nutrientes (controle). Os resultados foram submetidos à análise de variância e as médias agrupadas pelo teste de Scott-Knott, a 5% de...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1533

MODELAGEM HIPSOMÉTRICA DE Eucalyptus grandis W. HILL EX MAIDEN. NO SUDESTE DO ESTADO DE GOIÁS
Provedor de dados: 196
Autores: Soares, Kálita Luis; Costa, Lidiomar Soares da; Araújo, Matheus da Silva; Calixto Júnior, José Eduardo Dias; Interamnense, Márcio Torreão.
A mensuração da altura é considerada difícil, exigindo um maior tempo para sua determinação. Por isso, em trabalhos de inventários em florestas equiâneas normalmente são mensuradas as alturas de poucas árvores em cada parcela e as alturas das demais árvores do povoamento são estimadas por meio de relações hipsométricas. O presente trabalho objetivou avaliar o ajuste e selecionar modelos hipsométricos para estimar a altura total de povoamento clonal de Eucalyptus grandis W. Hill ex Maiden. no sudeste do Estado de Goiás. O trabalho foi desenvolvido em um plantio florestal clonal de Eucalyptus grandis W. Hill ex Maiden. de um povoamento com área total de 76 hectares. Os dados utilizados no ajuste dos modelos foram provenientes da medição do diâmetro a 1,30 m...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2184

EFICIÊNCIA DE INSETICIDAS NO CONTROLE DE Chrysodeixis includens (LEPIDOPTERA: NOCTUIDAE) NA CULTURA DA SOJA
Provedor de dados: 196
Autores: Martins, Gustavo Luís Mamoré; Tomquelski, Germison Vital.
O objetivo do trabalho foi estudar a eficiência de alguns inseticidas para o controle de Chrysodeixis includens (Lepidoptera: Noctuidae) em duas safras na cultura da soja. Desenvolveu-se dois experimentos, sendo um na safra 2006/07 (experimento 1) e outro na safra 2007/08 (Experimento 2), no município de Chapadão do Sul (MS), sendo delineados em blocos ao acaso com 7 tratamentos e 4 repetições (experimento 1) e 6 tratamentos e 4 repetições (experimento 2). No experimento 1, os tratamentos foram: 1. Testemunha; 2. Profenofós + Lufenuron (151 g i.a. ha-1); 3. Metomil (7,5 g i.a. ha-1); 4. Teflubenzuron (384 g i.a. ha-1); 5. Thiodicarb (24 g i.a. ha-1); 6. Clorpirifós (28,8 g i.a. ha-1); 7. Fenitrotion + esfenvarelate (384 g i.a. ha-1). No experimento 2,...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/396

TRICHODERMA NA PROMOÇÃO DO CRESCIMENTO VEGETAL
Provedor de dados: 196
Autores: Chagas, Lillian França Borges; Chagas Junior, Aloisio Freitas; Soares, Layssah Passos; Fidelis, Rodrigo Ribeiro.
Fungos do gênero Trichoderma são uns dos principais micro-organismos de importância para o aumento do crescimento vegetal. Desta forma, objetivou-se com este trabalho avaliar a eficiência da inoculação de Trichoderma asperellum UFT 201, como promotores de crescimento vegetal nas culturas da soja, feijão caupi, arroz e milho, em casa de vegetação. As características de biomassa das culturas foram determinadas através da massa seca da parte aérea, massa seca da raiz e massa seca total, bem como a eficiência relativa. Nas diferentes culturas estudadas, a inoculação de T. asperellum UFT 201 foi superior para as características de biomassa, mostrando o potencial como promotor de crescimento, com aumento acima de 60% em relação à testemunha, para todas as...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1529

ADUBAÇÃO DE COBERTURA COM ENXOFRE NA CULTURA DA RÚCULA
Provedor de dados: 196
Autores: Soares, Michel Moreira; Bardiviesso, Diógenes Martins; Barbosa, Willams Ferreira Souza; Barcelos, Michelle Nunes.
O enxofre apresenta grande importância para o desenvolvimento das culturas, sendo normalmente constatado o aumento da produtividade com o fornecimento deste nutriente em cobertura, entretanto, há poucos estudos que relatam o efeito da adubação com enxofre na cultura da rúcula. Portanto, o objetivo foi de avaliar o desenvolvimento da cultura da rúcula submetida à adubação com enxofre aplicado em cobertura. O delineamento experimental utilizado foi o de blocos ao acaso, com cinco tratamentos (0; 20; 40; 60; 80 mg de S planta-1) e quatro repetições, cada parcela foi constituída por 5 vasos, com quatro plantas cada. Durante o desenvolvimento das plantas foi avaliada a intensidade de cor verde das folhas aos 16, 23 e 30 dias após a emergência. Aos 30 dias após...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1171

EVALUATION OF Azospirillum brasilense DOSE RESPONSE ON FRESH AND DRY MATTER OF SHOOT AND ROOT OF CORN PLANTS
Provedor de dados: 196
Autores: do Amaral Júnior, Wellington Elias; Rodrigues Esteves, Flávia; Pereira de Menezes Filho, Antonio Carlos; Abadia Ventura, Matheus Vinicius.
Zea mays (corn) is one of the leading crops focused on producing food and feed for humans and animals. The use of diazotrophic bacteria such as Azospirillum brasilense demonstrates a positive effect on nitrogen availability, a primordial element for the development of this plant. This study aimed to evaluate the gain of the fresh and dry matter of shoots and roots in a corn cultivar inoculated with A. brasilense at different doses. The experiment was carried out in pots containing soil. The corn seeds, cultivar Agroceres® 5055, were inoculated with A. brasilense at doses between 100 to 250 mL 20 kg-1. It was observed that inoculation with A. brasilense positively affected fresh and dry matter gain of both shoot and roots between doses of 100-200 mL 20 kg-1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrogen; Corn; Nitrogen fixing bacteria; Azospirillum; Nitrogênio; Milho; Bactéria fixadora de Nitrogênio; Azospirillum.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6993

ESPÉCIES DE Partamona SCHWARZ, 1939 (HYMENOPTERA: APIDAE: MELIPONINAE) EM FRAGMENTO DE CERRADO NO MUNICÍPIO DE CASSILÂNDIA, MS, BRASIL
Provedor de dados: 196
Autores: Barbosa, Carlos Aparecido Ferreira; Souza, Émerson Guilherme Aguiar; Rodrigues, Sérgio Roberto; Vieira, Gustavo Haralampidou da Costa.
As abelhas Meliponini desempenham importantes atividades de polinização nos diferentes ambientes e para o gênero Partamona, poucas são as informações conhecidas. Desta forma, foram desenvolvidos estudos para a localização e identificação de espécies de Partamona que ocorrem em um fragmento de Cerrado caracterizado como Savana Arbórea Densa, em Cassilândia, MS. O estudo foi realizado em uma área de oito hectares localizada, em uma área de preservação denominada de Salto. Foram encontrados 22 ninhos de Partamona, sendo 20 ninhos de P. nhambiquara Pedro &amp;amp; Camargo, 2003 e dois ninhos de P. combinata Pedro &amp;amp; Camargo, 2003. Para P. nhambiquara foram encontrados onze ninhos em uma parede de sustentação, oito ninhos em uma árvore de figueira e um...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/243

DECOMPOSITION OF THE REMAINING STRAW DURING SOYBEAN GROWING IN THE MIDWESTERN PARANÁ, BRAZIL
Provedor de dados: 196
Autores: Wenneck, Gustavo Soares; Saath, Reni; Araujo, Larissa Leite de; Pereira, Gustavo Lopes; Rezende, Roberto; Wenneck, Guilherme Soares.
Crop biomass plays an important role, especially in tropical and subtropical crops that adopt the no-tillage system, whose decomposition is related to material composition and environmental conditions. The objective of this work was to analyze the decomposition of straw remaining from autumn/winter crops in the development of soybean in succession in the Midwest region of Paraná. The experiment was conducted between 2019 and 2021 in a completely randomized design, with eight treatments (spontaneous, black oat, brachiaria, corn, wheat, oilseed radish, corn + brachiaria, and black oat + oilseed radish) and four replications. After autumn/winter cultivation, biomass samples were dried and placed in nylon bags, returning to the original plot during soybean...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Land cover; Organic matter; No-tillage system; Cobertura de solo; Matéria orgânica; Sistema plantio direto.
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6534

YIELD OF MARGARET QUEEN RADISH HYBRID ACCORDING TO THE SPACING
Provedor de dados: 196
Autores: Santos, Marlei Rosa dos; Moreira, Romário da Silva; Silva, Tadeu Barbosa Martins; Sousa, Ronildo Almeida de; Almeida, Rubenalto da Silva; Carreio, Laércio Gomes.
Currently, some important hybrids have replaced traditional radish cultivars, without, however, developing necessary studies on the best planting density for different Brazilian conditions. Thus, the present study aimed to evaluate the effect of spacing between rows and plants on the development and yield of the ‘Margaret Queen’ radish hybrid. A randomized blocks experimental design with four replications in a 3 x 3 factorial scheme was used. Three row spacings (10, 15, and 20 cm) and three spacings between plants in the row (3, 6, and 9 cm) were evaluated. The seeds were sown in furrows at 1.0 cm deep, and the harvest was carried out at 28 days after sowing. The following were determined: number of leaves, root diameter, root length, average root weight,...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4372

JATROPHA PRODUCTION IN FUNCTION OF ORGANIC FERTILIZATION WITH CASSAVA WATER AND COW URINE
Provedor de dados: 196
Autores: Nápoles, Fábio Agra de Medeiros; Aires Souza, José Thyago; Azevedo, Carlos Alberto Vieira de; Souza, Giliane Aparecida Vicente da Silva; Oresca, Denizard; Oliveira, Suenildo Josemo Costa.
The objective of this study was to evaluate the production of jatropha (Jatropha curcas L.) submitted to fertilization with cow urine and cassava water. The experiment was conducted under field conditions in the municipality of Lagoa Seca, Paraíba State, Brazil. A 5 x 5 factorial scheme was used in a randomized complete block design with 25 treatments and 4 replicates, using different volumes of cow urine and cassava water. Irrigation was performed twice a week corresponding to 100% of ET0, where all plants received the same water blade. The syrup with 750 mL of cassava water and 750 mL of cow urine provided a greater number of fruits (33.00); however, the larger green mass of the fruits (224.59 g) was obtained when cow urine was added into 1,000 mL of...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1855

VIBRAÇÃO OCORRENTE SOBRE O CORPO INTEIRO DO OPERADOR DE TRATOR AGRÍCOLA EM ENSAIO PADRONIZADO
Provedor de dados: 196
Autores: Sandi, Jefferson; Paulo Testa, João Vitor; Battistuzzi Martins, Murilo; Fiorese, Diego Augusto; Pereira Lanças, Kléber.
Uma das principais variáveis que afetam o rendimento produtivo dos operadores de tratores agrícolas causando sérios problemas de saúde é a vibração gerada durante o funcionamento da máquina. Este trabalho teve como objetivo avaliar a vibração que incide sobre o corpo inteiro do operador através do assento de um trator agrícola mediante ensaio em pista de vibração padronizada. Empregou-se um trator de 92 kW de potência em quatro condições de lastragem e quatro velocidades de deslocamento. Utilizou-se um acelerômetro de três eixos fixado sobre o assento do trator para avaliação do efeito da vibração no corpo do operador. Foram obtidos os parâmetros aceleração média resultante, valor da dose de vibração, fator de crista e projeção de dose para 8 horas de...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2152

AGENTES QUÍMICOS UTILIZADOS NO CONDICIONAMENTO FISIOLÓGICO MINIMIZAM ESTRESSES EM SEMENTES DE MILHO NO ESTABELECIMENTO INICIAL?
Provedor de dados: 196
Autores: Burin, Caio Cesar; Binotti, Flávio Ferreira da Silva; Silva, Elijanara Raissa; Silva, Fernando Lourenço Santana; Costa, Edilson.
As substâncias químicas utilizadas no condicionamento fisiológico pode ser uma das técnicas utilizadas para reduzir os estresses causados pelas adversidades que acometem as sementes de milhos durante a emergência e o estabelecimento da cultura. Objetivou-se avaliar diferentes substâncias utilizadas no condicionamento fisiológico de sementes de milho para a superação de estresses abióticos no momento da germinação e emergência. O delineamento experimental foi inteiramente casualizado em esquema fatorial 2 x 5, sendo constituído de dois lotes de sementes, e quatro agentes químicos utilizados no condicionamento fisiológico, mais a testemunha. As sementes foram submetidas a diferentes estresse abióticos: baixa temperatura, hipóxia, estresse salino e restrição...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Calcium Nitrate; Potassium Nitrate; Priming; Zea mays.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5780

COMPARAÇÃO ENTRE MÉTODOS PARA A AVALIAÇÃO DO VIGOR DE SEMENTES DE ALGODÃO
Provedor de dados: 196
Autores: Souza, Gabriel Elias de; Steiner, Fábio; Zoz, Tiago; Oliveira, Silvia Sanielle Costa de; Cruz, Sihélio Júlio Silva.
Em um programa de controle de qualidade, a avaliação do vigor de sementes é fundamental e necessária para o sucesso da produção. Métodos que possibilitam a rápida avaliação do vigor das sementes são de grande interesse no controle de qualidade das empresas produtoras. O objetivo foi avaliar a eficiência de diferentes testes de vigor na avaliação da qualidade fisiológica de sementes de algodão (Gossypium hirsutum L., cv. FM 951LL), buscando a diferenciação de lotes. O estudo foi realizado no Laboratório de Análises de Sementes da Universidade Estadual Paulista – FCA/UNESP, Botucatu–SP, em dezembro de 2011. O delineamento experimental utilizado foi o inteiramente ao acaso com cinco tratamentos e quatro repetições. Cinco lotes de sementes da Cultivar FM 951LL...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agronomia.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/237

MANAGEMENT OF Urochloa ruziziensis WITH GLYPHOSATE IN INTEGRATED SYSTEM WITH GLYPHOSATE-RESISTANT CORN
Provedor de dados: 196
Autores: Corrêa, Gilmarcos de Carvalho; Pinto, Cássio Augusto; de Freitas, Evandro Macedo; Cunha Jr., Luís Carlos; Morgado, Cristiane Maria Ascari.
This study aimed to evaluate the efficiency of the glyphosate doses in the suppression of Urochloa ruziziensis, to avoid the excessive competition of forage, intercropped with corn in an integrated crop-livestock system. The experiment was conducted in the experimental area of the Escola de Agronomia, of the Universidade Federal de Goiás with glyphosate-resistant corn (Zea mays L.) and Urochloa ruziziensis. The experimental design was randomized blocks with five treatments and four replications in a factorial scheme, with five herbicide doses x three evaluation periods. Treatments were control - non-sprayed, glyphosate herbicide at doses of 72, 144 and 288 g a.e. ha-1, and standard treatment of 8 g a.i. ha-1 of the nicosulfuron herbicide. The sowing was...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3377

ADUBAÇÃO FOLIAR DE NITROGÊNIO EM CAPIM MOMBAÇA (Panicum maximum cv. Mombaça)
Provedor de dados: 196
Autores: Pietroski, Marizane; Oliveira, Reginaldo de; Caione, Gustavo.
A adubação nitrogenada proporciona incremento na produtividade das pastagens, sendo a aplicação foliar uma alternativa complementar. Assim, objetivou-se avaliar o efeito da aplicação foliar de nitrogênio (N) na produção de forragem, acúmulo de N, proteína bruta e no índice de cor verde das folhas de capim Panicum maximum cv. Mombaça. O experimento foi realizado em uma propriedade rural situada no município de Nova Guarita - MT, Brasil. O delineamento experimental foi em blocos casualizados com quatro repetições. Os tratamentos foram constituídos pela aplicação foliar de cinco doses de N (0 (controle), 15, 30, 45 e 60 kg ha-1 de N). Foram conduzidos dois ciclos, realizando-se a coleta da forragem para a determinação da massa de matéria verde e seca, teor e...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/684

FEIJOEIRO COMUM IRRIGADO SUBMETIDO Á DIFERENTES DOSES DE MANGANÊS E ÉPOCAS DE APLICAÇÃO
Provedor de dados: 196
Autores: Rodrigues, Mateus Gonçalves; Ramos, Eliene Wellita Vieira Barcelos; Buso, Wilian Henrique Diniz.
Brazil is the largest beans producer, and this legume is one of the primary sources of plant-based proteins. Some minerals, such asmanganese, are essential for this crop development. From the socio-economic importance of the beans crop, this study aims to evaluate theagronomic performance of irrigated common beans grown under different doses of manganese on two application periods. The experiment was conducted in the experimental area of the Instituto Federal Goiano, Campus Ceres (GO), adopting an experimental design arranged in a 2x4 factorial scheme with four replications, comprising two periods of application (V4 and R5 phenological stages) and four Mn doses (0, 150, 300, 450 g ha-1). The variables evaluated were plant height (m), number of pods per...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertilization; Agronomic Parameters; Grain Yield; Adubação; Parâmetros Agronômicos; Produtividade.
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6018

GROWTH, YIELD AND POST-HARVEST EVALUATION OF LETTUCE PLANTS SUBJECTED TO DIFFERENT LEAF SILICON CONCENTRATIONS
Provedor de dados: 196
Autores: Neves, Myriam Galvão; da Silva Júnior, Mário Lopes; de Oliveira Neto, Candido Ferreira; Okumura, Ricardo Shigueru; Pamplona Albuquerque, Gerson Diego; Santiago, Tiago de Souza.
Lettuce is considered the most produced and consumed leafy vegetable; however, it has short post-harvest life, which generates significant losses for both producers and consumers. Studies have proven the beneficial effect of silicon on fruits and vegetables. Therefore, the aim of the current study is to evaluate the influence of leaf calcium silicate application on the growth, biomass production and postharvest conservation of curly lettuce. The experiment was carried out in greenhouse at Federal Rural University of Amazonia, Parauapebas Campus / PA. It followed a completely randomized design (CRD) with five Si concentrations (0.0, 2.0, 4.0, 6.0 and 8.0 mg L-1) and eight repetitions, which totaled 40 plants. Plants were grown in plastic pots (capacity = 3...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4448

EFFECT OF SELENIUM ON GROWTH AND PHYSIOLOGICAL TRAITS OF BASIL PLANT (Ocimum basilicum L.) UNDER ARSENIC STRESS CONDITIONS
Provedor de dados: 196
Autores: Rostami, Mahdi; Abbaspour, Hossein.
Arsenic is one of the common toxins in the environment that enters the environment through natural and artificial sources and causes stress in plants through various ways, including the effect on growth and metabolism of the plant. Further, the absorbance of this element in plants and the entry into the food chain create toxicity for humans. On the other hand, Selenium is a non-biological stress reliever and has a considerable impact on improved plant growth and photosynthesis and reduced stress. Due to the interaction of Arsenic and Selenium in soil and different plants and the importance of Basil plant, an experiment was performed to investigate the effect of Selenium on growth and some physiological traits of Basil plant (Ocimum basilicum L.) under...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3324

ENRAIZAMENTO DE ESTACAS CAULINARES DE Piper crassinervium Kunth SOB DIFERENTES CONCENTRAÇÕES DE ÁCIDO INDOLBUTÍRICO
Provedor de dados: 196
Autores: Nunes Gomes, Erik; Krinski, Diones.
O objetivo do presente trabalho foi avaliar o efeito de diferentes concentrações do regulador vegetal ácido indolbutírico (AIB) no enraizamento e brotações de estacas caulinares de Piper crassinervium. Estacas caulinares de 12±1 cm, contendo uma folha reduzida a um terço de seu tamanho, tiveram suas bases imersas por 15 segundos em soluções hidroalcoólicas (50%) com concentrações de zero, 500, 1000, 2000 e 4000 mg L-1 de AIB. Após 45 dias da instalação do experimento, foram avaliadas as porcentagens de sobrevivência, enraizamento, estacas que mantiveram as folhas na região apical (retenção de folhas) e estacas com emissão de novas brotações, número, comprimento médio e massa seca de raízes e massa seca de brotações. Foram observadas altas porcentagens de...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1926

CRESCIMENTO VEGETATIVO DE MORANGUEIRO ATRAVÉS DO USO DE PROMOTORES DE CRESCIMENTO
Provedor de dados: 196
Autores: Richter, Adrik Francis; Ramos, Rodrigo Ferraz; Rohrig, Bruna; Tonin, Jeferson; Marks Machado, Jose Tobias.
O objetivo do presente trabalho foi avaliar os efeitos da inoculação individual e da coinoculação de Trichoderma e rizóbio, e a incorporação de silício, com e sem associação aos inoculantes, no crescimento vegetativo em mudas de morangueiro. O delineamento experimental foi em blocos casualizados, com oito tratamentos e quatro repetições, e duas plantas por repetição. As avaliações foram realizadas aos 22 e 55 dias após o transplantio. O tratamento com Trichoderma influenciou significativamente as variáveis ‘diâmetro de coroa’ e ‘massa seca da coroa’, enquanto o tratamento com aplicação de silício influenciou de forma significativa as variáveis ‘área radicular’, ‘massa fresca de raiz’, ‘massa seca de raiz’, ‘massa fresca de trifólios’ e ‘massa fresca total...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2564

TEOR E FITOQUÍMICA DE ÓLEO ESSENCIAL DE MANJERICÃO EM DIFERENTES HORÁRIOS DE COLHEITA
Provedor de dados: 196
Autores: Alcantara, Francisca Dayanne de Oliveira; da Silva, Toshik Iarley; Maciel, Tamires Coelho Matias; Marco, Cláudia Araújo; da Silva, Flávio Batista.
O manjericão (Ocimum basilicum) é uma das plantas medicinais e aromáticas mais consumidas no mundo, sendo seu óleo essencial amplamente utilizado nas indústrias químicas, farmacêuticas e de flavorizantes. No entanto, muitos fatores podem influenciar no teor do óleo essencial, dentre eles o horário de colheita das plantas. Com vista nisso, o objetivo deste trabalho foi avaliar o teor e fitoquímica do óleo essencial em cultivares de manjericão submetidos a diferentes horários de colheita. O experimento foi conduzido no Centro de Ciências Agrárias e da Biodiversidade da Universidade Federal do Cariri, Crato, Ceará. O delineamento experimental utilizado foi em blocos casualizados em esquema fatorial 2 x 4, com três repetições. Os fatores foram dois cultivares...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1682

GA3 EM SEMENTES DE TOMATEIRO: EFEITOS NA GERMINAÇÃO E DESENVOLVIMENTO INICIAL DE MUDAS
Provedor de dados: 196
Autores: Vendruscolo, Eduardo Pradi; Campos, Luiz Fernandes Cardoso; Martins, Angélica Pires Batista; Seleguini, Alexsander.
A obtenção de mudas de qualidade é uma fase crítica na produção de hortaliças, interferindo diretamente no desenvolvimento e produção da cultura. Portanto, buscam-se tecnologias que possibilitem a formação de mudas sadias e vigorosas. Neste sentido, objetivou-se, por meio deste trabalho, avaliar o efeito do tratamento de sementes de tomateiro com diferentes doses de ácido giberélico aplicado isolado ou em conjunto com outros fitormônios na germinação e crescimento inicial de mudas de tomateiro “Santa Clara”. O estudo caracterizou-se como um fatorial 2x6, conduzido em blocos inteiramente casualizados. Os fatores estudados consistiram da utilização de duas fontes de ácido giberélico (solução de GA3 e bioestimulante) e seis doses (0; 0,5; 1; 1,5; 2; 2,5 mg...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1165

ASPECTOS BIOMÉTRICOS DE FRUTOS E SEMENTES DE CAESALPINIA FERREA MART. EX TUL. PROVENIENTES DO SEMIÁRIDO BAIANO
Provedor de dados: 196
Autores: Silva, Reginaldo Muniz da; Cardoso, Adriana Dias; Dutra, Fabrício Vieira; Morais, Otoniel Magalhães.
A biometria de frutos e sementes fornece informações para a conservação e exploração da espécie, permitindo usá-los de forma eficaz e sustentável. Além disso, é considerado instrumento importante para detectar a variabilidade genética dentro de populações e relações com fatores ambientais. Assim, o objetivo do trabalho foi avaliar a morfometria de frutos e sementes da espécie Caesalpinia ferrea Mart. ex Tul.  provenientes de Vitória da Conquista, BA. Para avaliação da biometria foram coletados cem frutos maduros de diferentes árvores matrizes. As características avaliadas foram: comprimento, largura e espessura medidos na linha mediana dos frutos e das sementes com auxílio de um paquímetro digital. O comprimento, largura e espessura média encontrada para...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1427

AGRONOMIC EFFICIENCY OF FERTILIZERS BASED ON HUMUS, ROCK POWDER, AND MINERALS ON SOYBEAN YIELD IN PARAGUAY-PY
Provedor de dados: 196
Autores: Marques, Mônica Lau da Silva; Jesus, Jéssica Maria Israel de; Santos, Wanderson Moreira dos; Silva, Jeferson Wendling Graciano; Martins, Adriana Lau da Silva; Marques, Valter Santos.
Soybean is the most commercially cultivated crop in Paraguay, and obtaining high yields requires the application of large amounts of fertilizers, raising the cost of production. Developing strategies for the efficient use of applied nutrients is necessary. Therefore, the study aimed to evaluate the agronomic efficiency of combinations of mineral fertilizers with organic matter and rock powder in the development, nutrition, and yield of soybean. The experiment was carried out in Hernandarias, Paraguay, in the 2016-2017 harvest. The different fertilizers influenced the absorption of Zn, Mg and K, and grain yield. Among the treatments, the highlight was the agronomic efficiency index obtained by the replacement of 30% of mineral fertilizer by humus,...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4364

COMPATIBILITY OF AZOXYSTROBIN AND CYPROCONAZOLE ON PLANT GROWTH-PROMOTING MICROORGANISMS
Provedor de dados: 196
Autores: Rocha, Weslany Silva; Silva, Mara Caroline Alves da; Machado Filho, Gilberto Coutinho; dos Santos, Mauro Gomes; Chagas Júnior, Aloísio Freitas; Santos, Manoel Mota dos.
Avoiding the toxicity effect of chemical fungicides on rhizobacteria is a sustainable alternative for agroecosystem management. Rhizobacteria, whose bioprotective and plant growth-promoter potential have been reported in the literature, lack studies on their performance in integrated management with pesticides. Thus, this study aimed to evaluate the effects of azoxystrobin + cyproconazole on the growth of Bacillus subtilis, Streptomyces seoulensis, and Bradyrhizobium japonicum. Three independent experiments were set up, i.e., one for each microorganism, and carried out in a completely randomized design in a factorial scheme (3 × 6), with three doses (recommended by the manufacturer, half, and twice) and six periods of evaluations (48, 96, 144, 192, 240,...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5281

PRODUTIVIDADE E CARACTERÍSTICAS AGRONÔMICAS DA CANA-DE-AÇÚCAR EM DIFERENTES SISTEMAS DE PREPARO DO SOLO
Provedor de dados: 196
Autores: Moraes, Emmerson Rodrigues de; Domingues, Luis Augusto da Silva; Medeiros, Matheus Henrinque; Peixoto, Joicy Vitória Miranda; Lana, Regina Maria Quintão.
O preparo do solo pode contribuir para a melhoria das condições físicas e químicas objetivando o adequado desenvolvimento da cultura da cana-de-açúcar. O objetivo foi avaliar a interferência de diversos tipos de preparo de solo e do plantio direto nas características agronômicas e produtividade da cana-de-açúcar em uma área de reforma. O experimento foi conduzido no município de Goianésia (GO) em um Latossolo Vermelho-Amarelo de textura média, utilizando-se a variedade IAC 87-3396. O delineamento experimental utilizado foi o de blocos casualizados com seis tratamentos e quatro repetições. Os tratamentos foram: T1) dessecação + calcário + aração + gradagem; T2) calcário + subsolador + gradagem; T3) dessecação + calcário + plantio direto; T4) dessecação +...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/992

POTENCIAL FISIOLÓGICO DE SEMENTES DE SOJA EM DIFERENTES DOSES E ÉPOCAS DE APLICAÇÃO DE ZINCO
Provedor de dados: 196
Autores: Oliveira, Fernando Castro de; Benett, Cleiton Gredson Sabin; Benett, Katiane Santiago Silva; Arruda, Natália; Vieira, Bruna do Carmo.
A soja é uma das culturas mais importantes do mundo, porém, quando cultivada em solos com deficiências de nutrientes pode influenciar negativamente no potencial fisiológico das sementes. O objetivo desta pesquisa é avaliar o efeito de doses e épocas de aplicação de zinco no potencial fisiológico de sementes de soja, cultivada em solo da região do Cerrado. O experimento foi instalado no município de Ipameri – Goiás, utilizou-se o delineamento inteiramente casualizado, em esquema fatorial 2 (épocas V9 e R1) x 5 (doses 0, 3, 6, 9 e 12 kg ha-1 de zinco), com quatro repetições. Para avaliar o potencial fisiológico das sementes foi realizado o teste de germinação, os testes tradicionais de vigor para espécie e o teste de tetrazólio. Os resultados foram...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2191

OCORRÊNCIA DE Glycaspis brimblecombei SOBRE Eucalyptus EM CHAPADÃO DO SUL, MATO GROSSO DO SUL
Provedor de dados: 196
Autores: Vieira, Ricardo de Lima; Pessoa, Luis Gustavo Amorim; Loureiro, Elisângela de Souza; Poersh, Nerison Luís.
Glycaspis brimblecombei (Moore, 1964) (Hemiptera: Psyllidae) é um inseto sugador de origem australiana que ataca várias espécies do gênero Eucalyptus, causando danos significativos na produção florestal. No Brasil, sua presença foi descrita pela primeira vez no estado de São Paulo em 2003 e posteriormente sua ocorrência foi registrada nos estados como Paraná, Goiás, Minas Gerais, Santa Catarina e Rio Grande do Sul. A ocorrência deste inseto na região nordeste de Mato Grosso do Sul foi constatada no Município de Chapadão do Sul em povoamento de Eucalyptus camaldulensis, em setembro de 2014. Causa redução da área fotossintética devido ao elevado número de conchas, seguidas da presença de fumagina em volta destas e o amarelecimento de folhas. A ocorrência...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1543

ATRIBUTOS FÍSICOS DO SOLO CULTIVADO COM CANA-DE-AÇÚCAR EM FUNÇÃO DO PREPARO E ÉPOCA DE AMOSTRAGEM
Provedor de dados: 196
Autores: Arcoverde, Sálvio Napoleão Soares; Souza, Cristiano Márcio Alves de; Suarez, Andres Hideki Tanaka; Colman, Bruno Agostini; Nagahama, Hideo de Jesus.
Objetivou-se avaliar os atributos físicos de um Latossolo Vermelho Distroférrico cultivado com cana-planta em função do preparo e época de amostragem. O trabalho foi conduzido na FAECA-UFGD, em um Latossolo Vermelho Distroférrico, onde a área experimental foi dividida em duas subáreas, compostas pelo sistema plantio direto (SPD) e preparo reduzido (PR). Em cada tipo de preparo foram cultivadas oito cultivares de cana-de-açúcar em delineamento inteiramente casualizado, com quatro repetições. Nas unidades experimentais, amostras com estrutura preservada foram coletadas após o preparo do solo (45 DAP) e após os tratos culturais (180 DAP), para determinação da densidade do solo, porosidade total, macroporosidade, microporosidade e resistência mecânica do solo...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2761

Bradyrhizobium japonicum AND PHOSPHORUS FERTILIZATION ON Vigna Unguilata (L.) WALP
Provedor de dados: 196
Autores: Rocha, Weslany Silva; Barros, Ana Paula Ribeiro; Ribeiro, Marcelo Alves; Martins, Albert Lennon Lima; Chagas Júnior, Aloísio Freitas; Santos, Manoel Mota dos.
This study aimed to estimate the association of P2O5 doses with and without rhizobia inoculation to maximize the agronomic performance and yield of cowpea on an Oxisol in the Cerrado region of Tocantins. The experiments were carried out in two periods during the 2014/2015 growing season at the Experimental Farm of Gurupi belonging to the Federal University of Tocantins, using the variety BRS Novaera. Inoculation was carried out with a standard strain recommended for cowpea. The experimental designs were randomized in blocks in a 2×6 factorial arrangement, with the first factor consisting of the inoculation (presence and absence) and the second factor consisting of six phosphorus doses (0, 30, 60, 90, 120, and 150 kg ha−1 of P2O5), totaling 12 treatments...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5551

ELABORAÇÃO DE BEBIDA COM EXTRATO HIDROSSOLÚVEL DE SOJA SABORIZADA COM FRUTOS DO CERRADO
Provedor de dados: 196
Autores: Perfeito, Danielle Godinho Araújo; Corrêa, Ivna Moreira; Peixoto, Nei.
Os frutos do Cerrado apresentam atrativas características sensoriais, porém seu consumo é restrito à população local. Visando contribuir para expansão do consumo de cagaita e mangaba, o objetivo do estudo foi elaborar e avaliar a aceitação de bebidas com extrato hidrossolúvel de soja saborizada com esses frutos. Para isso elaborou-se três formulações tendo como base fixa 10% de polpa de fruta e 15% de açúcar, sendo Formulação 1: 10% de polpa de mangaba, Formulação 2: 10% de polpa de cagaita e Formulação 3: 5% de cagaita e 5% de mangaba. Realizou-se a caracterização físico-química tanto das polpas como das bebidas. Estas foram submetidas às análises de pH, acidez total titulável, sólidos solúveis (°Brix), ratio (SS/AT), sólidos totais e cinzas. Para a...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1216

EXTRATO AQUOSO E ÓLEO ESSENCIAL DE GENGIBRE INDUZEM MECANISMOS BIOQUÍMICOS DE DEFESA EM FEIJOEIRO
Provedor de dados: 196
Autores: Costa, Ana Paula; Moura, Gabriela Silva; Gebauer, Jéssica Tais; Franzener, Gilmar.
Derivados de algumas plantas medicinais apresentam potencial no controle alternativo de doenças de plantas, mas ainda há necessidade de maior compreensão sobre os mecanismos envolvidos. O objetivo desse trabalho foi avaliar a indução de mecanismos bioquímicos de defesa em feijoeiro (Phaseolus vulgaris) pelo extrato aquoso (EA) e óleo essencial (OE) de gengibre (Zingiber officinale). Foram avaliadas a atividade de peroxidases e polifenoloxidases em folhas de plântulas e plantas de feijoeiro das variedades Preto Tuiuiu e Carioca Pérola. Em plântulas, avaliou-se concentrações de OE (0, 0,1, 0,5 e 1%) e EA (0, 1, 5 e 10%). Em plantas, foram avaliadas concentrações de OE (0,1% e 1%) e EA (1% e 10%) em folhas tratadas e não tratadas. Também foi avaliada a...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2721

CRESCIMENTO INICIAL DE CULTIVARES DE ALGODOEIRO SUBMETIDO AO ESTRESSE SALINO
Provedor de dados: 196
Autores: Pedro, Álvaro Alberto; Steiner, Fábio; Zuffo, Alan Mario; Douradinho, Gabriel Zanuto; Oliveira, Camilla Paulino de.
A seleção de cultivares de algodoeiro com maior tolerância ao estresse salino pode melhorar a emergência das plantas e garantir a adequada uniformidade de estande. Este estudo teve como objetivo comparar a tolerância à salinidade de cultivares de algodoeiro (Gossypium hirsutum L.) durante a fase inicial de crescimento das plântulas. Os tratamentos foram constituídos por seis cultivares de algodão (FM 910, FM 980 GLT, TMG 42 WS, TMG 82 WS, DP 1240 B2RR e DP 1228 B2R) e por cinco níveis de condutividade elétrica da água de irrigação [0,0; 2,5; 5,0, 10,0 e 20,0 dS m–1]. Os cultivares de algodão DP 1228 B2RF e DP 1240 B2RR apresentaram os melhores índices de emergência das plântulas até o nível de salinidade de 10,0 dS m–1, sugerindo que estes cultivares são...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1183

FORRAGEIRAS TROPICAIS EM CONSÓRCIO COM MILHO E ADUBAÇÃO NITROGENADA SOBRE AS PROPRIEDADES FÍSICAS DO SOLO
Provedor de dados: 196
Autores: Mattei, Eloisa; Rabello de Oliveira, Paulo Sérgio; Costa Crusciol, Carlos Alexandre; Rocha de Moraes Rego, Carlos Augusto; Piano, Jeferson Tiago; da Silveira, Lucas.
Os sistemas integrados de produção lavoura-pecuária (SIPAs) em associação ao sistema de semeadura direta, sofrem ação do pisoteio animal ou do tráfego intenso de máquinas agrícolas, podendo resultar em alterações nas propriedades físicas do solo. O objetivo deste trabalho foi avaliar o efeito da adubação nitrogenada e manejos das forrageiras tropicais nas propriedades físicas do solo. O experimento foi realizado entre outubro de 2017 e janeiro de 2020, em Marechal Cândido Rondon – PR, em blocos ao acaso, com parcelas sub-subdivididas com uma testemunha adicional e quatro repetições. As parcelas foram constituídas por duas espécies forrageiras consorciadas com o milho: Urochloa brizantha e Magathyrsus maximum, mais a testemunha adicional (milho solteiro)....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Porosity; Soil physical quality; Resistance to penetration; Integrated systems; Porosidade; Qualidade física do solo; Resistência à penetração; Sistemas integrados.
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6318

CAPACIDADE COMBINATÓRIA DE MILHO PARA PRODUÇÃO DE GRÃOS SOB NÍVEIS DE FÓSFORO
Provedor de dados: 196
Autores: Melo, Aurélio Vaz de; Taubinger, Markus; Santos, Valdere Martins dos; Cardoso, Dione Pereira; DoVale, Júlio César.
Objetivou-se determinar o tipo de ação gênica predominante no controle de algumas características estimando a capacidade geral de combinação (CGC) e a capacidade específica de combinação (CEC) entre híbridos comerciais de milho para produção de grãos sob diferentes níveis de fósforo. O delineamento experimental utilizado foi em látice 8 x 8 com duas repetições, sendo analisadas três características de interesse para a produção de grãos. As combinações híbridas responderam de forma diferenciada às capacidades de combinações quando submetidas às condições de baixa e alta disponibilidade de fósforo indicando que a seleção deverá ser realizada em ambientes onde os mesmos serão utilizados. Conclui-se que o híbrido AG 8060 possui maior concentração de alelos...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1666

RESISTANCE OF SOYBEAN GENOTYPES TO WHITE MOLD IN DISTINCT AGROECOSYSTEMS
Provedor de dados: 196
Autores: Andrade, Gabriela Carolina Guimarães; Carrer Filho, Renato; Cunha, Marcos Gomes da.
White mold (Sclerotinia sclerotiorum) is one of the most important fungal diseases that affect soybean, primarily due to the production of resistant structures called sclerotia. The disease is difficult to control, and sources of genetic resistance are poorly understood. As such, the present study aimed to assess the resistance of soybean genotypes to white mold in two agroecosystems in the Brazil (Barreiras-BA, and Jataí-GO) and analyze the relationship between the disease incidence and the phenotypic characteristics of the genotypes, as well as determine the lodging index, crop cycle and yield. A total of 165 and 33 genotypes were assessed in the regions of Barreiras and Jataí, respectively. To verify the effect of the area, 37 genotypes were planted in...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1759

PHYSIOLOGICAL QUALITY OF MUNG BEAN SEEDS ACCORDING TO THE PLANT DENSITY
Provedor de dados: 196
Autores: Silva, Edvan Costa; Peixoto, Nei; Arruda, Natália; Ferreira, Natália Cássia de Faria; Oliveira, Luís Augusto Batista de.
Mung beans (Vigna radiata L.) are of Asian origin and have gained national importance with the production of moyashi. The study aimed to evaluate the seed physiological quality of mung beans according to the row spacing and number of plants per meter. The experiment was conducted at Goiás State University, Ipameri Campus. Tests were performed to determine the water content, germination, and vigor to evaluate the physiological quality of the seeds. The experimental design was completely randomized, with the treatments arranged in a 2 x 6 factorial scheme, having as factors the row spacing (25 and 50 cm) and the number of plants per meter (4, 8, 12, 16, 20, and 24 plants) with four replications. Based on the results of the analysis of variance, germination,...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3580

GEOESTATÍSTICA APLICADA NA DETERMINAÇÃO DA COMPACTAÇÃO DO SOLO NO CULTIVO DA CANA-DE-AÇÚCAR
Provedor de dados: 196
Autores: Marasca, Indiamara; Gladenucci, Joanina; Spadim, Emanuel Rangel; Barbosa, Rodrigo Domingues; Lanças, Kleber Pereira.
As ferramentas de agricultura de precisão diversificam-se cada vez mais para facilitar a tomada de decisão no campo com o intuito de aumentar a produtividade das culturas para alimentar uma população crescente. A responsabilidade dos profissionais das áreas agronômicas deve ser embasada em estudo e domínio de novas tecnologias. Com esta pesquisa objetivou-se demonstrar a técnica de interpolação de dados para confeccionar mapas de solos utilizando software Gamma Desing e as técnicas da geoestatística.  A resistência à penetração do solo foi obtida até a profundidade de 0,45 m. Para confecção dos mapas dos transeptos para os tratamentos foi utilizado o software Gamma Desing. Os dados para a camada de 0,30 a 0,45 m no preparo convencional foi o único que não...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1462

ANÁLISE FITOSSOCIOLÓGICA E ESTRUTURA FLORÍSTICA DE UMA FLORESTA ESTACIONAL DECIDUAL
Provedor de dados: 196
Autores: Bambolim, Amauri; Donde, Abilene Rodrigues; Wojciechowsk, Júlio César.
A análise fitossociológica bem como a composição florística de florestas naturais é de grande valor para compreensão da dinâmica das comunidades florestais. O presente trabalho teve como objetivo analisar uma área de floresta estacional decidual localizada no município de Santa Tereza no estado do Rio Grande do Sul. Foram instaladas 100 parcelas de 10 x 10 demarcadas em um hectare no interior da floresta, onde foram medidos e identificados todos os indivíduos com circunferência à altura do peito (CAP) ≥ 30 cm. O levantamento foi realizado adotando-se o método de parcelas contíguas, seguindo a metodologia de Muller-Dombois e Ellemberg (1974). A densidade total de 875 indivíduos por hectare, sendo 56 espécies, 46 gêneros e 30 famílias. As famílias Fabaceae e...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1544

CARACTERÍSTICAS TECNOLÓGICAS DE FARINHAS VEGETAIS COMERCIAIS
Provedor de dados: 196
Autores: Santana, Gabriela Silva; Oliveira Filho, Josemar Gonçalves de; Egea, Mariana Buranelo.
As farinhas são muito utilizadas no processamento de diversos produtos de panificação e o seu desempenho tecnológico depende de características funcionais previamente descritas. O objetivo deste trabalho foi avaliar as propriedades funcionais tecnológicas de farinhas comerciais de origem vegetal. Foram realizadas análises de índice de absorção de água, capacidade de absorção de óleo, solubilidade em água, capacidade de formação de espuma, estabilidade da espuma, capacidade emulsificante, estabilidade da emulsão e capacidade de formação de gel. A farinha da casca de maracujá apresentou o maior índice de absorção de água (4,85%). Todas as farinhas apresentaram valores satisfatórios para capacidade de absorção de óleo. Os maiores valores de solubilidade em...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1549

PREJUÍZOS DECORRENTES DE PERDAS NA COLHEITA DO ALGODÃO COM DIFERENTES TIPOS DE COLHEDORAS
Provedor de dados: 196
Autores: Leite, Leonardo Aparecido Inacio; Nuss, Aldo.
Com o aumento da procura de algodão, surgiram novas técnicas de cultivo que reduzem o espaçamento entre linhas (0,76 m e 0,45 m), aumentando a densidade de plantas, diminuindo o ciclo da cultura e conduzindo à um consequente aumento de produção. Com as novas tecnologias associadas à fatores tais como climáticos, de topografia do solo, das variedades utilizadas e das regulagens e modelos de colhedoras, surgiram também os problemas com perda na colheita. O objetivo do trabalho foi mensurar e analisar a viabilidade econômica das perdas na colheita do algodão, com alguns modelos de colhedoras, verificando qual modelo oferece melhor rendimento para o espaçamento de 0,45 m entre linhas. A metodologia utilizada foi de estudo de campo, avaliando áreas colhidas por...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1669

ATRIBUTOS QUÍMICOS DE UM CAMBISSOLO POR MEIO DE ANÁLISE MULTIVARIADA NA CULTURA DA PUPUNHA
Provedor de dados: 196
Autores: Lovera, Lenon Henrique; Lima, Elizeu de Souza; Montanari, Rafael; Tomaz, Pamela Kerlyane; Rosa, Poliana Aparecida Leonel.
Por se tratar de um cultivo perene, a pupunheira se torna bastante exigente quanto às propriedades físicas e químicas do solo, sendo que os atributos químicos do solo refletem de forma mais imediata ao efeito causado pelo manejo que é adotado. O objetivo do presente trabalho foi identificar por meio de análises multivariadas os atributos químicos do solo que melhor explicam a variabilidade da cultura da pupunha em Registro, SP. Em 2014, no município de Registro (SP), foi analisado os componentes produtivos da cultura da pupunha em função de alguns atributos químicos de um Cambissolo eutrófico. Foi demarcada a malha geoestatística, com 54 pontos amostrais, numa área de 1 ha. A classificação em grupos foi feita por três métodos: método de agrupamentos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solos.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/236

YIELD OF IRRIGATED CABBAGE SUBMITTED TO DIFFERENT SOURCES AND DOSES OF BORON
Provedor de dados: 196
Autores: Leão Junior, Laidson Alves; Buso, Wilian Henrique Diniz.
Cabbage is an important vegetable for food. The use of micronutrients, more specifically boron, is important for plant development and head formation. The study aimed to evaluate the agronomic performance and yield of the cabbage crop submitted to the application of different sources and doses of boron. The study was carried out in the Água Verde farm, located in Nova Glória-GO, under irrigation by a center pivot system. The soil tillage consisted of operation with a subsoiler and a disk harrow. The fertilization was carried out by applying 48 kg ha-1 of N, 360 kg ha-1 of P2O5, and 120 kg ha-1 of K2O, in the planting furrow. The seedling transplant took place on 06/22/2019. At 20 days after transplanting, topdressing fertilization was carried out, with 200...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4166

INTERFERÊNCIA DE PLANTAS DANINHAS NO CRESCIMENTO DA CULTURA DO TRIGO
Provedor de dados: 196
Autores: Pereira, Gustavo Antônio Mendes; Maciel, Josiane Costa; Santos, José Barbosa dos; Reis, Ricardo Felix dos; Ferreira, Evander Alves.
Dentre os fatores que limitam a expressão do potencial produtivo da cultura do trigo a competição com as plantas daninhas é um dos mais severos causando grandes prejuízos à produtividade e qualidade da produção. Dessa forma, o estudo teve como objetivo avaliar o efeito da competição das espécies E. fosbergii, B. pilosa e G. parviflora, isoladas e em associação no crescimento das plantas de trigo em condição de campo. Para isso, as plantas foram semeadas em diferentes densidades: 0; 23; 46 e 66 plantas daninhas m-2, convivendo com a cultura por 85 dias após a semeadura. As plantas daninhas apresentaram diferentes interferências sobre as variáveis agronômicas e cada espécie competiu com a cultura por diferentes nutrientes. A cultura do trigo é afetada...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1559

WEED CONTROL BY SOLARIZATION AND MULCHING IN COWPEA DEVELOPMENT
Provedor de dados: 196
Autores: Maia Júnior, Sebastião de Oliveira; Andrade, Jailma Ribeiro de; Reis, Lígia Sampaio; Santos, Claudiana Moura dos; Silva, Lennon Kledson dos Santos; Martins, Gleica Maria Correia.
Weeds are a serious threat to agriculture because they compete with crops, thereby interfering in production. As such, this study aimed to assess weed control using soil solarization and mulching on the growth and yield of cowpea. A completely randomized design was used, with eight treatments and four repetitions. The treatments consisted of a combination of two management practices, namely soil solarization (with and without) and three mulches (castor bean, rattlepod and spontaneous vegetation), as well as no mulching. Non-solarized soil and without mulch increased the number and dry weight of weeds, while the main stem length of the cowpea plants decreased. Mulching increased the pod length and number of seeds per pod regardless of solarization, as well...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3938

SINGLE-HEAD BROCCOLI PRODUCTION UNDER DIFFERENT SPACING AND CONDITIONS OF BAIXADA FLUMINENSE
Provedor de dados: 196
Autores: Macedo, Taísa Gonçalves; dos Santos, Carlos Antônio; Brandão, Antônio de Amorim; Silva Pereira Costa, Evandro; Goréte Ferreira do Carmo, Margarida.
This study aimed to evaluate different spacings between rows on the development and yield of single-head broccoli under the soil and climate conditions of Seropédica, in the Baixada Fluminense region, the State of Rio de Janeiro (Brazil). Tests were carried out under field conditions using the Avenger hybrid. The experimental design adopted was randomized blocks with four treatments and four replications per treatment. Four spacings between rows were tested: 0.6 m, 0.7 m, 0.8 m, and 1.0 m. The spacing between plants in the rows was 0.6 m in all treatments. The number of leaves (NL), plant height (PHT), fresh leaf mass (FLM), stem fresh mass (SFM), inflorescence fresh mass (IFM), inflorescence longitudinal diameter (ILD), and estimated yield (YLD) were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brassica oleracea var. italica; Brassicaceae; Population density; Brassica oleracea var. italica; Brassicaceae; Densidade populacional.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6908

COMPARAÇÃO DAS PROPRIEDADES QUÍMICAS E DO PERFIL LIPÍDICO DAS FARINHAS DE BOCAIUVA (Acrocomia spp.) DESPOLPADA DE FORMA MANUAL E MECÂNICA
Provedor de dados: 196
Autores: do Amaral, Luane Aparecida; Loubet Filho, Paulo Sérgio; Cavalheiro, Leandro Fontoura; Galvani, Fábio; dos Santos, Elisvânia Freitas.
A palmeira Acrocomia spp, também conhecida como bocaiuva, tem sido explorada de forma extrativista por agricultores de subsistência que vivem na área de ocorrência, gerando fonte de renda e a valorização dos frutos nativos. A bocaiuva é de difícil despolpa, então este estudo tem como objetivo comparar as propriedades químicas e o perfil lipídico das farinhas de bocaiuva despolpadas de forma manual e mecânica. Foram realizadas as análises químicas: umidade, cinzas, lipídios, proteínas, carboidratos e fibras. Os ácidos graxos foram determinados por cromatografia gasosa. Todos os parâmetros químicos diferiram estatisticamente entre as duas farinhas, exceto os valores de proteínas. Os valores de umidade, cinzas e carboidratos foram superiores na farinha da...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2737

MANEJO DA ADUBAÇÃO NITROGENADA NAS CULTURAS DE ALFACE, REPOLHO E SALSA
Provedor de dados: 196
Autores: Nascimento, Mariana Vieira; Silva Junior, Rogério Lamim; Fernandes, Luiz Roberto; Xavier, Ricardo Caldas; Benett, Katiane Santiago Silva; Seleguini, Alexsander; Benett, Cleiton Gredson Sabin.
O adequado fornecimento de nitrogênio é um dos principais fatores de manejo que afetam o rendimento e a qualidade da produção de hortaliças. Este trabalho teve como objetivo avaliar os efeitos da aplicação de doses e fontes de nitrogênio no desenvolvimento e produtividade de alface, repolho e salsa. Os experimentos foram desenvolvidos na Universidade Estadual de Goiás, Campus Ipameri no período de agosto a novembro de 2014. O delineamento experimental utilizado para cada espécie, foi o de blocos ao acaso, em esquema fatorial 2 x 5, sendo duas fontes de N (ureia convencional e ureia revestida com polímero) e cinco doses de nitrogênio (de acordo exigência de cada espécie), com quatro repetições. As espécies utilizadas foram alface crespa Itapuã Super,...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1099

HYGROSCOPIC BALANCE IN PUMPKIN SEEDS
Provedor de dados: 196
Autores: Wenneck, Gustavo Soares; Saath, Reni; Santi, Danilo Cesar; Araújo, Larissa Leite de; Santos, Josélia Portilho dos; Oliveira, Giovanna Gabriela Ferreira de.
The commercial exploitation of pumpkin seeds, at the flour form toasted or to the production of oil, requires knowledge about the activity of water and equilibrium moistures. This study aimed to determine the equilibrium isotherms to the pumpkin seeds and describe the dynamics of the process upon its physicochemical quality. With the static method, the equilibrium isotherms were determined for different temperatures and activities of water (0.110 to 0.885 dry basis), provided conditions by the conditioner chamber of atmosphere, with the weighing of the samples until the constant mass. The hygroscopic balance of the seeds was directly proportional to the activity of water and decreased with increasing temperature, for the same value of water activity. The...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4090

ADUBAÇÃO POTÁSSICA NA PRODUÇÃO DE DUAS CULTIVARES DE MELOEIRO
Provedor de dados: 196
Autores: Bardiviesso, Diógenes Martins; Maruyama, Wilson Itamar; Pessato, Luis Eduardo; Pereira, Ana Carolina Bueno; Modesto, Joyce Helena.
As recomendações de adubação potássica para a cultura do meloeiro variam de região para região, sendo essas recomendações influenciadas principalmente pelas condições de clima, solo, e condições de cultivo. Portanto, o objetivo foi avaliar doses de potássio sobre a produtividade e a qualidade dos frutos de duas cultivares de meloeiro produzidas em céu aberto no município de Cassilândia-MS. O delineamento experimental foi de blocos casualizados com quatro repetições, em esquema fatorial 2x5 (cultivares x doses de potássio), utilizando-se duas cultivares, o híbrido Amarelo Giorgio (Cucumis melo var. inodorus), e o híbrido Cantaloupe Rafael (Cucumis melo var. cantalupensis) e cinco doses de potássio (0, 60, 120, 180 e 240 kg ha-1 de K2O) aplicadas no plantio...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agronomia.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/244

IRRIGATION WITH WATER DEFICIT APPLYING MAGNETIC WATER ON SCARLET EGGPLANT
Provedor de dados: 196
Autores: Seron, Cássio de Castro; Rezende, Roberto; Lorenzoni, Marcelo Zolin; Souza, Álvaro Henrique Candido de; Gonçalves, Antonio Carlos Andrade; Saath, Reni.
The work aimed to evaluate the effect of irrigation with magnetically treated water on development, growth, and yield of the scarlet eggplant (Solanum gilo Raddi) cv. Morro Grande, in two growing seasons (autumn and spring). A completely randomized design in a 3x2 factorial scheme with three replications for the first growing season and 2x2 with five replications for the second growing season was used. Each experimental unit consisted of four plants spaced 0.75 m between plants and 1.00 m between rows. Factors consisted of irrigation using magnetically treated water, untreated water, three replacement of the crop evapotranspiration (50%, 75%, and 100% ETc) for the first growing season and two replacement of the crop evapotranspiration (75% and 100% ETc)...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3809

DIVERSIDADE DE MACROFAUNA EDÁFICA EM DIFERENTES AMBIENTES DE CULTIVO NO AGRESTE DA PARAÍBA, BRASIL
Provedor de dados: 196
Autores: Aires Souza, José Thyago; Costa Oliveira, Suenildo Josemo; Medeiros Nápoles, Fábio Agra de; de Souza, Mileny dos Santos; Medeiros, Marcio Raimundo de.
A diversidade da fauna edáfica tem sido indicadora da qualidade do solo em ambientes explorados para atividades agrícolas com constante interferência antrópica; tem se tornado um fator essencial para a manutenção da estrutura e fertilidade edáfica. Objetivou-se identificar a população de macrofauna presente em solo cultivado com as culturas do pinhão manso (Jatropha curcas L.) e laranjeira (Citrus sinensis L.). Foram selecionados sete pontos de coletas fixos onde utilizou-se armadilhas do tipo Provid, enterradas com os bordos das quatro aberturas ao nível da superfície do solo. Após a quantificação dos indivíduos, calculou-se a riqueza (nº de grupos identificados), os índices de frequência, abundância, dominância e constância, obtidos através programa...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1681

EFFICIENCY LOSS OF RECORDED FUNGICIDES FOR THE CONTROL OF ASIAN SOYBEAN RUST IN CENTRAL REGION OF BRAZIL
Provedor de dados: 196
Autores: Aguiar, Renata Alves; Cunha, Marcos Gomes; Araújo, Fernando Godinho; Carneiro, Luciana Celeste; Borges, Edson Pereira; Carlin, Valtemir José.
Due to grower allege of low efficiency of triazole fungicides in recent years in Central Brazil on the control of Asian soybean rust (Phakopsora pachyrhizi), this study was undertaken to demonstrate the efficiency loss of products registered for rust and applied alone and to evaluate the efficiency of fungicides mixtures. The trials were carried out in five locations in Brazil, in the 2009/10 growing season. The experimental design was completely randomized blocks with four replications. Ten mixtures of triazole + strobilurin and two applications of pure triazoles were evaluated and the control without application. The application of fungicides started in the R1/R2 stage or in any vegetative stage if infections occurred early. The mixtures of fungicides...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1066

VARIABILIDADE ESPACIAL DAS PROPRIEDADES DENDROMÉTRICAS DO EUCALIPTO E ATRIBUTOS QUÍMICOS DE UM NEOSSOLO QUARTZARÊNICO
Provedor de dados: 196
Autores: Lima, Elizeu de Souza; Montanari, Rafael; Lovera, Lenon Henrique; Teixeira Filho, Marcelo Carvalho Minhoto; González, Antonio Paz.
A geração de grandes quantidades de resíduos sólidos e efluentes pelas indústrias de celulose e papel tem se constituído em preocupação ambiental. Este trabalho objetivou analisar as correlações lineares do desenvolvimento individual das árvores de Eucalyptus urograndis, em função dos atributos químicos de um Neossolo Quartzarênico, com vistas a evidenciar zonas específicas de manejo intimamente associadas ao desenvolvimento do eucalipto no intuito de utilizar a lama de cal da extração da celulose na forma de fertilizantes de maneira sustentável ao ambiente. Foi instalada uma malha experimental de aproximadamente 2 ha, contendo 50 pontos amostrais em um Neossolo Quartzarênico e posteriormente coletados atributos de planta e solos para a determinação dos...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1194

DETERMINAÇÃO DA CINÉTICA DE SECAGEM DE PRODUTOS ALIMENTÍCIOS USANDO ALGORITMOS GENÉTICOS
Provedor de dados: 196
Autores: Barbosa, Thaís Alves; Lobato, Fran Sérgio.
A secagem de produtos alimentícios consiste na redução do seu volume e de sua massa durante o processo de desidratação que ocorre através da remoção de água. Esta operação unitária é amplamente utilizada na indústria com o objetivo de obter um produto com determinadas especificações de mercado. Entre as variáveis que mais influenciam este fenômeno, pode-se citar o tempo e a temperatura. Matematicamente, o estudo da cinética de secagem de produtos alimentícios é realizado considerando a determinação de parâmetros que caracterizam a cinética de secagem. Neste trabalho é formulado e resolvido um problema de otimização que consiste da minimização da diferença entre os dados experimentais e o calculado usando diferentes modelos matemáticos, empregados para...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1205

DESENVOLVIMENTO E CARACTERIZAÇÃO DE GELEIA DE LARANJA ENRIQUECIDA COM AVEIA
Provedor de dados: 196
Autores: Oliveira, Camila Fernanda Dias de; Pinto, Ellen Godinho; Tomé, Alessandra Cristina; Quintana, Rosangela Coelho; Dias, Bruna Ferreira.
Este trabalho objetivou a caracterização físico-química e microbiológica da geleia de laranja enriquecida com aveia. As laranjas foram selecionadas manualmente, considerando-se ausência de manchas ou defeitos. As geleias foram elaboradas com a proporção de 50%/50%, (polpa/sacarose) enriquecida com teor de aveia em três concentrações, sendo 1,5%, 3% e 4,5%. Após o processamento das geleias foram avaliadas quanto ao teor de umidade, pH, vitamina C, sólidos solúveis totais e análise microbiológica. Diante dos resultados obtidos das análises físico-química, verificou-se que enriquecimento da geleia de laranja com aveia influenciou significativamente nos resultados de pH e sólidos solúveis totais °Brix. Os resultados da análise microbiológica mostraram-se todas...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1203

PRODUÇÃO E COMPOSIÇÃO BROMATOLÓGICA DA SILAGEM DE HÍBRIDOS DE MILHO SOB DUAS ALTURAS DE CORTE
Provedor de dados: 196
Autores: Buso, Wilian Henrique Diniz; Machado, Alan Soares; Ribeiro, Taiz Borges; Silva, Lidiane Oliveira.
Objetivou-se avaliar a produção e composição químico-bromatológica da matéria original e da silagem de cinco híbridos de milho em duas alturas de corte. Utilizou-se o delineamento de blocos completos casualisados em esquema fatorial 5x2, cinco híbridos de milho (AGN30A95H, DKB399Y, DKB390Y, P3862H e TRUCK) e duas alturas de corte (0,25 e 0,50 m) com três repetições. As plantas foram cortadas, picadas na ensiladeira e ensiladas em tubos de PVC. Para altura das plantas, os híbridos DKB399Y e P3862H diferiram (P&amp;lt;0,05) dos demais, apresentando maior altura (2,35 m). De forma geral, a composição bromatológica do material original e da silagem dos híbridos estudados esteve dentro dos parâmetros recomendados de silagem de qualidade. Todos os híbridos de...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2682

DESPERDÍCIO DE IOGURTE POR EMBALAGENS
Provedor de dados: 196
Autores: Ferreira, Monica Aparecida Campos; Freire, Lucas de Alvarenga Santos; Barbosa, Thaís Alves; Siqueira, Ana Paula Silva.
O desperdício de alimentos é inaceitável diante da quantidade de pessoas que passam fome no mundo. Novas tendências tecnológicas visando estética e praticidade tem transformado as embalagens em novas fontes de desperdício. Diante do exposto objetivou-se com o presente trabalho contabilizar o desperdício de iogurte causado por diferentes tipos de embalagens comerciais e verificar a opinião de consumidores a respeito da importância da embalagem e do desperdício que algumas podem causar. Observou-se que o desperdício causado por essas embalagens pode chegar a ordem de 12% de produto, variando entre tampa e corpo e que a impressão das pessoas sobre as embalagens realmente está relacionada à praticidade e estética e até mesmo a marca, além do que, não se dá...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1204

Desempenho agronômico da chia sob diferentes arranjos espaciais
Provedor de dados: 196
Autores: Teodoro Maia, João Paulo; Garcia da Silva, Wellington; Vieira Silva, Ariana; Duarte Giunti, Otavio; Henrique Sartori, Raul Henrique.
The nutritional benefits and functional potential of chia seeds have been highlighted in the literature. However, few studies address the planting system of the species, especially its spatial arrangement. Thus, this study proposes to evaluate chia cultivation under different spatial arrangements, aiming at its agronomic performance. The experimental design was randomized in blocks in a 3×2 factorial scheme, with three inter-row spacings (0.30, 0.45, and 0.60 m), two plant densities per linear meter (7.5 and 15 plants m−1), and four replications. Plant height, stem diameter, leaf area index, dry matter, chlorophyll index, leaf nitrogen content, panicle size, harvest index, and yield were evaluated. The evaluated spatial arrangements did not influence plant...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Harvest index; Lamiaceae; Agronomic management; Salvia hispanica L.; Índice de colheita; Lamiaceae; Manejo agronômico; Salvia hispanica L.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/7015

In vitro CONFRONTATION OF Trichoderma spp. ISOLATES WITH PHYTOPATHOGENIC AND NON-PHYTOPATHOGENIC FUNGI
Provedor de dados: 196
Autores: Lima, Milton Luiz da Paz; Vaz, Maria Cristina Araújo; Silva, Aline Suelen da; Souza, Karoliny de Almeida; Tuñon, Gabriel Isaias Lee.
The aim of this study was the confrontation of Trichoderma spp. with pathogenic and non-pathogenic fungi. The Trichoderma spp. and filamentous fungi (Fusarium solani, Alternaria sp., Colletotrichum gloeosporioides, and Aspergillus niger) were transferred to potato-dextrose-agar (PDA). The confrontation was performed using Petri dishes inoculated with mycelial disks in opposite position (9 mm) of Trichoderma spp. and filamentous fungi. After inoculation the plates remained under 25 ° C regime to 12 hours light for a period of seven days. After this period was evaluated qualitatively according to the scale of Bell et al. (1982), which consists of the suitability scores for the area percentage of the culture medium under expression of antagonism. The isolate...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/810

INFLUÊNCIA DE FATORES AMBIENTAIS, COR E ALTURA DE ARMADILHAS NA CAPTURA DO CARUNCHO DO BAMBU
Provedor de dados: 196
Autores: Silveira, Edilson Soares; Silva, Rudieli Machado; Roel, Antonia Railda; Cereda, Marney Pascoli.
O objetivo deste trabalho foi avaliar o efeito da influência dos fatores ambientais, cor e altura de instalação de armadilhas com toletes de bambu na captura do Dinoderus minutus, considerado a principal praga pós-colheita do bambu. A literatura aponta a cor e altura das armadilhas como elementos capazes de influenciar na captura deste inseto. Para avaliar essas hipóteses, foram fabricadas 30 armadilhas de garrafas PET nas cores amarela, preta, branca, azul e transparente. Toletes de bambu Bambusa vulgaris foram cortados e secos em uma estufa a 50±3°C durante 48 h. Em cada armadilha foi inserido um tolete de bambu na posição vertical. As armadilhas foram instaladas a 1,5 m e 2,5 m de altura em relação ao solo, em uma touceira de B. vulgaris. No período do...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1672

CUSTO DE PRODUÇÃO DE SOJA TRANSGÊNICA EM SISTEMA DE SEMEADURA DIRETA EM SÃO DESIDÉRIO-BA
Provedor de dados: 196
Autores: Santos, Conrado Garcia; Martins, Gustavo Luís Mamoré; Silva, Pedro Augusto; Zoz, Tiago.
O objetivo do trabalho foi estimar o custo de produção da soja transgênica, em sistema de semeadura direta na região oeste do estado da Bahia. A pesquisa foi conduzida, na forma de estudo de caso, em uma propriedade rural localizada no município São Desidério (BA). Para levantamento do custo de produção utilizou-se a metodologia do sistema de Custo Operacional Total (COT). Os dados relativos aos coeficientes técnicos da cultura, utilizados no cálculo do custo de produção, foram levantados de uma planilha de controle administrativo, na safra 2015/2016. Foram calculadas médias e porcentagens de cada item do custo de produção de soja em um hectare. O Custo Operacional Total foi de R$ 2001,37 ha-1, contribuindo com maior impacto os herbicidas (33,82%) e adubos...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1430

BIOESTIMULANTE, BIOFERTILIZANTE E INOCULAÇÃO DE SEMENTES NO CRESCIMENTO E PRODUTIVIDADE DA SOJA
Provedor de dados: 196
Autores: Alderete Prieto, Carlos; Rasche Alvarez, Jimmy Walter; Karajallo Figueredo, Julio César; Aguayo Trinidad, Simeón.
Com o objetivo de avaliar o efeito da aplicação de biostimulante (BES), de biofertilizante (BIO) e da inoculação (INO) de sementes de soja com Bradyrhizobium sobre o crescimento e a produtividade da soja foi realizada a pesquisa em Minga Porã, Paraguai, em um Rhodic Paleudult (Latossolo Vermelho). O delineamento experimental foi de blocos ao acaso num arranjo fatorial 3x3x3, com 5 repetições. O fator um foi a aplicação de bioestimulante – controle, 500 mL em 100 kg de semente e 500 mL no estágio R2 da soja. O fator dois foi a aplicação de biofertilizante - controle, 160 e 320 L ha-1 no estágio V1 da soja, e o fator três foi a inoculação com Bradyrhizobium - controle, 200 mL e 400 mL em 100 kg de semente. Foi determinada a altura final de planta, massa de...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1167

INTERFERÊNCIA DO ARRANJO DE PLANTAS DANINHAS NO CRESCIMENTO DO FEIJOEIRO
Provedor de dados: 196
Autores: Lage, Patrícia; da Silveira Júnior, Marcos Antônio; Ferreira, Evander Alves; Pereira, Gustavo Antônio Mendes; Silva, Enilson de Barros.
A produtividade média da cultura do feijoeiro pode ser considerada baixa e entre os fatores que mais impactam nessa perda está a competição com plantas daninhas. Com isso, objetivou-se com esse trabalho quantificar a interferência de duas das principais plantas daninhas que ocorrem na cultura do feijoeiro e o efeito da associação (comunidades) dessas plantas no crescimento da cultura. Foram estudados dois fatores constituído pela combinação de 5 densidades de infestação de plantas daninhas (fator A) e duas espécies de plantas daninhas, Urochloa plantaginea (capim-marmelada) e Bidens pilosa (picão-preto) e a associação das duas (Capim-marmelada + Picão-preto) (fator B). Nas condições em que o experimento foi conduzido, é possível afirmar que o picão-preto...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1568

MUDAS DE Tectona grandis PRODUZIDAS EM DIFERENTES NÍVEIS DE SATURAÇÃO POR BASES DO SOLO
Provedor de dados: 196
Autores: Oliveira, Reginaldo de; de Souza, Naiara Fernanda; Pietroski, Marizane; Ferbonink, Guilherme Ferreira; Caione, Gustavo.
A teca (Tectona grandis L. F) é uma espécie florestal que é favorecida pela elevação da saturação por bases do solo (V%) devido, principalmente, à sua alta exigência em cálcio (Ca). Objetivou-se com este trabalho avaliar o efeito de doses de calcário e saturação de base alcançadas, sobre os atributos químicos de fertilidade do solo e no desenvolvimento vegetativo, acúmulo de matéria seca e qualidade de mudas de teca. O experimento foi conduzido em delineamento inteiramente casualizado. Os tratamentos foram quatro doses de calcário equivalentes a 0 (tratamento controle); 1,4; 3,7 e 5,2 Mg ha-1, com oito repetições. Por ser um atributo que melhor representa o solo e diretamente relacionado às doses de calcário aplicadas, utilizou-se os valores de saturação...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2234

GROWTH AND VOLUMETRIC PRODUCTION OF EUCALYPTUS CLONES IN DIFFERENT PLANTING SPACES
Provedor de dados: 196
Autores: Silva, Wesley Gomes; Santos, Darcy Maria da Conceição Laura dos; Lima, Ana Paula Leite; Mattos, Filipi Duran; Lima, Sebastião Ferreira; Paula, Rita de Cássia Mariano de.
In forest stands, the ideal planting spacing can provide each tree with enough space for its establishment, aiming at greater growth and wood quality, according to the objective of planting. The objective of this study was to evaluate the growth in height, diameter, and volumetric production of three eucalyptus clones planted in different spacings. The experiment was carried out in an area belonging to Campo Bom Farm, in Chapadão do Sul, MS. A randomized block design was used in a factorial scheme, combining six spacings (2.5 x 0.5 m; 2.5 x 1.0 m; 2.5 x 2.0 m; 3.0 x 0.5 m; 3.0 x 1.0 m and 3.0 x 2.0 m) and three clone of Eucalyptus grandis x Eucalyptus urophylla (GG 680, GG 157 and GG 100) with three replications. The diameter at breast height (DBH) and...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3386

Previsão da produtividade de grãos de milho em função da altitude e da população de plantas
Provedor de dados: 196
Autores: da Rosa Sarturi, Marlon Vinicius; Menegassi Bianchi Teixeira, Cleusa Adriane; Carvalho, Ivan Ricardo; Demari, Gustavo Henrique; Vieira Loro, Murilo; Pradebon, Leonardo Cesar; Donadel Port, Eduarda.
This study aimed to evidence the best arrangement of plants according to altitudes to potentialize corn grain yield. An information survey was performed in the 2019/20 harvest, using 144 producers responsible for corn grain production fields totaling 2,301.3 hectares in 144 environments of Rio Grande do Sul. Within 144 environments, 14 corn hybrids were arranged: DKB 240 PRO, DOW 2A620, AG 9045 PRO3, AS1555 PRO3, AS1572 PRO2, AS1656, BIOGENE 7046, DKB 250 PRO2, DKB 290 PRO3, DKB 330RR, NS56, P1630HX, P30F53HX, and SH7910. Yield, morphological, and phenological variables were measured, and geographic and meteorological information was collected. There is a positive influence on grain yield according to altitude and plant population characteristics. At lower...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays; Geographic variables; Principal components; Linear association; Zea mays; Variáveis geográficas; Componentes principais; Associação linear.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/7070

INDUSTRIAL TOMATO FOR FRESH CONSUMPTION: A TECHNICAL AND ECONOMICALLY VIABLE ALTERNATIVE
Provedor de dados: 196
Autores: Costa, Daianna Pereira; da Silva, Juliana Nascimento; Assunção, Donielsin da Silva; Penteado, Fritz Mohn; Nascimento, Abadia dos Reis.
The cultivation of hybrid tomatoes, intended for fresh consumption, with a determined growth habit, and without support, is an alternative that has a lower production cost. The research aimed to evaluate the productivity and economic viability of different tomato genotypes, with a determinate and indeterminate growth habit. The experimental design was in completely randomized blocks. Ten hybrids and a variety were grown in 2016, and nine hybrids, and a variety in 2018, with a spacing of 0.5 meters between plants. Harvests were carried out in four periods in 2016, at 72, 82, 97, and 105 days after transplanting (DAT); and in 2018 at 81, 87, 97, and 111 DAT. After harvesting, the gross value of production and profit were quantified. The hybrids that obtained...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3823

TESTE DE LIXIVIAÇÃO DE POTÁSSIO PARA AVALIAÇÃO RÁPIDA DO VIGOR DE SEMENTES DE TRIGO
Provedor de dados: 196
Autores: Douradinho, Gabriel Zanuto; Souza, Gabriel Elias de; de Oliveira, Camilla Paulino; Bortolazzo, Guilherme; Zoz, Tiago; Steiner, Fábio.
A avaliação do vigor das sementes é de fundamental importância para o sucesso dos sistemas de produção agrícola. Métodos que possibilitam a rápida avaliação do vigor das sementes são de grande interesse no controle de qualidade das empresas produtoras. Este estudo teve como objetivo avaliar a eficiência do teste de lixiviação de potássio na avaliação da qualidade fisiológica de sementes de trigo (Triticum aestivum L., cv. BRS 331), buscando a comparação com outros métodos na diferenciação do vigor dos lotes de sementes. O delineamento experimental utilizado foi o inteiramente casualizado com quatro repetições de 50 sementes. Cinco lotes de sementes do cultivar BRS 331 foram submetidos ao teste de germinação (8 dias), primeira contagem da germinação (4...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/266

ASSOCIATION MAPPING OF MORPHOLOGICAL AND PHYSIOLOGICAL TRAITS OF FLAG LEAF RELATED TO DROUGHT TOLERANCE IN BARLEY
Provedor de dados: 196
Autores: Jabbari, Mitra; Ali Fakheri, Barat; Aghnoum, Reza; Mahdi Nezhad, Nafiseh; Ataei, Reza; Koochakpour, Zahra.
Association mapping has proven to be a powerful approach for dissecting the genetic basis of complex traits. In this study, QTLs controlling flag leaf characteristics under drought stress were detected in a set of 148 modern spring barley cultivars using AM analysis. Flag leaf length (FLL), flag leaf width (FLW), relative water content (RWC), chlorophyll content, and maximum quantum efficiency of PSII (Fv/Fm) which are important in photosynthetic rate, were evaluated under normal irrigation and drought stress conditions at grain filling stage. Population structure was estimated using Structure2.3 and linkage disequilibrium (LD) was estimated by the ‘Full Matrix LD’ using Tassel5.0. Significant marker/trait associations were investigated based on K-Q matrix...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3323

BIOLOGIA DE Bemisia tabaci (GENN.) BIÓTIPO B (HEMIPTERA: ALEYRODIDAE) EM GENÓTIPOS DE TOMATEIRO EM DUAS ÉPOCAS
Provedor de dados: 196
Autores: Toscano, Luciana Claudia; Boiça Junior, Arlindo Leal; Martins, Gustavo Luís Mamoré; Maruyama, Wilson Itamar.
Bemisia tabaci biótipo B é, atualmente, uma das mais importantes pragas da cultura do tomate. Este trabalho teve o objetivo de estudar a biologia da praga em genótipos de tomateiro em duas épocas. O ensaio foi conduzido em casa-de-vegetação instalada na área experimental do Departamento de Fitossanidade, da FCAV/Unesp, Jaboticabal. Foram utilizados os genótipos comerciais, híbrido Bruna VFN e Santa Clara e exóticos, LA 716, PI 134417, PI 127826 e PI 127827 em duas épocas diferentes, “inverno” e “primavera”. O período de incubação variou de 12,11 dias (PI 134417) a 13,85 dias (LA 716). O período ninfal variou de 21,12 dias (PI 127827) a 22,56 dias (híbrido Bruna VFN). O período total de desenvolvimento variou de 37,31 dias (híbrido Bruna VFN) a 34,48 dias...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1124

QUALIDADE DOS SOLOS DE UMA MICROBACIA NA REGIÃO DE ILHA SOLTEIRA – SP
Provedor de dados: 196
Autores: Queiroz, Hernandes Andrade; Alves, Marlene Cristina; Silva, Hélio Ricardo.
&amp;Eacute; inquestion&amp;aacute;vel a degrada&amp;ccedil;&amp;atilde;o de mananciais devido &amp;agrave; eros&amp;atilde;o e a polui&amp;ccedil;&amp;atilde;o, decorrentes do desenvolvimento econ&amp;ocirc;mico. Neste sentido este trabalho teve como objetivos caracterizar a fisiografia e alguns atributos f&amp;iacute;sicos dos principais solos de uma microbacia na cidade de Ilha Solteira, S&amp;atilde;o Paulo. Foram utilizadas imagens de sat&amp;eacute;lite de alta resolu&amp;ccedil;&amp;atilde;o 0,6 m Quickbird e o programa SPRING vers&amp;atilde;o 4.3. Utilizando a metodologia de topossequ&amp;ecirc;ncia em rela&amp;ccedil;&amp;atilde;o &amp;agrave; vertente, em cinco transectos com pontos locados no sentido do espig&amp;atilde;o at&amp;eacute; a foz,...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/222

PRODUÇÃO DE CANA-DE-AÇÚCAR CORRELACIONADA COM O TEOR DE FÓSFORO EM MATO GROSSO DO SUL
Provedor de dados: 196
Autores: Montanari, Rafael; Tomaz, Pamela Kerlyane; Pellin, Douglas Martins Pereira.
A caracteriza&amp;ccedil;&amp;atilde;o da variabilidade espacial de atributos envolvidos nos sistemas de produ&amp;ccedil;&amp;atilde;o &amp;eacute; fundamental para o planejamento estrat&amp;eacute;gico do setor sucroenerg&amp;eacute;tico brasileiro. Assim, o objetivo foi avaliar a correla&amp;ccedil;&amp;atilde;o espacial e linear entre os atributos da composi&amp;ccedil;&amp;atilde;o tecnol&amp;oacute;gica da cana-de-a&amp;ccedil;&amp;uacute;car correlacionados com o teor de fosf&amp;oacute;ro de um Latossolo Vermelho distrof&amp;eacute;rrico, no munic&amp;iacute;pio de Rio Brilhante, MS. Foi instalada uma malha geoestat&amp;iacute;stica, para a coleta de dados do solo e planta, com 80 pontos amostrais, numa &amp;aacute;rea de 80 ha. A...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/224

DANOS E POTENCIAL REPRODUTIVO DE Pratylenchus brachyurus EM CINCO ESPÉCIES VEGETAIS
Provedor de dados: 196
Autores: Mainardi, Janile Tamiozzo; Asmus, Guilherme Lafourcade.
O nematoide Pratylenchus brachyurus tem se destacado como a espécie de nematoide fitoparasita mais frequente em áreas de produção agrícola do Brasil-Central. A reação de espécies vegetais ao nematoide tem sido pouco estudada. Por essa razão, foram realizados dois experimentos em casa de vegetação, com o objetivo de caracterizar a reação de cinco espécies vegetais de interesse econômico (soja, algodoeiro, milho, capim-marandú e capim-mombaça) à presença de P. brachyurus. Cada espécie foi inoculada com zero, 333, 1.000, 3.000 e 9.000 nematoides/planta no primeiro experimento e zero, 1.500, 4.500, 13.500 e 40.500 nematoides/planta no segundo experimento. Sessenta dias após a inoculação, foram realizadas avaliações morfo-fisiológicas das espécies vegetais...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/683

PERDAS DE AMÔNIA POR VOLATILIZAÇÃO EM RESPOSTA A ADUBAÇÃO NITROGENADA DO FEIJOEIRO.
Provedor de dados: 196
Autores: Cardoso dos Santos, Susiane Moura; Antonangelo, João Arthur; Deus, Angélica Cristina Fernandes; Fernandes, Dirceu Maximino.
O nitrogênio (N) é um dos nutrientes que mais limita o crescimento e o desenvolvimento das plantas, principalmente, devido a sua grande dinâmica no sistema solo-planta-atmosfera. Dentre os vários processos que este elemento está sujeito, pode-se destacar a volatilização. As perdas de amônia (N–NH3) por volatilização podem atingir 78% do N aplicado na forma de ureia, e variam de acordo com a fonte utilizada. Esse trabalho teve como objetivo quantificar as perdas de amônia (N–NH3) por volatilização, decorrentes da aplicação de diferentes doses e fontes de N na cultura do feijão (Phaseolus vulgaris L.). O delineamento experimental utilizado foi o de blocos ao acaso, com dezesseis tratamentos e cinco repetições. Os tratamentos foram constituídos de três doses...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/545

DOSES DE NITROGÊNIO NO DESENVOLVIMENTO DE MUDAS ALTAS DE MARACUJÁ-AMARELO
Provedor de dados: 196
Autores: Bertani, Rosemary Marques de Almeida; Silva, Sueellen Pereira da; Deus, Angélica Cristina Fernandes; Antunes, Andrea Maria; Fischer, Ivan Herman.
Com a disseminação do vírus do endurecimento dos frutos do maracujazeiro amarelo, surge a necessidade de produção de mudas maiores e mais vigorosas. Atualmente, há carência de informações sobre os aspectos nutricionais na formação de mudas com qualidade; desta forma, objetivou-se avaliar doses de nitrogênio (N) no desenvolvimento de mudas altas de maracujá amarelo. O delineamento experimental foi em blocos casualizados, com cinco tratamentos e cinco repetições. Os tratamentos foram compostos por doses de nitrogênio (0, 0,17, 0,34, 0,51 e 0,68 g L-1) na forma de nitrato de cálcio, aplicadas em forma de solução nutritiva. As doses 0,34, 0,51 e   0,68 g L-1N aumentaram o teor de N nas folhas, proporcionando maior desenvolvimento em altura, diâmetro do caule e...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2403

CONTROLE BIOLÓGICO DE FORMIGAS-CORTADEIRAS: O CASO DA PREDAÇÃO DE FÊMEAS DE Atta SPP. POR Canthon virens
Provedor de dados: 196
Autores: Araújo, Márcio da Silva; Rodrigues, Camila Alves; Oliveira, Marco Antônio de; Jesus, Flávio Gonçalves de.
As formigas-cortadeiras são importantes pragas dos setores agrícola e florestal do Brasil. O controle dessa praga, em geral, tem sido realizado com uso de inseticidas químicos, especialmente iscas formicidas envenenadas. Formas alternativas ao controle químico são conhecidas e podem representar significativo controle dessa praga, entretanto são pouco estudadas. O propósito deste texto é discorrer sobre aspectos bioecológicos e perspectivas de uso de um característico predador de fêmeas de Atta Fabricius, 1804 (Hymenoptera: Formicidae), o besouro predador Canthon virens Mannerhein (1929) (Coleoptera: Scarabaeidae). Esse predador, comumente encontrado em áreas de cerrado do Brasil, decapta as fêmas de saúvas assim que elas aterrizam ao solo pós voô nupcial...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/273

MICROPROPAGATION AND PLOIDY STABILITY OF Lippia lacunosa Mart. &amp; Schauer: AN ENDANGERED BRAZILIAN MEDICINAL PLANT
Provedor de dados: 196
Autores: José, Diego Pandeló; de Campos, José Marcello Salabert; Viccini, Lyderson Facio; Alkimim, Emilly Ruas; Santos, Marcelo de Oliveira.
Lippia lacunosa is a Brazilian savanna plant that belongs to the Verbenaceae family. It has been used in folk medicine as a treatment for different diseases. This species represents an endangered Brazilian medicinal plant, and this is the first report documenting a reliable protocol for the in vitro propagation and regeneration of L. lacunosa. Axenic explants were cultivated in MS medium containing different concentrations of naphthalene acetic acid (NAA) to induce root growth. The mean shoot length and the number of roots were highest with 0.06 mg·L-1 NAA. The highest number of buds in shoot regeneration was induced with 2 mg·L-1 6-benzylaminopurine (BA). To obtain a long-term culture, the dwarf shoots were elongated on MS media containing 0.5 mg·L-1 BA...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3203

INFLUENCE OF THE FORM OF HARVESTING AND WASTE APPLICATION ON THE CARBON MANAGEMENT INDEX AND SOIL AGGREGATION UNDER SUGARCANE CULTIVATION
Provedor de dados: 196
Autores: Rosset, Jean Sérgio; Schiavo, Jolimar Antonio; Panachuki, Elói; Salton, Julio Cesar; Ozório, Jefferson Matheus Barros; Souza, Camila Beatriz da Silva; Farias, Paulo Guilherme da Silva.
teste
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environmental assessment; Waste application; Soil structure.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6744

MONITORAMENTO DE VARIÁVEIS MICROMETEOROLÓGICAS EM DIFERENTES AMBIENTES PROTEGIDOS NO PERÍODO DE INVERNO
Provedor de dados: 196
Autores: Paula, Rita de Cássia Mariano de; Silva, Abimael Gomes da; Costa, Edilson; Binotti, Flávio Ferreira da Silva.
Ambientes distintos podem exercer influência sobre o crescimento e desenvolvimento de mudas devido à diferença entre as variáveis micrometeorológicas. Objetivou-se desta forma, monitorar e comparar as variáveis micrometeorológicas no interior de ambientes protegidos, na Universidade Estadual de Mato Grosso do Sul, Unidade Universitária de Cassilândia, MS, no período de 28 de junho a 27 de agosto de 2017. Os ambientes avaliados foram: 1. estufa agrícola coberta com filme de polietileno com tela lateral e frontal de 30% de sombreamento, com tela termorrefletora aluminizada móvel (42/50%); 2. estufa agrícola coberta com filme de polietileno com tela lateral e frontal de 30% de sombreamento, com tela termorrefletora aluminizada móvel (22/30%); 3. telado...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2210

PERFIL NUTRICIONAL DE USUÁRIOS DE UM SPA SOB OS EFEITOS DE UMA DIETA HIPOCALÓRICA
Provedor de dados: 196
Autores: dos Santos, Daiane Costa; Egea, Mariana Buranelo; de Andrade, Cristina Beozzo Junqueira; Silva, Daniella Gonçalves.
Como busca de tratamentos para redução de peso existem alguns programas de SPA onde se tem um tratamento de reeducação alimentar restritiva aliada com a atividade física. O presente trabalho teve o intuito de verificar a perda de peso corporal de usuários de um SPA sob os efeitos de uma dieta hipocalórica em um período de seis dias de internação. Os dados foram coletados através de avaliação do índice de massa corporal, circunferência da cintura e percentual de gordura corporal por bioimpedância elétrica. Trata-se de estudo longitudinal descritivo onde a amostra foi composta por 30 usuários internos de um SPA, sendo 66,7% do sexo feminino e 33,3% do sexo masculino. Os dados obtidos foram analisados pelo teste T student, com confiabilidade de p &amp;lt;...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1210

APPLICATION OF DIFFERENT SOURCES AND DOSES OF BORON IN THE CORN CROP
Provedor de dados: 196
Autores: Silva, Angela Oliveira; Buso, Wilian Henrique Diniz.
One of the main problems faced in corn cultivation, especially in Cerrado regions, is the deficiency of micronutrients. Among the micronutrients essential for the development of plants, boron (B) stands out for participating in a series of physiological processes. Based on this, the present work aimed to evaluate the performance of corn under fertilization with different sources and doses of boron. The randomized block design in a 4x3 factorial scheme was used. Four boron doses (0, 1, 2, and 3 kg ha-1) and three nutrient sources (boric acid, borax, and ulexite), applied in topdressing, were evaluated. Plant height (cm), stem diameter (mm), first ear insertion height (m), ear length (cm), ear diameter (mm), number of rows per ear, number of grains per row,...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4464

PHYSICAL PROTECTOR IN DIRECT SOWING OF BARU INFLUENCING IN THE INITIAL GROWTH OF THE SEEDLINGS
Provedor de dados: 196
Autores: Silva, Rogério Costa da; Lima, Ana Paula Leite de; Lima, Sebastião Ferreira de; Trevizani, Guilherme Marchesini; Leite Junior, João Batista.
The objective of this study was to evaluate the influence of using physical protectors on the emergence and initial growth of Baru seedlings in a direct sowing system. The experiment was installed in a randomized complete block design, testing the use of physical protectors (no protection, P0; plastic cup (500 mL) without the bottom, P1; laminated wood, P2), with 12 repetitions. Weekly soil temperature monitoring was carried out in the morning and in the afternoon in the period between 14 and 56 days after sowing (DAS). Daily emergence follow-up was also performed, and the stem diameter, total height and number of leaves were measured at 81 DAS. The use of physical protectors in the direct seeding of Baru interfered in the soil surface temperature on the...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2726

PROPRIEDADES FÍSICO-QUÍMICAS DE FRUTOS DE JURUBEBA DE TRÊS REGIÕES DO CERRADO
Provedor de dados: 196
Autores: Campos, Luiz Fernandes Cardoso; Peixoto, Joicy Vitória Miranda; Oliveira, Renata Maria de; Seleguini, Alexsander; Nascimento, Abadia dos Reis.
A jurubeba é uma espécie solanácea amplamente difundida em toda a América Tropical, sendo nativa nas Regiões Norte e Nordeste do Brasil. Os seus frutos são utilizados na culinária, na medicina popular para o tratamento de fígado e disfunções gástricas. A planta apresenta potencial de controle biológico contra fitopatógenos e pragas de relevância agronômica. Diante dos seus benefícios e devido à escassez de estudos relacionado a esta, objetivou-se com este trabalho caracterizar os parâmetros físicos e químicos de frutos de jurubeba, colhidos em diferentes regiões do Cerrado; em Goiânia, Itapuranga no Estado de Goiás e Araguari em Minas Gerais. Analisou-se a massa, diâmetro longitudinal (DL), diâmetro transversal (DT), relação DL/DT, pH, sólidos solúveis,...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/740

DEVELOPMENT OF AN ELECTRONIC CONTROLLER FOR LETTUCE PRODUCTION IN GREENHOUSES
Provedor de dados: 196
Autores: Marques Filho, Aldir Carpes; Rodrigues, Jean Paulo; Sartorio de Medeiros, Simone Daniela; Rodrigues de Medeiros, Sergio Ricardo.
The objective of this study was to develop an electronic controller for microclimate control in greenhouses, as well as to verify if the automated control system affects the productivity of two varieties of lettuce “Lactuca sativa”. The control system was developed based on the Atmega 2560 and compatible transducers. An experimental field analysis was carried out over a production cycle for two lettuce varieties. The experimental results showed that the designed equipment worked according to the implemented programming algorithm. However, the ventilation, nebulization and shading actuators did not control environmental variables, due to under sizing. The irrigation process was correctly controlled throughout the experimental period. The electronic...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4043

CRESCIMENTO DE BERINJELA VERDE EM DIFERENTES SUBSTRATOS
Provedor de dados: 196
Autores: Bardiviesso, Estefânia Martins; Costa, Edilson; Barcelos, Michelle Nunes; Bardiviesso, Diógenes Martins; Murakami, Lucas Francisco.
A berinjela tem como centro de origem a China e a &amp;Iacute;ndia. Seu cultivo apresenta elevada import&amp;acirc;ncia pelas propriedades nutricionais dos frutos, principalmente vitaminas e minerais. Este trabalho teve o objetivo de avaliar o crescimento de berinjela verde em diferentes substratos, cultivada em vasos de 13,0 litros. O experimento foi conduzido num delineamento inteiramente casualizado, com os seguintes tratamentos: 100% de esterco bovino; 75% de esterco bovino + 25% de h&amp;uacute;mus de minhoca; 50% de esterco bovino + 50% de h&amp;uacute;mus de minhoca; 25% de esterco bovino + 75% de h&amp;uacute;mus de minhoca; e 100% de h&amp;uacute;mus de minhoca. A semeadura foi realizada em 08 de dezembro de 2012 e o transplante para os vasos no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Artigo científico.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/217

DRY MATTER ACCUMULATION AND SUGAR AND ALCOHOL YIELD OF SUGARCANE SUBMITTED TO NITROGEN SOURCES AND DOSES
Provedor de dados: 196
Autores: Gomes, Flávio Henrique Ferreira; Soares, Frederico Antonio Loureiro; Sousa, Antonio Evami Cavalcante; Silva, Edson Cabral da; Teixeira, Marconi Batista; Bastos, Alefe Viana Souza; Costa, Cicero Teixeira Silva; Vidal, Vitor Marques; Dantas, Leonardo Rodrigues.
The study aimed to evaluate the nitrogen sources and doses application effects on the dry matter production and the sugar and alcohol gross yield of sugarcane (SP80-1816) in the cane-plant cycle in a dystrophic Red Oxisol. The experiment was conducted in the Fazenda Rio Paraiso II field, belonging to Usina Raízen, in Jataí - GO. The experimental design used was randomized blocks, arranged in a factorial scheme (2 x 4), with three replications. The treatments consisted of two nitrogen sources (urea and ammonium nitrate) and four nitrogen doses (0, 60, 120, and 180 kg ha-1). Dry matter variables were analyzed in sub-subdivided plots, as four evaluation periods were added (210, 250, 290, and 330 days after planting). The evaluation periods influenced...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5446

USE OF NANOCOMPOSITE HYDROGEL WITH N-UREA IN THE PRODUCTION OF EGGPLANT SEEDLINGS
Provedor de dados: 196
Autores: Salles, Josiane Souza; Jorge, Marçal Henrique Amici; Costa, Edilson; Melo, Raphael Augusto de Castro e; Lima, Alexandre Henrique Freitas de; Binotti, Flávio Ferreira da Silva.
The use of quality seedlings of eggplant is directly related to the success of their production, with polymers added to the substrate, which work as water conditioners, increase the water retention capacity, and provide better seedling quality. The study aimed to evaluate the use of nanocomposite hydrogel enriched with different proportions of N-urea in the production of eggplant seedlings. The experiment was conducted at the State University of Mato Grosso do Sul, Cassilândia, MS, Brazil, from June to August 2019, under sombrite® 30%. Five treatments were evaluated, using the commercial substrate, Carolina Soil®: 1) commercial substrate without hydrogel; 2) commercial substrate with 0.075g of pure hydrogel (0.00g of N-urea)/15 mL of a substrate; 3)...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5472

FOLIAR SPRAYING OF DOSES OF BORIC ACID IN CORIANDER (Coriandrum sativum L.)
Provedor de dados: 196
Autores: Mello Duarte, Jéssica Rodrigues de; Basílio, Scarlet de Aguiar; Silva, Isabela Carolina; Moreira, Elaine Gleice Silva; Pelá, Adilson.
Coriander (Coriandrum sativum) is a species highly appreciated in Brazilian cuisine and of high nutritional importance due to the presence of vitamins, calcium, and iron. Leafy vegetables are considered nutritionally demanding as their cycles are relatively short and the lack of any essential element affects their growth, yield and quality. This study aimed to evaluate the response of coriander plants (Coriandrum sativum L.) to foliar spraying of boron doses. The experiment was carried out in a greenhouse at The State University of Goiás, Campus Ipameri, in Ipameri-GO. The experimental design was completely randomized, with five treatments and four replications. The treatments consisted of five boron doses applied by foliar spray (0, 1.0, 1.5, 2.0 and 3.0...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3427

PHYSIOLOGICAL QUALITY OF RICE IN THE FUNCTION OF SELENIUM DOSES
Provedor de dados: 196
Autores: Fidelis, Rodrigo Ribeiro; Campestrini, Raphael; Martinez, Roberto Antonio Savelli; Tavares, Taynar Coelho de Oliveira; Lopes, Marília Barcelos Souza.
Objetivou-se com este trabalho avaliar o efeito da aplicação de doses de selênio elementar e selenito na germinação de sementes de genótipos de arroz. O experimento foi conduzido em delineamento experimental inteiramente casualizado, com quatro repetições. Os tratamentos foram dispostos em um esquema fatorial 2x5x2, sendo dois genótipos de arroz (BRS – Primavera e BRSMG – Conai), cinco doses de selênio (0,0; 0,2; 0,4; 0,6 e 0,8 g. L-1 em água), aplicados em duas formas de Se (selenito de sódio – Na2SeO3 e selênio elementar – Se0). Os testes utilizados foram o padrão de germinação e envelhecimento acelerado. As contagens foram realizadas ao quinto e décimo quarto dia, avaliando a porcentagem de plântulas normais, anormais, sementes não germinadas,...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1893

APLICAÇÃO DE ÁCIDO BÓRICO SOBRE AS CARACTERÍSTICAS PRODUTIVAS DO REPOLHO EM DIFERENTES ÉPOCAS
Provedor de dados: 196
Autores: Silva, Luciana Maria da; Basílio, Scarlet de Aguiar; Silva Junior, Rogério Lamim; Nascimento, Mariana Vieira; Benett, Cleiton Gredson Sabin; Benett, Katiane Santiago Silva.
A cultura do repolho é realizada principalmente em pequenas áreas e depende de grande mão de obra, sendo na maior parte conduzida pela agricultura familiar. O objetivo deste trabalho foi identificar a melhor época de aplicação e doses de boro para as características produtivas e qualidade de cabeças de repolho. O experimento foi realizado na fazenda experimental da Universidade Estadual de Goiás, Câmpus de Ipameri (UEG/Ipameri). O delineamento experimental utilizado foi o de blocos casualizados no esquema fatorial 2 x 5, sendo duas épocas de aplicação (15 e 25 dias após o transplante (DAT)) e cinco doses de boro (0; 2,5; 5,0; 7,5 e 10,0 kg ha-1), com quatro repetições. As parcelas foram constituídas por quatro linhas de 1,6 m dispostas no espaçamento de...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/228

QUALIDADE DA ÁGUA DO CÓRREGO DO CEDRO PARA FINS DE IRRIGAÇÃO DE ALIMENTOS “IN-NATURA”
Provedor de dados: 196
Autores: Dalastra, Cleiton; Hernandez, Fernando Braz Tangerino; Barboza, Gustavo Cavalari; Sonego, Carolina Rocha.
A água tem papel vital como elemento mantenedor da vida terrestre; essencial para a sobrevivência humana e essencial na produção de alimentos. O avanço da urbanização tem comprometido o equilíbrio ecológico do ambiente principalmente no despejo de efluentes contaminantes nos corpos d’águas ou nas suas adjacencias. O grande problema está na reutilização dessa água contaminada na produção de alimentos, fato que ocorre na circuvizinhança do perimetro urbano de Cassilandia-MS, abastecido pelo córrego do Cedro, objeto de estudo do presente trabalho, o qual recebe resíduos sanitários de forma direta das residências próximas ou oriundos de uma estação de tratamento de esgoto. Neste contexto este trabalho avaliou a qualidade da água, comparando-a com os parâmetros...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/242

EFEITO DA APLICAÇÃO DE RESÍDUOS URBANOS E INDUSTRIAIS NA CULTURA DA AVEIA PRETA CULTIVADA EM LATOSSOLO VERMELHO EM SISTEMA PLANTIO DIRETO
Provedor de dados: 196
Autores: dos Santos, Susiane de Moura Cardoso; Antonangelo, João Arthur; Deus, Angélica Cristina Fernandes; Büll, Leonardo Theodoro.
O emprego racional de resíduos industriais e urbanos na agricultura sob sistema plantio direto (SPD) promove inúmeros benefícios sobre as propriedades físicas, químicas e biológicas do solo, reduzindo assim, a utilização de fertilizantes sintéticos, proporcionando efeitos benéficos ao solo e ao ecossistema. Além de atuarem como atenuadores da acidez do solo, esses resíduos são excelentes fontes de nutrientes às plantas. O trabalho teve como objetivo avaliar o estado nutricional e a produção de matéria seca da aveia preta após aplicação de resíduos industriais e urbanos sob sistema plantio direto. Trata-se de um trabalho em longo prazo, perfazendo um período de nove anos, onde até o presente momento ocorreram cinco aplicações de resíduos em 2002, 2005,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nutrição de plantas.
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/247

SUBSTRATOS ORGÂNICOS NA PRODUÇÃO DE MUDAS DE CAFEEIRO EM TUBETES
Provedor de dados: 196
Autores: Pereira, Igor Souza; Lima, Karen Cristina Corrêa de; Melo Junior, Heliomar Baleeiro de.
Considerando-se a importância das mudas na formação de lavoura cafeeira (Coffea arabica L.), objetivou-se avaliar características agronômicas e índices de qualidade de mudas do cafeeiro cv. Topázio MG 1190, produzidos em tubetes com a utilização de diferentes proporções de materiais orgânicos no substrato comercial. O experimento foi em delineamento experimental em blocos casualizados, dispostos em esquema fatorial 4 x 4, sendo quatro fontes de esterco: bovino, cama de frango, coelho e suíno em quatro proporções (0, 20, 40 e 60%) no substrato comercial Bioplant® com quatro repetições. As parcelas foram formadas por sete plantas dispostas em tubetes com volume de 180 mL.  Foram avaliadas as características agronômicas: altura da planta, número de par de...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1254

EFEITO ANTIALIMENTAR DE EXTRATOS HIDROALCOÓLICOS DE MELIA AZEDARACH (MELIACEAE) SOBRE HELICOVERPA ARMIGERA (LEPIDOPTERA: NOCTUIDAE)
Provedor de dados: 196
Autores: Andrade, Jessica Velasco; Alcassio, Thamiris Penajo; Saldanha, Fabíola Gonzaga; Toscano, Luciana Cláudia; Dias, Pamella Mingotti.
O objetivo desse trabalho foi avaliar o efeito de extrato hidroalcoólico de Melia azedarach sobre a preferência alimentar de Helicoverpa armigera. O delineamento utilizado foi inteiramente casualizado com 4 tratamentos e 5 repetições em parcelas subdivididas, sendo parcela (tratamento) e subparcela (tempo). Os tratamentos utilizados foram: extratos de folhas, ramos, folhas + ramos de M. azedarach a 5% (p/v) e água destilada (testemunha). Foram realizados testes com e sem chance de escolha, onde avaliaram-se os parâmetros: número de insetos atraídos, consumo de massa seca (g) e índice de preferência (%). Para o teste com chance de escolha foram observadas diferenças significativas para a atratividade apenas quando utilizou-se extrato de folhas + ramos de M....
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/800

PRODUTIVIDADE E ANÁLISE ECONÔMICA DO CULTIVO CONSORCIADO DE MILHO E BRAQUIÁRIA NO NOROESTE DO PARANÁ
Provedor de dados: 196
Autores: Wenneck, Gustavo Soares; Saath, Reni; Araujo, Larissa Leite de; Pereira, Gustavo Lopes; Oliveira, Giovanna Gabriela Ferreira de; Sá, Nathália de Oliveira; Volpato, Camila de Souza.
A consorciação de milho e Urochloa ruziziensis apresenta potencial para os sistemas de produção agrícola, permitindo a produção de grãos e biomassa remanescente. O estudo tem como objetivo avaliar a produtividade e a viabilidade econômica das modalidades de consórcio de milho e U. ruziziensis na região noroeste do Paraná. O experimento foi conduzido em Maringá-PR, em delineamento inteiramente casualizado com cinco tratamentos (milho solteiro; U. ruziziensis solteira; milho com U. ruziziensis na entre linha; milho com U. ruziziensis na mesma linha; milho com U. ruziziensis em linhas intercaladas) e quatro repetições. Foi analisado o desenvolvimento inicial e produtividade de grãos do milho, e produção de biomassa de milho e U. ruziziensis. Os dados foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biomass; Grain production; No-Tillage System; Biomassa; Produção de grãos; Sistema Plantio Direto.
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6163

EXTRAÇÃO E EXPORTAÇÃO DE NITROGÊNIO, FÓSFORO E POTÁSSIO PELO MILHO ADUBADO COM DEJETOS DE SUÍNOS
Provedor de dados: 196
Autores: Scherrer Menezes, June Faria; da Silva Berti, Mariana Pina; Vieira Júnior, Valter Divino; Ribeiro, Rênystton de Lima; Berti, Christian Luis Ferreira.
O objetivo deste trabalho foi avaliar a extração de nitrogênio (N), fósforo (P) e potássio (K) pela cultura do milho adubada com dejetos líquidos de suínos (DLS). O experimento foi conduzido no período de outubro de 2013 a abril de 2014, na Fazenda Fontes do Saber, localizada na Universidade de Rio Verde, Goiás. O experimento foi conduzido em um Latossolo Vermelho distroférrico de textura argilosa (540 g kg-1), e os tratamentos constituíram da aplicação ou não de DLS na dose de 30 m3 ha-1. Após a aplicação dos dejetos na superfície do solo foi feita a semeadura do milho e a partir das análises foliares avaliaram-se a extração de N, P e K pelas plantas de milho, em oito épocas, com intervalos médios de 15 dias, durante o ciclo de crescimento e...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1645

ESTIMATIVAS VOLUMÉTRICAS PARA UM POVOAMENTO ADENSADO DE EUCALYPTUS SP. EM REGIME DE CURTA ROTAÇÃO
Provedor de dados: 196
Autores: Nunes, Jéssica Silva; Soares, Thelma Shirlen.
Este estudo teve como objetivo estabelecer equações volumétricas, fatores de forma, de empilhamento e de cubicação para um povoamento de eucalipto com 24 meses de idade, implantado em regime de curta rotação, sob diferentes espaçamentos (3,0 m x 0,5 m; 3,0 m x 1,0 m; 3,0 m x 1,5 m; 3,0 m x 2,0 m; 3,0 m x 2,5 m e 3,0 m x 3,0 m), em Jataí-GO. Para o ajuste volumétrico as árvores foram cubadas pelo método de Smalian, sendo avaliadas seis equações para cada espaçamento. Após a seleção das equações realizou-se o teste de identidade de modelos. Também foram obtidos, para cada espaçamento, os fatores de forma, empilhamento e cubicação. A equação oriunda do modelo de Spurr foi selecionada para os espaçamentos 3,0 m x 0,5 m; 3,0 m x 1,5 m e 3,0 m x 2,0 m. Para os...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1661

RESPOSTA DA RÚCULA À ADUBAÇÃO ORGÂNICA COM DIFERENTES COMPOSTOS ORGÂNICOS
Provedor de dados: 196
Autores: Salles, Josiane Souza; Steiner, Fábio; Abaker, João Eduardo Pereira; Ferreira, Thales Silva; Martins, Gustavo Luíz Mamoré.
A adubação orgânica pode conferir maior produtividade ao sistema de produção de hortaliças por melhorar a qualidade do solo e aumentar a rentabilidade do olericultor. Neste contexto, o objetivo deste trabalho foi avaliar a eficiência da aplicação de diferentes resíduos orgânicos no crescimento e na produção de rúcula. O experimento foi realizado na Universidade Estadual de Mato Grosso do Sul, em Cassilândia-MS, em condições de ambiente protegido. Os tratamentos foram constituídos da aplicação isolada ou combinada de diferentes fontes de resíduos orgânicos: 1) esterco de aves (EA); 2) esterco bovino (EB); 3) torta de filtro (TF); 4) esterco de aves + esterco bovino (EA +EB); 5) esterco de aves + torta de filtro (EA+TF); 6) esterco bovino + torta de filtro...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1450

CYCLING OF WINTER FORAGE NUTRIENTS UNDER INTEGRATED CROP-LIVESTOCK SYSTEMS
Provedor de dados: 196
Autores: Perini Vengen, Andressa; Bartzen, Bruna Thaina; Mattei, Eloisa; Rocha de Moraes Rego, Carlos Augusto; Piano, Jeferson Tiago; Rabello de Oliveira, Paulo Sergio.
This study aimed to evaluate the decomposition and release of nutrients from the remaining straw of two annual forage species conducted in an integrated crop-livestock system (ICLS). The experimental design used was randomized blocks, in split plots, with three replicates. The managements were allocated in the plots (52 m2): without grazing, one grazing, and two grazings. Subplots were defined by material collection times after the forage’s desiccation (0, 30, 60, 90, and 120 days after desiccation). Dry matter yield, amounts of carbon, nitrogen, phosphorus, and potassium, and half-life time were evaluated. Oat cultivar IPR Esmeralda had the highest initial dry matter yield (6,099 kg ha-1) when not grazed, while triticale cultivar IPR 111 showed the...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/4963

ÉPOCAS DE SEMEADURA DO TRIGO PARA A REGIÃO CENTRO-SUL MATO-GROSSENSE
Provedor de dados: 196
Autores: Silva, Elijanara Raissa; de Oliveira, Juliana Nunes; Rubio, Crislane Pereira; de Lyra, Gabriel Albuquerque; Steiner, Fábio.
A época de semeadura é um dos principais fatores que afeta o rendimento da cultura do trigo na região do Centro-Oeste, devido aos riscos de ocorrência de deficiência hídrica no período de outono-inverno. O objetivo deste trabalho foi identificar a melhor época de semeadura e avaliar o potencial de rendimento da cultura de trigo (Triticum aestivum L., cv. Valente) para a região Centro-Sul Mato-Grossense. O experimento foi realizado no município de Santo Antônio do Leverger (MT), na safra 2013. O delineamento experimental foi em blocos ao acaso com quatro repetições e cinco tratamentos, sendo eles compostos por cincos épocas de semeadura: 24 de fevereiro, 03, 10, 17 e 24 de março de 2013. Os resultados reportaram que as épocas de semeadura testadas não...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1762

PRIMING AND GROWTH INHIBITOR IN THE PRODUCTION OF HIGH-QUALITY PEPPER SEEDLINGS
Provedor de dados: 196
Autores: Silva, Abimael Gomes; Binotti, Flávio Ferreira da Silva; Matos, Adriana Hernandes Pinto; Silva, Talita Cristina Campos Pereira da; Silva, Tatiane Carla; Costa, Edilson.
This study aimed to evaluate the effect of nitrate salts and a growth regulator on seed conditioning. Subsequently, the responses of the influence of the leaf application of paclobutrazol (PBZ) and nitrogen on the quality of seedlings of Capsicum frutescens L. were evaluated. Two experiments were carried out. The first experiment was conducted in a completely randomized design to evaluate priming, as follows: T1 – control, T2 – control (water), T3 – 0.2% calcium nitrate, T4 – 0.2% potassium nitrate, T5 – 0.1% calcium nitrate + 0.1% potassium nitrate, T6 – PBZ, and T7 – PBZ + 0.1% calcium nitrate + 0.1% potassium nitrate. The second experiment was carried out in a completely randomized design in a 2×5 factorial scheme consisting of priming (absence and...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5828

MANEJO DA MUCUNA-PRETA NA SUPRESSÃO DE PLANTAS DANINHAS NA CULTURA DA ALFACE-CRESPA
Provedor de dados: 196
Autores: Barbosa, Jaqueline de Araujo; Franke, Douglas Elias; Ferreira, Silvio Douglas; Salvalaggio, Adriana Cologni; da Costa, Neumarcio Vilanova.
Plantas de cobertura podem causar a supressão de plantas daninhas devido aos efeitos físicos e alelopáticos produzidos pela palhada. O objetivo deste trabalho foi o de avaliar o manejo da palhada de mucuna-preta (superficial ou incorporada) no controle de plantas daninhas na cultura da alface-crespa. O delineamento experimental foi o de blocos ao acaso, dispostos em parcelas subdividas, com quatro repetições. As parcelas compreenderam os dois sistemas de manejo de palhada da mucuna-preta (superficial ou incorporada) e as subparcelas foram constituídas pela prática da capina manual (com ou sem capina). Os resultados reportaram que não houve redução na massa seca de plantas daninhas com o uso da palhada superficial ou incorporada. No entanto, o manejo com a...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1872

VARIAÇÃO ESPAÇO-TEMPORAL DA TEMPERATURA DO SUBSTRATO EM BANDEJAS DE PRODUÇÃO DE MUDAS
Provedor de dados: 196
Autores: Cavalcanti, Sávio Duarte Lopes; Gomes, Nicoly Farias; Pandorfi, Héliton; Almeida, Gledson Luiz Pontes; Montenegro, Abelardo Antônio de Assunção.
A temperatura do substrato nas bandejas é um fator variável no tempo e no espaço, que assume relevante importância nos processos físicos e nas trocas de energia com a atmosfera. Esta grandeza física interfere na germinação, crescimento radicular, absorção de água e nutrientes. Dessa forma, o conhecimento da dinâmica da temperatura do substrato é fundamental para a agricultura. Para tanto, essa pesquisa foi conduzida com o objetivo de verificar a variação espaço-temporal da temperatura do substrato em bandejas de produção de mudas. Foram utilizadas bandejas de polipropileno convencional (preta) e polipropileno pintada de branco. O registro da temperatura do substrato foi realizado em 48 células de cada bandeja, consecutivamente, às 8, 10, 12, 14 e 16 horas....
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2648

OCORRÊNCIA DE ÁCAROS EM SERINGUEIRA IRRIGADA EM CULTIVO INICIAL
Provedor de dados: 196
Autores: Rocha, Livia de Freitas; Toscano, Luciana Cláudia; Martins, Gustavo Luís Mamoré; da Silva, Eliamara Marques.
O objetivo deste estudo foi avaliar a ocorrência de ácaros em seringueira irrigada com talhões de diferentes idades em cultivo inicial. Foi estudada a fauna de ácaros fitófagos e predadores em dois talhões de seringueira com duas idades de implantação (26 e 31 meses), localizados em Cassilândia-MS. Foram realizadas coletas quinzenais, no período de novembro de 2010 a maio de 2011. Foram estabelecidos 30 pontos por talhão, onde 10 plantas foram amostradas coletando-se dois folíolos por planta, totalizando 120 folíolos por coleta. Foi registrado o número total de ácaros encontrados em ambas as faces. No total, foram coletados 477 ácaros, sendo as famílias Tetranychidae e Tenuipalpidae com o maior número de indivíduos, 150 e 148, respectivamente. A espécie de...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2680

PLANTING FERTILIZATION AND NITROGEN DOSES IN TOPDRESSING IN SECOND-CROP CORN
Provedor de dados: 196
Autores: Silva, Luciana Maria da; Silva Junior, Rogério Lamim; Leão Pereira Resende, Cecília; Marangoni Montes, Rafael; Santiago Silva Benett, Katiane; Benett, Cleiton Gredson Sabin.
O presente trabalho teve como objetivo avaliar a influência da adubação com formulados na semeadura e doses de nitrogênio em cobertura sobre as características produtivas do milho cultivado na safrinha. O experimento foi conduzido entre os meses de março a junho de 2018, na fazenda da Universidade Estadual de Goiás, Unidade Universitária de Ipameri-GO. O delineamento experimental utilizado foi o de blocos casualizados no esquema fatorial 3 x 5 sendo três formulações de adubos na semeadura (06-22-12; 08-20-15 e 06-22-12 + 2% de carbono orgânico) e cinco doses de N (0, 50, 100, 150 e 200 kg ha-1) em cobertura, com quatro repetições. Determinou-se o teor de nitrogênio foliar, massa fresca e seca de folhas, altura de plantas, diâmetro do colmo, altura de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays L.; Nitrogen fertilization; Fertilizer of planting; Zea mays L.; Adubação nitrogenada; Adubo de plantio.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6968

CAN SOWING SPEED AFFECT CORN YIELD?
Provedor de dados: 196
Autores: Marques Filho, Aldir Carpes; Ventura, Heitor Cardoso.
In sowing operation, it is essential to control the factors that can affect the quality of seed and fertilizer deposition. These factors range from the correct choice of dosing mechanisms to machine regulation and operating speed control. The present research aimed to analyze the influence of sowing speed on the productive performance of the corn crop. The study was carried out at Fazenda São Geraldo, in the municipality of Boracéia, São Paulo. Four operating speeds 3, 5, 7 and 9 km h-1 were applied in a seeder, with a mechanical horizontal seed meter. The experimental design was carried out in strips. The results showed that sowing operational speed directly influences the final corn yield. There is a positive correlation between sowing speed and...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6486

CALCÁRIO LÍQUIDO E CALCÁRIO CONVENCIONAL NA CORREÇÃO DA ACIDEZ DO SOLO
Provedor de dados: 196
Autores: Bambolim, Amauri; Caione, Gustavo; Souza, Naiara Fernanda; Seben Junior, Getulio de Freitas; Ferbonink, Guilherme Ferreira.
A acidez pode alterar a disponibilidade dos nutrientes no solo. Objetivou-se com o presente trabalho avaliar o efeito da aplicação de calcário líquido e calcário convencional na correção da acidez de um Latossolo Vermelho-Amarelo distrófico do Cerrado. O delineamento experimental utilizado foi inteiramente casualizado, com três repetições. As doses de calcário líquido aplicadas foram equivalentes a 5; 10; 15 e 20 L ha-1 e as doses de calcário convencional utilizadas foram equivalentes a 1,0; 1,5; 2,0 e 2,5 t ha-1. Após a aplicação dos corretivos de acidez, o solo foi acondicionado em recipientes com capacidade para 0,4 dm3 com umidade próxima a capacidade de campo. Aos 70 dias após a aplicação dos corretivos foram mensurados o pH do solo, teores de...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/277

ATRIBUTOS TECNOLÓGICOS, STAND E PRODUTIVIDADE DA CANA-PLANTA CORRELACIONADOS COM ASPECTOS DA FERTILIDADE DO SOLO
Provedor de dados: 196
Autores: Alves, Vinicius; Montanari, Rafael; Carvalho, Morel de Passos e; Correa, Adriany Rodrigues; Roque, Cassiano Garcia.
A agricultura de precisão, que pode ser aplicada em qualquer etapa da produção de cana-de-açúcar, visa proporcionar maior produtividade, redução do impacto ambiental e melhor rendimento econômico pela aplicação correta dos insumos agrícolas. Objetivou-se com este trabalho caracterizar as zonas específicas de manejo do solo, empregando-se correlações lineares e espaciais entre atributos da cultura da cana-de-açúcar e atributos químicos de um Latossolo Vermelho-Amarelo distrófico, no sentido de indicar aquele que mais eficientemente esteja relacionado com o aumento da produtividade. O trabalho foi desenvolvido no ano agrícola de 2012/13, no município de Chapadão do Céu, Goiás, Brasil. Foram analisadas as correlações lineares e espaciais entre atributos da...
Tipo: Info:eu-repo/semantics/article
Ano: 2015
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/255

INITIAL SPROUT GROWTH OF POTATO SEED MINITUBERS UNDER SALT STRESS
Provedor de dados: 196
Autores: Oliveira, Camilla Paulino de; Douradinho, Gabriel Zanuto; Bortolazzo, Guilherme; Steiner, Fábio.
Potato (Solanum tuberosum L.) is a major crop worldwide and the tuber yield of currently used cultivars is strongly reduced at high soil salt levels. The effects of salt stress on early sprout growth of potato plants were investigated using the cultivar Ágata. Potato seed minitubers were planted in 0.4 L pots filled with commercial substrate (Bioplant®), and maintained under greenhouse conditions. A completely randomized design with five treatments and five replications was used. Three days after sprouting, potato plants were exposed to five salinity levels [0 (control), 25, 50, 75 and 100 mmol L–1 of NaCl] for 28 days. Results showed that the exposure of plants to 100 mmol L–1 NaCl reduced the shoot height (72%), shoot dry matter (76%) and root dry matter...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/741

PHYSICOCHEMICAL CHARACTERIZATION OF FERMENTED BOKASHI COMPOST PRODUCED ON FARM IN SOUTHERN BRAZIL
Provedor de dados: 196
Autores: Lopes Pereira, Gustavo; Leite de Araújo, Larissa; Soares Wenneck, Gustavo; Saath, Reni; Ghuidotti, Gabriela Cristina; Presotto Bertolo, Raissa.
Bokashi is fermented organic compost capable of improving the physical, chemical, and biological conditions of the soils. The compost action in the agricultural production system is influenced by its preparation, resulting in products with different physicochemical characteristics. The study aimed to characterize bokashi produced on-farm and compare it with commercial products. The produced composts in southern Brazil were obtained through efficient microorganisms (EM), collected in an area of permanent preservation, and kefir. Two commercial composts were used for comparison (Plantae FertTM and Bokashi Sementes BrasilTM). Physical characteristics related to apparent specific gravity, water content, and water retention capacity and chemical characteristics...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Microorganisms; On-farm; Organic compost; Residues; Microrganismos; On-farm; Composto orgânico; Resíduos.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6926

EFEITOS DE DIFERENTES FONTES DE RADIAÇÃO NA FISIOLOGIA E VIDA ÚTIL PÓS-COLHEITA DE CAMU-CAMU
Provedor de dados: 196
Autores: Sanches, Alex Guimarães; Silva, Maryelle Barros da; Moreira, Elaine Gleice Silva; Costa, Jaqueline Macedo; Cordeiro, Carlos Alberto Martins.
Por se tratar de um fruto climatérico, o camu-camu (Myrciaria dúbia (H.B.K.) McVaugh)apresenta uma rápida deterioração em temperatura ambiente, tal fato é atribuído à elevada taxa respiratória do fruto, ao aumento da produção de etileno e perda de água. Assim, o presente trabalho tem por objetivo avaliar os efeitos da irradiação gama e ultravioleta na sua conservação in natura. Os frutos foram mantidos sob refrigeração por um período de 21 dias em DIC fatorial composto por cinco tratamentos e oito tempos de avaliação. A cada três dias os frutos foram avaliados quanto à: perda de massa fresca, firmeza, sólidos solúveis, acidez titulável, pH, vitamina C, carotenóides e taxa respiratória. As fontes de irradiação não diferiram estatisticamente ao longo do...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1190

STRUCTURAL QUALITY INDICATORS IN COMPACTED OXISOLS GROWN WITH CORN
Provedor de dados: 196
Autores: de Vares Rossetti, Karina; Centurion, José Frederico.
In the face of the elevated cost of economic and environmental order to recover degraded soil, the monitoring of the structural quality of the soil through physical and plant indicators is recommended. This way, this work aimed to verify which parameters may be used together with soil penetration resistance (PR), after compression induced by agricultural machinery traffic in Haplustox (LVd) and an Eutrustox (LVef), grown with corn. The experiment was conducted with a randomized block design in a split-plot scheme with four replications. Five treatments and three soil layers (0-0.10; 0.10-0.20, and 0.20-0.30 m) for each soil class were evaluated. The treatments were: NC = conventional preparation without additional compression; C14, C17, and C110 = one pass...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5092

ALTERNATIVE SUBSTRATES FOR PRODUCTION OF YELLOW PASSION FRUIT SEEDLINGS
Provedor de dados: 196
Autores: Aires, Eduardo Santana; Aragão, Carlos Alberto; Gomes, Itala Laiane Silva; Souza, Gilmário Noberto de; Andrade, Isa Gabriela Vieira de.
This study aimed to evaluate different substrates to produce yellow passion fruit seedlings. For this purpose, an experiment was carried out in a greenhouse, from April to June 2016. A completely randomized design with five replications, in a 6 x 5 factorial scheme was used. The first factor was the alternative substrates (poultry, cattle and equine manure, sugarcane and coconut bagasse, and Organomais compost). The second factor was the replacement levels to the commercial substrate of Plantmax® (100:0, 75:25, 50:50, 25:75, 0:100). The seedling evaluation was carried out 42 days after sowing. The following variables were analyzed: length, width, and the number of leaves; plant height and shoot dry matter. A significant effect (P&amp;lt;0.05) for the...
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/3890

PROPRIEDADES QUÍMICAS DE UM LATOSSOLO SOB DIFERENTES SISTEMAS DE MANEJO
Provedor de dados: 196
Autores: Santos, Osvaldir Feliciano; Souza, Hugo Manoel; Oliveira, Marcela Pacola; Caldas, Marilise Bittencourt; Roque, Cassiano Garcia.
A utilização do solo para fins agrícolas provoca alterações químicas, físicas e biológicas no solo, podendo ser necessária a intervenção por meio do manejo e utilização de calagem e adubação, sendo que a falta destes procedimentos pode afetar drasticamente os índices de produção. Desta forma, objetivou-se avaliar os efeitos de sistemas de manejo nas propriedades químicas de um Latossolo Vermelho distrófico argiloso do Cerrado brasileiro. Os sistemas avaliados foram: i) sistema de plantio convencional; ii) sistema de plantio direto; e, iii) área de floresta de eucalipto. As amostras de solo foram coletadas nas profundidades de 0-0,20 e 0,20-0,40 m. O delineamento experimental foi em blocos ao acaso no esquema fatorial 3x2 com três repetições. O sistema de...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1185

BIOMASS: BIOETHANOL TRANSFORMATION AND PRODUCTION PROCESS
Provedor de dados: 196
Autores: Fasioli Silva, Rebeca; Mascarenhas, Maria do Socorro; Batistote, Margareth.
The economic development of a country depends on the use of energy in various processes, the use of natural sources to generate energy resources has great potential. Environmental issues such as global warming have aroused interest around the world regarding bioenergy, such as biomasses that generate a low carbon impact and are susceptible to transformation, such as sugarcane and corn. The study aims to evaluate the main energy crops and their transformation processes, as well as obtain an overview of the main bioethanol producing countries and analyze the productivity of ethanol from sugarcane and corn. Exploratory research was carried out, using published databases related to the topic and classification by relevance. It was possible to observe that the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy resources; Sugarcane and corn; Bioethanol; Bioenergy; Recursos energéticos; Cana e milho; Bioetanol; Bioenergia.
Ano: 2022
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/7089

PRODUÇÃO DE CONÍDIOS EM SUBSTRATO SÓLIDO E COLONIZAÇÃO SUPERFICIAL POR Trichoderma harzianum
Provedor de dados: 196
Autores: Pereira Costa Muniz, Paulo Henrique; Silva Peixoto, Gustavo Henrique; Pereira Martins Teixeira, Maysa; Corrêa Marques de Mello, Sueli; Costa Carvalho, Daniel Diego.
Alguns fungos apresentam difícil esporulação em meios artificiais. Neste contexto, o processo de produção massal de conídios de Trichoderma sp., para o emprego em biocontrole mais utilizado, se baseia na multiplicação por meio da fermentação em substrato sólido. O objetivo deste trabalho foi estudar a produção de conídios de cinco isolados de T. harzianum em substrato sólido e a capacidade destes para colonização superficial de meio de cultura rico em sacarose. Para tanto, os isolados foram submetidos à produção de conídios em substrato sólido (arroz parboilizado umedecido e autoclavado) a 25 ºC e a fotoperíodo de 12h por sete dias. Em seguida, os conídios foram inoculados em quadrados (1,5 x 1,5 cm) de batata dextrose ágar-sacarose (BDA-S) para se estimar...
Tipo: Info:eu-repo/semantics/article
Ano: 2018
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2608

THERMAL STRESS IN THE ADEQUACY OF THE CHEMICAL SCARIFICATION PERIOD IN BRACHIARIA SEEDS
Provedor de dados: 196
Autores: Pinto, Adriana Hernandes; Batista, Thiago Barbosa; Binotti, Flávio Ferreira da Silva; Binotti, Eliana Duarte Cardoso; Costa, Edilson.
Forage seeds often have a low germination percentage due to their seeds' dormancy, such as seeds of the genus Urochloa. Chemical scarification is chosen to overcome the dormancy, yet the seed's vigor level is not taken into account. On this wise, the method can harm the seed's quality. In this context, the study aimed to investigate the appropriate scarification period in brachiaria seeds and how the lot's thermal stress can affect this result. The experimental design was completely randomized, arranged in a 3x4 factorial scheme, designated by thermal stress (0, 24, and 48 hours) and periods of chemical scarification with concentrated sulfuric acid (0, 5, 10, and 15 minutes), with four repetitions. After scarification of the treatments, the seeds were...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5753

Potencial seletividade de herbicidas em pré e pós-emergência em linhaça (Linum usitatissimum L.)
Provedor de dados: 196
Autores: Dalpubel Mattiuzzi, Mateus; Paiola Albrecht, Alfredo Junior; Baccin, Luisa Carolina; Moreira Silva, André Felipe; Paiola Albrecht, Leandro; Larini, Willian Felipe.
A linhaça é uma oleaginosa amplamente utilizada na alimentação humana e animal, como cultura de cobertura em agroecossistemas e para produção de fibras. Para facilitar o manejo de plantas daninhas na cultura, este trabalho teve como objetivo avaliar potenciais herbicidas seletivos para o cultivo de linhaça aplicados em pré-plantio incorporado (PPI), pré-emergência (PRE), pós-emergência inicial (POS), pós-emergência tardia (POS tardio) uma vez que ainda não existem herbicidas registrados para uso em linhaça no Brasil. Portanto, quatro experimentos foram conduzidos em delineamento inteiramente casualizado com quatro repetições, e cinco (exp. 1), 21 (exp. 2), 26 (exp. 3) e quatro (exp. 4) tratamentos. Foram avaliadas a injúria na cultura e a matéria fresca e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Injury; Bentazon; Protoporphyrinogen oxidase (PPO) inhibitors; Acetolactate synthase (ALS) inhibitors; Acetyl-CoA carboxylase (ACCase) inhibitors; Injúria; Bentazon; Inibidores da protoporfirinogênio oxidase (PPO); Inibidores da acetolactato sintase (ALS); Inibidores da acetil-CoA carboxilase (ACCase).
Ano: 2023
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/7058

CHEMICAL FERTILIZATION THROUGH FERTIRRIGATION IN THE EVALUATION OF THE BIOCHEMICAL CHARACTERISTICS OF THE WATERMELON FRUITS
Provedor de dados: 196
Autores: Santos de Andrade, Antonio Ricardo; Franco, Euler Soares; Guerra, Hugo Orlando Carvallo; Jadoski, Sidnei Osmar; Silva, Edijailson Gonçalves da; Cruz, Adiel Felipe da Silva; Ferreira, Maria Emanuely da Silva; Silva, Edes Torres da; Soares, Hammady Ramalho e.
The objective of this work was to evaluate the effects of splitting in three different doses of phosphorus and potassium, combined with each other, and it was applied fertirrigation in watermelon crop, and to evaluate their effects on fruit quality. The statistical was in a complete randomized block design, and the treatments were arranged in a factorial scheme (3 x 3) in subdivided splits, resulting in 9 treatments with tree replications, totaling 27 plots in the experimental area. In the horizontal plots the three doses of phosphorus fertilization (100, 150 and 300 kg.ha-1 of P2O5) were randomly allocated, and in the subplots the three potassium doses (50, 100 and 200 kg.ha-1 of K2O), were applied in fertirrigation. The cultivar used was Crimson Sweet....
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/5561

ATITUDES EM RELAÇÃO À INFORMAÇÃO DE PREÇOS DE ALIMENTOS
Provedor de dados: 196
Autores: Groot, Etiénne.
O Brasil passa por um período com tendência inflacionária e, desta forma, as alterações de preços repercutem no comportamento dos consumidores. Objetivou-se com o presente estudo a avaliação da percepção dos consumidores em relação aos preços dos alimentos, a sua atitude em buscar os menores preços de mercado e a sua propensão a utilizar informações de mídia eletrônica. Para isso, foram consideradas 54 entrevistas pessoais realizadas com consumidores de Dracena/SP, com auxílio de questionário estruturado. Os resultados mostram que, mesmo em ambiente inflacionário, a percepção dos consumidores em relação ao conhecimento dos preços dos produtos ainda é alta, principalmente entre as pessoas com mais de 45 anos de idade. Muitos consumidores pesquisam os preços...
Tipo: Info:eu-repo/semantics/article
Ano: 2017
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1632

RECORD OF THRIPS (INSECTA: THYSANOPTERA) AND FUNGI AFFECTING SOURSOP TREES IN THE STATE OF ACRE, BRAZIL
Provedor de dados: 196
Autores: Santos, Rodrigo Souza; Nogueira, Sônia Regina; Gonçalves, Rivadalve Coelho.
The drying and death of soursop seedlings (Annona muricata L.) were reported on Viveiro da Floresta in Rio Branco, state of Acre, Brazil, in March 2017. The seedlings were obtained from municipalities of Dona Euzébia, Minas Gerais state, and the seeds from Capixaba, Acre state, Brazil. Seedlings with dieback symptoms were taken to the Laboratories of Entomology and Phytopathology of Embrapa Acre and analyzed with a stereomicroscope. The thrips found were preserved in ethanol (70%), mounted on slides, and identified in the specialized literature. Moreover, the isolation of fungi from leaves and stems was performed, which were inserted on Petri dishes with a PDA medium. The insect was identified as Pseudophilothrips sp., and the fungi pertained to the genera...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/6301

CARACTERIZAÇÃO FISÍCO-QUÍMICA E ANÁLISE MICROBIOLÓGICA DE COOKIE DE FARINHA DE AVEIA
Provedor de dados: 196
Autores: Dias, Bruna Ferreira; Santana, Gabriela Silva; Pinto, Ellen Godinho; de Oliveira, Camila Fernanda Dias.
A aveia é uma gramínea, pertencente à família poaceae e ao gênero avena. Seu grão é amplamente utilizado para a fabricação de produtos de panificação.  O biscoito é um produto que apresenta grande interesse comercial e está em constante desenvolvimento. Com base nos estudos o objetivo no trabalho foi explorar o efeito da incorporação da farinha de aveia no processamento de biscoito tipo cookie, com relação às características físico-químicas e microbiológicas. Foi elaborado biscoito tipo cookie enriquecido com farinha de aveia, com diferentes concentrações de aveia (2%, 4%, 6%). Estes foram avaliados quanto às características físico-químicas (pH, Sólidos Solúveis Totais, vitamina C e umidade) e microbiológica (Coliformes Totais). A partir das análises...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1201

PARCHMENT PRESENCE AND TREATMENT WITH VITAMINS ON THE EMERGENCE OF COFFEE SEEDLINGS
Provedor de dados: 196
Autores: Campos, Luiz Fernandes Cardoso; Vendruscolo, Eduardo Pradi; Nascimento, Lucas Marquezan; Campos, Camila Meira de Abreu; Pires, Larissa Leandro; Seleguini, Alexsander.
The seedling production of is a stage of great importance for several crops. The seeds of the coffee tree present germination difficulties due to the physical barrier imposed by the parchment. The objective of this study was to evaluate the effect of parchment presence and pre-sowing treatment with vitamins on the emergence of coffee seedlings. The experimental design was completely randomized, in a 2x4 factorial design (parchment presence x types of vitamins), in four replicates with 15 seeds per plot. Vitamins concentration was 100 mg l-1 of thiamine, 100 mg l-1 niacin, 50 mg l-1 thiamine + 50 mg l-1 niacin and a control treatment. The evaluations were performed weekly, with the emerged seedlings being counted until the 76th day after sowing. The...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/2769

CONSERVAÇÃO DE REPOLHO MINIMAMENTE PROCESSADO SOB EFEITO DE DIFERENTES EMBALAGENS, TEMPO DE ESTOCAGEM E TEMPERATURA
Provedor de dados: 196
Autores: Moreno, Leandro Bassi; scherwinski, Rainer; da Silva, João Manoel Teixeira; Scalon, Silvana de Paula Quintão; Carnevalli, Thiago Oliveira.
A utilização de atmosfera modificada e redução da temperatura de armazenamento aumentam a vida útil de diversas hortaliças e frutas minimamente processadas. O presente estudo consistiu em avaliar os efeitos de diferentes embalagens, temperaturas e tempo de estocagem (0, 4, 8 e 12 dias) nas propriedades físico-químicas de repolho minimamente processado. As amostras foram acondicionadas em bandeja pet, bandeja de isopor embaladas com filme PVC e em sacos plásticos sob diferentes temperaturas (8 °C, 15 °C e 25 °C), que foram arranjados em esquema fatorial 3 x 3, no delineamento experimental de blocos inteiramente casualizados, com três repetições. Após o processamento do repolho foram retiradas 150 g do material e acondicionado nas diferentes embalagens. De...
Tipo: Info:eu-repo/semantics/article
Ano: 2016
URL: http://periodicosonline.uems.br/index.php/agrineo/article/view/1139

Ocupação inicial e herança cultural do Vale Rural
Provedor de dados: 25
Autores: Ricci, Fabio.
A comunicação foi feita no seminário futuro do vale rural promovida pelo programa de pós graduação em Gestão e desenvolvimento regional, instituto de estudos valeparaibanos e Comitê das Bacias Hidrográficas do vale do Paraíba.
Tipo: Article
Palavras-chave: Vale do Paraíba: História.
Ano: 2007
URL: http://hdl.handle.net/2315/74

Hidrologia de encosta numa cabeceira de drenagem com cobertura de eucalipto na bacia do rio Sesmarias: médio vale do rio Paraíba do Sul
Provedor de dados: 25
Autores: Sato, Anderson Mululo; Avelar, André de Souza; Coelho Netto, Ana Luiza.
Since early 21 century the landscape mosaic of middle Paraíba do Sul river valley has been rapidly modified by spreading of Eucalyptus patches in substitution to cattle grazing grasslands. On the other hand, the region have evidences of geomorphological instability due to occurrence of deep gullies caused by groundwater flows and landslide scars. Our current research interests are driven to understand the role played by Eucalyptus controlling the hillslope hydrology and explain how these changes may affect the regional landscape system. This paper presents the hydrological results in the headwater zone of a first order drainage basin in response to biota-soil-water interactions.
Tipo: Article
Palavras-chave: Eucalyptus serrapilheira atravessamento; Cabeceira de drenagem escoamento superficial.
Ano: 2007
URL: http://hdl.handle.net/2315/93

Uso do território pelo circuito espacial produtivo de celulose em Eunápolis, sul da Bahia
Provedor de dados: 25
Autores: Joly, Carolina.
This study analyses the insertion of the spatial productive circuit of cellulose in Eunápolis, in the extreme south of Bahia state, with the installation of the Veracel Celulose enterprise. Result of a joint venture between Aracruz Celulose and Stora Enso, Veracel Celulose is one of the largest industrial plants of this world circuit. The research shows that land concentration increase, caused by the intensive land purchasing carried out by the company, and the large contingent of migrants attracted to Eunápolis, are not compensated by jobs offered and tributes paid by Veracel. So, this large cellulose venture brought little social and economic gains for people living in the region. As a conclusion, the regional development speech still do not consider the...
Tipo: Article
Palavras-chave: Celulose; Território brasileiro; Desenvolvimento regional; Eunápolis-BA; Veracel.
Ano: 2007
URL: http://hdl.handle.net/2315/109

Índice de área foliar de Eucalyptus grandis em resposta à adubação com potássio e sódio
Provedor de dados: 25
Autores: Almeida, Julio Cesar Raposo de; Laclau, Jean-Paul; Gonçalves, José Leonardo de Moraes; Moreira, Rildo Moreira e; Rojas, Juan Sinforiano Delgado.
Leaf Area Index (LAI, i.e. horizontal projection of leaf area per unit ground area) is highly correlated with water balance and net primary production in forest ecosystems. LAI is related with species, but it is also highly dependent on environmental conditions and management practices which influence the availability of water and nutrients. This work aimed at establishing allometric relationships in fast-growing Eucalyptus grandis plantations in Brazil (Itatinga – São Paulo) making it possible to predict the LAI under K and Na fertilization. Dendrometric inventories (Crown diameter – CD, Diameter at Breast Height - DBH and total height - H) were made at 5, 8, 11, 24 and 35 months after planting. The trees were divided into 8 crown index (CI) or basal area...
Tipo: Article
Ano: 2007
URL: http://hdl.handle.net/2315/82

Análise do tamanho e distância entre fragmentos florestais na bacia hidrográfica do Rio Una
Provedor de dados: 25
Autores: Catelani, Celso de Souza; Batista, Getulio Teixeira.
This article characterized the forest fragments of Una River hydrographic basin, affluent of the Paraíba do Sul River. Results showed that the average mean size of all fragments is 9.06 ha and that the correlation to the circular shape is 0.68 and the mean nucleus area of fragments considering a border effect of 60m is 5.86 ha. The mean distance among them is 245m. These parameters indicate that this basin has elongated fragments, with high border effect and may be in risk of biodiversity erosion. The image showing the different size classes of fragments allowed spatial observation of critical areas of the basin in ecological sustainability risk. The computing tools proved to be useful and easy to use as long as a previous georeferenced data basis is...
Tipo: Article
Palavras-chave: Remote sensing; Image processing; SIG processamento de imagens sensoriamento remoto GIS.
Ano: 2007
URL: http://hdl.handle.net/2315/84

Georreferenciamento do percurso de rafting no rio Paraibuna, no Parque Estadual Serra do Mar – Núcleo Santa Virgínia, SP
Provedor de dados: 25
Autores: Pereira, Ana Paula; Batista, Getulio Teixeira; Robim, Maria de Jesus.
Resumo: O presente trabalho visa subsidiar ações voltadas à implementação do rafting no Parque Estadual Serra do Mar – Núcleo Santa Virgínia. Teve-se como principal objetivo a caracterização do percurso do rafting no rio Paraibuna para auxiliar no manejo desta atividade dentro da Unidade de Conservação. Para atingir este objetivo foram utilizadas fotografias aéreas ortorretificadas e georreferenciadas, cartas IGC 1:10.000, assim como, o Sistema de Informação Geográfica – SIG, software SPRING, pois tais instrumentos auxiliam nas análises de informações ao permitir a integração de dados de diferentes fontes de forma georreferenciada. Os resultados podem ser veiculados na forma de mapas dinâmicos e interativos via Internet constituindo uma estratégia...
Tipo: Article
Palavras-chave: Rafting; Unidade de Conservação; Turismo Sustentável; Sistema de Informação Geográfica.
Ano: 2011
URL: http://hdl.handle.net/2315/166

Discutindo o futuro da sustentabilidade energética no Brasil
Provedor de dados: 25
Autores: Willian, J. Ferreira; Getulio, T. Batista.
Trabalho apresentado na Semana Nacional de Ciência e Tecnologia 2014 e na SIPAT-Meio Ambiente Avibras Indústria Aeroespacial 2014.
Tipo: Presentation
Palavras-chave: Energia; Desenvolvimento Sustentável; Economia; Ambiental.
Ano: 2014
URL: http://hdl.handle.net/2315/279

O ciclo hidrológico em plantações de Eucalipto
Provedor de dados: 25
Autores: Soares, João Vianei.
Ciclo hidrológico em Eucalipto Questões de primeira ordem  Qual é a relação entre oferta e demanda de água por plantações de Eucalipto? Qual é a estratégia de manutenção do funcionamento fisiológico durante períodos de seca? O Eucalipto seca o solo? Como se comparam os usos de água do eucalipto e da Mata Atlântica?
Tipo: Presentation
Palavras-chave: Ciclo Hidrológico; Controle ecofisiológico; Parametrização do solo; Balanço de água em Eucalipto.
Ano: 2007
URL: http://hdl.handle.net/2315/132

Avaliação da biota do solo na Serra dos Ferreiras no Povoado Mangabeiras
Provedor de dados: 25
Autores: Colaço, Alda Lara da Silva,; Santos, José Farias dos ,; Silva, Kelle Cristina Pereira,; Bezerra, Lílian Nunes,; Bezerra, Manuela Nunes,; Cavalcante, Viviane Aparecida dos Santos; Barros, Rubens Pessoa de,; Lopes, Esmeralda Aparecida Porto,.
O presente trabalho teve como objetivo caracterizar a distribuição da fauna do solo e avaliar o efeito do manejo do solo sobre a diversidade da fauna edáfica nos compartimentos solo e serrapilheira em duas diferentes coberturas vegetais (floresta não preservada e cultivo de mandioca) no Norte Arapiraquense.
Tipo: Article
Palavras-chave: Fauna do solo; Diversidade de espécies; Solos florestais; Solos em cultivo.
Ano: 2008
URL: http://hdl.handle.net/2315/140

ESTUDO PARA AVALIAR A QUALIDADE AGRONÔMICA DA TURFA
Provedor de dados: 25
Autores: Fortes Neto, Paulo Fortes Neto; Fortes, Nara Lúcia Perondi Fortes; Silva, Eliana Maria de Araújo Mariano Silva; Peixoto, Plinio Honorato Muella Peixoto.
Com o objetivo de avaliar a qualidade agronômica da turfa in natura e turfa processada como substratos na produção de rabanete, cultivar Early Scarlet Globe, realizou-se um experimento em casa de vegetação. Foi utilizado o delineamento experimental em blocos ao acaso, com quatro repetições. Os tratamentos foram constituídos por uma testemunha e seis proporções de turfa in natura e processada: T1 - Testemunha absoluta sem turfa; T2 0,5% de Turfa in natura ; T3 1,0% de Turfa in natura ; T4 - 1,5% de Turfa in natura ; T5 2,0% de Turfa in natura ; T6 - 0,5% de Turfa processada; T7 1,0% de Turfa processada; T8 1,5% de Turfa processada e T9 2,0% de Turfa processada. O cultivo foi feito em vasos (1,5L) de polietileno contendo em seu interior areia lavada e a...
Tipo: Technical Report
Palavras-chave: Turfa; Nutrientes.
Ano: 2012
URL: http://hdl.handle.net/2315/261

Reposição Florestal e Educação Ambiental na Bacia do Rio Una, Bacia do Paraíba do Sul, 40p.
Provedor de dados: 25
Autores: Cícero, Carlos Moure; Catelani, Celso de Souza; Batista, Getulio Teixeira.
Apresentação realizada pelo Prof. Dr. Getulio Teixeira Batista na Mesa 3 - O Plano de Bacia do Rio Paraíba do Sul e suas Implicações nas Atividades Rurais. Relatou-se o estudo de caso da Bacia do Rio Una, importante afluente do Rio Paraíba do Sul.
Tipo: Presentation
Palavras-chave: Essências Nativas; Áreas de Preservação.
Ano: 2006
URL: http://hdl.handle.net/2315/70

COLETA NA ESTIMATIVA DE EMISSÕES DE METANO POR RESERVATÓRIOS DE HIDRELÉTRICAS
Provedor de dados: 25
Autores: Bernardes Esteves Moreira, Luara; Ferreira, Willian José; Braz, Lia; Alvalá, Plínio Carlos; Teixeira Batista, Getulio.
Resumo apresentado no Encontro de Iniciação Científica, XIII Mostra de Pós-graduação - 16 a 20 de outubro de 2012, no Campus do Bom Conselho, Universidade de Taubaté - Taubaté – SP
Tipo: Other
Palavras-chave: GEE; Emissões de Metano.
Ano: 2012
URL: http://hdl.handle.net/2315/259

Prefácio
Provedor de dados: 25
Autores: Batista, Getulio Teixeira.
Apresentamos os anais do Primeiro Seminário de Recursos Hídricos da Bacia Hidrográfica do Paraíba do Sul (SERHIDRO-PS 2007). Esse evento marca o início de uma série de seminários a serem realizados a cada dois anos sempre focando uma questão atual e relevante para a Bacia Hidrográfica do Paraíba do Sul, sem, entretanto, deixar de trazer contribuições importantes para outras áreas temáticas relacionadas com o estudo dos recursos hídricos e de bacias hidrográficas. Esse primeiro seminário tem como principal tema a discussão sobre o eucalipto e o ciclo hidrológico, assim como, a cobrança pelo uso da água na Bacia. É um evento organizado em parceria entre a Universidade de Taubaté (UNITAU), o Instituto Nacional de Pesquisas Espaciais (INPE) e o Instituto de...
Tipo: Article
Palavras-chave: Serhidro; Recursos hidricos; Paraiba do Sul; Seminario.
Ano: 2007
URL: http://hdl.handle.net/2315/125

O uso futuro das áreas de mineração de areia no sub-trecho compreendido entre Jacareí e Pindamonhangaba, SP e sua inserção na dinâmica local e regional
Provedor de dados: 25
Autores: Marcondes Filho, Edarge; Batista, Getulio Teixeira; Targa, Marcelo dos Santos; Soares, Paulo Valadares.
This work was developed in the Paraíba River Valley between Jacareí and Pindamonhangaba municipalities. The objective was to analyze the different types of use of sand pits after the extraction of the mineral according to technical standards and economical viability. Based on the literature and consultations with environmental institutions and professionals that work in the area, several field observations campaigns were organized jointly by DEPRN, CETESB and the Environmental Police to characterize the profile of all mining companies. Different types of post-mining activities were found and the need to make the uses compatible with specific local characteristics was identified.
Tipo: Article
Palavras-chave: Mineração de areia; Cavas de areia; Uso futuro.
Ano: 2007
URL: http://hdl.handle.net/2315/92

Análisis espacio-temporal del paisaje en la microcuenca dos afonsos - municipio de redençao da serra - Sp
Provedor de dados: 25
Autores: Biffi, Pedro Victor Barreto; Rossin, Sergio; Valerio, Mario.
In this project "space-temporary Analysis of the landscape in the basin Dos Afonsos" was analyzed the patterns of change of use of the soils and the fragmentation of the wood, located in the basin Dos Afonsos, and inside the limits of the Redençao da Serra district that belongs to the Região do Vale do Paraíba-SP state. For it a was carried out an multitemporal analyzed on an area approximated of 6802,59 of hectares, using for that program SPRING, for the image of Landsat processing of the followings years 1984, 1994, 2005 and the images of CBERS of the 2005 years The analysis of detection of changes was made for the followings classes: Lake - Lagoon, Macrophytes, Wood, Grass, degraded Grass, implanted Grass, Burned, reforests and Bare soils. Concluding...
Tipo: Article
Palavras-chave: Remote sensing; Soils; Processamento de imagens; Sensoriamento remoto; The basin; Image processing.
Ano: 2007
URL: http://hdl.handle.net/2315/111

Estudo Hidrológico da Bacia do Rio Una, Afluente do Rio Paraíba do Sul: subsídios para estabelecimento de plano de macrodrenagem.
Provedor de dados: 25
Autores: Targa, Marcelo Santos; Batista, Getulio Teixeira; Dias, Nelson Wellausen; Silva, Paulo Augusto Romera.
Trata-se de um artigo referente aos resultados preliminares do trabalho de pesquisa da bolsa Pq do Dr. Marcelo Santos Targa
Tipo: Article
Palavras-chave: Drenagem; Ciências ambientais; Bacia hidrográfica; Planos.
Ano: 2012
URL: http://hdl.handle.net/2315/250

SITUAÇÃO DAS APP DAS MARGENS DO RIBEIRÃO DAS ANTAS NO ANO DE 2010
Provedor de dados: 25
Autores: Fantus Ribeiro, Thiago; Donizeti de Carvalho, Giovanni; Almeida Rodrigues, Pedro; Mendes de Moura, Yhasmin; Teixeira Batista, Getulio.
Resumo apresentado no Encontro de Iniciação Científica, XIII Mostra de Pós-graduação - 16 a 20 de outubro de 2012, no Campus do Bom Conselho, Universidade de Taubaté - Taubaté – SP
Tipo: Other
Palavras-chave: Áreas de preservação; Código Florestal.
Ano: 2012
URL: http://hdl.handle.net/2315/254

Análises físico-químicas e bacteriológicas das águas superficiais e subterrâneas da área da várzea do rio Paraíba do Sul sujeita à extração de areia, no município de Tremembé, SP
Provedor de dados: 25
Autores: Diniz, Helio; Galina, Marcia; Lindeberg, Mariuza; Batista, Getulio; Targa, Marcelo.
Apresentado no XIX Simpósio Brasileiro de Recursos Hídricos, Maceió, 2011.
Tipo: Article
Palavras-chave: Mineração; Cavas; Análises físico-químicas; Análise bacteriológica.
Ano: 2012
URL: http://hdl.handle.net/2315/239

Sensoriamento Remoto para a Caracterização do Aporte de Sedimentos e Compostos Orgânicos da Represa de Paraibuna, São Paulo.
Provedor de dados: 25
Autores: Dias, Nelson Wellausen; Batista, Getulio; Targa, Marcelo dos Santos; Novo, Evlyn Marcia Leão Moraes; Barbosa, Claudio Clemente.
As águas do rio Paraíba do Sul apresentam um alto nível de degradação ambiental em função do despejo direto de efluentes domésticos sem tratamento e de contaminações de origem difusa (sedimentos, nutrientes e matéria orgânica) provenientes do carreamento de solo erodido, fertilizantes, pesticidas, herbicidas e dejetos de animais para os canais de drenagem. Comparativamente, a água do reservatório de Paraibuna possui qualidade de água significativamente superior aos demais trechos do Rio Paraíba do Sul devido ao fato de estar a montante dos principais centros urbanos do Vale do Paraíba. Entretanto as águas que abastecem esta represa são provenientes de duas bacias (Paraibuna e Paraitinga) com características de cobertura e uso do solo bastante distintas que...
Tipo: Article
Palavras-chave: Represas; Sedimentação; Sensoriamento remoto hiperespectral; Hyperspectral remote sensing; Reservoirs; Sedimentation.
Ano: 2006
URL: http://hdl.handle.net/2315/41

Descobrindo os Aspectos Geográficos de Guaratinguetá
Provedor de dados: 25
Autores: Siqueira, Meire Regina de Almeida; Campos, Maria Regina Nunes de; Urban, Márcia Virgínia Mendes.
Este trabalho foi desenvolvido na EE Professor José Pereira Éboli, com o objetivo de desenvolver o conhecimento e análise dos aspectos naturais e culturais da cidade, a partir de uma visão histórica.  Através de atividades de campo levamos os alunos para observar as diversas paisagens que formam Guaratinguetá. As visitas a Serra do Mar e da Mantiqueira tiveram como objetivos conhecer particularidades geológicas, climáticas e botânicas e diagnosticar os impactos causados ao meio ambiente pela ocupação humana desordenada, percebendo os rastros de destruição deixados pela intervenção humana. Em oficinas de criação de textos e de artes plásticas, os alunos expressaram suas impressões do que foi apreendido. O material produzido pelos alunos foi organizado em um...
Tipo: Book
Palavras-chave: Educação Ambeintal; Interdisciplinalidade; Guaratinguetá e Geografia; Arte e Educação Ambeintal.
Ano: 2007
URL: http://hdl.handle.net/2315/72

Tratamento de efluentes domésticos por leito cultivado
Provedor de dados: 25
Autores: Fortes Neto, Paulo.
O efluente doméstico por ser resíduo altamente poluidor, promove sérios impactos ambientais quando disposto diretamente sem tratamento em cursos d'água.
Tipo: Presentation
Palavras-chave: Reuso da água; Tratamento de efluentes; Fossa séptica.
Ano: 2007
URL: http://hdl.handle.net/2315/131

Mapeamento do conflito de uso em áreas de preservação permanente na microbacia Santa Cruz, município de Porto Nacional – Tocantins – Brasil
Provedor de dados: 25
Autores: Barros, Emmanuel Kirlian Evangelista; Martins, Alan Kardec Elias; Bonatto, Frederico; Faria, Viviane Machado Lettry de.
The present work had as objective to use techniques of systems of geographic information and remote sensing to mapear the use and covering of the land in the basin Santa Cruz located in the city of Porto Nacional-TO, qualitying and quantitying the level of degradation in areas of permanent preservation of the edges of the water courses having for base the limits established for the forest code and the Resolution nº 303 of the CONAMA. The results had pointed efficiency of the used tools and although the existence of conflicts of use in areas of permanent preservation the basin discovers conserved well.
Tipo: Article
Palavras-chave: Remote sensing; Bacia; SIG; Sensoriamento remoto; GIS; Basin.
Ano: 2007
URL: http://hdl.handle.net/2315/94

Uso de SIG (Sistema de Informações Geográficas) para diagnóstico das áreas de preservação permanente (APP)
Provedor de dados: 25
Autores: Paula, Geberson; Batista, Getulio; Targa, Marcelo.
Apresentado no Simpósio Brasileiro de Geografia F/isica Aplicada em Dourados / MS em julho de 2011.
Tipo: Article
Palavras-chave: SIG; Fazenda Una.
Ano: 2012
URL: http://hdl.handle.net/2315/236

A importância da publicação de pesquisas brasileiras sobre as questões ambientais em periódicos nacionais: contribuições da revista Ambiente &amp; Água
Provedor de dados: 25
Autores: Malafaia, Guilherme; Rodrigues, Aline Sueli de Lima.
Apresenta-se neste manuscrito uma breve discussão a respeito do crescimento da revista Ambiente &amp; Água e da sua importância no âmbito da divulgação de artigos desenvolvidos no Brasil. Além disso, discorre-se sobre a necessidade da quebra dos preconceitos que ainda existem em torno da publicação de artigos em periódicos brasileiros.
Tipo: Article
Palavras-chave: Periódicos brasileiros; Divulgação científica; Ambi-Agua; Artigos; Ciências ambientais; Recursos hídricos.
Ano: 2010
URL: http://hdl.handle.net/2315/152

Sustentabilidade e Desenvolvimento
Provedor de dados: 25
Autores: Batista, Getulio T.
Palestra apresentado no XVI Encontro de IniciaÃ§Ã£o CientÃ­fica, XII Mostra de PÃ³s-graduaÃ§Ã£o da Universidade de TaubatÃ© focando a questÃ£o do desenvolvimento sustentÃ¡vel com discussÃ£o de um novo paradigma de desenvolvimento baseado em premissas ecolÃ³gicas.
Tipo: Presentation
Palavras-chave: Analise Ambiental; Pegada Ecologica.
Ano: 2011
URL: http://hdl.handle.net/2315/179

O FUTURO DO BIODIESEL COMO COMBUSTÍVEL SUSTENTÁVEL NO BRASIL
Provedor de dados: 25
Autores: Gabriel, Marinho; Lia, Braz; Getulio, T. Batista; Marcelo, dos S. Targa; Willian, J. Ferreira.
O biodiesel tem sido considerado como o mais promissor dos produtos na busca por combustíveis alternativos para o segmento de transportes, de cargas e passageiros. O setor espera que em 2014 seja comercializado um volume pelo menos 16% maior do que em 2013, taxa projetada pelo aumento da mistura de biodiesel no diesel fóssil, de 6% (B6) para 7% (B7) em volume, já aprovado pelo governo. A fim de alinhar fatores econômicos com benefícios socioambientais aonde vem sendo produzido, faz-se necessário que a produção seja sustentável, proveniente de novos cultivares de oleaginosas. Neste trabalho procurou-se investigar o futuro do biodiesel no país, observando dados divulgados pela Agência Nacional do Petróleo, Gás Natural e Biocombustíveis (ANP) e barreiras para...
Tipo: Presentation
Palavras-chave: Bioenergia; Transporte; Diesel; Combustíveis.
Ano: 2014
URL: http://hdl.handle.net/2315/281

Emissão e Seqüestro de Carbono
Provedor de dados: 25
Autores: Batista, Getulio Teixeira.
Essa apresentação em formato pdf foi utilizada em uma palestra para o programa de pòs-Graduação em Ciências Ambientais da Universidade de Taubaté. Vários slides são apresentados para ilustrar os forçantes da geração dos gases de efeito estufa e para ilustrar o mercado de carbono dentro do contexto do protocolo de Kyoto.
Tipo: Presentation
Palavras-chave: Biomass; Biomassa; Gases de efeito estufa; Mudanças Climáticas; Mudanças globais; Mercado de carbono.
Ano: 2006
URL: http://hdl.handle.net/2315/50

Monitoramento hidroclimático e hidrogeológico na área de várzea do município de Tremembé (SP) no período de fev/2010 a mar/2011
Provedor de dados: 25
Autores: Diniz, Helio; Galina, Marcia; Batista, Getulio; Targa, Marcelo.
Apresentado no XIX Simpósio Brasileiro de Recursos Hídricos, Maceió, 2011.
Tipo: Article
Palavras-chave: Várzea do rio Paraíba do Sul.
Ano: 2012
URL: http://hdl.handle.net/2315/237

PLANO DIRETOR DE MACRODRENAGEM: Aplicação ao caso da bacia hidrográfica do Rio Una, Vale do Paraíba do Sul,SP
Provedor de dados: 25
Autores: Targa, Marcelo Santos; Dias, Nelson Wellausen; Batista, Getulio Teixeira; Cicero, Carlos Moure; Simões, Silvio Jorge Coelho; Diniz, Helio Nóbile; Santoro, Jair; Silva, Paulo Augusto Romera; Reis, Benedito Jorge.
O presente trabalho tem como objetivo propor uma metodologia de estudo da macrodrenagem para a bacia do rio Una na região do Vale do Paraíba do Sul, SP com vistas a minimizar os problemas de cheias e inundações freqüentes de forma a auxiliar ao poder público municipal a criação de leis específicas que regulamente o uso e ocupação da bacia do rio Una no futuro, contribuindo para a efetivação do Plano Diretor Municipal de Taubaté. Preconiza-se nessa metodologia a realização de atividades em campo para determinação de vazões e nível de sedimentos, determinação de características de infiltração dos solos, determinação das propriedades físicas dos solos, coleta de dados em postos meteorológicos, caracterização morfométrica das bacias e atividades relativas ao...
Tipo: Article
Palavras-chave: Bacia hidrográfica; Macrodrenagem.
Ano: 2009
URL: http://hdl.handle.net/2315/150

RELAÇÃO ESPACIAL DO MERCÚRIO E ELEMENTOS TRAÇOS EM SEDIMENTO DE FUNDO NO ALTO RIO MADEIRA
Provedor de dados: 25
Autores: Galvão, Roberta Carolina Ferreira; Bernardi, José Vicente Elias; Almeida, Ronaldo; Bastos, Wanderley Rodrigues; Gomes, João Paulo de Oliveira.
The presence of mercury in several compartments of the aquatic ecosystems represents a problem of great concern in the Amazonian basin. The goal of this work is to correlate the amount mercury found in bottom sediment with other trace elements as well as its spatial distribution in the upper Madeira River. Field samples were acquired on February of 2004. Total mercury quantitative determination was carried out through atomic absorption spectrophotometer analysis with cold vapor generation in flow injection system. Trace elements data analysis was implemented using multiple regression and spatial distribution analysis was developed using indicative kriging geostatistic technique. Multiple regression analysis showed that Hg has a strong dependence with Co,...
Tipo: Article
Palavras-chave: Mercúrio; Krigagem; Regressão múltipla; Sedimento de fundo; Rio Madeira.
Ano: 2007
URL: http://hdl.handle.net/2315/81

Interpretação de testes de vazão em poços tubulares profundos, dimensionamento e especificações de bombas submersas
Provedor de dados: 25
Autores: Diniz, Hélio Nóbile; Michaluate, Walter Jorge.
Este trabalho tem o objetivo de divulgar técnicas sobre a realização e interpretação de testes de vazão em poços tubulares profundos. O teste de vazão é uma ferramenta usada para conhecer o comportamento hidráulico dos poços tubulares profundos e sua interpretação adequada possibilita o cálculo preciso do equipamento para extração de água dos poços e a determinação dos parâmetros hidrodinâmicos dos aqüíferos. Os conceitos apresentados neste manual são produtos de uma ampla consulta e revisão bibliográfica realizada pelos autores, nas bibliotecas do Instituto Geológico da Secretaria do Meio Ambiente do Estado de São Paulo, Instituto Astronômico e Geofísico, Instituto de Geociências e Faculdade de Engenharia Civil da Escola Politécnica da Universidade de São...
Tipo: Learning Object
Palavras-chave: Água subterrânea; Ensaios de bombeamento; Extração de água.
Ano: 2006
URL: http://hdl.handle.net/2315/64

Metodologia para Avaliação dos Processos Hidrológicos e da Sedimentação na Bacia Hidrográfica Experimental do Ribeirão Itaim, Município de Taubaté, no Vale do Rio Paraíba do Sul - Estado de São Paulo
Provedor de dados: 25
Autores: Targa, Marcelo dos Santos; Batista, Getulio Teixeira; Cícero, Carlos Moure; Dias, Nelson Dias.
Esse artigo descreve uma metodologia para o estudo de processos hidrológico e sedimentológicos de uma microbacia (Itaim), envolvendo medição de parâmetros físico-hídricos (precipitação, infiltração, escoamento superficial, carga de sedimentos e potencial de água no solo). Involve também a caracterização do balanço hídrico para a bacia experimental e a comparação dos dados de vazão obtidos em campo com valores de vazão calculados pelo método Curva Número (SCS-USDA) para cada compartimento da bacia e na bacia como um todo, síntese e relatório final.
Tipo: Article
Palavras-chave: Recursos hídricos; Sedimentação; Infiltração de água; Escoamento superficial.
Ano: 2006
URL: http://hdl.handle.net/2315/54

Educação Ambiental voltada para Recursos Hídricos: Um Estudo de Caso
Provedor de dados: 25
Autores: Batista, Getulio Teixeira; Fortes Neto, Paulo; Dias, Nelson Wellausen; Targa, Marcelo dos Santos; Oliveira, Luciana A. M.
Resumo. Em resposta ao "Edital CT-HIDRO/MCT/CNPq - Nº 15/2005 - Popularização da Ciência: Olhando para a Água", foi selecionada uma bacia hidrográfica, a bacia do Ribeirão das Almas - Caieiras, que contempla a comunidade organizada através da Associação Amigos do Bairro do Ribeirão das Almas - Caieiras e abriga a Escola Municipal de Ensino Infantil e Fundamental "Mário Lemos de Oliveira" do sistema de educação municipal de Taubaté, SP. Essa escolha se deveu ao fato do Departamento de Ciências Agrárias da Universidade de Taubaté (UNITAU) estar desenvolvendo vários projetos para o Comitê das Bacias Hidrográficas do Paraíba do Sul (CBH-PS) para a Bacia do Rio Una, da qual a microbacia selecionada para a presente proposta é parte. Outros fatores importantes...
Tipo: Other
Palavras-chave: Tratamento de efluentes; Bacias hidrográficas; Repovoamento florestal; Recursos  hídricos; Popularização da ciência; Balanço hídrico.
Ano: 2006
URL: http://hdl.handle.net/2315/61

Análise preliminar do contaminante Geogênico Ferro no aquífero freático do grupo Tremembé, subbacia do Itaim, na área do campus de Ciências Agrárias.
Provedor de dados: 25
Autores: LIMA, Flavio Jorge; DINIZ, Hélio Nóbile; TARGA, Marcelo dos Santos.
O trabalho em questão está relacionado com o tema da dissertação de mestrado em ciências ambientais, do departamento de Agrociências da UNITAU. Consiste numa análise inicial e exploratória, incentivada pelo aparecimento em alta concentração dos elementos ferro, bário, chumbo, manganês e cromo, detectados através de análises físico-químico da água do aquífero freático, em piezômetros localizados no campus de ciências agrárias.
Tipo: Article
Palavras-chave: Aquífero Freático; Contaminantes; Geogênico.
Ano: 2011
URL: http://hdl.handle.net/2315/184

VAZÃO DE PROJETO EM BACIAS HIDROGRÁFICAS RURAIS COM ÁREAS EM DECLIVE
Provedor de dados: 25
Autores: Targa, Marcelo Santos.
A determinação de vazões de projeto em bacias hidrográficas rurais com áreas em declive torna-se difícil pela pequena disponibilidade de dados de vazão, provenientes de monitoramentos e medições, para a maioria das bacias. Dessa forma a obtenção dessas vazões são, freqüentemente, baseadas em dados de chuvas. No presente trabalho procurou-se demonstrar a aplicação da fórmula Racional e da Curva Número, para determinação da vazão máxima de projeto em bacias hidrográficas essencialmente rurais. Essas metodologias foram desenvolvidas para as condições dos estados Unidos da América e embora, sejam consideradas consagradas por apresentarem resultados bastante satisfatórios, sua aplicação no Brasil deve ser feita com bastante critério.
Tipo: Article
Palavras-chave: Hidrógrafas; Bacias hidrográficas; Vazões.
Ano: 2011
URL: http://hdl.handle.net/2315/169

A dinâmica da água em microbacias hidrográficas reflorestadas com eucalipto
Provedor de dados: 25
Autores: Oleriano, Eliseu dos Santos; Dias, Herly Carlos Teixeira.
The importance of the water in the current geo-political context turns it into a research theme that focuses on conserving its quality and improving its use conditions in certain systems. The hidrologic cycle consists of water exchanges among rivers, lakes, and oceans, as well as atmosphere and soil. The species of the gender eucalyptus possess a very fast growth rate in relation to native species, what causes a large demand for water, even though their water use efficiency is better. As well as any vegetable species, the eucalyptus uses water to satisfy their physiologic demands, promoting its growth. As a result eucalyptus promotes reduction in the flow of water in watercourses. Areas covered with forest plantations, besides improving the landscape as a...
Tipo: Article
Palavras-chave: Hidrologic cycle; Microbacia; Eucalipto; Florestas plantadas; Ciclo hidrológico; Small watershed; Eucalyptus; Forest plantation.
Ano: 2007
URL: http://hdl.handle.net/2315/102

MONITORAMENTO DA CULTURA DE CAFÉ NA REGIÃO DE SÃO SEBASTIÃO DO PARAÍSO – MG, COM BASE NA ANÁLISE DE SÉRIES TEMPORAIS MODIS
Provedor de dados: 25
Autores: Luciano, Almeida Pinto; Melchiades, Cardeal da Costa; Paulo Henrique, Lima Magalhães; Getulio, Teixeira Batista; Yhasmin, Mendes de Moura.
Resumo apresentado no Encontro de Iniciação Científica, XIII Mostra de Pós-graduação - 16 a 20 de outubro de 2012, no Campus do Bom Conselho, Universidade de Taubaté - Taubaté – SP
Tipo: Other
Palavras-chave: Café; Sensoriamento Remoto; Landsat; Imagens de satélite.
Ano: 2012
URL: http://hdl.handle.net/2315/252

Incidência de Varroa destructor (Anderson &amp; Trueman) em Criação de Abelhas com Ferrão na Região de Sinop, Mato Grosso, Brasil
Provedor de dados: 25
Autores: Torres, Rodrigo de Nazaré Santos; Barreto, Marliton Rocha.
Resumo. Quanto às enfermidades apícolas descreve-se que o Brasil está em situação vantajosa comparando com outros países, por apresentar enxames rústicos que, por serem mais resistentes a doenças, dispensam a utilização de antibióticos. Entretanto, a dinâmica de populações do ácaro Varroa mostrou ser muito diferente das outras regiões afetadas pela varroose sendo os primeiros índices registrados superiores a 20% e, ainda, se têm poucos trabalhos em relação à taxa de infestação em diferentes regiões do Brasil. Desta forma, este trabalho teve como objetivo realizar um levantamento de incidência do ácaro Varroa destructor (Anderson &amp; Trueman) em colmeias na região de Sinop, MT. As coletas foram realizadas nos meses de julho e agosto de 2011 em oito...
Tipo: Article
Palavras-chave: Ácaro; Apis; Infestação; Infestation; Mite.
Ano: 2013
URL: http://hdl.handle.net/2315/269

A água no contexto da Zona de Amortecimento
Provedor de dados: 25
Autores: Santos, Henrique Cardoso dos.
The water resources in the Buffer Zone of a Conservation Unit of the Atlantic Rain Forest is important to the quality of life of the community that leaves in the border zone of this unit. The planning of occupation of the Buffer Zone must consider not only all elements of ecological interest of the Conservation Unit, but also it must necessarily focus on measures to preserve and restore the vegetation cover of humid areas for the maintenance of the balance between natural environment sustainability and human use.
Tipo: Article
Palavras-chave: Mata Atlântica; Zona de Amortecimento; Zona de Amortecimento.
Ano: 2007
URL: http://hdl.handle.net/2315/103

Fundo de recursos hídricos aplicado à caracterização do uso e cobertura do solo e análise da qualidade da água como base para apoio às decisões do Comitê das Bacias Hidrográficas do Rio Paraíba do Sul, SP
Provedor de dados: 25
Autores: Targa, Marcelo; Dias, Nelson; Batista, Getulio.
Apresentado no XIX Simpósio Brasileiro de Recursos Hídricos, Maceió, 2011.
Tipo: Article
Palavras-chave: Banco de dados geoespaciais ambie; Avaliação de recursos hídricos; Qualidade da água.
Ano: 2012
URL: http://hdl.handle.net/2315/238

TAXONOMIA E IDENTIFICAÃ‡ÃƒO DE  Fusarium spp
Provedor de dados: 25
Autores: Fortes, Nara Lucia Perondi.
Universidade de Taubaté (UNITAU)
Tipo: Article
Palavras-chave: Fusarium spp.
Ano: 2006
URL: http://hdl.handle.net/2315/68

Modelagem Ambiemtal e a sustentabilidade
Provedor de dados: 25
Autores: Silva, Paulo Augusto Romera e; Valente, Ancelmo Arantes; Leite, Marli Aparecida Reis Maciel.
O mundo atual está mais e mais atento às exigências de controle ambiental, com o envolvimento dos atores nos estágios importantes do processo. O presente trabalho apresenta para discussão uma proposta de modelagem de sistema ambiental baseada nesse contexto dinâmico da nossa sociedade atual, concebido para aplicação na gestão colegiada de áreas de recuperação e proteção de mananciais de abastecimento, como alternativa para o acompanhamento permanente do seu estado e modificações, com a possibilidade de realização de simulações no processo de tomadas de decisão, frente à complexidade dos sistemas envolvidos. Diante disso, a concepção da presente proposta é a da identificação dos componentes representativos do sistema, para a aferição e simulação de...
Tipo: Article
Palavras-chave: Otimização de uso; Sustentabilidade; Modelagem ambiental; Estratégias para gestão.
Ano: 2007
URL: http://hdl.handle.net/2315/115

Minicurso: Área de Preservação Permanente (APP)
Provedor de dados: 25
Autores: Oliveira, Ivan Silva de; Batista, Getulio Teixeira; Catelani, Celso de Souza.
Slides e Anexo descrevendo a metodologia para caracterização de APPs.
Tipo: Presentation
Palavras-chave: Área de Preservação Permanente; Legislação Ambiental; Código Florestal; Resolução CONAMA 303/2002.
Ano: 2006
URL: http://hdl.handle.net/2315/66

The ectoparasite mite Varroa destructor Anderson and Trueman in southeastern Brazil apiaries: effects of the hygienic behavior of Africanized honey bees on infestation rates
Provedor de dados: 25
Autores: Pinto, Fábio de Assis.
No Brasil, o ácaro ectoparasita de abelhas Varroa destructor Anderson e Trueman (Acari: Varroidae) se mantém em índices de infestação baixos, não causando grandes prejuízos. Todavia com a introdução e possível predominância de um novo haplótipo (K) do ácaro, geralmente encontrado em regiões com altas taxas de infestação (TI), faz-se necessário o monitoramento e seleção de colônias resistentes à praga, evitando problemas futuros. Vários fatores são relacionados como possíveis responsáveis pela dinâmica de infestação do ácaro, dentre os quais se destaca o comportamento higiênico (CH). Nesse contexto buscamos avaliar o CH de abelhas africanizadas Apis mellifera L. (Hymenoptera: Apidae) correlacionando com as TI do ácaro em apiários de dois municípios do...
Tipo: Article
Palavras-chave: Acari; Varroidae; Pest management; Apidae; Bee pathology.
Ano: 2012
URL: http://hdl.handle.net/2315/270

Áreas para captação de água de chuva
Provedor de dados: 25
Autores: André Luiz Rezende, Ferreira; Getulio Teixeira, Batista; Paulo, Fortes Neto.
Este artigo constitui-se da revisão de artigos científicos, livro e revista com o intuito de fazer uma análise das áreas de captação da água de chuva. Inicialmente foi feito um estudo das reservas de água no planeta,  simbolismo nas religiões, consumo humano, uso sustentável, demanda, uso irracional e problemas da escassez. Em seguida, foi abordado o uso do telhado convencional com melhor inclinação e escoamento, tipos de cobertura com melhor coeficiente de escoamento (argamassa de cimento e areia, telha de cerâmica, telha de fibrocimento, lona plástica de polietileno), telhado verde (retenção, escoamento, qualidade da água) e chão (contra-piso, estradas, encostas) como áreas de captação.
Tipo: Article
Palavras-chave: Água de chuva; Escoamento; Captação; Catchment; Flow; Rainwater.
Ano: 2011
URL: http://hdl.handle.net/2315/173

Realidade e futuro do pinhão manso (Jatropha curcas L.) na produção sustentável de biodiesel no Vale do Paraíba/SP
Provedor de dados: 25
Autores: Ferreira, Willian J.; Batista, Getulio T.
A utilização mais eficiente de energia e a transição de fontes fósseis para alternativas energéticas renováveis têm sido propostas desafiadoras para o mundo atual. Cresce o número de pesquisas no setor dos biocombustíveis e existem motivações para a produção e uso do biodiesel. No Vale do Paraíba/SP, o pinhão manso tem despertado o interesse dos produtores rurais e seu plantio em áreas degradadas favorecerá o melhoramento das propriedades do solo e das condições ambientais. Ao criar cenários de otimismo à  cadeia produtiva do biodiesel a espécie se torna um importante elemento de sustentabilidade, fomentando o desenvolvimento da região.
Tipo: Presentation
Palavras-chave: Jatropha; Energia alternativa; Biodiesel; Mudanças climáticas.
Ano: 2010
URL: http://hdl.handle.net/2315/157

IDENTIFICAÇÃO E TRANSFORMAÇÃO DAS UNIDADES DA PAISAGEM NO MUNICÍPIO DE SÃO JOSÉ DOS CAMPOS (SP) DE 1500 A 2000
Provedor de dados: 25
Autores: Morelli, Ademir Fernando; Cavalheiro, Felisberto  (Orientador).
MORELLI, A.F. Identificação e Transformação das Unidades da Paisagem no Município de São José Dos Campos (SP) de 1500 a 2000. Rio Claro, 2002. 404 p. Tese (Doutorado em Geociências e Meio Ambiente) – Instituto de Geociências e Ciências Exatas de Rio Claro. 2002. Universidade Estadual Paulista “Júlio de Mesquita Filho”.
Tipo: Thesis
Palavras-chave: Ecologia da paisagem; Unidades da paisagem; História da paisagem; Planejamento da paisagem; Sensoriamento remoto; Geoprocessamento; Transformação da paisagem; São José dos Campos.
Ano: 2006
URL: http://hdl.handle.net/2315/67

Desempenho de girassol cultivado no período de safrinha  em Taubaté-SP
Provedor de dados: 25
Autores: Almeida, Julio Cesar Raposo; Alvarenga, Brummer Seda; Almeida, Ana Aparecida Silva; Targa, Marcelo dos Santos.
The sunflower (Helianthus annus L.) represents an important alternative crop for rotation programs, because sunflower can be cultivated at different times of the year. The objective of this work was to select sunflower cultivars adapted to production in Taubaté-SP. Experimental data from 2000 to 2001 evaluated the performance of four cultivars: Cargill 11, CATISSOL, RUMBOSSOL-90 e MORGAN 734 in a randomized complete blocks design, with five blocks and plots consisting of six lines of 5.0 m each, distanciated 0.80 m; the distance between plants inside the row was 0,25 m. The cultivars RUMBOSSOL-90 and MORGAN 734 were the most productive for cultivation in Taubaté-SP off-season
Tipo: Article
Palavras-chave: Helianthus annuus L.; Oleaginosas; Balanço hídrico; Cultivares girassol.
Ano: 2011
URL: http://hdl.handle.net/2315/183

Reflorestamento ciliar com espécies nativas ao reservatório de Furnas
Provedor de dados: 25
Autores: Togoro, Aluísio Hideki; Silva, Juliana Aparecida dos Santos da; Campos, José Carlos de; Landgraf, Paulo Roberto Correa; Cunha Neto, Francisco Rodrigues da.
The native forests in the south of Minas Gerais represent 6% of paisage approximately, composed for forest fragments, in its great majority with inferior area ha 50 ha. This resulted of intense the forest devastation in this region, during centuries XIX and XX, mainly had the expansion of the farming sector. Currently it has intense rew in such a way in the authorities of the ambient sector, as also of the society, in the direction that if makes the ambient recovery, mainly with regard to resetting of ciliar bushes and protection of springs. With this objective the ciliar reforestation to the reservoir of Furnas in the city of Privets in 2002 was effected, totalizing 2,6 ha as area model with educative and experimental purpose, in the space of 3X2 meters...
Tipo: Article
Palavras-chave: Ciliar reforestation; Native forests; Protection of springs.
Ano: 2007
URL: http://hdl.handle.net/2315/99

UTILIZAÇÃO DE GEOTECNOLOGIAS PARA ANÁLISE DO USO DO SOLO E ESTIMATIVA DO ESCOAMENTO SUPERFICIAL DA BACIA HIDROGRÁFICA DO MACHADO, TREMEMBÉ, SP
Provedor de dados: 25
Autores: Lacerda Silveira de Melo, Walkiria; Teixeira Batista, Getulio; Marcelo, Santos Targa.
Resumo apresentado no Encontro de Iniciação Científica, XIII Mostra de Pós-graduação - 16 a 20 de outubro de 2012, no Campus do Bom Conselho, Universidade de Taubaté - Taubaté – SP
Tipo: Other
Palavras-chave: Uso da terra; Imagens de satélite.
Ano: 2012
URL: http://hdl.handle.net/2315/256

ANÁLISE DAS CONDIÇÕES DAS ESTRADAS LIGADAS AO PLANTIO FLORESTAL NOS MUNICÍPIOS DE CUNHA E GUARATINGUETÁ, SP
Provedor de dados: 25
Autores: Brandão, Roberto; Batista, Getulio; Catelani, Celso.
A crescente atividade do setor florestal voltado à produção de papel e celulose no vale do Paraíba no Estado de São Paulo tem despertado indagações sobre os potenciais impactos que essa atividade pode causar ao meio ambiente. Dentre outros pontos a serem avaliados, as estradas rurais que dão acesso aos maciços florestais de eucalipto têm ligação direta com a qualidade dos recursos hídricos existentes nas bacias onde são implantados os talhões de eucalipto, principalmente no que se refere à erosão e ao transporte de material erodido para os cursos d’água. Nesse contexto, o presente trabalho teve como objetivo analisar as condições das estradas utilizadas nos plantios de eucalipto nos municípios de Cunha e Guaratinguetá, SP. Para isso foram analisados os...
Tipo: Article
Palavras-chave: Erosão; Erosion; Estradas florestais; Eucaliptus.
Ano: 2006
URL: http://hdl.handle.net/2315/47

Rede de plataformas de coleta de dados para monitoramento automático da qualidade da água do rio Paraíba do Sul
Provedor de dados: 25
Autores: Magina, Flávio de Carvalho; Reis, Benedito Jorge dos; Alves, Mário Luiz; Santos, Reinaldo José Tavares de Paula.
This work describes the implementation of an automated water quality monitoring network designed for operation at the Paraíba do Sul river, Brazil. Equipments, sensors and telecommunications systems, engineering solutions, site selection factors for the water-quality stations and the minimal requirements for operation were analyzed and specified. A set of preliminary data collection graphics are presented as example to demonstrate the application.
Tipo: Article
Palavras-chave: Data collection platforms; Qualidade da água; PCD; Plataformas de coleta de dados; Multiparameter sondes; Water quality monitoring.
Ano: 2007
URL: http://hdl.handle.net/2315/107

Gestão para o controle de efluentes líquidos provenientes de indústria siderúrgica do estado do Rio de Janeiro, Brasil
Provedor de dados: 25
Autores: Pereira, Wilma de Carvalho; Silva, Dalton Marcondes; Carvalho, Juremi de Oliveira; Sobrinho, Nelson Moura Brasil do Amaral; Boas, Roberto Cerrini Villas.
The purpose of this work is to study the potentially contaminating trace elements present in industrial waste that is discharged into the environment. The aim was to assess the parameters needed for it to be used in controlling the mobility of the potentially contaminating trace elements present in the residues. In this way were studied a refuse slag from Cia Siderúrgica Nacional – CSN). Even though this waste is considered relatively stable within the established standards set by current legislation due to its characteristics (Cd&lt;0.5 mg/Kg, Pb&lt;10 mg/Kg, Co&lt;5 mg/Kg, Cu=61 mg/Kg, Cr=280 mg/Kg, Ni&lt;1.5 mg/Kg, Zn=75 mg/Kg), there is so far no feasible alternative for its total reutilization. Bench-scale tests were performed whereby an acidified...
Tipo: Article
Palavras-chave: Gestão ambiental; Resíduos industriais; Disposição; Argila.
Ano: 2007
URL: http://hdl.handle.net/2315/87

O USO DO SPRING NO CÁLCULO DO ÍNDICE DE ÁREA VERDE EM BAIRRO PERIFÉRICO DA CIDADE DE TAUBATÉ, SP
Provedor de dados: 25
Autores: Santos, Claudia Helena Vitor dos; Batista, Getulio Teixeira.
RESUMO: A vegetação arbórea é de suma importância para o equilíbrio de um ecossistema quando se considera os aspectos ambientais, econômicos e sociais. O presente trabalho teve como objetivo avaliar quantitativamente as espécies arbóreas existentes no bairro Marlene Miranda, Taubaté, SP e simular o plantio de árvores utilizando técnicas de Sensoriamento Remoto, visando subsidiar ações que aumentem o índice de área verde do bairro para uma melhor qualidade de vida da comunidade residente. Para a quantificação das árvores nas áreas do bairro foi utilizada uma imagem do Google Earth de 2008, registrada em um banco de dados georreferenciado do aplicativo SPRING, versão 4.3.3, além de observações em campo. A área possui 47.5 ha, antes da simulação do plantio de...
Tipo: Article
Palavras-chave: Arborização; Índice de área verde; SIG; Geoprocessamento.
Ano: 2011
URL: http://hdl.handle.net/2315/167

O desenvolvimento proporcionado pelo uso de  energias renováveis: conhecer para planejar.
Provedor de dados: 25
Autores: Ferreira, Willian J.; Batista, Getulio T.
Palestra apresentada aos estudantes que participaram da Câmara Jovem de Jacareí em 2010.
Tipo: Presentation
Palavras-chave: Energias renováveis; Meio ambiente; Desenvolvimento.
Ano: 2011
URL: http://hdl.handle.net/2315/161

Análise de dados de Estações Meteorológicas de Superficie Automatica e Convencional
Provedor de dados: 25
Autores: Paula, Geberson Ricardo; Fisch, Gilberto.
Conhecer a atmosfera do planeta Terra é uma das aspirações que vêm sendo perseguidas pela humanidade desde os tempos mais remotos. A partir do momento em que o homem tomou consciência da interdependência das condições Climáticas e daquelas resultantes de sua deliberada intervenção no meio natural como necessidade para o desenvolvimento social, ele passou a produzir e registrar o conhecimento sobre os componentes da natureza. Neste contexto, se torna necessario a instalação de estações meteorologicas, porem existem diversos tipos de estações, desde manuais ate as mais modernas que são informatizadas.Assim, foi feito a comparação de dados de duas estações, uma convencional e outras duas automaticas, no Vale do Paraiba Paulista.
Tipo: Presentation
Palavras-chave: Estações Meteorológicas; Meteorologia; Climatologia.
Ano: 2011
URL: http://hdl.handle.net/2315/164

GPS TrackMaker: principais funções e aplicações
Provedor de dados: 25
Autores: Sauruk, Gilson Sauruk; Disperati, Attilio Antonio; Oliveira Filho, Paulo Costa.
A presente publicação aborda os seguintes itens:  1) Considerações gerais do software,  2) Tela inicial do programa nas versões gratuito e profissional, 3) Detalhes da tela inicial, 4) Configurações e ajustes iniciais,  5) Tutorial para descarregar os dados armazenados no receptor de navegação GPS,  6) Tela principal após descarregamento de dados do receptor GPS, 7) Tela principal após a seleção e edição de pontos e de trilhas; o resultado final em forma de mapa, 8) Cálculo da área do polígono inserido no mapa, 9) Inserção e georreferenciamento de imagens; cruzamento de dados do GPS em uma imagem georreferenciada, 10) Referência bibliográfica.
Tipo: Presentation
Palavras-chave: GPS; Software TrackMaker; Georreferenciamento de imagem; Avaliação de recursos naturais.
Ano: 2007
URL: http://hdl.handle.net/2315/73

CARACTERIZAÇÃO MORFOMÉTRICA DA MICROBACIA DO RIBEIRÃO DA SERRA NO MUNICÍPIO DE TREMEMBÉ - SP
Provedor de dados: 25
Autores: M. de O. Anacleto, Lucas; Almeida Valente, Larissa; Gomes Del Santo, Mayara; Teixeira Batista, Getulio; Mendes de Moura, Yhasmin; Santos Targa, Marcelo.
Resumo apresentado no Encontro de Iniciação Científica, XIII Mostra de Pós-graduação - 16 a 20 de outubro de 2012, no Campus do Bom Conselho, Universidade de Taubaté - Taubaté – SP
Tipo: Other
Palavras-chave: Bacia; Uso da terra; Morfometria de bacias; SRTM.
Ano: 2012
URL: http://hdl.handle.net/2315/255

DIAGNÓSTICO E PROPOSTA DE MANEJO DE FRAGMENTOS FLORESTAIS NATIVOS E DA PAISAGEM EM UMA PROPRIEDADE FLORESTAL
Provedor de dados: 25
Autores: SCOLFORO, JOSÉ ROBERTO.
Existe uma controvérsia histórica sobre o papel desempenhado pelo eucalipto. Duas questões freqüentemente abordadas são:  1. a crença de que o eucalipto provoca rápido secamento do solo e;  2.  as perdas de biodiversidade ecológica em relação   ao ecossistema original.
Tipo: Presentation
Palavras-chave: MANEJO FLORESTAL; Microbacias; Inventario Florestal; Ciências Florestais.
Ano: 2007
URL: http://hdl.handle.net/2315/133

Estudo comparado de biogeografia fisionômica - caracterização da vegetação do Vale do Paraíba paulista nos anos de 1817 e 2007 (*)
Provedor de dados: 25
Autores: Freitas Junior, Gerson de; Marson, Anelise Aparecida.
This article is a study of phisionomic biogeography. It describes the vegetation (trees and forests, scrubs, grasslands, brazilian savannas, etc.) on the “Vale do Paraíba paulista” (East of the São Paulo state, Brazil, South America) in two periods – 1817, when the vegetation conditions were primitive, and 2007, when the vegetation conditions are very different. It describes yet, the historic process of occupation in this area and the modification of the natural formations. The work of the two german naturalists - Spix &amp; Martius - and field works was utilized for the knowledge of the vegetation conditions. In 1817, the forests were founded in many places, but actually, the forests to be founded in few places, restricted to the mountains or isolated in...
Tipo: Article
Palavras-chave: Biogeografia fisionômica; Vale do Parai­ba uso da terra fitogeografia.
Ano: 2007
URL: http://hdl.handle.net/2315/88

Reposição florestal na bacia hidrográfica do Rio Una: a experiência da UNITAU
Provedor de dados: 25
Autores: Cicero, Carlos Moure; Catelani, Celso de Souza; Targa, Marcelo dos Santos; Batista, Getulio Teixeira; Dias, Nelson Wellausen.
This article presents the experience in the implementation of a native species forest recovering project in private rural properties located in the Una river basin, municipality of Taubaté, in degraded areas with inadequate land use practices, and located in Permanent Protected Areas (APPs) determined by the Federal Law No 4.771/65. Twelve areas of one hectare each were selected based on diagnose results obtained from the Una river basin georreferenced environmental database. Forest recovering strategy followed the secondary succession conceptual framework for tropical forests utilizing only native species listed in the State Resolution SMA 21/01. A total of approximately 20,000 trees were planted in those areas. The implantation phase was fully successful...
Tipo: Article
Palavras-chave: Reposição florestal; Bacia hidrográfica; Preservação permanente.
Ano: 2007
URL: http://hdl.handle.net/2315/86

Óleos vegetais e a produção de biodiesel no Brasil.
Provedor de dados: 25
Autores: Ferreira, Willian J.
Material apresentado ao PPGCA-Belém, disciplina Desenvolvimento Sustentável, em outubro de 2010.
Tipo: Presentation
Palavras-chave: Biocombustíveis; Oleaginosas; Soja; Pinhão manso.
Ano: 2011
URL: http://hdl.handle.net/2315/163

Potencialidade das emissões de metano frente a produção de eletricidade no Brasil
Provedor de dados: 25
Autores: Braz, Lia; Ferreira, Willian J.; Targa, Marcelo S.; Batista, Getulio T.
Gás de efeito estufa com destacado papel na química e na física da atmosfera terrestre, o metano é produzido pela degradação anaeróbia de compostos orgânicos em ambientes diversificados. Hoje, o meio aquático responde por aproximadamente 40% das emissões globais do gás para a atmosfera e a densa rede hidrográfica brasileira pode ter grande participação nesses números, devido ao acúmulo e degradação de matéria orgânica nos trechos de baixa vazão de rios e áreas inundadas. A disponibilidade de recursos hídricos favorece a produção de energia pelas usinas hidrelétricas no país. No entanto, a matéria orgânica que se decompõe no fundo dos reservatórios apresenta potencial para elevar de maneira significativa as taxas de emissão de metano, causando alterações...
Tipo: Presentation
Palavras-chave: Gases de efeito estufa; Aquecimento global; Energia; Represas.
Ano: 2011
URL: http://hdl.handle.net/2315/159

Ação de Inseticidas Botânicos sobre a Preferência Alimentar e sobre Posturas de Spodoptera frugiperda (J.E. Smith) (Lepidoptera: Noctuidae) em Milho
Provedor de dados: 25
Autores: Mazzonetto, Fábio; Coradini, Flávia; Corbani, Renato Zapparoli; Dalri, Alexandre Barcellos.
Resumo. O presente trabalho objetivou comparar o efeito de diferentes extratos de origem vegetal na preferência alimentar e na postura da lagarta do cartucho Spodoptera frugiperda (J.E. Smith) em folhas de milho. Extratos aquosos a 10% p/v de Chenopodium ambrosioides (Linnaeus) (Erva de Santa Maria), Corymbia citriodora (Hill &amp; Johnson) (Eucalipto Cheiroso), Chrysanthemum leucanthemum (Linnaeus) (Crisântemo) e Azadirachta indica (A. Juss) (Nim) foram aplicados em discos de folhas de milho e oferecidos às lagartas em testes com e sem chance de escolha. A atratividade das lagartas pelos discos com os extratos não diferiu da testemunha no teste com chance de escolha, porém os extratos de Nim e Crisântemo apresentaram efeito fagodeterrente a S. frugiperda....
Tipo: Article
Palavras-chave: Extratos Vegetais; Lagarta do Cartucho; Fall Armyworm; Vegetal Extracts.
Ano: 2013
URL: http://hdl.handle.net/2315/265

FERTIRRIGAÇÃO COM ESGOTOS TRATADOS POR PROCESSOS ANAERÓBIOS E PÓS -TRATAMENTO
Provedor de dados: 25
Autores: Santos, Roberto Jose dos; Fortes Neto, Paulo; Batista, Getulio Teixeira.
Citação: SANTOS, R. J. dos; FORTES NETO, P.; BATISTA, G. T. Fertirrigação com esgotos tratados por processos anaeróbios e pós –tratamento. Repositório Eletrônico Ciências Agrárias, Coleção Ciências Ambientais, &lt;http://www.agro.unitau.br/dspace&gt;. p. 1-10, 2011.  Resumo. Este trabalho foi desenvolvido a partir de pesquisas de artigos científicos de experimentos efetuados na cidade de Campina Grande, com esgotos domésticos, tratados inicialmente por reatores anaeróbios do tipo UASB e posteriormente submetidos a diversos tipos de pós- tratamentos, em todas as experiências avaliou-se a eficiência de cada sistema, buscando-se verificar basicamente, alguns indicadores tais como: remoção de nutrientes, organismos patogênicos, eficiência de DBO, DQO, sólidos...
Tipo: Article
Palavras-chave: Reatores; Irrigação; Reuso de águas; Águas residuárias; Water reuse; Waste waters.
Ano: 2011
URL: http://hdl.handle.net/2315/172

Entraves na sustentabilidade do biodiesel de pinhão manso (Jatropha curcas L.) em países emergentes.
Provedor de dados: 25
Autores: Ferreira, Willian J.; Batista, Getulio T.
Palestra apresentada no Seminário de alunos: Energia, Meio Ambiente e Desenvovimento, do Programa de Pós Graduação em Energia do IEE/USP.
Tipo: Presentation
Palavras-chave: Política energética; Sustentabilidade; Biocombustíveis; Barreiras.
Ano: 2011
URL: http://hdl.handle.net/2315/162

ESTUDO DA ADEQUABILIDADE DE USO DO SOLO E VIABILIDADE ECONÔMICO-AMBIENTAL: O CASO DA FAZENDA CAMBURI
Provedor de dados: 25
Autores: Dias, Nelson W.; Batista, Getulio T.; Targa, Marcelo S.; Catelani, Celso S.
Neste estudo foram analisadas as condições de uso atual da terra da Fazenda Camburí comparando-as com as características naturais do meio físico e cruzando, com auxílio de um sistema de informações geográficas, estas informações espaciais com as limitações legais impostas pela legislação vigente de proteção ambiental para dar subsídios à elaboração de diretrizes de ação econômica e ambiental que visem o uso sustentável desta propriedade. Os resultados demonstraram que se aplicada a legislação vigente que define as APPs de topos de morro a área de solo economicamente utilizável desta fazenda se reduziria em 186,14 hectares (quase um terço da área total). Também foi demonstrado que a área da fazenda que pode ser utilizada para fins agrícolas intensivos...
Tipo: Article
Palavras-chave: Adequabilidade; Viabilidade econômico-ambiental; Sustentabilidade de propriedade rural.
Ano: 2006
URL: http://hdl.handle.net/2315/59

Plano Nacional de Recursos Hí­dricos: A Bacia do Paraí­ba do Sul no Contexto do Plano
Provedor de dados: 25
Autores: SILVA, PAULO AUGUSTO ROMERA E.
Para o uso racional da Bacia hidrográfica do Pariaba do Sul é necessário: CONSOLIDAR O MARCO INTITUCIONAL; FORTALECER O SISTEMA DE GESTÃO; AÇÕES DE GESTÃO NA DEMANDA; INTEGRAÇÃO DA POLÍTICAS PÚBLICAS; CONTRIBUIR PARA A DESCONCENTRAÇÃO ECONÔMICA E A EQUIDADE SOCIAL; ANTECIPAR-SE AOS PROBLEMAS DE REGIÕES CRÍTICAS; FORTALECER A CAPACITAÇÃO; ESPAÇO PARA PARTICIPAÇÃO SOCIAL NA  IMPLANTAÇÃO DA POLÍTICA PÚBLICA; OPORTUNIDADE DA INSERÇÃO DA QUESTÃO DA ÁGUA NOS DEBATES NACIONAIS; GRADATIVA SENSIBILIZAÇÃO SOCIAL SOBRE SUA RELEVÂNCIA PARA O DESENVOLVIMENTO; RESPONSABILIDADES COMPARTILHADAS QUE DECORREM DOS ORGANISMOS COLEGIADOS; EXIGÊNCIA DE CAPACITAÇÃO DOS AGENTES NO EXERCÍCIO DE SUAS COMPETÊNCIAS; ENTENDIMENTO DOS PROCESSOS DE NEGOCIAÇÃO O QUE PRESSUPÕE ACEITAR...
Tipo: Presentation
Palavras-chave: Gestão de recursos hídricos; Uso sustentável da água; Cenários do uso da água.
Ano: 2007
URL: http://hdl.handle.net/2315/136

Geoprocessamento: uma ferramenta para o desenvolvimento regional sustentável
Provedor de dados: 25
Autores: Dias, Nelson Wellausen; Batista, Getulio Teixeira.
Tópicos do Capítulo: 1. O geoprocessamento e o conhecimento espacial 2. A estrutura básica de um banco de dados geográfico 3. A análise espacial e o desenvolvimento regional sustentável 4. Aplicabilidade das ferramentas de conhecimento espacial ao planejamento regional 5. O monitoramento das intervenções humanas no meio físico 6. Situação das bases de dados geográficos brasileiras e as necessidades atuais 7. A integração de informações espaciais como indicador da sustentabilidade
Tipo: Book chapter
Palavras-chave: Banco de dados georreferenciados; Análise espacial.
Ano: 2008
URL: http://hdl.handle.net/2315/145

Pagamento por serviços ambientais
Provedor de dados: 25
Autores: Batista, G. T.
O ambiente nos fornece produtos ambientais, tais como: madeira, frutos, peles, carne, sementes, medicinas e serviços ambientais tais como: regulação de gases (produção de oxigênio e seqüestro de carbono), belezas cênicas, conservação da biodiversidade, proteção de solos e dos recursos hídricos que permitem a regulação do clima e a conservação da biodiversidade. O uso dos recursos naturais, seguindo normas legais, diminui o impacto sobre o meio ambiente, mas implicam em custos que muitas vezes são evitados, causando sérios problemas para a sustentabilidade de nosso planeta. Dessa forma, foram instituídos mecanismos de controle, tais como: licenciamento, repressão (multas, etc.) para monitorar e eventualmente sancionar quem não respeite estas regras de...
Tipo: Presentation
Palavras-chave: Meio ambiente; Preservação; Ecologia; Conservação.
Ano: 2010
URL: http://hdl.handle.net/2315/156

Recursos hídricos na Mata Atlântica: estudo de caso do Laboratório de Hidrologia Florestal Walter Emmerich, Cunha - SP
Provedor de dados: 25
Autores: Arcova, Francisco Carlos Soriano Arcova; Cicco, Valdir de; Ranzini, Maurício; Santos, João Batista Amaro dos; Forti, Maria Cristina.
The Forestry Institute of São Paulo State have been studying the water and forest relationships in Laboratory of Forest Hydrology Walter Emmerich at Cunha in the Serra do Mar State Park in the last three decades. From the obtained long-term data the knowledge about the hydrologic cycle and hydrochemical processes are being deepen within the Atlantic Forest. The starting point of these researches is the named “hydrometric method of experimental catchments” which monitors three catchments covered with secondary natural forest. In this paper it is presented a synthesis of the relevant results obtained up to now whose objective is to show the importance of the Atlantic Forest conservation for the maintenance of the Serra do Mar mountain range water resources.
Tipo: Article
Palavras-chave: Hidroquímica; Mata Atlântica; Serra do Mar; Hidrologia; Alto Vale do Paraíba do Sul.
Ano: 2007
URL: http://hdl.handle.net/2315/78

CARACTERIZAÇÃO DO POTENCIAL HIDROGEOLÓGICO E HISTÓRICO DA UTILIZAÇÃO DAS ÁGUAS SUBTERRÂNEAS NA BACIA HIDROGRÁFICA DO PARAÍBA DO SUL, NO ESTADO DE SÃO PAULO
Provedor de dados: 25
Autores: Dias, Nelson W.; Diniz, Hélio N.; Batista, Getulio T.; Targa, Marcelo S.
Este é um projeto de pesquisa com ênfase ao estudo das áreas de recarga dos aqüíferos na parte paulista da bacia hidrográfica do rio Paraíba do Sul. O estudo tem como objetivo proporcionar conhecimento do meio físico e de avaliar as áreas de recarga dos aqüíferos subterrâneos, por meio do levantamento e formação de um cadastro com uma sólida base de dados hidrogeológicos, climáticos e geológicos e, através de mapas e cartas temáticas apropriadas ao gerenciamento dos recursos hídricos subterrâneos. O projeto permitirá o levantamento das áreas de recarga da bacia do rio Paraíba do Sul no Estado de São Paulo, com vistas à sua proteção e conservação dos recursos hídricos. O desenvolvimento de um projeto sobre a hidrogeologia da bacia hidrográfica do rio...
Tipo: Article
Palavras-chave: Áreas de recarga; Mapeamento hidrogeológico; Água subterrânea.
Ano: 2006
URL: http://hdl.handle.net/2315/60

REPOSIÇÃO FLORESTAL E EDUCAÇÃO AMBIENTAL NA BACIA DO RIO UNA, BACIA DO RIO PARAÍBA DO SUL
Provedor de dados: 25
Autores: Cícero, Carlos Moure; Carvalho, Vicente de Jesus; Batista, Getulio T.; Targa, Marcelo S.
Este trabalho tem como objetivo desenvolver ações ambientais na Bacia Hidrográfica do Rio UNA, no Município de Taubaté, que visem a integração institucional e a educação ambiental, para promover uma adequação nas formas de uso do solo, da água e a reposição florestal, para normalizar a disponibilidade e o abastecimento de água no Município de Taubaté.  Propor a organização comunitária das famílias rurais, fortalecer as formas organizacionais já existentes e estimular a participação de toda a comunidade, garantindo a continuidade das ações na bacia hidrográfica, transformando os agricultores e suas famílias em agentes de desenvolvimento. Ações conjuntas nas áreas de conservação do solo, dos recursos hídricos, reposição florestal nas áreas degradadas e...
Tipo: Other
Palavras-chave: Reflorestamento; Essências nativas.
Ano: 2006
URL: http://hdl.handle.net/2315/55

Condições ambientais na bacia do Paraíba do Sul e a efetividade da cobrança pelo uso da água pelo Estado do Rio de Janeiro
Provedor de dados: 25
Autores: Acselrad, Moema; Barcellos, Frederico Cavadas; Costa, Valéria Grace.
The Paraíba do Sul river basin is located in Brazilian southeast region and is composed by 180 districts from São Paulo, Minas Gerais and Rio de Janeiro states. Based on an IBGE research results about districts environment, it is analyzed the environmental problems ant their reasons. In this context, the water pollution and erosion questions are analyzed in district extent. After that, the effectiveness of bulk water charge in Rio de Janeiro state, in the four hydrographic regions that compose the Paraíba do Sul river basin in the state, is analyzed. A comparison is made between environment problems that have relationship with water resources and actions to solve them in those four hydrographic regions. The results show that there is a delay between...
Tipo: Article
Palavras-chave: Instrumentos de gestão; Poluição hídrica; Assoreamento; Cobrança.
Ano: 2007
URL: http://hdl.handle.net/2315/76

Processo de Perfuração Mecânica de Séptos de Bambu Gigante para Fabricação de Tubos de Drenagem
Provedor de dados: 25
Autores: Targa, Marcelo Santos; Neto, Argemiro Targa.
Procedimento desenhado para produzir tubos de bambu gigante para drenagem.
Tipo: Article
Palavras-chave: Drenagem; Sistema; Tubos; Bambu.
Ano: 2012
URL: http://hdl.handle.net/2315/249

Projeto piloto de recarga artificial na bacia do rio Una, Município de Taubaté
Provedor de dados: 25
Autores: Diniz, Hélio Nóbile; Batista, Getulio Teixeira; Santoro, Jair; Targa, Marcelo dos Santos.
This paper describes the sedimentary aquifer artificial recharge experiment perfomed by deep wells and the rain water collect in roofs, in the municipality of Taubaté, SP.
Tipo: Article
Palavras-chave: Bacia de Taubaté; Recarga artificial; Hidrogeologia; Aqüífero sedimentar.
Ano: 2007
URL: http://hdl.handle.net/2315/80

Avaliação da revegetação das margens do rio Gualaxo do Norte após a extração de ouro por draga em Mariana/MG
Provedor de dados: 25
Autores: Costa, Adriana Albuquerque da; Gonçalves, Iolanda de Sena; Dias, Herly Carlos Teixeira.
The objective was to evaluate a reforestation carried out by the goldwashers. The studied area is situated along the Gualaxo do Norte river margins in Mariana - MG. The seedlings were received by donation of regional nurseries and were planted on December of 2006 in hole of 25x25 cm and plant spacing 3x2 meters. The evaluations were carried through on March of 2007. The height was measured with metric ribbon and the diameter, 5 cm above the ground, was done by using digital pachymeter. They planted 538 seedlings of 20 different species, pertaining to twelve botanical families. The most abundant species were Enterolobium  contortisiliquum (96), Mimosa schomburgkii (76) and Chorisia speciosa (45). It was not possible to identify 19 individuals due to...
Tipo: Article
Palavras-chave: Riparian forest; Forest hydrology; Reforestation.
Ano: 2007
URL: http://hdl.handle.net/2315/110

PROJETO ÁGUA E VIDA
Provedor de dados: 25
Autores: Targa, Julio; Batista, Getulio; Dias, Nelson; Targa, Marcelo.
Água e Vida possui o significado simbólico da conjunção das palavras “água“ e “vida“com o seguinte enfoque: água representa o recurso natural, o qual demanda respeito e manejo adequado visto à sua vital importância à vida humana; vida representa a essência da razão pela qual o homem existe, toma decisões e age em seu entorno, ou seja, vida simboliza os fatores sócio-econômicos que ditam a atuação do homem em seu meio. O objetivo geral deste projeto é desenvolver e disseminar estratégias para a melhoraria no uso responsável da água, recuperação de corpos d’água e iniciativas conservacionistas voltadas para a melhoria da quantidade e qualidade da água em duas sub-bacias do Rio Paraíba do Sul (Una e Boqueira), através da capacitação de atores de gestão,...
Tipo: Other
Palavras-chave: Gestão de bacia hidrográfica; Educação ambiental; Produtor de água.
Ano: 2006
URL: http://hdl.handle.net/2315/57

A produção mineral pode ser sustentável? Uma análise epistemológica da questão
Provedor de dados: 25
Autores: Lima, Flavio Jorge; Fortes Neto, Paulo; Batista, Getulio Teixeira.
A bibliografia estudada para discutir a sustentabilidade da produção mineral aponta para duas correntes que debatem o assunto, caracterizadas de acordo com o ponto central das teses: a dos recursos fixos e custos oportunidades. A primeira encara os recursos explorados pela mineração como não renováveis e passíveis de exaustão. A segunda indica que novas tecnologias suprirão as demandas futuras à medida que os recursos poderão ser extraídos de fontes com menor concentração de minérios. Ambas pressupõem que o Estado poderia interferir incisivamente na questão da internalização dos custos da produção e da recuperação dos impactos ambientais. Legalmente, o Estado instituiu o principio “poluidor-pagador”, que parece não atender efetivamente a demanda degradante...
Tipo: Article
Palavras-chave: Sustentabilidade; Epistemologia e mineração.
Ano: 2011
URL: http://hdl.handle.net/2315/175

New Report of Costalimaita ferruginea (Fabricius) (Coleoptera: Chrysomelidae) on Eucalyptus sp. (Myrtaceae) in Sinop - Mato Grosso, Brazil
Provedor de dados: 25
Autores: Pires, Evaldo Martins; Corassa, Janaína de Nadai; Barreto, Marliton Rocha; Soares, Marcus Alvarenga.
Abstract. Costalimaita ferruginea (Fabricius) (Coleoptera: Chrysomelidae) is the main Coleoptera defoliator of eucalyptus in Brazil and has a strong association with plants of the family Myrtaceae, bein the eucalyptus important for the sectors of energy, paper, pulp and furniture industry. The objective of the present study was to record the occurrence of this Chrysomelidae in eucalyptus plants in Sinop, State of Mato Grosso, Brazil, during the months of November 2010 to January 2011, thus contributing to increase in knowledge on the geographic distribution of this insect and also hypothesize that the Coleoptera may soon become a major pest of eucalyptus in the state of Mato Grosso.  Resumo. Costalimaita ferruginea (Fabricius) (Coleoptera: Chrysomelidae) é...
Tipo: Book
Palavras-chave: Attack; Damages; Geographical distribution; Occurrence; Ataque; Danos; Distribuição geográfica; Ocorrência.
Ano: 2013
URL: http://hdl.handle.net/2315/266

Educação Ambiental com Ênfase na Preservação dos Recursos Hídricos no Município de Campos do Jordão-SP.
Provedor de dados: 25
Autores: Chung, Fabiola Granato; Lima, Marta Maria Vieira de.
Every day kids and adolescents received a lot of information by the media, making them be away of their own natural environment. Using a special didactic material (specific profile and water analyze kits) , the main propose of this project was to involved the students of a poor neighborhood of Campos do Jordão, to make a deep analyzes about the environmental conditions of the stream that pass by near their school. During a semester students were invite to analyze the river, the water quality, the abundant vegetation and the urban occupation along the river and it influence. This analyze allow the students build their own conclusions, enrich the learning process and developing values through the natural resources.
Tipo: Article
Palavras-chave: Environmental Education; Water quality and preservation Vila Albertina stream; Educational Interpretation.
Ano: 2007
URL: http://hdl.handle.net/2315/91

Conscientização ambiental de alunos de uma escola da periferia de Guaratinguetá como forma de proteger os recursos hídricos locais
Provedor de dados: 25
Autores: Sant`Anna, Luiz Guilherme Simões de; Silva, Luciane Aparecida Lemes da.
This project has the goal of providing ecological awareness to students from Ramão Gomes Portão State School. This school is located in periphery of the city of Guaratinguetá. In this region there are three small streams connected to Cacunda Creek that further connects to Paraíba do Sul River, which is the main river of this city. Field research has been used as a way to stimulated students to develop ecological sense, since the problems had been presented to them and their solutions depend on student’s actions. Considering that they are living in the area, they are also polluting agents of those streams. Improvements in student’s actions during class periods have been observed such as reduction of water consumption at school and garbage/recycle selection...
Tipo: Article
Palavras-chave: Recursos hídricos; Sustentabilidade hídrica; Educação ambiental.
Ano: 2007
URL: http://hdl.handle.net/2315/124

O “Nó” do Eucalipto: A sustentabilidade da silvicultura na Metade Sul
Provedor de dados: 25
Autores: Anesi, Sidinei Antonio.
The article makes a discussion regarding the sustentability of a new productive initiative based on reforestation. This project is presented as a solution for the economical stagnation of the Southern Half of Rio Grande do Sul due to its economical and social impacts. It is analyzed the conceptual evolution of sustainable development and its appropriation, in favor or against eucalyptus plantations. As well as the creation of a productive chain that will culminate in export cellulose factories. Its analyzed the economical and social reality of the region, the lack of knowledge by most of its population and the strong media influence supported by great capitalist groups and government institutions. Results and discussions lead to the formation and or...
Tipo: Article
Palavras-chave: Desenvolvimento sustentável; Eucalipto; Sustentabilidade; Silvicultura.
Ano: 2007
URL: http://hdl.handle.net/2315/119

SEQUESTRO DE CARBONO: O quê é isso?
Provedor de dados: 25
Autores: Almeida, Ana Aparecida Silva.
Nessa apresentação parte-se de conceitos básicos sobre o fluxo de carbono nos ecossistemas e sua relação com  o efeito estufa e mudanças no clima do planeta Terra.
Tipo: Presentation
Palavras-chave: Sequestro de carbono; Mudanças climáticas.
Ano: 2011
URL: http://hdl.handle.net/2315/181

Aplicação de rotinas morfológicas para detecção de redes de drenagem
Provedor de dados: 25
Autores: Leonardi, Fernando; Silva, Erivaldo Antônio da.
Brazil presents great deficiency in cartographic updating area. Many products are outdated around in 30 years in the several scales. A country that has the continental dimensions as Brazil needs have a solid cartographic base to take important decisions about urban planning and consequenting to administration of the territory. One way of updating the cartographic products is the combined use of remote sensing products and techniques of Digital Processing Images (DPI). Among many DPI tools, the Mathematical Morphology allied to the remote sensing data, is one alternative method used to minimize this problem. For the development of this work three images taken with the Landsat sensor was used, having draining net, as the interest features. In this paper was...
Tipo: Article
Palavras-chave: Sensoriamento Remoto; Remote Sensing; PDI; Detecção de Feições; Morfologia Matemática; Mathematical Morphology; Features of detection.
Ano: 2007
URL: http://hdl.handle.net/2315/97

A alfabetização em Ciências e as mudanças climáticas globais
Provedor de dados: 25
Autores: Ferreira, Willian J.
Semana do Meio Ambiente - 2010.
Tipo: Presentation
Palavras-chave: Ensino informal; Concepções alternativas; Aquecimento global; Efeito estufa.
Ano: 2010
URL: http://hdl.handle.net/2315/155

Preferência Floral de Vespas (Hymenoptera, Vespidae) no Rio Grande do Sul, Brasil
Provedor de dados: 25
Autores: Somavilla, Alexandre; Köhler, Andreas.
As vespas integram a comunidade de visitantes florais e podem constituir uma parcela representativa dos polinizadores. Por este motivo, objetivou-se conhecer e analisar a preferência floral das espécies de Vespidae, bem como investigar o uso de recursos florais por estas vespas. Foram realizadas coletas entre o período de 2001 a 2008 em diferentes localidades do Estado do Rio Grande do Sul (Estrela Velha, Santa Cruz do Sul, São Francisco de Paula e Sinimbu), entre 08:00 a 17:00 horas, utilizando redes entomológicas para a captura dos vespídeos visitando flores. Os espécimes coletados foram depositados na Coleção Entomológica de Santa Cruz do Sul (CESC). Coletou-se 1.483 indivíduos alocados em 73 espécies de vespas, sendo que 78,9% são Polistinae (30...
Tipo: Article
Palavras-chave: Asteraceae; Flower visitors; Polistes versicolor; Schinus terebinthifolius; Trophic niche overlap; Sobreposição de nicho trófico; Visitantes florais.
Ano: 2012
URL: http://hdl.handle.net/2315/245

Florestamento compensatário com vistas à  retenção de água no solo da bacia hidrográfica do Ribeirão Itaim, Taubaté, SP
Provedor de dados: 25
Autores: Rodrigues Junior, Caio; Targa, Marcelo dos Santos; Batista, Getulio Teixeira; Dias, Nelson Wellausen.
The objective of this work was to quantify the area of compensatory forestation (AFC) for the retention of water in the soil in the Itaim Stream watershed, in Taubaté, SP. The estimations were based on the Compensatory Forestation for Water Retention in Small Watersheds (FCRAM) methodology that takes into consideration the following parameters: 1) the international percentage of water that has to infiltrate into the soil equal to 20.55%; 2) land cover and use classes; 3) soil permeability; and 4) mean annual precipitation. Ribeirão Itaim's watershed has an area of 5,770 ha. The results showed that the compensatory reforestation to guarantee the annual volume of water loss equal to 5,79 million m³ should contemplate an reforestation area of 433,9 ha,...
Tipo: Article
Palavras-chave: Permeabilidade; Uso e ocupação; Florestamento compensatório.
Ano: 2007
URL: http://hdl.handle.net/2315/83

A Simple Mathematical Model to Study the Mixture Processes in a northeast River Basin
Provedor de dados: 25
Autores: Alcântara, E.H.
O presente trabalho tem como objetivo analisar os processos de mistura no sistema estuarino do Rio Periá (Maranhão State, Brazil) e zonear o sistema através da classificação de Kjerfve (1987). Foi utilizado o modelo matemático de Dyer e Taylor (1973), para analisar os processos de mistura. Para obtenção dos objetivos, a batimetria do sistema estuarino foi levantada, e com a mesma foram delimitados os limites atingidos pelas marés alta e baixa. Foram analisados, num padrão unidimensional: as salinidades e as concentrações e/ou frações de água doce nas marés alta e baixa; as taxas e os tempos de descarga; e os volumes de água doce retidos no estuário nas estofas de enchente e vazante. Foram obtidos os seguintes resultados: o volume de água no sistema possuí...
Tipo: Article
Palavras-chave: Salinidade; Rio Periá (MG); Estuários; Análise unidimensional; Processos de mistura; Tempo de descarga.
Ano: 2007
URL: http://hdl.handle.net/2315/118

Análises dos índices físicos do solo e de sondagens SPT na área da várzea do rio Paraíba do Sul no município de Tremembé, SP
Provedor de dados: 25
Autores: Diniz, Helio; Galina, Marcia; Batista, Getulio; Targa, Marcelo.
Apresentado no XIX Simpósio Brasileiro de Recursos Hídricos, Maceió, 2011.
Tipo: Article
Palavras-chave: Hidrogeologia; Várzea do rio Paraíba do Sul; Município de Tremembé.
Ano: 2012
URL: http://hdl.handle.net/2315/243

Definição de zonas de captura e concentração de águas subterrâneas, em  parte do Vale do Paraíba e serras do Mar e Mantiqueira - SP: Uma Abordagem por Sensoriamento Remoto Orbital
Provedor de dados: 25
Autores: Mattos, Juércio Tavares de; Silva, Anderson Rodrigo da; Prata, Bruno Laisner.
This research is based on a study of landforms using remote sensing techniques. A satellite image and topographic maps were used for identifying groundwater resources. Precipitation information and well flow data were also used. The final result is a thematic map showing the location of recharge areas, circulation and concentration of groundwater.
Tipo: Article
Palavras-chave: Underground hydric resources; Análise ambiental; Sensoriamento remoto; Recursos hídricos Subterrâneos; Analysis environmental; Remote sensing.
Ano: 2007
URL: http://hdl.handle.net/2315/116

MODELO DE BANCO DE DADOS AMBIENTAIS GEORREFERENCIADOS VOLTADO À RECUPERAÇÃO E PRESERVAÇÃO DE RECURSOS HÍDRICOS DE UMA BACIA DE MÉDIO PORTE, O MODELO DA BACIA DO RIO UNA, PARAIBA DO SUL, SP
Provedor de dados: 25
Autores: Batista, Getulio Teixeira; Targa, Marcelo dos Santos; Dias, Nelson Wellausen; Catelani, Celso de Souza.
RESUMO - O Rio Una recebe grande aporte de sedimentos provindos de margens erodidas, obras mal planejadas e vastas áreas de pastagem degradada, os quais transportam um grande volume de sedimentos para o Rio Paraíba do Sul, inviabilizando o uso dessas águas para o abastecimento urbano. A criação do banco de dados ambientais da bacia Una (com 476 km²) é importante pela grande quantidade de vertentes naturais (com alto potencial de produção de água) e pela crescente perda de qualidade pelo aumento da carga de sedimentos. A estruturação do banco georreferenciado envolveu: geração de um mosaico ortorretificado com resolução de 0,60 m; mapeamento de uso do solo na escala 1:25.000; rede de drenagem e malha viária na escala 1:10.000; geração de um MDE; mapeamento...
Tipo: Article
Palavras-chave: Banco de dados ambientais; Bacia de médio porte; SIG; Recuperação e preservação.
Ano: 2006
URL: http://hdl.handle.net/2315/63

CHUMBO E ZINCO EM SOLOS E PLANTAS ÀS MARGENS DE UMA RODOVIA COMO INDICADORES DE POLUIÇÃO
Provedor de dados: 25
Autores: Silva, Luis Celso; Almeida, Ana Aparecida Silva.
Due to fast urbanization and the access and traffic facilities, many cities had been constructed close the great highways, where soils next to these highways are subject to many potential pollution sources, mainly the emissions from discharge for automotive vehicles. Concentrations of lead and zinc had been determined in soils and plants samples within 50 m of the edges from Presidente Dutra highway, in the valley of the Paraíba do Sul River, in the southeastern region of Brazil. The results had shown that the biggest concentrations of these metals find at 0-10 m of distance from the highway edges and decrease with increasing distance from highway. The average Pb and Zn concentrations in the study areas, respectively, were: 34,9 e 189,6 ppm (0-10 m); 10,6...
Tipo: Article
Palavras-chave: Poluição do solo; Sontaminação do solo; Metais pesados; Fitoextração.
Ano: 2011
URL: http://hdl.handle.net/2315/182

ALOC – Modelo de alocação de carga e vazão de diluição visando subsidiar a gestão integrada dos recursos hídricos
Provedor de dados: 25
Autores: Rodrigues, Roberta Baptista.
The main objective of this study is to develop a tool (ALOC model) to help with the implementation of water management mechanisms such as the analysis of authorization of water uses (permits) and water charging. An integrated analysis of both water quality and quantity is needed and the decision process must also take into account watershed plans and the designated uses of the water.
Tipo: Article
Palavras-chave: Gestão integrada; Outorga e cobrança; Enquadramento.
Ano: 2007
URL: http://hdl.handle.net/2315/90

Caracterização espaço-temporal do regime pluviométrico na parte paulista da bacia hidrográfica do rio Paraíba do Sul
Provedor de dados: 25
Autores: Folhes, Marcelo Theophilo; Rennó, Camilo Daleles; Fisch, Gilberto.
The objective of this study is to evaluate existing temporal and spatial patterns in the precipitation historical data in the Paraíba do Sul watershed, using newly available geostatistical analysis. Resulting rainfall maps showed pronounced regional and seasonal variations as well as a strong association with the topographic map. This study is a work in progress and the authors are in the process of modeling the hydrological cycle components in the watershed to characterize the variations in consideration of the water demands of Eucaliptus plantations.
Tipo: Article
Palavras-chave: Precipitação; Krigagem; Bacia do rio Paraíba do Sul.
Ano: 2007
URL: http://hdl.handle.net/2315/120

Mirmecofauna (Hymenoptera, Formicidae) de Duas Marismas do Estuário da Lagoa dos Patos, RS: Diversidade, Flutuação de Abundância e Similaridade como Indicadores de Conservação
Provedor de dados: 25
Autores: Bolico, Cristiane Ferras; Oliveira, Eduardo Alves; Gantes, Marcel Lucas; Dumont, Luiz Felipe Cestari; Carrasco, Daiane Silveira; D´Incao, Fernando.
O trabalho objetiva inventariar a mirmecofauna de duas marismas distintas e estimar a diversidade, similaridade, bem como relacionar a temperatura, umidade relativa do ar e a pluviosidade aos padrões de flutuação de abundância desses insetos. Além disso, foram reconhecidas as espécies que atuam como indicadores ambientais. O estudo foi realizado em duas marismas localizadas no Estuário da Laguna Lagoa dos Patos, Ilha da Torotama e Molhe Oeste da Barra. Foram capturados 853 formicídeos, distribuídos em 19 gêneros. As duas marismas apresentaram índices de diversidade e abundância semelhantes, Ds = 0,958 e I = 0,042 na Ilha da Torotama e Ds = 0,8889 e I = 0,111 no Molhe Oeste da Barra. As flutuações dos grupos de formicídeos coincidiram em ambas as áreas,...
Tipo: Article
Palavras-chave: Bioindicador; Ecossistema Costeiro; Formigas; Insetos; Ants; Malaise; Bioindicator; Coastal Ecosystem; Insects.
Ano: 2012
URL: http://hdl.handle.net/2315/246

Georreferenciamento de Trilhas do Parque Natural Municipal Trabiju, Pindamonhangaba, SP
Provedor de dados: 25
Autores: Lobo, Thais F.; Batista, Getulio T.; Targa, Marcelo dos Santos.
Resumo. Este trabalho teve por objetivo o georreferenciamento das trilhas existentes no Parque Natural Municipal do Trabiju, localizado na cidade de Pindamonhangaba, estado de São Paulo. Com o georreferenciamento das trilhas, torna possível a elaboração de mapas das trilhas com a caracterização dos pontos atrativos delas e a identificação do nível de dificuldade que por outro lado darão subsídio para o seu manejo adequado para abertura à visitação do Parque. As Unidades de Conservação são de extrema importância para biomas ameaçados e ao mesmo tempo nelas são permitidos o uso sustentável de seus recursos. Após o mapeamento das trilhas será possível desenvolver programa de Gestão Ambiental para conservação da vida silvestre para a proteção e o uso público,...
Tipo: Article
Palavras-chave: SIG; Ecoturismo.
Ano: 2011
URL: http://hdl.handle.net/2315/168

Reprodução de Trichospilus diatraeae Cherian &amp; Margabandhu (Hymenoptera: Eulophidae) em Pupas de Anticarsia gemmatalis Hübner (Lepidoptera: Noctuidae) em Relação à Idade do Parasitóide e Hospedeiro
Provedor de dados: 25
Autores: Pastori, Patrik Luiz; Zanuncio, José Cola; Silva, Robson Oliveira; Pereira, Fabricio Fagundes; Azambuja, Rosalia; Pereira, José Milton Milagres.
A reprodução de parasitóides apresenta etapas interligadas e a idade de hospedeiros e parasitóides pode afetar o desenvolvimento desses últimos. Características biológicas de fêmeas de Trichospilus diatraeae Cherian &amp; Margabandhu (Hymenoptera: Eulophidae), com até 96 horas de idade, foram estudadas em pupas do hospedeiro alternativo Anticarsia gemmatalis Hübner (Lepidoptera: Noctuidae). Cada pupa de A. gemmatalis com 0-24, 24-48, 48-72 ou 72-96 horas de idade, foi oferecida ao parasitismo por 10 fêmeas de T. diatraeae com 0-24, 24-48, 48-72 ou 72-96 horas de idade, por 24 horas à 25 ± 2oC, umidade relativa de 70 ± 10% e fotofase de 14 horas. A emergência, o número de descendentes, a duração do ciclo, a razão sexual, a longevidade e largura da cápsula...
Tipo: Article
Palavras-chave: Criação massal; Hospedeiro alternativo; Resposta funcional; Alternative host; Functional response; Mass rearing.
Ano: 2012
URL: http://hdl.handle.net/2315/231

MONITORAMENTO DE POLUENTES ATMOSFÉRICOS POR MEIO DE SENSORES ELETRÔNICOS DE BAIXO CUSTO
Provedor de dados: 25
Autores: Marcos, A. Silveira; Gabriel, Marinho; Lia, Braz; Ericka, V. C. Mariano; Dawilmar, G. de Araújo; Willian, J. Ferreira.
Trabalho submetido e apresentado no III CICTED, Taubaté, 2014.
Tipo: Presentation
Palavras-chave: Sensor MQ-9; Sensor MQ-2; Arduíno; Gases de Efeito Estufa.
Ano: 2014
URL: http://hdl.handle.net/2315/283

Emissões de carbono em função da implantação de eucalipto em áreas ocupadas com pastagem
Provedor de dados: 25
Autores: Bassanelli, Hélio Rodrigues; Batista, Getulio T.; Loos, Rodolfo Araujo.
Apresentado no The 4th International Congress on University-Industry Cooperation – Taubate, SP – Brazil – December 5th through 7th, 2012 ISBN 978-85-62326-96-7
Tipo: Article
Palavras-chave: Geoprocessamento; Mudança de uso da terra; Sequestro de carbono.
Ano: 2012
URL: http://hdl.handle.net/2315/263

O FLORESTAMENTO NA CONSERVAÇÃO DA ÁGUA EM BACIA HIDROGRÁFICA
Provedor de dados: 25
Autores: Rodrigues, Bruna Andressa; Souza, Gustavo Tadeu Alvarenga M.; Anacleto, Lucas Michel de Oliveira; Babosa, Natália Rabelo; Dias, Valerian; Targa, Marcelo Santos.
O presente estudo tem por objetivo verificar a conservação da água por meio da estimativa da infiltração potencial e do escoamento superficial na Bacia hidrográfica do ribeirão do Itaim, em Taubaté-SP em função das modificações ocorridas no período de 1896 a 2003 e a simulação de escoamento para 2020 adotando-se uma política que valorize a conservação da área. Sendo atualmente a única possibilidade de crescimento, a malha urbana do município de Taubaté esta direcionada para a bacia, que está no limite entre a área expansão urbana e da área de Preservação Ambiental. Com base em dados de escoamento superficial já existentes para a área nos anos de 1986 e 2003, utilizou-se a técnica do Curva Número que permite verificar a capacidade de infiltração potencial...
Tipo: Article
Palavras-chave: Ciências ambientais; Escoamento superficial; Infiltração potencial; Solos.
Ano: 2014
URL: http://hdl.handle.net/2315/277

Coleta de dados para gestão do Rio Paraíba do Sul no trecho do município de Jacareí.
Provedor de dados: 25
Autores: Lima, Carlos Alberto Cerqueira; Trancho, Maurício Braga; Oliveira, Jéferson Andrade de; Ramos, Carlos Lhoret.
This work describes the way as the system of Administration of “Paraíba do Sul” river was elaborated for the accompaniment of the evolution of the bed and obtaining of a diagnosis of the present and potential problems, for a previous planning of the necessary actions in the sense of avoiding the erosion or silting of the fund and of the margins of the river, inhibiting the development of problems that you/they can win larger proportions in the future. They were made batimétric and hydrometric measurement, and modeling simulations for the formation of this base of information, which was incorporated to our geodatabase.
Tipo: Article
Palavras-chave: Batimetria; Gestão do rio.
Ano: 2007
URL: http://hdl.handle.net/2315/96

URBANIZAÇÃO SUSTENTÁVEL E O ESCOAMENTO SUPERFICIAL EM BACIA HIDROGRÁFICA
Provedor de dados: 25
Autores: Santos, Eduardo Rodrigues dos; Leite, Cláudia Regina da Silva; Perim, Marli Aparecida; Gonçalves, Solange Fátima; Targa, Marcelo Santos.
No presente artigo foi estimado a precipitação efetiva (Pe), que gera o escoamento superficial na sub-bacia do Ribeirão do Itaim para 2020, e os respectivos coeficientes de escoamento superficial( C ) considerando o uso e ocupação do solo, e as modificações ocorridas no período de 1986 a 2003 e um acréscimo de urbanização para 2020 de modo desordenado e também pela adoção de política de desenvolvimento sustentável. Aplicou-se a metodologia do Curva Número (CN) desenvolvida pela SCS- USDA. Foi considerado o Tempo de retorno (TR) de chuvas variando de 2 a 200 anos, escolhidos os valores de (CN), para cada classe de uso e cobertura do solo, e de urbanização em duas situações: Urbanização A em que a mesma é desordenada, sem planejamento, apresentando um índice...
Tipo: Article
Palavras-chave: Ciências ambientais; Infiltração potencial; Precipitação excedente; Solos.
Ano: 2014
URL: http://hdl.handle.net/2315/276

PROJETO PILOTO DE RECARGA ARTIFICIAL NA BACIA DO RIO UNA, MUNICÍPIO DE TAUBATÉ
Provedor de dados: 25
Autores: Diniz, Hélio Nóbile; Batista, Getulio Teixeira; Santoro, Jair; Targa, Marcelo dos Santos.
O projeto de recarga artificial de aqüíferos está sendo implementado na bacia hidrográfica do rio Una, no Município de Taubaté. O local do projeto é o Departamento de Ciências Agrárias da Universidade de Taubaté. A área foi escolhida porque é favorável à captação das águas em telhados e há condições topográficas para a injeção em poços, por gravidade .
Tipo: Presentation
Palavras-chave: Aqüífero freático; HIDROGEOLÓGICA; HIDROCLIMÁTICA.
Ano: 2007
URL: http://hdl.handle.net/2315/138

Estudo do uso e cobertura do solo e do escoamento superficial na bacia hidrográfica do Ribeirão Serragem no município de Tremembé, SP
Provedor de dados: 25
Autores: Rodrigues, Neyrianne d´Angelis; Batista, Getulio Teixeira; Targa, Marcelo dos Santos.
O presente trabalho objetivou avaliar o escoamento superficial da área que engloba os afluentes do Ribeirão Serragem no município de Tremembé, SP no vale do Paraíba do Sul, localizada na parte a montante da barragem da Fazenda Maristela, bem como mapear o uso do solo da mesma para subsidiar possíveis intervenções visando o uso sustentável dessa bacia. Foram empregadas técnicas de geoprocessamento com o uso de ferramentas do SPRING para a caracterização do uso e ocupação do solo, da caracterização física da bacia e para o cálculo da precipitação efetiva. Os resultados indicaram que a bacia do Ribeirão Serragem apresenta um bom estado de conservação, levando em consideração que ocorre o predomínio de florestas em todas as classes de APP com maior predomínio...
Tipo: Article
Palavras-chave: Basin; Flow; Land use; Environmental science.
Ano: 2012
URL: http://hdl.handle.net/2315/242

Sensibilidad de ecuaciones de Evapotranspiración en la estimación de los consumos de agua de Eucalyptus dunnii.
Provedor de dados: 25
Autores: Rébori, Maria Graciela.
A correct election of potential evapotranspiration (PET) equation is critical for water balance estimation of forest. The objective of this work was analyze the PET equations of SIMGRO model (SIMulation of GROundwater). SIMGRO model solves water balance in the unsaturated zone and the acuifer of diverse landuse covers, forest inclusively. The water consumption of the Eucalyptus dunnii was measured in a commercial forest. The weather data was measured daily and the humidity contents were measured up to 2 ms of depth monthly. The experimental sites were two: 1) old mounts, 8 years old and 2)young mounts ,2 years old. The PET equations of Makkink,Priestley- Taylor and Penman-Monteith were compared and ordered in increasing of meteorological data.requirments....
Tipo: Article
Palavras-chave: Evapotranspiración; SIMGRO; Eucalyptus dunnii; Balance de agua; Requerimientos hídricos.
Ano: 2007
URL: http://hdl.handle.net/2315/105

ESTUDO DE VIABILIDADE E EFICIÊNCIA DO USO DO HIDROGEL NO DESENVOLVIMENTO DO FEIJÃO
Provedor de dados: 25
Autores: Fortes Neto, Paulo Fortes Neto; Fortes, Nara Lúcia Perondi Fortes; Silva, Eliana Maria de Araújo Mariano Silva; Evangelista, Flavia de Oliveira.
O presente estudo teve como objetivo avaliar o consumo de água pela planta em função da evapotranspiração do feijão com vistas a estabelecer uma relação entre o consumo de água e a dosagem de hidrogel aplicada ao solo. Foram determinadas a evapotranspiração (ET) diária, as biomassas secas da parte aérea (BSA) e das raízes das plantas (BSR), o diâmetro do coleto (DC) e altura das plantas (H). A aplicação de diferentes doses (0; 0,025; 0,05; 0,075 e 0,10%) de hidrogel apresentou efeito significativo sobre a ET, limitando o estabelecimento de uma relação entre D x ET com o intuito de se estabelecer critérios para o uso do hidrogel em campo. No entanto, estas dosagens apresentaram efeito significativo sobre as variáveis DC, H e BSA, possibilitam inferir que o...
Tipo: Technical Report
Palavras-chave: Hidrogel; Resíduo.
Ano: 2012
URL: http://hdl.handle.net/2315/260

Análise do uso e ocupação do solo na sub-bacia do Ipiranga no município de Taubaté, SP nos anos de 2003 e 2010
Provedor de dados: 25
Autores: Silva, Deivid; Batista, Getulio.
Apresentado no Apresentado no XVI Enic, XII MPG, VI SEMEX e III SEDUNI da Universidade de Taubaté, 2011
Tipo: Other
Palavras-chave: Mudanças; Crescimento urbano.
Ano: 2012
URL: http://hdl.handle.net/2315/247

Mapa de Infiltração do Alto e Médio Vale do Paraíba do Sul com base em elementos da paisagem
Provedor de dados: 25
Autores: Soares, Paulo Valladares; Pereira, Sueli Yoshinaga; Simões, Silvio Jorge Coelho; Bernardes, George de Paula; Barbosa, Sérgio Augusto.
This work presents a methodological approach to characterize the infiltrations conditions in Paraiba do Sul river basin (7,600 km2). To each landscape feature (rock, and structure, relief, soil, rainfall and land-use) was applied a loading that corresponded to higher (5) or lower (1) influence in the infiltration potential through its geographical postion. A Map of Infiltration was created in ArcGIS. The results showed that areas with higher infiltration capacity are located in Serra da Bocaina in the Northeast region or associated with Serra do Mar relief in the Southeast region as well as with gentle hills and sandstones along the Paraiba do Sul river. The creation of a Map of Infiltration may contribute to a long-term water resources management plans...
Tipo: Article
Palavras-chave: Processos de infiltração; Sistemas de informação geográfica; Elementos da paisagem.
Ano: 2007
URL: http://hdl.handle.net/2315/85

Fronteira de expansão dos plantios de eucalipto no geoecossistema do médio vale do rio Paraíba do Sul (SP/RJ)
Provedor de dados: 25
Autores: Vianna, Lílian Gabriela Gomes; Sato, Anderson Mululo; Fernandes, Manoel do Couto; Coelho Netto, Ana Luiza.
Since early 21 century the landscape mosaic of middle Paraíba do Sul river valley (MPSRV) has been rapidly modified by spreading of Eucalyptus patches in substitution to cattle grazing grasslands. This work aims to recognize the modifications caused by the insertion of this new economical cycle in MPSRV landscape mosaic. The study area is located between Mar and Mantiqueira range, including Sesmarias, Barreiro de Baixo and Bananal drainage basins, where previous studies have been conducted. A headwater zone of a first order drainage basin in Sesmarias basin was chosen in 2006 to measure Eucalyptus plantations hydrological responses to biota-soil-water interactions. Two use and cover maps (2000 and 2007 years) were made using Landsat-7 and Landsat-5 images,...
Tipo: Article
Palavras-chave: Eucalyptus; Landsat; Fragmentos florestais; Gramíneas; Uso e cobertura; Dinâmica da paisagem.
Ano: 2007
URL: http://hdl.handle.net/2315/122

Diagnóstico do escoamento superficial urbano no Parque Residencial Beira Rio I no município de Guaratinguetá, SP
Provedor de dados: 25
Autores: Siqueira, Meire Regina de Almeida; Targa, Marcelo dos Santos; Batista, Getulio Teixeira; Dias, Nelson Wellausen.
This work had the objective of analyzing the flooding events that frequently affect the Parque Residencial Beira Rio I neighborhood, in the municipality of Guaratinguetá, Rio Paraíba do Sul Valley, state of São Paulo. This study has shown that this neighborhood has an area of 330,000m², a population of 1,361 inhabitants, a sloping area without vegetation cover facing the residential area, an open drainage system of 0.60m diameter tubes, several open points that captures the water that descends from the sloping area allowing sediment loaded water to enter the tubes, residential area located in a low plain area, cemented curbs and lawn yards and crossroads with round lawns located in higher level than the drainage system. Lowering the level of those lawn...
Tipo: Article
Palavras-chave: Sustentabilidade da drenagem urbana; Low impact development; Escoamento superficial.
Ano: 2007
URL: http://hdl.handle.net/2315/79

PLANO DIRETOR PARA O SETOR RURAL DO MUNICÍPIO DE PINDAMONHANGABA, SP
Provedor de dados: 25
Autores: Batista, Getulio; Targa, Marcelo; Dias, Nelson.
A Constituição do Estado de São Paulo, em consonância com Constituição Federal, estabeleceu no seu artigo 181 a obrigatoriedade da elaboração do plano diretor em todos os municípios, ressaltando inclusive, a necessidade desse plano abranger a totalidade do território municipal, ou seja, tanto o setor urbano quanto o rural. (CONSTITUIÇÃO, 1989). Deve-se ressaltar a importância da parceria do Poder Público de Pindamonhangaba com a Universidade de Taubaté, por ser a mais próxima universidade repositória de conhecimentos agrícola da região ao manter serviços de ensino, pesquisa e extensão rural associados ao curso de Agronomia por mais de vinte anos de funcionamento. Em adição, há mais de cinco anos, a UNITAU, implementou um laboratório de geoprocessamento, o...
Tipo: Other
Palavras-chave: Diagnóstico municipal; Zoneamento municipal.
Ano: 2007
URL: http://hdl.handle.net/2315/126

Respostas fisiológicas de dois clones de eucalipto submetidos a diferentes potenciais  hídricos
Provedor de dados: 25
Autores: Tonello, Kelly Cristina; Teixeira Filho, José.
For the growth, development and hydrology of Eucalyptus plantation understanding, it’s necessary to know the factors that control the water flows. Aiming to improve hydrologic models of water balance on basins with planted forests, this work evaluates transpiration behavior and leaf water potential in two eucalyptus clones. Leaf water potential (Ψb) and climatic parameters had been related to foliar transpiration (E). In general, the changes with Ψb minor had shown to minor variation and throughout the day. One noticed behavior differentiated between the two clones in reply to the Ψb, total incident radiation (RIT) and vapour pressure deficit (DPVS). Clone A presented E average 76% greater in -0,5MPa when compared with clone B, indicating highest...
Tipo: Article
Palavras-chave: Ecofisiologia vegetal; Balanço hídrico; Hidrologia; Transpiração.
Ano: 2007
URL: http://hdl.handle.net/2315/112

Banco de Dados Ambientais da Bacia do Rio Una, Bacia do Rio Paraíba do Sul
Provedor de dados: 25
Autores: Batista, Getulio Teixeira; Targa, Marcelo dos Santos; Fidalgo, Elaine C. C.
Trabalho técnico de pesquisa sobre a criação de um banco de dados ambientais, georreferenciado.
Tipo: Article
Palavras-chave: Uso da Terra; APP; Áreas de Preservação Permanente; Vulnerabilidade ambiental; Ortorretificação; Mapa de declividade.
Ano: 2006
URL: http://hdl.handle.net/2315/51

MUDANÇA DO USO E OCUPAÇÃO DO SOLO NA SUB BACIA DO BAIXO E MÉDIO UNA NO PERÍODO DE 2003 A 2010
Provedor de dados: 25
Autores: Alves, Tatiane; Batista, Getulio T.
Esse trabalho objetivou analisar a sub-bacia do Baixo e Médio Una - SP, em duas datas 2003 e 2010, utilizando técnicas de análise de imagens e geoprocessamento utilizando o aplicativo SPRING (Sistema de Processamento de Informações Georreferenciadas) para a estimativa da área e localização dos diversos visando uma avaliação das mudanças ocorridas em função do uso dessa área. Utilizando o banco de dados disponível no Projeto Una contendo informações de 2003 e resultados da análise de dados do Landsat TM de 2010 foram avaliadas a extensão das áreas que se modificaram ao longo desses sete anos analisados. Constatou-se que houve aumento significativo da área urbanizada e, por outro lado a área reflorestada também teve aumento neste mesmo período. As análises...
Tipo: Article
Palavras-chave: Bacia Hidrográfica; Sensoriamento Remoto; Uso da Terra; SIG.
Ano: 2011
URL: http://hdl.handle.net/2315/165

Diagnostico geomorfológico en cuencas hidrográficas precordilleranas: Río de la Ciénaga. Departamento Zonda, Provincia de San Juan, República Argentina
Provedor de dados: 25
Autores: Montenegro, Elvira Aideé Suarez.
The results exposed in the present work are framed in the activities of Internal Scholarship of CONICET that is developed in the Institute of Geography Applied in National San Juan University. The General Objective of the investigation work was based on application of the systemic approach, for the analysis of natural systems of “precordilleranas” hydrographic river basins. In this case it was chosen like object focused to the geomorphologic object. Satellite Techniques, Manual and Digital Mapping with ITC Symbol, Direct Wide Observations and SIG with Software Ilwis 3.3 Were used . It was selected as study unit the area drained by the river, that is located in Central Precordillera of San Juan Province, in virtue to fort influences new tectonics,...
Tipo: Article
Palavras-chave: Natural System; Geomorphology; Diagnosis.
Ano: 2007
URL: http://hdl.handle.net/2315/114

Resíduos sólidos na Estação Antártica Brasileira
Provedor de dados: 25
Autores: Ribeiro, Kelly; Ferreira, Willian; Batista, Getulio; Targa, Marcelo.
Artigo apresentado no XVI ENIC UNITAU, 2011. P.1-11.
Tipo: Article
Palavras-chave: Sistema de Gestão; Resíduos; Antártica; Waste.
Ano: 2012
URL: http://hdl.handle.net/2315/233

Parasitic Effects of Varroa destructor (Acari: Varroidae) on Hypopharyngeal Glands of Africanized Apis mellifera (Hymenoptera: Apidae)
Provedor de dados: 25
Autores: Pinto, Fábio de Assis; Souza, Gabriely Köerich; Sanches, Marcia Aparecida; Serrão, José Eduardo.
The mite Varroa destructor (Anderson &amp; Truemann 2000) (Acari: Varroidae) is one of the most studied parasites of Apis mellifera, as it causes many losses in apicultural business worldwide. Several research studies have demonstrated distinct levels of virulence of the mite and increased colony mortality rates due to its infestation; however only a few studies report the mite's effects on specific tissues, glands or other organs in bees. In this context, this study was conducted with the aim of studying the parasitic effect of the mite V. destructor on hypopharyngeal glands of Africanized A. mellifera. Mean gland cell areas for bees with and without mite infestations were significantly different. Variations in the number of vesicles and the presence of...
Tipo: Article
Palavras-chave: Apis mellifera; Parasitism; Hypopharyngeal glands; Varroosis; Varroa destructor.
Ano: 2011
URL: http://hdl.handle.net/2315/272

COMPARAÇÃO DOS NÍVEIS DE EMISSÃO DE RADIAÇÃO NA FAIXA DO INFRAVERMELHO TERMAL ENTRE MACIÇOS FLORESTAIS DE EUCALIPTO E DE MATA NATIVA UTILIZANDO DADOS DO INFRAVERMELHO TERMAL
Provedor de dados: 25
Autores: Catelani, Celso de Souza; Batista, Getulio Teixeira.
Resumo  As lacunas técnicas presentes nas acirradas discussões entre representantes da indústria de papel e celulose, a sociedade civil, organizações não governamentais e os órgãos fiscalizadores da legislação ambiental brasileira acerca da perda direta da disponibilidade hídrica em conseqüência da implantação de maciços florestais de eucalipto em uma área situada na região sudeste do Brasil, denominada Vale do Paraíba, no Estado de São Paulo, em especial os dados sobre a evaporação e a evapotranspiração potencial determinam a necessidade de respostas científicas sobre os fatores associados a esse tipo de monocultura que podem influenciar ou colocar em risco a preservação dos recursos hídricos dessa região. O uso de aplicações estado da arte do...
Tipo: Other
Palavras-chave: Infravermelho termal; Thermal infrared; ASTER; Water use conflict.
Ano: 2006
URL: http://hdl.handle.net/2315/48

ANÁLISE DO USO E OCUPAÇÃO DO SOLO NA MICROBACIA DOM TOMAZ NO MUNICÍPIO DE TRÊS LAGOAS - MS
Provedor de dados: 25
Autores: Silva, Laís Coêlho do Nascimento; Fernandes, André Luís Valverde; Oliveira, Wallace de.
The draining basins possess important paper in the landscape, therefore they are its modellers. For natural causes or mainly antrópicos factors, the disequilibrium of the basins have been accented gradual. The disordered occupation in the basin accents such disequilibria in the ground. Amongst the activities that cause degradation, the practical agriculturists, superpastoreiro and reforestation can be cited. For conservation of the ground the preservation will have to be understood and the development, in order to provide the greater for the biggest number and for the biggest period of time of the natural resources of renewable character well, which is the ground, the forests, the pastures, wild fauna e, in certain extension the water. The objective of...
Tipo: Article
Palavras-chave: Images of satellite; Landscape; Remote sensoriamento.
Ano: 2007
URL: http://hdl.handle.net/2315/117

Escoamento superficial de água de chuva no cultivo do eucalipto
Provedor de dados: 25
Autores: Ramos, José Geraldo de Ângelo; Dias, Herly Carlos Teixeira.
Today the preoccupation in if seize better the rain becomes more and more important for sharp of forest plantings. In this project are going to study the behavior of the rain in the soil in eucalyptus plantings. We will be evaluating the behavior of the terrace in eucalyptus planting. The obtained data in this project will show us the important of the terrace for sharp of forest plantings as the of the eucalyptus.
Tipo: Article
Palavras-chave: Escoamento superficial; Eucalipto.
Ano: 2007
URL: http://hdl.handle.net/2315/121

Programa de Microbacias: contribuição do planejamento de propriedades rurais para a ocupação sustentável da Bacia do Paraíba do Sul
Provedor de dados: 25
Autores: Ferreira Neto, Jovino Paulo; Martinelli, Marcos.
Programa estadual de microbacias hidrográficas do Estado de São Paulo. Planejamento Individual de Propriedades Rurais. Extensão Rural.
Tipo: Presentation
Palavras-chave: CATI; Desenvolvimento rural; Extensão rural.
Ano: 2007
URL: http://hdl.handle.net/2315/135

EXPERIÊNCIA PEDAGÓGICA NA CONSTRUÇÃO DE ITINERÁRIOS CULTURAIS REGIONAIS
Provedor de dados: 25
Autores: Cocco, Maria Dolores Alves; Vierno, Fernanda Moura; Perim, Marli Aparecida.
A experiência pedagógica baseada na Carta Internacional dos Itinerários Culturais, CIIC (ICOMOS, 2008) teve como objetivo principal identificar e conectar acontecimentos históricos a forma de ocupação do homem sobre o território do vale do Paraíba(SP).
Tipo: Article
Palavras-chave: Região metropolitana; Vale do Paraíba.
Ano: 2014
URL: http://hdl.handle.net/2315/275

Florestas &amp; Crédito Carbono
Provedor de dados: 25
Autores: Batista, Getulio Teixeira.
Palestra em formato pdf com 44 slides sobre mudanças climáticas e efeito estufa e as possibilidades do mercardo de carbono para o Brasil. Fontes de emissão e o papel das florestas na mitigação do efeito estufa.
Tipo: Presentation
Palavras-chave: Mudanças climáticas; Efeito estufa; Mercado de carbono; Protocolo de Quioto.
Ano: 2008
URL: http://hdl.handle.net/2315/141

Impacto das Cheias e a Necessidade de um Plano de Macrodrenagem
Provedor de dados: 25
Autores: Targa, Marcelo Santos.
Essa palestra em formato pdf foi realizada em uma atividade do evento " 1ª Semana do Ambiente da Universidade de Taubaté - UNITAU" - mesa redonda intitulada " Gestão de bacias Hidrográficas: O estudo de caso do rio Una" feita pelo Programa de Pós-Graduação em Ciências Ambientais da Universidade de Taubaté para alunos dos cursos de graduação em Geografia, Engenharias Ambiental e Civil, Agronomia e Biologia. Vários slides se referem a junção das condições climáticas, antrópicas e do meio físico para  ilustrar a degradação e os problemas inerentes a macrodrenagem e as cheias do rio Una.
Tipo: Presentation
Palavras-chave: Macrodrenagem; Cheias; Erosão; Água.
Ano: 2009
URL: http://hdl.handle.net/2315/151

Tratamento de efluentes por leito cultivado: Sistema para pequenas comunidades
Provedor de dados: 25
Autores: Santos, Roberto José dos; Fortes Neto, Paulo; Batista, Getulio Teixeira.
Resumo: A pesquisa teve como base o trabalho de campo desenvolvido nas dependências do Viveiro de Plantas Municipal de Jacareí, Estado de São Paulo, Brasil. Foi projetado um sistema constituído por fossa séptica e leito cultivado, com objetivo de solucionar os problemas dos esgotos gerados pelas comunidades rurais e das periferias de áreas urbanas. O sistema foi dimensionado para fazer o tratamento de esgotos gerado por 40 pessoas, funcionários e visitantes. O projeto é constituído de duas unidades, fossa séptica e leito cultivado. O efluente gerado na fossa séptica foi direcionado para o leito cultivado, formado por duas camadas, uma de brita e outra, de areia, sendo que na camada de brita foram plantadas 50 mudas de espécie Zantedeschia aethiopica L. O...
Tipo: Article
Palavras-chave: Coliformes; Efluentes; Esgoto doméstico; Leito cultivado; Domestic sewage; Effluents.
Ano: 2011
URL: http://hdl.handle.net/2315/177

A QUESTÃO AMBIENTAL: FLORESTAS E BIODIVERSIDADE
Provedor de dados: 25
Autores: Bertolino, Maria Lúcia.
This work has as objective to argue the environmental question concerning the conservation of the forests and biodiversity. One major issue in this question is that the Brazilian forest sector contributes with an important parcel for the Brazilian economy, generates products for direct consumption or for exportation, generates taxes and jobs for the population and, still, bring positive and negative consequences in the conservation and preservation of both renewable and not renewable natural resources. The forest economy has been, historically, responsible for one of the five largest positive commercial balances of the country and still it supplies 85% of all the products of forest origin found in the national market, therefore, alleviating the pressure on...
Tipo: Article
Palavras-chave: Preservation; Biodiversity; Forests.
Ano: 2007
URL: http://hdl.handle.net/2315/106

ROTEIRO PARA A IMPLANTAÇÃO E OPERACIONALIZAÇÃO DO PLANO DE GESTÃO DE RESÍDUOS PARA INSTITUIÇÕES DE ENSINO
Provedor de dados: 25
Autores: Fortes Neto, Paulo Fortes Neto.
O plano para o gerenciamento de resíduo gerado pela comunidade acadêmica da Universidade de Taubaté, hora denominado de “UNITAU RECICLANDO” tem como objetivo, coletar todo resíduo, buscar alternativas de tratamentos, depositar adequadamente o resíduo, fazer campanhas, implantar programas educacionais e incentivar medidas para diminuir a geração de resíduos na fonte geradora.  O “UNITAU RECICLANDO” irá estabelecer um conjunto de recomendações e procedimentos para o gerenciamento dos resíduos, tendo como base, a identificação e classificação dos resíduos, a seleção das alternativas adequadas para o tratamento e destinação  final, a documentação e registro dos aspectos relacionados ao processo de coleta, tratamento e destinação e o cumprimento de todas as...
Tipo: Technical Report
Palavras-chave: Gestão de residuos.
Ano: 2012
URL: http://hdl.handle.net/2315/262

Erosion due to rural roads: a case study in the Una River Basin, Taubaté, SP, Brazil
Provedor de dados: 25
Autores: Batista, Getulio Teixeira; Catelani, Celso de Souza; Targa, Marcelo dos Santos; Dias, Nelson Wellausen.
Aceito para apresentação como poster, no IWA World Water Congress, Vienna, 7-12 set 2008. (reference number:666237).
Tipo: Article
Palavras-chave: River sedimentation; GIS; Roads; Erosion.
Ano: 2008
URL: http://hdl.handle.net/2315/142

Agricultura Familiar Sustentabilidade Social e Ambiental
Provedor de dados: 25
Autores: Mello, Roxane Lopes.
Artigo desenvolvido na disciplina de Desenvolvimento Sustentável do curso de mestrado em Ciências Ambientais da UNITAU sobre o conceito de Desenvolvimento Sustentável é questionado, dentre outros argumentos, em função da dificuldade em se determinar a sustentabilidade de um sistema. O presente estudo procurou realizar uma leitura associada à agricultura familiar e à questão da sustentabilidade ambiental e social da agricultura familiar. A escolha da agricultura familiar está relacionada com multifuncionalidade da agricultura familiar, que além de produzir alimentos e matérias-primas, gera mais de 80% da ocupação no setor rural, responde no Brasil por sete de cada 10 empregos no campo e por cerca de 40% da produção agrícola. Atualmente a maior parte dos...
Tipo: Article
Palavras-chave: Desenvolvimento Sustentável; Agricultura Familiar; Ambiente.
Ano: 2007
URL: http://hdl.handle.net/2315/137

Análise temporal e espacial da qualidade da água na bacia hidrográfica do Zerede, Timóteo-MG
Provedor de dados: 25
Autores: Coluna, Naraisa Moura Esteves; Dias, Herly Carlos Teixeira; Pinheiro, Joana Angélica Cavalcanti.
A água é fundamental à manutenção da vida, sendo um recurso de múltipla utilização. A qualidade da água depende das condições naturais e da ocupação do solo na bacia hidrográfica.. Este trabalho teve como objetivo avaliar a qualidade físico-química da água da bacia hidrográfica do córrego Zerede, MG. As análises foram realizadas no Laboratório do Meio-Ambiente- LCP, UFV/Viçosa. Os parâmetros avaliados foram pH, condutividade elétrica (Ce), OD (oxigênio dissolvido), DQO (demanda química de oxigênio). De acordo, com a caracterização físico-química efetuada nesse trabalho, pode-se concluir que a qualidade da água está nos padrões da Resolução CONAMA 357 enquadrando nas classes especial e classe I.
Tipo: Article
Palavras-chave: Demanda química de oxigênio; Qualidade da água; Oxigênio dissolvido.
Ano: 2007
URL: http://hdl.handle.net/2315/101

PERSPECTIVAS DE PRODUÇÃO E USO DO BIOQUEROSENE DE AVIAÇÃO NO TRANSPORTE AÉREO BRASILEIRO
Provedor de dados: 25
Autores: Edison, S. Paiva; Pedro, H. R. Santos; Pedro, C. Russi; Getulio, T. Batista; Willian, J. Ferreira.
Trabalho submetido e apresentado no III CICTED, Taubaté, 2014.
Tipo: Presentation
Palavras-chave: Bioenergia; Aeronáutica; Sustentabilidade; Pinhão Manso.
Ano: 2014
URL: http://hdl.handle.net/2315/282

Análise de impactos ambientais gerados pela construção de uma barragem na Bacia do Médio Una, Taubaté, SP
Provedor de dados: 25
Autores: Silva, Silas Siqueira da; Batista, Getulio Teixeira; Targa, Marcelo dos Santos; Dias, Nelson Wellausen.
Based on data available from the Una Project (www.agro.unitau.br/una) this article reports results on the analysis of the impact of a planned dam implantation in the medium Una River, municipal district of Taubaté, SP, especially it presents: mapping and estimate of the flooded area and expected volume of the dam; analysis of permanent preservation areas APPs) before and after the dam and amount of forests flooded by the water; analysis of the land cover on the new APPs created by the implantation of the dam according to the Brazilian forest code and related regulations. An analysis of all the contributing area is presented.
Tipo: Article
Ano: 2007
URL: http://hdl.handle.net/2315/75

Cobrança pelo Uso da Água A Situação da Bacia do Paraíba do Sul
Provedor de dados: 25
Autores: Campos, Jander Duarte.
COBRANÇA NO CÓDIGO DE ÁGUAS DE 1934  Estabelece que: O uso comum das águas pode ser gratuito ou retribuído, conforme as leis e regulamentos da circunscrição administrativa a que pertencem (art. 36, §1º e § 2º). A ninguém é lícito conspurcar ou contaminar as águas que não consome, com prejuízo para terceiros (art. 109), ressaltando que os trabalhos de salubridade das águas serão realizados à custa dos infratores que, além da responsabilidade criminal, se houver, responderão pelas perdas e danos que causarem e por multas que lhes forem impostas pelos regulamentos administrativos (art. 110, CA).
Tipo: Presentation
Palavras-chave: Gestão de recursos hídricos; Recuperação de áreas degradadas; Uso da água.
Ano: 2007
URL: http://hdl.handle.net/2315/127

Fusion of High Spatial Resolution with Extended Spectral Resolution Bands of CBERS Satellite Sensors for Land Use Survey
Provedor de dados: 25
Autores: Batista, Getulio Teixeira; Catelani, Celso de Souza.
Trabalho aceito para apresentação no 2nd. International Conference on Computing, Communication and Control Technologies: CCCT'04
Tipo: Article
Palavras-chave: Image Analysis; Remote Sensing.
Ano: 2004
URL: http://hdl.handle.net/2315/147

O emprego do Geoprocessamento na Análise Espacial da Bacia Hidrográfica do Córrego Guariroba, Campo Grande – MS
Provedor de dados: 25
Autores: Yamaciro, Raony Moreira Gomes.
The present study aimed to use Geoprocessing techniques applied to basin management. The study area was the Guariroba microbasin in Campo Grande city - MS. Using the Digital Terrain Model, from EMBRAPA website, topographical data were extracted in Arcgis environment, a TIN grade was generated and from its, a hypsometric map and a three-dimensional declivity map. The land use/cover was also mapped, using a CBERS image and the MAXVER algorithm in ERDAS environment. The Guariroba basin presents low levels of declivity, with fragments of native vegetation and high degree of degradation, distributed in 24 % of the total of the area of the basin.
Tipo: Article
Palavras-chave: Geoprocessing; Bacia Hidrográfica; Digital Terrain Model.
Ano: 2007
URL: http://hdl.handle.net/2315/89

Estudo Integrado de Bacias Hidrográficas através de Técnicas de Sensoriamento Remoto e Geoprocessamento visando o Uso Sustentável e Programas de Recuperação de Áreas Degradadas no Vale do Paraíba
Provedor de dados: 25
Autores: Batista, Getulio Teixeira.
Avaliar e quantificar os impactos positivos da recuperação ambiental em bacias hidrográficas, através da medição da variação da disponibilidade hídrica, estabelecendo a variabilidade da depleção hidrológica na bacia em períodos de estiagem, como parâmetro hidrológico a ser monitorado para avaliação de diferentes condições de preservação ambiental.
Tipo: Article
Palavras-chave: Depleção hidrológica; Degradação; Manejo de bacias; Conservação de recursos hídricos.
Ano: 2006
URL: http://hdl.handle.net/2315/56

IPABHi - Intituto de Pesquisas Ambientais em Bacias Hidrográficas
Provedor de dados: 25
Autores: Dias, Nelson W.
Desenvolver estudos e pesquisas destinadas a elaborar, testar, avaliar e implementar estratégias que viabilizem formas sustentáveis de uso dos recursos naturais inseridos no contexto geográfico de bacias hidrográficas, em especial os fatores determinantes da qualidade e quantidade de água, com o objetivo de otimizar processos de preservação e conservação do meio ambiente e promover atividades humanas, econômicas e ambientais, orientadas ao desenvolvimento sustentável.
Tipo: Presentation
Palavras-chave: IPABHi; Recursos Hídricos; SERHIDRO-PS.
Ano: 2007
URL: http://hdl.handle.net/2315/128

Avaliação do escoamento superficial e infiltração de água em solo cultivado com Pinhão Manso consorciado à pastagem degradada no Vale do Paraíba/SP
Provedor de dados: 25
Autores: Ferreira, W. J.; Batista, G. T.; Targa, M. S.
Material apresentado IV ECOSP e VIII ECOVALE/2010.
Tipo: Presentation
Palavras-chave: Energia renovável; Biodiesel; Balanço hídrico; Sustentabilidade.
Ano: 2010
URL: http://hdl.handle.net/2315/280

Modelos para prognósticos da umidade relativa do ar em escala horária no município de Muriaé, MG
Provedor de dados: 25
Autores: Delgado, Rafael Coll; Sediyama, Gilberto Chohaku; Andrade, Ricardo Guimarães; Menezes, Sady Júnior Martins da Costa de.
Three physical-mathematical models were appraised starting from data of temperature of the air for the estimate of the relative humidity of the air for the area of Muriaé, MG. The estimates were compared with data obtained in the automatic station during the period of three months (10/09/2006 to 10/12/2006). The results of the models of relative humidity of the air presented determination coefficients (r2) high when compared with the observed values, the model that more it was adjusted to the analyzed data was the model UR2, that has as entrance variables the temperature of the hourly dew point, hourly minimum temperature and the hourly medium temperature.
Tipo: Article
Palavras-chave: Relative humidity of the air; Temperature of the air.
Ano: 2007
URL: http://hdl.handle.net/2315/113

Avaliação do comportamento da água no solo sob cobertura vegetal de eucalipto e pastagem dentro de um ciclo
Provedor de dados: 25
Autores: Rodrigues, Neyrianne; Melo, Walkiria; Targa, Marcelo; Batista, Getulio.
Artigo apresnetado no XVI ENIC UNITAU, 2011. P.1-10
Tipo: Article
Palavras-chave: Tensiômetro; Tensiômetro; Uso da água; Water infiltration.
Ano: 2012
URL: http://hdl.handle.net/2315/234

Evolução do Programa de Aquisição de Alimentos, operacionalizado pela CONAB.
Provedor de dados: 25
Autores: Travinski, Dannyel Arid.
O histórico de exclusão social no campo e na cidade é muito antigo, sendo necessárias políticas públicas para combater essa dura realidade. Problemas de segurança alimentar, miséria rural e urbana, que geram inúmeros problemas sociais. O presente trabalho faz uma reflexão sobre o Programa de Aquisição de Alimentos, desde sua criação, até os números atuais, passando pelas suas normas, ferramentas, gestores, não esquecendo de como ele foi criado e por quem foi e para quem foi criado. O Programa de Aquisição de Alimentos - o PAA, instituído pelo Art. 19 da Lei n. 10.696, de 02 de julho de 2003, e regulamentado pelo Decreto n. 6.447, de 07 de maio de 2008, tem por objetivo incentivar a agricultura familiar, por meio da aquisição de alimentos de agricultores...
Tipo: Thesis
Palavras-chave: Agricultura familiar; CONAB; Programa de Aquisição de Alimentos.
Ano: 2010
URL: http://hdl.handle.net/2315/158

Caracterização física da bacia hidrográfica do ribeirão Serragem, Tremembé/SP, por meio de geotecnologias
Provedor de dados: 25
Autores: Rodrigues, neyrianne; Targa, Marcelo; Batista, Getulio.
Apresentado no XVI ENIC UNITAU, 2011.
Tipo: Article
Palavras-chave: Geotecnologies; Basin physical characterization.
Ano: 2012
URL: http://hdl.handle.net/2315/235

Hidrogramas para a bacia hidrográfica do ribeirão Serragem no município de Tremembé, SP
Provedor de dados: 25
Autores: Targa, Marcelo dos Santos; Batista, Getulio Teixeira; Mostarda Neto, Nazareno; Maria Filho, Paulo José.
O presente trabalho objetivou determinar os Hidrogramas de Precipitações Efetivas Máximas a partir do método do Hidrograma Unitário (HU) da bacia do Ribeirão Serragem no município de Tremembé, SP no vale do Paraíba do Sul, localizada na parte a montante da barragem da Fazenda Maristela. Foram empregadas técnicas de geoprocessamento com o uso de ferramentas do SPRING para a caracterização do uso e ocupação do solo e caracterização física da bacia para o cálculo da Precipitação efetiva (Pe) resultante de chuvas máximas sobre a bacia simuladas para 2, 5, 10, 15, 20, 25, 50, 100 e 200 anos. O cálculo da Pe foi realizado pelo método do Curva Número (CN). Os resultados indicaram que a bacia do Ribeirão Serragem apresenta um bom estado de conservação, levando em...
Tipo: Article
Palavras-chave: Bacia; Ciências ambientais; Escoamento; Uso do solo; Basin; Environmental science; Land use; Water flow.
Ano: 2015
URL: http://hdl.handle.net/2315/284

Ocupação do solo urbano: Desafios pós Estatuto das Cidades
Provedor de dados: 25
Autores: Batista, Getulio Teixeira; Dias, Nelson Wellausen.
Pre-Print de capítulo do Livro: Uma agenda para a sustentabilidade regional: Reflexão e ação - Parte II: Desafios. Tópicos do Capítulo:  1. Situação do uso do solo urbano no Brasil, em especial da Região do Vale do Paraíba Paulista. 2. Revisão da legislação sobre o uso do solo – Inovações Estruturais do “Estatuto da Cidade”. 3. Realidade urbana versus legislação vigente. 4. Desafios para a efetiva implementação do “Estatuto da Cidade” - Em que medida os membros da sociedade (civil e governo) estão preparados para a “maioridade” sugerida pelo Estatuto? 5. Desafios para a definição de indicadores ambientais que permitam uma avaliação constante da sustentabilidade do processo de urbanização envolvendo aspectos econômico-sociais. 6. Considerações finais 7....
Tipo: Book chapter
Palavras-chave: Participação popular; Urbanização.
Ano: 2008
URL: http://hdl.handle.net/2315/146

Histórico e Sustentabilidade da Bacia Hidrográfica do Paraíba do Sul: Geoprocessamento e Hidrologia
Provedor de dados: 25
Autores: Batista, G. T.; Targa, M. S.
Apresentado na forma de seminário no Encontro de Iniciação Científica da Universidade de Taubaté em ATIVIDADES ACADÊMICAS, CULTURAIS e CIENTÍFICAS | ENIC | MPG | SEMEX Para alunos, professores, pesquisadores e comunidade em geral, na 4ª FEIRA - DIA 17 DE OUTUBRO de 2012.
Tipo: Presentation
Palavras-chave: Sensoriamento remoto; Hidrologia; Recursos hídricos; Bacia hidrográfic.
Ano: 2012
URL: http://hdl.handle.net/2315/251

Estudo do Comportamento Espectral das Principais Classes de Cobertura d Solo do Vale do Paraíba e Relação com o Índice de Área Foliar
Provedor de dados: 25
Autores: Batista, Getulio.
Proposta de pesquisa para suporte à Iniciação Científica.
Tipo: Article
Palavras-chave: Sensoriamento Remoto; Remote Sensing; Espectroscopia; Comportamento espectral; Radiometria de campo; Radiometer.
Ano: 2006
URL: http://hdl.handle.net/2315/45

Primeiro Seminário de Recursos Hídricos da Bacia Hidrográfica do Paraíba do Sul: Cultivo de Eucalipto e o Ciclo Hidrológico (1º SERHIDRO-PS 2007)
Provedor de dados: 25
Autores: Batista, Getulio Teixeira.
Esse primeiro evento com foco principal na questão do eucalipto e ciclo hidrológico permitiu aumentar o conhecimento e diminuir a polêmica relacionada com o crescimento do plantio do eucalipto na região. A expansão das áreas plantadas com eucalipto no Vale do Paraíba vem acompanhada de reações de natureza diversa, algumas com credibilidade técnica, outras não. Portanto, fêz-se necessário estabelecer mecanismos de interação e discussão técnica que possibilitaram avaliar os reais impactos da silvicultura do eucalipto na região. Dessa forma, esse evento foi organizado como uma mesa de discussão, com a participação de agências governamentais e da iniciativa privada, capaz de prover informações para elucidação desse conflito.
Tipo: Technical Report
Palavras-chave: Evento; Eucalipto.
Ano: 2008
URL: http://hdl.handle.net/2315/148

EFEITOS HIDROLÓGICOS DO MANENO DE FLORESTAS PLANTADAS COM EUCALIPTO
Provedor de dados: 25
Autores: Lima, Walter de Paula.
Eucalipto e água: a controvérsia continua viva! “O eucalipto seca o solo?” “Secou a minha nascente!” “O eucalipto fará o Jequitinhonha de São Paulo!” “O Espírito Santo será um imenso deserto verde”  “Tenebroso anúncio de massivas plantações de eucalipto!” Projetos de Lei em Assembléias Legislativas e Câmaras de Vereadores As mulheres da via campesina! “Nós não comemos eucalipto”
Tipo: Presentation
Palavras-chave: Manejo florestal; Eucalipto x água; Impactos ambientais; Balanço hídrico.
Ano: 2007
URL: http://hdl.handle.net/2315/134

ANÁLISE ESPACIAL DA EVOLUÇÃO DA MANCHA URBANA NO MUNICÍPIO DE GUARATINGUETÁ
Provedor de dados: 25
Autores: Bassanelli, Hélio Rodrigues; Batista, Getulio T.
Artigo vinculado ao Trabalho de Conclusão da Disciplina Fundamentos Epistemológicos da Sustentabilidade.
Tipo: Article
Palavras-chave: Crescimento urbano; SIG; Sustentabilidade; Geotecnologias.
Ano: 2011
URL: http://hdl.handle.net/2315/170

Biodiesel no Vale do Paraíba: a Jatropha como agente do desenvolvimento sustentável
Provedor de dados: 25
Autores: Ferreira, Willian J.; Batista, Getulio T.
Ferreira, W. J.;Batista, G. T. Biodiesel no Vale do Paraíba: a Jatropha como agente do desenvolvimento sustentável. 2010, 15p.
Tipo: Presentation
Palavras-chave: Bioenergia; Pinhão manso; Biocombustíveis; Sustentabilidade; Uso do solo; Carbono.
Ano: 2010
URL: http://hdl.handle.net/2315/154

Capacitação em gestão de recursos hídricos por educação a distância na bacia do rio Paraíba do Sul: a experiência da UNITAU
Provedor de dados: 25
Autores: Targa, Marcelo; Dias, Nelson; Batista, Getulio.
Apresentado no XIX Simpósio Brasileiro de Recursos Hídricos, Maceió, 2011.
Tipo: Article
Palavras-chave: Gestão; Recursos hídricos; Especialização a distância.
Ano: 2012
URL: http://hdl.handle.net/2315/244

Formigas (Hymenoptera, Formicidae) Associadas a Ninhos de Cornitermes cumulans (Kollar) (Isoptera, Termitidae) no Cerrado do Planalto Central do Brasil
Provedor de dados: 25
Autores: Gallego-Ropero, María Cristina; Feitosa, Rodrigo Machado; Pujol-Luz, Jose Roberto.
Resumo. Com o objetivo de conhecer a fauna de formigas que coabita os cupinzeiros de Cornitermes cumulans (Kollar) no Cerrado sensu stricto do Brasil Central, foram realizadas coletas em 36 cupinzeiros em três localidades. Os cupinzeiros foram fragmentados e o material coletado foi armazenado em frascos com álcool a 80%. Apresentamos aqui uma lista das formigas associadas aos cupinzeiros de C. cumulans. Um total de 61 espécies distribuídas em nove subfamílias e 32 gêneros foi coletado. A subfamília Myrmicinae apresentou o maior número de gêneros (15) e de espécies (22). Estes resultados indicam que ninhos de cupins são importantes recursos de nidificação para várias espécies de formigas no Brasil Central.  Abstract. In order to survey the ant fauna...
Tipo: Article
Palavras-chave: Cupins; Inquilinos; Nidificação; Riqueza de espécies; Inquilines; Nesting resource; Species richness; Termites.
Ano: 2013
URL: http://hdl.handle.net/2315/268

Técnica eletromagnética para o monitoramento ambiental
Provedor de dados: 25
Autores: Souza, Claudinei Fonseca.
Introdução geral  Técnica da TDR  Vantagens e desvantagens  Sondas de TDR  Problemas encontrados  Exemplos de aplicação
Tipo: Presentation
Palavras-chave: Monitoramento ambiental; Sondas de TDR; Técnica eletromagnética.
Ano: 2007
URL: http://hdl.handle.net/2315/129

GPS12. Manual prático de uso e operação. Principais funções e características técnicas
Provedor de dados: 25
Autores: Sauruk, Gilson; Disperati, Attilio Antonio.
É uma breve apresentação do funcionamento do GPS12. Serve como informações iniciais ao estudante. Após a leitura atenta do texto o estudante possuirá uma visão geral das funções técnicas do receptor, mas NÃO dispensa o futuro uso e leitura atenta do manual do aparelho. É um primeiro contacto com o aparelho.
Tipo: Learning Object
Palavras-chave: Recptor GPS; GPS 12; Garmin.
Ano: 2006
URL: http://hdl.handle.net/2315/65

Laboratório de Geoprocessamento Sensoriamento Remoto e Informática Rural
Provedor de dados: 25
Autores: Batista, Getulio Teixeira; Dias, Nelson W.
O Laboratório de Geoprocessamento, Sensoriamento Remoto e Informática Rural (LAGEO) do Departamento de Ciências Agrárias da Universidade de Taubaté desenvolve  projetos na área de geoprocessamento e sensoriamento remoto, através de convênios, parcerias e recursos externos de órgãos financiadores de pesquisas (FAPESP, FEHIDRO, CNPq e outros), a apresentação no Pré-Evento do SERHIDRO-PS 2007 abordará a apresentação de dis projetos realizados:    Projeto Una: ESTRUTURAÇÃO E DISPONIBILIZAÇÃO DO BANCO DE DADOS AMBIENTAIS DA BACIA DO RIO UNA, BACIA DO RIO PARAÍBA DO SUL, desenvolvido com recursos do FEHIDRO, contrato n° 280/2002.   Projeto Recarga: LEVANTAMENTO DAS ÁREAS DE RECARGA E DOS RECURSOS HÍDRICOS SUBTERRÂNEOS DA BACIA DO RIO PARAÍBA DO SUL, NORDESTE DO...
Tipo: Presentation
Palavras-chave: Geoprocessamento; Sensoriamento Remoto; Informática Rural.
Ano: 2007
URL: http://hdl.handle.net/2315/130

Avifauna em florestas tropicais fragmentadas: indicadores da sustentabilidade em Usinas Hidrelétricas
Provedor de dados: 25
Autores: Andrade, Fabiano Timóteo de; Fisch, Simey Thury Vieira; Fortes Neto, Paulo; Batista, Getulio Teixeira.
As florestas tropicais brasileiras em especial a floresta Atlântica e Amazônica foram e continuam sendo alvos constantes de diversas ações antrópicas humanas, que ocasionaram a redução de seus territórios ou ainda sua total fragmentação. Um dos dados mais alarmantes é a perda de sua biodiversidade, que em muitas situações sequer foi conhecida, o que demanda a preocupação com a manutenção sustentável, de forma que várias espécies ainda possam sobreviver. Através de levantamentos na literatura especializada com o tema “o uso de biondicadores na qualidade ambiental em florestas tropicais”, foram elencados os mais utilizados para esse tipo de avaliação com enfoque na avifauna, uma vez que a mesma responde positiva ou negativamente a qualquer fator que altere...
Tipo: Article
Palavras-chave: Fragmentação; Biodiversidade; Ambientes antroporizados; Biodiversity; Fragmentation.
Ano: 2011
URL: http://hdl.handle.net/2315/171

Aspectos Ecológicos de Atta sexdens piriventris Santschi (Hymenoptera: Formicidae) no Município de Capinzal, Santa Catarina, Brasil
Provedor de dados: 25
Autores: Spier, Manuelly Sartori; Spier, Edson Fernando; Dalavéquia, Máira Aparecida; Favretto, Mario Arthur.
Resumo. Entre as espécies de formigas economicamente importantes, devido aos danos que muitas vezes causam à agricultura, as mais significativas são as formigas-cortadeiras por possuírem o hábito de cortar e transportar fragmentos vegetais diversos para os seus ninhos subterrâneos. O objetivo deste estudo foi caracterizar alguns aspectos ecológicos de Atta sexdens piriventris Santschi no município de Capinzal, estado de Santa Catarina, Sul do Brasil. O material de origem vegetal transportado pelas formigas apresentou como característica folhas verdes/frescas 57%, folhas secas 23%, pedaços de frutos 7%, sementes 7% e flores 3%. Já os de origem animal tiveram uma representação de 3%, e eram compostos por pedaços de insetos. A média de distância percorrida...
Tipo: Article
Palavras-chave: Forrageio; Myrmicinae; Ninhos; Substratos; Foraging; Nests; Substrates.
Ano: 2013
URL: http://hdl.handle.net/2315/267

ESTUDO DOS EFEITOS DA APLICAÇÃO DA VINHAÇA NA QUALIDADE DE SOLOS EM CULTIVOS  DE CANA-DE-AÇÚCAR (Saccharum officinarum L.), E O USO DE INDICADORES NO SISTEMA DE PRODUÇÃO.
Provedor de dados: 25
Autores: Rubens Pessoa de Barros, Pedro Roberto Almeida Viégas; Francisco Sandro Rodrigues Holanda.
Este artigo trata de indicadores de sustentabilidade em um sistema de produção com aplicação de vinhaça em solos de cultura de cana-de-açúcar (Saccharum officinarum L.).
Tipo: Article
Palavras-chave: Sustentabilidade-Indicadores-Vinhaça-Agroecossistemas.
Ano: 2008
URL: http://hdl.handle.net/2315/139

Saldo de radiação e fluxo de calor no solo na região do município de Juiz de Fora, MG
Provedor de dados: 25
Autores: Andrade, Ricardo Guimarães; Sediyama, Gilberto Chohaku; Delgado, Rafael Coll; Lima, Evaldo de Paiva; Menezes, Sady Júnior Martins da Costa de.
The techniques of remote sensing have been applied extensively for obtaining the information regarding the management of the natural resources. The SEBAL is an algorithm that has as advantage the capability to estimate the energy fluxes from the soil surface in an effective and economical way. This work was carried out to estimate the radiation balance and the soil heat flux in regional scale by means of the SEBAL algorithm (Surface Energy Balance Algorithm for Land) and Landsat 5 images TM. The estimates of the radiation balance (Rn) and soil heat flux (G) for the 06/07/2003 presented average values in the scene of 548.57 Wm-2 and 47.48 Wm-2, respectively.
Tipo: Article
Palavras-chave: Remote sensing; Fluxo de calor no solo; Balanço de radiação; Sensoriamento remoto; Soil heat flux; Radiation balance.
Ano: 2007
URL: http://hdl.handle.net/2315/123

Benefícios fiscais a veículos poluidores
Provedor de dados: 25
Autores: Penna, Pedro Monteiro Machado de Almeida; Rezende Filho, Cyro de Barros.
O artigo trata do IPVA e princípios constitucionais tributários e ambientais.
Tipo: Article
Palavras-chave: Tributos; Poluição; Ambiental.
Ano: 2011
URL: http://hdl.handle.net/2315/178

Construção de indicadores para cidades sustentáveis.
Provedor de dados: 25
Autores: Cocco, Maria Dolores Alves; Targa, Marcelo dos Santos; Oliveira, José Oswaldo Soares de; Thaumaturgo, Leila Regina Youssef; Guimarães, Eduardo de Souza.
A expansão urbana acarreta impactos ambientais negativos como a destruição da mata ciliar, a crescente impermeabilização do solo, a poluição dos cursos de água, a contaminação dos lençóis freáticos, o assoreamento dos  rios.A relevância deste trabalho está na elucidação das ações antrópicas como forma de construção de indicadores para ações de conservação do meio ambiente.
Tipo: Presentation
Palavras-chave: Ciências ambientais; Bacia hidrografica; Meio ambiente; Soiedade.
Ano: 2014
URL: http://hdl.handle.net/2315/278

Estudo Hidrológico da Bacia do Rio Una: Subsídios para estabelecimento de planos de macrodrenagem no Vale do Paraíba do Sul - SP.
Provedor de dados: 25
Autores: Targa, Marcelo Santos.
O presente trabalho tem como objetivo propor uma metodologia de estudo hidrológico para a bacia do rio Una na região do Vale do Paraíba do Sul, SP com vistas a gerar subsídios para uma futura implantação de plano de macrodrenagem.  Preconiza-se nessa metodologia a realização de campanhas de campo para determinação de vazões e  nível de sedimentos, leitura de instrumentos de monitoramento automático, determinação de características de infiltração dos solos, atividades de laboratório para determinação das propriedades físicas das amostras de solo, coleta de dados em postos meteorológicos, caracterização morfométrica das bacias e atividades relativas ao processamento e integração dos dados. Espera-se com a realização de estudos dessa natureza, conhecer como o...
Tipo: Article
Palavras-chave: Macrodrenagem; Hidrologia.
Ano: 2009
URL: http://hdl.handle.net/2315/149

POTENCIAL DO ARARIBÁ NO DESENVOLVIMENTO DE FITOTERÁPICO: EXTRAÇÃO DE FENOIS E TANINOS TOTAIS
Provedor de dados: 25
Autores: Silva, Roberto Carlos de Sá; Akisue, Gokithi; Coelho, Matheus Diniz Gonçalves; Almeida, Julio Cesar Raposo de; Almeida, Ana Aparecida da Silva.
O desenvolvimento de fitoterápicos inclui várias etapas e processos interdisciplinares e multidisciplinares como a etnobotânica, agronomia, ecologia, química, fitoquímica, farmacologia, toxicologia, biotecnologia, química orgânica, tecnologia farmacêutica até ensaios clínicos. A caracterização de plantas ricas em taninos tem interessado a indústria farmacêutica que busca de fontes de taninos condensados para o tratamento e/ou suplementação da dieta dos ovinos, como métodos de controle de endoparasitas. O objetivo do presente trabalho foi extrair e quantificar as substâncias tanantes presentes nas folhas, na casca e lenho do araribá. Para tanto, extratos etanólicos a 70% de cada parte da planta foram preparados e concentrados e utilizados para a...
Tipo: Other
Palavras-chave: Método de Folin-Ciocalteu; Centrolobium tomentosum; Flavonoides.
Ano: 2012
URL: http://hdl.handle.net/2315/264

Plano de Bacia do Rio Una: Resultados do Projeto Una
Provedor de dados: 25
Autores: Batista, Getulio Teixeira; Targa, Marcelo dos Santos; Catelani, Celso de Souza.
Apresentação feita na Mesa 3 do 14° Seminário G&amp;DR/MCA - Atividades Rurais no Vale do Paraíba - do Ciclo do Café aos Nossos Dias.
Tipo: Presentation
Palavras-chave: Uso da Terra; Vulnerabilidade; Área de Preservação Permanente; Modelo Numérico do Terreno.
Ano: 2006
URL: http://hdl.handle.net/2315/69

Perfurador Eletromecânico de Séptos de Bambu Gigante
Provedor de dados: 25
Autores: Neto, Argemiro Targa; Targa, Marcelo Santos.
Sistema inovador de perfuração eletromecanica de septos de bambu gigante para fabricação de tubos de bambu gigante.
Tipo: Article
Palavras-chave: Drenagem; Perfuração; Tubos; Bambu.
Ano: 2012
URL: http://hdl.handle.net/2315/248

Procedimento para minimização do efeito de alta freqüência resultante de fusão entre bandas TM Landsat e pancromáticas Spot e Quickbird
Provedor de dados: 25
Autores: Sestini, Marcelo Francisco; Ferri, Clotilde Pinheiro.
The image fusion is a technique used to integrate images at different spatial resolutions to obtain better spatial information with spectral characteristics of the targets and is a important tool for environmental studies, including drainage and hydric resources. The IHS transformation is a technique used for to integrate images of different spatial resolution, but the resultant images presents redundant areas enhancement, due to abrupt transitions caused to high tonal variations. In this study, a procedure is described which aims to smooth the spatial high frequency areas and to improve the image quality, reducing the footprint by low pass filters. The study area is Igaratá and Jacarei cities, in São Paulo State, and and was applied a merge of Landsat TM...
Tipo: Article
Palavras-chave: IHS transformation; Fusão de imagens; Remote sensing; Image processing; Image fusion; Sensoriamento remoto; Processamento de imagens; Transformação IHS.
Ano: 2007
URL: http://hdl.handle.net/2315/77

Uso do geoprocessamento na qualidade de água superficial destinada ao abastecimento humano no Estado de Rondônia
Provedor de dados: 25
Autores: Lima, Maria Lucilene Alves de.
The use of geoprocessing has become a more important tool to map areas with substance concentrations above the patterns that may affect the quality of the water. The objective of such study was to evaluate the quality of the superficial waters of the rivers in Rondônia used for to the supplying. Through the espace measurement of the color and turbidity isoconcentration it was inferred that the quality of the waters are in agreement with the maximum limits allowed by the resolution of CONAMA n. 357/05.
Tipo: Article
Palavras-chave: Geoprocessing; Rondônia; Water quality.
Ano: 2007
URL: http://hdl.handle.net/2315/100

INTERVENÇÃO EM PROCESSOS EROSIVOS, SANEAMENTO, ABASTECIMENTO POR MEIO DE POÇOS PROFUNDOS, E LEVANTAMENTOS GEOLÓGICOS/HIDROGEOLÓGICOS NA CIDADE DE PIRAJUÍ, SP
Provedor de dados: 25
Autores: DINIZ, HÉLIO NOBILE; MARANHÃO, MARIA DA SAUDADE.
O presente projeto tem como objetivo principal o tratamento integrado de problemas geo-ambientais que ocorrem na cidade de Pirajuí, SP. Deverão ser supridas as demandas públicas de abastecimento de água e, de ausência de saneamento básico provocado pela ausência de tratamento de efluentes provenientes de esgotos domésticos, e a intervenção em processos erosivos, como a ocorrência de boçorocas e erosão laminar, que tem causado sérios problemas de assoreamento de corpos d’água existentes. Nos poços construídos serão realizados ensaios de bombeamento para caracterização hidrogeológica do aqüífero Bauru, e com os testemunhos das sondagens realizadas serão efetuados estudos geológicos/ paleontológicos do Grupo Bauru naquela área.
Tipo: Technical Report
Palavras-chave: Erosão; Saneamento.
Ano: 2010
URL: http://hdl.handle.net/2315/153

Parasitóides Associados a Cochonilhas e Aleirodídeos (Sternorrhyncha) de Plantas Cítricas no Estado do Rio de Janeiro
Provedor de dados: 25
Autores: Rodrigues, William Costa; Cassino, Paulo Cesar Rodrigues.
Com o propósito de conhecer os parasitóides de cochonilhas e aleirodídeos, associados às plantas cítricas no Estado do Rio de Janeiro, foram realizadas coletas de folhas contendo os fitoparasitos: Aleurothrixus floccosus (Maskell), Tetraleurodes (=Aleurotrachelus) cruzi (Cassino), Paraleyrodes bondari Peracchi, Coccus viridis (Green), Crysomphalus ficus (Ashmead), Orthezia praelonga (Douglas) e Pinnaspis aspidistrae (Signoret), sendo estas limpas, em seguida procedia-se a eliminação dos organismo que eram objeto de estudo (cada folha permanecia com um única espécie de fitoparasito, para que os parasitóides que surgissem fossem mesmo associados àquela espécie). Após este procedimento as folhas foram incubadas por um período de 25 dias, onde foi observado...
Tipo: Article
Palavras-chave: Citros; Controle biológico; Inimigos naturais; Hymenoptera; Parasitismo; Biological control; Citrus; Hymenoptera; Natural enemies; Parasitism.
Ano: 2012
URL: http://hdl.handle.net/2315/232

Varroa destructor in Juquitiba, Vale do Ribeira, Southeastern Brazil: Seasonal Effects on the Infestation Rate of Ectoparasitic Mites on Honeybees
Provedor de dados: 25
Autores: Pinto, Fábio de Assis; Puker, Anderson; Message, Dejair; Barreto, Lídia Maria Ruv Carelli.
We evaluated the infestation rate (IR) of the ectoparasite mite Varroa destructor in hives of the Africanized honeybee Apis mellifera in 10 commercial apiaries located in the municipality of Juquitiba (Vale do Ribeira, São Paulo, Brazil) during two seasons (summer and winter). From each apiary, three colonies were randomly selected for collection of bee samples in each season. The average mite IR was 7.3%, when pooling both seasons. For the summer period the average IR varied from 1.1 to 11.6% (KW = 25.9191; p &lt; 0.01). For the winter period, IR values were observed ranging from 0.3 to 19.1% (KW = 18.7760; p &lt; 0.05). In only three of the studied apiaries did the IR remain unchanged over both seasons, even though it tended to be higher during the...
Tipo: Article
Palavras-chave: Varroidae; Social insects; Apidae; Apidae; Africanized Apis mellifera; Bee pathology.
Ano: 2011
URL: http://hdl.handle.net/2315/271

Delimitação das áreas de preservação Permanente (Mata ciliar) da microbacia hidrográfica do Ribeirão Faxinal, Botucatu-SP.
Provedor de dados: 25
Autores: Santos, André Ferreira dos; Cardoso, Lincoln Gehring.
This paper consisted of the mapping the Riparian Areas on the Faxinal River watershed, located in Botucatu, State of Sao Paulo. The photointerpretation were used for determination of the riparian areas. The study to showed that increase of 3,72% the riparian forest areas in the watershed on the period analyzed.
Tipo: Article
Palavras-chave: Riparian Areas; Fotointerpretação; Microbacias; Áreas ciliares; Watershed and Photointerpretation.
Ano: 2007
URL: http://hdl.handle.net/2315/104

O AVANÇO DA OCUPAÇÃO NAS ÁREAS DE RISCO EM CAMPOS DO JORDÃO: UMA COMPARAÇÃO ENTRE 1986 E 2003
Provedor de dados: 25
Autores: Delgado, Isabel Cristina de Mattos Silva; Catelani, Celso de Souza; Batista, Getulio Batista.
Resumo: No verão do ano 2000, um evento extremo de chuvas concentradas ocorreu em Campos do Jordão, ocasionado pela formação de um episódio das ZCAS (Zonas de Convergência do Atlântico Sul), causando deslizamento de encostas em vários pontos da área urbana, em bairros considerados área de risco, o que provocou a morte de 10 pessoas e um saldo de aproximadamente 3000 desabrigados. Os impactos ambientais e sociais desse acontecimento foram catastróficos. Normalmente, o início da estação chuvosa na região do Vale do Paraíba acontece quando ocorre a passagem de uma frente fria na região, uma vez que essa frente fria ativa a circulação local de vapor d’água. Esse fenômeno ocorre entre os dias 23 a 27 de outubro e prolonga-se até o final de março. A ocupação de...
Tipo: Article
Palavras-chave: Imagens Landsat; Sensoriamento Remoto; Sustentabilidade; Declividade; Ocupação urbana; Área de risco; Deslizamento; Landslides; Risk area; Remote sensing.
Ano: 2006
URL: http://hdl.handle.net/2315/39

Perfil físico-químico do pólen apícola produzido em Taubaté, Vale do Paraíba, sudeste do Brasil
Provedor de dados: 25
Autores: Pinto, Fábio de Assis; Campos, Camila Neri; Barreto, Lídia Maria Ruv Carelli.
O pólen apícola é o resultado da aglutinação do pólen das flores, efetuada pelas abelhas operárias campeiras, mediante néctar e suas substâncias salivares. A composição química do pólen varia com a espécie vegetal assim como condições ambientais, estado nutricional e idade da planta. Devido sua alta concentração de proteínas, torna-se um alimento indispensável como fonte protéica das larvas e consequentemente no desenvolvimento da colônia, podendo ser utilizado inclusive na dieta humana. Nesse contexto, o presente estudo teve por objetivo avaliar o perfil físico-químico do pólen apícola produzido no município de Taubaté – SP e o efeito temporal no valor nutricional do produto. Foram analisadas amostras de pólen apícola in natura e desidratado nos quesitos:...
Tipo: Article
Palavras-chave: Africanização; Pólen apícola; Apidae; Apicultura.
Ano: 2012
URL: http://hdl.handle.net/2315/273

Seringueira - Cultivo
Provedor de dados: 25
Autores: Bernades, Marcos Silveira.
Necessita de informações sobre o cultivo da seringueira para a região de Macaubal-SP.
Tipo: Technical Report
Palavras-chave: Seringueira; Látex; Cultivo; Implantação; Adubação; Sangria; Cursos; Associações.
Ano: 2011
URL: http://hdl.handle.net/2315/186

Os indicadores físicos, químicos e biológicos da qualidade do solo e da sustentabilidade dos ambientes naturais
Provedor de dados: 25
Autores: Silva, Roberto Carlos de Sá; Almeida, Julio Cesar Raposo de; Batista, Getulio Teixeira; Fortes Neto, Paulo.
As atividades antrópicas sobre os ecossistemas, como a agricultura mecanizada, o predomínio das monoculturas e o uso de extensas pastagens, têm contribuído para a degradação dos solos, como consequência do uso intensivo e inadequado dos ambientes naturais. O conhecimento dos processos responsáveis por alterações ambientais, principalmente o manejo incorreto da terra, é essencial para obtenção de sistemas de produção agropecuária sustentáveis. Os impactos ambientais provocados pelos agrossistemas podem ser avaliados pelo estabelecimento e monitoramento de indicadores físicos, químicos e biológicos dos solos. Mudanças no modelo do agronegócio podem contribuir para a sustentabilidade dos sistemas naturais.
Tipo: Article
Palavras-chave: Atributos edáficos do solo; Sustentabilidade; Indicadores de degradação do solo; Bioindicadores.
Ano: 2011
URL: http://hdl.handle.net/2315/176

ANÁLISE DA CARGA DE SEDIMENTOS DA REPRESA DE PARAIBUNA COM BASE EM DADOS MULTIESPECTRAIS
Provedor de dados: 25
Autores: Dias, Nelson W.; Batista, Getulio T.; Targa, Marcelo S.; Catelani, Celso S.
Neste estudo foram utilizadas duas imagens Landsat TM de fevereiro e outubro de 2003 cobrindo as bacias contribuintes da represa de Paraibuna, estado de São Paulo. O objetivo foi comparar o aporte de sedimentos carreados das bacias, do Rio Paraitinga e do Rio Paraibuna, as quais apresentam diferentes condições de cobertura do solo e qualidade dos recursos hídricos, e avaliar as diferenças entre as respostas espectrais da água de diversos trechos da represa. As imagens foram classificadas pelo método supervisionado para determinação das classes de cobertura do solo. A área da represa, separada por máscara, foi classificada pelo método não-supervisionado para identificação das classes de turbidez. A análise de regressão dos números digitais dos píxels de...
Tipo: Article
Palavras-chave: Sensoriamento remoto; Turbidez; Sedimentação; Represa.
Ano: 2006
URL: http://hdl.handle.net/2315/58

Estimativa do escoamento superficial na bacia do Córrego João Pedro através de técnicas de geoprocessamento
Provedor de dados: 25
Autores: Ferreira, Denis Spoladore; Ribeiro, Carlos Alexandre Damasceno; Cecílio, Roberto Avelino; Xavier, Alexandre Cândido.
Global climate changes affect hydrological cycle on micro and macro scales. Due to the low efficiency in the use of water resources on the planet, scientific community comes research better methods to improve water use and economy. Many studies have been developed to predict runoff amount on agricultural watersheds intending to manage the natural resources. These studies are based on soil, topographical, vegetation and hydrological data. This paper presents on study carried out at “João Pedro stream” watershed located at the municipal districts of Linhares and Sooretama (Espírito Santo State, Brasil). Land use and occupation map produced using geoprocessing tools. Resources also showed maximum runoff rate equals to 23.6m3.s-1, and maximum runoff amount 64...
Tipo: Article
Palavras-chave: Curve Number geoprocessamento escoamento superficial uso da terra Número da Curva geoprocessing land use; Runoff.
Ano: 2007
URL: http://hdl.handle.net/2315/95

Water resource management knowledge transfer through distance education: UNITAU’s experience
Provedor de dados: 25
Autores: Targa, Marcelo dos Santos; Dias, Nelson Wellausen; Batista, Getulio Teixeira.
Resumo expandido, 2p. Aceito para apresentação no IWA International Congress, Vienna, 7-12 set 2008.
Tipo: Article
Palavras-chave: Water resource management; Technical training; Post-graduate distance education.
Ano: 2008
URL: http://hdl.handle.net/2315/143

AVALIAÇÃO DA VEGETAÇÃO DAS MARGENS DO RIBEIRÃO ITAIM, NO CAMPUS DO DEPARTAMENTO DE CIÊNCIAS AGRÁRIAS DA UNITAU, NO PERÍODO DE 2003 A 2010
Provedor de dados: 25
Autores: Emilson, Pohl; Diego, Salgado Coelho; Artur, Nicoletti Gomes; Yhasmin, Mendes de Moura; Getulio, Teixeira Batista.
Resumo apresentado no Encontro de Iniciação Científica, XIII Mostra de Pós-graduação - 16 a 20 de outubro de 2012, no Campus do Bom Conselho, Universidade de Taubaté - Taubaté – SP
Tipo: Other
Palavras-chave: Mata Ciliar; Geoprocessamento; Sensoriamento Remoto.
Ano: 2012
URL: http://hdl.handle.net/2315/253

Educação Ambiental para o Terceiro Setor Voltada para os Recursos Hídricos
Provedor de dados: 25
Autores: Batista, Getulio T.; Dias, Nelson W.; Targa, Marcelo S.
Resumo. Este projeto está centrado no objetivo principal de fortalecer a atuação de entidades do Terceiro Setor junto às suas comunidades fornecendo-lhes capacitação em técnicas inovadoras que incrementem a implementação de intervenções sustentáveis no meio rural, participação em práticas de conservação de recursos hídricos dentro de projetos de aplicação, através do desenvolvimento de material didático acompanhado de técnicas pedagógicas que promovam a compreensão dos conceitos e princípios a serem disseminados, equipamento para a realização de cursos e outras atividades similares, remuneração ponderada pela qualidade das atividades realizadas por essas entidades, compilação de resultados de outros projetos deste Programa para serem disseminados pela rede...
Tipo: Other
Palavras-chave: Conservação de água; Educação ambiental; Desenvolvimento sustentável; Water  resources.
Ano: 2006
URL: http://hdl.handle.net/2315/62

PROCESSO DE LEVANTAMENTO E DE ANÁLISE COMO FORMA DE MONITORAMENTO DE UM PATRIMÔNIO CULTURAL HISTÓRICO
Provedor de dados: 25
Autores: Cocco, Maria Dolores; Campos, Cristiane Z. S.; Raimundo, Caroline A.; Almeida, Jéssica M.; Oliveira, Luísa; Malta, Flávio J. N. C.; Mello, Benedito A. R.
Congresso Internacional de Ciência, Tecnologia e Desenvolvimento da Universidade de Taubaté.
Tipo: Article
Palavras-chave: Fazenda Histórica; Inventariação; Patrimônio Cultural; Vale do Paraíba Paulista.
Ano: 2013
URL: http://hdl.handle.net/2315/274

MANEJO DE PROPRIEDADE EM ZONA DE AMORTECIMENTO DO PARQUE ESTADUAL DA SERRA DO MAR: FAZENDA MARAFUNDA UM ESTUDO DE CASO
Provedor de dados: 25
Autores: Silva Menezes, Douglas; Teixeira Batista, Getulio.
Resumo apresentado no Encontro de Iniciação Científica, XIII Mostra de Pós-graduação - 16 a 20 de outubro de 2012, no Campus do Bom Conselho, Universidade de Taubaté - Taubaté – SP
Tipo: Other
Palavras-chave: Área de amortecimento; Cacau.
Ano: 2012
URL: http://hdl.handle.net/2315/257

MAPEAMENTO DO USO DO SOLO COM DADOS DO SENSOR ASTER PARA DELIMITAÇÃO DE FRAGMENTOS FLORESTAIS
Provedor de dados: 25
Autores: Horikoshi, Andréa Sanae; Batista, Getulio Teixeira; Catelani, Celso de Souza; Fisch, Gilberto Fernando.
Resumo. O processo histórico de ocupação e transformação do espaço geográfico na região sudeste do Brasil, numa área denominada Alto Vale do Paraíba no Estado de São Paulo, deixou como legado um modelo de uso da terra baseado no desmatamento e na fragmentação florestal. Atualmente essa fragmentação está aumentando numa curva crescente e contínua devido aos efeitos do crescimento populacional dos centros regionais próximos. Isso fomenta o aumento da procura por propriedades situadas na zona rural e, conseqüentemente, geram pressões econômicas e especulação imobiliária que determinam significativas mudanças na distribuição fundiária da região. Vários estudos investigaram os efeitos da fragmentação florestal em regiões e áreas diferentes. Entretanto, esses...
Tipo: Article
Palavras-chave: Fragmento Florestal; Uso da terra; Atlantic Forest; Land use; Thermal remote sensing; ASTER sensor; Forest fragmentation; Sensoriamento remoto.
Ano: 2006
URL: http://hdl.handle.net/2315/49

Comparativo entre dados de precipitação obtidos por pluviômetros  Tipping Bucket Rain Gauges e pluviômetro Ville de Paris em Taubaté/SP
Provedor de dados: 25
Autores: Silva, Claudomiro M.; Ferreira, Willian J.; Fisch, Gilberto.
A utilização de equipamentos automáticos para  medidas de precipitação é muito importante para a tomada de decisão em diversas áreas da Ciência, sendo a calibração destes equipamentos em laboratório necessária para a confiabilidade dos dados. Neste trabalho foram comparados os dados de precipitação obtidos a partir de um pluviômetro automático do tipo TBR, conhecido como pluviômetro tipo basculante, e um pluviômetro convencional do tipo Ville de Paris, ambos instalados no posto meteorológico do Departamento de Ciências Agrárias da Universidade de Taubaté.  Dentre os resultados, se pode concluir que a intercomparação das medidas com outros instrumentos é importante para evitar erros sistemáticos e há necessidade de investimentos nas atividades de calibração...
Tipo: Presentation
Palavras-chave: Calibração; Comparativo; Chuva.
Ano: 2011
URL: http://hdl.handle.net/2315/160

PROJETO DE EDUCAÇÃO AMBIENTAL REFLORESTAR: PLANTE ESSA IDÉIA-FORMAÇÃO DE MONITOR E AGENTE AMBIENTAL MIRIM
Provedor de dados: 25
Autores: Vieira, Maria Estela.
Este trabalho será desenvolvido na Rede Escolar Municipal, em Taubaté, Estado de São Paulo. O Projeto Reflorestar: Plante essa Idéia - com a Formação de Monitor e Agente Ambiental Mirim tem o objetivo de subsidiar a escola a inserir a temática ambiental no projeto pedagógico, de forma transversal e interdisciplinar, para ampliar e dar continuidade aos projetos bem – sucedidos da escola. O projeto possui programas de conservação do meio ambiente e dos recursos naturais que irá integrar as questões ambientais aos processos decisórios e atuar diretamente na formação de seres humanos que serão peças chave na edificação de novos e melhores tempos. A melhor forma de ensiná-los, portanto, é fazer com que sejam alvos de reflexões e de vivências. Mais do que...
Tipo: Other
Palavras-chave: Educação ambiental; Interdisciplinaridade; Reflorestamento; Ensino Médio; Ensino fundamental; Estudo do Meio.
Ano: 2006
URL: http://hdl.handle.net/2315/71

Agricultura e sustentabilidade
Provedor de dados: 25
Autores: Ricci, Écio A.; Rezende Filho, Cyro de B.; Fortes Neto, Paulo; Batista, Getulio T.
A agricultura como atividade econômica tem início na Pré-história. Essencial para a sedentarização da humanidade se desenvolveu para suprir as necessidades de alimentos e fibras que eram coletados na natureza. No período da Expansão Colonial européia, a atividade tornou-se empresarial na forma de plantation. A partir daí, aliado às formas primitivas de práticas agrícolas a atividade passa a ter caráter predatório. Considerando esse fato, vários autores destacados neste artigo, discutem a agricultura praticada de forma sustentável. Por outro lado, a Agricultura Familiar tem sido estudada por Veiga (1996), Gomes (2004), Pereira (2009), Caetano (2010) e Vargas (2010). Similarmente, a Agricultura Comercial foi analisada por Assad e Almeida (2004), Santos...
Tipo: Article
Palavras-chave: Agricultura Familiar; Agroecologia; Agricultura Comercial; Agronegócio; Family Farm; Agroecology; Commercial Agriculture; Agribusiness.
Ano: 2011
URL: http://hdl.handle.net/2315/174

Revista Ambiente &amp; Água – an Interdisciplinary Journal of Applied Science: Um resumo da situação em 2014
Provedor de dados: 25
Autores: Batista, G. T.
Relatório do ano de 2014 da Revista Ambiente &amp; Água - an Interdisciplinary Journal of Applied Science. Justificativa do apoio recebido do CNPq/CAPES
Tipo: Article
Palavras-chave: Publicação científica; Recursos hídricos; Editoração; Fator de Impacto.
Ano: 2015
URL: http://hdl.handle.net/2315/285

Análise de impactos ambientais de florestas plantadas, no contexto de bacias hidrográficas: princípios norteadores
Provedor de dados: 25
Autores: Mendes, Carlos André Bulhões; Lima, Walter de Paula.
this paper intends to give general guidelines for the environmental impact analysis of planted forest projects, specifically related to their hydrological impacts. These possible impacts are not inherent to the plantations themselves, but depend on the interactions of the plantations with the prevailing environmental conditions. In this regard, the impacts could occur at different intensities, but, for the same reason, they can also be minimized by the adoption of management strategies that consider the potentialities and limitations of the physical environment. Because of that, it is argued that the adoption of catchments as the basic unit for the planning and implementation of planted forest management is a consistent strategy that naturally takes into...
Tipo: Article
Palavras-chave: Environmental impact analysis manejo florestal sustentável microbacias florestas plantadas análise de impacto ambiental; Sustainable forest management catchment planted forests.
Ano: 2007
URL: http://hdl.handle.net/2315/108

ANÁLISE DO ESCOAMENTO SUPERFICIAL DA MICRO-BACIA DO RIBEIRÃO DO CASCUDO, MUNICÍPIO DE SÃO JOSÉ DOS CAMPOS – SP
Provedor de dados: 25
Autores: Oliveira, Luciana; Santos Targa, Marcelo; Teixeira Batista, Getulio.
Resumo apresentado no Encontro de Iniciação Científica, XIII Mostra de Pós-graduação - 16 a 20 de outubro de 2012, no Campus do Bom Conselho, Universidade de Taubaté - Taubaté – SP
Tipo: Other
Palavras-chave: Bacia; Mudanças de uso da terra.
Ano: 2012
URL: http://hdl.handle.net/2315/258

Water use fund applied to land cover characterization and water quality analysis to support hydrographic basin committee decisions in Brazil
Provedor de dados: 25
Autores: Dias, Nelson Wellausen; Batista, Getulio Teixeira; Targa, Marcelo dos Santos.
Artigo aceito para apresentação no IWA International Congress, Vienna, 7-12 set 2008. 8p.
Tipo: Article
Palavras-chave: Geospatial environmental database; Water quality; Water resource assessment.
Ano: 2008
URL: http://hdl.handle.net/2315/144

Variabilidade espacial das precipitações em Belo Horizonte
Provedor de dados: 25
Autores: Coelho, Carlos Wagner Gonçalves Andrade; Abreu, Magda Luzimar de.
In big cities like Belo Horizonte, human routine is influenced directly by extreme events, such as precipitations in the rainy season, which, besides being one of the water controllers, can cause problems like floods and earth sliding, mainly on areas at risk, where big tragedies are registered. Studies that were done to the capital of Minas Gerais obtained good results about the rain behavior, relating the rains to the topography and other meteorological factors, in both local and global scales This work is aimed to study the rains in Belo Horizonte under the perspective of a new network of pluviometers installed by CEMIG (Energy Company of Minas Gerais) in November 2003. The results indicate a true gain with these new collect points, which have totalized...
Tipo: Article
Palavras-chave: Precipitação; Rede pluviométrica variabilidade espacial.
Ano: 2007
URL: http://hdl.handle.net/2315/98

BEHAVIOR OF BROILERS UNDER THE INFLUENCE OF LED LIGHTING AND MICROMETEOROLOGICAL ELEMENTS
Provedor de dados: 70
Autores: Rodrigues,Tatiana P. N. da S.; Pandorfi,Héliton; Guiselini,Cristiane; Almeida,Gledson L. P. de; Morrill,Waldirene B. B.
ABSTRACT The objective of this research was to analyze the differences between the food behaviors observed under the factors of production environment, sex and lighting system, using stochastic tools of multivariate analysis. As for the thermal characteristics of the environment, air temperature (T, °C), enthalpy (H, kJ kg-1), and black globe temperature and humidity index (BGTHI) showed high positive correlation with each other and strong negative correlation with relative humidity (RH, %). The “male drinking” behavior was positively associated with thermal characteristics of the environment in the three periods of the day, that is, the act of drinking more water would be a way to alleviate thermal stress. Birds subjected to red LED showed a strong...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal welfare; Broiler farming; Lighting system; Principal component analysis; Thermal comfort.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300272

PRODUCTION AND QUALITY OF JAPANESE QUAIL EGGS SUBMITTED TO ENVIRONMENTS WITH DIFFERENT LIGHT SPECTRUMS
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Braz,José R. B.; Nascimento,Jose W. B. do; Lopes Neto,José P.; Oliveira,Daniele L.
ABSTRACT The aim of this research was to evaluate the performance of Japanese quail (Coturnix coturnix japonica), with 94 (+49) days of age, through the production and quality of the eggs, with the birds kept in environments illuminated with LED lamps in the colors white, blue and red. The experimental design was a completely randomized design with three treatments (lamp colors) and seven replications. In the three environments, the relative air temperature averages can be considered above the thermal comfort zone for quails; however, the black globe temperature index, humidity and the thermal radiation load can be considered comfortable. The laying percentage of the birds kept under white LED was inferior to those maintained in the red LED. The feed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Quail breeding; LED lamp; Lighting technology.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400504

Thermal comfort indices in individual shelters for dairy calves with different types of roofs
Provedor de dados: 70
Autores: Fonseca,Patrícia C. de F; Almeida,Eduardo A. de; Passini,Roberta.
Among the building materials used in rural facilities, roofs are noteworthy for being largely responsible for thermal comfort, influencing the thermal balance within the shelter. This study aimed to evaluate the influence of roof on the Enthalpy (H), Thermal Load of Radiation (TLR), and Black Globe Temperature and Humidity Index (BGHI) in individual shelters for dairy calves. The design was completely randomized with three treatments: Z - zinc tile, AC - asbestos-cement tile and ACW - asbestos-cement tile painted white on the upper side. The averages were compared by the Scott Knott test at 1% probability. The results showed no statistical difference between treatments (P&lt;0.01) and the external environment for H. For TLR, there was statistical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal indices; Construction materials and type of roof.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600002

Efeito da umidificação, tratamento térmico e deformação sobre a decorticação da castanha de caju 'CCP-76' por meio de impacto único e direcionado
Provedor de dados: 70
Autores: Araújo,Max C. de; Ferraz,Antonio C. de O.
O sistema mecanizado, de múltiplos impactos, utilizado pela indústria brasileira no beneficiamento da castanha de caju, provoca danos às amêndoas e obtenção de apenas 50 a 60% de amêndoas inteiras. Para investigar o desempenho da aplicação de deformação limitada, por meio de impacto único e direcionado, um dispositivo especial foi projetado e construído. Determinou-se, inicialmente, a deformação específica correspondente ao melhor desempenho na decorticação. Utilizando-se desse valor, denominado de deformação específica limite, investigou-se o efeito de várias combinações de tempos de umidificação e tratamento térmico, utilizados na preparação da castanha do clone CCP-76, no desempenho da decorticação com impacto único e direcionado. Caracterizaram-se as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anacardium ocidentale; Viscoelasticidade; Ruptura.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200029

Efeito do ambiente protegido cultivado com melão sobre os elementos meteorológicos e sua relação com as condições externas
Provedor de dados: 70
Autores: Vásquez,Manuel A. N.; Folegatti,Marcos V.; Dias,Nildo da S.; Silva,Cláudio R. da.
O objetivo deste trabalho foi estudar o efeito do ambiente protegido cultivado com melão (Cucumis melo L.) sobre os elementos meteorológicos e sua relação com as condições externas. O experimento foi conduzido no período de 5-10-2001 a 7-1-2002, em estufa plástica de 420 m², construída com estrutura metálica galvanizada, com dois vãos de altura central de 4,6 m e lateral de 3,0 m, composto de quatro janelas frontais, cobertas com filme de polietileno transparente de alta densidade, com aditivo ultravioleta e espessura de 150 µm. A irrigação foi efetuada por gotejamento, com lâmina total de 279,6 mm, manejada utilizando um minitanque instalado no interior do ambiente. Os elementos meteorológicos foram obtidos por sistema de aquisição automático instalado no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Radiação; Evapotranspiração; Irrigação; Cucumis melo L.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100015

WOOD UTILIZATION OF Eucalyptus grandis IN STRUCTURAL ELEMENTS: DENSITIES AND MECHANICAL PROPERTIES
Provedor de dados: 70
Autores: Lahr,Francisco A. R.; Nogueira,Marta C. de J. A.; Araujo,Victor A. De; Vasconcelos,Juliano S.; Christoforo,André L.
ABSTRACT Over the years, the species of eucalyptus has become a multipurpose raw material. In addition, the most relevant aspect of the use for various purposes is related to the production of a high quality wood, coming from short duration plantations, which is fundamental to the current demand of the industries. However, its use in civil construction has not yet reached a level of importance, due to the low knowledge of many of its resistance properties and the consequent popular fear in the use of reforestation woods, in particular the Eucalyptus grandis. This research investigated its main mechanical properties, aiming to reinforce its constructive applications in wood structures. For this, two physical properties and fourteen mechanical properties, in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Rose Gum; Eucalypt; Mechanical properties; Bulk density.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500642

Avaliação de características ergonômicas no posto do operador em colhedoras combinadas
Provedor de dados: 70
Autores: Fontana,Gustavo; Silva,Rouverson P. da; Lopes,Afonso; Furlani,Carlos E. A.
Com o propósito de fornecer dados para a avaliação de características ergonômicas no posto do operador de quatro colhedoras combinadas presentes na agricultura brasileira, foram realizadas, na região de Uberaba - MG, determinações das distâncias, a partir do ponto de referência do assento até os órgãos de comandos das colhedoras. Dentre as máquinas analisadas, a colhedora NH TC 57 foi a que apresentou melhores características ergonômicas do projeto interno da cabine.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ergonomia; Colhedoras combinadas; SIP.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300020

Custo de bombas centrífugas funcionando como turbinas em microcentrais hidrelétricas
Provedor de dados: 70
Autores: Balarim,Carlos R.; Targa,Luiz A.; Virgens Filho,Jorim S.; Andrade Filho,Alceu G.; Wiecheteck,Giovana K.
A implantação de microcentrais hidrelétricas é uma das alternativas para suprir com energia comunidades pequenas e isoladas, situadas normalmente na área rural. O aproveitamento de potenciais hidráulicos de pequeno porte é uma alternativa cada vez mais viável devido não só à falta de recursos financeiros para os grandes empreendimentos, mas também pelo imenso potencial de geração em centrais de pequeno porte, que pouco tem sido aproveitado. O objetivo deste trabalho foi de apresentar uma metodologia simples de engenharia para estimar o custo das Bombas Funcionando como Turbinas (BFTs) utilizadas em microcentrais hidrelétricas, que possam ser usadas em estudos preliminares de novos aproveitamentos hidrelétricos, sem uma investigação detalhada dos lugares...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Microcentral; Energia elétrica; Bombas hidráulicas.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100025

BRILLIANT BLUE DYE REMOVAL IN FUNGICIDE SPRAYING
Provedor de dados: 70
Autores: Oliveira,Rone B.; Marubayashi,Rodrigo Y. P.; Gandolfo,Marco A.; Alves,Karina A.
ABSTRACT The method used for removal of brilliant blue dye may have an influence in interpreting the results of spraying deposition studies. The aim of this study was to assess the number of washings and water volumes for brilliant blue dye removal from soybean leaflets and glass slides in fungicide sprayings with and without adjuvants. A completely randomized experimental design was used in a 3 × 3 × 2 × 4 factorial scheme. The factors consisted of number of washings (1st, 2nd, and 3rd), water volume (15, 20, and 30 mL), target type (soybean leaflets and glass slides), and spray solutions (fungicide ProdutorBR® 0.5 L ha−1 without and with the adjuvants vegetable oil Agr’óleo® 0.5% v v−1, mineral oil Nimbus® 0.5% v v−1, and surfactant Silwet® 0.04% v v−1)....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Adjuvants; Experimental methods.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300611

PHYSIOLOGICAL RESPONSES OF DAIRY COWS AS A FUNCTION OF ENVIRONMENT IN HOLDING PEN
Provedor de dados: 70
Autores: Silva,Danilo Corrêa; Passini,Roberta.
ABSTRACT This research aimed to assess the climatization configuration in a holding pen for dairy cattle considering physiological responses of animals and thermal comfort indexes. Experimental design consisted of 16 cows in a Latin square design containing four groups of four animals (G1, G2, G3 and G4) and four periods (P1, P2, P3 and P4), in which four environments were used as treatments: EXT – external environment (control); SHA – shading with polypropylene mesh, 80% light interception; S+S – shading and water sprinkling; and S+S+V – shading, sprinkling and ventilation. Dry and wet bulb temperature, black globe temperature, wind speed and humidity were recorded during the climatization process, between October 13 and December 7. Subsequently,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Shading; Adiabatic evaporative cooling system; Thermal indexes.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200206

Utilização do farelo de conchas de vôngole na adsorção de fósforo e como corretivo da acidez do solo
Provedor de dados: 70
Autores: Lo Monaco,Paola A. V.; Matos,Antonio T.; Eustáquio Júnior,Valdeir; Ribeiro,Ivan C. A.; Teixeira,Denis L.
Teve-se o objetivo de, com a realização deste trabalho, obter a curva de neutralização do pH de amostras dos horizontes A e B de um Latossolo Vermelho-Amarelo distrófico, utilizando-se de farelo de conchas de vôngole (Anomalocardia brasiliana); além disso, avaliar a capacidade de adsorção de fósforo, obtendo-se a isoterma de adsorção de melhor ajuste aos dados obtidos. Verificou-se que o farelo de concha de vôngole apresenta potencial para uso como corretivo de acidez do solo e que a dose recomendada para correção do pH do horizonte A do Latossolo Vermelho Amarelo distrófico estudado foi de 2,92 t ha-1, enquanto, para correção do horizonte B, foi de 3,35 t ha-1. O farelo de conchas de vôngole também apresentou alta capacidade de adsorção de fósforo, o que...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resíduos de maricultura; Correção da acidez do solo; Remoção de fósforo; Isotermas de adsorção.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500006

Produtividade da água de chuva em culturas de subsistência no Semiárido Pernambucano
Provedor de dados: 70
Autores: Brito,Luiza T. de L.; Cavalcanti,Nilton de B.; Silva,Aderaldo de S.; Pereira,Lúcio A.
Os diferentes sistemas de cultivo utilizados pelos agricultores do Semiárido brasileiro apresentam riscos de perdas devido às irregularidades das chuvas, sendo, portanto, necessário associá-los a práticas que propiciem maior disponibilidade de água no solo durante o ciclo de cultivo. Neste trabalho, objetivou-se avaliar a aplicação de quantidades mínimas de água e adubação orgânica na produtividade de feijãocaupi, cultivar BRS-Pujante e de milho, cultivar BRS-Caatingueiro. Os resultados indicam que as maiores produtividades de grãos foram obtidas com o tratamento que associou a irrigação de salvação com a adubação orgânica, sendo para o feijão-caupi de 1.422,5 kg ha-1, e para o milho, de 6.099,1 kg ha-1, seguido pelo tratamento que usou somente a adubação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vigna unguiculata; Zea mays L.; Irrigação de salvação; Adubação.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100011

Effect of cycle time and airflow in biological nitrogen removal from poultry slaughterhouse wastewater using sequencing batch reactor
Provedor de dados: 70
Autores: Lopes,Carla L.; Mees,Juliana B. R.; Sene,Luciane; Carvalho,Karina Q. de; Christ,Divair; Gomes,Simone D.
This study aimed to evaluate the influence of airflow (0.25, 0.50 and 0.75 L.L-1.min-1) and cycle time (10.45 h, 14.25 h and 17.35 h) on a sequencing batch reactor (SBR) performance in promoting nitrification and denitrification of poultry slaughterhouse wastewater. The operational stages included feeding, aerobic and anoxic reactions, sedimentation and discharge. SBR was operated in a laboratory scale with a working volume of 4 L, keeping 25% of biomass retained inside the reactor as inoculum for the next batch. In the anoxic stage, C: N ratio was maintained between 5 and 6 by adding cassava starch wastewater. A factorial design (22) with five repetitions was designed at the central point to evaluate the influence of cycle time and airflow on total...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrification; Denitrification; Response surface methodology; Fluorescent in situ hybridization.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300567

Fitorremediação de solo contaminado com o herbicida picloram por plantas de Panicum maximum em função do teor de água
Provedor de dados: 70
Autores: Assis,Renato L. de; Procópio,Sergio de O.; Carmo,Marcos L. do; Pires,Fábio R.; Cargnelutti Filho,Alberto; Braz,Guilherme B. P.; Silva,Wellington F. P.
O objetivo deste trabalho foi avaliar a influência de lâminas de água no solo sobre a fitorremediação de solo contaminado com o herbicida picloram por plantas de Panicum maximum cv Tanzânia. O experimento foi conduzido em casa de vegetação, e os tratamentos, em número de 12, foram compostos pela combinação entre quatro níveis diários de reposição da água, através das lâminas de água evaporada (80; 90; 100 e 110% da quantidade de água evaporada) e de três doses do picloram (0; 80 e 160 g ha-1). A quantidade de água evaporada foi determinada por meio de dois evaporímetros. Após a aplicação do herbicida, foi realizada a semeadura da espécie vegetal fitorremediadora. Noventa dias após a emergência, as plantas de capim-tanzânia foram dessecadas, e a parte...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Residual de herbicidas; Mimetizadores de auxinas; Soja; Evaporação de água.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500007

Technology for sugarcane agroindustry waste reuse as granulated organomineral fertilizer
Provedor de dados: 70
Autores: GURGEL,MARCÍLIO N. DO A.; CORREA,SIMONE T. R.; DOURADO NETO,DURVAL; PAULA JÚNIOR,DURVAL R. DE.
Aiming to evaluate the use of sugarcane industry waste such as byproducts from vinasse concentration process, it was assessed the organomineral fertilizer BIOFOM (concentrated vinasse, filter cake, boiler ash, soot from chimneys and supplemented with mineral fertilizers). The study included characterization and agronomic potential analysis of a test plant (corn), by noting the differences between mineral fertilizers and BIOFOM fertilization until 45 days after sowing. The technology traditionally used to produce BIOFOM was based on vinasse evaporation with high heat transfer coefficients. It was observed that the technology, which can be formulated according to the needs of any crop, could be used in many cases as mineral fertilizer. Therefore, the use of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biofertilizer; Vinasse; Sugarcane agribusiness; Organic waste; Filter cake.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100063

SUNFLOWER EMERGENCE AND INITIAL GROWTH IN SOIL WITH WATER EXCESS
Provedor de dados: 70
Autores: Loose,Luis H.; Heldwein,Arno B.; Lucas,Dioneia D. P.; Hinnah,Fernando D.; Bortoluzzi,Mateus P.
ABSTRACT: Sunflower crops are grown in different regions worldwide. However, the stress caused by water excess in the soil impairs this crop growth and yield. The aim of the present study was to determine the response of sunflower plants to long periods of water excess during initial development stages. Water excess treatments were applied at the initial development of these plants at the sowing day, three days after sowing, at plant emergence, and at V2 and V4 stages. The treatments had different duration periods (0, 48, 96, 144, 192, and 240 hours) and were applied at three sowing dates. The current experiment is factorial and was carried out according to a completely random design. Two plant pots, treated under greenhouse conditions, made up the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Helianthus annuus L.; Water stress; Plant emergence; Growth reduction.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400644

Internal environmental conditions of soybean processing plants and safety in workplace
Provedor de dados: 70
Autores: OLIVEIRA,ALEX L. DE; ARAUJO,ADAMO DE S.; GADOTTI,GIZELE I.; VILLELA,FRANCISCO A.; BAUDET,LEOPOLDO.
ABSTRACT Currently, the domestic agricultural sector has become increasingly professionalized; therefore, measures aimed at safety in the workplace and monitoring of environmental risks have been gaining major importance in this scenario. Thus, this study aimed at assessing internal environmental conditions of four soybean processing plants (SPPs) operating with a screen-air machine, densimetric table and with or without spiral separator. These plants are in the state of Rio Grande do Sul (Brazil), being assessed on site considering every feature related to machinery and equipment, as well as technological level. Field evaluations comprised measurements of noise, illuminance and suspended dust. Results showed that none of the SPPs is in full accordance...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Seed processing; Noise map; Lighting study; Chemical agents.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400673

MULTIVARIATE ANALYSIS OF PEANUT MECHANIZED HARVESTING
Provedor de dados: 70
Autores: Noronha,Rafael H. F.; Zerbato,Cristiano; Silva,Rouverson P. da; Ormond,Antonio T. S.; Oliveira,Mailson F. de.
ABSTRACT The peanuts harvesting mechanization is affected by the soil physical characteristics and it may increase the losses due to the production of pods in subsurface. The objective of the experiment was to identify the clusters through multivariate exploratory approaches from similarity in six soil textures (very clayey, clayey, silty clayey loam, clayey loam, sandy loam and sandy) in the state of São Paulo, Brazil, determining the main agronomic variables that most influenced the clustering division to assist the decision-making process in peanuts mechanized harvesting. The data were analyzed by the multivariate exploratory that is performed to simplify the description of a set of interrelated variables, using: yield, maturity, soil and pod moisture...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil textural classes; Arachis hypogaea L.; Principal components analysis.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200244

Análise espacial da redução da queima na colheita da cana-de-açúcar: perspectivas futuras ao cumprimento do protocolo agroambiental
Provedor de dados: 70
Autores: Novaes,Maikon R. de; Rudorff,Bernardo F. T; Almeida,Cláudia M. de; Aguiar,Daniel A. de.
Estimada em quase 8 milhões de hectares, a área cultivada com cana no País possui 60% de sua extensão dentro do Estado de São Paulo e encontra-se distribuída de maneira heterogênea pelo seu território. Em junho de 2007, a União da Indústria de Cana-de-Açúcar (UNICA) e a SMA-SP assinaram um protocolo agroambiental para antecipar a extinção da queima da palha para 2014, em áreas com declividade inferior a 12%. O objetivo deste trabalho é realizar uma análise sobre a adesão dos municípios a este protocolo frente à dinâmica da prática da queima, utilizando técnicas de análise espacial. Foram selecionadas duas regiões de acordo com o índice de Moran, e realizadas análises sobre a mudança em relação à prática da queima no período entre 2006 e 2008. Matrizes de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Protocolo agroambiental; Análise espacial; SIG.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300017

Potencial de redução de emissão de equivalente de carbono de uma unidade suinícola com biodigestor
Provedor de dados: 70
Autores: Angonese,André R.; Campos,Alessandro T.; Welter,Rosilene A.
O objetivo do presente trabalho foi avaliar o potencial de reduções de emissão de carbono, em tCO2 eq ano-1, e estimar o valor financeiro obtido anualmente para o total de suínos da granja e o valor médio anual por animal em suinocultura, em sistema de recria e engorda, com capacidade instalada para 600 animais. O sistema de tratamento dos dejetos é realizado de forma integrada, possibilitando a reciclagem dos nutrientes, em que o biodigestor anaeróbio tubular estabiliza a matéria orgânica, produzindo metano e biofertilizante no processo. A estimativa foi efetuada baseando-se na metodologia AM0006, aprovada pelo Conselho Executivo do Mecanismo de Desenvolvimento Limpo do IPCC. O potencial de redução de emissão de CO2 equivalente por ano foi de 325,16 t,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Protocolo de Kioto; Dejetos de suínos; Biodigestor.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400007

Spatial variability of air dry bulb temperature and black globe humidity index in a broiler house during the heating phase
Provedor de dados: 70
Autores: Ponciano,Patrícia F.; Yanagi Junior,Tadayuki; Ferraz,Gabriel A. E S.; Scalon,João D.; Schiassi,Leonardo.
The air dry-bulb temperature (t db),as well as the black globe humidity index (BGHI), exert great influence on the development of broiler chickens during their heating phase. Therefore, the aim of this study was to analyze the structure and the magnitude of the t db and BGHI spatial variability, using geostatistics tools such as semivariogram analysis and also producing kriging maps. The experiment was conducted in the west mesoregion of the states of Minas Gerais in 2010, in a commercial broiler house with heating system consisting of two furnaces that heat the air indirectly, in the firsts 14 days of the birds' life. The data were registered at intervals of five minutes in the period from 8 a.m. to 10 a.m. The variables were evaluated by variograms...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Broiler chickens; Kriging; Chick; Semivariogram; Thermal stress.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300001

Reflexos da variabilidade espacial e temporal da fase de avanço e do tempo de oportunidade de infiltração no tempo de aplicação d'água na irrigação por sulcos para um solo franco-arenoso
Provedor de dados: 70
Autores: Carvalho,Joaquim J. de; Azevedo,Carlos A.V. de; Henrique,Jacqueline; Dantas Neto,José; Lima,Vera L. Antunes de; Pordeus,Roberto V.
Esta pesquisa teve como objetivo verificar as variabilidades espaciais e temporais no tempo de avanço e no tempo de oportunidade de infiltração d'água e seus reflexos no tempo de aplicação d'água num sistema de irrigação por sulcos com fluxo reduzido para um solo franco-arenoso. As avaliações de campo foram realizadas no perímetro irrigado de São Gonçalo, Sousa - PB, onde foram feitas medições em seis sulcos, eqüidistantes, de forma a abranger o máximo possível a variabilidade em toda a área, nos 12 eventos de irrigação da estação de cultivo. Observando os tempos de avanço e de oportunidade de infiltração d`água no final da área irrigada em cada evento e em cada sulco ao longo do tempo, verificou-se que a variação espacial no tempo de avanço foi mais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tempo de avanço; Tempo de aplicação d'água; Irrigação por sulcos.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200026

Escoamento superficial na interação: cobertura vegetal e práticas de controle de erosão
Provedor de dados: 70
Autores: Carvalho,Marco A. R. de; Miranda,Jarbas H. de; Duarte,Sergio N.; Carvalho,Lilian C. C. de.
O escoamento da água oriunda das terras agricultadas é o principal fator poluente dos mananciais hídricos nas áreas rurais. Devido a esse fato, faz-se necessário o desenvolvimento e a aplicação de tecnologias que venham a reduzir descargas de resíduos indesejáveis. Nesse sentido, conduziu-se um experimento na área experimental do Departamento de Engenharia Rural - ESALQ/USP, Piracicaba - SP, com o objetivo de avaliar o efeito de diferentes condições de solo, (feijão, gramínea e solo nu) e diferentes práticas de controle de erosão (sulco de infiltração, terraço de infiltração e sem práticas de controle de erosão), buscando-se estimar o escoamento superficial. O delineamento estatístico adotado foi o em blocos aleatorizados, em esquema fatorial 3x3,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Terraço de infiltração; "mulching" vertical; Cobertura vegetal.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600013

TÉCNICAS PARA DETECÇÃO DE PONTOS INFLUENTES EM VARIÁVEIS CONTÍNUAS REGIONALIZADAS
Provedor de dados: 70
Autores: Richetti,Jonathan; Uribe-Opazo,Miguel A.; Bastiani,Fernanda de; Johann,Jerry Adriani.
RESUMO Na análise de dados espaciais em agricultura, a presença de pontos influentes pode alterar consideravelmente os resultados das análises de dependência espacial e, consequentemente, a construção dos mapas. Quando se referem a atributos físico-químicos do solo e da produtividade, os mapas devem representar uma estimativa eficiente das condições reais do campo, já que são importantes informações utilizadas para a manutenção de um sistema agrícola de manejo localizado, com a otimização da aplicação de insumos agrícolas, visando à maior produtividade. Este trabalho teve por objetivo apresentar as técnicas gráficas hair-plot, de influência local (Ci e |Lmax|) de identificação de observações influentes em dados contínuos espaciais georreferenciados,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Hair-plot; Influência local; Máxima verossimilhança; Atributos químicos.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100152

Condutividade e difusividade térmica do figo (Ficus carica L.) "Roxo de Valinhos"
Provedor de dados: 70
Autores: Sarria,Saul D.; Honório,Sylvio L.
O resfriamento e/ou congelamento de produtos hortícolas, depois da colheita, é realizado com o objetivo de retirar o calor desses produtos, permitindo-lhes, em função disso, um tempo maior de conservação. Portanto, o conhecimento das propriedades físicas que envolvem transferência de calor do figo "Roxo de Valinhos" é útil para o cálculo de projetos e a análise de sistemas de engenharia de alimentos em geral, assim como para o emprego em equações de modelos matemáticos termodinâmicos. Neste trabalho, foram determinadas, experimentalmente, a condutividade e a difusividade térmica do figo inteiro no estádio rami e, a partir desses valores, foi determinado o calor específico. Foi utilizado o método transiente da Fonte Linear de Calor. Foi introduzida nas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Figo inteiro; Transferência de calor; Calor específico.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100021

Nocturnal thermal comfort in facilities for growing swines
Provedor de dados: 70
Autores: Sarubbi,Juliana; Rossi,Luiz A.; Moura,Daniella J. de; Oliveira,Rafael A. de; Maia,Ana Paula de A.
In most of Brazilian pig farms, the environmental acclimatization systems run manually. For night and early morning periods, this practice isn't appropriate, because, in general, there are not employees available to run these manual systems. This research aimed to compare the bioclimatic profile of two differently constructed facilities to the external environment, considering the period from 6 p.m. to 6 a.m. during the spring, in order to show that night and early morning temperatures do not coincides with growing pig's thermoneutral zone. For this reason, acclimatization must be also carried out at these periods. It was analyzed the dry bulb temperature, relative air humidity, temperature-humidity index (THI) and enthalpy data of the sheds and external...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal environment; Animal welfare; Pig farming; Acclimatization system.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600004

Perdas de água e solo sob diferentes padrões de chuva simulada e condições de cobertura do solo
Provedor de dados: 70
Autores: Carvalho,Daniel F. de; Souza,Wanderley de J.; Pinto,Marinaldo F.; Oliveira,João R. de; Guerra,José G. M.
Este trabalho foi realizado com o objetivo de determinar as perdas de solo e água em um Argissolo Vermelho-Amarelo, submetido a quatro diferentes padrões de precipitação de chuva simulada e duas condições de cobertura: área com solo descoberto e com palhada após plantio de milho. O experimento foi conduzido no Campo Experimental da Embrapa-Agrobiologia, localizado no município de Seropédica-RJ, e consistiu na aplicação de chuvas simuladas com diferentes padrões, caracterizados como avançado (AV), intermediário (IN), atrasado (AT) e constante (CT), em uma área amostral de 0,80 m de largura por 1,0 m de comprimento. Utilizando um simulador de chuvas portátil, foram aplicadas chuvas com 30 mm de lâmina total durante 60 minutos. Nos padrões com intensidade...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão hídrica; Padrões de precipitação; Simulação de chuva.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400010

Zoneamento bioclimático da região sudeste do Brasil para o conforto térmico animal e humano
Provedor de dados: 70
Autores: Oliveira,Lutércia M. F. de; Yanagi Junior,Tadayuki; Ferreira,Elizabeth; Carvalho,Luiz G. de; Silva,Mariano P. da.
O objetivo deste trabalho foi avaliar as condições de clima da região Sudeste do Brasil, por meio do índice de temperatura e umidade (ITU), e apresentar o zoneamento bioclimático relacionado ao conforto térmico animal e humano. Os valores de ITU foram estimados a partir de dados de temperatura e umidade relativa do ar para o período de 1980 a 2000. Quatro intervalos de ITU foram usados para classificar o desempenho humano (ITU &lt; 74: conforto; 74 &lt; ITU &lt; 79: quente; 79 &lt; ITU &lt; 84: muito quente, e ITU &gt; 84: extremamente quente), e dois intervalos para classificar a produção animal (79 &lt; ITU &lt; 84: perigoso e ITU &gt; 84: emergência). Os resultados mostraram maior risco de desconforto térmico no período de outubro a abril, comparado ao...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiente térmico; Produção animal; Rendimento humano.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300020

Comparação entre dois métodos para avaliar a eficácia de limpeza durante o beneficiamento de tomates
Provedor de dados: 70
Autores: Magalhães,Ana M.; Ferreira,Marcos D.; Moretti,Celso L.
A etapa de limpeza em uma linha de beneficiamento para tomate de mesa é muito importante, pois retira as impurezas externas dos frutos, todavia poucos são os métodos utilizados para avaliar a eficácia desse processo. Assim, o objetivo deste trabalho foi avaliar duas metodologias com relação à eficácia do processo de limpeza. As metodologias estudadas foram: análise com o colorímetro e análise com o turbidímetro. Os ensaios foram realizados em laboratório, na etapa de limpeza do protótipo UNIMAC (Unidade Móvel de Auxílio à Colheita), utilizando-se de esferas de borracha, com peso similar ao tomate, que foram sujas artificialmente e passaram pela limpeza no protótipo com cerdas de náilon e rotação de 100 rpm. Observou-se que o método de análise com o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lycopersicon esculentum; Colorímetro; Turbidímetro.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400020

Análise espacial da ocorrência do índice de cone em área sob semeadura direta e sua relação com fatores do solo
Provedor de dados: 70
Autores: Molin,José P.; Magalhães,Raphael P. de; Faulin,Gustavo D. C.
O presente estudo teve o objetivo de analisar, em uma lavoura sob semeadura direta, a distribuição vertical e horizontal da resistência à penetração medida por valores georreferenciados do índice de cone (IC) e a influência do teor de água do solo, permitindo a interpolação para análise de relações causa e efeito. Fatores importantes, como o teor de argila, silte, densidade, espaço poroso e teor de matéria orgânica do solo também foram mensurados. Utilizou-se de um penetrômetro hidráulico eletrônico, receptor de GPS, amostrador de solo e programas computacionais para o tratamento e obtenção dos resultados. A análise foi feita a partir dos mapas (não apresentados) para a espacialização dos atributos e pela regressão entre os dados interpolados por meio da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compactação do solo; Geoestatística; Agricultura de precisão.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200012

Coffea arabica (cv Catuaí) production and bean size under different population arrangements and soil water availability
Provedor de dados: 70
Autores: Sakai,Emilio; Barbosa,Eduardo A. A.; Silveira,Jane M. de C.; Pires,Regina C. de M.
The purpose of this research was to evaluate the effect of drip irrigation under different population arrangements on the phytometric features, coffee productivity and bean size classification according to sieve retention. The experiment with Coffea arabica L. cv Catuaí was carried out in Mococa, São Paulo, Brazil. The experimental design was a 6 x 2 factorial scheme in randomized blocks, with four replications. The six densities of plantation were E1 (1.60 x 0.50 m); E2 (1.60 x 0.75 m); E3 (1.60 x 1.00 m); E4 (3.20 x 0.50 m); E5 (3.20 x 0.75 m) and E6 (3.20 x 1.00 m), which were divided according to the availability of water (irrigated - I - or non-irrigated - NI - groups). Data were submitted to analysis of variance and averages compared by Tukey test at...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drip irrigation; Coffee productivity; Coffee crop phytometry; Coffee bean size.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100015

Intervalo hídrico ótimo em um latossolo vermelho distroférrico sob diferentes sistemas de produção
Provedor de dados: 70
Autores: Serafim,Milson E.; Vitorino,Antônio C. T.; Peixoto,Paula P. P.; Souza,Cristiano M. A.; Carvalho,Daniel F. de.
Este trabalho teve o objetivo de caracterizar sistemas de cultivo quanto à qualidade estrutural do solo para o desenvolvimento de plantas por meio da determinação do Intervalo Hídrico Ótimo (IHO). O estudo foi realizado com amostras indeformadas de um Latossolo Vermelho distroférrico, sob os sistemas de cultivo convencional, direto e integração lavoura-pecuária, no município de Dourados - MS. Em cada sistema de cultivo, foram amostrados 28 pontos, nas camadas de 0-0,05 m, 0,05-0,10 m, e 0,10-0,20 m, totalizando 84 amostras por sistema, que foram utilizadas para a determinação da curva de retenção de água no solo, da curva de resistência do solo à penetração e da porosidade. No sistema de cultivo convencional e no direto, a menor limitação ao...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Integração lavoura-pecuária; Plantio direto; Água no solo.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400005

Situação dos recursos hídricos nas bacias hidrográficas dos rios Piracicaba, Capivari e Jundiaí utilizando modelo desenvolvido em dinâmica de sistemas
Provedor de dados: 70
Autores: Sánchez-Román,Rodrigo M.; Folegatti,Marcos V.; Orellana-González,Alba M. G.
Utilizou-se modelo desenvolvido em dinâmica de sistemas, especificamente para as Bacias Hidrográficas dos Rios Piracicaba, Capivari e Jundiaí (BH-PCJ), com cinco simulações para 50 anos de horizonte, como ferramenta para auxiliar na gestão dos recursos hídricos. O modelo estimou as ofertas e demandas de água, e a geração de águas residuárias dos diversos consumidores existentes nas BH-PCJ. Realizou-se simulação utilizando-se das taxas de consumo e de oferta existentes em 2004, e as precipitações com os valores médios constantes. Sob essas premissas, foi encontrado que as demandas de água aumentarão cerca de 76%, que aproximadamente 39% do volume de água disponível terá origem no reúso das águas residuárias, a carga contaminante aumentará em 91%. O Índice...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recursos hídricos; Modelagem; Simulação.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400008

Desempenho de um regulador automático de vazão para canais de irrigação
Provedor de dados: 70
Autores: Amaral,Luís G. H. do; Ramos,Márcio M.; Silva,Demetrius D. da; Cecon,Paulo R.; Freitas,Letícia C. da S. R.
As estruturas de controle comumente utilizadas nas tomadas de água dos canais de irrigação não permitem a distribuição da quantidade correta de água, favorecendo o desperdício e, consequentemente, reduzindo a eficiência no uso da água. O objetivo deste trabalho foi determinar o desempenho de um regulador automático de vazão no controle da vazão derivada. Para tanto, um exemplar do equipamento, construído em fibra de vidro, foi instalado na lateral de um canal de concreto do Laboratório de Hidráulica da Universidade Federal de Viçosa, em Viçosa-MG. O equipamento foi avaliado em toda a sua faixa de operação, sendo que, em cada regulagem prefixada, determinou-se a vazão derivada com o nível da água a montante variando de 0,30 a 0,45 m. A variação média na...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Automação hidráulica; Comportas hidráulicas; Condutos livres.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600017

PERFORMANCE OF ESTIMATIVE MODELS FOR DAILY REFERENCE EVAPOTRANSPIRATION IN THE CITY OF CASSILÂNDIA, BRAZIL
Provedor de dados: 70
Autores: Cunha,Fernando F. da; Magalhães,Fernando F.; Castro,Marco A. de; Souza,Epitácio J. de.
ABSTRACT Before choosing the method of the estimate of reference evapotranspiraton (ET0) in a region, it is important to evaluate the degree of precision of the model. The present research aimed to evaluate the performance of 30 methods for daily ET0 estimate in the Cassilândia city, Brazil. The meteorological data had been obtained from the National Institute of Meteorology in the period of four years (from April, 2008 to March, 2012). As standard method it was chosen the Penman-Monteith-FAO56, and the comparison of the results was by means of the estimated standard error (ESE), the determination coefficient (R2), the coefficients “a” and “b” of the linear regressions, Willmott's index of agreement (d), Pearson's correlation coefficient (r) and the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agrometeorology; ET0; Evaporation; Irrigation; Penman-Monteith-FAO 56 method.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100173

Auditoria energética em uma agroindústria de laticínios
Provedor de dados: 70
Autores: Debastiani,Gilson; Nogueira,Carlos E. C.; Lawder,José H.; Vidotto,Magno L.; Azevedo,Ricardo L.
O foco deste trabalho consiste num estudo de caso referente a uma Auditoria Energé­tica efetuada numa agroindústria de laticínios localizada na cidade de Guaíra, Extremo-Oeste para­naense. Neste contexto, o presente artigo teve por objetivos: efetuar uma auditoria energética de suas instalações, analisando o consumo de energia elétrica associado aos processos produtivos, sis­temas e equipamentos existentes; identificar e quantificar as cargas instaladas na agroindústria, veri­ficando a energia consumida e a potência demandada em cada uma delas; determinar o potencial de conservação de energia para os usos finais existentes na empresa, por meio da identificação de oportunidades para implantação de medidas que otimizassem o uso da energia; e efetuar um...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eficiência energética; Energia elétrica; Auditoria energética; Redimensionamento energético.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200001

Efeito da utilização de sistemas de climatização nos parâmetros fisiológicos do gado leiteiro
Provedor de dados: 70
Autores: Perissinitto,Maurício; Moura,Daniella J. de; Matarazzo,Soraia V.; Silva,Iran J. O. da; Lima,Karla A. O. de.
Este trabalho avaliou diferentes sistemas de resfriamento adiabático evaporativo (SRAE) (aspersão e nebulização), conjugados com a ventilação forçada, quanto à eficiência térmica na redução do estresse térmico de bovinos leiteiros. O experimento foi desenvolvido em um rebanho leiteiro comercial localizado em São Pedro - SP, compreendendo 28 dias consecutivos de novembro de 2003, utilizando-se de 10 animais da raça Holandesa em lactação, alojados em sistema de "freestall". A umidade relativa do ar, a temperatura ambiente e a temperatura de globo negro foram registradas a cada 15 minutos, durante todo o período. A temperatura retal, a freqüência respiratória e a temperatura dos pelames branco e preto foram medidas nos horários das 9; 11; 13; 15 e 17 h,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fisiologia animal; Ambiência; Conforto térmico.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300002

Behavior of chicks subjected to thermal challenge
Provedor de dados: 70
Autores: Ferraz,Patricia F. P.; Yanagi Junior,Tadayuki; Alvarenga,Talita A. C.; Reis,Gregory M.; Campos,Alessandro T.
In the first week of a chick life, broilers are very sensitive to different conditions outside their thermoneutral zone. Thus, the goal of this study was to evaluate the behaviors and productive responses of broilers subjected to conditions of thermal comfort or challenge at different intensities (27, 30, 33 and 36ºC) and durations (1, 2, 3 and 4 days starting on the second day of life). In the experiment, ten minutes of images from each hour of each treatment were analyzed to evaluate the key behaviors of the birds. Similar behavior at different dry-bulb air temperatures were identified by using Ward's method of cluster analysis. These behaviors were grouped by dendograms in which the similarity of these data was qualified. Feed intake, water intake and...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Grouping of data; Dendogram; Broiler; Productive responses.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600002

Anaerobic biodigestion of pigs feces in the initial, growing and finishing stages fed with diets formulated with corn or sorghum
Provedor de dados: 70
Autores: Miranda,Adélia P.; Lucas Junior,Jorge de; Thomaz,Maria C.; Pereira,Gener T.; Fukayama,Ellen H.
The objective of this study was to evaluate the quality and the production of biogas and biofertilizer obtained from biodigester supplied with pig feces in the initial, growing and finishing stages, fed with diets formulated based on corn or sorghum. Twenty bench biodigesters were used with hydraulic retention time of 30 days and daily loads that contained 4 to 6% of total solids (TS) and 3.6 to 5.2% of volatile solids (VS). In the effluent of the biodigesters, mean levels of TS were observed ranging between 1.6 and 2.0% and of VS between 1.2 and 1.6%. The mean reductions of TS were 57.7 to 64.7% and of VS from 61.7 to 69.0%, and there was only difference in the finishing phase, in which the major averages reductions were produced by the biodigesters...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biodigesters; Biogas; Pig feces; Environmental impact.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100006

Polyphenoloxidase activity in peaches after vibration
Provedor de dados: 70
Autores: Dantas,Tiago B. H.; Ferraz,Antônio C. de O.; Honório,Sylvio L.; Lima,Giuseppina P. P.
The vibration during transportation is one of the main causes of fruit damage. The actual methodologies used for damage evaluation in fruits seem to be subjective, since most of them are based on visual evaluation. In this study the effect of vibration, for one and two hours, on polyphenoloxidase (PPO) activity in peach pulp was investigated. The relation among PPO activity variation, postharvest time and resting time were also considered. Results showed that vibration affects PPO activity. However, it was not possible to correlate PPO activity variation and vibration.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Polyphenoloxidase; Vibration; Damage; Peach.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200010

SPATIAL VARIABILITY OF SOIL RESISTANCE TO PENETRATION IN NO TILLAGE SYSTEM
Provedor de dados: 70
Autores: Cortez,Jorge W.; Matos,Wéliton P. da S.; Arcoverde,Sálvio N. S.; Cavassini,Victor H.; Valente,Igor Q. M.
ABSTRACT In areas of no tillage system where there is intense traffic of machines and minimal soil mobilization, the periodic monitoring allied on localized soil compaction represent important strategies aiming agricultural sustainability. Thus, the objective of this study was to evaluate the spatial variability of soil resistance to penetration (RP) in no tillage system. Data collection took place in an experimental area of 7.65 ha using a sample grid composed of 40 points. At each point the RP was determined by three replications from which was obtained the mean RP, the maximum RP, and the depth of the maximum RP in the 0-0.40m layer. Deformed samples were randomly collected in the area to determine the water content in the soil (θ). Then the RP data...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Agricultural mechanization; Geostatistics.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500697

Perda de carga localizada em emissores não coaxiais integrados a tubos de polietileno
Provedor de dados: 70
Autores: Rettore Neto,Osvaldo; Frizzone,José A.; Miranda,Jarbas H.; Botrel,Tarlei A.
Este trabalho apresenta os resultados de experimento conduzido para avaliar as perdas de carga localizadas em gotejados não coaxiais integrados a tubos de polietileno. As perdas de carga para diferentes vazões foram determinadas em quatro modelos de tubos-gotejadores, com dez repetições. Para cada vazão, a perda de carga localizada foi calculada pela diferença entre a perda de carga no tubo com emissor e a perda de carga contínua no tubo uniforme estimada pela equação de Darcy-Weisbach com o fator de atrito (f) previamente determinado. Aproximações matemáticas foram sugeridas para calcular hfe com base no coeficiente de carga cinética (K) e em um valor constante de comprimento equivalente (Le). Para os modelos de tubos-gotejadores estudados, a perda de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coeficiente de carga cinética; Comprimento equivalente; Irrigação por gotejamento; Fator de atrito.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100004

Economic feasibility of irrigation systems in broccoli crop
Provedor de dados: 70
Autores: Oliveira,Fabricio C. de; Geisenhoff,Luciano O.; Almeida,Alexsandro C. dos S; Lima Junior,Joaquim A. de; Lavanholi,Rogério.
ABSTRACT This study aimed to analyze the economic feasibility of different irrigation systems in broccoli cropping, in Dourados - MS, Brazil. Initially, irrigation was performed using different systems (surface drip, subsurface drip, micro sprinkler, Santeno® and conventional sprinkler). Both yield of commercial inflorescence (CIY) and applied water depth (AWD) were determined during trial. Economic feasibility was analyzed through estimates of acquisition cost (AC), total annual cost (TAC), gross revenue (GR), net revenue (NR), benefit-cost rate (BCR), return rate (RR) and return time (RT). Subsurface drip irrigation was the most feasible in addition to using the second lowest AWD (170.3 mm) compared to the other systems. The values of CIY, AC, RR, BCR...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Economic indicators; Vegetables; Irrigation.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300460

ASYMMETRIC WETTED SECTOR ANGLE IN WATER DISTRIBUTION OF TRAVELING GUN IRRIGATION SYSTEMS
Provedor de dados: 70
Autores: Prado,Giuliani do; Colombo,Alberto.
ABSTRACT This work aimed to simulate the water distribution of traveler gun irrigation, working with asymmetrical wetted angles and in windy conditions. In the simulations of a sprinkler with uniform radial profile, the following were considered: i) wetted angles between 180 and 330°; ii) wetted angle asymmetries from 0 to 90°; iii) wind speeds from 0 to 4.5 m s-1; and iv) wind direction of 0, 45, and 90°. Christiansen uniformity coefficients (CU) were calculated for strip widths from 30 to 100% of the sprinkler wetted diameter (WD). Regardless of the wetted angle adjustment, irrigations under wind speeds of 4.5 m s-1 should be avoided and strip spacings of less than 50% WD provide high CU for wind speeds up to 3.0 m s-1. For any wind conditions,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Strip width; Travel path; Uniformity coefficient.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400443

VARIATION OF WATER QUALITY ALONG A RIVER IN AGRICULTURAL WATERSHED WITH SUPPORT OF GEOGRAPHIC INFORMATION SYSTEMS AND MULTIVARIATE ANALYSIS
Provedor de dados: 70
Autores: Wrublack,Suzana C.; Mercante,Erivelto; Boas,Marcio A. Vilas; Prudente,Victor H. R.; Silva,Jefferson L. G.
ABSTRACT This study demonstrates using remote sensing, geographic information systems and multivariate statistics to study water quality in an agricultural watershed. The monitoring of water quality in the watershed of Lontras's river in the southwestern region of the State of Paraná had been done in 2012 and 2013 with a multi-parameter probe in ten sites that were defined upstream and downstream watershed, during four different seasons. Mosaicked images were used from Google Earth, Digital Elevation Model and soil types of maps, defined as the explanatory variables. The definition of the areas of influence and multivariate statistical techniques, particularly the Redundancy Analysis (RDA), were used for the correlation between variables. In a spring area,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoprocessing; Mapping land use and occupation; Water quality.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100074

Produtividade de grãos verdes do feijão-caupi sob diferentes regimes hídricos
Provedor de dados: 70
Autores: Ramos,Herbert M. M.; Bastos,Edson A.; Cardoso,Milton J.; Ribeiro,Valdenir Q.; Nascimento,Fábio N. do.
O objetivo deste trabalho foi avaliar a produtividade de grãos verdes, os componentes de produção e a eficiência do uso da água do feijão-caupi, sob regimes hídricos. O experimento foi conduzido na Embrapa Meio-Norte, em Teresina - PI, entre setembro e novembro de 2009. Foram avaliadas cinco lâminas de irrigação, estabelecidas com base em frações da evapotranspiração de referência (25; 50; 75; 100 e 125% da ETo), e as cultivares BRS Guariba e BRSParaguaçudefeijão-caupi. Aplicou-se a irrigação por sistema de aspersão convencional fixo. Utilizou-se o delineamento experimental de blocos ao acaso, com quatro repetições e parcelas subdivididas (cultivares). As máximas produtividades de grãos verdes, 2.937,3 kg ha-1 (BRS Guariba) e 2.492,9 kg ha-1 (BRS...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vigna unguiculata; Feijão-verde; Lâminas de irrigação.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400008

Efeito da adição de cinza da casca de arroz em misturas cimento-casca de arroz
Provedor de dados: 70
Autores: Zucco,Loris L.; Beraldo,Antonio L.
A casca de arroz e sua cinza são abundantes e renováveis, podendo ser empregadas na obtenção de materiais de construção alternativos. O aumento do consumo desses resíduos poderia ajudar a minimizar os problemas ambientais provenientes da sua eliminação inadequada. Este trabalho teve o objetivo de avaliar a utilização de cinzas como carga mineral (filler). Todavia, a casca de arroz interferiu quimicamente no comportamento das misturas à base de cimento. Assim, diferentes misturas cimento-casca de arroz, com e sem adição de cinzas, foram avaliadas, a fim de destacar a influência de seus componentes (casca; cinza) que, de outra forma, poderiam ser excluídas ou subestimadas. Amostras cilíndricas (teste de compressão simples e de tração por compressão...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Casca de arroz; Cinza; Compósito.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200002

Effects of thermal environment and supplementation levels on the physiological parameters of moxotó goats in confined and semi-confined rising systems
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Gomes,Carlos A. V.; Medeiros,Ariosvaldo N.; Pimenta Filho,Edgard C.; Júnior,Valdi L.
The objective of this work was to determine the effect of environmental variables and supplementation levels on physiological parameters of Moxotó goats in confined and semi-confined rising systems, in the Brazilian semi-arid region. The semi-confined individuals were kept on a grass based diet during the day and arrested in the end of the afternoon. The confined animals were kept in a management center, receiving two diets composed by forage cactus and maniçoba hay into two different levels (0.5 and 1.5% of the body weight). Inside the management center and in the external environment the environmental comfort parameters were set high during the afternoon period characterizing a situation of thermal discomfort for the animals. During the morning the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermoregulation; Environmental variables; Native goat race; Semi-arid.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300001

Comparação de mapas temáticos de diferentes grades amostrais para a produtividade da soja
Provedor de dados: 70
Autores: Kestring‎,Franciele B. F.; Guedes,Luciana P. C.; Bastiani,Fernanda de; Uribe-Opazo,Miguel A.
RESUMO Este trabalho teve como objetivo comparar mapas temáticos construídos a partir de conjuntos de dados referentes à produtividade da soja, com diferentes grades amostrais regulares de 25x25 m; 50x50 m; 75x75 m e 100x100 m, utilizando técnicas de krigagem. No ajuste dos modelos teóricos a semivariâncias experimentais, utilizou-se para a estimação dos parâmetros o método de máxima verossimilhança. A comparação dos mapas temáticos foi realizada por meio dos índices de acurácia, obtidos a partir da matriz de erros. Foi verificado que fatores tais, como o tamanho amostral e a densidade amostral entre pontos, interferem na escolha do modelo teórico espacial, nas estimativas dos parâmetros e na construção dos mapas temáticos.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dependência espacial; Geoestatística; Máxima verossimilhança.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400733

Influência do tempo de uso sobre as características hidráulicas do microaspersor do grupo modular
Provedor de dados: 70
Autores: Sandri,Delvio; Mesquita,Márcio; Bessa,Kady S. E.; Prado,Lázaro C. R. A.
O desenvolvimento de novos equipamentos de irrigação e o aprimoramento dos já existentes, como dos microaspersores, devem considerar a avaliação das características hidráulicas, disposição adequada dos mesmos em condições de campo e interferência devido ao tempo de uso, garantindo índices de desempenho satisfatório. Nesse contexto, este trabalho teve o objetivo de determinar a equação vazão x pressão, o coeficiente de variação de fabricação - CVf e de vazão - CVq, a uniformidade de distribuição de água para diferentes graus de sobreposição do microaspersor do grupo modular de bocal laranja, novo e usado, sob funcionamento na posição invertida. O aumento do espaçamento entre microaspersores e entre laterais reduziu os índices de uniformidade em todas as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Produção de mudas; Irrigação localizada; Ambiente protegido.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600010

Spatial variability of leaf nutrient contents in a drip irrigated citrus orchard
Provedor de dados: 70
Autores: Armindo,Robson A.; Coelho,Rubens D.; Teixeira,Marconi B.; Ribeiro Junior,Paulo J.
This study aimed to evaluate the spatial variability of leaf content of macro and micronutrients. The citrus plants orchard with 5 years of age, planted at regular intervals of 8 x 7 m, was managed under drip irrigation. Leaf samples were collected from each plant to be analyzed in the laboratory. Data were analyzed using the software R, version 2.5.1 Copyright (C) 2007, along with geostatistics package GeoR. All contents of macro and micronutrients studied were adjusted to normal distribution and showed spatial dependence.The best-fit models, based on the likelihood, for the macro and micronutrients were the spherical and matern. It is suggest for the macronutrients nitrogen, phosphorus, potassium, calcium, magnesium and sulfur the minimum distances...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrus latifolia Tan.; Macronutrients; Micronutrients; Geostatistics.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300007

Efeitos de sistemas de preparo do solo na cultura da soja (Glycine max (L.) Merrill)
Provedor de dados: 70
Autores: Carvalho Filho,Alberto; Carvalho,Luís C. C.; Centurion,José F.; Silva,Rouverson P. da; Furlani,Carlos E. A.
Com o objetivo de avaliar o efeito de cinco equipamentos de preparo do solo sobre o desenvolvimento e a produtividade da cultura da soja (Glycine max L. (Merril)), foi conduzida uma pesquisa em Latossolo Vermelho distrófico, no município de Uberaba-MG, em delineamento experimental em blocos casualizados, com cinco tratamentos (escarificador, enxada-rotativa, arado de aivecas, arado de discos e grade aradora) e quatro repetições. Os sistemas de preparo do solo não mostraram diferenças para o número médio de dias para a emergência das plântulas, estande final, altura da primeira vagem e produtividade da cultura da soja. Os tratamentos com arado de disco, arado de aivecas e grade aradora proporcionaram as maiores populações iniciais da cultura. A altura das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Altura da planta; Altura da primeira vagem; Emergência.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300015

Manejo da fertirrigação e salinidade do solo no crescimento da cultura da beterraba
Provedor de dados: 70
Autores: SILVA,ALEXSANDRO O. DA; SILVA,ÊNIO F. F. E; KLAR,ANTÔNIO E.
Com o aumento da população mundial e a escassez dos recursos naturais, o uso eficiente dos fertilizantes torna-se necessário para uma agricultura intensiva. O experimento foi realizado em casa de vegetação no Departamento de Engenharia Rural da UNESP, no Município de Botucatu-SP. Os tratamentos foram provenientes da combinação dos fatores salinidade do solo (CE: 1,0; 3,0; 6,0; 9,0; 12,0 dS m-1), manejo da fertirrigação (M1=tradicional e M2=com controle da concentração iônica da solução do solo) e cultivares de beterraba (C1=Early Wonder e C2=Itapuã), em um esquema fatorial 5x2x2, com 4 repetições, em um delineamento em blocos. Durante todo o cultivo, foram avaliadas as seguintes variáveis: altura, diâmetro do pecíolo, comprimento e diâmetro das raízes das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Beta vulgaris L solução do solo; Condutividade elétrica.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200230

Development of an automated bench top electronic penetrometer
Provedor de dados: 70
Autores: Bianchini,Aloísio; Roque,Márcio W.; Rosa,Rodrigo P.
The aim of this study was to develop a an automated bench top electronic penetrometer (ABEP) that allows performing tests with high rate of data acquisition (up to 19,600 Hz) and with variation of the displacement velocity and of the base area of cone penetration. The mechanical components of the ABEP are: a supporting structure, stepper motor, velocity reducer, double nut ball screw and six penetration probes. The electronic components of ABEP are: a "driver" to control rotation and displacement, power supply, three load cells, two software programs for running and storing data, and a data acquisition module. This penetrometer presented in compact size, portable and in 32 validation tests it proved easy to operate, and showed high resolution, high...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Soil resistance to penetration; Velocity test; Cone index.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600012

PERFORMANCE OF FERTILIZER METERING MECHANISMS OF PLANTERS AS A FUNCTION OF LONGITUDINAL INCLINATION
Provedor de dados: 70
Autores: Garcia,Luiz C.; Diniz,Renan N.; Rocha,Carlos H.; Souza,Nátali M.; Weirich Neto,Pedro H.
ABSTRACT: Sowing occurs in agricultural areas with irregular relief, influencing the quality of seed and fertilizer distribution. The aim of this study was to analyze the performance of different fertilizer metering mechanisms of planters as a function of longitudinal inclination. The experimental design was a completely randomized design with five treatments and six replications. Treatments consisted of five longitudinal inclinations to the metering mechanism (−10, −5, 0, 5, and 10 degrees). The mass of fertilizer collected per minute was considered as a replication. We worked with two types of fertilizers: a mixture of granules and powder. Metering mechanisms used were a horizontal toothed rotor, helical without flow restrictor, helical with lateral...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Powder fertilizer; Operational efficiency; Granule mixtures; Variation in dosage.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601155

Estimativas de chuvas intensas para o Estado de Goiás
Provedor de dados: 70
Autores: Oliveira,Luiz F. C. de; Antonini,Jorge C. dos A.; Griebeler,Nori P.
A ausência de estações pluviográficas e de séries históricas longas, tem levado os Engenheiros à utilização de metodologias que permitam expressar a relação intensidade-duração-freqüência de precipitações críticas. Com o objetivo de estimar as alturas de chuvas intensas, associadas a uma duração e freqüência, desenvolveu-se uma rotina computacional para ajustar os parâmetros do modelo de Bell para alguns municípios do Estado de Goiás. Para tal, empregaram-se séries históricas de precipitações diárias e de relações intensidade-duração-freqüência disponíveis para alguns municípios. Determinou-se, também, a relação entre a precipitação de 60 minutos e 1 dia de duração, para um período de retorno de dois anos. As informações geradas neste trabalho foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelo de Bell; Drenagem; Escoamento superficial.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100003

Estimativa da evapotranspiração de referência (ETo padrão FAO), para Minas Gerais, na ausência de alguns dados climáticos
Provedor de dados: 70
Autores: ALENCAR,LEONIDAS P. DE; SEDIYAMA,GILBERTO C.; MANTOVANI,EVERARDO C.
A equação para determinar a evapotranspiração de referência (ETo), método de Penman-Monteith, parametrizada pela FAO (PM-FAO56), requer dados que, muitas vezes, não estão disponíveis na maioria das estações climatológicas. Para superar o problema da disponibilidade de dados climáticos, o boletim 56 da FAO propõe vários procedimentos para estimar a ETo na ausência dos dados de radiação, umidade relativa e velocidade do vento, e posterior substituição. Baseado nisto, o objetivo do presente estudo foi comparar a ETo estimada na ausência de dados de velocidade do vento ou da umidade relativa ou radiação solar com a ETo estimada, com os dados completos para várias localidades de Minas Gerais. A comparação foi realizada utilizando o coeficiente angular da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dados ausentes; Evapotranspiração de referência; Penman-monteith.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100039

Energetic analysis of landrace varieties and hybrids of corn produced in different technological levels of management
Provedor de dados: 70
Autores: Araujo,Alisson V. de; Brandão Junior,Delacyr da S.; Colen,Fernando.
The aim of this study was to analyze, under the energetic point of view, the cultivation of corn in three management systems (low, medium and high-tech), using two landrace varieties ('Argentino' and 'BR da Várzea'), a double hybrid cultivar (SHS 4080) and a simple hybrid (IAC 8333). Five performance indicators were used: energy efficiency, liquid cultural energy, cultural efficiency, energy balance and productive energy efficiency. From the perspective of family farming, it was verified the largest social importance of the systems under low and medium levels of technology, due to the increase employment capacity of rural labor. The liquid cultural energy and energy balance were more favorable for the system under high technological level, unlike cultural...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy balance; Cultural efficiency; Productive energy efficiency; Sustainability; Zea mays L.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400004

Níveis de ruído emitidos por uma recolhedora-trilhadora de feijão
Provedor de dados: 70
Autores: Souza,Luiz H.; Vieira,Luciano B.; Fernandes,Haroldo C.; Lima,Julião S. S.
Foram avaliados os níveis de ruído emitido por uma recolhedora-trilhadora de feijão. Empregou-se o delineamento experimental em blocos casualizados, com quatro repetições e esquema de parcelas subdivididas. Utilizaram-se três declividades do terreno (0 a 10; 10 a 20 e 20 a 30%) e três velocidades de operação (2,0; 2,5 e 3,0 km h-1) para compor as parcelas e subparcelas, respectivamente. Os dados foram interpretados pela análise de variância (teste F) e as médias comparadas pelo teste de Tukey, a 5% de probabilidade. Os níveis de ruído determinados ultrapassaram o limite de 85 dBA para oito horas de exposição diária estabelecido pela NR-15. Ocorreu aumento do nível de ruído com o incremento da declividade e com a diminuição da velocidade de trabalho.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Colheita mecânica; Ergonomia; Feijão.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300027

Errata: volume 29, número 4
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300020

MORTALITY, PRODUCTION AND QUALITY OF EGGS OF DIFFERENT REARING SYSTEMS
Provedor de dados: 70
Autores: Tavares,Bartira de O.; Pereira,Danilo F.; Salgado,Douglas D'Alessandro; Mac-Lean,Priscilla A. Bustos.
ABSTRACT The conventional production of eggs in cage systems is intense and compromises the laying hens welfare. More demanding consumer markets have been pushing to abolish the use of cages and thus provide better welfare in poultry laying. This research evaluated the mortality, production, and egg quality of two alternative production systems (free-range and organic free range free-range) and compared them with the conventional system. The research was carried out in two commercial poultry farms and the variables egg weight, shell egg resistance, Haugh unit, mortality and production were recorded during eight months. The results showed that the conventional system presented better production, lower mortality and better shell egg quality. The alternative...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry egg farming; Alternative egg production; Quality of eggs; Animal welfare.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400478

Methodology for spatialization of intense rainfall equation parameters
Provedor de dados: 70
Autores: Xavier,Alexandre C.; Cecílio,Roberto A.; Pruski,Fernando F.; Lima,Julião S. de S.
The aim of this study was to generate maps of intense rainfall equation parameters using interpolated maximum intense rainfall data. The study area comprised Espírito Santo State, Brazil. A total of 59 intense rainfall equations were used to interpolate maximum intense rainfall, with a 1 x 1 km spatial resolution. Maximum intense rainfall was interpolated considering recurrence of 2; 5; 10; 20; 50 and 100 years, and duration of 10; 20; 30; 40; 50; 60; 120; 240; 360; 420; 660; 720; 900; 1,140; 1,380 and 1,440 minutes, resulting in 96 maps of maximum intense rainfall. The used interpolators were inverse distance weighting and ordinary kriging, for which significance level (p-value) and coefficient of determination (R²) were evaluated for the cross-validation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Intensity-duration-frequency equation; Geostatistics; Hydrology.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300012

Characterization of soil parameters of two soils of Rio Grande do Sul in modeling the prediction of tractive effort
Provedor de dados: 70
Autores: Machado,Antônio L. T.; Trein,Carlos R.
The interaction between the soil and tillage tool can be examined using different parameters for the soil and the tool. Among the soil parameters are the shear stress, cohesion, internal friction angle of the soil and the pre-compression stress. The tool parameters are mainly the tool geometry and depth of operation. Regarding to the soils of Rio Grande do Sul there are hardly any studies and evaluations of the parameters that have importance in the use of mathematical models to predict tensile loads. The objective was to obtain parameters related to the soils of Rio Grande do Sul, which are used in soil-tool analysis, more specifically on mathematical models that allow the calculation of tractive effort for symmetric and narrow tools. Two of the main...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil cohesion; Soil-tool adhesion; Pre-compression stress.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400010

Desempenho de um aquecedor de água a biogás
Provedor de dados: 70
Autores: Silva,Fabio M. da; Lucas Junior,Jorge de; Benincasa,Mario; Oliveira,Ezequiel de.
Estudos foram desenvolvidos para dimensionar e adaptar o injetor do queimador principal de um aquecedor de água tipo acumulação de 75 L. O diâmetro do injetor foi redimensionado em função da pressão de serviço de 100 mm H2O e poder calorífico inferior do biogás de 21.600 kJ m-3 n, garantindo a manutenção da potência calorífica do equipamento de 20.900 kJ h-1. Os resultados demonstraram que o queimador adaptado operou com biogás adequadamente, com chama estável. A eficiência média do aquecedor foi de 68%, para ganho térmico de 36,7 ºC, correspondendo à temperatura final da água igual a 62,7 ºC, sendo consumido 0,796 m³n de biogás, aquecendo 75 L de água em 72 minutos.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogás; Poder calorífico; Digestão anaeróbia.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300005

Spray deposition and chemical control of the coffee leaf-miner with different spray nozzles and auxiliary boom
Provedor de dados: 70
Autores: GITIRANA NETO,JEFFERSON; CUNHA,JOÃO P. A. R. DA.
ABSTRACT The coffee crop requires great spray ability to penetrate into the plant canopy during the application of pesticides. The aim of this study was to evaluate the spray deposition on leaves of coffee plants and the chemical control of the leaf miner provided by the application of different spray nozzles, with and without the use of an auxiliary boom. The deposition on the upper, middle and lower parts of the plants and the losses to the soil were evaluated using a tracer quantified by spectrophotometer. We also evaluated the chemical control of the leaf miner, counting the larvae, after the application of the insecticides cartap and fenpropathrin. The trial was carried out in a randomized block design, with four replications, in a factorial model...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica L; Leucoptera coffeella; Spray; Application technology.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400656

Influência da relação volumoso: concentrado e do tempo de retenção hidráulica sob a biodigestão anaeróbia de dejetos de bovinos
Provedor de dados: 70
Autores: Orrico Júnior,Marco A. P.; Orrico,Ana C. A.; Lucas Júnior,Jorge de.
O objetivo deste trabalho foi avaliar as possíveis alterações existentes na composição e no processo de biodigestão anaeróbia dos dejetos de bovinos em fase de terminação alimentados com diferentes proporções de volumoso: concentrado e com diferentes tempos de retenção hidráulica (TRH). Foram utilizados 24 biodigestores batelada de bancada com 12 litros de capacidade, dos quais 12 foram abastecidos com dejetos de bovinos alimentados com a dieta 1 (60% volumoso:40% concentrado) e dieta 2 (40% volumoso:60% concentrado) e submetidos a 30, 60, 90 e 120 dias de TRH. A eficiência do processo de biodigestão anaeróbia foi avaliada pelas reduções de sólidos totais, sólidos voláteis, fibra em detergente neutro, fibra em detergente ácido, celulose e número mais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dietas; Biodigestor; Energia; Metano.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300003

SPATIAL AUTOCORRELATION OF PHYSICAL ATTRIBUTES OF AN OXISOL
Provedor de dados: 70
Autores: Oliveira,Job T. de; Oliveira,Rubens A. de; Cunha,Fernando F. da; Santos,Eduardo S. dos.
ABSTRACT Studies that seek to identify a smaller number of soil attributes that represent others can generate less expenditure of time and financial resources for monitoring cultivated areas. Thus, this study aimed to analyze the spatial distribution and spatial autocorrelation of physical attributes of an Oxisol (Latossolo Vermelho Amarelo, Brazilian Soil Classification System). The evaluated attributes consisted of soil density (SD), total porosity (TP), free porosity (FP), field capacity (FC), permanent wilt point (PW), and total water availability (TW). Semivariogram adjustments and semivariance estimates were performed to characterize the structure and magnitude of the spatial dependence of soil attributes. The attributes were distributed on thematic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Spatial dependence; Geostatistics; Moran index.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200255

Seasonality of net radiation in two sub-basins of Paracatu by the use of modis sensor products
Provedor de dados: 70
Autores: Lima,Evaldo de P.; Sediyama,Gilberto C.; Silva,Bernardo B. da; Gleriani,José M.; Soares,Vicente P.
The net radiation (Rn) represents the main source of energy for physical and chemical processes that occur in the surface-atmosphere interface, and it is used for air and soil heating, water transfer, in the form of vapor from the surface to the atmosphere, and for the metabolism of plants, especially photosynthesis. If there is no record of net radiation in certain areas, the use of information is important to help determine it. Among them we can highlight those provided by remote sensing. In this context, this work aims to estimate the net radiation, with the use of products of MODIS sensor, in the sub-basins of Entre Ribeiros creek and Preto River, located between the Brazilian states of Goiás and Minas Gerais. The SEBAL (Surface Energy Balance...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Meteorological information; River basins; Remote sensing.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600020

Relative reduction in annual soil loss in micro watersheds due to the relief and forest cover
Provedor de dados: 70
Autores: Mingoti,Rafael; Vettorazzi,Carlos A.
With the intense debate, in Brazil, between landowners and public agencies about the amount of area with forest cover needed in different regions, there is an increase of the need for provision of technical data used as a basis for decision making. One of the criteria to evaluate the effect of forest cover in protecting water resources is the soil loss, which leads to several consequences on the environment, including the silting of the rivers. Therefore, this study aimed to evaluate the reduction in the soil loss in micro watersheds with different reliefs, size and location of forest cover, in the Corumbataí River watershed, in the state of São Paulo, using the Revised Universal Soil Loss Equation (RUSLE) in a GIS environment. For this study, 18...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: GIS; RUSLE; Legal reserve; Permanent preservation area.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600017

NUTRIENT REMOVAL FROM SWINE WASTEWATER IN A COMBINED VERTICAL AND HORIZONTAL FLOW CONSTRUCTED WETLAND SYSTEM
Provedor de dados: 70
Autores: Bôas,Regina B. Vilas; Fia,Ronaldo; Fia,Fátima R. L.; Campos,Alessandro T.; Souza,Gabriela R. de.
ABSTRACT This study aimed to assess the performance of a combined vertical flow (VFCW) and horizontal subsurface-flow (HFCW) constructed wetland systems built on a pilot scale and submitted to different configurations and organic load application rates of pre-treated swine wastewater (SWW) in anaerobic systems on the nitrogen and phosphorus removal. The average values of redox potential in the systems were between anoxic and aerobic conditions, favoring an increased nitrate concentration in VFCW. Nitrogen removal by VFCW–HFCW system can be considered as satisfactory, reaching removal values of 75%. VFCW and HFCW proved to be limited in phosphorus removal, reaching values of 48%.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cynodon spp; Phosphorus; Nitrogen; Post-treatment; Typha sp.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300411

Metodologia para obtenção do hidrograma de escoamento superficial em encostas e canais. Parte II: modelo computacional e análise de sensibilidade
Provedor de dados: 70
Autores: Silva,José M. A.; Pruski,Fernando F.; Silva,Demetrius D.; Cecílio,Roberto A.
Estimativas de vazão máxima de escoamento superficial são necessárias para o projeto de obras hidráulicas em bacias urbanas e rurais. A dificuldade em aplicar os procedimentos disponíveis para calcular a variação do escoamento superficial com o tempo e de seu valor máximo deve-se à inexatidão dos métodos usados para esse objetivo e à variabilidade nos resultados que podem ser obtidos por profissionais que usem o mesmo procedimento. Dessa forma, a investigação de um método que produza estimativas confiáveis da vazão máxima e do hidrograma de escoamento superficial é de grande interesse. Neste trabalho, desenvolveu-se e avaliou-se a sensibilidade de um software (HIDROGRAMA 2.1) que permite a obtenção do hidrograma de escoamento superficial, da vazão máxima e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelagem hidrológica; Conservação de água e solo.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300006

Técnicas de mineração de dados para análise da precipitação pluvial decenal no Rio Grande do Sul
Provedor de dados: 70
Autores: Boschi,Raquel S; Oliveira,Stanley R. de M; Assad,Eduardo D.
O objetivo deste trabalho foi analisar o comportamento espaçotemporal da precipitação pluvial no Estado do Rio Grande do Sul, entre os decênios de 1987-1996 e 1997-2006, por meio de técnicas de mineração de dados. As séries históricas foram adquiridas no sistema de informações hidrológicas Hidroweb. A metodologia utilizada teve como base o modelo CRISP-DM (Cross Industry Standard Process for Data Mining). Foram definidas áreas pluviometricamente homogêneas para os decênios de 1987-1996 e 1997-2006. Em seguida, pela sobreposição dos agrupamentos obtidos para os dois períodos, encontraram-se seis zonas comuns aos dois decênios (A a F). As alterações ocorridas foram avaliadas nas seguintes escalas temporais: anual, sazonal e mensalmente. Os resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chuva; Agrupamento; Zonas pluviometricamente homogêneas.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600016

Georeferenced database generation with the purpose of hydrologic molding in reservoirs of the hydrographic basin of Jaguaribe river in the state of Ceará, Brazil
Provedor de dados: 70
Autores: Leão,Raimundo A. de O.; Soares,Antônio A.; Teixeira,Adunias dos S.; Silva,Demetrius D. da.
The edafoclimatic conditions of the Brazilian semiarid region favor the water loss by surface runoff. The state of Ceará, almost completely covered by semiarid, has developed public policies for the construction of dams in order to attend the varied water demand. Several hydrological models were developed to support decisive processes in the complex management of reservoirs. This study aimed to establish a methodology for obtaining a georeferenced database suitable for use as input data in hydrological modeling in the semiarid of Ceará. It was used images of Landsat satellite and SRTM Mission, and soil maps of the state of Ceará. The Landsat images allowed the determination of the land cover and the SRTM Mission images, the automatic delineation of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoprocessing; GIS; Hydrologic models; Curve number; Jaguaribe River; Semiarid.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200017

Backpressure effects on the flow-pressure relation of driplines
Provedor de dados: 70
Autores: Thebaldi,Michael S; Lima,Luiz A; Almeida,Willian F. de; Andrade,Rafaella R.
ABSTRACT For drip irrigation design and management, it is necessary to know the relation between flow and pressure acting on emitters. In the case of subsurface drip irrigation, the backpressure phenomenon may change the hydraulic characteristics of emitters. Thus, this study aimed at determining such relationship between flow and pressure of different driplines in surface and subsurface conditions; aiming to find possible differences in hydraulic behavior. We tested four emitter types; two pressure compensating (D5000 and Hydro PCND) and two non-pressure compensating (TalDrip and Jardiline). Emitter flow rates were attained in atmospheric conditions and submerged in water, in which submergence levels represented backpressure. Assays were performed using...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Discharge exponent; Proportionality constant; Trickle irrigation.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100055

Heat loss in one day old pullets inside a hatchery
Provedor de dados: 70
Autores: Nääs,Irenilza de A.; Graciano,Daniela E.; Garcia,Rodrigo G.; Santana,Mayara R. de; Neves,Diego P.
After hatching, pullets are transported to brooding area and vaccinated. One day old chicks have not already developed thermoregulation ability; thus, brooding temperature variations may affect pullet quality leading to broiler meat production losses. This research aimed to calculate sensible heat loss in one day old pullets in hatching area and vaccination room. Ten one day old pullets were randomly selected from hatching area of a commercial hatchery. Infrared images were used to calculate bird surface temperature. Exposure areas for the two conditions were quantified, and both air temperature and wind speed was recorded. Total sensible heat loss was calculated as heat loss by radiation plus heat loss by convection. It was found that heat transfer occurs...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensible heat; Post-hatching; Infrared thermography.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400001

Caracterização da estrutura fundiária do município de Bandeirantes - PR, utilizando geoprocessamento
Provedor de dados: 70
Autores: Reis,Luiz C.; Reis,Teresinha E. S.; Abi Saab,Otávio J. G.
As técnicas de sensoriamento remoto e o uso dos Sistemas de Informações Geográficas (SIG) facilitam a elaboração de mapas temáticos. Mapas com informações detalhadas são importantes instrumentos para que os municípios conheçam melhor sua realidade. O trabalho foi desenvolvido no município de Bandeirantes, Estado do Paraná, Brasil, visando a analisar sua estrutura fundiária, baseada nas classes de tamanho dos imóveis rurais. A partir de mapas de imóveis rurais e de cartas topográficas do IBGE, obteve-se o mapa fundiário digital do município. Imagens orbitais e fotografias aéreas foram utilizadas para o ajuste das linhas divisórias dos imóveis, cuja validação se deu por incursões a campo. O número e o tamanho dos imóveis de 1950 foram comparados com dados de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: SIG; Módulo rural; Estimador Kernel.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200015

Forças de atrito em silos verticais de paredes lisas em diferentes relações altura/diâmetro
Provedor de dados: 70
Autores: Lopes Neto,José P.; Nascimento,José W. B. do; Silva,Rafael C.
Para desenvolver um projeto de silo, é necessário que fatores como o fluxo e cargas sejam criteriosamente avaliados. Portanto, como objetivo principal deste trabalho destacam-se a mensuração, a análise e a comparação com normais internacionais das forças de atrito nas paredes de um silo cilíndrico de fundo plano. Para a medição das forças de atrito, foram utilizados dois conjuntos de três células de carga e um sistema de aquisição de dados. O silo foi carregado concentricamente com areia seca e descarregado concêntrica e excentricamente a partir de duas excentricidades através de orifícios de 80 mm de diâmetro. Os resultados evidenciam que o modelo de silo-piloto é adequado para a medição das forças de atrito nas paredes e que os valores teóricos propostos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Normas internacionais; Fundo plano; Excentricidade; Descarregamento; Silo cilíndrico.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100002

Procedimento fuzzy aplicado à avaliação da insalubridade em atividades agrícolas
Provedor de dados: 70
Autores: Yanagi Junior,Tadayuki; Schiassi,Leonardo; Abreu,Lucas H. P.; Barbosa,Jackson A.; Campos,Alessandro T.
Diante do alto grau de mecanização a que as atividades agrícolas estão sendo submetidas, objetivou-se, com esta pesquisa, desenvolver um modelo fuzzy capaz de avaliar e classificar o nível de insalubridade em diversos ambientes de trabalho. O modelo desenvolvido tem como variáveis de entrada: o índice de bulbo úmido e temperatura de globo (IBUTG, °C), o nível de ruído (dBA), a taxa de metabolismo (W m-2) e o tempo de descanso (%) e, como variável de saída, o índice de bem-estar humano (IBEH). O método de inferência utilizado foi o de Mandani e, na defuzificacão, utilizou-se o método do centro de gravidade. O sistema de regras foi desenvolvido com base nas combinações das variáveis de entrada. Foram definidas 400 regras com pesos iguais a 1, sendo que, na...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bem-estar humano; Modelagem matemática; Sistema especialista.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300002

Distribuição longitudinal de sementes de soja e características físicas do solo no plantio direto
Provedor de dados: 70
Autores: Cortez,Jorge W.; Furlani,Carlos E. A.; Silva,Rouverson P. da; Lopes,Afonso.
As técnicas do plantio direto são complementares às atuais técnicas de conservação do solo, que envolvem menor mobilização e permanência de cobertura vegetal na superfície do solo. O trabalho foi realizado na UNESP - Jaboticabal, de novembro de 2003 a março de 2004, e teve como objetivo avaliar o efeito de culturas, manejos e marchas do trator na semeadura da soja no plantio direto. O delineamento utilizado para instalação do experimento foi em blocos ao acaso, no esquema de parcelas subsubdivididas, com quatro repetições. Foram analisados: estande inicial, distribuição longitudinal de plantas, resistência mecânica à penetração, densidade e teor de água no solo. O estande inicial não foi influenciado pelos tratamentos. A distribuição longitudinal das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Velocidade; Manejo; Mecanização agrícola.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200019

Aplicação de danos mecânicos em abacates e seus efeitos na qualidade dos frutos
Provedor de dados: 70
Autores: Sanches,Juliana; Durigan,José F.; Durigan,Maria F. B.
Este trabalho teve por objetivo avaliar o efeito da aplicação de danos mecânicos por impacto, compressão e corte em abacates 'Geada'. O trabalho consistiu em duas etapas: na primeira, o impacto foi aplicado deixando-se os frutos caírem, em queda livre, de 1,5 m a 3,0 m, com intervalo de 0,5 m; na compressão, os frutos sofreram a ação dos pesos: 6 kg por 12 horas e 12 kg por 6 horas. Para os cortes, foram realizados quatro cortes com 80 mm de comprimento e 4 mm de profundidade. Na segunda etapa, para a compressão, utilizou-se peso de 12 kg por tempo maior (24 h). No impacto, foi aplicada queda de 2,0 m, e os cortes, realizados da mesma maneira que na primeira etapa. Os efeitos de cada dano foram avaliados nos frutos armazenados sob condição ambiente quanto...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compressão; Corte; Impacto; Persea americana.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100017

Comportamento das formas de nitrogênio em solo cultivado com milho irrigado com água residuária da suinocultura
Provedor de dados: 70
Autores: Sampaio,Silvio C.; Fiori,Marciane G. S.; Opazo,Miguel A. U.; Nóbrega,Lúcia H. P.
A utilização de água residuária com características químicas capazes de complementar ou substituir a adição de fertilizantes químicos tem beneficiado amplamente, tanto em regiões onde ocorre a necessidade de se fazer uso de irrigação, quanto em solos que necessitam de fertilizantes. Porém, uma preocupação ambiental e agronômica deve sempre persistir no uso dessa técnica. Dessa forma, o presente trabalho teve como objetivo avaliar o comportamento das formas de nitrogênio no material percolado e no solo quando cultivado com milho (Zea mays L.) irrigado com água residuária da suinocultura (ARS), em quatro taxas de aplicação (112,5; 225; 337,5 e 450 kg N ha-1) e adubação convencional (AD), em dois níveis (15 e 25 kg N ha-1). O trabalho foi desenvolvido com a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Efluente; Meio ambiente; Contaminação.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100015

Demanda tractiva en función de la resistencia mecánica del suelo a la penetración
Provedor de dados: 70
Autores: Borges,Pedro H. M.; Bianchini,Aloísio; Maia,João C. S.; Fernándes,Haroldo C.; Mendoza,Zaíra M. S. H.
No presente estudo, foram elaborados modelos empíricos para determinar a força de tração demandada por arados de discos, escarificadores e semeadoras adubadoras, em função da resistência mecânica do solo à penetração. A média da referida resistência, determinou-se até as profundidades de 25; 35 e 15 cm, em correspondência com as regulagens do arado de discos, escarificador e semeadora adubadora. O ajuste foi verificado de acordo com o coeficiente de determinação, gráficos de dispersão, análise residual e teste t (Student). Com base nessas análises, confirmou-se a normalidade dos resíduos, e foram estabelecidos intervalos de confiança com 95% de probabilidade. Os valores estimados e obtidos experimentalmente não discreparam significativamente. Concluiu-se...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Desempenho de máquinas; Modelos empíricos; Modelos não lineares.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200009

Variabilidade espacial da emissão de CO2 em Latossolos sob cultivo de cana-de-açúcar em diferentes sistemas de manejo
Provedor de dados: 70
Autores: Panosso,Alan R.; Pereira,Gener T.; Marques Júnior,José; La Scala Júnior,Newton.
Neste trabalho, foi determinada a estrutura da variabilidade espacial da emissão de CO2, temperatura e umidade de solos desprovidos de vegetação em duas localidades sob cultivo da cana-de-açúcar, em sistemas de manejos de cana crua e de cana queimada, no nordeste do Estado de São Paulo. A emissão de CO2 e a temperatura do solo foram registradas utilizando-se de câmara de fluxo portátil e sensor de temperatura do sistema LI-6400. A umidade foi avaliada utilizando sistema portátil TDR. A maior emissão foi observada no local sob manejo de cana queimada, com valor médio de 2,05 μmol m-2 s-1, porém a dependência espacial na emissão de CO2 foi encontrada somente na área sob manejo de cana crua. Os mapas de krigagem da emissão de CO2, temperatura e umidade do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Respiração do solo; Geoestatística; Manejo da cana-de-açúcar.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200003

Application of x-ray computed tomography in the evaluation of soil porosity in soil management systems
Provedor de dados: 70
Autores: Beraldo,José M. G.; Scannavino Junior,Francisco de A.; Cruvinel,Paulo E.
The study aimed to evaluate a methodology to quantify the porosity of the soil using computed tomography in areas under no-tillage, conventional tillage and native forest. Three soil management systems were selected for the study: forest, conventional tillage and no-tillage. In each soil management system, undisturbed soil samples were collected in the surface layer (0.0 to 0.10 m). The tomographic images were obtained using a X-ray microtomography. After obtaining the images, they were processed, and a methodology was evaluated for image conversion into numerical values. The statistical method which provided the greatest accuracy was the percentile method. The methodology used to analyze the tomographic image allowed quantifying the porosity of the soil...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Precision farming; Image processing; X-ray microtomography; Macroporosity.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600012

Ação dos meios reativos peróxido de hidrogênio e carvão ativado na remediação de solos contaminados por BTEX
Provedor de dados: 70
Autores: Lourenço,Edneia S. De O.; Cardoso,Décio L.; Mateus,Fabiano H.
Esta pesquisa teve como objetivo avaliar o potencial das barreiras reativas permeáveis (BRP) na redução dos hidrocarbonetos aromáticos BTEX (Benzeno, Tolueno, Etilbenzeno e Xilenos) no solo, provenientes de vazamento de gasolina. O experimento foi conduzido em escala laboratorial, simulando dois tipos de BRP, denominadas de AS (H2O2 + solo) e de ACA (H2O2 + carvão ativado). Foram determinadas as concentrações dos BTEX na amostra da gasolina ao entrar na BRP e no percolado, em tempos de retenção preestabelecidos de 24; 36; 48; 60; 72 e 84 h, utilizando cromatografia gasosa. Os resultados obtidos mostraram que as duas barreiras reativas reduziram a concentração dos BTEX, próximo a níveis permissíveis de contaminação e de prevenção, e a barreira ACA...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gasolina; Contaminação; Barreiras reativas.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100014

Energetic efficiency of an agricultural tractor in function of tire inflation pressure
Provedor de dados: 70
Autores: Monteiro,Leonardo de A.; Albiero,Daniel; Lanças,Kleber P.; Bueno,André V.; Masiero,Fabricio C.
The tire inflation pressure, among other factors, determines the efficiency in which a tractor can exert traction. It was studied the effect of using two tire inflation pressures, 110.4 kPa in the front and rear wheels, 124.2 kPa in the front wheel and 138 kPa in the rear wheels, the energetic efficiency of an agricultural tractor of 147 kW of engine power, in the displacement speed of 6.0 km.h-1, on track with firm surface, with the tractor engine speed of 2000 rpm. For each condition of the tire pressure, the tested tractor was subjected to constant forces in the drawbar of 45 kN and 50 kN, covering 30 meters. It was used a randomized complete block with a 2x2 factorial arrangement (tire pressure and drawbar power) with four replications, totaling 16...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuel consumption; Slippage; Traction test.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400015

Codigestão anaeróbia dos dejetos de bovinos leiteiros e óleo de descarte
Provedor de dados: 70
Autores: Orrico,Ana C. A.; Lopes,Walter R. T.; Manarelli,Débora M.; Orrico Junior,Marco A. P; Sunada,Natália da S.
RESUMO Este trabalho foi realizado com o intuito de se avaliarem a codigestão dos dejetos de bovinos leiteiros e óleo de descarte, por meio das produções específicas de biogás, reduções dos teores de sólidos totais (ST) e voláteis (SV), da demanda química de oxigênio (DQO) e fibra em detergente neutro (FDN). Utilizaram-se 28 biodigestores batelada, abastecidos com substratos contendo 4% de ST e compostos por dejetos de bovinos leiteiros, óleo de descarte (nas doses de 0; 2; 4; 6; 8; 10 e 12% dos STs do substrato e representado pelo resíduo de frituras que foi doado por pastelaria), inóculo e água para diluição. As máximas reduções de SV, DQO e FDN, além das produções específicas de biogás, foram obtidas por modelos quadráticos de predição, estimando-se,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biodigestor; Biogás; Bovinocultura.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300537

The effects of irrigation management on floral induction of ‘Tommy Atkins' mango in bahia semiarid
Provedor de dados: 70
Autores: Faria,Leandro N.; Soares In memoriam,Antônio A.; Donato,Sérgio L. R.; Santos,Marcelo R. dos; Castro,Luciana G.
ABSTRACT This study aimed to evaluate reduction strategies of irrigation for proper management of floral induction and production of 'Tommy Atkins' mangoes, in the semiarid region of the Bahia state, Brazil. Five treatments with reduced irrigation levels based on crop evapotranspiration (ETc) were applied in two development stages, FI - flowering and FII – fruiting. Water depths were T1 - 0% of ETc in FI and 100% in FII; T2 - 25% of ETc in FI and 100% in FII; T3 - 50% of ETc in FI and 100% in FII; T4 - 75% of ETc in FI and 100% in FII; and T5 - 100% of ETc in FI and FII. The treatments were arranged in a randomized complete block design with six replications. Photosynthesis and transpiration rates in phases FI and FII were larger at 8 am than at 2 pm,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mangifera; Controlled water deficit; Irrigation strategies.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300387

Métodos de preparo do solo: alterações na rugosidade do solo
Provedor de dados: 70
Autores: Carvalho Filho,Alberto; Centurion,José F.; Silva,Rouverson P. da; Furlani,Carlos E. A.; Carvalho,Luís C. C.
Procurando relacionar os métodos de preparo de solo com alguns dos efeitos em um Latossolo Vermelho distrófico, foi conduzido, no município de Uberaba - MG, um trabalho utilizando-se do delineamento experimental em blocos casualizados, com cinco tratamentos e quatro repetições, tendo como tratamentos os preparos de solo: escarificador, enxada rotativa, arado de aivecas, grade aradora e arado de discos. Foram avaliadas a área mobilizada do solo e a área de elevação, tendo-se como referência a superfície natural do solo antes da mobilização, o empolamento do solo, a espessura média da camada mobilizada, o índice de rugosidade e a modificação da rugosidade do solo para a comparação da rugosidade antes e após sua mobilização. O escarificador proporcionou menor...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Área de elevação; Área mobilizada; Índice de rugosidade.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100017

CHICKEN MANURE AND LUMINOUS AVAILABILITY INFLUENCE GAS EXCHANGE AND PHOTOCHEMICAL PROCESSES IN Alibertia edulis (Rich.) A. Rich SEEDLINGS
Provedor de dados: 70
Autores: Santos,Cleberton C.; Bernardes,Rodrigo da S.; Goelzer,Ademir; Scalon,Silvana de P. Q.; Vieira,Maria do C.
ABSTRACT Information on the physiological responses of native plants from the Brazilian Cerrado regarding the use of chicken manure and luminosities are important for their silvicultural management. Thus, aimed to evaluate the effect of chicken manure and luminous availability on the photosynthetic metabolism of Alibertia edulis (Rich) A. Rich. The experiment was carried out in pots, testing five doses of chicken manure – CM (0.00, 2.08, 4.16, 6.24 and 8.32 g kg-1) incorporated at Dystroferric Red Latosol, and two luminous environmental (full sun and 50% shaded). The higher CO2 assimilation rate, stomatal conductance and carboxylation efficiency of Rubisco occurred in seedlings grown in full sun. The seedlings showed higher photochemical indicators in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Marmelo-do-cerrado; Chlorophyll-a fluorescence; Physiological adjustments; Organic residue; Shaded.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400420

EFFECT OF TRANSPORTATION DISTANCE ON WEIGHT LOSSES IN PIGS FROM DEHYDRATION
Provedor de dados: 70
Autores: Machado,Sivanilza T.; Nääs,Irenilza De A.; Mollo Neto,Mario; Vendrametto,Oduvaldo; Reis,João G. M. Dos.
ABSTRACT: The increasing of global demand for food has required more efficiency in the production process. Transportation represents a source of body dehydration for pigs transported from farm to slaughterhouses. This study aimed to evaluate the effects of the distances on the body dehydration of pigs transported to slaughter in tropical conditions. We analyzed 350 pigs shipments with a total of 68,588 heads using statistical software SAS by anova, means and corr procedures. The results showed a liveweight loss estimated at 12% which was increased gradually as the distance increased as pigs were deprived of water for a long time. The most cost-effective distance for the pigs' transportation under tropical condition is within the range below 100 km, where...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pre-slaughter logistics; Tropical conditions; Live weight losses; Animal welfare.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601229

Avaliação física do tomate de mesa 'Romana' durante manuseio na pós-colheita
Provedor de dados: 70
Autores: Ferreira,Marcos D.; Cortez,Luís A. B.; Honório,Sylvio L.; Tavares,Marcelo.
As perdas na pós-colheita para tomate de mesa são altas, e esta pesquisa teve como objetivo quantificá-las, avaliando-se o efeito do manuseio e transporte na qualidade física dos frutos, cultivar Romana, nas etapas de colheita, pesagem e transporte para o galpão de beneficiamento. Tomates foram colhidos em caixas plásticas de colheita, transportados para um ponto de pesagem e, em seguida, enviados para um galpão de beneficiamento e classificação. Utilizaram-se como testemunha frutos retirados diretamente da planta. Os parâmetros observados foram: perda de peso e incidência de danos físicos originados em cada etapa, avaliando-se a aparência externa dos frutos após armazenamento por 21 dias. Observou-se aumento progressivo na perda de peso e incidência de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lycopersicun esculentum; Pós-colheita; Danos físicos.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100034

IDENTIFICATION OF DESERTIFICATION- SENSITIVE AREAS IN THE BRAZILIAN NORTHEAST THROUGH VEGETATION INDICES
Provedor de dados: 70
Autores: Ferreira,Thomás R.; Pace,Frederico T. Di; Silva,Bernardo B. Da; Delgado,Jéssica R.
ABSTRACT: The aim of this study was to identify areas susceptible to drought and under desertification in the Brazilian Northeast, more specifically in the states of Alagoas, Pernambuco, and Sergipe. The study was based on the 2000-2014 time period, relative frequency, Vegetation Condition Index (VCI) dataset derived from MOD13Q1 products (vegetation indices derived from the Moderate Resolution Imaging Spectroradiometer sensor). The areas located within the desertification nucleus of Cabrobó, in the southwestern of Pernambuco and surrounding the Águas Belas municipality were considered susceptible to drought and desertification. Some municipalities in the countryside of Alagoas showed a very low relative frequency of VCI data (45-50%), and occurrence of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Degradation; Vegetation; Remote sensing.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601190

Uso da fertirrigação e teores de macronutrientes em planta de pimentão
Provedor de dados: 70
Autores: Marcussi,Francisco F. N.
Este estudo teve o objetivo de determinar os teores de macronutrientes (N, P, K, Ca, Mg e S) nos diferentes órgãos do híbrido de pimentão Elisa, sob fertirrigação e ambiente protegido, por meio de coletas de plantas durante o ciclo. Ao final do experimento, obtiveram-se os teores dos macronutrientes no fruto, folha, caule, raiz e na planta como um todo, em cada etapa de crescimento. A fertilização no ciclo estudado, 140 dias, foi feita via irrigação localizada (gotejamento). O experimento foi desenvolvido nas dependências do Departamento de Recursos Naturais - Ciência do Solo, FCA-UNESP, Câmpus de Botucatu - SP, e constou de oito tratamentos (épocas de coleta de planta: 0; 20; 40; 60; 80; 100; 120 e 140 dias após o transplante das mudas) e quatro...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gotejamento; Concentrações de macronutrientes; Capsicum annuum L.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300009

ENERGY EFFICIENCY OF A CENTER PIVOT IRRIGATION SYSTEM
Provedor de dados: 70
Autores: Barbosa,Brenon D. S.; Colombo,Alberto; Souza,João G. N. de; Baptista,Victor B. da S.; Araújo,Ana C. S. de.
ABSTRACT This study aimed to evaluate the energy efficiency of a center pivot irrigation system operating in a terrain of variable topography. Values of Pumping Energy Efficiency (PEE), Supply Energy Efficiency (SEE), Global Energy Efficiency (GEE) and Specific Energy (Es in kWh m-3) computed at 18 different angular positions of the lateral line were used as energy efficiency indicators. An ultrasonic flow meter, digital pressure transducers and a power quality analyzer were used in order to evaluate hydraulic (total system flow-Q and total dynamic head-TDH) and electrical parameters (active electrical power - AEP) of the center pivot pumping unit that were required for evaluating the selected energy efficiency indictors. Topographic elevations of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy performance; Pumping unit; Performance indicators.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200284

Microencapsulation of pequi pulp by spray drying: use of modified starches as encapsulating agent
Provedor de dados: 70
Autores: Santana,Audirene A.; Oliveira,Rafael A. de; Kurozawa,Louise E.; Park,Kil J.
The aim of this study was to evaluate the microencapsulation of pequi pulp by spray drying. A central composite rotational design was used in order to evaluate the effect of the independent variables: inlet air temperature, surfactant concentration and modified starch concentration. The dependent variables were assumed as yield of the process and the product features microencapsulated. A selection of the best process condition was performed to obtain the best condition of a product with the highest vitamin C and carotenoids content. Powders showed moisture content below 2%. The experimental values of hygroscopicity, yield, water activity, total carotenoids and vitamin C powders ranged from 7.96 to 10.67 g of adsorbed water/100g of solids, 24.34 to 49.80%,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Caryocar brasiliense; Spray drying; Experimental design; Encapsulation; Morphology.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500017

Modelos de transferência de metal pesado na cana-de-açúcar adubada com composto de lixo urbano
Provedor de dados: 70
Autores: Silva,Fábio C. da; Bergamasco,Alessandra F.; Vendite,Laercio L.
A pesquisa aborda a reciclagem do composto de lixo urbano (CLU) como fertilizante alternativo na cana-de-açúcar e como solução social e ambiental ao acúmulo de resíduos sólidos nos centros urbanos. Utilizou-se da modelagem matemática para conhecer a dinâmica dos metais pesados, visando ao estabelecimento de critérios e procedimentos para o uso seguro do CLU, limitado pela quantidade desses elementos. Foram construídos modelos compartimentais a partir de dados de experimentos em condições controladas e parcialmente validados com dados de campo. Esse modelo descreveu a transferência de metais pesados no sistema solo-raiz-parte aérea para a cana-de-açúcar. Pôde-se concluir, pelas condições desta pesquisa, que o metal mais preocupante foi o níquel, pois...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Composto orgânico; Modelo matemático; Meio ambiente.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100005

Época de semeadura da soja para a região de Dourados - MS, com base na deficiência hídrica e no fotoperíodo
Provedor de dados: 70
Autores: Fietz,Carlos R.; Rangel,Marco A. S.
O objetivo deste trabalho foi definir a época de semeadura da soja para a região de Dourados - MS, em função da deficiência hídrica e do fotoperíodo. Foram avaliadas três épocas de semeadura (15 de outubro, 15 de novembro e 15 de dezembro), utilizando-se de série de 20 anos de dados. A deficiência hídrica da soja foi estimada por meio de balanço hídrico-climatológico diário sequencial, e o fotoperíodo foi calculado em função da latitude e da data. O atraso da semeadura reduziu o déficit hídrico. Analisando-se conjuntamente os fatores déficit hídrico e fotoperíodo, concluiu-se que semeaduras da soja em novembro são mais indicadas para a região de Dourados.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycine max; Balanço hídrico; Estresse hídrico.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400006

Removal of organic matter and nutrients from slaughterhouse wastewater by using Eichhornia crassipes and evaluation of the generated biomass composting
Provedor de dados: 70
Autores: Mees,Juliana B. R.; Gomes,Simone D.; Boas,Márcio A. Vilas; Fazolo,Ajadir; Sampaio,Sílvio C.
The objective of this research was to evaluate the performance of the aquatic macrophyte Eichhornia crassipes applied in situ in a slaughter house treatment system, located in the west of the Paraná state, Brazil, regarding the nutrients removal and organic matter. Moreover, it aimed to obtain data from the production, management and composting practices of the biomass generated in the system. During 11 months of macrophytes development, physic and chemical parameters were monitored and plant density was controlled by periodical removal of excess biomass, which was weekly monitored and it is expressed in kg of aquatic plant per m² covered area. The degradation of the macrophytes removed from the treatment system was evaluated at the pilot scale in eight...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agroindustrial effluent; Nutrient removal; Water hyacinth; Composting; C:N ratio.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300013

Air flow humidification for air-assisted boom sprayer
Provedor de dados: 70
Autores: Stanislavski,Wilson M.; Antuniassi,Ulisses R.; Chechetto,Rodolfo G.
The air-assisted ground spray is fairly widespread. However, due to the unpredictable weather conditions, the operational efficiency is impaired by stops on grounds of low humidity and high temperatures. The aim of this work was to assess an air humidification method and evaluate its impact on temperature and air humidity for the air curtain of the air-assisted sprayer. With respect to relative air humidity, it has increased in 6.59%, being the maximum change when inserting 1.92 L min-1. So, it is concluded that the pipeline humidification might significantly reduce temperature and enhance air humidity. The treatments performed in this study consisted of a varied flow of a humidity device, related to weather conditions. Temperature and relative air...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Weather Conditions; Air-assisted Boom; Application Technology.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100006

Comportamento compressivo de um nitossolo: efeito do tamanho de agregados, do teor de água e da pressão aplicada
Provedor de dados: 70
Autores: Pereira,Joaquim O.; Benez,Sérgio H.; Silva,Suedêmio de L.; Tabile,Rubens A.; Toledo,Anderson de.
A compactação do solo tem sido assunto de intensivas pesquisas nos últimos anos; no entanto, os mecanismos que implicam o processo de compactação dos solos agrícolas, ainda permanecem pouco conhecidos. A contribuição do tamanho de agregados do solo, bem como o efeito do teor de água e da pressão normal aplicada na compactação e pressão de pré-compactação do solo, foi investigada em um Nitossolo Vermelho eutrófico. Amostras de solo deformado, constituídas por agregados menores que 2,5 mm e de 9,3 a 19,4 mm, foram submetidas a ensaio de compressão uniaxial drenado. O índice de vazios e a pressão de pré-compactação foram avaliados. Os resultados obtidos mostram que o tamanho de agregados teve efeito no processo de compactação do solo. A mudança da compactação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compressão uniaxial; Compactação do solo; Pressão de pré-compactação.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300021

Estimation methods of reference evapotranspiration (ETo) for Uberlândia -MG
Provedor de dados: 70
Autores: LACERDA,ZILDA C. DE; TURCO,JOSÉ E. P.
One approach to verify the adequacy of estimation methods of reference evapotranspiration is the comparison with the Penman-Monteith method, recommended by the United Nations of Food and Agriculture Organization - FAO, as the standard method for estimating ET0. This study aimed to compare methods for estimating ET0, Makkink (MK), Hargreaves (HG) and Solar Radiation (RS), with Penman-Monteith (PM). For this purpose, we used daily data of global solar radiation, air temperature, relative humidity and wind speed for the year 2010, obtained through the automatic meteorological station, with latitude 18° 91' 66" S, longitude 48° 25' 05" W and altitude of 869m, at the National Institute of Meteorology situated in the Campus of Federal University of Uberlandia -...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Penman-monteith; Hargreaves; Makkink; Solar radiation.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100027

DEFORMATION OF PEACHES SUBMITTED TO CYCLIC LOADING USING THE DISCRETE ELEMENT METHOD
Provedor de dados: 70
Autores: Pinto,Eduardo M.; Ferraz,Antonio C. de O.
ABSTRACT This study aimed to use and validate a simple contact force model that describes the behavior of peaches stored in a wooden box, loaded cyclically, by using the discrete element method. The Kelvin-Voigt contact force model was used and the cyclic loading in the simulation was performed with an amplitude of 1 mm and frequency of 12 Hz for time intervals of 3600, 5400, and 7200 s. The laboratory test was performed with a peach box attached to a vibrating table by applying the same excitation conditions used in the simulation. For validation, model results were compared with those from the laboratory test by using deformation values of fruits in the contact regions. To measure this deformation, we adapted the methodology for determining the radius of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modeling; Simulation; Post-harvest; Prunus persica (L.) Batsch.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300434

Modelo de programação linear para seleção de pulverizadores agrícolas de barras
Provedor de dados: 70
Autores: Baio,Fábio H. R.; Antuniassi,Ulisses R.; Balastreire,Luiz A.; Caixeta Filho,José V.
A seleção de pulverizadores agrícolas que se adaptem às necessidades da propriedade, é um processo trabalhoso, sendo uma das etapas mais importantes dentro do processo produtivo. O objetivo do presente trabalho foi o de desenvolver e utilizar um modelo de programação linear para auxiliar na seleção de pulverizadores agrícolas de barras, baseado no menor custo horário do equipamento. Foram utilizadas as informações técnicas referentes a 20 modelos de pulverizadores disponíveis no mercado, sendo quatro autopropelidos, oito de arrasto e oito do tipo montado. A análise de sensibilidade dos componentes dos custos operacionais mostrou que as taxas de reparo e depreciação foram os fatores que mais interferiram na variação do custo horário do conjunto...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Programação linear; Tratamento fitossanitário; Máquinas agrícolas.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200014

Avaliação do bombeamento de água em um sistema alimentado por painéis fotovoltaicos
Provedor de dados: 70
Autores: Michels,Roger N.; Ricieri,Reinaldo P.; Gnoatto,Estor; Sousa,Samuel N. M. de; Silva,Suedêmio de Lima; Fischborn,Marcos.
O presente trabalho foi desenvolvido com a finalidade de avaliar um sistema de bombeamento de água acionado por painéis fotovoltaicos instalados nas dependências da Universidade Tecnológica Federal do Paraná, Câmpus Medianeira - PR. O município está localizado no oeste paranaense (25º17'43" S; 54º03'38" e 500,7 m). O sistema trabalhou em situação real de funcionamento, bombeando água à altura de 20 m. Foram coletados dados de fevereiro a novembro de 2005; utilizou-se coletor de dados computadorizado da Campbell Scientific INC. , que possibilitou adquirir e armazenar os dados de irradiância solar no plano do painel, tensão e corrente gerada, temperatura no painel e vazão. Por meio de cálculos, obtiveram-se os valores de potência e eficiência do sistema. O...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bombeamento; Energia; Fotovoltaica; Eficiência.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300004

Development of capacitive sensor for measuring soil water content
Provedor de dados: 70
Autores: Segundo,Alan K. Rêgo; Martins,José H.; Monteiro,Paulo M. de B.; Oliveira,Rrubens A. de; Oliveira Filho,Delly.
The irrigation management based on the monitoring of the soil water content allows for the minimization of the amount of water applied, making its use more efficient. Taking into account these aspects, in this work, a sensor for measuring the soil water content was developed to allow real time automation of irrigation systems. This way, problems affecting crop yielding such as irregularities in the time to turn on or turn off the pump, and excess or deficit of water can be solved. To develop the sensors were used stainless steel rods, resin, and insulating varnish. The sensors measuring circuit was based on a microcontroller, which gives its output signal in the digital format. The sensors were calibrated using soil of the type “Quartzarenic Neosoil”. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Process control; Control system; Irrigation system.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200006

PESTICIDES DEPOSITION IN VINEYARDS ON DIFFERENT CONDITIONS OF LEAF WETNESS
Provedor de dados: 70
Autores: Saab,Otavio J. G. Abi; Griesang,Fabiano; Alves,Karina A.; Higashibara,Leandro R.; Genta,Werner.
ABSTRACT The high susceptibility to diseases of fine table grapes cultivars demand intensive use of pesticides, and the presence of water on the leaf surface can worsen the deposition of these products. The objective of this study was to evaluate the spray deposition in vine leaves in different conditions of leaf wetness, and test the effectiveness of an artificial ventilation method to remove water on the leaf surface. We evaluated the spray deposition in vine applied over: wet canopy (presence of high leaf wetness); canopy dried artificially (dried with air jet from air-assisted sprayer, wind speed of 25 km h−1) and canopy dried naturally (naturally dried leaves and free of water on its surface). Saline marker was used in the spray and the deposition on...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Air assistance; Air-assisted sprayer; Application technology; Dew; Electrical conductivity; Vitis vinifera.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200286

Penetrômetro de cone com taxa constante de penetração no solo: desenvolvimento e teste de funcionalidade
Provedor de dados: 70
Autores: Reinert,Dalvan J.; Collares,Gilberto L.; Reichert,José M.
Penetrômetros auxiliam na determinação da capacidade de suporte do solo na engenharia civil e na avaliação da resistência mecânica de solos agrícolas, relacionando-a com compactação do solo e crescimento do sistema radicular das plantas. Este trabalho relata o desenvolvimento de um penetrômetro de cone com taxa constante de penetração, suas partes e funcionalidade, bem como resultados do uso na avaliação comparativa da compactação em experimentos e em lavoura. A quantificação da resistência é realizada com célula de carga, a distância de penetração no solo com potenciômetro, e a aquisição e o armazenamento de dados com placas eletrônicas. A concepção do equipamento, que emprega velocidade constante de penetração da haste no perfil do solo, possibilitou a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Penetrometria; Resistência mecânica; Compactação do solo.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100025

Application of simulated annealing in simulation and optimization of drying process of Zea mays malt
Provedor de dados: 70
Autores: Benvenga,Marco A. C.; Araújo,Sidnei A. de; Librantz,André F. H.; Santana,José C. C.; Tambourgi,Elias B.
Kinetic simulation and drying process optimization of corn malt by Simulated Annealing (SA) for estimation of temperature and time parameters in order to preserve maximum amylase activity in the obtained product are presented here. Germinated corn seeds were dried at 54-76 °C in a convective dryer, with occasional measurement of moisture content and enzymatic activity. The experimental data obtained were submitted to modeling. Simulation and optimization of the drying process were made by using the SA method, a randomized improvement algorithm, analogous to the simulated annealing process. Results showed that seeds were best dried between 3h and 5h. Among the models used in this work, the kinetic model of water diffusion into corn seeds showed the best...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulated annealing; Zea mays; Drying curves; Optimization; Simulation.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500012

Crescimento de plantas jovens de limeira ácida 'Tahiti' sob lâminas de irrigação
Provedor de dados: 70
Autores: Alves Júnior,José; Silva,Cláudio R. da; Ribeiro,Rafael V.; Silva,Tonny J. A. da; Folegatti,Marcos V.
Este estudo avaliou o efeito de lâminas de irrigação no crescimento vegetativo de limeira ácida 'Tahiti' (Citrus latifolia Tan) sob condições de campo. Os tratamentos consistiram de irrigações por gotejamento baseadas em 100% (T3) e 50% (T2) da evapotranspiração da cultura medida em lisímetro de pesagem e o tratamento sem irrigação (T1). O delineamento experimental foi inteiramente casualizado, com dez repetições. Mediram-se o diâmetro do caule e a altura das plantas mensalmente, ao passo que a área foliar, o volume e a projeção de copa foram determinados após 14 meses do início dos tratamentos. Medidas de assimilação de CO2, condutância estomática e potencial da água na folha foram realizadas para verificar o estado fisiológico das plantas em virtude dos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrus latifolia Tan.; Manejo da irrigação; Estresse hídrico.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100019

Sistema automatizado para coleta de dados de umidade relativa e temperatura do ar
Provedor de dados: 70
Autores: Palmieri,Anderson M.; Silveira,Luciano R. da; Miranda,Jarbas H.; Miranda,Késia O. da S.
Algumas variáveis climáticas, tais como a temperatura do ar (T) e a umidade relativa do ar (UR) exercem grande influência sobre a produção agrícola. Uma vez combinadas adequadamente, podem resultar em incrementos quantitativos e qualitativos do produto final, o que as tornam indispensáveis no monitoramento e manejo dentro do ambiente de produção. A aquisição de dados é uma importante ferramenta que pode auxiliar nesse processo, resultando em maior eficiência e uso racional dos recursos. Desse modo, o presente trabalho teve por objetivo o desenvolvimento de um sistema de aquisição de dados (SAD) compacto, na forma de um datalogger (de construção simples), para monitorar T e UR. Os dados provenientes dos sensores utilizados são gravados numa memória do tipo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistema de aquisição de dados; Variáveis climáticas; Microcontrolador embarcado.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400004

Formas de mecanização e manejo do solo para a cultura da batata II - desenvolvimento vegetativo
Provedor de dados: 70
Autores: Saito,Larissa R.; Jadoski,Sidnei O.; Maggi,Marcio F.; Sales,Livia L. S. R.; Suchoronczeck,Adriano.
O objetivo da pesquisa foi estudar os efeitos do manejo com diferentes formas de preparo do solo, tipos de resteva e infestação do solo com o fungo Trichoderma harzianum Rifai sobre as características de componentes do dossel vegetativo da cultura da batata. O experimento foi desenvolvido em Guarapuava-PR, em delineamento inteiramente casualizado, com parcelas subsubdivididas, em um esquema fatorial 4 x 5 x 2, com quatro repetições. Para o fator 1, foram avaliadas quatro formas de mecanização do preparo do solo (P): preparo-base (escarificação e sulcamento) - P1; preparo-base mais grade niveladora - P2; preparo-base mais enxada rotativa - P3 preparo-base mais grade niveladora e enxada rotativa - P4. No fator 2, utilizaram-se restevas de aveia, milho,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Preparo do solo; Tipos de resteva; Trichoderma harzianum; Infestação; Área foliar.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500011

Análise de mapas de represas publicados na web usando imagens orbitais CCD/CBERS no estado de Minas Gerais
Provedor de dados: 70
Autores: Ferreira,Elizabeth; Dantas,Antonio A. A.
Neste trabalho, bancos de dados públicos e gratuitos disponíveis na World Wide Web (WEB) foram utilizados para avaliar as áreas das superfícies dos espelhos d'água das represas de Furnas e do Funil, no Estado de Minas Gerais. O objetivo foi comparar as informações obtidas nos bancos da WEB com os valores das áreas calculadas a partir de imagens do sensor CCD a bordo dos satélites CBERS2 e CBERS2B. A área da represa de Furnas obtida a partir das imagens CCD/CBERS2B, ano 2008, foi de 1.138 km², mas nos bancos de dados consultados esta área estava entre 1.182 e 1.503 km². A represa do Funil, construída em 2003, com superfície de espelho d'água de 29,37 km² e uma ilha com área de 1,93 km² não aparecem nos bancos Atlas, Geominas, IGAM e IBGE. Os resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: SIG; Espelhos d'água; Mapas digitais.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100012

Características físicas e mecânicas de misturas de solo, cimento e casca de arroz
Provedor de dados: 70
Autores: Milani,Ana P. S.; Freire,Wesley J.
Na presente pesquisa, estudaram-se os efeitos da adição da casca de arroz nas propriedades físico-mecânicas da mistura de solo-cimento, visando a obter composições de solo-cimento-casca de arroz com potencialidade para fabricação de materiais alternativos de construção. Foram realizados o fracionamento, o peneiramento e o pré-tratamento em solução de cal da casca de arroz. Foram determinadas as características físicas do solo e da casca de arroz, sendo executados ensaios de dosagem das misturas de solo-cimento-casca de arroz, aplicando-se às mesmas os ensaios de compactação normal de Proctor e o de compressão simples. Posteriormente, as composições de solo-cimento-casca de arroz foram submetidas aos ensaios de compressão simples e de tração na compressão...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resíduo agroindustrial; Solo estabilizado; Material alternativo.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100001

THEORETICAL ANALYSIS AND EXPERIMENTAL STUDY ON THE PROCESS OF CONVEYING AGRICULTURAL FIBER MATERIALS BY SCREW CONVEYORS
Provedor de dados: 70
Autores: Wulantuya,; Wang,Hongbo; Wang,Chunguang; Qinglin,.
ABSTRACT To improve the conveying efficiency and working stability of a screw conveyor, the feeding methods, running conditions and flow characteristics of materials were studied by theoretical analysis and experiments. The theoretical analysis results show that the screw conveyor runs more stably when the helix angle of the screw blade is equal to the moving helical angle. A new spring-finger was designed by us and was used in the experiment. The experimental results show prove that the spring-finger feeder can help homogeneously and continuously to feed the screw conveyor and to improve the working stability of the screw conveyor. The movement state of materials along a pitch was videotaped by a high-speed camera with different filling rates and rotation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coarse fodder; Experimental study; Theoretical analysis; Screw conveyor.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500589

CALCIUM NITRATE CONCENTRATIONS IN FERTIGATION FOR ‘TERRA’ BANANA PRODUCTION
Provedor de dados: 70
Autores: Andrade Neto,Torquato M. De; Coelho,Eugênio F.; Silva,Ana Carina P. Da.
ABSTRACT The aim of this study was to evaluate the effect of calcium nitrate concentration of irrigation water on soil chemical attributes and productivity during the first ‘Terra’ banana crop cycle. The experiment followed a completely randomized design with six treatments and five replications, with six plants per plot. Treatments consisted in the use of three calcium nitrate concentrations (3.0, 10.0 and 13.0 g.L−1), applied via dripping and micro-micro-sprinkling irrigation. The results showed that the soil chemical properties under fertigation are influenced by the water and nutrient delivery system. There was a linear tendency of increase in electrical conductivity of the saturation extract and soil solution with the increase in calcium nitrate...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil solution; Saturation extract; Electric conductivity; Trickle irrigation.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200385

Influence of nails size and layout to obtain the reduction coefficient of moment of inertia for timber beams with composite cross section
Provedor de dados: 70
Autores: LAHR,FRANCISCO A. R.; CHRISTOFORO,ANDRÉ L.; FIORELLI,JULIANO.
ABSTRACT A significant portion of rural building’s roof is supported by timber trusses. Increasing distance between the trusses can be achieved by using composite cross sections ("T" and "I") for beams. With this, it is possible to reduce the number of columns and trusses, bringing significant savings in material and the desired cost reduction, mainly using wood from planted forests. The Brazilian Code ABNT NBR 7190:1997 establishes a coefficient (αr) for the reduction of the theoretical moment of inertia (Iteo) of 0.95 and 0.85, for beams with "T" and "I" composite profile, respectively. However, no specification is showed about connections responsible for conferring such coefficients. This research aimed to investigate, based on static bending tests,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Timber beams; Composite cross section; Steel connectors.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400715

Sistema de informação geográfica para mapeamento da renda líquida aplicado no planejamento da agricultura irrigada
Provedor de dados: 70
Autores: Silva,Wilson A.; Carvalho,Daniel F.; Varella,Carlos A. A.; Ceddia,Marcos B.
O objetivo deste trabalho foi desenvolver um algoritmo na linguagem computacional MATLAB para aplicações em sistemas de informações geográficas, visando ao mapeamento da renda líquida maximizada de cultivos irrigados. O estudo foi desenvolvido para as culturas do maracujá, da cana-de-açúcar, do abacaxi e do mamão, em área de aproximadamente 2.500 ha, localizada no município de Campos dos Goytacazes, norte do Estado do Rio de Janeiro. Os dados de entrada do algoritmo foram informações edafoclimáticas, funções de resposta das culturas à água, dados de localização geográfica da área e índices econômicos referentes ao custo do processo produtivo. Os resultados permitiram concluir que o algoritmo desenvolvido se mostrou eficiente para o mapeamento da renda...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: SIG; Agricultura irrigada; Funções de produção.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100008

Using fraction images derived from modis data for coffee crop mapping
Provedor de dados: 70
Autores: Bispo,Rafael C.; Lamparelli,Rubens A. C.; Rocha,Jansle V.
Coffee production was closely linked to the economic development of Brazil and, even today, coffee is an important product of the national agriculture. The State of Minas Gerais currently accounts for 52% of the whole coffee area in Brazil. Remote sensing data can provide information for monitoring and mapping of coffee crops, faster and cheaper than conventional methods. In this context, the objective of this study was to assess the effectiveness of coffee crop mapping in Monte Santo de Minas municipality, Minas Gerais State, Brazil, from fraction images derived from MODIS data, in both dry and rainy seasons. The Spectral Linear Mixing Model was used to derive fraction images of soil, coffee, and water/shade. These fraction images served as input data for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spectral linear mixing model; Supervised classification; Overall Accuracy; Kappa Index.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100012

The position effect of structural Eucalyptus round timber on the flexural modulus of elasticity
Provedor de dados: 70
Autores: Christoforo,André L; Panzera,Túlio H; Batista,Fabiano B; Borges,Paulo H. R; Lahr,Francisco A. R; Franco,Claudenir F.
Round timber has great use in civil construction, performing the function of beams, columns, foundations, poles for power distribution among others, with the advantage of not being processed, such as lumber. The structural design of round timber requires determining the elastic properties, mainly the modulus of elasticity. The Brazilian standards responsible for the stiffness and strength determination of round timber are in effect for over twenty years with no technical review. Round timber, for generally present an axis with non-zero curvature according to the position of the element in the bending test, may exhibit different values of modulus of elasticity. This study aims to analyze the position effect of Eucalyptus grandis round timber on the flexural...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Round timber; Bending of beams; Modulus of elasticity.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600019

Qualidade de sementes de feijão colhidas por colhedora autopropelida em sistema semimecanizado
Provedor de dados: 70
Autores: Tertuliano,Paulo C.; Souza,Cristiano M. A. de; Rafull,Leidy Z. L.; Souza,Luiz C. F. de; Robaina,Antônio D.
Este trabalho teve por objetivo avaliar as qualidades física e fisiológica de sementes de feijão-carioca Iapar 81, colhidas em sistema semimecanizado, utilizando-se de colhedora autopropelida. Foi avaliada a influência da velocidade de deslocamento (6,5; 8,8; 10,2 e 10,8 km h-1), da rotação do cilindro trilhador (430 e 480 rpm) e do efeito latente dos danos mecânicos durante o armazenamento das sementes (0; 60; 120 e 180 dias). Foram determinados a impureza, o índice de danos mecânicos, o vigor e a germinação das sementes. O efeito latente dos danos mecânicos foi avaliado pelo teste de vigor, pela germinação e pela condutividade elétrica. Os menores valores de impureza foram obtidos nas velocidades de 10,2 e 10,8 km h-1 e na rotação do cilindro trilhador...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus vulgaris L.; Impureza; Dano mecânico; Germinação.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100009

Soybean yield maps using regular and optimized sample with different configurations by simulated annealing
Provedor de dados: 70
Autores: Guedes,Luciana P. C.; Ribeiro Junior,Paulo J.; Uribe-opazo,Miguel A.; Bastiani,Fernanda de.
ABSTRACT This study aimed to compare thematic maps of soybean yield for different sampling grids, using geostatistical methods (semivariance function and kriging). The analysis was performed with soybean yield data in t ha-1 in a commercial area with regular grids with distances between points of 25x25 m, 50x50 m, 75x75 m, 100x100 m, with 549, 188, 66 and 44 sampling points respectively; and data obtained by yield monitors. Optimized sampling schemes were also generated with the algorithm called Simulated Annealing, using maximization of the overall accuracy measure as a criterion for optimization. The results showed that sample size and sample density influenced the description of the spatial distribution of soybean yield. When the sample size was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Accuracy indices; Optimization; Sampling grids; Spatial variability.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100114

INTERFERENCE OF THE NUMBER OF REMOTE CONTROL VALVES IN USE ON THE ENERGY PERFORMANCE OF AN AGRICULTURAL TRACTOR WITH PRODUCTIVITY MANAGEMENT
Provedor de dados: 70
Autores: Neto,Lauro S.; Kmiecik,Leonardo L.; Jasper,Samir P.; Zimmermann,Gabriel G.; Savi,Daniel.
ABSTRACT The hydraulic remote control system allows the transfer of energy from the engine through a flow of hydraulic oil to engines and implements pulled by agricultural tractors, which can interfere with its energy and operational performance. This study aimed to evaluate the interference of the number of remote control valves in use on the operational and energy performance of an agricultural tractor, using a productivity management system. The experiment was conducted in a strip-plot design, with five replications and three treatments, which consisted of the number of remote control valves in use (1, 2, or 3), totaling 15 experimental units. The results were subjected to normality and homogeneity tests and analysis of variance, followed by the Tukey...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Power on the drawbar; Hydraulic system; Operational speed; Specific consumption; Engine thermal efficiency.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300356

Impact of different light sources on broiler rearing environment
Provedor de dados: 70
Autores: Lima,Karla A. O.; Nääs,Irenilza de A.; Garcia,Rodrigo G.; Borille,Rodrigo; Caldara,Fabiana R.
Broiler production is highly dependent on the use of artificial light. The light source may affect the effectiveness of housing conditions due to increasing ambient temperature and concentration of noxious gases. This research aimed to evaluate the effects of different bulb types on the thermal, aerial, and acoustic environment of broiler aviaries. The experiment was carried out at a commercial broiler farm in Dourados, Mato Grosso do Sul State, Brazil. Three aviaries were used, and two flocks of male broilers from Cobb® genetic strain were reared from the first day to slaughter. Each aviary was equipped with a different light source, comprising the adopted treatments (A1 - incandescent light bulb, control; A2 - sodium vapor light bulb; A3 - fluorescent...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry industry; Gas concentration; Lighting; Temperature.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300006

Variabilidade espacial da rentabilidade, perdas na colheita e produtividade do feijoeiro
Provedor de dados: 70
Autores: Johann,Jerry A.; Silva,Maria C. A.; Uribe-Opazo,Miguel A.; Dalposso,Gustavo H.
O feijoeiro comum é cultivado em todas as regiões do País e apresenta grande importância econômica e social. É uma cultura de subsistência em pequenas propriedades, porém apresenta alguns problemas que influenciam em sua comercialização, como oscilação de preço pago ao produtor. Os métodos de colheita são diversos e, atualmente, o mais utilizado no Brasil é a colheita semimecanizada. Com o objetivo de avaliar a produtividade, rentabilidade, perdas manual e mecânica na colheita da cultivar de feijão Juriti, realizou-se o levantamento de dados georreferenciados em uma área de 10,45 ha, com o auxílio de uma grade de amostragem regular de 50 x 50 m. Para estudar a variabilidade espacial, foram utilizadas técnicas geoestatísticas, que geraram mapas temáticos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dados georreferenciados; Feijão Juriti; Geoestatística.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400014

INFLUÊNCIA DE IMPLEMENTOS DE PREPARO E DE NÍVEIS DE COMPACTAÇÃO SOBRE ATRIBUTOS FÍSICOS DO SOLO E ASPECTOS AGRONÔMICOS DA CULTURA DO MILHO
Provedor de dados: 70
Autores: DEPERON JÚNIOR,MILTON A.; NAGAHAMA,HIDEO DE J.; OLSZEVSKI,NELCI; CORTEZ,JORGE W.; SOUZA,ELDER B. DE.
RESUMO Os sistemas de preparo do solo e o aumento do tráfego nas áreas agrícola têm contribuído para o aumento da compactação do solo e diminuição da produtividade das culturas. Assim, objetivou-se avaliar a influência de implementos de preparo do solo e de níveis de compactação sobre atributos físicos de Argissolo Amarelo distrófico típico, textura arenosa, e os impactos nos atributos agronômicos da cultura do milho. Os tratamentos foram constituídos por três implementos de preparo do solo (IP1 = grade aradora; IP2 = arado de aivecas, e IP3 = escarificador) e quatro níveis de compactação (NC0 = solo não trafegado; NC3 = 3 passadas; NC6 = 6 passadas, e NC9 = 9 passadas de trator). No solo, foram avaliados os atributos: densidade do solo, porosidade total e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Produtividade de grãos; Resistência à penetração de raízes; Zea mays.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200367

Comparação de elementos filtrantes no grau de obstrução em irrigação por gotejamento
Provedor de dados: 70
Autores: Ribeiro,Tulio A. P.; Paterniani,José E. S.
Esta pesquisa teve como finalidade mostrar a variação da qualidade da água e sua influência na perda de carga de dois sistemas de filtragem (filtro de disco e manta sintética não tecida) utilizados em um sistema de irrigação localizada por gotejamento. Utilizou-se água de um reservatório aberto, onde foi instalado um módulo de irrigação localizada para o estudo. Para melhor comparação dos filtros, foram utilizados dois índices de uniformidade de distribuição de água para verificar o grau de entupimento dos gotejadores. A pesquisa foi desenvolvida em quatro etapas de 30 dias, realizadas em diferentes estações do ano. Em cada etapa, foram analisados os principais parâmetros físicos, químicos e biológicos da água de irrigação que causam problemas de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Qualidade de água; Manta sintética não tecida; Filtragem.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300006

Deficit irrigation in grapevine cv. Syrah during two growing seasons in the brazilian semiarid
Provedor de dados: 70
Autores: Bassoi,Luís H.; Correia,Joselina de S.; Santos,Ana R. L. dos; Silva,Juliano A.; Costa,Bruno R. S.
Irrigation plays an important role for grape’s yield as well as on its quality for winemaking. Thus, the effects of deficit irrigation strategies on yield and quality of wine grapes cv. Syrah were evaluated in Petrolina, State of Pernambuco, Brazil. Evaluations were carried out throughout the second and third growing seasons, which were from November 2010 to February 2011 (rainy season) and from May to September 2011 (dry season), respectively. Vines were drip irrigated and the experimental design was completely randomized with three treatments and four replications. The treatments were full irrigation (FI), performed according crop evapotranspiration; regulated deficit irrigation (RDI), in which irrigation was interrupted in phenological growth stage of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vitis vinifera L.; Soil water content; Leaf water potential.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300430

Estimativa da variação na demanda de água para irrigação por pivô-central no Distrito Federal entre 1992 e 2002
Provedor de dados: 70
Autores: Sano,Edson E.; Lima,Jorge E. F. W.; Silva,Euzebio M.; Oliveira,Elaine C.
O aumento da demanda de água para a irrigação tem sido objeto de constante preocupação dos órgãos de gestão dos recursos hídricos e da população do Distrito Federal. Os objetivos deste trabalho foram determinar a variação da área irrigada por pivôs-centrais no Distrito Federal entre os anos de 1992 e 2002, estimar a demanda hídrica desses sistemas, bem como verificar sua importância em relação ao consumo humano. Utilizando imagens de satélite e ferramentas de geoprocessamento, foram determinadas as áreas irrigadas por pivô-central. O consumo de água dessas áreas irrigadas foi estimado com base em dados da literatura referentes às principais culturas semeadas na região. Entre 1992 e 2002, o número de pivôs-centrais no Distrito Federal passou de 55 para 104,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura irrigada; Geoprocessamento; Recursos hídricos.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200025

TOPOGRAPHYC SHADOW INFLUENCE ON OPTICAL IMAGE ACQUIRED BY SATELLITE IN THE SOUTHERN HEMISPHERE
Provedor de dados: 70
Autores: França,Michelle M.; Fernandes Filho,Elpidio I.; Ferreira,Williams P. M.; Lani,João L.; Soares,Vicente P.
ABSTRACT During image acquisition, is usually chosen scenes with a lesser cloud cover to avoid loss of spectral information. However, when training samples are collected for image classification, the user finds shadowed areas. Such situation is similar to the presence of clouds since spectral information of these classes is the same in all optical bands of the sensor. This fact becomes more pronounced in mountainous relief areas due to shadow projection on the terrain, which can vary among all seasons during the solar year. With the goal to obtain images with a lower presence of shadow, it was simulated, under the same relief conditions, shading variation in function of latitude (0° to 40° S). Solar radiation models were processed for the days and times...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Landsat; Remote sensing; Solar radiation.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500728

Quality of peanut mechanical sowing in function of seeding density and size of the seeds
Provedor de dados: 70
Autores: Zerbato,Cristiano; Furlani,Carlos E. A.; Almeida,Rodrigo F; Voltarelli,Murilo A.; Silva,Vicente F. A.
ABSTRACT Peanut crop (Arachis hypogaea L.) mechanization has been improved over the years; however there are drawbacks that affect the quality of operations. Thus, this article’s objectives were to evaluate the operational performance of the mechanized sowing of peanut crop according to seeding densities (10, 14, and 18 seeds m-1) and seed sizes (21 and 23 mm). It was observed that the seeds of 23 mm had shorter average number of days to emergence and a higher percentage of emergences, occurring the opposite to the seeding density of 18 seeds m-1. The higher the seeding density, the largest was the plant stand, whereas the 23 mm seed obtained the best results and the same with the seeding density of 14 seeds m-1 that had a higher percentage of normal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Arachis hypogaea L.; Agricultural mechanization; Seeder-fertilizer.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400711

Digital surface area assessment of broiler chickens
Provedor de dados: 70
Autores: Yanagi Júnior,Tadayuki; Silva,Éberson; Braga Júnior,Roberto A.; Lopes,Marcos A.; Damasceno,Flávio A.; Silva,Gleice C. de A. E.
Surface area (SA) of poultry is an important parameter for heat and mass transfer calculations. Optical approaches, such as the moiré technique (MT), are non-destructive, result in accuracy and speed gains, and preserve the object integrity. The objective of this research was to develop and validate a new protocol for estimating the surface area (SA) of broiler chickens based on the MT. Sixty-six Ross breed broiler chickens (twenty-seven male, thirty-nine female, ages spanning all growth phases) were used in this study. The dimensions (length, width and height) and body mass of randomly selected broiler chickens were evaluated in the laboratory. Chickens were illuminated by a light source, and grids were projected onto the chickens to allow their shape to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Image analysis; Moiré technique; Poultry.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300007

Sweet grape mini tomato grown in culture substrates and effluent with nutrient complementation
Provedor de dados: 70
Autores: Cunha,Ananda H. N.; Sandri,Delvio; Vieira,Jonas A.; Cortez,Thiago B.; Oliveira,Thiago H. de.
The objective of this study was to evaluate production of Sweet Grape mini tomato (Lycopersicum esculentum Mill.) using culture substrates and nutrient solution sewage effluent, applied by drip irrigation (fertigation). The experiment was conducted at the University of Goiás State (UEG-UnUCET), from June to November 2011 in Anápolis-GO, Brazil. The experimental design was a 2 x 3 factorial arrangement in a randomized complete block design with four repetitions. The plots were made by combining two nutrient solutions, effluent supplemented with mineral fertilizers (EcS); conventional nutrient solution (SnC); in addition three cultivation substrates: 60% of fine sand washed + 40% substrate composed by 20% coconut fiber plus 80% pine bark (S1); 20% coconut...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mini tomato; Nutrient solution; Reuse.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400010

Tratamento anaeróbio de resíduos orgânicos com baixa concentração de sólidos
Provedor de dados: 70
Autores: Luna,Maria L. D. de; Leite,Valderi D.; Lopes,Wilton S.; Sousa,José T. de; Silva,Salomão A.
Este trabalho foi realizado com o objetivo de avaliar o desempenho de reator anaeróbio compartimentado no tratamento de resíduos sólidos orgânicos com baixa concentração de sólidos. O reator anaeróbio compartimentado possuía capacidade unitária de 2.200 litros, era dividido em seis câmaras de iguais dimensões e foi operado com tempo de retenção de sólidos de 90 dias. Os resíduos sólidos orgânicos utilizados para alimentação do reator eram constituídos de resíduos sólidos vegetais e de lodo de esgoto sanitário na proporção de 80% e 20%, respectivamente. A mistura desses dois tipos de resíduos originava o substrato, o qual, após a correção da umidade para 95% (percentagem em massa), era alimentado ao reator. A eficiência de redução de material carbonáceo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reator anaeróbio compartimentado; Biogás; Resíduos sólidos orgânicos.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100012

Qualidade da água e sua relação espacial com as fontes de contaminação antrópicas e naturais: bacia hidrográfica do rio São Domingos - RJ
Provedor de dados: 70
Autores: Menezes,Juliana M.; Prado,Rachel B.; Silva Júnior,Gerson C. da; Mansur,Kátia L; Oliveira,Elba dos S. de.
O objetivo do trabalho foi avaliar a qualidade das águas da Bacia Hidrográfica do Rio São Domingos (BHRSD), correlacionando-a com as possíveis fontes poluidoras advindas das características naturais e antrópicas da área. Alguns parâmetros físico-químicos foram analisados em 65 pontos (superficiais e subterrâneos) de amostragem. Os resultados foram confrontados com os limites estabelecidos pelas Resoluções CONAMA 357/05 (classe 2), que trata das águas superficiais, e CONAMA 396/08 (consumo humano), que contempla as águas subterrâneas. Foram analisados diversos cátions e ânions, temperatura, alcalinidade, pH, condutividade elétrica (CE), sólidos totais dissolvidos (STD), oxigênio dissolvido (OD), demanda bioquímica de oxigênio (DBO), coliformes...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Qualidade de água superficial e subterrânea; Agrotóxicos; Poluição difusa e pontual; Aquíferos fraturados.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400019

Teores de nutrientes na alface irrigada com água residuária aplicada por sistemas de irrigação
Provedor de dados: 70
Autores: Sandri,Delvio; Matsura,Edson E.; Testezlaf,Roberto.
Desenvolveu-se este trabalho para avaliar a composição química da parte aérea da alface, cv. Elisa, irrigada com água residuária tratada com leitos cultivados com macrófitas e água de um depósito de fonte hídrica superficial, cultivada em Latossolo Vermelho Distroférrico, utilizando-se dos sistemas de irrigação por aspersão convencional, gotejamento subterrâneo e superficial. O experimento compreendeu o período de 17-8 a 3-10-2001, e as análises químicas da alface foram realizadas aos 47 dias após o transplantio das mudas em campo. A parte aérea da alface foi analisada quanto ao teor de nitrogênio total, nitrato, fósforo, potássio, cálcio, magnésio, enxofre, ferro, manganês, cobre, zinco, sódio, boro, cobalto e molibdênio. O sódio e o enxofre apresentaram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lactuca sativa L.; Aspersão; Gotejamento.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100006

CONSTRUCTION AND TESTING OF GLUED LAMINATED TIMBER FRAMES FOR USE IN LAYING POULTRY HOUSES
Provedor de dados: 70
Autores: Stringari,Eduardo H.; Petrauski,Alfredo; Petrauski,Sandra M. C.; Azevedo,Ricardo L.; Savaris,Gustavo.
ABSTRACT This study aimed to present a solution in glued laminated timber to replace frame structures built in reinforced concrete and metallic structure, which are common in agricultural buildings in western Paraná such as those destined to laying poultry house building by agricultural cooperatives. Structural behavior of frames build from Araucaria angustifolia glued boards and vegetable oil-based polyurethane adhesive was evaluated. Tests were carried out to characterize wood and adhesive to obtain verification/sizing parameters. Initially, a full-scale structural project was conducted to meet standard laying poultry house specifications. Afterwards, five units of straight three-articulated frames on a 1:2.5 reduced scale were designed, built, and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Timber structure; Rural buildings; Adhesives; Araucaria angustifolia.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200122

Fertilização com dejetos suínos: influência nas características bromatológicas da Brachiaria decumbens e alterações no solo
Provedor de dados: 70
Autores: SILVA,ADRIANE DE A.; LANA,ÂNGELA M. Q.; LANA,REGINA M. Q.; COSTA,ADRIANA M. DA.
O objetivo deste trabalho foi avaliar as características bromatológicas de uma pastagem de Brachiaria decumbens fertilizada com dejetos suínos, bem como avaliar as alterações que a utilização desse dejeto causa em alguns atributos químicos do solo. O delineamento foi em blocos casualizados, com seis tratamentos: T1: ausência de adubação mineral e orgânica (tratamento- -controle); T2 apenas com adubação mineral; T3, T4 e T5 com diferentes doses de dejetos líquidos de suínos (respectivamente ao equivalente a 60; 120 e 180 m3 por hectare), e T6 tratamento organomineral (120 m3por hectare) de dejetos líquidos de suínos, com adição de fertilizante mineral). Observou-se que houve incremento em produtividade de massa seca (MS). O uso de dejetos de suínos resultou...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Atributos do solo; Fertilização de pastagem; Resíduos orgânicos; Suinocultura.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200254

Precision agriculture in Australia: present status and recent developments
Provedor de dados: 70
Autores: Bramley,Robert; Trengove,Sam.
A brief account of the present status of Precision Agriculture (PA) in Australia is presented, and areas of opportunity in the grains, sugar and wine industries are identified. In particular, these relate to the use of spatially-distributed experimentation to fine-tune management so as to achieve production efficiencies, reduced risk of environmental impact and enhanced food security, and the management of crop quality through selective harvesting and product streaming. The latter may be an important avenue by which farmers can take a more active role in the off-farm part of agricultural value chains. The important role of grower groups in facilitating PA adoption is also discussed.
Tipo: Info:eu-repo/semantics/article
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300014

Aspectos lineares e espaciais da correlação entre a produtividade de forragem de milho e a porosidade do solo sob plantio direto
Provedor de dados: 70
Autores: Lima,Ronaldo C.; Mello,Luiz M. M. de; Carvalho,Morel de P. e; Lima,Cesar G. da R.; Mello,Arthur M. de.
A porosidade do solo é de extrema importância à produtividade agrícola, uma vez que, em condições adversas, pode dificultar a penetração das raízes e, consequentemente, limitar o adequado aproveitamento dos nutrientes e da água disponível. Na Fazenda Bonança, em Pereira Barreto - SP, em 2005, foi analisada a produtividade de forragem do milho (MSF), a macroporosidade (MA), a microporosidade (MI) e a porosidade total (PT) de um Latossolo Vermelho distrófico (Acrustox Háplico), sob plantio direto, em três profundidades. O objetivo foi estudar as correlações lineares e espaciais entre os atributos da planta e do solo, na tentativa de selecionar, entre os do solo, um indicador da sua qualidade física de boa representatividade para a produtividade da forragem....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manejo do solo; Qualidade física do solo; Forragicultura.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100005

Corn productivity in function of surface application of lime in differents management systems and cultural preparation
Provedor de dados: 70
Autores: Narimatsu,Karem C. P.; Mello,Luiz M. M. de; Domingues,Luis A. da Silva; Chioderoli,Carlos A.; Lima,Ronaldo C.
The evaluation of technologies employed at the agricultural production system such as crop rotation and soil preparation, both associated with crop-livestock integration, is crucial. Therefore, the aim of the present study was to evaluate the incorporation of lime for three no-tillage systems and cultural managements in system of crop-livestock integration, with emphasis on corn grain yield. The experiment was conducted from January 2003 to April 2005 at Selvíria city, MS, in Dystroferric Red Latosol, clay texture. The experimental design was randomized blocks with split plots consisted of three main treatments, aimed the soil physics conditioning and the incorporation of lime: PD - No-no-tillage; CM - minimum no-tillage, and PC - conventional no-tillage;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: No tillage system; Minimum tillage; Conventional tillage; Crop-livestock integration; Crop rotation.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200007

Variabilidade espacial e controle estatístico do processo de perdas na colheita mecanizada do algodoeiro
Provedor de dados: 70
Autores: Silva,Rouverson P.; Souza,Fábio G.; Cortez,Jorge W.; Furlani,Carlos E. A.; Vigna,Gustavo P.
Dentro do processo produtivo, a colheita, se mal conduzida, poderá causar prejuízos quali-quantitativos no produto final. Dessa forma, esse trabalho teve o objetivo de avaliar as perdas quantitativas, no solo e na planta, na colheita mecanizada de algodão, no ano agrícola de 2006, em Ipameri-GO, em um talhão de 1,4 ha, sendo georreferenciados 41 pontos, distanciados de 50 m no sentido da curva de nível e 9 m entre fileiras. As amostras foram coletadas colocando-se uma armação de 4,5 m² sobre o solo, coletando todo o algodão caído no solo e, em seguida, fez-se a coleta do algodão que permaneceu na planta após a passagem da colhedora. Além das perdas quantitativas determinaram-se o teor médio de água do algodão e o Rendimento Potencial Máximo (RPM). Foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Colhedora de algodão; Geoestatística.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400018

EVALUATION OF DROPLET SPECTRA OF THE SPRAY TIP AD 11002 USING DIFFERENT TECHNIQUES
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Reis,Elton F. dos; Assunção,Heli H. T. de; Landim,Thiago N.
ABSTRACT Knowledge of droplet spectra generated by spray nozzle tips is important to ensure the quality of applications of plant protection products. However, there are different methods for this evaluation, which can cause difficulty in interpreting the results. This study aimed to evaluate the droplet spectra produced by the flat fan spray tip AD 11002 operated under different pressures and using different techniques and equipment. The volume median diameter (VMD), percentage of spray volume in droplets smaller than 100 µm diameter and relative spam (RS), considering pressures of 200, 300, and 400 kPa were determined using two direct measurement equipment (Spraytec and Shadow Sizer), based on laser diffraction and image analysis, respectively, and a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Droplet size; Water-sensitive paper; Laser diffraction.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400476

Produtividade do meloeiro sob lâmina de irrigação e adubação potássica
Provedor de dados: 70
Autores: Sousa,Antonio E. C; Bezerra,Francisco M. L; Sousa,Carlos H. C. de; Santos,Francisco S. S. dos.
Teve-se o objetivo de avaliar o efeito de quatro lâminas de irrigação e quatro doses de potássio aplicadas por irrigação localizada na produtividade do híbrido Gold Mine AF 10.00 do melão Amarelo (Cucumis melo L.). O experimento foi conduzido no Câmpus do Pici da Universidade Federal do Ceará. O delineamento experimental utilizado foi em blocos casualizados, com parcelas subdivididas, em esquema fatorial 4 x 4, onde o primeiro fator correspondeu às lâminas de irrigação, e o segundo, às doses de potássio, em quatro repetições. O fator lâmina de irrigação apresentou efeito altamente significativo sobre a produtividade do melão, enquanto a adubação potássica e a interação entre os fatores não foram significativas. A produtividade de frutos aumentou de forma...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cucumis melo; Lâmina de irrigação; Fertirrigação.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200009

Desempenho de derriçadora portátil de frutos do cafeeiro
Provedor de dados: 70
Autores: Souza,Cristiano M. A. de; Queiroz,Daniel M. de; Pinto,Francisco de A. de C.; Teixeira,Mauri M.
Este trabalho avaliou o desempenho de uma derriçadora portátil para cafeicultura de montanha durante a colheita de frutos de cafeeiros Catucaí e Catuaí, em vários estádios de desenvolvimento. Foram determinados as características dos cafeeiros, as curvas características do motor da derriçadora, a capacidade e a eficiência de derriça, o consumo de energia, a desfolha e o nível de ruído emitido pela máquina. A derriçadora portátil teve desempenho satisfatório por apresentar baixa desfolha e número de galhos quebrados, capacidade de derriça regular, baixo consumo específico de energia e elevada eficiência de derriça. O nível de ruído aumentou com o aumento da potência requerida na derriça.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energia elétrica; Dano mecânico; Ergonomia.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300026

Comparação do Coeficiente Global de Perdas de Calor para casa de vegetação aquecida usando diferentes técnicas para eficiência energética
Provedor de dados: 70
Autores: Oliveira,Celso E. L. de; Garcia,José L.; De La Plaza,Saturnino; Chaya,Carolina.
O Coeficiente Global de Perdas de Calor (U) permite o equacionamento das necessidades térmicas de uma casa de vegetação climatizada. No presente trabalho, determinou-se esse coeficiente cujo referencial foi uma casa de vegetação localizada em Madri (Espanha), em que foram utilizadas medidas noturnas de temperatura do ar no interior, no exterior, bem como o consumo de energia para aquecimento. As comparações entre as técnicas de aquecimento utilizadas foram: solo radiante e aerotermos combinados com duas técnicas que visavam a promover melhor aproveitamento térmico, ou seja, a utilização de cobertura plástica formando dupla capa ou a utilização de túnel plástico. Os menores coeficientes foram conseguidos para a utilização de solo radiante com túnel e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Climatização; Eficiência energética; Estufas.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200003

DEVELOPMENT OF A TRANSFER FUNCTION FOR WEIGHT PREDICTION OF LIVE BROILER CHICKEN USING MACHINE VISION
Provedor de dados: 70
Autores: Amraei,Somaye; Mehdizadeh,Saman A.; Nääs,Irenilza de A.
ABSTRACT The objective of this study was to process digital images to investigate the possibility of broilers body weight estimation based on the dynamic model. For this experiment, 2440 images were recorded by a top-view camera from 30 birds. An ellipse fitting algorithm was applied to localize chickens within the pen, by using a generalized Hough transform. Chickens’ head and tail were removed efficiently using the Chan-Vese method. After that, using image processing, six body measures were calculated. Next, they were used to design a Transform Function (TF) model with weight measurements as output. Second-order dynamic models were used to predict the weight of life broiler chicken, without delay, stable and with the highest R2 were predominantly...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Automatic weight estimation; Image processing; Ellipse fitting; Transfer function modeling.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500776

Curva de retenção de água elaborada pelo método do psicrômetro para uso na determinação do índice "S" de qualidade física do solo
Provedor de dados: 70
Autores: Melo Filho,José F. de; Sacramento,José A. A. S. do; Conceição,Bruna P. S.
RESUMO A curva de retenção representa a relação entre o teor de água no solo e a energia com a qual a mesma está retida nos poros e/ou adsorvida nas partículas minerais do solo. Trata-se de uma relação com várias e importantes aplicações práticas relacionadas à relação solo-água em agricultura. Atualmente, é também utilizada como base para determinação de índices de qualidade física do solo, a exemplo do índice "S" proposto por Dexter em 2004. Para sua elaboração existe uma grande variedade de métodos, dentre os quais o que usa a câmara de pressão de Richards é o mais tradicional. Atualmente equipamentos eletrônicos, a exemplo do psicrômetro WP4, têm sido sugeridos como instrumentos úteis para a elaboração da curva de retenção. Neste contexto, o presente...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água no solo; Câmara de Richards; Psicrômetro e equação de Van Genuchten.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500959

PROTECTED ENVIRONMENTS AND SUBSTRATES FOR ACHACHAIRU SEEDLINGS
Provedor de dados: 70
Autores: Silva,Bruna L. B. da; Costa,Edilson; Salles,Josiane S.; Binotti,Flávio F. da S.; Benett,Cleiton G. S.
ABSTRACT The Achachairu (Garcinia humilis) is a Bolivian exotic fruit that has been produced and commercialized a few years in Brazil. Information about the production of high quality seedlings is essential for the implementation and the renewal of orchards. The objective was to evaluate protected environments and substrates for Achachairu seedlings. Two protected environments were evaluated, one covered with aluminized thermal reflector screen of 50% of shading and the other with Sombrite® of 50% of shading. Inside the protected environments were tested substrates derived from combinations of various proportions of cattle manure (CM), ravine soil (RS), medium vermiculite (MV), super fine vermiculite (FV) and sand (S). For each protected environment was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Garcinia humilis; Cattle manure; Exotic fruit; Plant's environment; Soil; Vermiculite.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300309

Microclima, idades das matrizes e tempos de estocagem influenciam na perda de água dos ovos no transporte?
Provedor de dados: 70
Autores: Nazareno,Aérica C.; da Silva,Iran J. O.; Vieira,Afrânio M. C.; Vieira,Frederico M. C.
RESUMO Objetivou-se, por meio desta pesquisa, avaliar a perda de água de ovos férteis oriundos de diferentes idades de matrizes de corte e tempos de estocagem, durante o transporte. A pesquisa foi conduzida em uma empresa integradora avícola no Estado de São Paulo, por meio do acompanhamento de três carregamentos em diferentes estações do ano. Foram utilizadas diferentes densidades de caixas durante as três viagens. Porém, para o estudo da perda de água dos ovos, foi usado um total de 18 caixas contendo 4.320 ovos, em um caminhão climatizado. Estas caixas de ovos eram referentes às três idades das matrizes e aos três intervalos de tempos de estocagem; portanto, em cada viagem, foram transportadas seis caixas com 1.440 ovos. A caracterização microclimática...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência; Operação pré-porteira; Avicultura; Perda de massa; Ovos férteis.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400635

Bartlett-Lewis of rectangular pulse modified model: estimate of parameters for simulation of precipitation in sub-hourly duration
Provedor de dados: 70
Autores: Teixeira-Gandra,Claudia F. A.; Damé,Rita de Cássia F.
The Bartlett-Lewis Rectangular Pulse Modified (BLPRM) model simulates the precipitous slide in the hourly and sub-hourly and has six parameters for each of the twelve months of the year. This study aimed to evaluate the behavior of precipitation series in the duration of 15 min, obtained by simulation using the model BLPRM in situations: (a) where the parameters are estimated from a combination of statistics, creating five different sets; (b) suitability of the model to generate rain. To adjust the parameters were used rain gauge records of Pelotas/RS/Brazil, which statistics were estimated - mean, variance, covariance, autocorrelation coefficient of lag 1, the proportion of dry days in the period considered. The results showed that the parameters related...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sub-hourly rainfall; Daily rainfall disaggregation; Hydrologic modeling.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500011

Evapotranspiração e coeficiente da cultura do mamoeiro
Provedor de dados: 70
Autores: Posse,Robson P.; Bernardo,Salassier; Sousa,Elias F. de; Gottardo,Romildo D.
O trabalho teve como objetivos determinar a evapotranspiração da cultura (ETc) e o coeficiente da cultura (Kc) para o mamoeiro (Carica papaya L.). O experimento foi realizado na área de convênio UENF/PESAGRO-RIO, no município de Campos dos Goytacazes - RJ, no período de 25-4-2006 a 20-8-2007, utilizando o mamoeiro cultivar Híbrido UENF/CALIMAN01. Para a determinação da ETc e do Kc, foi utilizado lisímetro de pesagem com área superficial de 6 m². A evapotranspiração de referência (ETo) foi estimada pelo método de Penman-Monteith (FAO). A evapotranspiração máxima da cultura foi de 2,9 mm dia-1, aos 229 dias após o transplantio (DAT), sendo a evapotranspiração média da cultura, em todo o período, de 1,8 mm dia ¹. O valor do Kc do mamoeiro variou linearmente...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carica papaya L.; Consumo hídrico; Irrigação; Manejo.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400008

Distribuição de palha por colhedoras autopropelidas na colheita da soja
Provedor de dados: 70
Autores: Kunz,Vilson L.; Gabriel Filho,Antonio; Primo,Marcelo A.; Gurgacz,Flavio; Fey,Emerson.
A dificuldade de obter distribuição uniforme dos resíduos, na largura de corte da plataforma da colhedora, tem sido constatada visualmente em culturas comerciais. Assim, o objetivo deste trabalho foi avaliar a uniformidade de distribuição transversal de palha por colhedoras autopropelidas na colheita da soja. Foram avaliadas nove colhedoras nas condições de operação e regulagem que estavam sendo usadas pelo operador. Foi utilizado o coeficiente de variação para a comparação das máquinas e a avaliação da uniformidade de distribuição, e realizada análise multivariada para avaliar a similaridade entre as colhedoras em função do coeficiente de variação, umidade da palha e largura da plataforma de corte. Todas as colhedoras apresentaram distribuição desuniforme...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Máquinas agrícolas; Plantio direto; Resíduo vegetal.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100013

COMPUTATIONAL ANALYSIS OF LOAD VENTILATION IN BROILER TRANSPORT
Provedor de dados: 70
Autores: Pinheiro,Daniel G.; Machado,Nítalo A. F.; Barbosa Filho,José A. D.; Silva,Iran J. O. Da.
ABSTRACT The characterization of ventilation during the transport of broiler chickens is essential for identifying and characterizing the potential problems of a convective heat flow and its effects on the welfare and the health and production conditions of the chickens. The objective of this study was to evaluate the ventilation patterns in two layout models of a live transport load: conventional (LC) and alternative (LA) with spacers placed between the chicken transport crates. Computational fluid dynamics (CFD) simulations and wind tunnel tests were performed using small scale models. The results showed that the use of spacers between crates (LA model) modified the ventilation patterns and increased the wind circulation between crates. However, wind...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry; Animal welfare; CFD simulation; Precision livestock farming.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100009

CONSTRUCTION AND PRACTICAL APPLICATION OF A CANOPY OPENER DEVICE
Provedor de dados: 70
Autores: PRADO,EVANDRO P.; Pogetto,MÁRio H. F. Do A. Dal; Cerqueira,Denise T.R. De; Raetano,Carlos G.; Costa,Saulo Í. De A.
ABSTRACT: Accurate application of pesticides is difficult for crops with dense leaves, such as soybean crops. To improve spray deposits on the lower leaves of soybean plants, the aim of this study is to build a canopy opener (CO) from a previously developed prototype and to assess its practical application and efficiency on soybean crops. Laboratory experiments were conducted to determine the amount of spray deposits on the top and the lower leaves using a Brilliant Blue dye. The influence of the CO device on the number of flowers knocked down during spraying was also investigated. The data showed that the use of the CO attached to the spray boom enabled more spray deposit on the lower leaves and less spray depositson the upper leaves compared with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Soybean; Spray deposit.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601126

Mechanical properties of grain in silos for simulation designs
Provedor de dados: 70
Autores: Lopes Neto,José P.; Nascimento,José W. B. do; Marques,Jordânio I.; Costa,Carlos A. da.
ABSTRACT For the calculation of silos structures it has been used new methods and computational tools that require mechanical properties knowledge that are still unknown for most storable materials, especially grains. In this context, we aimed to determine the mechanical properties of rice and beans grains with moisture contents of 10, 12, and 14% by applying four compressive loads (5, 10, 15 and 20). The determined mechanical properties were Poisson's ratio (ν), Modulus of Elasticity (E), and the dilatancy angle (ψ). The procedure consisted in the application of the load in compression cell, adapted from MOLENDA &amp; STASIAK, aiming to simulate loading and unloading of silos. We observed that the Poisson's ratio calculated for both loading and unloading,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poisson’s coefficient; Compression; Modulus of elasticity; Silos; Simulation.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400573

Desenvolvimento de equipamento motorizado para aplicação líquida de produtos fitossanitários na cultura do café
Provedor de dados: 70
Autores: Matuo,Tomás K.; Raetano,Carlos G.; Matuo,Tomomassa; Martinelli,Nilza M.; Leite,Gilson J.
O trabalho teve como objetivo desenvolver um protótipo aplicador de líquidos na superfície do solo para cafezais localizados em regiões de topografia acidentada ou cultivados em sistema de plantio adensado. O protótipo do aplicador construído é um trator de rabiças acionado por um motor de dois tempos a gasolina, de 2,61 kW (3,5 cv), com duas rodas motrizes com bitola de 0,60 m e uma terceira roda direcional, equipado com sistema de pulverização dotado de depósito de 40 L, bomba centrífuga, filtros de linha, regulador de pressão, manômetro, mangueiras, válvulas e suporte de bicos. Para avaliar a eficiência do protótipo, foram instalados dois experimentos de campo em São Sebastião do Paraíso - MG (2003 e 2004), onde foram aplicados inseticidas sistêmicos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Equipamento aplicador; Quesada gigas.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300015

Anaerobic reactors with biofilter and different diameter-length ratios in cassava starch industry wastewater treatment
Provedor de dados: 70
Autores: Kunzler,Kathia R.; Gomes,Simone D.; Piana,Pitágoras A.; Torres,Douglas G. B.; Vilas Boas,Marcio A.; Tavares,Maria H. F.
The use of anaerobic reactors with media support in the treatment of wastewater from the cassava starch industry has emerged as a viable option because it allows the application of high organic loads and a significant reduction of the HDT needed for the treatment. This research aimed at studying the process of biodigestion in two anaerobic reactors with bamboo support, in the treatment of effluent of cassava starch, by evaluating their performance. The two reactors used present the following diameter: length ratio, 1:6 and 1:3. The organic loads applied to the systems were 0.519, 1.156, 1.471, 3.049, 4.347, 4.708 and 5.601g.L-1.d-1. Regarding the efficiency of removal of COD, TS and TVS, no statistically significant differences were obtained between the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biodigestion; Organic load; Piston flow.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400003

THERMODYNAMIC PROPERTIES OF SORPTION OF RICE IN THE HUSK
Provedor de dados: 70
Autores: Zeymer,Juliana S.; Corrêa,Paulo C.; Oliveira,Gabriel H. H. de; Baptestini,Fernanda M.; Faria,Igor L.
ABSTRACT This study aimed to determine the thermodynamic properties of sorption processes (desorption and adsorption) of rice in the husk, cv. Urucuia. A static-gravimetric method was used to reach equilibrium moisture content at different temperatures (10, 20, 30, 40, and 50 °C ± 1°C) and relative humidity levels (10, 30, 50, 70, and 90 % ± 2%). A decrease in moisture content led to an increment of the integral isosteric heat of sorption, indicating a higher demand for energy to remove moisture from the product. Differential entropy of sorption decreased along with a moisture content increment, with higher values for desorption. This indicates a higher mobility of water molecules during desorption if compared to adsorption. Gibbs free energy decreased...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Equilibrium moisture content; Integral isosteric heat of sorption; Differential entropy; Gibbs free energy; Enthalpy-entropy compensation theory.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300369

Reconhecimento de variedades de soja por meio do processamento de imagens digitais usando redes neurais artificiais
Provedor de dados: 70
Autores: Khatchatourian,Oleg; Padilha,Fábio R. R.
Neste trabalho, foi aplicado o processamento de imagens digitais auxiliado pelas Redes Neurais Artificiais (RNA) com a finalidade de identificar algumas variedades de soja por meio da forma e do tamanho das sementes. Foram analisadas as seguintes variedades: EMBRAPA 133, EMBRAPA 184, COODETEC 205, COODETEC 206, EMBRAPA 48, SYNGENTA 8350, FEPAGRO 10 e MONSOY 8000 RR, safra 2005/2006. O processamento das imagens foi constituído pelas seguintes etapas: 1) Aquisição da imagem: as amostras de cada variedade foram fotografadas por máquina fotográfica Coolpix995, Nikon, com resolução de 3.34 megapixels; 2) Pré-processamento: um filtro de anti-aliasing foi aplicado para obter tons acinzentados da imagem; 3) Segmentação: foi realizada a detecção das bordas das...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Propriedades morfológicas de soja; Análise morfológica de sementes; Reconhecimento de padrões.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400016

STREAMFLOW REGIONALIZATION IN PIQUIRI RIVER BASIN
Provedor de dados: 70
Autores: Araujo,Fernanda C.; Mello,Eloy L. de; Gollin,Gisele M.; Quadros,Luciana E. de; Gomes,Benedito M.
ABSTRACT The objective of this study was to regionalize 7-day 10-year low flows, long-term annual mean, and 90% and 95% permanence flows from Piquiri (PR) river basin. The following regionalization methods were adopted: Traditional, Linear interpolation, Chaves, Modified linear interpolation, and Modified Chaves. The equations obtained by the Traditional method, adding main river length or drainage density as independent variables, significantly improved R2 equations value. Streamflow forecasting by Linear Interpolation and Chaves methods were as good as those provided by the Traditional Method, thus, these methods could be applied to Piquiri River basin, especially when drainage area is the only available spatial information.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water availability; Water resources management; Average streamflow; Low flows; Flows permanence.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100022

Balanço energético comparativo para rotas de escoamento de soja
Provedor de dados: 70
Autores: Biaggioni,Marco A. M.; Bovolenta,Fábio C.
O presente trabalho objetivou analisar o fluxo energético no escoamento de soja da região Centro-Oeste do Brasil, considerando as rotas atualmente existentes, mais precisamente, do município de Rio Verde -GO até o porto de Santos - SP, visto que este é um grande polo exportador de granéis sólidos. Foram selecionadas duas rotas para a análise, uma contemplando a multimodalidade, ou seja, os modais rodoviário, ferroviário e hidroviário, e outra, uma única modalidade, o modal rodoviário. A conversão dos fatores físicos e operacionais em unidades energéticas foi realizada por meio de coeficientes energéticos levantados junto à literatura. Os resultados obtidos indicaram, pela rota 1 multimodal, um gasto energético específico maior para o modal rodoviário (0,50...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Transporte multimodal; Rodovia; Ferrovia; Hidrovia; Escoamento de soja; Balanço energético.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400003

Qualidade na semeadura do milho
Provedor de dados: 70
Autores: WEIRICH NETO,PEDRO H.; FORNARI,ALISSON J.; JUSTINO,ALTAIR; GARCIA,LUIZ C.
O objetivo deste trabalho foi estabelecer um padrão para a qualidade na semeadura do milho. Durante cinco anos agrícolas, acompanhou-se a semeadura da cultura do milho em aproximadamente 13.500 ha, divididos em 30 propriedades da região dos Campos Gerais – PR, totalizando 64 semeadoras-adubadoras. Os parâmetros avaliados foram: variação da dosagem de adubo entre linhas, população inicial, variação de plantas emergidas entre fileiras, distribuição longitudinal, população final e produtividade. Conclui-se que é possível obter variação da quantidade de adubo distribuída entre linhas da semeadora-adubadora, plantas emergidas entre fileiras, espaçamentos falhos e múltiplos abaixo de 5%. Recomenda-se determinar como meta espaçamentos aceitáveis acima de 90% para...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semeadora-adubadora; Dosagem de adubo; Distribuição longitudinal de sementes.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100171

Efeito da taxa de carregamento sobre a remoção de poluentes de esgoto em sistemas alagados construídos
Provedor de dados: 70
Autores: Matos,Antonio T. de; Brasil,Mozart da S.; Monaco,Paola A. V. Lo.
Objetivou-se estudar o efeito da taxa de carregamento sobre a eficiência de sistemas alagados, construídos de escoamento horizontal subsuperficial (SAC-EHSS), em remover poluentes de esgoto sanitário. Os SAC-EHSS foram alimentados com efluente proveniente de tanque séptico, sob taxas de carregamento orgânico volumétrico (TCO V) de 53 a 231 g m-3d-1 de demanda química de oxigênio (DQO total) e as associadas taxas de carregamento (TC V) de demanda química de oxigênio solúvel, sólidos suspensos totais (SST), nitrogênio total (N-Total) e fósforo total (P-Total). Para avaliação de desempenho dos SAC-EHSS, as mesmas variáveis foram quantificadas em seu efluente. Relação linear e positiva foi obtida entre as taxas de remoção de DQO total, DQO solúvel e SST, e as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carga orgânica; Sistemas wetland; Tratamento biológico.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200011

CONTRIBUTION OF SOIL ATTRIBUTES AND MORPHOLOGICAL VARIABLES TO YIELD OF IRRIGATED GARLIC
Provedor de dados: 70
Autores: Oliveira,Job T. de; Oliveira,Rubens A. de; Furtado Junior,Marconi R.
ABSTRACT This study aimed to investigate relationships between the soil attributes that most affect garlic yield, which can be useful to choose a new area for the growing of this vegetable. We also aimed to study the effects of irrigation deficit at bulb formation stage (cloves) on final garlic quality and yield. The variables evaluated were garlic yield, irrigation, nitrogen, lateral shoot growing, plant water potential, bulb volume, leaf area index, soil electrical conductivity, soil mechanical resistance to penetration, and volumetric soil moisture content. Initially, the Pearson's correlation was estimated for the phenological indexes, and a correlation network was used to graphically express the results and to correct multicollinearity between...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Allium sativum L.; Path analysis; Precision irrigation; Precision agriculture.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200215

Análise operacional de um sistema fotovoltaico de bombeamento de água
Provedor de dados: 70
Autores: Kolling,Evandro M.; Souza,Samuel N. M. de; Ricieri,Reinaldo P.; Sampaio,Silvio C.; Dallacort,Rivanildo.
O bombeamento de água é uma das atividades mais difundidas quanto ao emprego da energia solar fotovoltaica. Porém, apesar de se apresentar como alternativa interessante, o alto custo, a baixa eficiência dos sistemas e os projetos inadequados restringem sua aplicação. O uso racional, baseado na utilização mais eficiente de seus equipamentos, está vinculado ao conhecimento do comportamento operacional desses sistemas. No presente trabalho, teve-se o objetivo de avaliar o comportamento de um sistema fotovoltaico de bombeamento de água diretamente acoplado, sob diferentes condições de irradiância solar, por meio da montagem de uma bancada de testes, submetendo-o a diferentes alturas manométricas e determinando-se a vazão fornecida. A análise dos resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irradiância solar; Carga de bombeamento; Vazão do sistema.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300005

Broiler breeder hen performance and egg hatchability during rainy season in Brazilian semi-arid region
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Tota,Laura D. C. A.; Nascimento,José W. B.; Guimarães,Mércia C. da C.; Lopes Neto,José P.
Henhouse thermal comfort and bird age influence broiler breeder hen productivity; this way, the present research aimed to assess thermal comfort indexes and broiler breeder hen performance during winter in North East semi-arid region from Brazil, using a Cobb Avian 48 broiler strain at the age of 38 and 50 weeks. We measured the following bioclimatic indexes: air temperature and relative humidity, black globe temperature and humidity, CO2 concentration and sound pressure levels at henhouse facility. Data analysis design was complete randomized in a 3 x 3 factorial scheme with three treatments (months) and three replications (week number of collection by month). A number of 25 climatic data were observed. Bioclimatic indexes at the most warm hours...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Thermal comfort; Egg-laying; Noise.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300001

Viabilidade econômica do sistema de adubação diferenciado comparado ao sistema de adubação convencional em lavoura cafeeira: um estudo de caso
Provedor de dados: 70
Autores: Ferraz,Gabriel A. E S.; Silva,Fábio M. da; Carvalho,Francisval de M.; Costa,Pedro A. N. da; Carvalho,Luis C. C.
A agricultura de precisão surge como uma importante ferramenta para maximizar o gerenciamento da atividade cafeeira, principalmente para esta cultura, que possui elevado custo de produção. O presente trabalho teve por objetivo fazer um estudo comparativo da viabilidade econômica de dois sistemas de adubação na lavoura cafeeira: o sistema utilizando as técnicas da agricultura de precisão e o sistema de aplicação convencional. Os dados utilizados foram extraídos dos custos de produção da fazenda Brejão, no sul de Minas Gerais, em três áreas (22 ha, 10,52 ha e 6,23 ha), onde foram realizadas aplicações de adubos de forma diferenciada nas safras de 2007/2008 e 2008/2009. O sistema de adubação em agricultura de precisão caracterizou-se por coleta de amostras de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adubação a taxas variáveis; Agricultura de precisão; Custos; Viabilidade; Cafeicultura; Adubação convencional.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500008

INFLUENCE OF DIFFERENT THERMAL ENVIRONMENTS ON THE PERFORMANCE OF LAYING HENS DURING THE INITIAL STAGE OF REARING
Provedor de dados: 70
Autores: Andrade,Rafaella R.; Tinôco,Ilda de F. F.; Baêta,Fernando da C.; Albino,Luiz F. T.; Cecon,Paulo R.
ABSTRACT This study was conducted with the aim of assessing the effects of different ambient temperature values on the performance of laying birds from one to 42 days of age in order to obtain optimal comfort temperatures. A total of 864 laying hens were distributed in four climatic chambers with different temperature ranges. One of the chambers was maintained within the thermal range recommended by the literature and the others were maintained under temperatures that consisted of mild and moderate cold stress and moderate heat stress. The experiment was conducted according to a completely randomized design in a split-plot arrangement and six replications. The data were analyzed by means of the analysis of variance and regression. The final performance of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Zootechnical performance; Cold stress; Light laying hens; Thermoneutrality.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100032

USE OF REMOTELY PILOTED AIRCRAFTS FOR THE APPLICATION OF PLANT PROTECTION PRODUCTS
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Alvarenga,Cleyton B. de; Rinaldi,Paula C. N.; Marques,Matheus G.; Zampiroli,Renan.
ABSTRACT The use of remotely piloted aircrafts (RPAs) to apply plant protection products has grown a lot in agriculture worldwide. However, little research data are available regarding the efficiency and safety of this method, especially in Brazil. Thus, this review aimed to present the current scenario of scientific research involving RPAs in the application of pesticides. Several factors interfere with the quality of this type of application. Among them are height and flight speed, droplet generator elements, application rate, and spray solution properties. In general, applications have been performed between 1.0 m and 3.0 m of height and 1.0 m s-1 and 7.0 m s-1 of speed. As for the droplet generator element, there is still no clarity as to the ideal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Drones; Pesticides; Spraying.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200245

Modelagem da extração de óleos essenciais empregando coeficiente de difusão variável
Provedor de dados: 70
Autores: SILVEIRA,JENIFFER C.; COSTA,ANDRÉA O. S. DA; COSTA JUNIOR,ESLY F.DA.
Óleos essenciais são compostos químicos voláteis, característicos por sua fragrância e frequentes atividades antimicrobianas e antioxidantes. São extraídos dos tricomas de plantas aromáticas a partir de diversos métodos diferentes de extração. As indústrias dão preferência à extração por arraste a vapor (destilação a vapor), por ser um processo tradicional, de simples operação e baixo custo. A modelagem matemática deste processo é um passo inevitável para projetar plantas industriais de extração de óleo essencial visando a boas condições operacionais. O modelo empregado neste trabalho é baseado na difusão do óleo no interior da folha. Apresentam-se o procedimento de discretização deste modelo por método de diferenças finitas e a validação deste por...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Óleos essenciais; Modelagem; Estimação de parâmetros.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200302

Investment recovery period in electric motor of higher efficiency in pumping for irrigation
Provedor de dados: 70
Autores: Zocoler,João L.; Leite,Maurício A.; Saad,João C. C.; Cruz,Raimundo L.; Zocoler,João G.
In this study, it was adjusted a mathematical model to measure the effect of electric motor efficiency on pumping system costs for irrigation on the tariff structure of conventional electricity and green horo-seasonal , and also to calculate the recovery period of the invested capital in higher efficiency equipment. Then, it was applied to a center pivot irrigation system in two options of electric motor efficiency, 92,6% (standard line) and 94,3% (high efficiency line), and the acquisition cost of the first corresponded to 70% the of the second. The power of the electric motor was 100hp. The results showed that the model allowed us to evaluate if a high efficiency motor was economically viable compared to the standard motor in each tariff structure. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Conventional tariff; Green horo-seasonal tariff; High efficiency.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200001

Degradation of sewage sludge compost disposed on the soil
Provedor de dados: 70
Autores: DINIZ,ISABELA C. C.; MATOS,ANTONIO T.; BORGES,ALISSON C.; AQUINO,JULIANA M. G. L.; MATOS,MATEUS P.
ABSTRACT This study aimed to monitor degradation of compost from undigested sewage sludge disposed on soil surface or incorporated it. The sewage sludge was blended with wood sawdust during a 90-day composting to achieve a C/N ratio of 9. Each waste was dosed based on its total content of nitrogen and on an annual dose of 500 kg ha-1, which is broadly recommended for forage fertilization. After incorporation and surface applied (five replicates each), waste mineralization was monitored for 131 days by samplings taken from both conditions for further analyses. The samples were measured for total organic carbon (TOC); easily oxidizable carbon (OOC); total nitrogen (TN); ammonia and nitric nitrogen, and from them the total organic nitrogen (ON); volatile...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Composting; Undigested sewage sludge; Mineralization fraction.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500822

LED TUBS ARTIFICIAL LIGHTING SYSTEM IN BROILER PRODUCTION
Provedor de dados: 70
Autores: Seber,Rogério; Moura,Daniella; Lima,Nilsa; Massari,Juliana.
ABSTRACT Light is important for the physiology and zootechnical development of broilers and is characterized by the type of source defined by the spectral emission and geometry of the lamp, as well as the intensity and spatial distribution of the illuminance. The aim of this study was to verify the influence of an artificial lighting system based on tubular Light Emitting Diode (LED) lamps on the productive performance of broilers. The study was carried out in two broiler houses located in Londrina-PR. The lighting system for one of the broiler houses was composed of 52 tubular LED bulbs of 18 W powers, and the control broiler house consisted of 75 incandescent bulbs with 60 W powers. This research was divided into two parts; the first phase was evaluated...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Broiler; Light; Tubular light emitting diode.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300319

Efeito de subdoses de 2,4-D na produtividade do algodão e suscetibilidade da cultura em função de seu estádio de desenvolvimento
Provedor de dados: 70
Autores: Constantin,Jamil; Oliveira Júnior,Rubens S. de; Fagliari,Júlio R.; Pagliari,Paulo H.; Arantes,João G. Z. de; Cavalieri,Sidnei D.; Framesqui,Vagner P.; Gonçalves,Diego A.
O objetivo deste trabalho foi avaliar o efeito de subdoses de 2,4-D no desenvolvimento e produtividade da cultura do algodoeiro. Dois experimentos foram conduzidos utilizando-se da variedade IAPAR-95 e o sistema de avaliação por meio de testemunhas duplas. No primeiro experimento, as aplicações foram realizadas no estádio F1 (início do florescimento), aplicando-se dosagens de 0,84; 1,68; 3,36; 6,72; 13,44 e 26,88 g de equivalente ácido (e.a.) por hectare, equivalentes a derivas de 0,125; 0,25; 0,5; 1,0; 2,0 e 4,0% da dose de 670 g e.a. ha-1. No segundo experimento, os tratamentos foram constituídos pela combinação em esquema fatorial de duas doses (6,72 e 13,44 g e.a. ha-1) e três épocas de aplicação (C1, C3/C4 e C6), visando a avaliar a variação da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Herbicidas fenóxicos; Fitointoxicação; Injúrias.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200004

Vazão de gotejadores com distintos tempos de irrigação aplicando água residuária de suinocultura e água de abastecimento
Provedor de dados: 70
Autores: Batista,Rafael O.; Oliveira,Rubens A. de; Figueiredo,Vladimir B.; Silva,Ketson B. da; Ferreira,Daianni A. da Costa.
Este trabalho objetivou analisar o efeito das proporções do tempo de irrigação com água residuária de suinocultura (ARS) e água de abastecimento (AA) na alteração da vazão de gotejadores. O experimento foi montado no esquema de parcelas subsubdivididas, em delineamento inteiramente casualizado, com três repetições, tendo nas parcelas as proporções de tempo de irrigação (1E3A - 1 h de ARS e 3 h de AA; 2E2A - 2 h de ARS 2 h de AA; 3E1A - 3 h de ARS e 1 h de AA, e 4E - 4 h de ARS); nas subparcelas, os tipos de gotejadores (G1, G2 e G3) e nas sub-subparcelas os tempos das avaliações (0; 20; 40; 60; 80; 100; 120; 140 e 160 h). Os atributos físico-químicos e biológicos da ARS e AA foram obtidos a cada 20 h e 80 h, respectivamente. Realizou-se a medição de vazão...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Emissores; Obstrução; Efluente.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600022

Sistema radicular de plantas de cobertura sob compactação do solo
Provedor de dados: 70
Autores: Gonçalves,Wainer G.; Jimenez,Rodrigo L.; Araújo Filho,Jerônimo V. de; Assis,Renato L. de; Silva,Gilson P.; Pires,Fábio R.
Com o objetivo de avaliar a capacidade de crescimento de raízes em camadas de solo compactadas, quatro espécies de plantas de cobertura (amaranto, milheto ADR 500, capim pé-de-galinha e kenaf) foram cultivadas em anéis de PVC, com níveis de compactação em subsuperfície (densidade do solo: 1,18; 1,34; 1,51 e 1,60 Mg m-3), sendo o experimento conduzido em casa de vegetação, utilizando-se de um Latossolo Vermelho distroférrico. A camada compactada em subsuperfície foi restritiva ao crescimento de raízes das espécies estudadas, ocasionando a concentração de raízes na camada superficial. O milheto ADR 500 e o amaranto foram as espécies que se destacaram na produção de massa seca da parte aérea e conseguiram desenvolver-se nas camadas compactadas e abaixo delas....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resistência do solo; Densidade de comprimento radicular; Crescimento radicular.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100008

Geotechnology application for data acquisition for agricultural and environmental management of the municipality of Vitória Brazil-SP
Provedor de dados: 70
Autores: ZANARDO,FÁBIO H.; RODRIGUES,RICARDO A. F.; SILVA,HELIO R.; MARQUES,ARTUR P.; FARIA,GLAUCIA A.
ABSTRACT The present study aimed at associating geoprocessing procedures for analysis of land use and native vegetation for municipal management, using an easy access and low cost methodology to the public administration of the municipality of Vitória Brazil/SP. Initially, the land use and the land occupation were evaluated, being delimited the municipal hydrographical micro basin and the permanent preservation areas (PPAs). For this purpose, multispectral images of high spatial resolution were used, available by the government partnerships between the City Hall, the state and federal authorities. From the obtained results it was possible to efficiently determine that only 3% of the original vegetation is preserved; the livestock is the main municipal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Land occupation; Remote sensing; Hydrographical micro basin.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400684

Pressurização da calda de pulverização na viabilidade de microrganismos entomopatogênicos
Provedor de dados: 70
Autores: Garcia,Luiz C.; Raetano,Carlos G.; Wilcken,Silvia R. S.; Ramos,Hamilton H.; Leite,Luis G.; B. Filho,Antônio; Moscardi,Flávio.
Avaliou-se a influência da pressurização da calda de pulverização na viabilidade dos seguintes microrganismos entomopatogênicos: o fungo Metarhizium anisopliae, a bactéria Bacillus thuringiensis var. kurstaki, o nucleopoliedrovirus de Anticarsia gemmatalis (AgMNPV) e o nematóide Steinernema glaseri. Utilizou-se do sistema hidráulico de um pulverizador, sem filtros, equipado com ponta de pulverização de jato cônico JA-2. O delineamento experimental adotado foi o inteiramente casualizado, com sete tratamentos: pressurização da calda em 172; 345; 517; 689; 1.034 e 1.379 MPa, e a testemunha (calda não submetida à pressurização). A avaliação da viabilidade de M. anisopliae foi realizada por meio da porcentagem de germinação dos conídios. Para B. thuringiensis,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Controle biológico.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300025

Ambiências térmica, aérea e acústica para reprodutores suínos
Provedor de dados: 70
Autores: Tolon,Yamilia B.; Baracho,Marta S.; Nääs,Irenilza de A.; Rojas,Marcelo; Moura,Daniella J. de.
O ambiente de alojamento de instalações para reprodutores suínos tem influência direta no desempenho dos animais. Este trabalho teve como objetivo estimar um padrão de avaliação dos ambientes térmicos, aéreo e acústico em instalações para reprodutores de suínos (cachaços), de maneira que pudesse prover os animais de bem-estar. O experimento foi realizado em granja comercial localizada no município de Salto -SP. Foram levantados os dados de ambiências térmica, aérea e acústica do ambiente de criação, sendo analisados estatisticamente, tendo como base a condição de ambiência ideal para proporcionar bem-estar animal. Os resultados mostraram que a temperatura ambiente ficou cerca de 70% fora da normalidade, enquanto a umidade relativa do ar, a velocidade do ar...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Machos reprodutores; Conforto térmico; Bem-estar de suínos.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100001

Influência da granulometria dos sólidos triturados de sabugo de milho e bagaço de cana-de-açúcar como materiais filtrantes no tratamento de águas residuárias da suinocultura
Provedor de dados: 70
Autores: Lo Monaco,Paola A. V.; Matos,Antonio T. de; Brandão,Viviane dos S.
Teve-se o objetivo de avaliar a influência da granulometria de sólidos triturados do sabugo de milho e do bagaço de cana-de-açúcar, utilizados como materiais filtrantes, na eficiência de remoção de poluentes da água residuária da suinocultura (ARS). Utilizaram-se colunas de filtragem contendo o material em três faixas granulométricas (0,84 a 1,19; 1,19 a 2,00 e 2,00 a 2,83 mm). Para a avaliação da eficiência do sistema, o afluente e o efluente foram caracterizados em relação às seguintes variáveis: demanda bioquímica de oxigênio (DBO5), demanda química de oxigênio (DQO), sólidos totais (ST), nitrogênio total (N-total), fósforo total (P-total), potássio (K), sódio (Na), cobre total (Cu-total) e zinco total (Zn-total). Geraram-se curvas, relacionando-se as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Filtros orgânicos; Tratamento de água; Tamanho da partícula.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500015

Cellulase effect on anaerobic digestion of maize silage under discontinuous operation
Provedor de dados: 70
Autores: Oliva-Merencio,Deny; Pereda-Reyes,Ileana; Schimpf,Ulrike; Koehler,Stefan; Silva,Ariovaldo J. da.
ABSTRACT This paper studied the effect of adding an enzyme (ellulose) on anaerobic digestion of maize silage. We compared materials at chopping lengths of 8 mm (MSL), 4mm (MSS) and natural size (Ms) under a mesophilic and discontinuous operation (batch process). Hence, we found the process to be significantly influenced by particle size. Moreover, the ellulose addition did not significantly impact biogas production after a 35-day digestion period. Ms and MSS displayed an improved response to all variables when compared with MSL and MSL+C, with significant differences. Studies on the refractory fraction at infinite time (R0) have demonstrated that the lowest values correspond to Ms and MSS (0.122 and 0.155, respectively). The Kinetic approach and the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ellulose; Silage; Biogas; Kinetics; Biodegradability.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500951

Desempenho do trator agrícola no manejo da cultura de cobertura e pressão de inflação do pneu da semeadora
Provedor de dados: 70
Autores: Cortez,Jorge W.; Furlani,Carlos E. A.; Vigna,Gustavo P.; Borsatto,Edinan A.; Silva,Rouverson P. Da.
O adequado manejo de culturas de cobertura no plantio direto tem-se mostrado excelente alternativa para melhorar as condições de semeadura. O objetivo do presente trabalho foi avaliar o desempenho do trator agrícola no manejo dos restos culturais do sorgo (rolo-faca e triturador de palhas) e a pressão de inflação (525 e 385 kPa) do pneu da semeadora-adubadora, no estabelecimento da cultura do milho em plantio direto. O experimento foi conduzido na UNESP - Jaboticabal, em delineamento de blocos ao acaso, com parcela subdividida, e os tratamentos consistiram nos manejos da cultura de cobertura do solo e pressões de inflação do pneu da semeadora, com quatro repetições. Foram mensurados nas máquinas: velocidade de deslocamento, capacidade de campo, consumo de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Patinhagem; Plantio direto; Zea mays.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100008

Measurement systems of soil water matric potential and evaluation of soil moisture under different irrigation depths
Provedor de dados: 70
Autores: Beraldo,José M. G.; Cora,José E.; Fernandes,Edemo J.
The development of new methodologies and tools that enable to determine the water content in soil is of fundamental importance to the practice of irrigation. The objective of this study was to evaluate soil matric potential using mercury tensiometer and puncture digital tensiometer, and to compare the gravimetric soil moisture values obtained by tensiometric system with gravimetric soil moisture obtained by neutron attenuation technique. Four experimental plots were maintained with different soil moisture by irrigation. Three repetitions of each type of tensiometer were installed at 0.20 m depth. Based on the soil matric potential and the soil water retention curve, the corresponding gravimetric soil moisture was determined. The data was then compared to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tensiometer; Digital tensiometer; Neutron attenuation technique.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300006

Tratamento de águas residuárias de suinocultura em reatores anaeróbios de fluxo ascendente com manta de lodo (uasb) em dois estágios seguidos de reator operado em batelada sequencial (RBS)
Provedor de dados: 70
Autores: Oliveira,Roberto A. de; Santana,Adriana M. de.
Neste trabalho, avaliou-se o desempenho de dois reatores anaeróbios de fluxo ascendente com manta de lodo (UASB), em série, seguidos de um reator operado em batelada sequencial (RBS) com etapa aeróbia, no tratamento de águas residuárias de suinocultura. O sistema de tratamento anaeróbio em dois estágios foi alimentado com águas residuárias de suinocultura com concentrações médias de sólidos suspensos totais (SST), de 4.427 a 16.425 mg L-1 . As cargas orgânicas volumétricas (COV) aplicadas no reator UASB do primeiro estágio variaram de 14,8 a 24,4 g DQO (L d)-1. Os tempos de detenção hidráulica (TDH) foram de 28 e 11 h e de 14 e 6 h no primeiro e segundo reatores UASB, respectivamente. O RBS foi operado com 1 e 2 ciclos diários de alimentação e com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Remoção de nutrientes; Tratamento anaeróbio-aeróbio; Pós-tratamento; Nitrificação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100018

Distribuição, probabilidade de ocorrência e período de retorno dos índices de erosividade EI30 e KE&gt;25 em Seropédica - RJ
Provedor de dados: 70
Autores: Carvalho,Daniel F de; Machado,Roriz L; Evangelista,Adão W. P; Khoury Júnior,Joseph K.; Silva,Leonardo D. B. da.
O presente trabalho foi desenvolvido com o objetivo de estudar as características da erosividade da chuva em Seropédica (RJ), quanto à sua distribuição, probabilidade de ocorrência e período de retorno. Para isso, foi utilizada uma série mensal de dados pluviométricos referente ao período de 1973 a 2002 e, com o auxílio de modelos ajustados para a região, foi possível obter os índices mensais e anuais de erosividade EI30 e KE&gt;25. Com base nos resultados obtidos, foi possível concluir que: a) os valores médios anuais de EI30 e de KE&gt;25 foram de 5.960,4 MJ mm ha-1 h-1 e de 99,2 MJ ha-1, respectivamente, e estão associados a períodos de retorno de 1,97 ano, com uma probabilidade de ocorrência de 50,82%; e b) valores anuais de EI30 da ordem de 5.995;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosividade da chuva; Erosão hídrica; Função de probabilidade.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200006

Definição do posicionamento de sensores para monitoramento da água no solo em bananeira irrigada por diferentes sistemas de irrigação localizada
Provedor de dados: 70
Autores: Coelho,Eugênio F.; Silva,Alisson J. P. Da; Miranda,Jarbas H. De.
O uso eficiente da água na irrigação localizada dependerá, além de outros fatores, também do correto monitoramento da água no solo. Portanto, este trabalho teve como objetivo caracterizar as zonas efetivas de comprimento de raízes e de extração de água, bem como indicar o correto posicionamento de sensores de água no solo para o manejo da irrigação por gotejamento na bananeira em fase de produção. No experimento, conduzido na Embrapa Mandioca e Fruticultura Tropical, foram estudados diferentes sistemas de irrigação localizada, diante dos seguintes tratamentos: T1 - dois emissores de 4 L h-1 por planta em uma lateral por fileira de plantas; T2 - quatro emissores de 4 L h-1 por planta em uma lateral por fileira de plantas; T3 - cinco emissores de 4 L h-1 por...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Umidade do solo; Manejo de irrigação; Tensiometria; Irrigação localizada.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400005

Caracterização da pulverização de fungicida na cultura do trigo com pontas hidráulicas e atomizadores rotativos de discos
Provedor de dados: 70
Autores: Stefanelo,Maurício S.; Sari,Bruno G.; Lenz,Giuvan; Arrué,Adriano; Pes,Maiquel Pizzuti; Costa,Ivan F. D. da.
O objetivo deste trabalho foi avaliar as características de pulverização de pontas hidráulicas e atomizadores rotativos de discos, utilizando diferentes volumes de calda, na cultura do trigo, bem como seus rendimentos operacionais. Foram realizados dois experimentos, nas safras agrícolas de 2009 e 2010. No primeiro ano, utilizou-se da cultivar Fundacep 30, e no segundo das cultivares Pampeano e Nova Era. As pontas testadas foram do tipo leque e cone vazio, ambas com volume de calda de 120 L ha-1, e atomizadores rotativos de discos utilizando baixo volume oleoso (BVO®), com volumes de calda de 24 e 34 L ha-1. Os parâmetros avaliados foram densidade de gotas (DG) e diâmetro mediano volumétrico (DMV) nos terços superior, médio e inferior, através da análise...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Densidade de gotas; Diâmetro mediano volumétrico; Capacidade operacional.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500020

Perda de carga localizada em gotejadores integrados em tubos de polietileno
Provedor de dados: 70
Autores: Gomes,Anthony W. A.; Frizzone,José A.; Rettore Neto,Osvaldo; Miranda,Jarbas H. de.
Este trabalho foi desenvolvido para analisar as perdas de carga localizadas em gotejadores coaxiais integrados em tubos de polietileno. A perda de carga para diferentes vazões foi determinada em quatro modelos de tubos gotejadores, com sete repetições. Para cada vazão, a perda de carga localizada foi calculada pela diferença entre a perda de carga no tubo com emissor e a perda de carga contínua no tubo uniforme, estimada pela equação de Darcy-Weisbach. Aproximações matemáticas foram sugeridas para calcular a perda de carga com base no coeficiente de carga cinética (K) e em um valor constante de comprimento equivalente (Le). A desconsideração da perda de carga localizada levou à superestimativa do comprimento máximo da linha lateral de até 25,7%, para os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação por gotejamento; Coeficiente de carga cinética; Perda de carga localizada; Índice de obstrução; Comprimento equivalente.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300008

SPATIALIZATION OF SOIL RESISTANCE TO PENETRATION FOR LOCALIZED MANAGEMENT BY PRECISION AGRICULTURE TOOLS
Provedor de dados: 70
Autores: Cortez,Jorge W.; Cavassini,Victor H.; Motomiya,Anamari V. de A.; Orlando,Roberto C.; Valente,Igor Q. M.
ABSTRACT Soil resistance to penetration is an indicator of easy measurement which can be used to make scarification / subsoiling recommendations in areas that work with localized management. The objective of this study was to evaluate the spatial variability of soil resistance to penetration (RP) in the area of direct sowing system, and to carry out the recommendation of scarification / subsoiling in a localized way through precision agriculture. The research was conducted in commercial area, in a field of 49.12 ha. The RP collection was with an electronic penetrometer in a sample mesh of 47 points distributed regularly in the area, with georeferenced points. The data were analyzed every 0.10 m being collected up to 0.40 m depth, in addition to obtaining...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compaction; Cone index; Decompaction.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500690

Produção específica de biogás a partir de manipueira em reator de fase única
Provedor de dados: 70
Autores: Kuczman,Osvaldo; Gomes,Simone D; Tavares,Maria H. F; Torres,Douglas G. B; Alcântara,Michael S.
O presente artigo mostra um estudo sobre a produção de biogás a partir de manipueira, considerando o volume de um reator de fluxo tubular horizontal de fase única. O objetivo do trabalho foi avaliar a produção de biogás aumentando-se as cargas orgânicas e os volumes de alimentação, o que resultou em redução do tempo de retenção hidráulica (TRH). O reator foi alimentado continuamente, com cargas orgânicas de 1,18; 1,28; 1,57 e 2,68 g DQO L-1rd-1 (gramas de demanda química de oxigênio por litro de reator por dia) em TRHs de 15; 13,0; 8,3; 6,6 dias, respectivamente. As produções de biogás foram de 0,52; 0,41; 0,65 e 0,63 L L-1rd-1, destacando-se que o primeiro TRH avaliado foi o de 13 dias, seguido de 8,3; 6,6 e 15 dias. Do estudo, concluiu-se que, com a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água residuária; Digestão anaeróbia; Fecularia; Mandioca; Metano.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100014

Desempenho agronômico de Mentha aquatica cultivada em sistemas alagados construídos sob diferentes taxas de aplicação orgânica
Provedor de dados: 70
Autores: AVELAR,FABIANA F.; MATOS,ANTONIO T. DE; LEITE JUNIOR,ALVIMAR R.; PORTES,MATHEUS R.; GUALHANO,DANIEL S.
Em vista da escassez de informações sobre o comportamento da espécie Mentha aquatica quando cultivada sob condições de alagamento e altas concentrações orgânicas, objetivou--se avaliar o efeito de diferentes taxas de carregamento orgânico (TCOs) sobre a produtividade e o estado nutricional da espécie cultivada em sistemas alagados construídos (SACs) de escoamento horizontal subsuperficial no tratamento de efluente primário de esgoto sanitário. Dois SACs de 24,0 m x 1,0 m x 0,35 m, preenchidos com brita “zero” até a altura de 0,20 m, foram cultivados com a espécie. O experimento foi realizado em duas etapas: na primeira, avaliaram-se as TCOs de 40,35 kg ha-1 d-1 e 53,80 kg ha-1 d-1 de DBO5; na segunda etapa, as TCOs de 79,66 kg ha-1 d-1 e 160,35 kg ha-1 d-1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tratamento de esgoto; Macrófitas; Matéria seca; Concentração foliar de nutrientes.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200322

Effects of vinasse application under the physical attributes of soil covered with sugarcane straw
Provedor de dados: 70
Autores: Costa,Cicero da S.; Pedrosa,Elvira M. R.; Rolim,Mario M.; Santos,Hugo R. B.; Cordeiro Neto,Aluízio T.
Areas under vinasse application have been associated to favorable physical conditions for root development, aeration, infiltration and water movement in soil profile. This study aimed to evaluate changes on physical attributes of soil under sugarcane straw after vinasse application in two sugarcane growing areas (Area 1 and Area 2) under mechanized management in the state of Paraíba, Brazil. In each area, the samples were collected in the 0-0.20, 0.20-0.40 and 0.40-0.60m layers of the soil, in 36 points, distributed in a 10×10m mesh, one day before and 40 days after vinasse application. The data were submitted to multivariate analysis with repeated measures and geostatistics. The vinasse application decreased soil density and increased total porosity in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Residue use; Saccharum; Geostatistics; Soil moisture; Soil density.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400005

Prediction of mean surface temperature of broiler chicks and load microclimate during transport
Provedor de dados: 70
Autores: NAZARENO,AÉRICA C.; SILVA,IRAN J. O. DA; FERNANDES,DANIELLE P. B.
ABSTRACT This study aimed to determine a model to predict mean surface temperature of broiler chicks and live load microclimate conditions during transport by using neural networks. The research was conducted in the state of São Paulo, Brazil, by monitoring nine shipments with different density of boxes using an air-conditioned truck with an average capacity of 380 boxes. Fourteen chick boxes were chosen on each shipment, assessing five chicks per box. The mean surface temperature of chicks (MST) was measured with an infrared thermometer in both loading and unloading. By assessing the container microclimate (center and inside boxes), air temperature (T), relative humidity (RH) and specific enthalpy (h) were recorded; thereby, seventeen data loggers were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry; Ambience; Neural networks; Air-conditioned truck.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400593

Caracterização da produção agroecológica do sul do Rio Grande do Sul e sua relação com a mecanização agrícola
Provedor de dados: 70
Autores: Teixeira,Sandro S.; Machado,Antônio L. T.; Reis,Ângelo V. dos; Oldoni,André.
A agricultura agroecológica tem-se destacado como uma das alternativas de renda para os pequenos agricultores devido à crescente busca por parte da população por alimentação mais saudável. No Rio Grande do Sul, a Associação Regional de Produtores Agroecológicos da Região Sul (Arpasul), constituída por 48 famílias, é representativa do processo de produção e de comercialização de produtos agroecológicos, servindo como referencial para o presente estudo. O objetivo principal deste trabalho foi o levantamento das necessidades dos produtores agroecológicos em relação à mecanização agrícola. As informações obtidas foram baseadas no sistema de produção utilizado, sendo caracterizados aspectos referentes à propriedade, às operações agrícolas e às necessidades...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agroecologia; Pesquisa de campo; Máquinas agrícolas.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100016

Vocalization of broilers can be used to identify their sex and genetic strain
Provedor de dados: 70
Autores: PEREIRA,ERICA M.; NÄÄS,IRENILZA DE A.; GARCIA,RODRIGO G.
In order to reach higher broiler performance, farmers target losses reduction. One way to make this possible is by rearing sexed broilers as male and female present diverse performance due to their physiological differences. Birds from different genetic strain also have a distinct performance at the same age. Considering that sexed flocks may present higher performance this study aimed to identify one-day-old chicks’ sex throughout their vocalization. This research also investigated the possibility of identifying the genetic strain by their vocalization attributes. A total of 120 chicks, half of them were from Cobb® genetic strain and the other half from Ross® genetic strain. From each group, a total of 30 were males and 30 females, which were previously...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Signal analysis; Sex identification; Bioacoustics.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200192

Identificação eletrônica para avaliação do comportamento dos suínos na fase de gestação
Provedor de dados: 70
Autores: Silva,Késia O. da; Nääs,Irenilza de A.
O desempenho eficiente da produção de suínos depende da gestão do rebanho, bem como da nutrição, do controle sanitário, das instalações e de condições ambientais adequadas. O conceito desse tipo de produção está diretamente relacionado com a redução das perdas seletivas e o controle do processo. Cada segmento da produção é controlado de maneira a alcançar a otimização na totalidade do sistema, ou seja, é necessário aplicar conceitos de manejo dos animais. Sendo assim, o presente trabalho apresenta como objetivo o desenvolvimento de modelo matemático para avaliar as interações do ambiente interno da instalação com a preferência térmica dos animais, detectando relação entre a freqüência de acesso ao bebedouro e as condições do ambiente, temperatura ambiente,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Conforte térmico; Dispositivos eletrônicos; Etologia.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200005

Recuperação da topografia de ovos por meio da técnica de moiré e calibração independente
Provedor de dados: 70
Autores: Silva,Gleice C. de A. e; Yanagi Júnior,Tadayuki; Silva,Eberson; Braga Júnior,Roberto A.; Campos,Alessandro T.
A recuperação da topografia de ovos por meio de análise de imagens digitais permite, de forma não destrutiva, a estimativa das massas da gema, da clara, da casca e totais, que são produtos amplamente utilizados na esfera industrial. O presente trabalho buscou desenvolver uma metodologia para a recuperação da forma tridimensional de ovos por meio de análise de imagens, em especial usando a técnica de moiré. Foram utilizados ovos de diferentes tamanhos, classificados em: XL (mais de 73 g), L (63 a 73 g), M (53 a 63 g) e S (até 53 g). Em cada teste realizado em laboratório, um ovo, aleatoriamente selecionado, foi iluminado com a projeção de grades, e as imagens foram capturadas e processadas para a obtenção da forma tridimensional do objeto pela técnica de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Análise de imagens; Ovo; Forma tridimensional.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200001

CHEMICALLY TREATED GLUED LAMINATED PARICÁ TIMBER (Schizolobium parahyba var. amazonicum)
Provedor de dados: 70
Autores: Terezo,Rodrigo F.; Córdova,Franciele O. de; Sampaio,Carlos A. de P.
ABSTRACT In the production of glue-laminated timber (GLT), boards derived from planted forest wood with easy workability are glued on top of one another. The main objective of the present work was to evaluate the performance of paricá timber GLT beams (5 × 10 cm) on GLT. Three procedures were performed: (1) GLT beams (5 × 10 cm) were produced using natural lamellae without chemical preservatives; (2) the individual lamellae (2.5 × 5 cm) were chemically treated, and then glued together; and (3) the beams formed from the glued natural lamellae (5 × 10 cm) were treated chemically. The positions of lamellae on the beams were determined by their modulus of elasticity values (MOE), which were estimated by a non-destructive bending test with a three-point load....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Timber; Beams; Structure.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200158

Method adjustment and equation set of maximum rainfall intensity, duration and frequency in the Mato Grosso do Sul State
Provedor de dados: 70
Autores: Pereira,Silvio B.; Nóia,Carlos P. Z.; Almeida,Rafael A.; Coelho,Clívia D.
Due to the lack of information concerning maximum rainfall equations for most locations in Mato Grosso do Sul State, the alternative for carrying out hydraulic work projects has been information from meteorological stations closest to the location in which the project is carried out. Alternative methods, such as 24 hours rain disaggregation method from rainfall data due to greater availability of stations and longer observations can work. Based on this approach, the objective of this study was to estimate maximum rainfall equations for Mato Grosso do Sul State by adjusting the 24 hours rain disaggregation method, depending on data obtained from rain gauge stations from Dourado and Campo Grande. For this purpose, data consisting of 105 rainfall stations...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Intense rainfall; Rainfall disaggregation; Weather stations.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400011

Diferentes diâmetros de gotas e equipamentos para aplicação de inseticida no controle de Pseudoplusia includens
Provedor de dados: 70
Autores: Oliveira,José R. G. di; Ferreira,Marcelo da C.; Román,Rodrigo A. A.
Teve-se o objetivo de avaliar o espectro e a uniformidade de gotas em função de equipamentos de pulverização, volumes de calda e dosagem de inseticida na mortalidade de Pseudoplusia includens em laboratório. O trabalho foi conduzido na UNESP de Jaboticabal, sendo realizada uma aplicação sobre as lagartas com os tratamentos: dois equipamentos (bico rotativo e bico hidráulico); dois volumes de calda (17 e 50 L ha-1 para o bico rotativo, e 50 e 100 L ha-1 para o bico hidráulico), e duas dosagens do inseticida endosulfan (0,5 e 1,0 L p.c. ha-1), segundo delineamento inteiramente casualizado, no esquema fatorial 2x2x2 + 1 testemunha. Avaliou-se diariamente a mortalidade das lagartas até o sexto dia após a aplicação dos tratamentos. O espectro de gotas foi...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bico rotativo; Espectro de gotas; Lagarta falsa-medideira.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100010

Nova metodologia para interpretação de dados de análise sensorial de alimentos
Provedor de dados: 70
Autores: Silva,Francisco de A. S. e; Duarte,Maria E. M.; Cavalcanti-Mata,Mario E. R. M.
Os métodos atualmente utilizados para realização de análise sensorial têm deixado muito a desejar por não traduzir satisfatoriamente os resultados. Diante deste problema, analisou-se a possibilidade de introdução de um fator que medisse o índice de concordância dos provadores sobre determinado aspecto analisado. Para validação deste coeficiente, foi avaliada a concordância entre julgadores na análise sensorial para três diferentes amostras de suco de pinha (Annona squamosa L.): uma constituída apenas do suco de pinha sem leite e duas com diferentes concentrações pinha/leite. Utilizou-se a Análise de Componentes Principais (ACP) e também a nova metodologia proposta pelos autores, com base na definição do desvio-padrão, aplicada às frequências absolutas das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coeficiente de concordância; Propriedades sensoriais; Degustadores.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500018

Avaliação do modelo HYDRUS-1D na simulação do transporte de água e potássio em colunas preenchidas com solos tropicais
Provedor de dados: 70
Autores: Pinho,Roque E. da C. de; Miranda,Jarbas H. de.
A preocupação com o destino de produtos químicos e água, aplicados ao solo, tem motivado vários pesquisadores a desenvolverem e aplicarem modelos teóricos, a fim de descrever os processos físicos envolvidos no transporte desses produtos no perfil do solo. Nesse sentido, esta pesquisa teve como objetivo aplicar o modelo HYDRUS-1D, bem como avaliar sua performance, em simulações do deslocamento do potássio e água (umidade do solo), em colunas segmentadas, preenchidas com dois tipos de solos tropicais, em condições não saturadas (Latossolo Vermelho- - Amarelo e Nitossolo Vermelho). Os parâmetros de transporte do potássio foram obtidos por meio de curvas de distribuição de efluentes (Breakthrough Curves (BTC)). O desempenho do modelo foi avaliado com base nos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Transporte de contaminantes; Lixiviação; Modelagem computacional; HYDRUS-1D.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500009

Análise econômica da geração de energia elétrica a partir do biogás na suinocultura
Provedor de dados: 70
Autores: Martins,Franco M.; Oliveira,Paulo A. V. de.
A demanda por fontes alternativas de energia tem crescido nos últimos anos em função das variações do preço do petróleo aliadas à recente crise energética. Por meio da digestão anaeróbia é possível transformar os dejetos de suínos em biogás. No presente trabalho, estudou-se a viabilidade econômica do uso do biogás como fonte alternativa para a geração de energia elétrica para diferentes períodos de geração. O método utilizado para a avaliação econômica foi o Valor Presente Líquido. O tempo de retorno do capital investido também foi calculado levando em consideração o desconto da taxa de juros nos fluxos de caixa. O estudo demonstrou ser economicamente viável a utilização do biogás da suinocultura, como fonte para geração de energia elétrica. O aumento da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogás; Suínos; Energia elétrica; Análise econômica.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300008

Ambientes protegidos e substratos com doses de composto orgânico comercial e solo na formação de mudas de Jatobazeiro em Aquidauana-MS
Provedor de dados: 70
Autores: Santos,Léia C. R. dos; Costa,Edilson; Leal,Paulo A. M.; Nardelli,Evandro M. V.; Souza,Guilherme S. A. de.
O Cerrado brasileiro possui inúmeras espécies frutíferas com potencial econômico para exploração em cultivo comercial. Neste contexto, desenvolveu-se um experimento com mudas de jatobá-do-cerrado na Universidade Estadual de Mato Grosso do Sul, em Aquidauana - MS, de 29-outubro-2009 a 25-fevereiro-2010, em estufa agrícola coberta com filme de polietileno de 150 μm, difusor de luz, possuindo tela termorrefletora de 50% sob o filme e fechamentos laterais e frontais com tela de monofilamento, malha para 50% de sombreamento e viveiro com tela preta de monofilamento para sombreamento de 50%, fechamento em 45º. Nesses ambientes, as mudas foram formadas em vasos plásticos de 5,0 L, preenchidos com 100% de solo, 100% de composto orgânico e as doses de 10; 20; 30;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hymenaea stigonocarpa; Fruteiras do cerrado; Propagação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200005

Granjas leiteiras na região de Ribeirão Preto - SP
Provedor de dados: 70
Autores: Milani,Adhemar P.; Souza,Fernando A. De.
Nas atividades de exploração leiteira, as construções para os animais são fundamentais e de suma importância no processo de produção. Sendo assim, suas concepções devem basear-se em soluções técnicas e econômicas, que ofereçam condições eficientes e funcionais. O objetivo deste trabalho foi realizar um levantamento sobre as principais características de granjas leiteiras localizadas em municípios paulistas próximos a Ribeirão Preto e no sul de Minas Gerais e recomendar soluções, com base na literatura, para a execução de projeto para a região de Ribeirão Preto-SP. O trabalho foi desenvolvido com base em estudos teóricos e observações in loco, considerando as seguintes construções: galpão de estabulação livre; bezerreiro; sala de ordenha e seus anexos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Construções rurais; Bovinocultura de leite; Granjas leiteiras.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400018

Armazenamento refrigerado da uva de mesa 'Romana' (A1105) cultivada sob cobertura plástica
Provedor de dados: 70
Autores: Lulu,Jorge; Castro,Josalba V.; Pedro Júnior,Mário J.
A videira é uma das principais fruteiras cultivadas em todo o mundo e atualmente a preferência por uvas do tipo "sem sementes" ou "apirênicas" vem aumentando gradativamente no mercado interno brasileiro. A cultivar 'Romana' (A1105) tem mostrado grande potencial como nova alternativa de uva de mesa apirênica na região de Jundiaí - SP. No entanto, a qualidade dos cachos tem sido afetada pela ocorrência de chuvas na época da colheita, propiciando a incidência de rachaduras nas bagas ("cracking") e podridões. Visando a solucionar essa dificuldade, foram conduzidos experimentos de campo em vinhedo cultivado em cortina dupla e sob cobertura plástica. Após a colheita, foram coletadas oito amostras com seis cachos cada, que foram armazenadas a 3 ºC e submetidas a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vitis sp.; Perda de massa; Podridões.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200022

Parâmetros de dimensionamento para biodigestores batelada operados com dejetos de vacas leiteiras com e sem uso de inóculo
Provedor de dados: 70
Autores: Xavier,Cristiane de A. N; Lucas Júnior,Jorge de.
Objetivou-se avaliar a adição de inóculo na biodigestão anaeróbia de dejetos de vacas leiteiras reciclados em biodigestores bateladas pela quantidade de biogás produzida, pela redução dos sólidos voláteis e pelos potenciais de produção de biogás para obtenção de parâmetros de dimensionamento. Foram utilizados 12 biodigestores bateladas de campo de 60 L, cujos substratos continham dejetos de vacas leiteiras, água e quatro adições de inóculo (0; 20; 30 e 40% v/v). Adotaram-se tempos médios de retenção hidráulica de 75 e 150 dias para os tratamentos contendo inóculo e sem inóculo, respectivamente, nos períodos intermediário, chuvoso e seco do ano. Maiores produções de biogás ocorreram com maiores temperaturas médias do ar. Maiores potenciais de produção de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Período chuvoso; Período seco; Potenciais; Produção de biogás; Redução.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200003

Geotecnologias para mapear lavouras de café nos estados de Minas Gerais e São Paulo
Provedor de dados: 70
Autores: Moreira,Mauricio A.; Rudorff,Bernardo F. T.; Barros,Marco A.; Faria,Viviane G. C. de; Adami,Marco.
O uso operacional de imagens de satélites de sensoriamento remoto para mapear lavouras de café em grandes áreas, para fins de obtenção de estatísticas agrícolas confiáveis e oportunas, ainda se encontra em desenvolvimento. Diversos são os fatores que dificultam a correta identificação e mapeamento do parque cafeeiro. Contudo, os avanços tecnológicos observados nos últimos anos em termos de aquisição de imagens com melhor qualidade e em maior quantidade, bem como o desenvolvimento de novas ferramentas de análise, propiciam o desenvolvimento de um método operacional que pode contribuir na formação das estatísticas agrícolas oficiais do café no Brasil. Neste sentido, o presente trabalho tem por objetivo relatar a metodologia e apresentar os resultados do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensoriamento remoto; Imagens de satélite; Geoprocessamento; Estatísticas agrícolas.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600013

Utilização da técnica por componentes principais (acp) e fator de iluminação, no mapeamento da cultura do café em relevo montanhoso
Provedor de dados: 70
Autores: Lamparelli,Rubens A. C.; Nery,Luiz; Rocha,Jansle V.
O objetivo deste trabalho foi avaliar as informações obtidas das imagens do satélite Landsat/TM5, utilizando técnicas de Análise por Componentes Principais (ACP) e Fator de Iluminação oriundo de um Modelo de Elevação do Terreno, calculado a partir de imagens ASTER, no mapeamento de áreas de café em terreno montanhoso. As imagens utilizadas (três) foram corrigidas para o efeito da atmosfera e cobriram, temporalmente, o ciclo da cultura. Foram calculadas as componentes principais e escolhidas as duas primeiras, as quais possuíam 94% das informações, para a definição das amostras. As amostras resultantes da ACP foram utilizadas na classificação supervisionada cujo resultado foi comparado com uma classificação convencional e uma classificação multitemporal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensoriamento remoto; ASTER; Correção atmosférica; Normalização radiométrica; Processamento digital de imagens.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300018

PARTICLEBOARDS PRODUCED WITH EPOXY INK WASTE AND BTH POLYMER AS ADHESIVES
Provedor de dados: 70
Autores: Christoforo,André L.; Souza,Amós M. de; Almeida,Diego H. de; Almeida,Tiago H. de; Lahr,Francisco A. R.
ABSTRACT The aim of this research was to analysis the feasibility of production of wood particleboard with two alternative adhesives: epoxy ink waste and polyhydroxybutyrate polymer (BTH). Particleboard were produced with Pinus sp. wood specie wastes from sawmill process. For each alternative adhesive was proposed different combinations of parameters: time and temperature of press, pressure; alternative adhesive content and mass of wood particles. Two alternative adhesive contents were adopted, 10% and 20% replacing ureaformaldehyde adhesive. Mechanical properties (perpendicular tensile strength, pullout strengths of screw on face and top; modulus of elasticity and rupture) were determined according to ABNT NBR 14810:3 Brazilian Standard Code. The obtained...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adhesives; Particleboards; BTH polymer; Mechanical properties; Epoxy ink waste.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500797

Cultivo de alface em solos com hidrogel utilizando irrigação automatizada
Provedor de dados: 70
Autores: Santos,Hugo T. dos; Carvalho,Daniel F. de; Souza,Claudinei F.; Medici,Leonardo O.
RESUMO Visando à otimização do uso da água na produção de alimentos, este artigo teve como objetivo avaliar o desempenho da TDR e de um acionador automático para irrigação na produção da alface em solos com diferentes doses de um polímero hidrofílico. Em casa de vegetação, foram realizados dois ensaios em vasos de 3 litros cultivados com alface. O primeiro foi realizado na primavera de 2011, utilizando 2 texturas de solo (arenosa e argilosa) e a presença/ausência do hidrogel. O segundo ensaio foi realizado no outono de 2012, utilizando 4 doses de hidrogel (0; 8; 16 e 24 g por vaso) no solo de textura arenosa. Aos 38 (2011) e 44 (2012) dias após o transplantio (DAT) das mudas, foram realizadas as colheitas e a avaliação das plantas cultivadas. O hidrogel...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Polímero hidrofílico; TDR; Automação e gotejamento.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500852

Consorciação de braquiárias com milho outonal em plantio direto sob pivô central
Provedor de dados: 70
Autores: Chioderoli,Carlos A.; Mello,Luiz M. M. de; Grigolli,Paola J.; Silva,José O. da R.; Cesarin,André L.
Em regiões de clima tropical, com altas taxas de decomposição do material orgânico, uma alternativa para suprir o aporte anual de palha exigido para proporcionar a sustentabilidade do sistema plantio direto é a consorciação de forrageiras com culturas produtoras de grãos. Com o objetivo de identificar, no sistema de integração agricultura-pecuária, a melhor modalidade de consorciação de três espécies de braquiária (Brachiaria brizantha B. decumbens, e B. ruzizienses) com milho outonal (linha, entrelinha e entrelinha na época de adubação de cobertura do milho), foi conduzido o presente trabalho. Foi utilizado o delineamento em blocos ao acaso, no esquema fatorial (3x3), com quatro repetições. Foram avaliadas: massa seca de palha do milho, massa seca da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cobertura do solo; Integração lavoura-pecuária; Palhada; Sucessão de culturas; Brachiaria.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600011

Produtividade do feijão-de-corda e acúmulo de sais no solo em função da fração de lixiviação e da salinidade da água de irrigação
Provedor de dados: 70
Autores: Assis Júnior,José O. de; Lacerda,Claudivan F. de; Silva,Flávio B. da; Silva,Francisco L. B. da; Bezerra,Marlos A.; Gheyi,Hans R.
Neste trabalho, avaliaram-se o acúmulo de sais no solo e a produtividade do feijão-de-corda, em função da fração de lixiviação (FL) e da salinidade da água de irrigação. Utilizou-se de delineamento em blocos ao acaso, com quatro tratamentos e cinco repetições. Foram estudados os seguintes tratamentos: 1 - água do poço com condutividade elétrica (CEa) de 0,8 dS m-1 (sem FL); 2 - água salina com CEa de 5,0 dS m-1 sem FL; 3 - água salina com CEa de 5,0 dS m-1 com FL de 0,14; 4 - água salina com CEa de 5,0 dS m-1 com FL de 0,28. Foram avaliadas as seguintes variáveis: acúmulo de sais no solo, crescimento vegetativo, produtividade, trocas gasosas e teores de Na+, Ca+2, K+ e Cl- nas folhas. A aplicação de água salina provocou acúmulo de sais no solo, porém esses...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água salina; Vigna unguiculata L. Walp.; Estresse salino.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400013

Economic analysis for sizing of sugarcane (Saccharum spp.) mechanized harvesting
Provedor de dados: 70
Autores: Santos,Neisvaldo B. dos; Silva,Rouverson P. da; Gadanha Junior,Casimiro D.
Sugarcane has a significant role on Brazilian agribusiness economy. The harvesting cane is considered as one of the most important operations of the process for it has to attend the raw material demanded by the sugar mill in quality and a competitive cost. The objective of this work it is it of analyzing, of systemic way, the variables influence on economical and operational performance in sugarcane mechanized harvesting process for sizing of machines. For this purpose a model called "ColheCana", was developed in a spreadsheet and in a programming language. The results showed that the field efficiency and harvester´s initial value are variables of great impact in the cost and that there is a maximum area that one equipment can attend and for this area the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural mechanization; Sugarcane harvester; Computational model.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500013

Comparative study of energy costs in irrigation according to the new brazilian electricity tariff model
Provedor de dados: 70
Autores: ALMEIDA,ALEX N. DE; COELHO,RUBENS D.; FARÍAS,ASDRÚBAL J.; MONTEIRO,RODRIGO O. C.; COSTA,JÉFFERSON DE O.
ABSTRACT The tariff flags on Brazil came into force in January 2015, applied to all electrical distribution agents of the national interconnected system (SIN) and all final consumers are being charged for this new model. Given this, the cost of electricity in irrigation suffered representative additions involving searches of alternatives, such as the use of diesel engines. This study aimed to analyze the costs and the total annual costs of pumping with diesel and electric operation in 3 regions of Brazil, considering the application of the tariff flags. We concluded that the Southeast region (SE) features an hourly cost of electricity above the Central-West (CO) and the Northeast (NE) regions at any adopted tariff, regardless of the time of pumping and the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tariff flags; Costs; Diesel; Irrigation.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500902

Potential of biogas production from swine manure supplemented with glycerine waste
Provedor de dados: 70
Autores: Konrad,Odorico; Koch,Fabio F.; Lumi,Marluce; Tonetto,Jaqueline F.; Bezama,Alberto.
In this study, was studied the biogas generation from swine manure, using residual glycerine supplementation. The biogas production by digestion occurred in the anaerobic batch system under mesophilic conditions (35°C), with a hydraulic retention time of 48 days. The experiment was performed with 48 samples divided into four groups, from these, one was kept as a control (without glycerin) and the other three groups were respectively supplemented with residual glycerine in the percentage of 3%, 6% and 9% of the total volume of the samples. The volume of biogas was controlled by an automated system for reading in laboratory scale and the quality of the biogas (CH4) measured from a specific sensor. The results showed that the residual glycerine has high...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogas; Residual glycerin; Swine manure; Renewable energy.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500004

Analysis and forecast of the storage needs of soybeans in Brazil
Provedor de dados: 70
Autores: Patino,Marco T. O.; Machado,Marina F.; Nascimento,Geraldo T. do; Alcantara,Milla R. de.
The existence of a minimum storage capacity of grains as a condition for the maintenance of regulator physical stocks has been used as a strategic factor in the agribusiness expansion. However, in Brazil the storage infrastructure has not followed the growth of the agricultural sector. This fact is evident in the case of soybeans that currently represent 49% of grain production in the country, whose volume production has been increasing significantly over the years. This study aimed to predict the futureï€ needs of static storage capacity of soybeans from historical data to estimate the investment needed to install storage units in Brazil for the next five years. A statistic analysis of collected data allowed a forecast and identification of the number of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agribusiness; Glycine max; Temporal series; Harvest seasons.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400022

Coeficiente de cultura (Kc) do cafeeiro (Coffea arabica L.) no período de outono-inverno na região de Lavras - MG
Provedor de dados: 70
Autores: Sato,Fabio A.; Silva,Antônio M. da; Coelho,Gilberto; Silva,Antônio C. da; Carvalho,Luiz G. de.
O balanço hídrico é de elevada importância para avaliar a intensidade das entradas e saídas de água em um volume de solo explorado por uma cultura, permitindo, ainda, estimar parâmetros característicos das suas necessidades hídricas, como a evapotranspiração e o coeficiente de cultura (Kc), que se apresentam como indicadores com significados físicos e biológicos da planta, sobretudo quando associados com o seu ciclo fenológico. Dessa forma, neste trabalho, monitorou-se o regime hídrico e climático, de abril a setembro de 2004, e estimou-se a evapotranspiração da cultura (ETc) e o Kc do cafeeiro Catuaí, após quatro anos de recepa, utilizando-se do método do balanço hídrico. Os resultados obtidos permitiram concluir que o cafeeiro, após quatro anos de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Balanço hídrico; Café; Irrigação.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300007

ERRATUM: RESIDUE ANALYSIS OF ORGANOCHLORINE AND ORGANOPHOSPHORUS PESTICIDES IN URBAN LAKE SEDIMENTS
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100158

Erratum
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500951

Citrus root distribution under water stress grown in sandy soil of central Florida
Provedor de dados: 70
Autores: Alves Júnior,José; Bandaranayake,Wije; Parsons,Larry R.; Evangelista,Adão W. P.
The experiment was conducted in an orchard located in University of Florida (Citrus Research and Education Center), Lake Alfred, Polk County, Florida, USA. The objective of this study was to evaluate the effects of water stress in root distribution of 'Valencia' orange tree on 'Swingle' citrumelo rootstock. Three treatments were imposed on the trees: 1) normal irrigation with microsprinklers, 2) no irrigation in winter (November through mid-March) and 3) rainfall exclusion by placing a water repelling fabric (Tyvek) under the trees. Trees in treatments 1 and 2 received normal rainfall during the winter, but treatment 3 received no rain. Normal irrigation was resumed on all treatments in mid March. Soil was collected using root auger head (0.09 m diameter...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Orange; Roots.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600012

FULL CHARACTERIZATION OF CALYCOPHYLLUM MULTIFLORUM WOOD SPECIE
Provedor de dados: 70
Autores: Christoforo,André L.; Arroyo,Felipe N.; Silva,Diogo A. Lopes; Panzera,Tulio H.; Lahr,Francisco A. R.
ABSTRACT: Wood is a material that for years has been used by man for a variety of purposes, particularly in rural and civil constructions and furniture industry. The possibility of shortages of some wood species, the characterization of other unfamiliar species is an alternative source for use in civil and rural construction. This study aimed to determine, with the aid of Brazilian standard NBR 7190, physical and mechanical properties of Castelo (Calycophyllum multiflorum) wood specie. Twelve determinations were obtained by property, totaling 204 experimental values. In the characterization of wood, regression models were used to estimate the values of timber strength and stiffness as a function of apparent density, being density the physical property more...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Calycophyllum multiflorum; Physical-mechanical properties; Hardwood; Regression model.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400637

ACOUSTIC ENVIRONMENT AND GAS PRODUCTION IN DIFFERENT GROWING-FINISHING SWINE FACILITIES
Provedor de dados: 70
Autores: Andrade,Rafaella R.; Campos,Alessandro T.; Cecchin,Daiane; Sousa,Francine A.; Amaral,Pedro I. S.
ABSTRACT This study aimed to evaluate gas levels and the acoustic environment (noise) of growing-finishing swine in different facilities, one composed of shallow pool (SP) and another of partially slatted floor (PSF). Sensors and a sound level meter were used to measure gas concentrations (CO2 and NH3) and noise at 1.50 meters above the ground and at animal height. Data on gas concentrations and noise levels were measured at 9am, 12pm, and 3 pm. Results showed differences (P&lt;0.05) between noise levels at animal height and gas concentrations measured in relation to stall type and data collection time. The highest noise values were found in the shallow pool stall, measured at animal level. The highest NH3 (13 ppm) and CO2 (1174.5 ppm) values were observed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Welfare; Air quality; Noise.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000600953

Technical evaluation of artificial ligthing systems for broiler houses
Provedor de dados: 70
Autores: Pereira,Priscilla A.; Yanagi Junior,Tadayuki; Silva,Joaquim P. da; Lima,Renato R. de; Campos,Alessandro T.; Abreu,Lucas H. P.
The spatial distribution of illuminance and the electric consumption of artificial lighting system is one of the main problems related to broiler production. Therefore, the aim of this study was to evaluate the spatial distribution of luminance level and energy efficiency of different lighting systems for broiler houses. Six types of lamps were tested in two different configurations to find the minimum illuminance of 20 and 5 lux. The tested lamps were incandescent (IL) 100 W, compact fluorescent (CFL) 34 W, mixed (ML) 160 W, sodium vapor (SVL) 70 W, T8 fluorescent tube (T8 FTL) 40 W and T5 fluorescent tube (T5 FTL) 28 W. The first four were evaluated with and without reflective light fixture and the latter two without light fixture. It was observed that...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Artificial lighting; Spatial variability; Energy efficiency; Aviculture.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600002

Tendências recentes nos elementos do clima e suas implicações na evapotranspiração da cultura do milho em Viçosa - MG
Provedor de dados: 70
Autores: Alencar,Leonidas P. de; Sediyama,Gilberto C.; Mantovani,Everardo C.; Martinez,Mauro A.
A mudança nas condições climáticas tem gerado grandes preocupações em nível mundial, sendo que uma das grandes questões, neste contexto, é o aquecimento global. As alterações ocorridas nas condições climáticas podem afetar a demanda de água das plantas, porque a evapotranspiração é afetada por mudanças nos elementos climáticos. O objetivo deste trabalho foi analisar os efeitos das possíveis mudanças dos elementos do clima na evapotranspiração de referência e na evapotranspiração da cultura do milho para a região de Viçosa - MG. Mediante análise de tendência pelo teste de Mann-Kendall e da estatística do teste t da regressão linear, verificou-se o comportamento dos seguintes elementos climáticos: temperaturas máxima e mínima, insolação, velocidade do vento...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiração do milho; Tendência; Mudanças climáticas.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400002

Desenvolvimento de um sistema alternativo de trocador de calor para climatização de construções agroindustriais
Provedor de dados: 70
Autores: Soares,Milton; Souza,Samuel N. M. de; Halmeman,Maria C. R.; Fracaro,Guilherme de P. M.
No manejo de animais em propriedades rurais, é necessário o desenvolvimento de equipamentos de climatização de ambientes, tais como os resfriadores evaporativos. No presente estudo, foi construído e testado um resfriador evaporativo alternativo. O sistema é composto por um circuito de circulação de água impulsionada por uma bomba hidráulica e uma rede de tubulação em PVC formadora de uma cortina de água, uma calha condutora de água e um reservatório. A temperatura e a umidade relativa foram medidas na entrada e saída do equipamento, utilizando-se de termo-higrômetro digital, no período de 28 de novembro a 14 de dezembro de 2006 (dias quentes e secos do início de verão) e entre 6 e 13 de março de 2007 (dias quentes e úmidos). Associado a um sistema de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Trocador de calor; Resfriamento; Temperatura.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300001

Efeito da adição de diferentes substâncias químicas no extrato de sementes de moringa utilizado como coagulante no tratamento de esgoto sanitário
Provedor de dados: 70
Autores: Lo Monaco,Paola A. V.; Matos,Antonio T.; Pereira,Magno dos S.; Eustáquio Júnior,Valdeir; Batista,Ana Paula da S.; Baker,Sandy A. A.
Este trabalho foi realizado em duas fases. Na primeira, objetivou-se avaliar o efeito de diferentes concentrações de sementes de moringa, aplicadas na forma de extrato, na remoção de turbidez de esgoto sanitário. A segunda fase consistiu em avaliar o efeito da adição de diferentes sais (NaCl e KCl) e uma base (Ca(OH)2) no preparo do extrato de sementes de moringa, com a melhor faixa de remoção obtida na fase 1, utilizada como agente coagulante na remoção de turbidez de esgoto sanitário. De acordo com os resultados obtidos, pôde-se concluir que a máxima eficiência na remoção da turbidez, utilizando-se do extrato de semente de moringa preparado tanto com NaCl como com KCl, foi obtida na concentração de 2 g L-1; das três substâncias químicas utilizadas no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água residuária; Coagulantes naturais; Efluentes urbanos.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500015

Hydrogen production from cassava processing wastewater in an anaerobic fixed bed reactor with bamboo as a support material
Provedor de dados: 70
Autores: Andreani,Cristiane L.; Torres,Douglas G. B.; Schultz,Leonardo; Carvalho,Karina Q. de; Gomes,Simone D.
Attempting to associate waste treatment to the production of clean and renewable energy, this research sought to evaluate the biological production of hydrogen using wastewater from the cassava starch treatment industry, generated during the processes of extraction and purification of starch. This experiment was carried out in a continuous anaerobic reactor with a working volume of 3L, with bamboo stems as the support medium. The system was operated at a temperature of 36°C, an initial pH of 6.0 and under variations of organic load. The highest rate of hydrogen production, of 1.1 L.d-1.L-1, was obtained with application of an organic loading rate of 35 g.L-1.d-1, in terms of total sugar content and hydraulic retention time of 3h, with a prevalence of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fixed bed reactor; Agroindustrial wastes; Fermentation processes.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300578

Desempenho de motor ciclo Diesel em bancada dinamométrica utilizando misturas diesel/biodiesel
Provedor de dados: 70
Autores: Castellanelli,Marcio; Souza,Samuel N. M. de; Silva,Suedêmio L.; Kailer,Euro K.
Diante da previsão de escassez do petróleo, o éster etílico (biodiesel) tem-se apresentado como excelente opção de combustível alternativo para motores ciclo Diesel. As características do biodiesel são semelhantes às do diesel em termos de viscosidade e poder calorífico, podendo ser utilizado sem adaptações nos motores. Para a realização deste trabalho, utilizou-se de motor ciclo Diesel, de injeção direta, com quatro cilindros, sem adaptações. O motor foi acoplado a um dinamômetro e sistemas de aquisição de dados auxiliares. Avaliaram-se os desempenhos de torque, de potência e de consumo específico de combustível para as seguintes misturas diesel/éster etílico de soja: B2, B5, B10, B20, B50, B75 e B100. O melhor desempenho registrado deu-se com a mistura...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Éster etílico; Combustível alternativo; Motor ciclo Diesel.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100015

Força de tração necessária em função do número de linhas de semeadura utilizadas por uma semeadora-adubadora de precisão
Provedor de dados: 70
Autores: Modolo,Alcir J.; Gabriel Filho,Antonio; Silva,Suedêmio de L .; Gnoatto,Estor.
Este trabalho teve como objetivo avaliar o comportamento da força de tração solicitada por uma semeadora-adubadora, variando o número de linhas de semeadura. O experimento foi conduzido no Núcleo Experimental de Engenharia Agrícola - NEEA, pertencente à UNIOESTE - Câmpus de Cascavel - PR, em um Latossolo Vermelho distroférico com relevo plano e textura argilosa. Utilizou-se o delineamento experimental de blocos ao acaso, composto por cinco tratamentos e quatro repetições. Foram utilizados os seguintes tratamentos: semeadora equipada com uma, duas, três, quatro e cinco linhas de semeadura, deslocada à velocidade média de 5,5 km h-1. Avaliaram-se os parâmetros de profundidade do sulco, área de solo mobilizada, força de tração média e força de tração máxima....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semeadora-adubadora; Força de tração; Profundidade do sulco.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200020

Caracterização granulométrica de biomassa polidispersa pelo método de peneiramento mecânico
Provedor de dados: 70
Autores: Jordan,Rodrigo A.; Baldassin Junior,Ricardo; Cortez,Luiz A. B.; Motomiya,Anamari V. A.
RESUMO A biomassa polidispersa tem como uma de suas principais características as variações das dimensões e dos formatos de suas partículas. Os métodos de determinação do diâmetro médio por peneiramento, amplamente utilizados devido a sua relativa simplicidade e baixo custo, quando aplicados a materiais heterogêneos, como a biomassa polidispersa, podem levar a resultados equivocados. Assim, com o objetivo de obter resultados mais precisos, foram avaliados três métodos de determinação do diâmetro médio de partículas de biomassa polidispersa, baseados na técnica de fracionamento por peneiramento mecânico: um de forma analítica (Diâmetro de Sauter) e outros dois por meio de análise gráfica das funções de distribuição das partículas (Função de Densidade de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bagaço de cana-de-açúcar; Diâmetro médio; Distribuição granulométrica; Método gráfico; Método analítico.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100102

The use of ALOS/PALSAR data for estimating sugarcane productivity
Provedor de dados: 70
Autores: Picoli,Michelle C. A.; Lamparelli,Rubens A. C.; Sano,Edson E.; Rocha,Jansle V.
Some models have been developed using agrometeorological and remote sensing data to estimate agriculture production. However, it is expected that the use of SAR images can improve their performance. The main objective of this study was to estimate the sugarcane production using a multiple linear regression model which considers agronomic data and ALOS/PALSAR images obtained from 2007/08, 2008/09 and 2009/10 cropping seasons. The performance of models was evaluated by coefficient of determination, t-test, Willmott agreement index (d), random error and standard error. The model was able to explain 79%, 12% and 74% of the variation in the observed productions of the 2007/08, 2008/09 and 2009/10 cropping seasons, respectively. Performance of the model for the...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Synthetic aperture radar; L-band; Modeling; Remote sensing.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600019

Effect of time-temperature binomial in obtaining biochemical oxygen demand of different wastewaters
Provedor de dados: 70
Autores: Matos,Mateus P. de; Borges,Alisson C.; Matos,Antonio T. de; Silva,Edson F. da; Martinez,Mauro A.
Studies on the effects of temperature and time of incubation of wastewater samples for the estimation of biodegradable organic matter through the biochemical oxygen demand (BOD), that nowadays are rare, considering that the results of the classic study of STREETER &amp;amp; PHELPS(1925) have been accepted as standard. However, there are still questions how could be possible to reduce the incubation time; whether the coefficient of temperature (θ) varies with the temperature and with the type of wastewater and if it approaches 1.047. Aiming the elucidation of these questions, wastewater samples of dairy, swine and sewage treated in septic tanks were incubated at temperatures of 20, 30 and 35 °C, respectively for 5, 3.16 and 2.5 days. From the parameter of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Degradation deoxygenation coefficient temperature coefficient Streeter &amp;amp; Phelps.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200014

Physical attributes of a pasture soil in southeast Goiás determined by geostatistics
Provedor de dados: 70
Autores: Cardoso,Gabriel G. de G.; Wanderley,Rilley C.; Souza,Mara L. C.
ABSTRACT This study aimed to evaluate the spatial dependence of physical attributes in a soil cultivated with Brachiaria grass. A 12-m regular sampling grid was established within an area of 3.500 m2. Thirty-five soil samples were collected at 0-30 cm depth for particle density, bulk density, texture and total porosity analysis. These data were evaluated using statistical methods of indicator kriging and the GS+ software. The GS+ software was used to develop three-dimensional maps and evaluate semivariograms. The spatial dependence was evaluated using experimental semivariograms. The analyzed attributes indicated the occurrence of spatial dependence when fit to the exponential model. Areas with higher porosity occurred in the regions with lower bulk...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spatial variability; Management system; Kriging.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100143

Variação da evapotranspiração de referência calculada em diferentes intervalos de tempo
Provedor de dados: 70
Autores: Back,Álvaro J.
Valores de evapotranspiração de referência foram calculados em intervalos de um, cinco, dez, quinze dias e mensal. Foram utilizados dados meteorológicos da Estação Meteorológica de Urussanga - SC (latitude 28°31'S, longitude 49°19'W) referentes ao período de 1981 a 2004. A evapotranspiração de referência foi calculada pelo método de Penman-Monteith com base nas médias das variáveis meteorológicas dos diferentes períodos estudados. Observou-se que não houve diferenças significativas nas médias de evapotranspiração calculadas nos diversos intervalos de tempo. No entanto, houve diferenças significativas na dispersão dos valores em torno da média. Para valores diários, foi obtido coeficiente de variação (C.V.) entre 30 e 40%, e para valores mensais, variou...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Balanço hídrico; Probabilidade; Evapotranspiração.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100007

MOISTURE SORPTION ISOTHERMS OF QUINOA SEEDS: THERMODYNAMIC ANALYSIS
Provedor de dados: 70
Autores: Bustos-Vanegas,Jaime D.; Corrêa,Paulo C.; Zeymer,Juliana S.; Baptestini,Fernanda M.; Campos,Renata C.
ABSTRACT The present research aimed to study the water sorption behavior of quinoa seeds analyzing the hysteresis phenomenon and determining thermodynamic properties. Static gravimetric technique was used to obtain the equilibrium moisture content of quinoa seeds in different temperature conditions (15, 25, 35 e 50 °C) and relative humidity (between 11 and 96%). Equilibrium moisture content data were adjusted by eight mathematical models and the Modified Halsey model was the best one to describe the water sorption phenomena of quinoa seeds. Hygroscopic equilibrium moisture content of quinoa seeds is directly proportional to the water activity and decreases with increasing temperature. The hysteresis phenomena were observed throughout the range of water...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Entropy; Gibbs energy; Hysteresis; Isosteric heat; Mathematical modeling.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600941

PERCOLATE QUALITY IN SOIL CULTIVATED WITH APPLICATION OF WASTEWATER FROM SWINE SLAUGHTERHOUSE AND DAIRY PRODUCTS
Provedor de dados: 70
Autores: Oliveira,Jacineumo F. de; Rodrigues,Fernando N.; Fia,Ronaldo; Mafra,Dayana C. B.; Landim,Daniela V.
ABSTRACT The objective of this study was to evaluate the quality of the percolate in soil columns cultivated with Tiffon-grass 85 under different wastewater rates from swine slaughterhouse and dairy. The experiment was conducted at the Department of Engineering at the Federal University of Lavras, in PVC columns with 0.30 m of diameter and 1.2 m deep, filled with Dark Red Latosol cultivated with Tifton-grass 85. The treatments consisted of a (AQT0) control with recommended chemical fertilization for Tifton-grass 85 (300 kg ha-1 year-1 of N), and four doses of SSW and DPW (100, 200, 300 and 400% of the recommendation) in a CRD with 3 replications. The samples of percolated were collected and characterized weekly. The treatments of highest dosage have...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water reuse; Wastewater; Leaching; Soil disposal; Agroindustry wastewaters.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601222

PATH ERRORS IN SUGARCANE TRANSSHIPMENT TRAILERS
Provedor de dados: 70
Autores: Passalaqua,Bruna P.; Molin,José P.
ABSTRACT The need for accuracy in sugarcane machine traffic has boosted the adoption of automatic steering systems. These have been used in tractors pulling transhipment trailers. Such sets are long and articulated, which hinders their performance and benefits due to alignments in curved and laterally sloped paths. In this sense, this study aimed to quantify shifts in direction to which tractors and transshipment trailers are subjected while traveling straight and curved paths on different terrain slopes. We evaluated an internal transport system composed of one tractor and two three-axle transshipment trailers, equipped with GNSS receivers and RTK correction system, for their respective positioning. Pass-to-pass errors were evaluated by differences in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lateral slope; Automatic steering; Traffic control.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200223

SOIL PHYSICAL ATTRIBUTES AND PRODUCTION COMPONENTS OF SUGARCANE CULTIVARS IN CONSERVATIONIST TILLAGE SYSTEMS
Provedor de dados: 70
Autores: Arcoverde,Sálvio N. S.; Souza,Cristiano M. A. de; Cortez,Jorge W.; Maciak,Paulo A. G.; Suárez,Andrés H. T.
ABSTRACT Machine traffic and conventional tillage can cause structural degradation of the soil, affecting the physical attributes and, consequently, the production and longevity of the sugarcane field. The objective of this study was to evaluate the production components of sugarcane cultivars (RB965902, RB985476, RB966928, RB855156, RB975201, RB975242, RB036066 and RB855536) and physical attributes of a Dystroferric Red Latosol (Oxisol) under no-tillage and reduced-tillage systems. The experiment was conducted using a completely randomized experimental design in an 8 × 2 factorial arrangement, with four replicates. The soil attributes evaluated were density, total porosity, macroporosity, microporosity and penetration resistance. The production components...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum spp.; Plant cane; Soil management; Reduced-tillage; No-tillage.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200216

Physical properties of Brazil nuts
Provedor de dados: 70
Autores: Nogueira,Roberta M.; Álvares,Virgínia de S.; Ruffato,Solenir; Lopes,Roberto P.; Silva,Juarez de S. E.
The Brazil-nut, also known as Para-nut, is widely used as food and in cosmetic industries. The seeds are rich in lipids and protein, and also present a considerable amount of selenium. Limited research has been conducted on postharvest of the Brazil nut, being an important information to design equipment related to aeration, drying, storage and transportation steps. Thus, the objective of this study was to determine the physical properties of the Brazil-nut with and without tegument. The dimensions found for the almonds with tegument were 39.35 mm in the X axis, 24.19 mm in the Y axis, and 17.88 mm in the Z axis. However for the almond without tegument the values were 31.05 mm in X, 14.38 in Y and 15.91 mm in Z axis. The sphericity was 66.40% and 51.59%...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brazil nut; Physical properties; Postharvest.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500015

Avaliação hidráulica de um sistema de irrigação localizada de baixa pressão, projetado pelo software "bubbler"
Provedor de dados: 70
Autores: Souza,Ivam H. de; Andrade,Eunice M. de; Silva,Elio L. da.
Conduziu-se este trabalho com o objetivo de avaliar o desempenho de um sistema de irrigação a baixa pressão, bubbler, em condições de campo. A avaliação consistiu de um estudo dividido em duas fases, em que, na primeira, foi elaborado o dimensionamento hidráulico do sistema de irrigação, com uso do programa computacional Bubbler versão 1.1, enquanto, na segunda fase, ocorreram a instalação e os testes de campo. Estabeleceram-se as alturas de 0,77; 0,71; 0,68 e 0,67 m na saída das mangueiras emissoras no campo, conforme recomendação do programa. Foram feitas as avaliações de vazão em cada mangueira emissora, para determinar o Coeficiente de Uniformidade de Christiansen (CUC), a Uniformidade de Distribuição (UD) e a Eficiência de Aplicação (EA). Os testes...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação bubbler; Dimensionamento; Uniformidade.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100029

Influência da velocidade de deslocamento na semeadura do milho
Provedor de dados: 70
Autores: Garcia,Luiz C.; Jasper,Roberto; Jasper,Mônica; Fornari,Allison J.; Blum,Julius.
Teve-se o objetivo de verificar a influência da velocidade de deslocamento na semeadura de milho, variando de 3,0 a 9,0 km h-1, em quatro condições. As variáveis analisadas foram: população de plantas emergidas, distribuição longitudinal, população com espigas e os componentes de rendimento. Concluiu-se que há aumento na percentagem de espaçamentos falhos e múltiplos e queda de espaçamentos aceitáveis ao se elevar a velocidade de semeadura. A produtividade só foi afetada quando a população de plantas com espigas foi reduzida pelo incremento de velocidade.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pneumático; Disco perfurado horizontal; Plantio direto.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200021

STRUCTURAL PROPERTIES OF SOIL IN MAIZE AND FORAGE GRASS INTERCROPPING UNDER NO-TILLAGE IN THE BRAZILIAN CERRADO
Provedor de dados: 70
Autores: Cagna,Camila P.; Calábria,Zieglenristen K. P.; Guedes Filho,Osvaldo; Pacheco,Leandro P.; Silva,Tonny J. A. da.
ABSTRACT Integration of forage grasses with grain crops, such as maize, allows maintaining soil cover. The objective of this study was to evaluate the tensile strength, friability, and stability of soil aggregates in the maize and forage grass intercropping under no-tillage system. The study used a completely randomized block design with seven treatments and three replications. Undisturbed soil samples were collected in two seasons (2015 and 2016) at 0–0.10 m and 0.10–0.20 m soil depth. The following properties of soil aggregates were measured: tensile strength (TS), friability (F), gravimetric moisture (GM), weighted mean diameter (WMD), geometric mean diameter (GMD), and aggregate stability index (ASI). The intercropping of maize with Urochloa...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aggregate stability index; Tensile strength; Soil physical quality.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400512

Monotonic trend and change points in southern Brazil precipitation
Provedor de dados: 70
Autores: Damé,Rita de C. F.; Teixeira,Claudia F. A.; Bacelar,Luiz C. S.; Winkler,Antoniony S.; Santos,Jacira P. dos.
Scientific evidence on climate changes at global level has gained increasing interest in the scientific community in general. The impacts of climate change as well as anthropogenic actions may cause errors in hydro-agricultural projects existent in the watershed under study. This study aimed to identify the presence or absence of trend in total annual precipitation series of the watershed of the Mirim Lagoon, state of Rio Grande do Sul-RS / Brazil / Uruguay (Brazilian side) as well as to detect the period in which they occurred. For that, it was analyzed the precipitation data belonging to 14 weather stations. To detect the existence of monotonic trend and change points, it was used the nonparametric tests of Mann-Kendall and Mann-Whitney, the "t" test of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Parametric and nonparametric test; Climate change; Trends change.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200005

GAS EXCHANGE IN ‘POME’ BANANA PLANTS GROWN UNDER DIFFERENT IRRIGATION SYSTEMS
Provedor de dados: 70
Autores: Arantes,Alessandro de M.; Donato,Sérgio L. R.; Siqueira,Dalmo L. de; Coelho,Eugênio F.
Abstract This study aimed to evaluate Pome type bananas grown under different irrigation systems. Seventy-two treatments were used in a factorial 3×2×12 scheme, where factors consisted of three irrigation systems (under-tree sprinkling, micro-sprinkling, and dripping), two cultivars (‘Prata-Anã‘ and ‘BRS Platina’), and twelve evaluation periods (months). The treatments were arranged in a completely randomized design with five repetitions. During the third production cycle, plant phytotechnical and physiological traits were evaluated in different months at five different times of the day. The results showed no significant interactions between cultivars and irrigation systems. All the assessed traits varied for each irrigation system, except for plant yield....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Musa spp; AAB and AAAB genotypes; Physiology.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200197

DAIRY PRODUCTION OF ‘SAANEN’ GOATS BASED ON METEOROLOGICAL VARIABLES AND FUTURE CLIMATE SCENARIOS
Provedor de dados: 70
Autores: Pequeno,Izaac D.; Turco,Silvia H. N.; Silva,Thieres G. F. da; Facó,Olivardo.
ABSTRACT This study aimed to modeling and bioclimatic zoning of ‘Saanen’ goat milk production in northeastern Brazil. Data were obtained from a 14-year dairy control program for 246 ‘Saanen’ goat matrices. Dairy production meteorological influence and mathematical modeling were assessed through statistical analyses such as Pearson’s correlation matrix and path analysis. Bioclimatic zoning for current and future scenarios, with climate changes, were delineated using inverse-square distance (ISD) and spherical model (kriging) interpolations. Results showed maximum air temperature to contribute substantially to goat dairy production; therefore, its modeling was based thereon. Current and future dairy production maps highlighted Maranhão and Piauí as regions...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Path analysis; Welfare; Stress; Climate change.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200226

Energetic efficiency of a deep bed swine production system
Provedor de dados: 70
Autores: Veloso,Alessandro V.; Campos,Alessandro T.; Paula,Vanderson R. de; Dourado,David C.; Yanagi Júnior,Tadayuki; Silva,Enilson B.
The aim of this work was to evaluate the energy flows of a commercial production system of swine deep bed in its finishing phase, located in Juiz de Fora, in the State of Minas Gerais, Brazil. Thus, an energy efficiency study was carried out by monitoring a lot of animals, during a 94-day period. The energy rate of each compound involved in the production process was quantified and the matrixes of energy consumption were determined in the form of animal feeding, electrical energy, piglets, material used as deep bed, human labor, equipment, swine buildings, production of alive swine for slaughter, organic fertilizer production (swine deep bed or swine deep litter). From the direct input energy, 80.57% correspond to animal feeding, 11.90% to pigs for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy input and output; Swine buildings; Alternative management; Sustainability of biosystems.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600008

Tabular cusum control charts of chemical variables applied to the control of surface water quality
Provedor de dados: 70
Autores: Follador,Franciele A. C.; Boas,Márcio A. Vilas; Schoenhals,Marlise; Hermes,Eliane; Rech,Clovis.
The aim of this study was to evaluate the application possibility of tabular CUSUM control charts in the quality control of chemical variables in surface water. It was performed bibliographic and field research to collect water samples from 2003 to 2009, totaling 30 samples, some monthly and others semi-annual in order to observe the variables that regulate water quality. It was found that these charts may be applied to control the quality of river water; showing to be effective in the perception of changes during the process, especially for small samples (n=1) which there is no repetition as in this research. It was also concluded that the Mandurim River does not presents significant levels of pollution.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environmental planning; Control charts; Water quality.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500014

CLASSIFICATION OF RICE GRAINS OF LOWLAND CULTIVARS GROWN UNDER FLOOD IRRIGATION AND SPRINKLER IRRIGATION
Provedor de dados: 70
Autores: Meus,Lorenzo D.; Muttoni,Martina; Bartz,Alex C.; Kaminski,Tiago A.; Alberto,Cleber M.
ABSTRACT The objective of this study is to analyze the classification of rice grains of lowland cultivars grown under flood and sprinkler irrigation. The study was carried out in the agricultural years 2011/2012 and 2014/2015 using a completely randomized block design with split plots. In 2011/2012, the treatments were three lowland rice cultivars grown under flood irrigation system and five sprinkler irrigation depths with four replications. In 2014/2015, the experimental design was maintained but flood irrigation was not performed. After harvest, the samples were processed in a rice testing machine, including peeling, polishing and classification. Whole and broken grains were weighed to calculate hulling and milling yield. The classifications followed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Oryza sativa; Water availability; Grain quality; Productivity.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400599

Evapotranspiração da cultura da melancia irrigada com água de diferentes salinidades
Provedor de dados: 70
Autores: Figueirêdo,Vladimir B.; Medeiros,José F. de; Zocoler,João L.; Espinola Sobrinho,José.
Sabe-se que a determinação precisa da evapotranspiração da cultura (ETc) é de grande importância para o uso eficiente da água, principalmente em regiões áridas e semiáridas onde se faz necessária a utilização de água salina para irrigação. O objetivo deste trabalho foi determinar a evapotranspiração da melancia, cultivar Mickylee, com o uso de diferentes níveis de salinidade da água de irrigação. O experimento foi conduzido na Fazenda Experimental da Alagoinha, pertencente à Universidade Federal Rural do Semiárido, Mossoró - RN. Os níveis de salinidade da água de irrigação foram: S1 = 0,55; S2 = 1,65; S3 = 2,35; S4 = 3,5, e S5 = 4,5 dS m-1, sendo os tratamentos dispostos no delineamento de blocos ao acaso, com quatro repetições. A determinação da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrullus lanatus; Água salina; Coeficiente de cultivo.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200006

Ajuste do método de Priestley-Taylor às condições climáticas locais
Provedor de dados: 70
Autores: Villa Nova,Nilson A.; Pereira,André B.
A sustentabilidade da agricultura irrigada depende primariamente do manejo eficiente da irrigação, de modo a aumentar a produtividade primária de uma cultura em determinada localidade. A eficiência no uso de água pode ser melhorada pelo próprio esquema de irrigação adotado, sendo essencialmente governado pelas condições climáticas. O planejamento da irrigação e a tomada de decisão são funções do conhecimento da demanda evaporativa da atmosfera, sendo expressa pela demanda potencial (ETo). Em geral, quase todos os métodos de estimativa de ETo reportados na literatura referem-se a valores diários, incluindo-se nessa situação as perdas noturnas de evaporação, as quais serão expressivas apenas em alguns dias após a chuva ou irrigação. Desenvolveu-se, no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Balanço de energia; Modelagem; Demanda atmosférica.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200007

USE OF INOCULUM IN BIODIGESTERS WITH CATTLE MANURE UNDER CONVENTIONAL AND ORGANIC PRODUCTION SYSTEMS
Provedor de dados: 70
Autores: Paes,Juliana L.; Alves,Thaís B. S.; Silva,Leonardo D. B. da; Marques,Anieli de S.; Dias,Valentina R. S.
ABSTRACT One way of making livestock farming a more sustainable practice is to raise cattle organically. However, regardless of the production system, there is a generation of residues that can be converted into energy resources using biodigesters. This study aimed to evaluate the addition of inoculum in the anaerobic biodigestion of cattle manure under organic (OPS) and conventional production systems (CPS) in an Indian model biodigester. The physicochemical (pH, EC, TS, VS, DBO, and COD) and microbiological characteristics of the affluent and effluent, as well as the production, potential, and qualitative characteristics of the biogas, were evaluated. CPS showed higher reductions in TS, VS, BOD, and COD than OPS, with the highest effect of biogas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anaerobic biodigestion; Biogas; Starting point; Biofertilizer potential.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200146

Drip pulses and soil mulching effect on american crisphead lettuce yield
Provedor de dados: 70
Autores: Almeida,Willian F. de; Lima,Luiz A.; Pereira,Geraldo M.
ABSTRACT An experiment was conducted in a greenhouse at the Federal University of Lavras cultivated with American lettuce, cv. Raider-Plus. The aim of this study was to evaluate the effects of irrigation water depths applied by drip pulses and of soil coverage on crop yields and efficiency of water use. The experimental design used was randomized blocks with eight treatments and three replications, totaling twenty-four plots. The treatments consisted of soil with and without coverage (double-sided white and black plastic) associated with four irrigation management levels. Irrigation management consisted in reposition of irrigation depths based on crop evapotranspiration (ETc) with D1-100% of ETc, applied continuously (control), and D2 - 100% of ETc, D3 -...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water-use efficiency; Greenhouse; Water depth.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601009

Decomposição de culturas de cobertura no sistema plantio direto, manejadas mecânica e quimicamente
Provedor de dados: 70
Autores: Reis,Gustavo N. dos; Furlani,Carlos E. A.; Silva,Rouverson P. da; Gerlach,Juliano R.; Cortez,Jorge W.; Grotta,Danilo C. C.
O sistema plantio direto preconiza o uso de culturas de cobertura para produção de massa seca sobre o solo. O presente trabalho teve por objetivo estudar a produção e a taxa de decomposição de duas coberturas vegetais - crotalária juncea (Crotalária juncea L.) e mucuna-cinza (Stilozobium niveum L) - em três sistemas de manejo (rolo-faca, triturador de palhas e herbicida), e a capacidade de campo efetiva dos manejos. O experimento foi realizado na área do Laboratório de Máquinas e Mecanização Agrícola (LAMMA), do Departamento de Engenharia Rural, UNESP, Jaboticabal - SP, com delineamento em blocos ao acaso, em esquema fatorial 3x2, originando seis tratamentos, com quatro repetições. Foram analisadas as produções de massa seca das culturas de cobertura antes...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mucuna-cinza; Crotalária juncea; Capacidade de campo efetiva.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100013

Desenvolvimento de um dispositivo para medição de esforços em hastes de semeadoras de plantio direto
Provedor de dados: 70
Autores: Santo,Amauri C. E; Reis,Ângelo V. dos; Machado,Antônio L. T; Batista,Vilson J; Oldoni,André.
Inúmeros problemas relativos à mecanização dizem respeito aos esforços demandados pelas máquinas e implementos agrícolas. A medição dos esforços em implementos de hastes é geralmente feita por instrumentos complexos e de difícil construção, como os anéis octogonais. Sendo assim, o objetivo deste artigo é apresentar o desenvolvimento de um dispositivo de medição de esforços horizontais e verticais em hastes sulcadoras de semeadoras-adubadoras de plantio direto, utilizando transdutores de força extensiométricos do tipo viga em balanço, comercialmente disponíveis. Para tanto, projetou-se um dispositivo tipo pórtico, composto de dois transdutores para medição de esforços horizontais e um transdutor para medição do esforço vertical. Os três transdutores foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Transdutor de força; Ensaio de semeadoras; Dinamômetro.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200011

Produtividade do brócolis-de-cabeça sob diferentes sistemas de irrigação
Provedor de dados: 70
Autores: Geisenhoff,Luciano O.; Oliveira,Fabricio C. de; Biscaro,Guilherme A.; Almeida,Alexsandro C. dos S.; Schwerz,Francielli.
RESUMO Na agricultura sustentável, busca-se o sistema de irrigação que proporcione alta produtividade comercial com o mínimo de água aplicada. Assim, objetivou-se pelo presente estudo avaliar a produtividade do brócolis-de-cabeça irrigado por diferentes sistemas de irrigação. O delineamento experimental foi em blocos ao acaso, utilizando quatro repetições e cinco tratamentos que correspondem aos sistemas de irrigação: gotejamento superficial, gotejamento subsuperficial, microaspersão, Santeno® e aspersão convencional. A cultivar utilizada foi o brócolis-de-cabeça (Brassica oleracea var.italica, híbrido Lord Summer). Foram avaliados o diâmetro de inflorescência (DI), a produtividade comercial de inflorescência (PCI) e a produtividade da água (PA). O...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brassica oleracea; Produtividade da água e uniformidade de distribuição.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500863

DETERMINATION OF SOIL VOLUME BY PLANIALTIMETRIC SURVEY METHODS
Provedor de dados: 70
Autores: Vanzela,Luiz S.; Araujo Junior,Osvaldo; Lima,Ronaldo C.
ABSTRACT Considering the importance of topographic surveys to determine soil volumes and study efficient and accessible alternatives for this operation, this study aimed to analyze methods and respective equipment for planialtimetric surveys to determine soil volume. An experimental grid was installed in an area locate in Fernandópolis, SP, Brazil, in which quotas were measured by geometric leveling (standard method), trigonometric leveling, leveling with receivers of the Global Navigation Satellite System (GNSS) by relative (frequencies L1/L2) and absolute positioning (code C/A) and extraction of altitudes in digital terrain model from SRTM and ASTER images. In comparison to geometric leveling, trigonometric leveling was the most accurate in determining...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: GNSS; Geometric leveling; Trigonometric leveling; Geomatics.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200207

Demanda de potência do ventilador para aeração de material em compostagem
Provedor de dados: 70
Autores: Matos,Antonio T. de; Teixeira,Denis L.; Ribeiro,Ivan C.; Paiva,Ed Carlo R.; Lacerda Filho,Adílio F.
Neste trabalho, objetivou-se ajustar curvas de perda na pressão estática do ar, quando forçado em camadas de material orgânico, com diferentes espessuras, e dois estádios de degradação bioquímica, para possibilitar o cálculo da demanda de potência do sistema de ventilação. Os resíduos utilizados para a medição da perda de pressão do ar foram cama de frango misturada com casca dos frutos do cafeeiro, razão entre massas de 2,5:1, de forma a se obter relação C/N inicial de 30:1. Foi verificado que a perda na pressão estática do ar aumentou linearmente com a espessura da camada de composto orgânico e que houve aumento na perda de pressão estática com o aumento na vazão específica do ar, o que praticamente não foi alterado pelo estádio de degradação bioquímica...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resíduos sólidos; Leiras estáticas aeradas; Processos aeróbios.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300013

Errata: volume 30, número 2
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/article
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600021

Desenvolvimento e calibração de um tensiômetro eletrônico de leitura automática
Provedor de dados: 70
Autores: Teixeira,Adunias S.; Coelho,Silvana L.
O presente trabalho apresenta o desenvolvimento e calibração de tensiômetro de leitura automática, sendo o tensiômetro de mercúrio utilizado como padrão de comparação. Os ensaios foram conduzidos no Laboratório de Mecânica e Eletrônica do Departamento de Engenharia Agrícola da UFC. Esse equipamento difere do tensiômetro tradicional por substituir o manômetro de mercúrio por sensor de pressão. Tal dispositivo gera uma saída com valor de até no máximo 4,5 volts. O tensiômetro eletrônico é conectado a uma placa de aquisição de dados (DAQ) contendo um microprocessador, conversor analógico/digital (ADC) e saída serial, sendo tal placa ligada a um microcomputador. A bancada de ensaio constituiu-se de três caixas plásticas preenchidas com solo de textura franco-...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensor de pressão; Automação; Potencial matricial.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200010

Avaliação de parâmetros hidráulicos e manejo da irrigação por microaspersão em área de assentamento
Provedor de dados: 70
Autores: Santiago,Fábio S.; Montenegro,Abelardo A. A.; Montenegro,Suzana M. G. L.
Este trabalho foi desenvolvido em solo aluvial do semi-árido de Pernambuco, suscetível à salinização, visando a orientar agricultores de assentamento para instalar, avaliar e manejar racionalmente sistemas de irrigação por microaspersão, para atender ao plantio da cultivar de repolho Midori. Adotando-se percentagem de área molhada igual a 100%, foram avaliados nos setores da unidade operacional a variação de vazão e pressão, os coeficientes de uniformidade (CU) e a eficiência de aplicação (EA). A uniformidade da irrigação apresentou valores elevados, superiores a 93%. A eficiência de aplicação foi boa, com valores maiores que 80%. O sistema foi então utilizado na irrigação, utilizando como controle o tanque "Classe A", durante um período de 75 dias, e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aluviões; Microaspersão; Manejo de salinidade.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300015

Economic optimization method to design telescope irrigation of multiples outlets
Provedor de dados: 70
Autores: Pinto,Marinaldo F.; Camargo,Antonio P. de; Coelho,Rubens D.
In this study is presented an economic optimization method to design telescope irrigation laterals (multidiameter) with regular spaced outlets. The proposed analytical hydraulic solution was validated by means of a pipeline composed of three different diameters. The minimum acquisition cost of the telescope pipeline was determined by an ideal arrangement of lengths and respective diameters for each one of the three segments. The mathematical optimization method based on the Lagrange multipliers provides a strategy for finding the maximum or minimum of a function subject to certain constraints. In this case, the objective function describes the acquisition cost of pipes, and the constraints are determined from hydraulic parameters as length of irrigation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Conduits in series; Minimum cost; Lagrange multipliers.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400017

Evapotranspiração máxima do capim "Tanzânia" (Panicum maximum J.) em pastejo rotacionado, baseada na evaporação do tanque "Classe A " e no índice de área foliar
Provedor de dados: 70
Autores: Delgado-Rojas,Juan S.; Novaes,Marcelo; Lourenço,Leandro F.; Coelho,Rubens D.
Em função do índice de área foliar (IAF) do Capim Tanzânia (Panicum maximum J.) e da lâmina de evaporação do tanque "Classe A" (ECA), foi gerado um modelo multiplicativo para determinar a evapotranspiração máxima (ETm) desse cultivo forrageiro. Foi adotada uma correlação entre a ETm em função da evaporação do tanque "Classe A" e do índice de área foliar (IAF), por meio de uma regressão linear múltipla dos valores logarítmicos, correspondentes a períodos diários durante 11 meses (janeiro a novembro de 2000). Considerando a dificuldade para determinar o IAF e aplicar como variável no modelo proposto, foi desenvolvido outro modelo por meio da correlação entre a ETm e as variáveis ECA e o valor equivalente de IAF, em dias de descanso (NDd), adotando-se como...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Balanço hídrico; Irrigação; Pasto.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100026

Programa computacional para o dimensionamento de colhedoras considerando a pontualidade na colheita de soja
Provedor de dados: 70
Autores: Borges,Iackson O.; Maciel,Antonio J. S.; Milan,Marcos.
A colheita de soja (Glycine max (L.) Merril) é uma operação crítica que pode sofrer atrasos resultando em perdas na quantidade e na qualidade do material colhido. Embora o valor das perdas seja desconhecido no País, os produtores empregam colhedoras com reserva de capacidade para concluir a operação no menor prazo possível. O excesso de capacidade aumenta os custos fixos e a falta dela aumenta os custos das perdas por atraso e, em ambos os casos, reduzem a renda líquida da operação, ao que se denomina custo de pontualidade. O problema do dimensionamento consiste em ajustar o custo do capital extra investido na capacidade da máquina para garantir a pontualidade e o custo das perdas por atraso, buscando maximizar a renda líquida. Devido à importância da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Máquinas agrícolas; Perdas na colheita; Simulação/computadores.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100015

Wet bulbs from the subsurface drip irrigation with water supply and treated sewage effluent
Provedor de dados: 70
Autores: ELAIUY,MARCELO L. C.; SANTOS,LEONARDO N. S. DOS; SOUSA,ALLAN C. M. DE; SOUZA,CLAUDINEI F.; MATSURA​,EDSON E.
The use of treated sewage effluent (TSE) combined with the subsurface drip irrigation (SDI) method in agriculture can decrease the costs of agricultural production, in attempts to fertigate crops more efficiently. In this study it was compared the dimensions of the wet bulb formed by the application of TSE and municipal water supply (MWS) in an Oxisoil. We have evaluated the effect of water quality and discharge between drippers used in sugarcane crop. Three trenches were opened and 21 three-rod TDR probes were setup in a mesh and a dripper was buried at 0.30 m, for each constant discharge of 1.0 L h-1and 1.6 L h-1. Comparing results from different wetted soil profiles it was observed that the vertical and horizontal dimensions of the wet bulb are similar...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Oxisoil; Wastewater; TDR; Water content; Electrical conductivity.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200242

Selection of microorganisms producer of lipase for fat removal from biodiesel purification water
Provedor de dados: 70
Autores: Rocha,Dayane C. da; Gomes,Benedito M.; D.Gomes,Simone; Sene,Luciane; Zenatti,Dilcemara C.
The objective this study has been the selection of lipase productor microorganism, for removal of oils and grease, in the pre-treatment of biodiesel wastewater washing. For this, analyses of the physicist-chemistries characteristics had been made with the wastewater of the biodiesel washing, and then it had been isolated and chosen, by means of determinations of the lipase activity. Following, it was made a test of fat biodegradation, in the conditions: pH (5.95), temperature (35 ºC), rotation (180 rpm) and ammonium sulfate as nitrogen source (3 g L-1) and establishing as variable the two microorganism preselected and the time (24; 48; 72; 96 and 120 h). The biodiesel purification wastewater had presented high potential of environmental impact, presenting...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Enzymatic degradation; Fatty effluent; Lipolytical activity.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200012

Índice de previsão de produção de leite para vacas Jersey
Provedor de dados: 70
Autores: Laloni,Luiz A.; Nääs,Irenilza A.; Macari,Marcos; Pereira,Danilo F.; Pinheiro,Maria Das G.
No Brasil, o uso de vários modelos de criação intensiva e semi-extensiva desfavorece a adoção generalizada de métodos de manejo do gado bovino, principalmente do gado leiteiro. Mesmo assim, a produção leiteira pode ser melhorada a partir do uso de tecnologias que possam garantir o manejo adequado do rebanho. O objetivo deste trabalho foi desenvolver um índice de previsão de produção de leite para vacas Jersey em lactação, de genética de alta produtividade, em regime semi-estabulado, nas condições tropicais. Para a obtenção do índice, consideraram-se a temperatura e a umidade relativa do ambiente e a velocidade do ar, assim como valores de precipitação pluviométrica, temperatura do solo do pasto e a radiação solar como agentes estressores, os quais podem...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bovinocultura de leite; Ambiência animal; Índice de produção.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200002

Lixiviação de íons em colunas de solo deformado e indeformado
Provedor de dados: 70
Autores: Sampaio,Silvio C.; Caovilla,Francielle A.; Opazo,Miguel A. U.; Nóbrega,Lúcia H. P.; Suszek,Morgana; Smanhotto,Adriana.
Neste trabalho, foi avaliada a dinâmica da lixiviação de íons em colunas de solo deformado e indeformado. O solo utilizado era proveniente de área fertirrigada com água residuária da suinocultura diluída em 0%, 25%, 50%, 75% e cultivada com soja. Foram construídas curvas de eluição para nitrato, potássio e condutividade elétrica. De acordo com os resultados obtidos nas colunas de solo deformado, e proporcionalmente aos tratamentos, o nitrato apresentou maior mobilidade, seguido pela concentração de sais totais e do potássio. A metodologia de colunas de solo indeformado não se mostrou adequada, devido, possivelmente, à compactação do solo durante a amostragem e à dificuldade no bloqueio de caminhos preferenciais ao longo de toda a coluna.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água residuária; Meio ambiente; Dinâmica de íons.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100016

ANAEROBIC DIGESTION AND CO-DIGESTION OF POULTRY LITTER SUBMITTED TO DIFFERENT REUSES
Provedor de dados: 70
Autores: Vicente Jr.,Donizete J.; Costa,Monica S. S. de M.; Costa,Luiz A. M.; Pereira,Dercio C.; Santos,Francielly T. dos.
ABSTRACT Considering the constant increase in the waste generation from poultry and pigs’ husbandries, the main contributions of this study were to verify the potential of biogas production through the anaerobic digestion and co-digestion of the residues generated by these two activities, as well as to highlight the recovery of the nutrients contained in the obtained digestate. The wastes used were poultry litters after six, seven and eight production lots, as well as the sifted wastewater from one Piglets Producer Unit (PPU). Higher biogas production (p &lt;0.05) was observed in the treatments in which anaerobic codigestion was used with the swine wastewater (SW): 0.179; 0.158 and 0.117 m3 per kg of total solids (TS) added for poultry litters with six,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agroindustry; Digestate; Biogas; Waste treatments.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600961

TREATMENT OF SEPTIC TANK SLUDGE IN A VERTICAL FLOW CONSTRUCTED WETLAND SYSTEM
Provedor de dados: 70
Autores: Andrade,Cynthia F.; Sperling,Marcos Von; Manjate,Elias S.
ABSTRACT: The study consisted of the evaluation of the treatment of septic tank sludge in a vertical constructed wetland system (CW), built according to the first stage of the French system. The system operated also for sewage treatment and one of the beds (area of 29.1 m2, height of the support medium of 0.7 m and planted with Tifton 85 grass, Cynodon dactylon Pers), began to receive the application of sludge from clean-pit trucks once a week. The percolated liquid was directed to post-treatment in the other two beds of the French system. The application of the raw sludge had average hydraulic loading rate of 13.1 m3/m2.year and solids loading rate of 81 kgTS/m2.year. The system improved the quality of percolated liquid in terms of carbonaceous and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Constructed wetlands; Septic tank; Post-treatment; Sludge.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400811

EFFECT OF AERATION AND RECIRCULATION IN THE REMOVAL OF NITROGEN AND CHEMICAL OXYGEN DEMAND FROM SANITARY SEWAGE IN A STRUCTURED BED REACTOR
Provedor de dados: 70
Autores: Leick,Sheilla A.; Oliveira,João G B. De; Tavares,Karoline A.; Lopes,Deize D.; Barana,Ana C.
ABSTRACT This study aimed to evaluate a structured bed reactor with intermittent aeration in the simultaneous removal of Chemical Oxygen Demand (COD) and Total Nitrogen (TN) from sanitary sewage. The reactor was operated for 339 days with a Hydraulic Retention Time (HRT) of 12 hours, temperature of 30 ± 1°C and continuous feeding. Nine trials were carried out in which three different effluent recirculation flow (Qr), 3, 2 and 1 time the incoming flow, were evaluated in three different aeration times, of 1h, 2h, and 3h, in 3 hour cycles. The results showed that different recirculation flows and aeration times did not influence the removal of COD, which reached 89%±12. It was observed that the efficiency of TN removal was higher in the tests with higher...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bioreactor; Wastewater; Denitrification; Nitrification; SND (Simultaneous Nitrification and Denitrification).
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601236

PHYSICAL AND MECHANICAL PROPERTIES OF THE BAMBUSA VULGARIS AS CONSTRUCTION MATERIAL
Provedor de dados: 70
Autores: Gomes Neto,José A.; Barbosa,Normando P.; Beraldo,Antônio L.; Melo,Aluísio B. de.
ABSTRACT The fabrication of traditional construction materials consumes a large amount of energy, emits pollutants, and utilizes nonrenewable raw materials. Therefore, it is important to reduce the environmental impact of construction through the use of eco-friendly materials, such as bamboo. This work presents the characterization of Bambusa vulgaris, which is widely available in Brazil. The aim is to employ this raw material as a construction material. The geometric and physical properties were obtained. The results showed that, when bamboo is soaked in water, dimensional variations up to 7% were observed along the radial direction. The mechanical properties depend on the moisture content. The compressive strength can exceed 60 MPa with approximately 7%...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bamboo; Mechanical properties; Physical properties; Sustainable construction.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200119

Variação da temperatura e do teor de água do café em secador rotativo usando lenha e GLP como combustíveis
Provedor de dados: 70
Autores: Reinato,Carlos H. R.; Borém,Flávio M.
O presente estudo foi realizado no Pólo de Tecnologia em Pós-Colheita de Café, na Universidade Federal de Lavras - MG. Seu objetivo foi estudar a distribuição da temperatura e do teor de água na direção radial do secador rotativo. Para a realização do teste, foram usados, concomitantemente, dois secadores da marca Pinhalense, com capacidade de 5.000 kg cada; em um secador usou-se lenha e no outro GLP, como combustíveis para o aquecimento do ar. A medição da temperatura do ar de secagem e da massa de café foi feita por meio de termopares distribuídos em 18 pontos no secador. As leituras de todas as temperaturas, registradas em um indicador, foram feitas em intervalos de meia hora. A redução do teor de água foi acompanhada em nove pontos na massa de café....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gradiente; Secagem; Coffea arabica L.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200026

Climate trends in the municipality of Pelotas, state of Rio Grande do Sul, Brazil
Provedor de dados: 70
Autores: Kruel,Izabele B.; Meschiatti,Monica C.; Blain,Gabriel C.; Ávila,Ana M. H. de.
ABSTRACT Changes in the frequency of occurrence of extreme weather events have been pointed out as a likely impact of global warming. In this context, this study aimed to detect climate change in series of extreme minimum and maximum air temperature of Pelotas, State of Rio Grande do Sul, (1896 - 2011) and its influence on the probability of occurrence of these variables. We used the general extreme value distribution (GEV) in its stationary and non-stationary forms. In the latter case, GEV parameters are variable over time. On the basis of goodness-of-fit tests and of the maximum likelihood method, the GEV model in which the location parameter increases over time presents the best fit of the daily minimum air temperature series. Such result describes a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: General extreme value distribution; Time dependent model; Extreme weather events.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400769

Control system for forced-air cooling of horticultural products
Provedor de dados: 70
Autores: Silva,João C. T. R. da; Mederos,Bárbara J. T.
This work is a study of the implementation of a classical controller using a tuning method referred to as IMC (Internal Model Control) and aimed at the reduction of electrical energy consumption by the appropriate relation between energy consumption and the cooling time with forced air. The supervisory system installed was able to manipulate the variable of frequency of the signal power of the exhaust fan engine (forced air module), to accelerate or decelerate the loss of heat from the product to be cooled by airflow variation that passes through the mass of the produce. The results demonstrated a reduction in energy consumption from 64% and an increase of only 8% in the cooling time to the system using PI/IMC (Proportional - Integral with IMC) tuning...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Instrumentation; Controller tuning; IMC method; Cooling time; Supervisory system.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400001

Comparação de equações de chuvas intensas para localidades do estado de São Paulo
Provedor de dados: 70
Autores: Fiorio,Peterson R.; Duarte,Sergio N.; Rodrigues,Guilherme de O.; Miranda,Jarbas H. de; Cooke,Richard A.
Dada a importância das equações de chuvas intensas para o dimensionamento de obras de controle de enxurradas, este trabalho teve como objetivo comparar as alturas precipitadas geradas pelas equações de Martinez &amp;amp; Magni (1999) com aquelas obtidas com o programa PLUVIO 2.1, considerando as primeiras como padrão. Foram comparadas chuvas intensas de 10; 20; 30; 60; 120 e 1.440 minutos, e períodos de retorno de 2; 5; 10; 50 e 100 anos, para 30 localidades do Estado de São Paulo. Os resultados revelaram que, principalmente para as chuvas de 24 horas e período de retorno de 100 anos, houve desvios importantes para 4 postos localizados na região central e a leste do Estado. Para as demais localidades o programa apresentou bom desempenho.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Relações intensidade-duração-frequência; Precipitações; Escoamento superficial.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600009

Biodigestão anaeróbia de dejetos de suínos com e sem separação da fração sólida em diferentes tempos de retenção hidráulica
Provedor de dados: 70
Autores: Orrico Júnior,Marco A. P.; Orrico,Ana C. A.; Lucas Júnior,Jorge de.
O objetivo deste trabalho foi avaliar o processo de biodigestão anaeróbia utilizando dejetos de suínos, com e sem separação da fração sólida, considerando-se diferentes tempos de retenção hidráulica. Para tanto, foram utilizados biodigestores tubulares semicontínuos abastecidos com água residuária de suinocultura, com e sem separação da fração sólida (CSFS e SSFS, respectivamente), manejados com tempos de retenção hidráulica (TRH) iguais a 36; 29; 22 e 15 dias. A eficiência dos tratamentos foi avaliada pela redução dos números mais prováveis de coliformes totais e fecais, teores de fibra em detergentes neutro e ácido, demandas química e bioquímica de oxigênio e dos potenciais de produção de biogás e metano. A qualidade do biofertilizante foi avaliada...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coliformes; Sólidos totais; TRH.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300014

Caracterização espectral de áreas de gramíneas forrageiras infectadas com a doença "mela-das-sementes da braquiária" por meio de imagens CCD/CBERS-2
Provedor de dados: 70
Autores: Rosatti,José C.; Silva,Erivaldo A. da; Silva,Hélio R.; Kruppa,Pedro C.
Imagens CCD/CBERS-2, nas bandas espectrais CCD2, CCD3 e CCD4, dos anos de 2004 e 2005, de Mirante do Paranapanema - SP, foram transformadas em reflectância de superfície usando o modelo 5S de correção atmosférica e normalizadas radiometricamente. O objetivo principal foi caracterizar espectralmente áreas de pastagens de Brachiaria brizantha em fase de florescimento, isentas e infectadas com a doença "mela-das-sementes da braquiária", possibilitando a sua detecção por meio da comparação entre os valores de reflectância de superfície denominada de Fator de Reflectância Bidirecional de Superfície (FRBS). Teve-se, também, o objetivo de avaliar a eficácia das imagens CCD/CBERS-2 para a obtenção de respostas espectrais de pastagens. Os dosséis sadios e doentes...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensoriamento remoto; Brachiaria brizantha; ACWSI.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300019

Crescimento inicial de duas cultivares de cafeeiro adensado influenciado por níveis de irrigação localizada
Provedor de dados: 70
Autores: Santana,Márcio S.; Oliveira,Carlos A. da S.; Quadros,Michael.
O experimento foi conduzido na Fazenda Água Limpa, Universidade de Brasília, tendo como objetivo avaliar o crescimento das cultivares de café IAPAR-59 e Obatã, submetidas a cinco níveis de irrigação por gotejamento durante o primeiro ano de formação e estudar formas de manejo da água do solo. O delineamento experimental usado foi o de blocos completos ao acaso para o fator irrigação em parcelas, com o fator cultivar em subparcela e o fator tempo em dias após o transplante (dat) em subsubparcela, com seis repetições. Os cinco níveis de irrigação foram tensões de 20; 40 e 60 kPa determinadas com o auxílio de tensiômetros, sistema Irrigas com tensão definida pelo próprio sensor e sem irrigação. As variáveis de crescimento avaliadas foram índice de área...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica; Manejo de água do solo; Sistema Irrigas.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300016

Spray adjuvant characteristics affecting agricultural spraying drift
Provedor de dados: 70
Autores: OLIVEIRA,RONE B. DE; ANTUNIASSI,ULISSES R.; GANDOLFO,MARCO A.
This study defined the main adjuvant characteristics that may influence or help to understand drift formation process in the agricultural spraying. It was evaluated 33 aqueous solutions from combinations of various adjuvants and concentrations. Then, drifting was quantified by means of wind tunnel; and variables such as percentage of droplets smaller than 50 μm (V50), 100 μm (V100), diameter of mean volume (DMV), droplet diameter composing 10% of the sprayed volume (DV0.1), viscosity, density and surface tension. Assays were performed in triplicate, using Teejet XR8003 flat fan nozzles at 200 kPa (medium size droplets). Spray solutions were stained with Brilliant Blue Dye at 0.6% (m/ v). DMV, V100, viscosity cause most influence on drift hazardous....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Droplet size; Wind tunnel; Experimental methods; Correlations; Multivariate analysis.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100109

PERFORMANCE AND WELFARE OF FINISHING PIGS SUBJECTED TO CLIMATECONTROLLED ENVIRONMENTS AND SUPPLEMENTARY LIGHTING
Provedor de dados: 70
Autores: Barnabé,Janice M. C.; Pandorfi,Héliton; Gomes,Nicoly F.; Ameida,Gledson L. P. de; Guiselini,Cristiane.
ABSTRACT An adequate thermal environment in pig farming facilities is essential to ensure productivity and animal welfare. The objective of this study was to evaluate the behavior and performance of finishing pigs, subjected to climate-controlled environments and supplementary lighting. Twenty-seven pigs (3/4 Duroc, 1/4 Pietrain) were kept in pens with no climate control, pens with forced ventilation and pens with adiabatic evaporative cooling system, associated with 12 h of natural light, 12 h of natural light + 4 h of artificial light and 12 h of natural light + 6 h of artificial light. The experimental design was completely randomized, in a 3x3 factorial arrangement and the means were compared by Tukey test (p&lt;0.05). Meteorological variables,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal ambience; Behavior; Thermal comfort; Weight gain.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300294

APPARENT DENSITY AS AN ESTIMATOR OF WOOD PROPERTIES OBTAINED IN TESTS WHERE FAILURE IS FRAGILE
Provedor de dados: 70
Autores: Christoforo,André L.; Couto,Natalia G.; Almeida,João P. B.; Aquino,Vinicius B. de M.; Lahr,Francisco A. R.
ABSTRACT The use of new wood species in construction requires knowledge of their properties for safer and more economical structural sizing. In Brazil, structural projects are carried out according to the standard document ABNT NBR 7190:1997. Tests required by this standard for the complete characterization of species require large machines with high costs, which are present only in large research centers. Considering the lack of experimental determination, this study aimed, with the help of analysis of variance of regression models, to investigate the possibility of estimating, through apparent density, wood properties obtained in tests where failure is considered fragile, allowing the estimation of properties of species still little used. Ten wood...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hardwoods; Fragile failure; Regression models; Analysis of variance.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100105

IMPLICATIONS FOR PEAK FLOWS OF THE MARRECAS RIVER BASIN DUE TO CHANGES IN THE BRAZILIAN FOREST CODE
Provedor de dados: 70
Autores: Aguiar,Wagner de; Sampaio,Silvio C.; Paisani,Julio C.; Reis,Ralpho R. dos.
ABSTRACT Changes in the Brazilian Forest Code (BFC) have soften the criteria for recovery and conservation of permanent preservation areas (PPAs), enhancing processes related to surface runoff. The aim of this study is to understand the effects of changes in PPA classification criteria established by BFC of 2012 to the detriment of BFC from 1965 considering the surface runoff response in the basin draining the upper Marrecas River valley in the flow peaks. The HEC–HMS model was used to simulate flow peaks considering three land-use scenarios, representative of the current use, adapting it to PPAs fitted to the BFC of 1965 and 2012 and seven precipitation return periods. In the proposed scenarios, the use of BFC of 2012, to the detriment of that from 1965,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Surface runoff; Forestry legislation; Hydrological simulation; Land use.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200277

Uniformidade de picado processado por colhedora de forragem
Provedor de dados: 70
Autores: Schlosser,José F; Dornelles,Marçal E; Pinheiro,Eder D; Durigon,Reges; Russini,Alexandre.
A ensilagem de plantas é prática comum no Brasil, onde se busca o armazenamento de alimentos com altos teores de energia, provenientes de plantas forrageiras para utilização em períodos de escassez. A obtenção de silagem de boa qualidade começa com a uniformidade de processamento das culturas pelas máquinas ensiladoras. Assim, este trabalho buscou avaliar a uniformidade de tamanho do picado de milho e sorgo forrageiro processado por colhedora de forragem, avaliando a metodologia para a determinação granulométrica das partículas e definindo a melhor regulagem para o uso da colhedora. Foram avaliadas duas regulagens da colhedora para tamanhos de corte entre 4 e 22 mm, sobre as culturas de milho e sorgo forrageiro. Foi determinado que a regulagem de corte...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Máquinas agrícolas; Ensilagem; Avaliação; Colhedora de forragem.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200012

Spatial distribution of canine Visceral Leishmaniasis in Ilha Solteira, São Paulo, Brazil
Provedor de dados: 70
Autores: Paulan,Silvana de C.; Silva,Hélio R.; Lima,Elizete A. C. de Freitas; Flores,Edílson F.; Tachibana,Vilma M.; Kanda,Cláudia Z.; Noronha Junior,Antonio C. F. de; Dobre,Paulo R.
Visceral Leishmaniasis (VL) is caused by protozoan of genus Leishmania and transmitted by sand flies of genus Lutzomyia, which has been adapted to the peridomicile environment where dogs are their mainly food source, increasing the risk for human cases. In this study, techniques of geoprocessing and spatial statistics were utilized as a contribution to understanding the epidemiological dynamics of VL in the urban area of Ilha Solteira, SP.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoprocessing; Sand fly; Epidemiology; Spatial statistics.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400016

EFFECT OF AUDITORY ENRICHMENT (MUSIC) IN PREGNANT SOWS WELFARE
Provedor de dados: 70
Autores: Silva,Flávia R. S.; Miranda,Késia O. da S.; Piedade,Sônia M. de S.; Salgado,Douglas D'Alessandro.
ABSTRACT Studies have shown that the benefits from music can improve the welfare conditions of laboratory, pet and production animals. The study aimed to evaluate the influence of music (Antonio Lucio Vivaldi compositions) on behavior aspects (position, activity, stereotypes, social and agonistic behavior) and physiological responses (respiratory rate and rectal temperature) in gestating sows in individual cages (stage 1), and collective stalls (stage 2). 28 animals were studied, 14 belonged to music group, and 14 to the control group (without music).The respiratory rate had the lowest averages in the group with music, for example, in stage 1, time 1, values of 19.28 and 21.50 mov.min−1. In stage 2, the values found in the same time were 20.36 and 24.16,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal behavior; Physiological parameters; Sound stimuli stereotypes.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200215

Reatores anaeróbios operados em batelada sequencial seguidos de lagoas de polimento para o tratamento de águas residuárias de suinocultura. Parte II: remoção de nutrientes e coliformes
Provedor de dados: 70
Autores: Duda,Rose M.; Oliveira,Roberto A. de.
Neste trabalho, avaliou-se o desempenho de dois reatores anaeróbios operados em batelada sequencial (ASBR), instalados em série, em escala-piloto (volumes de 280 L e 140 L, respectivamente), no tratamento de águas residuárias de suinocultura, com concentrações de sólidos suspensos totais (SST) em torno de 10.000 mg L-1. Para o pós-tratamento do efluente do sistema de tratamento com os ASBR, utilizou-se de duas lagoas de polimento (volume de 1.000 L, cada) em série. As cargas orgânicas volumétricas (COV) aplicadas no primeiro ASBR variaram de 4,43 a 12,75 g DQOtotal (L d)-1. As eficiências médias de remoção de nitrogênio total Kjeldahl (NTK) e fósforo total (P-total) variaram de 30 a 82% e de 42 a 100%, respectivamente, no sistema de tratamento anaeróbio...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carga orgânica volumétrica; Digestão anaeróbia; Dois estágios; Pós-tratamento; Remoção de metais.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100014

ESTIMATE OF REFERENCE EVAPOTRANSPIRATION THROUGH CONTINUOUS PROBABILITY MODELLING
Provedor de dados: 70
Autores: Uliana,Eduardo M.; Silva,Demetrius D. da; Silva,José G. F. da; Fraga,Micael de S.; Lisboa,Luana.
ABSTRACT This study aimed at testing the fit of continuous probability distributions to a daily reference evapotranspiration dataset (ET0) at a 75% probability level for designing of irrigation systems. Reference evapotranspiration was estimated by the Penman-Monteith method (FAO-56-PM) for eight locations, within the state of Espírito Santo (Brazil), where there are automatic gauge stations. The assessed probability distributions were beta, gamma, generalized extreme value (GEV), generalized logistic (GLO), generalized normal (GN), Gumbel (G), normal (N), Pearson type 3 (P3), Weibull (W), two- and three-parameter lognormal (LN2 and LN3). The fitting of the probability distributions to the ET0 daily dataset was checked by the Kolmogorov-Smirnov's test....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiration; Probability; Irrigation.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200257

Uso de imagens do sensor orbital modis na estimação de datas do ciclo de desenvolvimento da cultura da soja para o estado do Paraná – Brasil
Provedor de dados: 70
Autores: Johann,Jerry A.; Becker,Willyan R.; Uribe-Opazo,Miguel A.; Mercante,Erivelto.
RESUMO O Estado do Paraná caracteriza-se por uma grande variabilidade de épocas de semeadura (DS) e, consequentemente, pelo desenvolvimento máximo vegetativo (DMDV), colheita (DC) e ciclo (CI) para a cultura da soja. O objetivo deste trabalho foi estimar essas datas para o período de primavera-verão do ano-safra de 2011/2012, por meio de séries temporais de imagens do Índice de Vegetação Realçado (do inglês Enhanced Vegetation Index - EVI) do sensor Modis (Moderate Resolution Imaging Spectroradiometer). Gerou-se um perfil espectrotemporal médio de EVI, considerando todos os pixels mapeados como soja dentro de cada município. Estes dados serviram de entrada no software Timesat para estimar os decêndios do ciclo da cultura (DS, DMDV, DC e CI) por municípios....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ciclo fenológico; Índice de vegetação; EVI; Timesat.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100126

Fungicidas, doses e volumes de calda no controle químico da ferrugem da folha da aveia (Puccinia coronata f. sp. avenae)
Provedor de dados: 70
Autores: Oliveira,Ana R. de; Boller,Walter; Forcelini,Carlos A.; Blum,Rubens; Lopes,André.
A ferrugem da folha (Puccinia coronata f. sp. avenae) é a doença mais destrutiva da aveia, e aplicações de fungicidas com volumes baixos de calda podem reduzir a eficácia do controle químico. O objetivo do trabalho foi avaliar a eficiência técnica e econômica de fungicidas, doses e volumes de calda no controle da ferrugem da folha da aveia. O experimento foi conduzido no ano de 2003, na área experimental da FAMV/UPF, com a cultivar de aveia UPFA-20. Os tratamentos foram compostos pelas combinações entre dois fungicidas (tebuconazole, Folicur, 0,75 L ha-1 e epoxiconazole + piraclostrobim, Opera, 0,5 L ha-1), quatro doses (40; 60; 80 e 100% da dose recomendada) e dois volumes de calda (100 e 200 L ha-1). O delineamento experimental foi o de blocos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Produtos fitossanitários; Análise econômica.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200008

Temperaturas de acionamento de sistemas de climatização para perus em épocas de baixa umidade relativa do ar
Provedor de dados: 70
Autores: Mendes,Angélica S.; Moura,Daniella J. de; Nääs,Irenilza de A.; Sonoda,Lília T.
Este estudo teve o objetivo de avaliar distintos programas de acionamento dos sistemas de climatização (ventiladores e nebulizadores), visando a aprimorar o ambiente interno e o bemestar das aves, evitando possíveis perdas produtivas e gastos excessivos em energia elétrica. O estudo foi conduzido em dois aviários localizados no município de Uberlândia - MG, durante a época de baixa umidade relativa do ar (junho a dezembro). Os aviários foram comparados sob os parâmetros de concentrações de CO2, temperatura e umidade relativa do ar, temperatura superficial da cama e índices produtivos. Os dados climáticos foram submetidos à análise de variância, e os dados produtivos submetidos ao teste de Qui-quadrado, utilizando-se do software MINITAB V.14. Os resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ventiladores; Nebulizadores; Conforto térmico; Consumo de energia elétrica.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500002

Manejo de água em arroz de terras altas no sitema de plantio direto, usando o tanque classe A
Provedor de dados: 70
Autores: Rodrigues,Ricardo A. F.; Soratto,Rogério P.; Arf,Orivaldo.
O presente trabalho teve como objetivo estudar o efeito do manejo de água em cultivares de arroz de terras altas no sistema de plantio direto, usando o tanque Classe A. Os tratamentos consistiram na combinação de três manejos (sequeiro e duas lâminas) e duas cultivares (Confiança e Maravilha), com quatro repetições. A irrigação proporcionou aumento na altura de plantas, massa de 100 grãos, massa hectolítrica, produtividade de grãos, rendimento de benefício e redução do número de dias para o florescimento e ciclo total da cultura. Os valores adotados de coeficientes de cultura não influenciam nas características fenológicas e produtivas da cultura. A produtividade de grãos não diferiu entre as cultivares Confiança e Maravilha.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Oryza sativa L.; Coeficiente de cultura; Irrigação por aspersão.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300007

Influência da embalagem de polietileno de baixa densidade e da temperatura na conservação do repolho minimamente processado
Provedor de dados: 70
Autores: Rinaldi,Maria M.; Benedetti,Benedito C.
Neste trabalho, foi estudado o efeito da embalagem de polietileno de baixa densidade e da temperatura de armazenagem na conservação de repolho minimamente processado. Os repolhos, previamente resfriados à temperatura de 10 ºC, foram submetidos à seleção, lavagem, corte em quatro partes com a retirada do talo central, sanitização, corte em tiras, enxágüe, centrifugação, pesagem e acondicionamento em embalagens plásticas de polietileno de baixa densidade (70 µm) e armazenados em câmaras frias nas temperaturas de 1 e 10 ºC por 20 dias. Avaliaram-se dióxido de carbono, oxigênio e etileno na atmosfera interna da embalagem, bem como pH, acidez titulável, sólidos solúveis totais, vitamina C, perda de massa fresca e relação sólidos solúveis totais/acidez no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Atmosfera modificada; Armazenamento; Brassica oleracea var. capitata.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200021

Integração agricultura-pecuária em plantio direto: produção de forragem e resíduo de palha após pastejo
Provedor de dados: 70
Autores: Mello,Luiz M. M. de; Yano,Élcio H.; Narimatsu,Karem C. P.; Takahashi,Celso M.; Borghi,Émerson.
O objetivo deste trabalho foi verificar, no sistema integração agricultura-pecuária, a possibilidade de utilizar uma cultura para pastejo cujos resíduos permitam produção de palha suficiente para a manutenção do plantio direto, bem como avaliar a produção da forrageira e do resíduo em diferentes distâncias em relação ao centro do pivô, em três épocas, e o desempenho econômico do sistema. Avaliaram-se o impacto do pastejo rotacionado de sorgo forrageiro em plantio direto, sob irrigação em um pivô central de 75 ha, sobre a produção de matéria seca do sorgo forrageiro, a quantidade de resíduos, o custo de produção e o ganho de peso animal. O ensaio foi conduzido num Latossolo Vermelho Distrófico. O delineamento experimental utilizado foi o de blocos ao acaso,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sorgo forrageiro; Pastejo rotacionado; Produção de palha.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100014

Setting efficiency indicators for center pivots
Provedor de dados: 70
Autores: Schons,Ricardo L.; Robaina,Adroaldo D.; Peiter,Márcia X.
In this study, it was discussed the efficiency criteria in each of the elements that compose a central pivot, and this analysis was applied to two sets of systems located in regions of Cruz Alta and Santo Augusto, state of Rio Grande do Sul, Brazil. The methodology used combines water and energy assessment through an indicator called Normalized Specific Consumption in Irrigation (C ENI), allowing thus a comparison between equipment and projects. The C ENI in Cruz Alta region showed 72% of the equipment above the standard (8.68 kWh mm-1 ha-1 100m-1), and in Santo Augusto region 64.28% with consumption above the standard. The mean irrigation efficiency for Cruz Alta region was 29.85%, with standard deviation of 5.41%, and for Santo Augusto region, it was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Consumption; Parameter.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300005

Comparação de três métodos de estimativa da evapotranspiração de referência para a região de Araraquara - SP
Provedor de dados: 70
Autores: Vescove,Humberto V.; Turco,José E. P.
Uma forma de verificar a eficiência de métodos de estimativa da evapotranspiração de referência (ETo) é a comparação com o método-padrão. Este trabalho tem por finalidade comparar três métodos de estimativa da ETo: Radiação Solar (RS), Makkink (MAK) e Tanque Classe A (TCA) em relação ao método de Penman-Monteith (PM), em dois períodos distintos das fases de desenvolvimento da cultura de citros, com dados médios quinzenais para os períodos inverno-primavera e verão-outono. A pesquisa foi desenvolvida em uma fazenda de citros, em Araraquara - SP, onde foi instalada uma estação meteorológica automatizada e um tanque Classe A. Por intermédio da estação meteorológica automatizada, foram obtidas medidas da radiação solar global, saldo de radiação, temperatura do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Citros; Evapotranspiração de referência.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300017

Software for calculation of reservoir active capacity with the sequent-peak algorithm
Provedor de dados: 70
Autores: Silva,Rogério T. da; Sánchez-Román,Rodrigo M.; Teixeira,Marconi B.; Franzotti,Celso L.; Folegatti,Marcos V.
It is presented a software developed with Delphi programming language to compute the reservoir's annual regulated active storage, based on the sequent-peak algorithm. Mathematical models used for that purpose generally require extended hydrological series. Usually, the analysis of those series is performed with spreadsheets or graphical representations. Based on that, it was developed a software for calculation of reservoir active capacity. An example calculation is shown by 30-years (from 1977 to 2009) monthly mean flow historical data, from Corrente River, located at São Francisco River Basin, Brazil. As an additional tool, an interface was developed to manage water resources, helping to manipulate data and to point out information that it would be of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation planning; Seasonal water demand; Water resources management; Watershed management.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300007

ANALYSIS OF SPATIAL AUTOCORRELATION OF GRAIN PRODUCTION AND AGRICULTURAL STORAGE IN PARANÁ
Provedor de dados: 70
Autores: Cima,Elizabeth G.; Uribe-Opazo,Miguel A.; Johann,Jerry A.; Rocha Jr.,Weimar F. da; Dalposso,Gustavo H.
ABSTRACT This work aimed to study the spatial autocorrelation of the total static capacity storage, the total number of warehouses in 2013/2014 (CONAB) and the average of the total grain production (soybean, corn 1st and 2nd crops and wheat) in the harvest years 2008/2009 to 2013/2014 (SEAB) in Paraná State, Brazil. The study was based on Moran's global autocorrelation index, Moran's local and Moran's bivariate correlation. It was possible to identify regions with low and high total grain production. There was positive spatial autocorrelation for the Total Static Storage Capacity (TSSC) and Total Quantity of Warehouses (TQW). For the total grain production, significant spatial autocorrelation were found. The total static storage capacity showed similarity...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Static capacity; Logistics; Corn; Soybean; Wheat and total warehouses.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300395

Sistema de sincronismo entre a colhedora de cana-de-açúcar e o veículo de transbordo
Provedor de dados: 70
Autores: Magalhães,Paulo S. G.; Baldo,Rodrigo F. G.; Cerri,Domingos G. P.
Um dos problemas encontrados na colheita mecanizada da cana-de-açúcar é a falta de sincronismo entre a colhedora e o transbordo, ocasionando perdas tanto de material como de capacidade operacional. A presente pesquisa teve como objetivo desenvolver um sistema capaz de auxiliar no sincronismo entre a colhedora e o veículo de transbordo por meio de comunicação sem fio. Dois sensores de ultra-som acoplados ao elevador e um microprocessador gerenciam tais informações, gerando correta sincronia entre as máquinas. O sistema foi testado em laboratório e em campo, cumprindo corretamente a função de manter as máquinas em sincronia, indicando e alertando aos operadores as suas posições relativas. O sistema desenvolvido reduziu as perdas de rebolo em cerca de 60 kg...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ultra-som; Otimização; Controle.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200008

Manejo da irrigação na cultura do crisântemo em vaso, cultivar rage, cultivado em ambiente protegido
Provedor de dados: 70
Autores: Farias,Maryzélia F. de; Saad,João C. C.; Villas Bôas,Roberto L.
Dentre as dificuldades que os produtores têm encontrado ao adotarem o cultivo em ambiente protegido, destaca-se a falta de dados específicos sobre o uso racional da água e o desconhecimento da quantidade e do momento de irrigar. Esta pesquisa foi desenvolvida na propriedade de um produtor, no Distrito de Holambra II, região de Paranapanema - SP, em cultivos rotineiramente desenvolvidos pelo produtor, buscando melhor representatividade dos dados obtidos. O objetivo principal deste experimento foi identificar a tensão de água no solo que pudesse resultar em melhor qualidade comercial da cultivar de crisântemo "Rage", cultivado em vaso e mantido em ambiente protegido. O delineamento experimental foi o inteiramente casualizado, com duas repetições. Os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dendranthema grandiflora; Tensão de água no substrato; Vaso.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100007

Uso da grade aradora superpesada, pesada e arado de discos na incorporação de calcário em profundidade e na produção de milho
Provedor de dados: 70
Autores: Prado,Renato de M.; Natale,William.
Este trabalho teve o objetivo de avaliar o efeito dos modos de incorporação de calcário na correção da acidez no perfil do solo e na produção do milho. Para tanto, foi conduzido um experimento em Latossolo Vermelho Distrófico, textura argilosa, em Uberlândia - MG, no período de maio de 1995 a março de 1997. O delineamento experimental foi em esquema de parcelas subdivididas. As parcelas principais foram constituídas pelos modos de incorporação do calcário: grade aradora pesada (14 discos de 0,86 m) e grade niveladora (60 discos de 0,56 m); arado de disco (4 discos de 0,66 m) e grade niveladora; grade aradora superpesada (14 discos de 0,86 m) e grade niveladora; as subparcelas foram as doses de calcário dolomítico: 0; 6 e 9,2 t ha-1. O modo de incorporação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modos de incorporação; Calagem; Zea mays L.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100019

Desempenho de lisímetro de pesagem hidráulica de baixo custo no semi-árido nordestino
Provedor de dados: 70
Autores: Santos,Francisco X. dos; Rodrigues,José J. V.; Montenegro,Abelardo A. de A.; Moura,Ronaldo F. de.
Medidas diretas de evapotranspiração de referência são importantes na avaliação e na calibração de métodos indiretos. Avaliou-se o desempenho de lisímetro de pesagem hidráulica de baixo custo, visando à determinação direta da evapotranspiração de referência (ETo), em área de assentamento rural no Semi-Árido nordestino. O lisímetro é de concepção simplificada, com travesseiros hidráulicos confeccionados com mangueira flexível de butil e revestida em náilon, interligados a um sistema manométrico com mercúrio e água. O equilíbrio do lisímetro foi estável, sendo o maior erro médio posicional de 3,93%. As calibrações geraram coeficientes de correlação superiores a 0,9993 e resoluções de leituras entre 0,095 e 0,134 mm. As leituras lisimétricas foram comparadas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lisímetro de pesagem; Penman-Monteith; Necessidade hídrica; Evapotranspiração.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100012

PEDOFUNCTIONS APPLIED TO THE LEAST LIMITING WATER RANGE TO ESTIMATE SOIL WATER CONTENT AT SPECIFIC POTENTIALS
Provedor de dados: 70
Autores: Tavanti,Renan F. R.; Freddi,Onã da S.; Tavanti,Tauan R.; Rigotti,Adriel; Magalhães,Wellington de A.
ABSTRACT The least limiting water range (LLWR) is a soil physical quality indicator that receives much attention. It has been criticized and put to the test regarding mathematical models that compose it since they describe the behavior of soil physical attributes in a simplified way. This study aimed to assess the efficiency of some pedofunctions proposed in the literature and artificial neural networks on the accuracy in predicting soil water retention at potentials equivalent to field capacity (θFC) and permanent wilting point (θPWP). In other words, to apply the best models to LLWR of two soil types (Oxisol and Ultisol) and verify changes in their structure. The results indicated that pedofunctions using sand, silt, clay, bulk density, and soil organic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil physics; Soil physical quality indicator; Available water; Pedotransfer functions; Artificial neural networks.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400444

Ferramenta computacional para dimensionamento de silo unicelular de concreto armado – parte I: silo de seção circular
Provedor de dados: 70
Autores: SILVA,MARIA C. A. T. DA; CARVALHO,LEONARDO DA S.
Silos são construções que, em função de sua finalidade de utilização, estão sujeitos a carregamentos peculiares, tais como pressões horizontais e verticais - estáticas ou dinâmicas, dependendo da fase de operação - atrito nas paredes e cargas térmicas, todos causados pela presença do produto armazenado. Com o objetivo de sistematizar os procedimentos necessários para o dimensionamento de silos unicelulares de concreto armado, um programa computacional denominado SILOS foi desenvolvido, sendo composto por dois módulos: Módulo 1, para silos cilíndricos de seção circular e Módulo 2, para silos prismáticos de seção retangular. Neste artigo (Parte I), são apresentados os procedimentos que compõem o Módulo 1. O Módulo 2 será apresentado em artigo subsequente...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Silo; Concreto armado; Produto sólido; Análise estrutural; Dimensionamento; Automação.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200378

Estimation of transpiration of the 'Valencia' orange young plant using thermal dissipation probe method
Provedor de dados: 70
Autores: Coelho,Rubens D.; Vellame,Lucas M.; Fraga Júnior,Eusímio F.
Most studies on measures of transpiration of plants, especially woody fruit, relies on methods of heat supply in the trunk. This study aimed to calibrate the Thermal Dissipation Probe Method (TDP) to estimate the transpiration, study the effects of natural thermal gradients and determine the relation between outside diameter and area of xylem in 'Valencia' orange young plants. TDP were installed in 40 orange plants of 15 months old, planted in boxes of 500 L, in a greenhouse. It was tested the correction of the natural thermal differences (DTN) for the estimation based on two unheated probes. The area of the conductive section was related to the outside diameter of the stem by means of polynomial regression. The equation for estimation of sap flow was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lysimetry; Sap flow; Xylem.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300016

Impact of elevated temperature scenarios on potato leaf development
Provedor de dados: 70
Autores: Streck,Nereu A.; Uhlmann,Lilian O.; Zanon,Alencar J.; Bisognin,Dilson A.
The objective of this study was to simulate the impact of elevated temperature scenarios on leaf development of potato in Santa Maria, RS, Brazil. Leaf appearance was estimated using a multiplicative model that has a non-linear temperature response function which calculates the daily leaf appearance rate (LAR, leaves day-1) and the accumulated number of leaves (LN) from crop emergence to the appearance of the upper last leaf. Leaf appearance was estimated during 100 years in the following scenarios: current climate, +1 °C, +2 °C, +3 °C, +4 °C e +5 °C. The LAR model was estimated with coefficients of the Asterix cultivar in five emergence dates and in two growing seasons (Fall and Spring). Variable of interest was the duration (days) of the crop emergence...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solanum tuberosum; Global warming; Leaf appearance; Agricultural crops; Food security.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400008

Comportamento de atributos físicos de um Latossolo Amarelo sob agroecossistemas do Amazonas
Provedor de dados: 70
Autores: Souza,Zigomar M.; Leite,José A.; Beutler,Amauri N.
O desmatamento da floresta tropical da Amazônia e a utilização do solo para fins agrícolas potencializam sua degradação física, química e biológica, quando realizados de forma inadequada. Este estudo teve o objetivo de avaliar o efeito de sistemas de uso e manejo de um Latossolo Amarelo, muito argiloso, mediante avaliações de atributos físicos determinados nas profundidades de 0,0-0,2 e 0,2-0,4 m, em área da Universidade do Amazonas, Manaus (AM). Os sistemas de uso e manejo foram: milho, laranja, pupunha, guaraná, pastagem, capoeira e floresta. Nos sistemas com milho, laranja, pupunha e pastagem, foram realizados o desmatamento, a queima e as operações de preparo e cultivo mecanizados. Foram avaliados a composição granulométrica, o grau de floculação da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Matéria orgânica; Propriedades físicas; Sistemas de uso.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300017

Sowing depths of brachiaria in intercropping with corn in no tillage planting
Provedor de dados: 70
Autores: Gazola,Rodolfo de N.; Melo,Luiz M. M. de; Dinalli,Raíssa P.; Teixeira Filho,Marcelo C. M.; Garcia,Cássia M. de P.
The forage production in crop-livestock integration is critical both for formation of straw for no tillage planting and food for livestock farm. The experiment was conducted in the autumn/winter of 2009 and 2010, in the city of Selvíria -state of Mato Grosso do Sul -MS, Brazil, at Experimental Station of FEIS/UNESP. The objective was to evaluate the optimal depth for deposition of seeds of two Brachiaria species intercropped with corn with emphasis on grain yield and straw. The experimental design was a randomized block design in a factorial scheme 3 x 3, with four replications. The main treatments were two species of Brachiaria (Urochloa brizantha "Marandú" and Urochloa ruziziensis), which seeds were mixed with corn fertilizer and a control treatment...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Crop-livestock integration; Mechanization; Grain yield; Urochloa brizantha; Urochloa ruziziensis.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100016

CHEMICAL AGENTS AND SHADING LEVELS FOR THE PRODUCTION OF PEPPER SEEDLINGS
Provedor de dados: 70
Autores: Binotti,Eliana D. C.; Costa,Edilson; Binotti,Flávio F. da S.; Batista,Thiago B.
ABSTRACT The aim of this study was to evaluate protected cultivation environments with different levels of shading and application of foliar chemical agents, on growth, photosynthetic pigments and seedling quality of Capsicum frutensens L. The experiment was developed at the State University of Mato Grosso do Sul, University Unit of Cassilândia, with chili pepper. Three cultivation environments (screen of 18, 35 and 50% of shading) and six leaf chemical agents were used [(1) control – without application; (2) Nitrogen (N) 1%; (3) Paclobutrazol 50 mg L-1 + N 1%; (4) Auxin 0.05 g L-1 + N 1%; (5) Gibberellin 0.05 g L-1 + N 1%; and (6) Auxin 0.05 g L-1 + Gibberellin 0.05 g L-1 + N 1%]. Each environment was considered an experiment in which the completely...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Auxin; Capsicum frutensens L; Gibberellin; Light; Nitrogen; Paclobutrazol.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400450

Compton scattering tomography for agricultural measurements
Provedor de dados: 70
Autores: Cruvinel,Paulo E.; Balogun,Fatai A.
This paper presents a new approach in tomographic instrumentation for agriculture based on Compton scattering, which allows for the simultaneous measurements of density and moisture of soil samples. Compton tomography is a technique that can be used to obtain a spatial map of electronic density of samples. Quantitative results can be obtained by using a reconstruction algorithm that takes into account the absorption of incident and scattered radiation. Results show a coefficient of linear correlation better than 0.81, when comparison is made between soil density measurements based on this method and direct transmission tomography. For soil water contents, a coefficient of linear correlation better than 0.79 was found when compared with measurements...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compton tomography; Soil density and moisture; Agricultural automation.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100017

NEURO-FUZZY MODELING OF EYEBALL AND CREST TEMPERATURES IN EGG-LAYING HENS
Provedor de dados: 70
Autores: Lins,Ana C. de S. S.; Lourençoni,Dian; Yanagi Júnior,Tadayuki; Miranda,Isadora B.; Santos,Italo E. dos A.
ABSTRACT Considering the challenges faced by poultry farming, this study aimed to develop a neuro-fuzzy model to predict eyeball and crest temperatures of egg-laying hens based on environmental conditions (dry bulb temperature and relative humidity). To develop the models and simulations, Matlab’s Fuzzy Toolbox® (Anfisedit) was used. Different configurations were used for each of the several neuro-fuzzy models developed. Eyeball temperature (ET) and chicken crest temperature (CCT) were simulated from the developed neuro-fuzzy models, and the obtained results were validated with the variables collected experimentally with the aid of recorder sensors and an infrared thermographic camera. The proposed neuro-fuzzy models allow the accurate estimation of ET and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Neuro-fuzzy; Thermography; Poultry farming; Simulation; Artificial intelligence.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100034

ENVIRONMENTAL VARIABLES AND QUALITY TOOLS APPLIED TO THE OPERATOR OF AN AGRICULTURAL MICROTRACTOR
Provedor de dados: 70
Autores: Estevam,Francisca N. de L.; Queiroz,Renata F. de; Damasceno,André F.; Silva,Rouverson P. da; Voltarelli,Murilo A.; Barbosa Filho,José A. D.
ABSTRACT Work in the field is characterized as unstructured because it is performed in inconvenient postures, without a fixed workstation, exposing the worker directly to the sun and other inclement weather. This may interfere in the health and the performance of the activity. The objective of this work was to characterize the environment of the agricultural microtractor operator, evaluating the thermal comfort during the activity in the municipality of Quixadá, CE. A model TC14 Super Yanmar Agritech microtractor, coupled to a rotary spindle, was used. For the measurements of the environmental variables, sensors and devices were installed on the operator and in the microtractor. The experimental design adopted the assumptions of statistical quality...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Operator health; Thermal load; Ergonomics.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200208

Diagnóstico das condições, tempo de uso e manutenção de pulverizadores no Estado de Mato Grosso do Sul
Provedor de dados: 70
Autores: Bauer,Fernando C.; Pereira,Francisco de A. R.; Scheeren,Bruno R.; Braga,Luiz W.
O estudo teve por objetivo avaliar a condição de manutenção de pulverizadores com capacidade de tanque superior a 2.000 litros, em áreas de produção de soja do Estado de Mato Grosso do Sul. Foram inspecionados 38 pulverizadores de arrasto e automotrizes e 45 conjuntos de pontas de pulverização. O levantamento a campo foi realizado em parceria com a DuPont do Brasil S.A. Foram feitas inspeções em componentes e equipamentos determinantes para o controle e a qualidade da pulverização: tacômetro, manômetro, Sistema de Posicionamento Global (GPS), tanque de água limpa e reservatório para lavagem de embalagens e pontas de pulverização. A avaliação da vazão de 12 pontas por conjunto foi realizada com o uso de provetas graduadas. Os resultados indicaram que a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Pontas; Avaliação de pulverizadores.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300017

Desempenho de três teorias de simulação do comportamento de um trator agrícola em tração
Provedor de dados: 70
Autores: Schlosser,José F.; Linares,Pilar; Sousa Filho,Eduardo G. de.
A simulação matemática é uma ferramenta importante na diminuição de custos de produção e viabilização de novos projetos de máquinas agrícolas. Este trabalho trata da comparação entre três teorias de simulação, as chamadas teorias de predição de tração clássicas, desenvolvidas por Wismer, Brixius e Gee-Clough, na simulação do desempenho de um trator agrícola de rodas. Para efetuar uma comparação entre as três teorias e apurar as condições mais apropriadas de uso das mesmas, realizou-se um experimento de campo com um trator de tração simples (4x2), com o controle de um número apreciável de variáveis relevantes, para criar condições de comparação com uma simulação posterior. No trabalho de campo, foram utilizados tratamentos que envolviam a condição do solo,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Teorias de predição; Patinamento; Índice de cone.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300024

DOES THE PRESENCE OF STRAW IN THE BILLET AFFECT THE QUALITY OF SUGARCANE PLANTING SYSTEMS?
Provedor de dados: 70
Autores: Frazão,Aycon T. L.; Noronha,Rafael H. de F.; Furlani,Carlos E. A.
ABSTRACT The mechanized harvesting process of sugarcane seedlings affects the mechanized planting operation in the sense that straw adhered to the billet can reduce the quantity of non-viable gems obtained as a result of mechanical damage sustained during the mechanized operation. This study proposes a method to improve the quality of the implantation of sugarcane crop by prevention of damages caused mainly during October/November, when adverse climatic conditions of higher water stresses and high temperatures exist. The objective of this study is to evaluate the quality of the sugarcane planting operation using seedlings with and without straw, distributed by planters and distributors of chopped sugarcane, and comparing their performance to that of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Control letters; Distributor; Primary extractor.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500616

Taxa de aplicação e uso de surfactante siliconado na deposição da pulverização e controle da ferrugem da soja
Provedor de dados: 70
Autores: Prado,Evandro P.; Raetano,Carlos G.; Dal Pogetto,Mário H. F. do A.; Costa,Saulo I. de A; Christovam,Rafael de S.
A eficiência do controle químico da ferrugem-asiática da soja (FAS), além de outros fatores, está associada ao uso da técnica de aplicação de fungicida mais adequada. O trabalho teve por objetivo avaliar tecnologias de aplicação sobre os depósitos da pulverização e controle da FAS nos anos agrícolas de 2009-2010 e 2010-2011. O delineamento experimental foi em blocos casualizados, e os tratamentos distribuídos no esquema fatorial 3x2 (três taxas de aplicação: 60; 110 e 160 L ha-1 com e sem adição de surfactante siliconado) sobre os depósitos da pulverização, usando como marcador o corante Azul Brilhante, em quatro repetições (Experimento 1). Para avaliação da severidade da doença, peso de mil grãos (PMG) e produtividade, foi adotado o mesmo delineamento do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adjuvantes; Depósitos da pulverização; Tecnologia de aplicação.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300514

MODELING OF DRAFT AND ENERGY REQUIREMENTS OF A MOLDBOARD PLOW USING ARTIFICIAL NEURAL NETWORKS BASED ON TWO NOVEL VARIABLES
Provedor de dados: 70
Autores: Al-Janobi,Abdulrahman; Al-Hamed,Saad; Aboukarima,Abdulwahed; Almajhadi,Yousef.
ABSTRACT Draft and energy requirements are the most important factors in the activities of farm machinery management owing to their role in matching the tractor with implements for different tillage operations. This study's aim was to model the draft and energy requirements of a moldboard plow based on two novel variables. The first was the soil texture index (STI), which was formed from the clay, sand, and silt contents with a range of 0.03–0.84. The second variable was the field working index (FWI), formed by combining the plow width, plowing speed, soil bulk density, soil moisture content, plowing depth, and tractor power into one dimensionless variable, which had a range of 7.17–82.45. The coefficient of determination (R2) values obtained using a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil texture index; Field working index; Artificial neural network; Prediction; Tillage.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300363

SOIL MESO- AND MACROFAUNA IN TWO SOYBEAN CROPS AFTER SWINE WASTEWATER APPLICATION
Provedor de dados: 70
Autores: Maciel,Ana P. C.; Sampaio,Silvio C.; Remor,Marcelo B.; Rosa,Danielle M.; Reis,Ralpho R. Dos.
ABSTRACT Hog raising generates a large amount of residues that is commonly discarded into the soil as fertilizer even with environmental risks. In this context, the aim of this study was to assess the application effects of different doses of swine wastewater (SW) associated with mineral fertilization on the abundance and diversity of organisms of soil meso- and macrofauna in two soybean crops. Treatments consisted of four doses (0, 100, 200, and 300 m3 ha−1) of SW with or without mineral fertilization in two soybean crop, totaling 24 experimental units. Soil meso- and macrofauna were sampled using pitfall traps installed at each plot. Samples were sorted and the organisms were separated and identified. The highest abundances were found between groups of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mineral fertilization; Swine wastewater; Soil fauna.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300556

Estimativa da irradiação solar global com partição mensal e sazonal para a região de Cascavel - PR
Provedor de dados: 70
Autores: Valiati,Melania I.; Ricieri,Reinaldo P.
No presente trabalho, mostram-se equações de estimativa da irradiação solar global (R G), por meio do modelo de Angstrom, com partições sazonal e mensal para a região de Cascavel - PR. Os dados experimentais foram cedidos pelo IAPAR, coletados na sua estação meteorológica localizada na COODETEC/Cascavel - PR, no período de 1983 a 1998. Dos 16 anos de dados, 12 anos foram utilizados para cálculo dos coeficientes (a e b) e quatro anos para a validação das equações. Os coeficientes de determinação encontrados foram superiores a 80% para as duas partições. O mínimo da R G é superestimado e o máximo é subestimado quando comparados com o mínimo e o máximo para dados reais, sendo esses encontrados no solstício de inverno e equinócio de primavera, respectivamente....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Heliógrafo; Actinógrafo; Modelo de Angstrom.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100009

ERRATA: volume 33, número 4
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600024

Spatial autocorrelation of ndvi and gvi indices derived from landsat/tm images for soybean crops in the western of the state of Paraná in 2004/2005 crop season
Provedor de dados: 70
Autores: Dalposso,Gustavo H.; Uribe-Opazo,Miguel A.; Mercante,Erivelto; Lamparelli,Rubens A. C.
This research aims at studying spatial autocorrelation of Landsat/TM based on normalized difference vegetation index (NDVI) and green vegetation index (GVI) of soybean of the western region of the State of Paraná. The images were collected during the 2004/2005 crop season. The data were grouped into five vegetation index classes of equal amplitude, to create a temporal map of soybean within the crop cycle. Moran I and Local Indicators of Spatial Autocorrelation (LISA) indices were applied to study the spatial correlation at the global and local levels, respectively. According to these indices, it was possible to understand the municipality-based profiles of tillage as well as to identify different sowing periods, providing important information to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spatial statistics of areas; Spatial correlation; Vegetation index.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300009

Proposta de mecanismo de lavagem em equipamentos de beneficiamento de tomate de mesa
Provedor de dados: 70
Autores: Silva,Michele C.; Testezlaf,Roberto; Ferreira,Marcos D.
A etapa de limpeza no sistema de beneficiamento do tomate de mesa é essencial tanto para a aceitação do produto pelo consumidor, quanto para a conservação da qualidade do fruto. Entretanto, a etapa de lavagem nos atuais sistemas de limpeza utilizados em unidades de beneficiamento, demanda volume excessivo de água, trazendo sérias preocupações econômicas e ambientais. O objetivo deste trabalho foi contribuir com informações para otimizar o sistema de lavagem em equipamentos de beneficiamento de tomate de mesa. Para tanto, comparou-se o sistema convencional de limpeza, utilizado atualmente, e constituído de tubos de PVC com orifícios, com sistema redimensionado utilizando-se sprays comerciais. Foram determinadas as curvas características (vazão versus...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lycopersicum esculentum; Limpeza; Pós-colheita.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200034

Velocidade econômica de escoamento e custos de energia de bombeamento
Provedor de dados: 70
Autores: Perroni,Bruno L. T.; Carvalho,Jacinto de A.; Faria,Lessandro C.
Diversos fatores podem atuar como limitante para a atividade agrícola irrigada, dentre os quais a energia utilizada no sistema de irrigação tem grande destaque. Ainda que o sistema esteja hidraulicamente correto, ele pode não estar sendo economicamente viável para o produtor. Neste trabalho, foram feitas simulações para a determinação do diâmetro mais econômico para adutoras de aço galvanizado e PVC. Também foram obtidos modelos para a determinação dos custos de bombeamento. Foi constatado que, para tubulações de aço galvanizado, a velocidade econômica variou entre 0,67 e 1,63 m s-1 e para PVC variou entre 0,62 e 1,97 m s-1. Com os modelos gerados neste trabalho, é possível obter de forma mais rápida os parâmetros econômicos que envolvem os sistemas de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Diâmetro econômico; Energia de bombeamento; Tubulação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300009

DOES MOISTURE IN PODS INTERFERE WITH MECHANIZED HARVESTING OF PEANUTS?
Provedor de dados: 70
Autores: Santos,Adão F. dos; Alcântara,Aline S.; Corrêa,Lígia N.; Queiroz,Renata F. de; Silva,Rouverson P. da.
ABSTRACT Although peanut harvesting results in significant losses, it has rarely been investigated. Thus, this study aimed to analyze the interference of different pod moisture contents on peanut harvesting and their influence on the process quality based on losses and impurities. An experiment was performed in a peanut seed producing area, in Luzitânia, district of Jaboticabal - SP, using average moisture contents of 15% and 20% in the pods; 16 and 14 data points were collected for the 20% and 15% treatments, respectively. The experimental design used statistical process control (SPC) to analyze the collected variables. The results indicated higher losses in the platform than in the machine. In addition, the harvest quality was not affected by the pod...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Harvest losses; Harvest impurities; Peanut gathering; Adjustment of machines.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100098

Desempenho e características construtivas de um protótipo de dosador pneumático para sementes de arroz
Provedor de dados: 70
Autores: Reis,Ângelo V. dos; Forcellini,Fernando A.
Tendo em vista a elevação do custo das sementes miúdas e a inadequação das semeadoras de precisão atuais, que não semeiam culturas com pequenos espaçamentos entre linhas, o presente trabalho teve o objetivo de apresentar os resultados dos testes de um protótipo de dosador pneumático, tipo cilindro vertical, para sementes de arroz. Foram avaliadas em laboratório a precisão na captação de sementes (com pressões de -56,0; -62,7 e -73,1 kPa, velocidades tangenciais de 0,10; 0,22 e 0,30 m s-1, e orifícios dosadores de 1,2 e 1,5 mm), a regularidade de distribuição longitudinal de sementes (com o reservatório de sementes com 25 e 50% da capacidade, inclinação lateral de 0 e 11º, orifícios com 1,5 mm) e o dano mecânico de sementes, em experimentos inteiramente...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dosador de precisão; Dosagem a vácuo; Sementes miúdas.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200009

Biodigestão anaeróbia de dejetos de suínos sob efeito de três temperaturas e dois níveis de agitação do substrato: considerações sobre a partida
Provedor de dados: 70
Autores: Souza,Cecília F.; Lucas Júnior,Jorge de; Ferreira,Williams P. M.
Neste trabalho, avaliou-se a biodigestão anaeróbia de dejetos de suínos. Para isso, foi utilizado esquema laboratorial, constituído de 24 digestores com volume total de 14 L, sendo cada um abastecido com dejetos de suínos em fase de terminação, diluídos em água, perfazendo 10 L de volume útil de substrato com concentração inicial de sólidos totais de 6%. Três grupos formados por oito desses biodigestores foram expostos a três temperaturas (25; 35 e 40 ºC) e a dois níveis de agitação (com e sem) do substrato. A análise da fase de partida foi feita com base na produção média acumulada de biogás, num período de 71 dias. Os resultados demonstraram que a agitação não interferiu e que o melhor desempenho, inclusive o menor tempo gasto para atingir determinado...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biodigestor; Suinocultura; Etapa de partida.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200027

EFFECTS OF SIZE AND SAMPLING GRID ON THE QUALITY OF APPARENT SOIL ELECTRICAL CONDUCTIVITY MAPS
Provedor de dados: 70
Autores: Oldoni,Henrique; Costa,Bruno R. S.; Rocha Junior,Romero C.; Rabello,Ladislau M.; Bassoi,Luís H.
ABSTRACT The apparent soil electrical conductivity (ECa) is an attribute commonly used for the characterization of the spatial variability of soil, but its determination by handheld sensors consumes considerable time and labor. The reduction in the number of sampling points allows minimize them but can result in increased uncertainty of interpolated maps. Thus, the goal of this study was to identify the best spacing and number of ECa measurements, to guarantee the quality of maps generated in three vineyards. The ECa values were obtained using a handheld sensor in different sampling grids. The data were submitted to descriptive statistical and geostatistical analyses. The relative deviation and Kappa coefficient of agreement were used to assess the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spatial variability; Geostatistics; Agricultural instrumentation.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800001

Modelagem da dinâmica do potássio no solo sob irrigação por gotejamento: validação do modelo
Provedor de dados: 70
Autores: Rivera,René N. C.; Duarte,Sergio N.; Miranda,Jarbas H. de; Botrel,Tarlei A.
A compreensão do transporte simultâneo de água e solutos a partir de uma fonte pontual permite desenvolver estratégias eficientes na fertirrigação, sendo importante no dimensionamento, operação e manejo de sistemas de irrigação localizada. Assim, o presente trabalho teve como objetivo apresentar a validação de modelo matemático desenvolvido para simular o deslocamento simultâneo de água e potássio na irrigação por gotejamento. O desenvolvimento do modelo baseou-se na resolução numérica de equações diferenciais parciais de segunda ordem, aplicadas à fonte puntiforme sob fluxo transiente de água e solutos. O experimento de validação foi conduzido no Departamento de Engenharia Rural da ESALQ/USP. O solo utilizado foi um Latossolo Vermelho, fase arenosa, série...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulação; Transporte de potássio; Bulbo úmido.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200006

Índíces de conforto térmico e concentração de gases em galpões avícolas no semiárido Paraibano
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Rocha,Herlucio P.; Nascimento,José W. B.; Silva,José H. V.
Esta pesquisa teve o objetivo de determinar os índices de conforto térmico e a concentração de gases no interior de galpões avícolas e suas influencias sobre o desempenho de frangos de corte comercias, em condições de verão, na região semiárida paraibana. Utilizaram-se dois aviários, um coberto com telha de cerâmica e outro coberto com telha de fibrocimento. Observou-se que não houve diferença significativa (p &gt; 0,05) entre a temperatura ambiente (TA), umidade relativa do ar (UR), temperatura da água de bebida (Tágua) e da cama entre os galpões, sendo que os valores médios de TA (das 8h às 17h) e UR (das 10h às 16h) podem ser considerados fora do limite da zona de termoneutralidade recomendada para frangos de corte, como também a Tágua, no período...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Condições climáticas; Produtividade; Qualidade do ar.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600001

Avaliação térmica de placas de argamassa de cimento e casca de arroz aquecidas por resistência elétrica
Provedor de dados: 70
Autores: Rossi,Luiz A.; Cardoso,Paulo E. dos R.; Beraldo,Antonio L.
Neste trabalho, apresenta-se uma proposta alternativa para o sistema de aquecimento de piso por resistência elétrica em granjas de aves e suínos. Após o dimensionamento do sistema, foram confeccionadas placas com argamassa de cimento, areia e casca de arroz, com diferentes traços, a fim de avaliar esse material alternativo de construção, sendo construído um controlador eletrônico de temperatura para dar mais autonomia ao sistema de aquecimento. O sistema mostrou-se eficiente no controle da temperatura da placa. Dentre os traços analisados, aquele com a placa mista de argamassa convencional e casca de arroz demonstrou melhor desempenho.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Conforto térmico; Aquecimento de piso; Casca de arroz.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100005

Manejo e viabilidade econômica da irrigação por gotejamento na cultura do cafeeiro acaiá considerando seis safras
Provedor de dados: 70
Autores: Oliveira,Ednaldo L. de; Faria,Manoel A. de; Reis,Ricardo P.; Silva,Mirian de L. O. e.
Este trabalho teve como objetivo estudar técnica e economicamente o efeito da irrigação por gotejamento na produção do cafeeiro (Coffea arabica L.) Acaiá MG-1474. O delineamento experimental utilizado foi o de blocos casualizados, com cinco tratamentos e quatro repetições. Os tratamentos foram: L0 = sem irrigação; L40 = 40%; L60 = 60%; L80 = 80% e L100 = 100% da Evaporação do Tanque Classe A (ECA). Para realizar a análise econômica, utilizou-se dos dados de produção acumulada das seis primeiras safras: 1999, 2000, 2001, 2002, 2003 e 2004. A análise dos custos da lavoura irrigada foi baseada na teoria dos custos de produção. A produtividade média dos tratamentos foi de 52,88; 66,99; 70,00; 71,93 e 79,50 sacas por hectare, para L0, L40, L60, L80 e L100,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Custo de produção; Acaiá MG-1474; Cafeicultura irrigada.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500011

STATIC PRESSURE DROP IN LAYERS OF CASTOR BEAN GRAINS
Provedor de dados: 70
Autores: Goneli,André L. D.; Corrêa,Paulo C.; Figueiredo Neto,Acácio; Kirsch,Michele R. H.; Botelho,Fernando M.
ABSTRACT Knowledge regarding the static pressure drop in granular layers is of fundamental importance in the development of efficient drying and aeration projects of agricultural products. Thus, the objective of this study was to evaluate the effects of impurity contents on the static pressure drop in different bed depth of castor bean grains, as well as modify the mathematical models per the obtained experimental data and select the model that best represents this phenomenon. First, impurities in castor bean grains of the Guarani variety were eliminated and 6% of the moisture content (dry basis) was retained. The coarse impurity contents were obtained with 2%, 4%, and 6% of mass addition. The pressure drop in different bed depth of clean and impure castor...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bulk density; Load loss; Porosity; Ricinus communis L.; Moisture content.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200184

EFFECTS OF PHOTOSELECTIVE SHADE NETS ON EARLY GROWTH OF SUGARCANE SEEDLINGS
Provedor de dados: 70
Autores: Cordeiro Júnior,José J. F.; Cavalcanti,Sávio D. L.; Souza,Rayanne T. de A.; Batista,Pedro H. D.; Guiselini,Cristiane.
ABSTRACT Sugarcane has a great economic interest in Brazil, so it needs technologies to increase its yield strength, especially for seedling production. This study aimed to ascertain the influence of shading nets on early growth and development of pre-sprouted sugarcane seedlings. An experiment was conducted in a protected environment, in the Rural Federal University of Pernambuco (UFRPE), in Recife-PE, Brazil. The protected environments were covered with anti-UV low-density polyethylene plastic plus: Solpack® red ultranet net, Solpack® white net, Solpack® freshnet net, and without shade net, and five replications each. The experiment was carried out in a completely randomized design, and multivariate principal component analysis (PCA) was used to verify...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Protected environment; Shade nets; Solar radiation; Saccharum officinarum.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100010

ENVIRONMENTAL THERMAL COMFORT OF A REDUCED MODEL USING CROSS-LAMINATED TIMBER
Provedor de dados: 70
Autores: Sampaio,Carlos A. de P.; Terezo,Rodrigo F.; Motta,Guilherme; Silva,Leonardo M. da C.; Vassem Júnior,Ilson.
ABSTRACT The challenges for the use of the cross-laminated timber (CLT) system in the Brazilian agricultural market are significant. This study evaluated the thermal performance of fiber cement tiles associated with a CLT non-conventional structure compared to those of ceramic, fiber cement and aluminum roof tiles based on following thermal comfort indexes (i.e., black globe humidity index (BGHI), radiant heat load (RHL) and specific enthalpy) using physical conventional models of reduced-scale rural facilities under summer conditions. The non-conventional CLT model comprised closing walls and a lining that form a self-supporting structure with few air inlets. This model presented reduced thermal comfort indexes compared to the other conventional roofs....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precasting in wood; Self-supporting; Thermal comfort; Environmental factors.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400413

Groundwater recharge estimate at Alto Rio Grande - MG watershed
Provedor de dados: 70
Autores: Silva,Lucas A. da; Silva,Antônio M. da; Coelho,Gilberto; Mello,Carlos R. de; Pereira,Donizete dos R.
Springs are outcrops of aquifers surface, and the water cycle in this environment pass through the recharge, generally defined as the amount of water added to the aquifer, which may occur locally from rainwater infiltration. This study uses the Water Table Fluctuation (WTF) method to estimate the direct recharge and a groundwater balance to estimate the deep recharge on unconfined aquifers. The WTF method employs data of the aquifer water levels and its specific yield to estimate the direct recharge. The groundwater balance considers the direct recharge estimated by the WTF method, as the water input in the system and outputs as the base flow and deep recharge. The recharge was estimated at four areas at the watershed of Alto Rio Grande city, Minas Gerais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Groundwater recharge; Aquifer surface; Springs.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600011

DIFFERENT GENDER DIVISION PATTERNS FOR SWINE HOUSING IN WEAN-TO-FINISH SYSTEM
Provedor de dados: 70
Autores: Massari,Juliana M.; Vercellino,Rimena do A.; Curi,Thayla M. R. de C.; Moura,Daniella J. de; Medeiros,Brenda B. L.; Salgado,Douglas D'Alessandro.
ABSTRACT This study aimed at identifying the best gender division pattern for swine at nursery stage, through the evaluation of behavioral and environmental parameters. Three treatments were established to achieve our objective: single-sex housing of 26 surgically castrated male pigs; mixed-sex housing of 13 castrated males and 13 females; and single-sex housing of 26 females. Environmental and behavioral data have been recorded. It was used an ethogram to make an inventory of behaviors and that was used in multivariate analysis. Bite addiction differed statistically among treatments, and the lowest occurrence was in mixed-sex housing. Results of the multivariate analysis suggested that regardless of the treatment chosen, relative humidity is positively...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Multivariate analysis; Welfare; Behavior; Facilities.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100013

Determinação do equilíbrio higroscópico e do calor isostérico do bagaço de cana-de-açúcar
Provedor de dados: 70
Autores: Teixeira,Luciana P.; Andrade,Ednilton T. de; Espíndola,Jéssica Z.; Pereira,Roberto G.
Com o intuito de analisar a dinâmica de sorção e a energia necessária para a vaporização da água na desidratação do bagaço da cana-de-açúcar, o presente trabalho teve como objetivo a determinação de seu equilíbrio higroscópico e calor isostérico, a partir de diferentes condições controladas de temperatura (20; 40; 55 e 70 ºC) e umidade relativa do ar (10; 12; 17; 18; 30; 40; 45; 50; 60 e 85%), assim como avaliar, entre diversos modelos descritos na literatura, o que melhor represente o comportamento de sorção. Como resultado, foi verificado que o modelo que melhor se ajustou aos dados empíricos do processo de sorção do bagaço de cana-de-açúcar foi o Modelo de Henderson Modificado, com coeficiente de determinação de 0,972, enquanto o calor isostérico...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bagaço de cana-de-açúcar; Equilíbrio higroscópico; Calor isostérico.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300555

Quantificação de macronutrientes no solo e em folhas de cana-de-açúcar em função de doses de resíduo da mineração de bauxita
Provedor de dados: 70
Autores: Nobile,Fabio O. De; Galbiatti,João A.; Muraishi,Reginaldo; Ribeiro,Adriano G.; Freddi,Onã da S.
O experimento foi realizado em ambiente protegido, com o objetivo de avaliar o efeito do resíduo da mineração de bauxita nos teores de macronutrientes, no solo e em plantas de cana-de-açúcar. Foram utilizados vasos de 10 L que receberam as seguintes doses de resíduo de bauxita: 0; 28;56; 84; 112 e 140 t ha-1, utilizando-se do clone de cana-de-açúcar SP92 4221. A incorporação do resíduo de bauxita no solo proporcionou aumento nos teores dos macronutrientes do solo, sendo que apenas para o enxofre doses acima de 83 t ha-1 proporcionaram reduções desse nutriente. Já para os teores de macronutrientes determinados na folha, doses acima de 70,5; 125; 101 e 56 t ha-1 diminuíram os teores de nitrogênio, fósforo, potássio e enxofre, respectivamente. Entretanto,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sacharum oficinarum; Condicionador de solo; Resíduo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100018

Modelo de regressão espacial para estimativa da produtividade da soja associada a variáveis agrometeorológicas na região oeste do estado do Paraná
Provedor de dados: 70
Autores: Araújo,Everton C. de; Uribe-Opazo,Miguel A.; Johann,Jerry Adriani.
Este trabalho apresenta o Modelo de Regressão Espacial Autorregressivo Misto (SAR) e Modelo do Erro Espacial (CAR) no intuito de investigar a associação entre a produtividade da soja e as variáveis agrometeorológicas relacionadas à precipitação pluvial, temperatura média e radiação solar global. O estudo foi realizado com os dados das safras dos anos agrícolas de 2005/2006 a 2007/2008, da região oeste do estado do Paraná. Como os dados agrometeorológicos estão disponíveis apenas para oito municípios da região em estudo, as estimativas foram obtidas por meio do uso de Polígonos de Thiessen. A estimativa de parâmetros dos modelos ajustados foi obtida utilizando o método de Máxima Verossimilhança. A avaliação do desempenho dos modelos foi realizada com base...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Autocorrelação espacial; Estatística espacial de área; Modelos espaciais SAR e CAR.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200010

Metodologia baseada em técnicas de mineração de dados para suporte à certificação de raças de ovinos
Provedor de dados: 70
Autores: Vieira,Fábio D.; Oliveira,Stanley R. de M.; Paiva,Samuel R.
RESUMO O objetivo deste trabalho foi desenvolver uma metodologia baseada em técnicas de mineração de dados para selecionar os principais marcadores SNP (Single Nucleotide Polymorphism) para as raças de ovinos: Crioula, Morada Nova e Santa Inês. Os dados utilizados foram obtidos do Consórcio Internacional de Ovinos e são compostos por 72 animais das raças citadas, e cada animal possui 49.034 marcadores SNP. Considerando que o número de atributos (marcadores) é muito maior que o de observações (animais), foram aplicadas as técnicas de predição LASSO (Least Absolute Shrinkage and Selection Operator), Random Forest e Boosting para a geração de modelos preditivos que incorporam métodos de seleção de atributos. Os resultados revelaram que os modelos preditivos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Polimorfismo de nucleotídeo único; Seleção de atributos; Modelos preditivos; Regressão penalizada.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601172

PHYSICO-MECHANICAL CHARACTERIZATION OF THE Anadenanthera colubrine WOOD SPECIE
Provedor de dados: 70
Autores: Christoforo,André L.; Aftimus,Bruno H. C.; Panzera,Tulio H.; Machado,Gilmara de O.; Lahr,Francisco A. R.
ABSTRACT In Brazil, the characterization of wood is carried out in accordance with the premises established by ABNT NBR 7190standard; however, the determination of wood properties requires the use of equipment, which hinders the wood characterization for the construction professional. To circumvent this problem, the properties of wood strength and stiffness can be estimated through regression models using the apparent density as estimator, being the density a physical property of easy determination. This study aimed to determine 4 physical and 13 mechanical properties of “Angico Branco” wood (Anadenanthera colubrina), and with the aid of regression models based on analysis of variance, estimate the strength and stiffness properties as a function of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anadenanthera colubrina; Physico-mechanical characterization; Apparent density; Regression models; Analysis of variance (ANOVA).
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200376

Pedological characterization and land use and occupation: influences on water quality in a watershed located in the zona da mata (MG)
Provedor de dados: 70
Autores: Andrade,Luana C. R.; Marques,Eduardo A. G.; Felicori,Thaís de C.
In order to verify the influence of class and use and occupation of land on water quality, it was performed the characterization and analyzes of land use and monitoring of seven springs inserted in a watershed located in the rural of Viçosa city - Minas Gerais (MG) state, in Brazil. Through soil analyzes, carried out in five different profiles, it was possible to identify three distinct pedological classes: Argisol, Cambisol and Latosol. Furthermore, the concentrations of Fe, Mn, Cu, Zn, Cr, Cd, Pb and Ni were identified in each of the horizons in the considered profiles. Water samples were collected and analyzed monthly, over eight months, twenty two parameters of water quality. Comparing the results of each survey, it was possible to identify a relation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil characteristics; Water quality; Rural watershed.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400021

SPATIAL DEPENDENCE DEGREE AND SAMPLING NEIGHBORHOOD INFLUENCE ON INTERPOLATION PROCESS FOR FERTILIZER PRESCRIPTION MAPS
Provedor de dados: 70
Autores: Amaral,Lucas R. do; Justina,Diego D. Della.
ABSTRACT Data interpolation is widely required in precision agriculture. However, its effectiveness is a function of the characteristics of the dataset, being necessary for the evaluation of several parameters. This study aimed to identify how the spatial interpolators, Kriging, and Inverse Distance Weighting, are influenced by the degree of spatial dependence of the variables analyzed and the number of neighbors considered in the interpolation process (sampling neighborhood). Soil samples were collected from three sugarcane fields. By the optimization process, we verified that the sampling neighborhood influences the accuracy of interpolations, but there is not a standard recommendation to follow. Thus, the best sampling neighborhood must ever be...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Data interpolation; Soil sampling; Geostatistics; Site-specific management.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800085

SOYBEAN AGRONOMIC PERFORMANCE AND SOIL PHYSICAL ATTRIBUTES UNDER TRACTOR TRAFFIC INTENSITIES
Provedor de dados: 70
Autores: Arcoverde,Sálvio N. S.; Souza,Cristiano M. A. de; Rafull,Leidy Z. L.; Cortez,Jorge W.; Orlando,Roberto C.
ABSTRACT Machinery traffic intensification has been recurrent in intensive agriculture in annual crops, which may lead to structural soil degradation and, consequently, a reduction of its productive capacity. Therefore, this study aimed to assess the influence of tractor traffic intensification on soil physical attributes and soybean yield components. The study was performed in an Oxisol under no-tillage for 10 years, using a randomized block design with five tractor traffic intensities (0, 2, 4, 6, 8, and 12 passes) and five replications. Density, porosity, macroporosity, microporosity, and penetration resistance were assessed in the soil and stem diameter, number of pods per plant, number of grains per pod, grain weight per plant, thousand-grain weight,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Yield components; Shoot; Soil penetration resistance; Machinery traffic.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100113

DROPLET DISTRIBUTION AS A FUNCTION OF COTTON INTERROW SPACING AND ANGLES OF SPRAYER DISPLACEMENT
Provedor de dados: 70
Autores: de Lima Junior,Izidro dos S.; Degrande,Paulo E.; de Souza,Cristiano M. A.; Viegas Neto,Antonio L.
ABSTRACT Application technology factors may be influenced by changes in plant architecture, such as height and leaf area. This study aimed to evaluate which angle of sprayer displacement in the application of pesticides in relation to the direction of cotton sowing, cultivated in the ultra-narrow row, narrow row, and conventional systems, provides the best application quality characteristics in the different thirds of plants. The experiment was installed in a split-plot design with four replications in the 3 × 4 factorial scheme, composed of three cotton cultivation systems and four angles of sprayer displacement in relation to the direction of the sowing rows. The evaluated characteristics were mean volumetric diameter, density and coverage of droplets,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Droplet deposition; Third of plants.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600927

ELECTRONIC MONITORING SYSTEM FOR MEASURING HEART RATE AND SKIN TEMPERATURE IN SMALL RUMINANTS
Provedor de dados: 70
Autores: Costa,Daniel dos S.; Turco,Silvia H. N.; Ramos,Rodrigo P.; Silva,Flaviane M. F. M.; Freire,Murilo S.
Abstract The electronic monitoring of physiological responses is essential for managing animal production systems considering market demands for animal welfare. The objective of this study was to design, build, and test an electronic monitoring system, with recording and wireless transmission capability, for measuring the heart rate and skin temperature in small ruminants. The system had two components: a mobile base unit, mounted on the animal under study, and a fixed base unit. Wireless communication between the mobile and fixed units was performed using a Xbee Series 2 radio frequency transceiver whereas data were recorded and transferred to a secure digital card in the mobile unit. The device was mounted in Santa Inês crossbred sheep using reference...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Embedded electronics; Physiological responses; Precision livestock farming.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200166

Tratamento de toletes de cana-de-açúcar para o controle da podridão-abacaxi em pulverização conjugada ao plantio mecanizado
Provedor de dados: 70
Autores: Ferreira,Marcelo da C.; Werneck,Carolina F.; Furuhashi,Silvio; Leite,Gilson J.
No plantio mecanizado da cana-de-açúcar, há dificuldades em se proteger a cultura contra pragas e doenças do solo, requerendo uma tecnologia de aplicação de produtos fitossanitários que respeite o ambiente e os custos de produção. O objetivo deste trabalho foi avaliar um sistema de pulverização para controle de doenças e pragas do solo, conjugado ao equipamento de plantio mecanizado de toletes de cana-de-açúcar, tomando como alvo-indicador a podridão-abacaxi. Delineou-se o experimento em blocos ao acaso, em área de plantio comercial da variedade SP-891115. A pulverização deu-se na região da calha do equipamento de plantio, por onde os toletes deslizam até o solo. Avaliaram-se o número de perfilhos brotados e a produção da cultura. Os resultados foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thielaviopsis paradoxa; Tecnologia de aplicação; Aplicação localizada.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200007

USE OF SURFACTANT WITH DIFFERENT VOLUMES OF FUNGICIDE APPLICATION IN SOYBEAN CULTURE
Provedor de dados: 70
Autores: Roehrig,Rafael; Boller,Walter; Forcelini,Carlos A.; Chechi,Amanda.
ABSTRACT Application volume, adjuvants that act on the drop surface tension and droplet spectrum are the main factors affecting leaf surface coverage and the spray penetration droplets inside the canopy of the soybean crop, which may have an impact on fungicide efficiency, since those used in the handling of Asian-rust, including those that are absorbed by the plant, present a small displacement from the point of deposition. Thus, it was sought to determine the impacts on the use of the organosilicone surfactant compared to the changes in the spray volumes. For that, five spray volumes and the combination of two adjuvants were compared in randomized blocks with a factorial arrangement 5×2. Reductions in volume negatively impacted the number of drops cm−2...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Leaf surface cover; Phakopsora pachyrhizi; Application rate.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400577

Variedades de cana-de-açúcar submetidas à irrigação suplementar no cerrado goiano
Provedor de dados: 70
Autores: Campos,Patrick F.; Alves Júnior,José; Casaroli,Derblai; Fontoura,Patricia R.; Evangelista,Adão W. P.
O Estado de Goiás é o segundo maior produtor de cana-de-açúcar do Brasil. Entretanto, ainda apresenta baixa produtividade, devido principalmente à falta de variedades adaptadas a esta região e ao déficit hídrico típico. Assim, objetivou-se avaliar o desempenho de dezesseis variedades de cana-de-açúcar submetidas à irrigação suplementar no Cerrado. O experimento foi conduzido em Goianésia-GO, em um Latossolo Vermelho-Amarelo Distrófico, de textura argilosa de abril de 2011 a maio de 2012. O delineamento foi em blocos casualizados (Bifatorial 16x5), com 16 tratamentos (variedades): CTC2, CTC4, CTC9, CTC11, CTC15, CTC18, IAC87-3396, IAC91-1099, IACSP94-3046, IACSP94-2094, IACSP94-2101, IACSP95-5000, RB857515, RB92579, RB966928 e SP86-0042; e cinco tempos de...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Saccharum officinarum; Déficit hídrico; Manejo da irrigação; Aspersão.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600010

Unidades combinadas RAFA-SAC para tratamento de água residuária de suinocultura – parte I carga orgânica removida
Provedor de dados: 70
Autores: Amorim,Fabiana de; Fia,Ronaldo; França,Flávia A.; Terra,Lorena M.; Luiz Fia,Fátima R.
RESUMO Na pecuária brasileira, tem-se destacado a suinocultura, cuja produção de carne foi apontada como a terceira maior do mundo, e como contrapartida os sistemas produtivos são, potencialmente, poluidores do ambiente. Os sistemas anaeróbios têm sido utilizados para tratamento de água residuária suinícola, necessitando de complementação para diminuir as cargas de nutrientes e reúso agrícola. Neste trabalho, avaliou-se o efeito combinado de duas unidades de tratamento na remoção de matéria orgânica, na forma de demanda química de oxigênio (DQO), sendo um reator anaeróbio de manta de lodo e fluxo ascendente tipo RAFA com volume útil de 96 L, seguido de um sistema alagado construído (SAC) com capacidade para 237 L. O experimento foi conduzido em três fases,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carga orgânica; Cynodon ssp; Taxa de aplicação superficial; Tratamento biológico; Sistemas wetlands.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601149

MILK PRODUCTION AS AN INDICATOR OF DROUGHT VULNERABILITY OF CITIES LOCATED IN THE BRAZILIAN SEMIARID REGION
Provedor de dados: 70
Autores: Andrade,Tafnes da S.; Cunha,John E. de B. L.; Galvão,Carlos de O.; Rufino,Iana A. A.
ABSTRACT Several spectral indices have been used to estimate droughts, however, these indicators only give evidence of a dry spell leaving out its impacts on significant economic activities performed in a given region. In this context, livestock breeding in one of the most important activities to analyze in the Brazilian semiarid region. The aim of this study was to evaluate the relationship between the drought indices, obtained through remote sensory devices, and annual milk production (2004 – 2014), identifying the most affected cities by the drought and were considered the most vulnerable and in need of special attention during dry periods. In order to analyze the data, the hierarchical grouping technique and correlation analyses between milk production...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drought management; Drought indices; Livestock.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601203

Proposta metodológica utilizando ferramentas de qualidade na avaliação do processo de pulverização
Provedor de dados: 70
Autores: Santos,Sérgio R. dos; Maciel,Antônio J. da S.
O objetivo deste trabalho foi gerar metodologia para avaliar o processo de pulverização com a utilização das ferramentas da qualidade. Para tanto, foram listados os fatores primários, secundários e terciários e, com auxílio da ferramenta "check list", foram elaboradas as listas de checagem. Foram avaliados os fatores mão-de-obra, máquina, material, meio e método de 32 processos de pulverização, antes da aplicação de agrotóxicos, em que cada fator recebeu uma pontuação, tendo como somatória total 750 pontos. A pontuação média dos fatores mão-de-obra, máquina, material, meio e método foram 78; 211; 49; 20 e 94 pontos, respectivamente. Considerando a somatória dos pontos dos fatores para os 32 processos, o valor mínimo encontrado foi de 230 e o máximo de 620...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pulverizadores; Histogramas; Gráfico de controle.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200033

Uso da lógica fuzzy na caracterização do ambiente produtivo para matrizes gestantes
Provedor de dados: 70
Autores: Pandorfi,Héliton; Silva,Iran J. O.; Guiselini,Cristiane; Piedade,Sonia M. S.
O objetivo desta pesquisa consistiu na avaliação do ambiente de alojamento, estimando as condições favoráveis ao melhor desempenho de matrizes gestantes. O experimento foi realizado no período compreendido entre 4-1 e 11-3-2005, em propriedade de produção industrial de suínos, localizada no município de Elias Fausto - SP. A pesquisa foi desenvolvida no setor de gestação, com 24 matrizes primíparas, 12 fêmeas alojadas em baias individuais (T1) e 12 em baias coletivas (T2). O trabalho foi dividido em duas etapas, em função da forma de avaliação dos dados: análise bioclimática e da qualidade do ar, e estimativa dos padrões de conforto térmico ambiental. As variáveis bioclimáticas T (ºC), UR (%), Tgn (ºC) e fisiológicas, taxa respiratória (mov min-1) e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Conforto térmico; Lógica fuzzy; Suinocultura.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100001

Composted sewage sludge in replacement of mineral fertilization on wheat production and development
Provedor de dados: 70
Autores: KUMMER,ANA C. B.; GRASSI FILHO,HELIO; LOBO,THOMAZ F.; LIMA,RODOLLPHO A. DE S.
ABSTRACT Several research lines are required to ensure a proper disposal of sewage sludge in Brazil; among them, we may highlight agricultural use. In this sense, this study aimed at assessing the effect of exchanging nitrogen sourcing via conventional fertilization (chemical) with growing doses of composted sewage sludge (CSS) on wheat crop performance. The experiment was performed in a completely randomized design with seven treatments and ten replications, being defined as T0 (control – without fertilization); T1 (100% mineral fertilization); T2 (50% mineral + 50% CSS); T3, T4, T5, and T6 (100, 150, 200, and 250% nitrogen fertilizing from CSS). Results showed that the use of CSS increased wheat production and development, therefore enhancing its...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrogen; Organic fertilization; Production; Triticum aestivum.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400706

TYPES OF HEADER, OPERATING SPEED, AND GEOMETRY OF COLLECTION FRAMES ON THE TOTAL LOSSES OF SOYBEAN HARVEST
Provedor de dados: 70
Autores: Cortez,Jorge W.; Syrio,Marina G.; Rodrigues,Sonia A.
ABSTRACT Soybean has significant economic importance in Brazil despite high production costs, making it necessary to increase the efficiency of mechanized harvest through the reduction of losses. Thus, this study aimed to evaluate the total losses in the mechanized soybean harvest as a function of the combination of header types, operating speeds, and geometry of collection frames. The study was carried out in a commercial farm in a randomized block design arranged in a 2 × 3 × 3 factorial with 10 replications, totaling 180 replications. The data were analyzed by descriptive statistics, analysis of variance, and quality control. The square frame can be used instead of the rectangular frame for the determination of the total losses. The increasing operating...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural mechanization; Control charts; Glycine max.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400482

ADSORPTION OF ATRAZINE BY BIOCHARS PRODUCED FROM BYPRODUCTS OF THE WOOD INDUSTRY
Provedor de dados: 70
Autores: Fruehwirth,Marcelo; Sbizzaro,Mariana; Rosa,Danielle M.; Sampaio,Silvio C.; Reis,Ralpho R. dos.
ABSTRACT Atrazine is a herbicide widely used in agriculture; however, because of its toxicity, alternatives are needed to remove this compound from the environment. In this study, we investigated the adsorption process and the atrazine-adsorbing ability of three biochars produced at different pyrolysis temperatures from byproducts of the wood industry. The biochars were characterized by Fourier-transform infrared spectroscopy (FTIR) and scanning electron microscopy (SEM), and their physical characteristics were evaluated by Brunauer-Emmett-Teller (BET) analysis. The biochar pyrolyzed at 350 °C (BM350) adsorbed 26.04% of the herbicide, showing the best performance among the three biochars tested, even though it had the lowest specific surface area (1.467 m2...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water contamination; Isotherm; Functional groups; Kinetics models.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600769

Evaluation of sediment production and siltation in a small earth dam in Fernandópolis, SP
Provedor de dados: 70
Autores: Vanzela,Luiz S.; Grecco,Diego L. G.; Costa Neto,José N. da; Santos,Gilmar O.
The siltation is a natural process, but can be accelerated by human actions and results in major problems for the reservoirs, reducing its useful volume for irrigation. An example of this problem was the reduction of the area of mirror water of Fernandópolis municipal dam in 48.3% during 20 years. Therefore, this study aimed to evaluate the production of sediments and siltation of Fernandópolis municipal dam from a methodology that can be applied to small earth dams for agricultural purposes. For this, it was monitored, monthly throughout the year, the volume of sediment deposited in the reservoir. The percentage of retention sediment in Fernandópolis municipal dam ranged from 53.9 to 94.5%, that associated with a high specific sediment yield, will cause...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydro-sedimentology; Use and land occupation; Erosion.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500010

Sistema fuzzy para estimativa do bem-estar de matrizes pesadas
Provedor de dados: 70
Autores: Pereira,Danilo F.; Bighi,Camila A.; Gabriel Filho,Luís R.; Gabriel,Camila P. C.
Entender o comportamento e suas pequenas variações decorrentes das mudanças do ambiente térmico e desenvolver modelos que simulem o bem-estar a partir de respostas das aves ao ambiente constituem o primeiro passo para a criação de um sistema de monitoramento digital de aves em galpões de produção. Neste trabalho, foi desenvolvido um sistema de suporte à decisão com base na teoria dos conjuntos fuzzy para a estimativa do bem-estar de matrizes pesadas em função de frequências e duração dos comportamentos expressos pelas aves. O desenvolvimento do sistema passou por cinco etapas distintas: 1) organização dos dados experimentais; 2) apresentação dos vídeos em entrevista com "especialista"; 3) criação das funções de pertinência com base nas entrevistas e na...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lógica fuzzy; Bem-estar animal; Simulação; Termoneutralidade; Avicultura.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400002

THE TECHNOLOGICAL LEVEL OF AGRICULTURAL MECHANIZATION IN THE STATE OF CEARÁ, BRAZIL
Provedor de dados: 70
Autores: Albiero,Daniel; Xavier,Reuel S.; Garcia,Angel P.; Marques,Arthur R.; Rodrigues,Ruan L.
ABSTRACT Agricultural mechanization is a significant factor of agricultural modernization, but there are few data on the technological levels of this mechanization in the State of Ceará, Brazil. To study this topic, we designed a structured questionnaire, and interviews were conducted across the state. The survey data made it possible to calculate an index of agricultural mechanization technology and study hypotheses specific to farms of Ceará. The results indicate that the technology levels are different between farms of different sizes: large and medium farms are level I-M5 (automation), while small farms ranged from level IV-M1/M2 (primary/animal) to III-M3 (preliminary). We conclude that public policy for training should be directed at small farms....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural mechanization; Technological level; Technical efficiency; Economic development.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100133

Association of swine wastewater and mineral fertilization on black oat production
Provedor de dados: 70
Autores: Herrmann,Daniela da R.; Sampaio,Silvio C.; Castaldelli,Ana P. A.; Tsutsumi,Claudio Y.; Prior,Maritane.
ABSTRACT Swine wastewater (SW) has high organic load, becoming an important source of macro and micronutrients to plants, promoting the improvement of soil quality and development in various cultures. However, when done without agronomic and environmental criteria, it can cause soil problems, nutrient leaching, water resource damage and plant toxicity. The objective of this study was to evaluate the soil chemical properties and the leachate in face of the association of swine wastewater and mineral fertilization (MF) in oat cultivation. An experiment in drainage lysimeter was carried out, using SW applications associated to MF or not, where treatments consisted of doses of 0, 100, 200 and 300 m3ha-1 with the absence or presence of MF, under field...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil fertility; Nutrient leaching; Drainage lysimeters.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500799

Estudo da associação de água residuária de suinocultura e adubação mineral na cultura do milho e no solo
Provedor de dados: 70
Autores: Prior,Maritane; Sampaio,Silvio C.; Nóbrega,Lúcia H. P.; Dieter,Jonathan; Costa,Mônica S. S. de M.
RESUMO O uso de água residuária em solo agrícola pode-se caracterizar como uma fonte alternativa de adubação, além de melhorar as condições edáficas do solo devido à matéria orgânica adicionada. Neste contexto, este trabalho teve por objetivo avaliar os efeitos na cultura do milho e em Latossolo Vermelho distroférrico típico, devido à aplicação de água residuária de suinocultura associada com adubação química. No experimento, utilizou-se de cinco doses de ARS (0; 112,5; 225; 337,5 e 450 m3 ha-1) durante o ciclo do milho, combinadas com duas adubações químicas (50 e 75% da dose recomendada), para compor os respectivos tratamentos, com três repetições. Os parâmetros da cultura do milho avaliados foram: produtividade (PROD), altura de plantas (AP), teor de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reúso de água; Resíduo animal; Valorização agronômica.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400744

IRRIGATION STRATEGIES WITH WATER DEFICIT IN ‘TOMMY ATKINS’ MANGO TREE
Provedor de dados: 70
Autores: Santos,Marcelo R. Dos; Donato,Sérgio L. R.; Faria,Leandro N.; Coelho,Eugênio F.; Cotrim Junior,Paulo R. F.
ABSTRACT With the limited availability of water in semi-arid regions, it is necessary that irrigation is accurate and there is high water use efficiency. This study aimed to evaluate the regulated deficit irrigation (RDI) and partial rootzone drying (PRD) in yield, water use efficiency and gas exchange of ‘Tommy Atkins’ mango tree in semi-arid conditions. The experimental design was a randomized block with seven treatments for RDI under micro sprinkler and five treatments for the PRD under drip. Treatments were applied in phases PI - early blooming to early fruit expansion, PII - early expansion to early physiologic ripening and in phase III - physiologic ripening of fruits, with application of the RDI of 100, 75 and 50 % of ETc in different combinations...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mangifera; Water deficit; Water use efficiency.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601096

Balanço energético em galpão de frangos de corte
Provedor de dados: 70
Autores: Santos,Tânia M. B.; Lucas Júnior,Jorge de.
Com o objetivo de avaliar o fluxo de energia em galpão de frangos de corte, realizou-se estudo de balanço energético após acompanhamento de oito lotes de criação, em galpão comercial da empresa Frango Sertanejo, Sertãozinho - SP. Foi quantificado o poder calorífico de cada componente envolvido no processo de produção (direto e indireto, entradas e saídas), utilizando-os posteriormente para o cálculo do coeficiente de eficiência energética. Determinaram-se os consumos de ração (kg), produção de frango vivo (kg), aves mortas/descartadas (kg), produção de cama de frango (kg), água (L), gás liquefeito de petróleo - GLP (kg), energia elétrica (kWh), combustíveis (L), mão-de-obra (hora-homem), máquinas e implementos (horas) e instalações e equipamentos (m² e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogás; Eficiência energética; Fluxo de energia.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100004

SIMULATING CROP YIELD, SOIL NITROGEN, AND ORGANIC CARBON IN NO-TILLAGE CROP SEQUENCES IN A SUBTROPICAL CLIMATE IN BRAZIL
Provedor de dados: 70
Autores: Silva,Bruna de O.; Santos,Gustavo A. de A.; Santos,Miquéias G. dos; Morais Filho,Luiz F. F.; Faria,Rogério T. de.
ABSTRACT Brazil stands out worldwide for its high grain production in areas of direct sowing. The objective of this study was to simulate and assess the relationship of soil organic carbon content and nitrogen, crop yield, and biomass of two crop sequences under the no-tillage system in a subtropical region of São Paulo, Brazil, using CSM-CROPGRO-Soybean and CSM-CERES-Maize models. The modeling was carried out considering the meteorological conditions of Jaboticabal, SP, Brazil. The treatments consisted of combining two summer crops (maize and soybean) with maize cultivation as a winter crop. The average biomass and productivity for corn were 15594 kg ha−1 and 5996 kg ha−1, respectively, and for soybeans they were 5905 kg ha−1 and 3441 kg ha−1,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: CSM-CROPGRO; CSM-CERES-Maize; Conservationist tillage; Greenhouse gas emission.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400536

Desempenho dos modelos CLIGEN, LARS-WG e PGECLIMA_R na simulação de séries diárias de temperatura máxima do ar para localidades do estado do Paraná
Provedor de dados: 70
Autores: Virgens Filho,Jorim S. das; Oliveira,Rafael B. de; Leite,Maysa de L.; Tsukahara,Rodrigo Y.
Este trabalho teve o objetivo de avaliar o desempenho dos modelos CLIGEN, LARS-WG e PGECLIMA_R na simulação de séries diárias de temperatura máxima do ar para localidades do Estado do Paraná. Foram utilizadas séries históricas de temperatura máxima do ar das localidades de Campo Mourão, Castro, Curitiba, Ivaí, Londrina, Maringá e Paranaguá. Foram geradas cinco séries de temperatura máxima do ar para cada modelo, nas localidades avaliadas, que foram confrontadas com as respectivas séries históricas. O processo de validação foi composto de análises estatísticas através de testes de significância (sobre as médias mensais (teste t), sobre a variância das médias mensais (teste F), sobre a forma das distribuições de frequência (teste K-S)), de gráficos de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simuladores climáticos; Estatística climatológica; Clima do Paraná; Séries climáticas sintéticas.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300010

Armazenamento de soja em silos tipo bolsa
Provedor de dados: 70
Autores: Faroni,Lêda R. A.; Alencar,Ernandes R. de; Paes,Juliana L.; Costa,André R. da; Roma,Rafaela C. C.
Avaliaram-se as principais alterações qualitativas de soja armazenada em silos tipo bolsa e do óleo bruto extraído de soja com teores de água de 17,4% e 13,3%, armazenada em dois silos tipo bolsa, por 180 dias. Realizaram-se amostragens no dia do enchimento das bolsas, aos 30; 90 e 180 dias de armazenamento. Analisaram-se o teor de água, a condutividade elétrica, o percentual de germinação, a massa específica aparente da soja, além do teor de ácidos graxos livres e o índice de peróxido do óleo bruto extraído dela. Os teores de água da soja armazenada úmida e seca mantiveram-se próximos dos valores obtidos no início do período de armazenamento. Observou-se tendência de elevação da condutividade elétrica e decréscimo do percentual de germinação somente na...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Armazenamento hermético; Qualidade; Óleo bruto.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100010

DATA MINING FOR THE ASSESSMENT OF MANAGEMENT AREAS IN PRECISION AGRICULTURE
Provedor de dados: 70
Autores: Schemberger,Elder E.; Fontana,Fabiane S.; Johann,Jerry A.; Souza,Eduardo G. De.
ABSTRACT Precision Agriculture (PA) uses technologies with the aim of increasing productivity and reducing the environmental impact by means of site-specific application of agricultural inputs. In order to make it economically feasible, it is essential to improve the current methodologies as well as proposing new ones, in which data regarding productivity, soil, and compound indicators are used to determine Management Areas (MAs). These units are heterogeneous areas within the same region. With these methodologies, data mining (DM) techniques and algorithms may be used. In order to integrate DM techniques to PA, the aim of this study was to associate MAs created for soy productivity using the Fuzzy C-means algorithm by SDUM software over a 9.9-ha plot as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Algorithms; EM; KDD; K-means; Weka.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100185

Influência de nitrogênio amoniacal e vazão de ar no processo de nitrificação, etapa de tratamento de efluente de abatedouro de peixe
Provedor de dados: 70
Autores: Andrade,Lidiana; Kummer,Ana C. B.; Fazolo,Ajadir; Dasmaceno,Simone; Hasan,Salah D. M.
O efluente proveniente de abatedouro de peixes possui alto teor de nitrogênio, um dos principais causadores de eutrofização nos corpos d'água. Sua remoção pode ser feita em duas etapas separadas: nitrificação e desnitrificação. Este experimento teve como objetivo testar a influência da vazão de ar (valores de 1 a 3 L min-1) e a concentração de nitrogênio amoniacal (de 40 a 100 mg L-1) no processo de nitrificação. Foi utilizado um reator em batelada sequencial com biomassa imobilizada, com volume útil de 2,5 L, operado conforme delineamento composto central rotacional, em que as variáveis-resposta analisadas foram percentagem de conversão de nitrogênio amoniacal a nitrato e percentagem de acúmulo de nitrito. Os resultados mostraram, com intervalo de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Efluente anaeróbio; Remoção de nitrogênio; Nitrificação.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100017

Modelos para estimativa do subfator cobertura-manejo (CiII) relativo à erosão entressulcos
Provedor de dados: 70
Autores: Martins Filho,Marcílio V.; Engler,Marcela P. C.; Izidorio,Ricardo; Cotrin,Flávio B.; Serra,Eugênia A.; Amaral,Nailton S.; Souza,Zigomar M.
A análise de um modelo de erosão é um crítico passo no desenvolvimento de uma ferramenta de predição da erosão aplicável e válida; isso é crucial para avaliar o desempenho dos modelos existentes para assegurar que as estimativas de um modelo condizem com a realidade. O objetivo do presente trabalho foi avaliar modelos para a predição do subfator cobertura e manejo (CiII) relativo à erosão entressulcos. Um experimento fatorial completo foi conduzido com cinco doses de resíduo de milho (0; 0,05; 0,15; 0,40 e 0,80 kg m-2), quatro declives e duas repetições, sob condições de prévio umedecimento para determinar as taxas de erosão entressulcos (Di) e enxurrada (R). Num primeiro experimento, foi avaliada a erodibilidade entressulcos (Ki) e o subfator cobertura e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelagem; Chuva simulada; Cobertura do solo.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300012

Avaliação do desempenho de dois sistemas modulares no tratamento anaeróbio de esgotos em comunidades rurais
Provedor de dados: 70
Autores: Javarez Júnior,Antônio; Paula Júnior,Durval R. de; Gazzola,Jonathan.
Este trabalho apresenta uma alternativa de baixo custo e fácil instalação para o tratamento de esgotos de pequenas comunidades. O experimento foi desenvolvido no Campo Experimental da Faculdade de Engenharia Agrícola (FEAGRI/UNICAMP). O volume total de esgoto gerado na FEAGRI é de cerca de 20 m³ dia-1, sendo metade desse tratado pelos sistemas modulares. O sistema da linha (A) é constituído por um reator UASB (Upflow Anaerobic Sludge Blanket), seguido de dois filtros anaeróbios e o outro sistema, linha (B), é constituído por um reator tipo RAC (Reator Anaeróbio Compartimentado), seguido de dois filtros anaeróbios (FA). Os sistemas foram operados de dezembro de 2002 a fevereiro de 2004, totalizando 30 coletas de amostras. Observou-se que, de maneira geral,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas modulares; Reator anaeróbio; Tratamento de esgoto.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400024

Comparison measures of maps generated by geostatistical methods
Provedor de dados: 70
Autores: Dalposso,Gustavo H.; Uribe-Opazo,Miguel A.; Mercante,Erivelto; Johann,Jerry A.; Borssoi,Joelmir A.
This study uses several measures derived from the error matrix for comparing two thematic maps generated with the same sample set. The reference map was generated with all the sample elements and the map set as the model was generated without the two points detected as influential by the analysis of local influence diagnostics. The data analyzed refer to the wheat productivity in an agricultural area of 13.55 ha considering a sampling grid of 50 x 50 m comprising 50 georeferenced sample elements. The comparison measures derived from the error matrix indicated that despite some similarity on the maps, they are different. The difference between the estimated production by the reference map and the actual production was of 350 kilograms. The same difference...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Error matrix; Confusion matrix; Local influence.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100018

MANOBRAS DE SEMEADURA COM SISTEMA DE NAVEGAÇÃO
Provedor de dados: 70
Autores: Garcia,Luiz C.; Meer,Roderik W. Van Der; Souza,Nátali M. de; Justino,Altair; Weirich Neto,Pedro H.
Resumo Os sistemas de navegação por posicionamento global (GPS) estão cada vez mais presentes no campo, prometendo diminuir os custos operacionais do agricultor. O objetivo deste trabalho foi avaliar o tempo de manobra durante a operação de semeadura da soja sem e com sistema de navegação. O delineamento experimental foi inteiramente aleatorizado, com dois tratamentos e doze repetições. Os tratamentos consistiram no tempo das manobras feitas de modo convencional e utilizando-se do sistema de navegação por GPS acoplado num piloto automático. Avaliaram-se o tempo de manobra e o retorno econômico. As manobras realizadas com auxílio do sistema de navegação foram, em média, 49% mais rápidas do que as manobras realizadas de forma convencional. Houve economia de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Piloto automático; Viabilidade econômica.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200361

Perdas de nutrientes por erosão e sua distribuição espacial em área sob cana-de-açúcar
Provedor de dados: 70
Autores: Izidorio,Ricardo; Martins Filho,Marcílio V.; Marques Júnior,José; Souza,Zigomar M. de; Pereira,Gener T.
O presente trabalho teve como objetivo principal determinar as perdas de nutrientes por erosão em entressulcos, sulcos e global (entressulcos + sulcos, A), em área cultivada com cana-de-açúcar submetida à queima da palhada na sua pré-colheita, na Fazenda Santa Bárbara, localizada em Guariba - SP, sob um Latossolo Vermelho eutroférrico (LVef). Parcelas experimentais foram submetidas à chuva simulada com intensidade de 80 mm h-1, durante 65 minutos. Análises do sedimento erodido indicaram altas taxas de enriquecimento: 1,62 (matéria orgânica, MO); 4,30 (P); 1,17 (K); 1,33 (Ca) e 1,24 (Mg) vezes em relação ao solo original. As perdas de solo e nutrientes, em função do tipo de erosão, obedeceram à seguinte ordem: sulcos &gt; global &gt; entressulcos. Análises...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão em entressulcos; Erosão em sulcos; Geoestatística.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300011

Comparação de três receptores GPS para uso em agricultura de precisão
Provedor de dados: 70
Autores: Stabile,Marcelo C. C.; Balastreire,Luiz A.
Diversos equipamentos que se utilizam dos sinais transmitidos pelo Sistema de Posicionamento Global (GPS) têm sido empregados na Agricultura de Precisão. Neste estudo, foi feita uma comparação de três receptores comerciais no intuito de verificar suas acurácias. As principais qualidades medidas foram a repetibilidade dos dados e a estabilidade do sistema. O estudo foi conduzido em campo aberto, na área experimental da ESALQ/USP, com três linhas paralelas de 50 m espaçadas 10 m entre si. A coleta de dados foi feita no dia 25-9-2002, totalizando seis repetições da comparação dos três sistemas. Os dados foram coletados simultaneamente, de acordo com a melhor configuração da constelação de satélites, sendo que os três sistemas apresentaram resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; GPS; Precisão de posicionamento.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100024

Desempenho operacional de uma semeadora-adubadora de precisão, em função do preparo do solo e do manejo da cobertura de inverno
Provedor de dados: 70
Autores: Furlani,Carlos E. A.; Gamero,Carlos A.; Levien,Renato; Lopes,Afonso; Silva,Rouverson P. da.
Avaliou-se o desempenho operacional de campo de uma semeadora-adubadora de precisão, equipada com seis linhas espaçadas de 550 mm, em um solo muito argiloso, classificado como Nitossolo Vermelho Distrófico Latossólico, na semeadura do feijoeiro (Phaseolus vulgaris L.). Os tratamentos consistiram de três métodos de preparo do solo: a) convencional (uma aração com arado de discos e duas gradagens niveladoras); b) escarificação (uma passagem de escarificador conjugado com rolo destorroador), e c) semeadura direta. Esses procedimentos foram combinados com quatro condições de cobertura do solo no inverno (consórcio aveia-preta + nabo forrageiro manejados com rolo-faca, triturador de palhas, herbicida e solo em pousio). Os métodos de preparo do solo e os manejos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Força de tração; Consumo de combustível; Feijão.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200018

ERRATA
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300571

Water consumption when exposed to sun and shade for native goats in the semiarid of the State of Paraiba, Brazil
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Leite,Jackson R. de S.; Nascimento,Jose W. B. do; Leal,Antonio F.; Silva,Andrea S.
This work aimed to evaluate the preference and water consumption of native goats in the semiarid of Brazil. The water was freely supplied, in individual buckets, one exposed to the sun and the other in the shade. The experiment was realized using 18 animals of Moxotó, Graúna and Azul breeds, with average weight of 16,6 ± 2,4 kg, kept in confinement in individual stalls equipped with feeders and drinkers, during the period from January to February of 2009. The water temperature was measured by sensors (thermocouples type T - copper/constantan), which were coupled to a system of data acquisition. It was observed that the average water temperature exposed to the sun was 29.02 ºC, and 23.85 ºC in the shade. For all breeds there was a preference for the water...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Goats behavior; Native breeds; Water temperature.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100003

SOFTWARE TO ASSESS BEEF CATTLE BODY MASS THROUGH THE FUZZY BODY MASS INDEX
Provedor de dados: 70
Autores: Gabriel Filho,Luís R. A.; Putti,Fernado F.; CREMASCO,CAMILA P.; BORDIN,DEYVER; Chacur,Marcelo G. M.; Gabriel,Luiz R. A.
ABSTRACT The Body Mass Index (BMI) can be used by farmers to help determine the time of evaluation of the body mass gain of the animal. However, the calculation of this index does not reveal immediately whether the animal is ready for slaughter or if it needs special care fattening. The aim of this study was to develop a software using the Fuzzy Logic to compare the bovine body mass among themselves and identify the groups for slaughter and those that requires more intensive feeding, using "mass" and "height" variables, and the output Fuzzy BMI. For the development of the software, it was used a fuzzy system with applications in a herd of 147 Nellore cows, located in a city of Santa Rita do Pardo city – Mato Grosso do Sul (MS) state, in Brazil, and a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Computer system; IMC; Mamdani and profits.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100179

USE OF ACTIVE OPTICAL SENSOR IN THE CHARACTERISTICS ANALYSIS OF THE FERTIGATED BRACHIARIA WITH TREATED SEWAGE
Provedor de dados: 70
Autores: Santos,Gilmar O.; Rosalen,David L.; Faria,Rogério T. de.
ABSTRACT Through the use of remote sensing, the productivity and the nutritional state of the plants can be estimated in relation to the nitrogen doses due to the modification of the canopy reflectance. In this study, values of the normalized difference vegetation index (NDVI) obtained by a terrestrial optical sensor were correlated with productivity and contents of nitrogen (N) and of foliar crude protein (CP) of Brachiaria brizantha cv. Marandu, fertigated with doses of sewage treatment effluent (STE) The NDVI average rates of the forage were obtained by the active terrestrial sensor (GreenSeeker) before the harvests that were realized every 28 days in 2014. Five fertigated treatments with the following fractions of STE in water were evaluated: E5 = 1.0;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Forage production estimation; GreenSeeker; Terrestrial remote sensing.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601213

Comportamento operacional de associações entre sulcadores e discos de corte para sistema de semeadura direta
Provedor de dados: 70
Autores: Francetto,Tiago R.; Alonço,Airton dos S.; Bellé,Mateus P.; Franck,Cristian J.; Carpes,Dauto P.
O objetivo foi avaliar o desempenho operacional quanto ao requerimento de tração, consumo energético e eficiência de trabalho de associações entre elementos de corte dos resíduos culturais e de rompedores do solo, em função da velocidade de deslocamento. Este trabalho foi realizado em propriedade agrícola situada no município de Santa Maria (RS), em solo classificado como Argissolo Vermelho e textura francoarenosa. O experimento foi composto por 24 combinações de tratamentos, em um esquema fatorial de 2x3x4. Estes foram obtidos pela interação dos fatores sulcadores (haste e disco), discos de corte (sem disco, liso e ondulado) e velocidades (1,11; 1,67; 2,22 e 2,78 m s-1). Os dados de desempenho do trator foram adquiridos com a utilização de instrumentação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semeadora-adubadora; Relação máquina-solo; Ensaio de máquinas agrícolas; Haste sulcadora; Discos duplos desencontrados; Mecanismo de corte.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300542

Níveis de irrigação e de composto de lixo orgânico na formação de mudas cítricas em casa de vegetação
Provedor de dados: 70
Autores: Fachini,Emerson; Galbiatti,João A.; Pavani,Luiz C.
O presente trabalho visou a estudar o efeito da associação entre a irrigação e tipos de substratos na formação de mudas de laranjeira. O delineamento experimental utilizado foi o de blocos casualizados, com parcelas subdivididas, com quatro repetições, três níveis de irrigação e cinco tipos de substratos. Foram utilizados os seguintes substratos: 100% de casca de pínus; 80% de casca de pinus + 20% de composto de lixo orgânico; 60% de casca de pinus + 40% de composto de lixo orgânico; 20% de casca de pinus + 80% de composto de lixo orgânico, e 100% de composto de lixo orgânico. A irrigação por gotejamento foi feita com lâminas de 50%, 100% e 150% da evaporação do atmômetro modificado. A avaliação do desenvolvimento das plantas foi feita quinzenalmente,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Substratos; Mudas cítricas.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300010

Caracterização analítica e geométrica da metodologia geral de determinação de distribuições de Weibull para o regime eólico e suas aplicações
Provedor de dados: 70
Autores: Gabriel Filho,Luís R. A; Cremasco,Camila P; Seraphim,Odivaldo J; Caneppele,Fernando de L.
O regime eólico de uma região pode ser descrito por distribuição de frequências que fornecem informações e características extremamente necessárias para uma possível implantação de sistemas eólicos de captação de energia na região e consequentes aplicações no meio rural em regiões afastadas. Estas características, tais como a velocidade média anual, a variância das velocidades registradas e a densidade da potência eólica média horária, podem ser obtidas pela frequência de ocorrências de determinada velocidade, que por sua vez deve ser estudada através de expressões analíticas. A função analítica mais adequada para distribuições eólicas é a função de densidade de Weibull, que pode ser determinada por métodos numéricos e regressões lineares. O objetivo deste...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Função de densidade; Velocidade eólica; Potência eólica.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100006

Teor de água limite para crioconservação de sementes de romã (Punica granatum L.)
Provedor de dados: 70
Autores: SILVA,LUZIA M. DE M.; MATA,MARIO E. R. M. C.; DUARTE,MARIA E. M.
Tradicionalmente, a determinação das condições ideais para a conservação de sementes é obtida através de experimentos que estudam a combinação dos fatores: teor de água e temperatura de armazenamento, monitorando a viabilidade das sementes ao longo do tempo. Ante o exposto, objetivou-se determinar o Teor de Água Limite para Crioconservação das sementes de romã, quando armazenadas nas temperaturas de -170 e -196 °C. As sementes passaram por um processo de umedecimento e secagem até atingirem os teores de água de 4; 6; 8; 10; 12 e 14% b.u.; logo após, foram crioconservadas durante cinco dias e, em seguida, descongeladas gradativamente nas temperaturas de -196, -170, -80, 10 ºC e ambiente, com intervalo de 3 horas para cada temperatura, para então serem...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sementes; Armazenamento criogênico; Qualidade fisiológica.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200313

TIMES OF EFFICIENCY AND QUALITY OF SOYBEAN CROP MECHANICAL OPERATION IN GEOMETRY FUNCTIONS OF PLOTS
Provedor de dados: 70
Autores: Paixão,Carla S. S.; Santos,Adão F. dos; Voltarelli,Murilo A.; Silva,Rouverson P. da; Carneiro,Franciele M.
ABSTRACT The knowledge of the operational quality of soybean harvester provides useful information to management in order to obtain the maximum performance of all available resources, with minimal expenses. The aimed of this study was to evaluate the quality of mechanized soybean harvesting operation in different formats of plots through statistical process control. Treatments were established from the formats of existing plots in the area (irregular, trapezoidal and rectangular). The activities carried out during the harvest were monitored (harvesting, unloading, handling, maneuvering and climate charts) and through these activities were made the calculation of capacity and harvesting operation efficiencies. In the determination of total losses were used...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Grain harvester; CUSUM; Machine performance; Glycine max (L.) Merrill.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100106

Ocorrência de veranicos no estado do Rio de Janeiro
Provedor de dados: 70
Autores: Cruz,Eleandro S.; Carvalho,Daniel F.; Ceddia,Marcos B.; Antunes,Mauro A. H.; Aquino,Renato M.
O objetivo deste trabalho foi simular veranicos com diferentes durações e identificar suas respectivas probabilidades de ocorrência para dezembro, janeiro e fevereiro no Estado do Rio de Janeiro. Para isso, foram utilizadas séries históricas pluviométricas, com período base de 16 anos referentes a 40 estações localizadas no Estado do Rio de Janeiro, 15 em Minas Gerais, 4 no Espírito Santo e 3 em São Paulo. Com os resultados obtidos, pôde-se concluir que, em geral, as maiores probabilidades de ocorrência de veranicos são previstas para o mês de dezembro, diminuindo para janeiro e, em seguida, para fevereiro. Os veranicos com durações de 1-5 dias e 6-10 dias ocorreram com maior probabilidade no Estado. A maior probabilidade de ocorrência de veranicos com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dias secos; Simulação.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100009

Demanda de potência de uma semeadora com dois tipos de sulcadores em áreas compactadas pelo pisoteio de animais no sistema integração lavoura-pecuária
Provedor de dados: 70
Autores: Andreolla,Veruschka R. M.; Gabreil Filho,Antonio.
O objetivo deste trabalho foi avaliar a potência requerida na barra de tração do trator por uma semeadora com dois tipos de elementos sulcadores, na semeadura da soja, em áreas compactadas pelo pisoteio de animais em sistema de integração lavoura-pecuária. Foi utilizado o delineamento em parcela subdividida inteiramente casualizado, sendo os tratamentos principais compostos de solo úmido com pastejo, solo seco com pastejo e solo sem pastejo, e nos secundários foram utilizados sulcadores de haste ou discos duplos. Foram avaliadas a densidade e a resistência do solo à penetração, a força de tração exercida pela semeadora, a velocidade e a potência requerida na barra de tração do trator. As alterações no solo causadas pelo pisoteio do gado não foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Máquinas agrícolas; Tração; Soja.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300014

Performance of small wind turbines: simulation of electricity supply to loads connected to the public or isolated grid
Provedor de dados: 70
Autores: Rodrigues,Rafael V.; Rossi,Luiz A.
ABSTRACT The successful in the implementation of wind turbines depends on several factors, including: the wind resource at the installation site, the equipment used, project acquisition and operational costs. In this paper, the production of electricity from two small wind turbines was compared through simulation using the computer software HOMER - a national model of 6kW and an imported one of 5kW. The wind resources in three different cities were considered: Campinas (SP/BR), Cubatão (São Paulo/BR) and Roscoe (Texas/ USA). A wind power system connected to the grid and a wind isolated system - batteries were evaluated. The results showed that the energy cost ($/kWh) is strongly dependent on the windmill characteristics and local wind resource. Regarding...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Homer; Wind power; Electricity.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200281

ESTIMATION OF FUEL CONSUMPTION IN AGRICULTURAL MECHANIZED OPERATIONS USING ARTIFICIAL NEURAL NETWORKS
Provedor de dados: 70
Autores: Borges,Pedro H. M.; Mendoza,Zaíra M. S. H.; Maia,João C. S.; Bianchini,Aloísio; Fernándes,Haroldo C.
ABSTRACT This study aimed to develop artificial neural networks for the estimation of tractor fuel consumption during soil preparation, according to the adopted system. The multilayer perceptron network was chosen. As input data: the soil mechanical penetration resistance, the mobilized area by implements, the working gear and the tractor engine speed. The number of layers and neurons varied to form different architectures. The adjustment was verified based on various statistical criteria. The values estimated by the networks did not differ significantly from those obtained experimentally. The conclusion was that the networks showed adequate reliability and accuracy to predicting the fuel consumption in each tillage system, in function of the input data...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Machine performance; Artificial intelligence; Agricultural planning.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100136

QUALITY OF A DIGITAL TERRAIN MODEL FOR SANTA CATARINA STATE
Provedor de dados: 70
Autores: Caten,Alexandre Ten; Dalmolin,Ricardo S. D.; Boeing,Evandro L.; Vitalis,Fernando A.; Silva,Walquíria C. Da.
ABSTRACT: Relief characterization using a digital terrain model (DTM) is widely applied in erosion, soil and vegetation modeling. However, factors, such as acquisition technology and the spatial resolution of the digital model, affect modeling results. The aim of this study was to characterize noises in a DTM of the entire state of Santa Catarina recently made available through the state's Sustainable Economic Development Secretary and to evaluate different methods of interpolation and smoothing of the original 1 m resolution to a new digital model with a spatial resolution of 15 m. Using the SAGA GIS program, spurious data that appeared as peaks and sinks were removed from the digital model. Of five processing procedures, the following three were used for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digital elevation model; Geomorphometry; Slope; Digital soil mapping; Aerial imagery.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601261

CORRELATIONS AMONG VEGETATION INDICES AND PEANUT TRAITS DURING DIFFERENT CROP DEVELOPMENT STAGES
Provedor de dados: 70
Autores: Carneiro,Franciele M.; Furlani,Carlos E. A.; Zerbato,Cristiano; Menezes,Patricia C. de; Gírio,Lucas A. da S.
ABSTRACT Active optical sensors have been widely used for the spatial and temporal monitoring of peanut culture because they are accurate, non-destructive methods for rapidly obtaining data. The objective of this study was to determine the optimal stage of crop growth for collecting sensor readings based on correlations between quality indicators. In addition, we compared vegetation indices (Normalized Difference Vegetation Index [NDVI], Normalized Difference Red-Edge Index, [NDRE], and Inverse Ratio Vegetation Index, [IRVI]) by monitoring temporal variability in the peanut crop in order to determine which of them obtained the best reading quality throughout the process. The experiment was performed on the 2016/17 crop in the agricultural area of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Remote sensing; Arachis hypogaea L.; Control charts; Precision agriculture.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800033

BIOGAS PRODUCTION IN DAIRY CATTLE SYSTEMS, USING BATCH DIGESTERS WITH AND WITHOUT SOLIDS SEPARATION IN THE SUBSTRATES
Provedor de dados: 70
Autores: Anjos,Isis Dos; Toneli,Juliana T. C. L.; Sagula,Alex L.; Lucas Junior,Jorge de.
ABSTRACT This research aimed to evaluate the biogas production during the anaerobic biodigestion process of dairy cattle manure, with and without solids separation. Sixteen biodigesters of the batch type were used, each one with 2L of capacity, supplied with manure in four different conditions: (1) pure manure, after washing the floors of the free stall system; (2) manure after the solids separator; (3) manure after the solids separator and sand decanter and (4) manure with the solid retained in separator solids, dissolved in water. The hydraulic retention time was of 196 days. The highest reductions of volatile solids (VS) were obtained for the biodigesters supplied with manure that went through some process of solids separation. The highest potential of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogas; Biodigester; Manure; Dairy cattle; Solid separation.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300426

Propriedades mecânicas dos grãos de soja em função do teor de água
Provedor de dados: 70
Autores: Ribeiro,Deise M.; Corrêa,Paulo C.; Furtado,Bruno F.; Goneli,André L. D.; Resende,Osvaldo.
O presente trabalho teve como objetivo verificar a influência do teor de água nos valores da força máxima de compressão para uma deformação fixa (2 mm) e do módulo proporcional de deformidade de grãos de soja submetidos à compressão em diferentes posições. Foram utilizados grãos com teores de água variando de 0,58 a 0,093 (b.s.), comprimidos uniaxialmente entre duas placas paralelas, na direção de suas três dimensões principais, sob velocidade de compressão de 0,001 m s-1. A partir dos resultados obtidos, concluiu-se que a força de compressão e o módulo proporcional de deformidade diminuem com o aumento do teor de água. Além disso, os grãos de soja apresentam maior resistência à compressão quando submetidos a esforços na posição de repouso (P1),...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Propriedades reológicas; Módulo proporcional de deformidade; Secagem.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300019

Avaliação por fotointerpretação das áreas de abrangência dos diferentes estados da erosão acelerada do solo em canaviais e pomares de citros
Provedor de dados: 70
Autores: Politano,Walter; Pissarra,Teresa C. T.
Este estudo foi realizado com o objetivo de avaliar os estados de erosão acelerada do solo presente em áreas com canaviais e pomares de citros localizados na região administrativa de Ribeirão Preto - SP. Foram empregadas fotografias aéreas verticais, na escala aproximada de 1:40.000, do vôo da cobertura aerofotográfica da região citrícola do Estado de 1988. O estudo foi realizado identificando-se e delimitando-se todas as áreas de abrangência de cinco estados da erosão acelerada do solo presentes nos canaviais e pomares de citros. A presença da erosão acelerada severa a extremamente severa foi constatada tanto nos canaviais como nos pomares de citros, nas quatro unidades de solos de ocorrências principais na área de estudo. Os valores da extensão total das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão acelerada; Cana-de-açúcar; Cultura de citros.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100027

Resistência específica do solo de um pomar frutícola relacionada ao manejo entrelinhas e intensidade de tráfego
Provedor de dados: 70
Autores: Draghi,Laura; Jorajuría,Daniel; Cerrisola,Cecilia; Márquez Delgado,Luis.
O tráfego necessário à exploração de pomar frutícola tem características que se denominam "tráfego controlado", já que se realiza sempre sobre os mesmos caminhos do espaço entrelinhas. No alto Valle do Rio Negro, Argentina, a essa situação deve ser agregado, como fator de predisposição das sobrecompactações, o fato de que ocorre com freqüência um excesso de irrigação, que obriga ao tráfego sobre um solo úmido e, portanto, com baixa capacidade de suporte e alta predisposição à compactação. O presente trabalho teve o objetivo de estabelecer a possibilidade de sustentabilidade do sistema produtivo, que se conseguiria com a redução do tráfego resultante das mudanças das aplicações fitossanitárias de calendário fixo, pelas propostas no Projeto Frutícola...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compactação dos solos; Tráfego do solo; Resistência à penetração.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200012

THE USE OF ARTIFICIAL INTELLIGENCE FOR ESTIMATING SOIL RESISTANCE TO PENETRATION
Provedor de dados: 70
Autores: Pereira,Tonismar dos S.; Robaina,Adroaldo D.; Peiter,Marcia X.; Torres,Rogerio R.; Bruning,Jhosefe.
ABSTRACT The aim of this study was to present and to evaluate methodologies for the estimation of soil resistance to penetration (RP) using artificial intelligence prediction techniques. In order to do so, a data base with values of physical-water characteristics of the soils available in the literature was used, and the performances of Artificial Neural Networks (ANN) and Support Vector Machines (SVM) were evaluated. The models generated from the ANNs were implemented through the multilayer perceptron with backpropagation algorithm of Matlab software, varying the number of neurons in the input and intermediate layers. For the procedure from SVM, the RapidMiner software was used, varying input variables, the kernel function and the coefficients of these...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Machine learning; Support vector machines; Artificial neural networks.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100142

Sanitary quality of broiler litter reused
Provedor de dados: 70
Autores: Vieira,Maria de F. A.; Tinoco,Ilda de F. F.; Santos,Bernadete M. dos; Inoue,Keles R. A.; Mendes,Múcio A. dos S. A.
ABSTRACT Considering the importance of the substrate to bedding in the poultry industry in Brazil, and the enormous pressure on environmental management as to the correct use and management of the waste generated by the production sector, this study aimed to analyze the effect of reuses of two types of litter on sanitary qualities and productive performance of broilers. The study was conducted with litter from 32 different broiler houses, two types of substrates and four cycles of reuses. The litter sanitary quality was verified by the identification of the presence of Escherichia coli and Salmonellaspp. and the incidence of footpad dermatitis. It was observed that the coffee hulls litter presented a reduction of 28.61 percentage points in the probability...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Salmonella spp.; E. coli; Footpad; Productive performance.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500800

Use of active canopy sensors to discriminate wheat response to nitrogen fertilization under no-tillage
Provedor de dados: 70
Autores: KAPP JUNIOR,CLAUDIO; GUIMARÃES,ALAINE M.; CAIRES,EDUARDO F.
ABSTRACT Spectral reflectance sensors may be useful in discriminating biomass and nitrogen status in plants. A field experiment was carried out on a loamy Typic Hapludox under no-tillage in Ponta Grossa, Parana State, Brazil, aiming to evaluate the efficiency of active canopy sensors (GreenSeeker 505 and Crop Circle ACS-470) to discriminate wheat response to nitrogen fertilization by determining the dry mass, nitrogen status, and grain yield. A randomized complete block design was used and four treatments were replicated 12 times. The treatments consisted of nitrogen application, as urea, at the rates of 0, 50, 100, and 150 kg ha-1. The nitrogen rates were applied in topdressing at tillering of wheat crop. The readings from the sensors were sensitive to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Triticum aestivum L.; GreenSeeker; Crop Circle; NDVI.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500886

Financial losses in pork supply chain: a study of the pre-slaughter handling impacts
Provedor de dados: 70
Autores: REIS,JOÃO G. M. DOS; MACHADO,SIVANILZA T.; SANTOS,RODRIGO C.; NÄÄS,IRENILZA DE A.; OLIVEIRA,RONE V.
Brazil is amongst the world’s largest swine producers. However, its competitiveness has been vulnerable due to a lack of cooperation between the supply chain players. This condition makes the financial losses to be evaluated taking into account only an individual node, and most of the time, these damages are imputed by swine breeders. Living weight losses occur between the farm to slaughterhouses, and the main cause of these losses is the pre-slaughter handling, especially during animal transportation. In this research, we analyzed the pre-slaughter handling in a swine farm in Brasilândia, MS, Brazil. Analyzed data were provided by five slaughterhouses (farm clients) from the studied region, in which it was considered living weight losses, carcass...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Supply chain management; Pork production; Economic impact.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100163

Depósito de pulverização com diferentes padrões de gotas em aplicações na cultura do algodoeiro
Provedor de dados: 70
Autores: Souza,Reginaldo T. de; Castro,Rogério D. de; Palladini,Luiz A.
Com os objetivos de avaliar a deposição da calda de pulverização sobre plantas de algodão e a eficiência da pulverização com diferentes padrões de gotas sob condições adversas de temperatura e umidade, realizou-se um experimento para a determinação dos volumes de depósitos da pulverização no final de ciclo da cultura. O trabalho foi executado com pulverizador automotriz, equipado com pontas JA3 (jato cônico vazio) e jato plano com indução a ar AD-IA/D 11003 (duplo), AD-IA 11003 que, na pressão trabalhada, proporcionaram volume de aplicação de 150 L ha-1, e a ponta AD-IA 11004 que, na mesma pressão, proporcionou volume aplicado de 200 L ha-1. Para a determinação dos volumes depositados nas folhas do terço superior, médio e inferior das plantas de algodão,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Deposição; Traçantes; Algodão.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200011

Potassium distribution in drip irrigation with fertigation for different injection distances in the main line
Provedor de dados: 70
Autores: Bomfim,Guilherme V. do; Manzano,Juan; Azevedo,Benito M. de; Vasconcelos,Denise V.; Viana,Thales V. de A.
The purpose of this research was to evaluate the K2O distribution uniformity by surface drip irrigation at Universitat Politecnica de Valencia, Valencia, Spain (39º 29′ N, 0º 23′ W, 20 m). The irrigation was performed by drip lines with not-compensated emitters, spaced 0.3 m. The fertigation was realized using a fertilizer injector pump of electric action with injection of 0.25 h. The experimental design used completely randomized blocks with five treatments and four replications. The treatments consisted of injection in five distances, located at 10; 20; 30; 40; 50 m of the first drip line. Samples were collected in emitters located at the start, at 1/3, at 2/3 and at the end of the drip lines. The nutrient concentration was determined by flame...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Uniformity; Chemigation; K2O.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600011

Desempenho produtivo e retorno econômico da cultura do sorgo submetida à irrigação deficitária
Provedor de dados: 70
Autores: Zwirtes,Anderson L.; Carlesso,Reimar; Petry,Mirta T.; Kunz,Junior; Reimann,Guilherme K.
RESUMO A irrigação deficitária é comumente utilizada em regiões de reduzida disponibilidade de água ou de energia para a irrigação e visa incrementar a eficiência de uso da água. Essa técnica pode ser adequada à cultura do sorgo, que apresenta produtividades satisfatórias, mesmo em condições limitadas de disponibilidade de água no solo. Os objetivos do trabalho foram: avaliar os efeitos de diferentes manejos de irrigação deficitária sobre o índice de área foliar, altura de plantas e rendimento de grãos do sorgo, e identificar o nível crítico de irrigação deficitária que proporciona maior produtividade da água irrigada e retorno econômico. O experimento foi desenvolvido no ano agrícola de 2012/2013, sob uma cobertura móvel, que impedia a ocorrência de chuva...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiração da cultura; Produtividade da água irrigada; Sorghum bicolor.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400676

MANAGEMENT SYSTEMS: SOIL COVER AND COMPACTION, LONGITUDINAL DISTRIBUTION, AND YIELD OF SOYBEAN CROP
Provedor de dados: 70
Autores: Cortez,Jorge W.; Pusch,Maiara; Silva,Rouverson P. da; Rufino,Mauricio V.; Anghinoni,Matheus.
ABSTRACT The way the soil is managed can influence its structuring and, consequently, crop yield. Thus, this study aimed to evaluate the effect caused by the management systems plowing followed by two intermediate harrowing operations, intermediate harrowing, chiseling, chiseling followed by intermediate harrowing, cross chiseling followed by intermediate harrowing, and non-tillage on soil and agronomic attributes of the soybean crop. A randomized block design with four replications was used. The percentage of soil cover, soil resistance to penetration, number of plants per meter, longitudinal distribution of seedlings, and soybean yield were evaluated. The data were submitted to analysis of variance by the Tukey test at 5% probability, and use of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resistance to penetration; Geostatistics; Soil tillage.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400490

Viabilidade econômica de aquisição de um silo-secador para pequenas áreas de produção
Provedor de dados: 70
Autores: Jasper,Samir P.; Biaggioni,Marco A. M.; Ribeiro,Jader P.
O objetivo deste trabalho foi avaliar, por meio de simulação econômica, a viabilidade de aquisição de um silo-secador, para pequenas propriedades rurais, tendo como referências as opções de terceirizar o processo de secagem/armazenagem ou a comercialização do milho úmido. Em virtude da alta diversificação encontrada nas pequenas propriedades rurais, a simulação foi realizada considerando-se diferentes tamanhos de áreas exploradas com milho (10; 20; 30 e 40 ha), níveis de produtividade (3.900; 4.500 e 5.100 kg ha-1) e preços por saca de milho (R$ 13,03; R$ 19,69 e R$ 34,29), no Estado de São Paulo. Comparando as rentabilidades obtidas, notou-se a superioridade da receita líquida na aquisição do silo secador nas áreas de produção de 20 ha com produtividade...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Silo secador; Milho; Simulação econômica.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300017

TRANSPORT PARAMETERS OF POTASSIUM FROM DIFFERENT SOURCES IN SOIL COLUMNS
Provedor de dados: 70
Autores: Vilela,Nathane M. S.; Thebaldi,Michael S.; Leal,Bruno De P.; Silva,Ascânio V.; Martins,Ivani P.
ABSTRACT This study aimed to determine some transport parameters of potassium in soil columns by miscible displacement of effluent from a Sewage Treatment Plant (STP). This effluent was collected at different stages of treatment, and potassium chloride solutions were prepared with the same K pulse concentration as the effluent. They were used to conduct a miscible displacement experiment of potassium in soil columns of dystrophic Red Latosol. Both types of solutions contained concentrations of 30 and 32 mg L-1 of potassium. STANMOD software was used to obtain the retardation factor (R) and the Peclet number (Pe) from pore volume and relative concentration. Both retardation factor and solid-water partition coefficient of the soil showed significant results...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Breakthrough curves; Environmental contamination; Miscible displacement.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100135

Temporal variability of soil CO2 emission after conventional and reduced tillage described by an exponential decay in time model
Provedor de dados: 70
Autores: Teixeira,Luis G; Lopes,Afonso; La Scala Jr,Newton.
To study Assessing the impact of tillage practices on soil carbon losses dependents it is necessary to describe the temporal variability of soil CO2 emission after tillage. It has been argued that large amounts of CO2 emitted after tillage may serve as an indicator for longer-term changes in soil carbon stocks. Here we present a two-step function model based on soil temperature and soil moisture including an exponential decay in time component that is efficient in fitting intermediate-term emission after disk plow followed by a leveling harrow (conventional), and chisel plow coupled with a roller for clod breaking (reduced) tillage. Emission after reduced tillage was described using a non-linear estimator with determination coefficient (R²) as high as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil respiration; Soil CO2 emission; Soil tillage; Greenhouse effect.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200004

Avaliação de danos mecânicos causados em banana "Nanicão" durante as etapas de beneficiamento, transporte e embalagem"
Provedor de dados: 70
Autores: Sanches,Juliana; Leal,Paulo A. M.; Saravali,José H.; Antoniali,Silvia.
Este estudo teve como objetivo a avaliação de danos mecânicos ocorridos na banana "Nanicão" durante o processo de beneficiamento, transporte, embalagem e distribuição, identificando os prováveis pontos críticos. Avaliaram-se os danos mecânicos causados após o transporte, despistilagem e primeira despenca; limpeza e classificação; acondicionamento nas embalagens e transporte, e amadurecimento. As embalagens estudadas foram: embalagem de madeira torito (18 kg), madeira tipo ½ caixa (13 kg) e papelão (18 kg). Verificou-se que, na etapa de acondicionamento e transporte das frutas até o centro de distribuição, duplicaram os defeitos leves e os defeitos graves quintuplicaram, causando podridões após a climatização. A embalagem de papelão não suportou o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Musa cavendishii; Qualidade; Injúrias.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100022

Avaliação do nível de ruído em colhedoras combinadas
Provedor de dados: 70
Autores: Silva,Rouverson P. da; Fontana,Gustavo; Lopes,Afonso; Furlani,Carlos E. A.
O presente trabalho teve o objetivo de determinar os níveis de pressão sonora nas cabines de colhedoras combinadas, por meio do uso de um medidor de nível de pressão sonora. Foram avaliadas as colhedoras New Holland TC-57, SLC 6200 e Massey Ferguson 3640, sendo determinado o nível de ruído na cabine do operador. O delineamento adotado foi o inteiramente casualizado, com 12 tratamentos e três repetições. Os resultados obtidos evidenciam que todas as colhedoras estudadas apresentaram ruído acima do nível máximo estabelecido pelas normas técnicas.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ruído; Colhedoras de grãos; Cabines.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200017

Influência da precipitação no escoamento superficial em uma microbacia hidrográfica do Distrito Federal
Provedor de dados: 70
Autores: Alencar,Danielle B. S. de; Silva,Cícero L. da; Oliveira,Carlos A. da S.
O conhecimento do escoamento superficial é importante para o dimensionamento de obras hidráulicas e para a conservação da água e do solo. O volume de água escoado superficialmente depende de fatores de natureza edafoclimática e fisiográfica da região. O objetivo deste estudo foi verificar a influência relativa do total precipitado (P), da precipitação antecedente (PA) e da intensidade de precipitação (IP) na ocorrência de eventos de escoamento superficial (Es), na microbacia do Córrego Capetinga, situada no Centro-Oeste do Brasil, região de cerrado. Foram analisados os dados de P, PA e IP obtidos durante seis anos hidrológicos, iniciando em 1º de julho de 1996 e terminando em 30 de junho 2002. Foram somente considerados valores de Es maiores ou iguais a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recursos hídricos; Cerrados; Variáveis hidrológicas.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100012

PHYSICAL PROPERTIES OF DIFFERENT SOYBEAN CULTIVARS DURING DRYING
Provedor de dados: 70
Autores: Hauth,Michele R.; Botelho,Fernando M.; Hoscher,Renata H.; Botelho,Sílvia de C. C.; Oliveira,Gabriel H. H. de.
ABSTRACT The knowledge of physical properties of grains is important for the optimization of postharvest operations. Thus, this study aimed to evaluate the effect of moisture content over physical properties of different cultivars of soybean. Soybean of cultivars NS7901RR, TMG1180RR, P98Y70 and TMG132RR were used, with initial moisture content of 0.32, 0.27, 0.25 and 0.21 dry basis (d.b.), respectively. In order to dry the samples, an oven of forced air circulation was used. Samples were dried at temperature of 50 °C, being the drying procedure stopped when the moisture content of soybean was equal or inferior than 0.15 (d.b.). During drying, for interested moisture contents, physical properties were determined: bulk density, equivalent diameter,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycine max (L.); Moisture content; Physical characteristics; Shape and size.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400590

Pontes protendidas de madeira: alternativa técnico-econômica para vias rurais
Provedor de dados: 70
Autores: Fonte,Thalita F. da; Calil Júnior,Carlito.
A necessidade de pontes novas e recuperação das existentes no Brasil é evidente, desde o âmbito municipal, estadual e até federal. A construção de malha rodoviária eficiente pode proporcionar, além do conforto aos usuários, diminuição do custo com o transporte de alimentos e outros produtos, visto que praticamente todo o transporte no País é feito por meio das rodovias. De acordo com estimativa feita pelo Laboratório de Madeiras e de Estruturas de Madeiras (LaMEM) do Departamento de Engenharia de Estruturas da Escola de Engenharia de São Carlos da Universidade de São Paulo, a necessidade de pontes de pequenos e médios vãos ultrapassa 100 mil unidades. Portanto, torna-se de extrema importância o estudo de novas tecnologias que sejam competitivas técnica e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pontes em placa; Estruturas de madeira; Protensão transversal.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300026

Determinação do módulo de elasticidade da madeira juvenil e adulta de Pinus taeda por ultra-som
Provedor de dados: 70
Autores: Ballarin,Adriano W.; Nogueira,Marcelo.
A madeira de Pinus sp. tem utilização crescente na indústria madeireira brasileira. O decréscimo constante do suprimento de árvores adultas com grandes diâmetros, provenientes de florestas naturais, tornou comum a produção de madeira em ciclos curtos, com grande proporção de madeira juvenil. Resultados de diversas pesquisas têm reportado que o módulo de elasticidade e a resistência a diferentes solicitações mecânicas são seriamente afetados pela presença de madeira juvenil. Este trabalho teve por objetivo determinar o módulo de elasticidade da madeira juvenil e adulta de Pinus taeda L. a partir da constante dinâmica C LL, obtida em ensaios não-destrutivos de ultra-som. A madeira de P. taeda era originária de plantios da Estação Experimental de Itapeva -...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ultra-som; Pinus taeda L.; Madeira juvenil.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100003

SPRAY RETENTION ON COFFEE LEAVES ASSOCIATED WITH TYPE AND CONCENTRATION OF ADJUVANTS
Provedor de dados: 70
Autores: Cação,José E. da C. R.; Moreira,Bruno R. de A.; Raetano,Carlos G.; Carvalho,Fernando K.; Prado,Evandro P.
ABSTRACT Agricultural spray adjuvants (ASA) are widely used in pesticide applications to enhance the performance of pesticides. The aim of this research was to investigate the effects of ASA on static surface tension (SST) and foliar spray retention on coffee leaves. The SST of ASA at different concentrations was determined by the drop weight method. Spray retention on adaxial and abaxial coffee leaf surfaces was performed using a micro-sprayer at solution concentrations of 0, 0.01, 0.1, 0.5, and 1.0% v v−1. The ASA assessed were: polyether-polymethylsiloxane-copolymer (PPC); Nonylphenol ethoxylate; nonyl polyethylene glycol ether; mineral oil; nonylphenoxy polyethoxy ethanol; carboxyl copolymer of styrene and butadiene; primary aliphatic oxyalkylated...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Surfactant; Run-off; Spreading area; Pesticide application technology.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500623

Method to evaluate the efficiency of manual overhead irrigation in citrus rootstock liner production
Provedor de dados: 70
Autores: SALVADOR,CONAN A.; FERRAREZI,RHUANITO S.; BARRETO,CARLOS V. G.; TESTEZLAF,ROBERTO.
ABSTRACT Brazil produces grafted citrus seedlings in closed screen houses to reduce pest and disease incidence. Irrigation is usually performed by hand using either breaker nozzles or drilled polyvinyl chloride (PVC) pipe wands on garden hoses. Rootstocks are produced in cone-shaped containers filled with soilless potting mix. Since the containers have a small upper diameter, nutrient solution capture is reduced with the potential to cause environmental contamination from inefficient fertigation. This study provides a method to assess the efficiency of manual overhead irrigation systems used in liner production. The method consists of determining both the volume of water applied and volume lost (i.e., directly and by percolation) in order to obtain an...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrus propagation; Drainage fraction; Irrigation efficiency; Nursery production.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400724

CHANGES IN PHYSICAL QUALITY OF OXISOLS UNDER DIFFERENT MANAGEMENT SYSTEMS IN THE BRAZILIAN CERRADO
Provedor de dados: 70
Autores: Feitosa,Carlos E. L.; Costa,Pedro H. dos S.; Meneses,Kamila C. de; Oliveira,Ulisses C. de; Farias,Maryzélia F. de.
ABSTRACT Soil compaction in agricultural areas has greatly increased in recent decades due to intensive farming practices, including short-cycle crops and machinery intensification. This study aimed to evaluate the impacts of management systems on the physical quality of a dystrophic Yellow Oxisol, in the Cerrado region of Brazil. Treatments consisted of five soil management systems, with five replications (native forest [control], slash-and-burn agriculture, pasture, no-tillage, and conventional tillage). Data analysis was performed using a completely randomized experimental design. All systems were analyzed for soil density, macroporosity, microporosity, total porosity, hydraulic conductivity, infiltration, water retention curve, penetration resistance,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: S index; Land cover change; Physical properties; Infiltration; Soil compaction.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500609

Distribuição da carga hidráulica em linhas de derivação otimizadas por programação linear
Provedor de dados: 70
Autores: Saad,João C. C.; Marcussi,Francisco F. N.
A existência de diferentes combinações de uniformidade de emissão na unidade operacional com a declividade do terreno favorece a ocorrência de várias possibilidades de configurações no sistema de irrigação, por conseguinte de diferentes custos de implantação e de posterior manejo do sistema. Desde que bem dimensionado, consegue-se verificar, no sistema de irrigação localizada, que a otimização do sistema por meio da programação linear é a melhor metodologia frente aos outros métodos propostos na pesquisa operacional, visto que se encontra a solução ótima global para as variáveis preestabelecidas no dimensionamento. Este trabalho teve por objetivo, analisar a distribuição da carga hidráulica na linha de derivação, sob diferentes uniformidades de emissão e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação localizada; Pesquisa operacional; Uniformidade de emissão.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200008

PERFORMANCE AND EMISSION OF POLLUTANTS OF AN AGRICULTURAL ENGINE WITH TWO POWER TAKE-OFF SETTINGS
Provedor de dados: 70
Autores: Schlosser,José F.; Farias,Marcelo S. de; Estrada,Javier S.; Santos,Gustavo O. dos; Gil,Emilio.
ABSTRACT Farming operations are usually performed implements driven by a power take-off (PTO) from tractors. Some manufacturers offer PTO settings named as economic (540E). Such configuration drives implements at lower tractor’s engine rotation, thus providing lower fuel consumption. An engine performance using standard (540) or 540E settings are different and poorly studied. The amounts of pollutants emitted by engines vary mainly with the applied load and rotation. The aim of this study was to compare the performance and exhaust emissions of a farming tractor engine under different PTO loads, using both standard (540) and 540E settings. Specific fuel consumption using 540E was an average 14.7% less than the standard setting. However, 540E promoted...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuel consumption; Exhaust gases; Agricultural tractor; 540E setting.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200277

APPLICABILITY OF THE SWAT HYDROLOGICAL MODEL IN THE MUCURI RIVER BASIN
Provedor de dados: 70
Autores: Almeida,Rafael A.; Pereira,Silvio B.; Pinto,Daniel B. F.; Rosa,David R. Q.
ABSTRACT Land-use changes promote significant variations in streamflow regimes, and hydrological models allow studying their impacts. Based on this approach, this study aimed to assess the applicability of the SWAT model for different land-use scenarios and their respective impacts on the flow regime of the Mucuri River. The average monthly and daily water balance was generated after the calibration and validation of the SWAT model in the basin. Three land-use scenarios were analyzed in relation to the current land use, as follows: replacement of the agricultural area by the eucalyptus crop, replacement of the native forest area by the sugarcane crop, and replacement of pasture by exposed soil. The results showed that the SWAT model is adequate to simulate...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Land use scenarios; Hydrological modeling; Streamflow.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500631

Modelagem matemática e simulação numérica do resfriamento rápido de morango com ar forçado
Provedor de dados: 70
Autores: Pirozzi,Daniela C. Z.; Amendola,Mariângela.
Este trabalho abordou o resfriamento rápido com ar forçado de morango via simulação numérica. Para tanto, foi empregado o modelo matemático que descreve o processo de transferência de calor, com base na lei de Fourier, escrito em coordenadas esféricas e simplificado para descrever o processo unidimensional. A resolução da equação expressa pelo modelo matemático deu-se por meio da implementação de um algoritmo, fundamentado no esquema explícito do método numérico das diferenças finitas, executado no ambiente de computação científica MATLAB 6.1. A validação do modelo matemático foi realizada a partir da comparação de dados teóricos com dados obtidos num experimento, no qual morangos foram resfriados com ar forçado. Os resultados mostraram que esse tipo de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Métodos numéricos; Transferência de calor; Computação científica.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100025

Rational use of water in a poultry slaughterhouse in the state of Paraná, Brazil: a case study
Provedor de dados: 70
Autores: Barana,Ana C.; Botelho,Viviani M. B.; Wiecheteck,Giovana K.; Doll,Maria M. R.; Simões,Deise R. S.
Agroindustries are major consumers of water. However, to adapt to environmental trends and be competitive in the market, they have sought rational use of water through water management in their activities. Cleaner Production can result in economic, environmental and social benefits, and in actions that promote reduction in water consumption. This case study was conducted in a slaughterhouse and poultry cold storage processing plant and aimed to identify points of excessive water consumption, and to propose alternatives for managing water resources by reducing consumption. Consumption data are presented in relation to the processing stages with alternatives proposed for the rational use of water, such as closure of mains water during shift changes....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water consumption; Cleaner production; Poultry processing.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100018

VEGETATION INDICES FOR IRRIGATED CORN MONITORING
Provedor de dados: 70
Autores: Alvino,Francisco C. G.; Aleman,Catariny C.; Filgueiras,Roberto; Althoff,Daniel; da Cunha,Fernando F.
ABSTRACT Monitoring of large agricultural lands is often hampered by data collection logistics at field level. To solve such a problem, remote sensing techniques have been used to estimate vegetation indices, which can subsidize crop management decision-making. Therefore, this study aimed to select vegetation indices to detect variability in irrigated corn crops. Data were collected in São Desidério, Bahia State (Brazil), using an OLI sensor (Operational Land Imager) embedded to a Landsat-8 satellite platform. Five corn growing plots under central pivot irrigation were assessed. The following vegetation indices were tested: NDVI (Normalized Difference Vegetation Index), EVI (Enhanced Vegetation Index), SAVI (Soil Adjusted Vegetation Index), GNDVI (Green...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vegetation cover; Decision-making; Remote sensing.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300322

Administração limpa e enxuta em sistemas hidráulicos de colhedoras de cana-de-açúcar
Provedor de dados: 70
Autores: Tomazela,Mauro; Daniel,Luiz A; Ferreira,José C.
Dentre as importantes mudanças nos processos de produção, está à necessidade de garantir sustentabilidade aos empreendimentos. Isso faz prever mudanças na gestão empresarial para adequar-se a um novo modelo, com a inserção dos conceitos de Produção Limpa, Mais Limpa, Enxuta e Manutenção Produtiva Total (MPT). O foco principal deste trabalho foi elaborar uma metodologia que possibilitou aumentar a confiabilidade nos sistemas hidráulicos das colhedoras de cana-de-açúcar, identificando e analisando os modos de falhas, visando à melhoria da qualidade ambiental e socioeconômica em uma indústria sucroalcooleira, promovendo a diminuição significativa do desperdício de óleo hidráulico durante o processo de colheita motomecanizada. O histórico existente no controle...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Produção limpa; Produção enxuta; Manutenção produtiva total.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200018

Soil salinization and maize and cowpea yield in the crop rotation system using saline waters
Provedor de dados: 70
Autores: Lacerda,Claudivan F.; Sousa,Geocleber G.; Silva,Francisco L. B.; Guimarães,Francisco V. A.; Silva,Giovana L.; Cavalcante,Lourival F.
The use of saline water and the reuse of drainage water for irrigation depend on long-term strategies that ensure the sustainability of socio-economic and environmental impacts of agricultural systems. In this study, it was evaluated the effects of irrigation with saline water in the dry season and fresh water in the rainy season on the soil salt accumulation yield of maize and cowpea, in a crop rotation system. The experiment was conducted in the field, using a randomized complete block design, with five replications. The first crop was installed during the dry season of 2007, with maize irrigated with water of different salinities (0.8, 2.2, 3.6 and 5.0 dS m-1). The maize plants were harvested at 90 days after sowing (DAS), and vegetative growth, dry...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays; Irrigation; Vigna unguiculata; Salt stress.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400005

Alternative methodology for calculating the modulus of elasticity of wooden beams of structural dimensions
Provedor de dados: 70
Autores: Christoforo,André L.; Panzera,Tulio H.; Neto Junior,Carlito Calil; Demarzo,Mauro A.; Ribeiro Filho,Sérgio L. M.; Toniolo,Luiz E.; Amstalden,Rogério A. S.; Lahr,Francisco A. R.
This study aims to present an alternative calculation methodology based on the Least Squares Method for determining the modulus of elasticity in bending wooden beams of structural dimensions. The equations developed require knowledge of three or five points measured in displacements along the piece, allowing greater reliability on the response variable, using the statistical bending test at three points and non-destructively, resulting from imposition of measures from small displacements L/300 and L/200, the largest being stipulated by the Brazilian norm NBR 7190:1997. The woods tested were Angico, Cumaru, Garapa and Jatoba. Besides obtaining the modulus of elasticity through the alternative methodology proposed, these were also obtained employing the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wood; Beam theory; Modulus of elasticity; Least Squares Method.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100016

Terrain forms and spatial variability of soil properties in an area cultivatedwith citrus
Provedor de dados: 70
Autores: Leão,Marisol G. A. de; Marques Júnior,José; Souza,Zigomar M. de; Siqueira,Diego S.; Pereira,Gener T.
The technique of precision agriculture and soil-landscape allows delimiting areas for localized management, allowing a localized application of agricultural inputs and thereby may contribute to preservation of natural resources. Therefore, the objective of this work was to characterize the spatial variability of chemical properties and clay content in the context of soil-landscape relationship in a Latosol (Oxisol) under cultivation of citrus. Soil samples were collected at a depth of 0.0-0.2 m in an area of 83.5 ha planted with citrus, as a 50-m intervals grid, with 129 points in concave terrain and 206 points in flat terrain, totaling 335 points. Values for the variables that express the chemical characteristics and clay content of soil properties were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geostatistics; Management zone; Oxisol; Orange.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400003

Classificação espectral de área plantada com a cultura da cana-de-açúcar por meio da árvore de decisão
Provedor de dados: 70
Autores: Delgado,Rafael C.; Sediyama,Gilberto C.; Costa,Marcos H.; Soares,Vicente P.; Andrade,Ricardo G.
O objetivo deste trabalho foi testar o classificador "árvore de decisão", em dados provenientes de sensores orbitais, para identificar área plantada com cana-de-açúcar, em diferentes épocas de plantio na Fazenda Boa Fé, localizada no Triângulo Mineiro, mais especificamente no município de Conquista, Minas Gerais. Acoplaram-se técnicas de Sensoriamento Remoto (SR) em um módulo de Sistema de Informação Geográfica (SIG), permitindo uma análise temporal do uso e ocupação do solo, especialmente com vistas a identificar e a monitorar as áreas agrícolas. Com base no cálculo do viés médio (VM), o presente estudo mostrou que, em áreas de cana-de-açúcar, onde a irrigação é frequente e ocorrem chuvas significativas que antecedem a passagem do satélite Landsat-5, os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Árvore de decisão; Sensoriamento remoto; SIG; Cana-de-açúcar.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200017

AGRONOMICAL ATTRIBUTES OF SOYBEANS AND SOIL RESISTANCE TO PENETRATION IN NO-TILLAGE AND CHISELED SURFACES
Provedor de dados: 70
Autores: Cortez,Jorge W.; Mauad,Munir; Souza,Luiz C. F. de; Rufino,Mauricio V.; Souza,Paulo H. N. de.
ABSTRACT Farming systems may affect soil properties and crop production of components, decreasing yields. This study aimed to assess penetration resistance (PR) and agronomic traits of soybeans under no-tillage (NT) and chiseling (CP). The experiment was carried out in a randomized block with two treatments (tillage and scarification) with 12 repetitions; yet soil penetration resistance (PR) was assessed in a factorial block, considering farming systems and sampling sites (row and interrows). PR was measured with an impact penetrometer, sampling in row and interrows within a 22.5 x 0.1 m2 mesh grid up to 0.60 m depth. The obtained values were higher for NT in the 0.10-0.20 m layer. Great PR values in interrows were only registered within the surface layer....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compaction; Soil physics; Chiseling.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100098

Fuzzy control applied to an electrical power generation system mounted on tractors for driving of agricultural implements
Provedor de dados: 70
Autores: Soares,Fabricio T.; Cappelli,Nelson L.; Garcia,Angel P.; Umezu,Claudio K.
ABSTRACT The demand of the agricultural sector for more operationally efficient machines and implements motivated the development of alternatives for driving of this equipment. Aiming an electrical supply to apply in agricultural implements, this study proposes a system that uses the tractor power take off to activate a synchronous generator, using a fuzzy logic controller designed to regulate the generated voltage level. Different control architectures were tested and evaluated by simulations. In the initial stage were evaluated fuzzy PI, fuzzy PD and fuzzy PID controllers of multiple inputs and single output (MISO) and the error of the generated voltage as state variable. Subsequently, it was evaluated a fuzzy PI controller of single input and multiple...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Synchronous generator; Power take off; Electrical implements.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500846

SPATIAL VARIABILITY IN LEAF ANALYSIS AND PRODUCTIVITY OF FERTIRRIGATED AÇAÍ
Provedor de dados: 70
Autores: Ribeiro,Felipe O.; Fernandes,Antonio R.; Matos,Gilson S. B. de; Lindolfo,Marcelo M.; Guedes,Rafael S.; Rodrigues,Graziele R.
ABSTRACT This study aimed to define management zones (MZs) for fertirrigated açaí cultivation, based on spatial variability of the foliar nutrients and productivity data. The work was carried out in an area of 5.75 ha of a 7-year crop, with 80 georeferenced sample points. Fresh fruit productivity and nutrient (N, P, K, Ca, Mg, S, B, Cu, Fe, Mn, and Zn) contents were determined. The average contents of macronutrients were considered adequate for adult açaí plants, and their spatial dependence associated with fruit productivity allowed the representation of their distributions through maps of variability. Through multivariate analysis, three main components were highlighted. These components explained 51.5 % of the total variability of the data, where PC1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Amazon; Management zones; Multivariate analysis; Nutrient contents; Precision agriculture.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600800

Biodigestão anaeróbia de dejetos de caprinos obtidos nas diferentes estações do ano
Provedor de dados: 70
Autores: Amorim,Ana C.; Lucas Júnior,Jorge de; Resende,Kléber T.
Foram utilizados dejetos produzidos por caprinos, em diferentes estádios fisiológicos e submetidos ao mesmo regime alimentar, nas quatro estações do ano. O objetivo foi avaliar o efeito das estações do ano sobre a digestão anaeróbia de resíduos de caprinos em biodigestores modelo batelada com volume útil de 60 L de substrato em fermentação e mantidos sob temperatura ambiente. Foram avaliadas as produções de biogás, as reduções de sólidos voláteis (SV), os potenciais de produção (m³ de biogás/kg de substrato, de estrume, de sólidos totais (ST) ou sólidos voláteis), os números mais prováveis de coliformes totais e fecais, e a composição do biogás. As reduções de SV foram de 38; 34; 33 e 39% para o verão, outono, inverno e primavera, respectivamente. Os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogás; Cabras; Esterco.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100003

Viabilidade técnica e econômica da substituição de fontes convencionais de energia por biogás em assentamento rural do Estado de São Paulo
Provedor de dados: 70
Autores: Esperancini,Maura S. T.; Colen,Fernando; Bueno,Osmar de C.; Pimentel,Andréa E. B.; Simon,Elias J.
O objetivo deste estudo foi avaliar a viabilidade econômica da implantação de dois biodigestores com uso de dejetos animais em área do Assentamento de Trabalhadores Rurais no município de Itaberá - SP, no ano de 2005; um deles para o fornecimento de energia para os domicílios e outro para as atividades produtivas. Foram avaliados os benefícios referentes ao fornecimento de energia elétrica e térmica, a partir do biogás, para cinco domicílios da agrovila do assentamento e para as atividades produtivas, comparativamente aos custos de construção e operação para produção de biogás. Os resultados mostraram a viabilidade econômica da produção de gás em ambos os biodigestores. Foram gerados benefícios no valor de R$ 3.698,00 por ano e R$ 9.080,57 por ano, nos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biodigestores; Economia de energia; Assentamentos rurais.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100004

Cassava starch extraction effluent treatment in a one phase tubular horizontal pilot reactor with support medium
Provedor de dados: 70
Autores: Kuczman,Osvaldo; Tavares,Maria H. F.; Gomes,Simone D.; Guedes,Luciana P. C.; Grisotti,Geovane.
The cassava starch industries generate a large volume of wastewater effluent that, stabilized in ponds, wastes its biogas energy and pollutes the atmosphere. To contribute with the reversion of this reality, this manipueira treatment research was developed in one phase anaerobic horizontal pilot reactor with support medium in bamboo pieces. The reactor was excavated into the ground and sealed with geomembrane in HDPE, having a volume equal to 33.6 m³ and continuous feeding by gravity. The stability indicators were pH, volatile acidity/total alkalinity ratio and biogas production. The statistical analyses were performed by a completely randomized design, with answers submitted to multivariate analysis. The organical loads in COD were 0.556; 0.670; 0.678 and...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Biodigester; Biogas; Anaerobic digestion; Cassava; Cassava wastewater.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600021

Computer tools applied to analysis of solar water heaters
Provedor de dados: 70
Autores: Altoé,Leandra; Oliveira Filho,Delly; Carlo,Joyce C.; Monteiro,Paulo Marcos de B.
The simulation programs are important tools to analyze the different energetic alternatives, including the use of renewable energy. The objective of this study was to analyze comparatively the different computer tools available for modeling of solar water heaters. Among the main simulation software of solar thermal systems, there are: RETScreen International, EnergyPlus, TRNSYS, SolDesigner, SolarPro, e T*SOL. Among the tools mentioned, only EnergyPlus and RETScreen International are free, but they allow obtaining interesting results when applied together. The first one has a detailed module of energy analysis of solar water heaters, while the second one provides an detailed economic feasibility study and an assessment of emissions of greenhouse gases....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulation; Solar energy; Water heating.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500018

Semeadura do milho em sistema de plantio direto sem e com manejo mecânico da matéria seca
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Justino,Altair; Antunes,Rodolfo K.; Fornari,Allison J.; Garcia,Luiz C.
O objetivo deste trabalho foi verificar se a cultura do milho é influenciada pelo manejo mecânico da aveia-preta dessecada antes de sua semeadura, pela utilização de rolo destorroador. Os tratamentos consistiram na semeadura do milho sob a matéria seca de aveia-preta dessecada sem manejo mecânico e rolada. O experimento foi realizado em quatro propriedades, duas na safra de 2007/2008 e as outras duas na safra de 2008/2009. O delineamento experimental adotado foi em blocos ao acaso, com 11 repetições, cujas parcelas possuíam 80 m² cada. Avaliaram-se a qualidade da semeadura e os componentes de rendimento. Conclui-se que o manejo mecânico da palha de aveia-preta antes da semeadura do milho pode elevar significativamente os espaçamentos falhos e reduzir...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aveia-preta; Rolo destorroador; Componentes de rendimento.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400019

ATR-FTIR FOR CHARACTERIZING AND DIFFERENTIATING DRIED AND GROUND COFFEE CHERRY PULP OF DIFFERENT VARIETIES (Coffea Arabica L.)
Provedor de dados: 70
Autores: Barrios-Rodríguez,Yeison; Collazos-Escobar,Gentil A.; Gutiérrez-Guzmán,Nelson.
ABSTRACT This study aimed to evaluate the performance of the infrared spectrum in the range of 4000−650 cm−1 for characterizing and differentiating dried and ground coffee cherry pulp of different varieties. The spectral data were subjected to first and second derivative treatments to perform the statistical analyses. Three varieties of coffee pulp were previously characterized for color, water activity, moisture, chlorogenic acids, and caffeine. The results of principal component analysis (PCA) showed that Fourier transform infrared (FTIR) spectroscopy is a viable technique for characterizing and differentiating dried and ground coffee cherry pulp among different varieties, showing the best differentiation with treatment of data from the first derivative,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffee cherry by-products; Coffee chemical compounds; Infrared spectrum analysis.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100070

SEWAGE PERFORMANCE OF A NEW TYPE OF FLAP FILTER
Provedor de dados: 70
Autores: Liu,Zhenji; Shi,Kai; Li,Man; Xie,Yan.
ABSTRACT The drainage performance of a mesh filter determines the water consumption degree of the filter and the efficiency of the next work cycle. Through analysis, we found that the influent flow rate and the sediment content of the influent were important influencing factors. This experiment focused on the drainage time, pressure difference, and cleanliness to investigate the drainage performance of a new type of flap filter. The results showed that with increasing inlet flow rates, the time to discharge the effluent decreased, and the time required for the difference between the primary and secondary sewage pressures to reach a constant level was shorter. The cleanliness and drainage effects were improved. To verify this, we established mathematical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Flap-type mesh filter; Discharge time; Pressure difference; Cleanliness; Sewage effect.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200135

Modelo de dimensionamento otimizado para sistemas energéticos renováveis em ambientes rurais
Provedor de dados: 70
Autores: Nogueira,Carlos E. C.; Zürn,Hans H.
Este trabalho teve por objetivo o desenvolvimento de novo modelo para dimensionamento de sistemas integrados de recursos energéticos renováveis, aplicados a ambientes rurais, a partir da utilização de ferramentas de simulação e otimização desenvolvidas em MATLAB 6.0. O dimensionamento realizado apresenta custo mínimo e atende a determinado nível de confiabilidade desejado para o sistema, baseado no conceito de probabilidade de perda de fornecimento de energia à carga (LPSP) para horas consecutivas. Um modelo de otimização é apresentado e três diferentes cenários de dimensionamento são calculados e comparados, mostrando a flexibilidade na elaboração de diferentes concepções de projeto. Os resultados obtidos contemplam o dimensionamento completo dos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recurso renovável; Metodologia de dimensionamento; Modelo de otimização.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200007

Hydrographic and hydrogeological basin of Entre-Ribeiros: probable recharge zone delimitation and environmental impact assessment
Provedor de dados: 70
Autores: Vasconcelos,Vitor V.; Martins Junior,Paulo P.; Hadad,Renato M.
The probable recharge zone delimitation of Entre-Ribeiros Basin (Northwest of the state of Minas Gerais / Brazil) is proposed in this study. The delimitation is based upon stratigraphy, geomorphology, geo-environmental domains and hydrogeology studies. Combining the recharge zone map with the land use variation between 1975 and 2008, the occupation trends of possible recharge zones are identified. Concluding, the environmental impacts for this basin are discussed.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydrogeology; Aquifer recharge; Land use zoning; Environment; Soil compaction.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300015

ARTIFICIAL NEURAL NETWORKS FOR PREDICTING ANIMAL THERMAL COMFORT
Provedor de dados: 70
Autores: Borges,Pedro H. M.; Mendoza,Zaíra M. S. H. de; Morais,Pedro H. M.; Santos,Ronei L. dos.
ABSTRACT The objective of this study was to develop artificial neural networks (ANNs) for predicting animal thermal comfort based on temperature and relative humidity of the air for each day of the year. The data on temperature and relative humidity for a 25-year historical series collected at the Padre Ricardo Remetter Conventional Meteorological Station, located in the city of Santo Antônio de Leverger - Mato Grosso (Brazil), were retrieved from the website of the National Institute of Meteorology. According to the day of the year, the temperature and humidity index was determined as a function of the climatic variables. Therefore, the day of the year was the input variable of the neural networks, and the temperature and humidity index (THI) was the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Time series; Artificial intelligence; Comfort index.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600844

Potencial de erosão da bacia do Rio Uberaba
Provedor de dados: 70
Autores: Valle Júnior,Renato F. do; Galbiatti,João A.; Martins Filho,Marcílio V.; Pissarra,Teresa C. T.
Este trabalho teve por objetivo identificar qualitativamente as áreas suscetíveis à erosão laminar na bacia do Rio Uberaba, localizada em Uberaba -MG, apoiado no modelo matemático da Equação Universal de Perda de Solo (EUPS). Foram utilizadas cartas de: solos, uso e ocupação das terras, redes de drenagem, declividade e dados pluviográficos, utilizando-se de um Sistema de Informação Geográfica (SIG -IDRISI). A espacialização do potencial de erosão só foi possível a partir da estimativa da tolerância às perdas laminares para cada tipo de solo da bacia, e da profundidade dos solos, por entender que as perdas são mais significativas em solos mais rasos do que em solos muito profundos. Na análise dos resultados, verificou-se que 37% da área total da bacia do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: USLE; Erosão; Impacto ambiental.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500012

Test of a microlysimeter for measurement of soil evaporation
Provedor de dados: 70
Autores: Flumignan,Danilton L.; Faria,Rogério T. de; Lena,Bruno P.
Quantifying soil evaporation is required on studies of soil water balance and applications aiming to improve water use efficiency by crops. The performance of a microlysimeter (ML) to measure soil evaporation under irrigation and non-irrigation was evaluated. The MLs were constructed using PVC tubes, with dimensions of 100 mm inner diameter, 150 mm depth and 2.5 mm wall thickness. Four MLs were uniformly distributed on the soil surface of two weighing lysimeters conducted under bare soil, previously installed at Iapar, in Londrina, PR, Brazil. The lysimeters had 1.4 m width, 1.9 m length and 1.3 m depth and were conducted with and without irrigation. Evaporation measurements by MLs (E ML) were compared with measurements by lysimeters (E L) during four...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water management; Water balance; Lysimeters; Soil water.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100009

Corn yield under various simulated irrigation depths
Provedor de dados: 70
Autores: Parizi,Ana R. C.; Robaina,Adroaldo D.; Gomes,Ana C. dos S.; Peiter,Marcia X.; Soares,Fátima C.
ABSTRACT Mathematical models are tools to estimate and understand system behaviors against diverse situations; they may help in decision-making through simplified representations of the reality, allowing simulating various scenarios and estimating impacts of different courses of action on production systems, assisting thus in activity planning. Thus, this paper proposed a simulation of corn crop yields according to different field experiment characteristics and weather conditions in which it was conducted, with the purpose of setting a simulation model already calibrated and tested for corn crop cycle in the region of Santiago – RS, Brazil. The increasing water levels had a positive effect on grain yield and corn dry matter. On the other hand, a level of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays L.; Irrigation strategies; Yield model.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300503

Efeitos da roda compactadora de semeadoras sob cargas verticais na deformação do solo com dois teores de água
Provedor de dados: 70
Autores: Silva,Rouverson P. da; Furlani,Carlos E. A.; Lopes,Afonso; Nascimento,Alessandro; Camara,Felipe T. da.
O presente trabalho foi conduzido na Pista de Ensaios de Semeadura do Laboratório de Máquinas e Mecanização Agrícola (LAMMA) da UNESP/Jaboticabal - SP, para o estudo da ação da roda compactadora de semeadoras sob cargas verticais, na deformação do solo, com dois teores de água. Os tratamentos consistiram da combinação de dois teores de água e seis cargas verticais, totalizando 12 tratamentos, com três repetições, em dois ensaios, analisando-se a resistência mecânica do solo à penetração e a deformação do solo provocada pela roda compactadora. A roda compactadora utilizada era de alumínio, com massa de 6,4 kg, 40 cm de diâmetro e 10 cm de largura, sob a ação de cargas verticais de 63; 161; 259; 357; 455 e 553 N, obtidas acoplando-se lastros de chumbo sobre...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Canal de solo; Semeadura; Resistência do solo à penetração.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200020

PROTECTED ENVIRONMENTS AND SUBSTRATES FOR MANGABEIRA SEEDLINGS (Hancornia Speciosa Gomez) PRODUCTION
Provedor de dados: 70
Autores: Arrua,Luan L. De C.; Costa,Edilson; Bardiviesso,EstefâNia M.; Nascimento,Daniele M. Do; Binotti,Flavio F. Da S.
ABSTRACT Mangabeira is a native fruit tree from Brazil, which provides a delicious fruit to taste and beneficial to health, whose information about the seedlings production will assist the entire productive chain of this important species. The aim of this research was to evaluate protected environments and substrates compositions in the formation of mangabeira seedlings. For this, two greenhouses with different screens were used, the first covered with aluminized thermo-reflective screen of 50% shading and the second with black screen of 50% shading. Inside the environments, were tested substrates derived from combinations of various proportions of bovine manure (M), soil (S), medium vermiculite (MV), super fine vermiculite (FV) and fine sand (FS). For...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hancornia Speciosa; Protected environment; Climatic factors; Vermiculite; Sand.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000600984

IN SITU MONITORING OF A CONTROLLED RELEASE OF FERTILIZERS IN LETTUCE CROP
Provedor de dados: 70
Autores: Souza,Claudinei F.; Faez,Roselena; Bacalhau,Fabiana B.; Bacarin,Murilo F.; Pereira,Tamires S.
ABSTRACT: Agriculture has sought ways to increase food production to meet global demands, intensifying dependence on natural resources. An alternative for intensive production has relied on the use of “smart” fertilizers that release nutrients in a controlled manner. Biodegradable polymers containing fertilizers has presented economic and environmental advantages when applied to the soil, as they release water and nutrients gradually to the environment without leaving residues. The objective of this study was to monitor the behavior of chitosan-clay hybrid microspheres, used as potassium nitrate soil ferti-releaser in lettuce cultivation. The experiment consisted of two treatments: (i) application of ferti-releasing chitosan-clay microspheres and (ii) use...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ferti-releasing biopolymer; Clay; Moisture; Electrical conductivity.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400656

Desempenho de equipamentos utilizados para o fechamento de taipas abertas para drenagem no arroz irrigado
Provedor de dados: 70
Autores: Frantz,Ulisses G.; Schlosser,José F.; Rodrigues,Fabrício A.; Farias,Marcelo S. de; Barbieri,Juan P.
RESUMO Na semeadura do arroz irrigado, é necessária a boa drenagem da área, sendo realizados drenos cortando as taipas transversalmente. Para o estabelecimento da lâmina de irrigação definitiva, é necessário o fechamento destes drenos realizado pelos agricultores por meio de diversas maneiras. O estudo de tempos e movimentos de diferentes operações agrícolas é uma importante ferramenta para a obtenção de dados que reflitam o desempenho das mesmas. Dessa forma, o presente trabalho objetivou avaliar o desempenho de cinco equipamentos utilizados na lavoura orizícola, na operação de fechamento de taipas abertas para drenagem (entaipadora de base larga, braço valetador, caçamba "scraper", pá de corte e um protótipo desenvolvido para realizar esta operação), em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drenos; Lavoura orizícola; Eficiência.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500875

USE OF USLE/ GIS TECHNOLOGY FOR IDENTIFYING CRITERIA FOR MONITORING SOIL EROSION LOSSES IN AGRICULTURAL AREAS
Provedor de dados: 70
Autores: Botelho,Thiago H. A.; Jácomo,Simone de A.; Almeida,Rherison T. S.; Griebeler,Nori P.
ABSTRACT The assessment of land use and occupation is essential for predicting soil loss due to water erosion. The objective of this study was to determine criteria for monitoring soil loss in agricultural areas using the Universal Soil Loss Equation (USLE). Soil loss data were intersected with USLE factors and slope using geoprocessing techniques for the Samambaia River watershed, located in Cristalina, Goiás state, Brazil. A slope of 3% to 8% was found in approximately 50% of the study area. However, mean soil losses &lt;10 t ha-1 year-1 were observed in slopes ≤ 3%, where the mean soil length (L) and slope steepness (S) were ≤2 and 0.2, respectively. The intersection of soil loss data with USLE factors was useful for identifying criteria for monitoring...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil cover; Water erosion; Topographic factor; Conservation management.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100013

INFLUENCE OF EXPOSURE TIME TO OPERATING TEMPERATURE ON SHEAR STRENGTH OF WOOD USED IN ROOF STRUCTURES
Provedor de dados: 70
Autores: Christoforo,André L.; Almeida,Tiago H. de; Almeida,Diego H. de; Balanco,Giovana G.; Lahr,Francisco A. R.
ABSTRACT Wood is one of the main materials used in the constructing of covering structures (roofs) because of its versatility. Under this situation, due to solar radiation incidence, the temperature can exceed 60 °C and, such as other environmental conditions, influence the mechanical properties of the wood in use. The aim of this research was to study the influence of exposure time of the wood of four different hardwood species at a temperature of 60 °C on the shear strength parallel to fibers. The wood of the following species was used: Cupiúba (Goupia glabra), Eucalyptus (Eucalyptus saligna), Garapeira (Apuleia leiocarpa), and Jatobá Tamarindo (Hymenaea sp.). In order to investigate the effect of exposure time (0, 168, 456, 720, and 2160 hours) of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hardwoods; Mechanical properties; Roofs; Temperature.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300365

Soil chiseling and fertilizer location in sugarcane ratoon cultivation
Provedor de dados: 70
Autores: Bianchini,Aloisio; Valadão Junior,Daniel D.; Rosa,Rodrigo P.; Colhado,Frederick; Daros,Rodrigo F.
While the pre-harvest sugarcane burning is a disused practice, green harvest requires changes concerning ratoon cultivation due to the presence of a thick layer of straw. The experiment, conducted in a mechanical green harvesting area cultivated with sugarcane, consisted of two stages: in the first stage, the mechanical straw cutting performance of flat disks with different geometry edges was evaluated, considering two types of disks and 10 replications in a completely randomized design; in the second stage, the effect of soil chiseling on both sides of planting lines, using shanks with straw cutting flat disks, was assessed, as well as fertilizer deposition form. The experimental design in the second stage was completely randomized, with seven treatments...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum officinarum; Cutting disk; Mulching.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100007

Compactação de solos cultivados com cana-de-açúcar: I -modelagem e quantificação da compactação adicional após as operações de colheita
Provedor de dados: 70
Autores: Severiano,Eduardo da C.; Oliveira,Geraldo C. de; Dias Júnior,Moacir de S.; Castro,Matheus B. de; Oliveira,Luiz F. C. de; Costa,Katia A. de P.
A colheita mecanizada da cana-de-açúcar, quando realizada em épocas da safra em que o solo se encontra com conteúdos inadequados de água, tem sido responsável pela compactação do solo e a redução da produtividade nos ciclos posteriores da cultura. Este estudo teve como objetivo avaliar o efeito das operações de colheita da cana-de-açúcar em diferentes épocas da safra sobre a pressão de preconsolidação em um Latossolo Vermelho-Amarelo (LVA) e em um Cambissolo Háplico (CX). A colheita mecanizada consistiu no tráfego de duas passadas de uma colhedora de cana e do conjunto trator + transbordo em cada entrelinha da cultura. As amostras indeformadas foram utilizadas na determinação dos modelos de capacidade de suporte de carga do solo e na quantificação da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum sp.; Mecanização da colheita; Pressão de preconsolidação; Capacidade de suporte de carga do solo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300005

Lodo têxtil e água residuária da suinocultura na produção de mudas de Eucalyptus grandis (W, Hill ex Maiden)
Provedor de dados: 70
Autores: Pelissari,Rodrigo A. Z.; Sampaio,Sílvio C.; Gomes,Simone D.; Crepalli,Mauro da S.
O objetivo deste trabalho foi avaliar os efeitos do lodo têxtil, adubação e irrigação com água residuária da suinocultura na produção de mudas de Eucalyptus grandis W, Hill ex Maiden. Os tratamentos foram constituídos de três fatores: adubação química (0;1 e 2 gramas de NPK 14-14-14 por tubete), irrigação (água e água residuária da suinocultura) e substrato com cinco níveis de fracionamento do lodo têxtil e substrato comercial (0; 25; 50; 75 e 100%). Avaliaram-se quatro épocas durante a produção das mudas: germinação. (21 dias), sombreamento (50%, 40 dias), sombreamento (18%, 20 dias) e pleno sol (9 dias), com total de 90 dias de produção. As irrigações foram realizadas por aspersão, com lâmina de 12 mm dia-1. Os parâmetros agronômicos avaliados foram:...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reúso de água; Resíduos sólidos; Aplicação de efluentes.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200012

Período de recuperação do investimento em bomba hidráulica de melhor rendimento em sistemas de bombeamento na tarifa horossazonal verde
Provedor de dados: 70
Autores: Zocoler,João L.; Hernandez,Fernando B. T.; Saad,João C. C.; Cruz,Raimundo L.
Neste trabalho, ajustou-se um modelo matemático para quantificar o efeito da variação do rendimento da bomba hidráulica na variação dos custos de um sistema de bombeamento, na estrutura tarifária horossazonal verde (subgrupo A4) e o tempo de recuperação do capital investido no equipamento de maior rendimento. Em seguida, o mesmo foi aplicado a um sistema de bombeamento para suprimento de um sistema de irrigação do tipo pivô central. As opções de rendimento da bomba hidráulica foram: 69,5% (bomba 1), 73% (bomba 2) e 78% (bomba 3), cujos custos de aquisição foram, respectivamente, R$ 6.176,00, R$ 8.479,00 e R$ 15.509,00. Os resultados da aplicação do modelo mostraram que: i) a substituição da bomba 1 pela bomba 2 foi viável, sendo o período de recuperação de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelo matemático; Energia; Custos.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200009

Teor de fósforo e pH no bulbo molhado, com diferentes freqüências de fertirrigação, utilizando ácido fosfórico
Provedor de dados: 70
Autores: Foratto,Leticia C.; Zanini,José R.; Natale,William.
A aplicação de fertilizantes fosfatados, tais como superfosfofato simples, superfosfofato triplo e monofosfato de amônio, via gotejamento, pode apresentar incrustações nas canalizações e obstruções de emissores. No presente trabalho, realizado na UNESP/Jaboticabal - SP, estudaram-se a distribuição do fósforo e a sua influência sobre o pH e a umidade em Latossolo Vermelho, fertirrigado durante um mês, com cinco aplicações semanais de ácido fosfórico. Utilizaram-se quatro repetições e oito tratamentos, constituídos da combinação de doses de P2O5 (0 e 50 kg ha-1) e freqüências de aplicação de 1; 3; 5 e 7 dias. Pelos resultados obtidos, observou-se que a freqüência de irrigação ou de fertirrigação não influenciou na distribuição final da umidade no bulbo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Acidez do solo; Gotejamento; Incrustação.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300012

INFLUENCE OF SEED TUBE CURVATURE ON SEED LONGITUDINAL DISTRIBUTION
Provedor de dados: 70
Autores: Savi,Daniel; Kmiecik,Leonardo L.; Strapasson Neto,Lauro; Silva,Thiago X. da; Jasper,Samir P.
ABSTRACT Studies on the longitudinal distribution of seeds in the sowing row seek to improve crop homogeneity, thus generating high productivity. In this context, seed tubes must be analyzed for their angular curvature. Thus, this study aimed to evaluate the influence of the seed tube curvature on the longitudinal distribution of corn and soybean seeds at different speeds. Two experiments were conducted completely randomized in a double factorial design. The first factor consisted of the seed tube curvature (straight and curved) and the second factor consisted of sowing speeds (1.11, 1.39, and 1.67 m s−1 for corn and 1.39, 1.67, 1.94, and 2.22 m s−1 for soybean), with five replications. The parameters analyzed to measure the longitudinal distribution were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sowing uniformity; Productivity; Seed drill; Performance monitoring; Bench experiment.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600732

Uso de cloração e ar comprimido no controle do entupimento de gotejadores ocasionado pela aplicação de água residuária
Provedor de dados: 70
Autores: Cararo,Denis C.; Botrel,Tarlei A.
O crescimento demográfico, o aumento da demanda por água e alimentos, a crescente geração de resíduos, a poluição de corpos de água e a escassez de água têm ocasionado a busca por soluções, das quais uma é o aproveitamento do efluente de estações de tratamento de esgoto na agricultura. Um modo seguro de efetuar a aplicação desse recurso, também fertilizante, é utilizando a irrigação por gotejamento, porém o entupimento nesse sistema consiste em fator restritivo. Assim, com o objetivo de minimizar o entupimento em quatro modelos de gotejadores por uso de águas residuárias oriundas de tratamento secundário de estação de tratamento de esgoto, testaram-se quatro tipos de manejo: (I) controle (somente filtragem), (II) cloração, (III) ar comprimido e (IV)...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação localizada; Entupimento de emissores; Efluente.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300002

Mineralização do resíduo da pupunheira em condições de campo e laboratório
Provedor de dados: 70
Autores: Pereira,Magno S.; Matos,Antonio T.; Borges,Alisson C.; Nunes,Michael F.
RESUMO Objetivou-se, neste trabalho, estudar o processo de decomposição do carbono (CO) e nitrogênio orgânico (NO) dos resíduos da pupunheira, em condições de campo e laboratório, e em duas formas de aplicação: com incorporação ou em disposição superficial no solo. O experimento de campo foi conduzido em Cambissolo Háplico Tb distrófico latossólico (CXbd), nas condições climáticas tropicais do período de primavera/verão, na cidade de Viçosa-MG, Brasil. Os resíduos foram incubados em condição de campo e laboratório, durante 112 dias, período no qual foram retiradas amostras para a análise das concentrações mineralizadas do CO e NO. A degradação do resíduo foi mais intensa em condição de campo que na de laboratório, e a incorporação do resíduo no solo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Degradação; Matéria orgânica; Fração de decomposição.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500918

Avaliação da acurácia no direcionamento com piloto automático e contraste da capacidade de campo operacional no plantio mecanizado da cana-de-açúcar
Provedor de dados: 70
Autores: Baio,Fábio H. R.; Moratelli,Rodrigo F.
Com o crescimento da mecanização da cana-de-açúcar, é necessária uma dinamização dos processos, como no uso de técnicas de agricultura de precisão para uma diminuição do custo de produção. O presente trabalho foi desenvolvido com o objetivo de contrastar a acurácia nas passadas orientadas por dois sistemas de direcionamento, autodirecionamento via satélite versus manual, assim como comparar as capacidades de campo e a eficiência operacional envolvidos no plantio mecanizado da cana-de-açúcar. Foram analisados dois tratamentos: com e sem o auxílio do piloto automático por GPS RTK na operação de plantio mecanizado. As avaliações foram realizadas em condições de campo, na Usina IACO Agrícola S.A., em Chapadão do Sul - MS. De acordo com os resultados obtidos,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Piloto automático; Direcionamento; GPS.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200017

Aplicação de água residuária de suinocultura em solo cultivado com soja: cobre e zinco no material escoado e no solo
Provedor de dados: 70
Autores: dal Bosco,Tatiane C.; Sampaio,Silvio C.; Opazo,Miguel A. U.; Gomes,Simone D.; Nóbrega,Lúcia H. P.
O objetivo deste trabalho foi avaliar a poluição difusa referente ao cobre e ao zinco no solo e no material de escoamento superficial quando da aplicação de água residuária de suinocultura (ARS) em solo cultivado com soja, sob condição de chuva simulada. O experimento foi instalado em Toledo - PR, sendo aplicadas ao solo cinco taxas de ARS (0; 50; 100; 150 e 200 m³ ha-1 no ciclo), em três repetições por tratamento, divididas em seis aplicações ao longo do ciclo da soja. Foram instaladas calhas coletoras do material escoado e fizeram-se seis simulações de chuva durante o experimento, resultando em seis coletas do material escoado. Ao final do ciclo da soja, foram coletadas amostras de solo em cada uma das parcelas experimentais, em três profundidades, para...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Escoamento superficial; Lixiviação de íons; Reúso de água.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400010

Hastes instrumentadas para a mensuração da resistência mecânica do solo
Provedor de dados: 70
Autores: Adamchuk,Viacheslav I.; Molin,José P.
A presença de camada de solo compactada pode significar sérios problemas ao desenvolvimento do sistema radicular das culturas em geral. A correção pode ser feita por métodos biológicos ou mecânicos. Uma das formas de diagnóstico da sua presença é com o uso de penetrômetros que exigem tempo considerável para a obtenção de dados. Com o advento dos recursos de espacialização das informações na forma de mapas, a necessidade de amostragem passou a ser ainda maior. Este trabalho reporta a busca de uma solução alternativa ao uso do penetrômetro. Envolve a geração de mapas de resistência mecânica do solo ao deslocamento de uma haste em três profundidades, baseado em três hastes instrumentadas, um receptor de GPS e um sistema de aquisição de dados. O sistema é...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Sensores de solo; Compactação.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100018

TEMPORAL DYNAMICS OF CLIMATOLOGICAL PARAMETERS AND HYDRIC BALANCE IN THE MANAGEMENT OF AGRICULTURAL CROPS
Provedor de dados: 70
Autores: Filgueiras,Roberto; Oliveira,Vinicius M. R. de; Cunha,Fernando F. da; Mantovani,Everardo C.
ABSTRACT One of the main factors that determine the success of decision-making in the fields is the climatic factor. This way, the geostatistical techniques have been used to represent and understand the spatial or temporal dynamics of meteorological parameters. Therefore, the aim of this research was to represent temporally through thematic maps, the average daily behavior for meteorological variables and the hydric balance for the municipality of Patos de Minas - MG. The climatic data were acquired from the automatic station INMET from the years 1990 to 2015. Later, it was calculated the evapotranspiration and the hydric balance for different capacities of available water in the soil (CAW): 24 mm, 48 mm, 80 mm and 112 mm. The climate variables showed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Climate; Geostatistical; Ordinary kriging; Thematic maps.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500705

Chemical attributes of soil and dry mass accumulation of maize fertilized with cassava wastewater
Provedor de dados: 70
Autores: Magalhães,Adriana G.; Rolim,Mario M.; Duarte,Anamaria S.; Pedrosa,Elvira M. R.; Silva,Enio F. de F. e.
The aim of this study was to evaluate chemical attributes alterations of a clay-loam textured soil and dry mass accumulation of maize submitted to application of cassava wastewater doses in three assessment periods. The experiment was conducted under greenhouse using a completely randomized experimental design in a factorial 5 × 3, with four replicates. The analyzed factors of research were doses of cassava wastewater (0; 12.6; 25.2; 50.4; 75.6 m3 ha-1) andassessment periods (20, 40 and 52 days after germination). The following parameters were determined: electric conductivity of soil saturation extract, pH in water, content of available P, content of exchangeable K+, Ca2+, Mg2+ and Na+ of soil, dry mass of leaves and stem. The application of cassava...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Residue; Starch; Nutrients; Organic fertilization; Zea mays.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300458

DESIGN AND IMPLEMENTATION OF FLC APPLIED TO A SMART GREENHOUSE
Provedor de dados: 70
Autores: Belkadi,Anouar; Mezghani,Dhafer; Mami,Abdelkader.
ABSTRACT Greenhouse cultivation needs an accurate modelling and an optimised control system to ensure an adequate microclimatic condition for plants. It represents a complex task due to the high number of input factors. For this reason, an improved intermediate modelling was established under the platform of the MATLAB/Simulink environment to simulate the energy balance and the fuzzy logic controller (FLC) in order to promote a suitable microclimate through the control of the relevant actuators which have been installed in the greenhouse. In addition, the control of the system has been improved through the integration of the Internet of things for data monitoring and recording in real time. The system was designed, prototyped, and tested in Tunis province...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuzzy logic; IoT; Microclimatic control; Smart Greenhouse; Wireless connectivity.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600777

SIMILITUDE AND THERMAL PERFORMANCE ON NON-CONVENTIONAL ROOFS
Provedor de dados: 70
Autores: Sampaio,Carlos A. de P.; Terezo,Rodrigo F.; Rosa,Talitha O.; Burigo,Mariana C.; Andrade,Leonardo de B.
ABSTRACT The objectives of this study were to evaluate the thermal comfort and the similitude between prototypes and reduced models, using non-conventional coverage with green roof and expanded clay aggregate, supported on wood frame structure. For this, were determined the Black Globe Temperature and Humidity Index (BGHI), the Human Discomfort Index (HDI), Effective Temperature (ET), Air Temperature (Tair) and Radiant Thermal Load (RTL), from March 2013 to December 2014. The results showed that there were no statistical differences to 5% significance in predicting heat indices between the prototypes and models. Observing all indexes simultaneously, it was observed that January was the month what led to the worst heat conditions, while June and July showed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Non-conventional roofs; Building; Scale; Environmental factors.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100007

Desempenho operacional de conjunto trator-recolhedora de feijão
Provedor de dados: 70
Autores: Garcia,Ricardo F.; Queiroz,Daniel M. de; Fernandes,Haroldo C.; Peternelli,Luiz A.
Estudos sobre a otimização do processo de colheita de grãos, dentre os quais, os de feijão, têm sido realizados pelo desenvolvimento e aperfeiçoamento de máquinas agrícolas, com a finalidade de aumentar o desempenho operacional, tornando-as mais eficientes e seguras, bem como aumentar a qualidade dos grãos colhidos. A avaliação do desempenho operacional de uma máquina viabiliza o seu emprego de forma técnica e economicamente organizada. Diante disso, este trabalho foi desenvolvido com o objetivo de avaliar o desempenho operacional de um conjunto trator-recolhedora de feijão. Foi utilizado um sistema de aquisição automática de dados, o que permitiu a coleta de dados, em tempo real, incluindo torque requerido e rotação da tomada de potência (TDP), e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aquisição de dados; LabVIEW; Mecanização.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100022

SPATIAL VARIABILITY OF SOYBEAN YIELD THROUGH A REPARAMETERIZED T-STUDENT MODEL
Provedor de dados: 70
Autores: Schemmer,Rosangela C.; Uribe-Opazo,Miguel A.; Galea,Manuel; Assumpção,Rosangela A. B.
ABSTRACT: The t-Student distribution has been used to the spatial dependence modelling of soybean yield as an alternative to the normal distribution, being used for data with heavier tails or discrepant values. However, a usual Student t-distribution does not allow direct comparisons of geostatistical methods with a normal distribution. The aim of this study was to assess the soybean yield spatial variability through a reparameterized t-Student linear model, comparing the results with those of a Gaussian linear model. For parameter estimation, a complete maximum likelihood (CML) method was used through an expectation-maximization (EM) algorithm. The maps constructed with both reparameterized t-Student and normal distributions are dissimilar and present a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: EM algorithm; Spatial dependence; Geostatistics; Complete maximum likelihood.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400760

Remoção de sólidos em suspensão na água residuária da despolpa de frutos do cafeeiro em filtros constituídos por pergaminho de grãos de café submetido a compressões
Provedor de dados: 70
Autores: Matos,Antonio T. de; Magalhães,Marcos A.; Fukunaga,Danilo C.
A remoção de sólidos em suspensão é fundamental para que se possa aplicar a água residuária gerada na despolpa de frutos do cafeeiro (ARC) na fertirrigação de culturas agrícolas. Dentre as opções disponíveis para efetuar a remoção de SS da ARC, está o uso de filtros orgânicos. Este trabalho foi desenvolvido com o objetivo de avaliar a influência do grau de compressão na redução do volume e na eficiência do pergaminho, utilizado como material filtrante, na remoção de sólidos em suspensão (SS) na ARC. Numa primeira etapa, foram realizados ensaios nos quais corpos-de-prova de pergaminho triturado (retido entre as peneiras de 2,5 e 3 mm) e não-triturado (na condição em que é produzido) foram submetidos a diferentes compressões para a redução do volume das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Café; Filtros orgânicos; Pergaminho de grãos do café.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200031

Zoneamento bioclimático para vacas leiteiras no Estado da Bahia
Provedor de dados: 70
Autores: Turco,Sílvia H. N.; Silva,Thieres G. F. da; Santos,Luiz F. C. dos; Ribeiro,Paulo H. B.; Araújo,Gherman G. L. de; Holanda Junior,Evandro V.; Aguiar,Mônica A.
Foram utilizados dados meteorológicos médios diários de 437 estações meteorológicas distribuídas por todo o Estado da Bahia para realizar o zoneamento bioclimático de vacas leiteiras e o declínio da produção de leite para vacas com nível de produção de 10 e 25 kg dia-1, nas condições térmicas desse Estado. As variáveis consideradas foram a temperatura (Ta) e a umidade relativa do ar (UR) que foram utilizadas no cálculo do índice de temperatura e umidade (ITU). Estimou-se o declínio da produção de leite (DPL) em função do ITU e do nível de produção (NP). Com os valores de ITU e DPL, foram traçadas as isolinhas dessas duas variáveis para a Bahia por meio do programa SURFER 7.0. Observou-se que, mesmo para os meses com temperaturas mais amenas, há grande...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Produção de leite; Índice de temperatura e umidade; Conforto térmico.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100003

IDENTIFICATION AND QUANTIFICATION OF FACTORS AFFECTING THE OPERATIONAL CAPACITY OF SUGAR CANE HARVESTERS
Provedor de dados: 70
Autores: Silva,João P. de L.; Ralisch,Ricardo; Saab,Otávio J. G. Abi.
ABSTRACT Several studies determined the theoretical and effective capacity of sugarcane harvesters. However, in field conditions, some variables affect sugarcane production and their effect on machine productivity is difficult to measure. The objective of this study is to analyze the correlation of the operational capacity of sugarcane harvesters with property size, sugarcane yield, total operation time of harvesters, and lost productive time. This correlation will be used to construct models that estimate machine capacity under different working conditions. Harvest data were collected from 41 farms with different sizes and rates of productivity, with the harvesting of 412,207 tons of sugarcane by eight harvesters. Property size was the variable that, in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mechanized harvest; Efficiency; Agricultural mechanization.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400563

Nitrogen fertilization by deep bedding swine production and its effects on dry matter production and accumulation of nutrients by maize
Provedor de dados: 70
Autores: Campos,Alessandro T.; Veloso,Alessandro V.; Silva,Enilson B.; Yanagi Júnior,Tadayuki; Mattioli,Matheus C.
The goal of this study was to evaluate the nitrogen fertilization as deep litter for pigs in order to produce biomass and accumulate nutrients by the corn. A deep litter made of rice husk as organic compound, from a commercial pig farm during finishing phase, was used. After three consecutive batches of pigs, the deep litter was subjected to a maturation period of 50 days, and samples of this material were taken for analysis of agronomic value. The experimental design was completely randomized with five replicates. The treatments consisted of doses of 0, 75, 150 and 300mg dm-3 of N of deep litter, as well as an additional treatment with ammonium sulfate, with a dosage of 150mg dm-3 of N. After 45 days, corn plants were harvested in order to evaluate the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pig farming; Pig facilities; Alternative management; Waste treatment; Organic fertilizer; Zea mays.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600018

Design and development of the architecture of an agricultural mobile robot
Provedor de dados: 70
Autores: Tabile,Rubens A; Godoy,Eduardo P; Pereira,Robson R. D; Tangerino,Giovana T; Porto,Arthur J. V; Inamasu,Ricardo Y.
Parameters such as tolerance, scale and agility utilized in data sampling for using in Precision Agriculture required an expressive number of researches and development of techniques and instruments for automation. It is highlighted the employment of methodologies in remote sensing used in coupled to a Geographic Information System (GIS), adapted or developed for agricultural use. Aiming this, the application of Agricultural Mobile Robots is a strong tendency, mainly in the European Union, the USA and Japan. In Brazil, researches are necessary for the development of robotics platforms, serving as a basis for semi-autonomous and autonomous navigation systems. The aim of this work is to describe the project of an experimental platform for data acquisition in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agricultural; CAD; CAE; ISOBUS; Robotic; Sensor.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100013

PAPAYA SEEDLING PRODUCTION UNDER DIFFERENT SHADING LEVELS AND SUBSTRATE COMPOSITIONS
Provedor de dados: 70
Autores: Salles,Josiane S.; Lima,Alexandre H. F. de; Costa,Edilson; Binotti,Eliana D. C.; Binotti,Flávio F. da S.
ABSTRACT Papaya is characterized as one of the most important crops in Brazil. Thus, good quality seedlings are essential for formation of orchards in agricultural production. This study aimed to evaluate shading levels and substrate compositions for production of papaya seedlings. Growing environments were evaluated with 0, 18, 35, and 50% shading and substrates from combinations (%) of hillside soil (HS), cattle manure (CM), Bioplant® (BP), washed fine sand (FS), and super fine-grained vermiculite (FV). As there was no replication for the growing environments, the group of experiments were analyzed using a 4 × 4 factorial arrangement (4 shades × 4 substrates), with five replications. Growth and biometric relationships were analyzed. Substrates consisting...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carica papaya L.; Plant ambience; Cattle manure; Vermiculite.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600698

Pastejo e nitrogênio no azevém sobre a qualidade física do solo e produtividade do feijão
Provedor de dados: 70
Autores: ANDREOLLA,VERUSCHKA R. M.; MORAES,ANÍBAL DE; BONA FILHO,AMADEU; SANDINI,ITACIR E.; BONINI,ANDREIA K.; DEISS,LEONARDO.
O entendimento da interação entre os fatores que compõem o sistema de integração lavoura-pecuária pode direcionar o uso sustentável do solo e das pastagens. Foi estudada a influência do pastejo e doses de nitrogênio em atributos físicos do solo (densidade, macroporosidade, microporosidade, porosidade total e resistência à penetração) e na produtividade da cultura do feijoeiro, em um sistema de integração lavoura-pecuária. O delineamento foi em blocos ao acaso, com parcelas subdivididas e 3 repetições. Os tratamentos foram as doses de nitrogênio de 0; 75; 150 e 225 kg ha-1, na pastagem de azevém (Lolium multiflorum Lam.) no inverno; e na sequência o cultivo do feijoeiro (Phaseolus Vulgaris Lam.), no verão. As subparcelas caracterizaram presença ou ausência...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas integrados; Compactação do solo; Física do solo; Pastagem.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100011

COD, TSS, nutrients and coliforms removals in UASB reactors in two stages treating swine wastewater
Provedor de dados: 70
Autores: Ramires,Roseane Del'Arco; Oliveira,Roberto Alves de.
The performance of two upflow anaerobic sludge blanket (UASB) reactors was evaluated in pilot scale (908 and 188 L), installed in series (R1 and R2), fed with swine wastewater with TSS around 5 and 13 g L-1. The UASB reactors were submitted to HDT of 36 and 18 h with VOL of 5.5 to 34.4 g COD (L d)-1 in the R1 and HDT of 7.5 e 3.7 h with VOL from 5.1 to 45.2 g COD (L d)-1 in the R2. The average removal efficiencies of COD ranged from 55 to 85% in the R1 and from 43 to 57% in the R2, resulting in values from 82 to 93% in the UASB reactors in two stage. Methane concentrations in the biogas were 69 to 74% with specific production from 0.05 to 0.27 L CH4 (g removedCOD)-1 in the R1 and of 0.10 to 0.12 L CH4 (g removedCOD)-1 in the R2. The average removal...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Volumetric organic load; Methane; N and P removal; Metal removal; Suspended solids.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600020

Comportamento de frangos de corte submetidos a diferentes ambientes térmicos
Provedor de dados: 70
Autores: Schiassi,Leonardo; Yanagi Junior,Tadayuki; Ferraz,Patrícia F. P.; Campos,Alessandro T.; Silva,Guilherme R. e; Abreu,Lucas H. P.
É um desafio manter o ambiente térmico, e como as aves alteram seu comportamento em resposta a este ambiente, entender o comportamento dos animais ajuda neste controle. Neste contexto, objetivou-se, com o presente trabalho, avaliar o comportamento de frangos de corte, durante as duas primeiras semanas de vida, submetidos a diversas variações de temperatura do ar em câmaras climáticas. Os animais foram filmados por câmeras de vídeo, possibilitando o monitoramento das aves no estudo dos comportamentos característicos de agrupamento, presença no bebedouro, presença no comedouro e presença em áreas intermediárias. Os resultados mostraram que, em condições de estresse térmico por frio, as aves apresentaram tendência de permanecer maior parte do tempo agrupadas,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência animal; Bioclimatologia; Conforto térmico; Avicultura.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300390

Distribuição de pressão em rede de irrigação localizada otimizada por algoritmos genéticos
Provedor de dados: 70
Autores: Marcuzzo,Francisco F. N.; Wendland,Edson.
Modelos matemáticos computacionais de otimização de redes de irrigação, sob vazão em marcha, capazes de fornecer dados hidráulicos, são importantes para a verificação do comportamento do sistema quanto à distribuição da carga hidráulica (energia) e da pressão nas tubulações da rede. Este trabalho teve como objetivo estudar a distribuição da carga efetiva e hidráulica da unidade operacional de uma rede de irrigação localizada otimizada por algoritmos genéticos. As variáveis de decisão para otimização, com auxílio de algoritmos genéticos, foram os diâmetros de cada trecho da rede: dois para linhas laterais, quatro para linhas de derivação, quatro para linhas secundárias e um para a linha principal. Foi desenvolvido um código em linguagem MatLab, considerando...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Condutos sob pressão; Carga hidráulica; Irrigação por microaspersão; Otimização matemática.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300010

PREDICTIVE MODELS OF WATER APPLICATION AND DISTRIBUTION EFFICIENCY IN CONVENTIONAL SPRINKLING
Provedor de dados: 70
Autores: Araújo,Edcássio D.; Santos,Dionei L.; Alvino,Francisco C. G.; Ferreira,Lucas B.; Cunha,Fernando F. da.
ABSTRACT Correct determinations of distribution (Ed) and application (EA) efficiencies allow adequate estimations of the gross irrigation depth. This study aimed: i) to determine the distribution efficiency using the Christiansen uniformity coefficient (CUC) in a sprinkler irrigation system under different weather conditions and working pressures; ii) to compare the mean, median, and cumulative CUC values; and iii) to evaluate the predictive capacity of four EA estimation models. CUC values were determined from 80 assessments, as well as the mean, median, and cumulative. The precipitated water depth accumulated in each collector was considered for the accumulated CUC. More uniform evaluations were used for EA (working pressure of 196 kPa), resulting in 20...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Uniformity coefficient; Irrigation efficiency; Evaporation and wind drift.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100024

Application of artificial neural networks as an alternative to volumetric water balance in drip irrigation management in watermelon crop
Provedor de dados: 70
Autores: ROCHA NETO,ODÍLIO C. DA; TEIXEIRA,ADUNIAS DOS S.; BRAGA,ARTHUR P. DE S.; SANTOS,CLEMILSON C. DOS; LEÃO,RAIMUNDO A. DE O.
Precision irrigation seeks to establish strategies which achieve an efficient ratio between the volume of water used (reduction in input) and the productivity obtained (increase in production). There are several studies in the literature on strategies for achieving this efficiency, such as those dealing with the method of volumetric water balance (VWB). However, it is also of great practical and economic interest to set up versatile implementations of irrigation strategies that: (i) maintain the performance obtained with other implementations, (ii) rely on few computational resources, (iii) adapt well to field conditions, and (iv) allow easy modification of the irrigation strategy. In this study, such characteristics are achieved when using an Artificial...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision irrigation; Automation; Neural algorithms.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200266

Viabilidade econômica da utilização do biogás produzido em granja suínícola para geração de energia elétrica
Provedor de dados: 70
Autores: Cervi,Ricardo G.; Esperancini,Maura S. T.; Bueno,Osmar de C.
A produção de biogás por meio de biodigestão anaeróbia representa um avanço para equacionar o problema dos dejetos produzidos pela suinocultura e disponibilidade de energia no meio rural. Este trabalho teve como objetivo estimar a viabilidade econômica de um sistema biointegrado para geração de eletricidade a partir do aproveitamento de dejetos de suínos. Os dados para este estudo foram coletados em uma agroindústria, onde são realizadas diversas atividades agrícolas; entretanto, a suinocultura foi selecionada para o processo de análise de biodigestão anaeróbia, pelo fato de gerar uma grande quantidade de dejetos, com dificuldade de disposição no meio ambiente, configurando um estudo de caso. O biodigestor analisado é um modelo tubular contínuo, com calha...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogás; Energia elétrica; Viabilidade econômica.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500006

Manejo da irrigação (tensiometria e balanço hídrico climatológico) para a cultura do feijoeiro em sistemas de cultivo direto e convencional
Provedor de dados: 70
Autores: Lopes,Adriano S.; Pavani,Luiz C.; Corá,José E.; Zanini,José R.; Miranda,Hector A.
Dois métodos de manejo de irrigação, por tensiometria e pelo balanço hídrico climatológico simplificado baseado no tanque "Classe A", foram aplicados e avaliados os resultados no balanço de água no solo, na evapotranspiração e na produtividade de grãos da cultura do feijoeiro, cultivar IAC-Carioca, conduzida na estação seca com irrigação por pivô central, após uma cultura de milho (estação úmida), no primeiro ano de cultivo, nos sistemas de plantio direto e convencional em uma área de Latossolo Vermelho. Concluiu-se que ambos os métodos são possíveis de serem adotados por irrigantes ou técnicos com níveis médios de tecnologia e conhecimento, embora com a tensiometria seja possível um melhor entendimento das reais condições hídricas do solo na região do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água no solo; Evapotranspiração; Pivô central.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100011

Economic viability of retrofiting emitters in center pivot irrigation systems
Provedor de dados: 70
Autores: Zolin,Cornélio A.; Coelho,Rubens D.; Paulino,Janaina; Folegatti,Marcos V.
Although several studies have been conducted to evaluate the uniformity of water application under center pivot irrigation systems, there are few studies concerning the economic perspective of such coefficient. The aim of this study is to present a methodology to accomplish an economic analysis as support for the decision-making to retrofit emitters in center pivot irrigation systems, and to attribute an economic meaning to the uniformity coefficient of water application taking into account the response function productivity to the amount of water applied and the sale price of the crops. In the hypothetic calculation example considering the variation of revenue of potato crop under center pivot irrigation system, it was verified that the area with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Heermann's uniformity coefficient; Production function; Sale price of crops.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300019

Avaliação de lavagem parcial de sais em neossolo flúvico irrigado, utilizando modelagem computacional
Provedor de dados: 70
Autores: Monteiro,Adriano L. N.; Montenegro,Abelardo A. de A.; Montenegro,Suzana M. G.; Santos,Francisco X. dos.
Este trabalho foi realizado em um vale aluvial irrigado do semiárido do Brasil (Estado de Pernambuco). O objetivo foi investigar o efeito de lâminas de lixiviação e de precipitação no controle da salinidade do solo em lisímetros de drenagem. Com base em simulações numéricas, utilizando-se do modelo HYDRUS-1D, avaliaram-se o fluxo e o transporte de sais na zona não saturada. Mediante medidas de campo de evapotranspiração real e precipitação, foi possível inferir que o modelo se apresentou como ferramenta adequada nas simulações realizadas, para diferentes cenários de lâminas de lixiviação. Verificou-se, experimental e numericamente, que a lixiviação parcial pode ser utilizada como alternativa de manejo para a redução da salinidade na zona radicular, desde...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semiárido; Salinidade; Aquífero aluvial.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200004

Uso de análise multivariada na classificação das fontes hídricas superficiais da bacia hidrográfica do Salitre
Provedor de dados: 70
Autores: Brito,Luiza T. de L.; Silva,Aderaldo de S.; Srinivasan,Vajapeyam S.; Galvão,Carlos de O.; Gheyi,Hans R.
Identificar as variáveis de maior significância na qualidade das águas da bacia hidrográfica do Salitre e classificar as fontes hídricas, segundo suas características, foi o objetivo principal deste trabalho. A partir dos resultados obtidos para as barragens/açudes, observa-se que a análise fatorial apresentou três fatores principais que explicam 83,50% e 74,98% da variância acumulada, enquanto, para os rios/riachos, explicaram 86,92% e 71,25%, nos períodos de chuvas e sem chuvas de 2001, respectivamente. As variáveis priorizadas no Fator 1, independentemente das fontes hídricas e dos períodos, estão diretamente relacionadas com a salinidade das águas. As fontes hídricas foram agrupadas em três classes, de forma que a classe C1 apresentou melhor qualidade...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Impactos ambientais; Irrigação; Agrupamento.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100007

Estimativa de produtividade da cultura do feijão irrigado em Cristalina-GO, para diferentes lâminas de irrigação como função da uniformidade de aplicação
Provedor de dados: 70
Autores: Mantovani,Everardo C.; Montes,David R. P.; Vieira,Gustavo H. S.; Ramos,Márcio M.; Soares,Antônio A.
O estudo foi realizado por meio de simulações, inseridas em seis cenários de níveis de uniformidade de aplicação de água, nas condições de Cristalina-GO, com o objetivo de avaliar o efeito da aplicação de diferentes lâminas de irrigação na produtividade comercial da cultura do feijão (Phaseolus vulgaris L.) cv. Carioca. Para tanto, utilizou-se o sistema de irrigação por aspersão convencional, mediante dados de produtividade obtidos por intermédio da função de produtividade desenvolvida para as condições locais. Os resultados obtidos permitiram concluir que a maior produtividade de grãos (2.946,52 kg ha-1) foi obtida com o maior coeficiente de uniformidade de aplicação da água do sistema de irrigação por aspersão (90%), que resultou no menor valor de lâmina...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus vulgaris; Irrigação; Função de produtividade; Aspersão; Eficiência de irrigação.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100012

Filtros de areia aplicados à irrigação localizada: teoria e prática
Provedor de dados: 70
Autores: Testezlaf,Roberto.
A aplicação de filtros de areia em sistemas de irrigação localizada é recomendada quando a água possui contaminação orgânica e de algas. O correto dimensionamento e manutenção desses equipamentos são essenciais para garantir o controle efetivo da qualidade da água de irrigação, visando a reduzir a obstrução de emissores, a manter a uniformidade de aplicação de água e a evitar o aumento nos custos de operação do sistema. Apesar da existência de informações técnicas sobre o projeto, a operação e a manutenção desses filtros na literatura, elas estão dispersas e com detalhamento insuficiente para permitir otimização do dimensionamento da estrutura hidráulica e da escolha do meio poroso a ser utilizado. Dessa forma, o objetivo deste trabalho é apresentar uma...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Filtração; Obstrução de emissores; Meios porosos.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300020

Distribuição de poros de um latossolo vermelho eutroférrico na fase de implantação de um sistema de plantio direto
Provedor de dados: 70
Autores: Laurani,Raffael A.; Ralisch,Ricardo; Tavares Filho,João; Soares,Décio S.; Ribon,Adriana A.
O estudo da distribuição de poros é importante na avaliação física do solo submetido a diferentes sistemas de produção. O objetivo deste trabalho foi avaliar a distribuição de poros de um Latossolo Vermelho Eutroférrico, como um parâmetro de sua qualidade física para analisar sua eficiência na implantação do sistema de plantio direto. Empregou-se um delineamento experimental inteiramente casualizado, com quatro tratamentos, na rotação de inverno (milho safrinha, coquetel de adubos verdes, aveia-preta e trigo) e duas profundidades (0-0,2 m e 0,2-0,4 m), com três repetições por tratamento. Após três anos de implantação dos tratamentos (coberturas vegetais), foram realizadas determinações físicas (densidade do solo), fisico-hídricas do solo (macroporosidade,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Porosidade; Curva de retenção; Manejo do solo.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200013

Segregação de fertilizantes aplicados a lanço
Provedor de dados: 70
Autores: Molin,José P.; Machado,Thiago M.; Magalhães,Raphael P.; Faulin,Gustavo D. C.
A uniformidade transversal da distribuição de fertilizantes e corretivos a lanço tem grande dependência da qualidade e da condição física do produto a ser aplicado. Especialmente no caso das formulações, esse aspecto é relevante e por isso o presente trabalho teve o objetivo de verificar a distribuição dos grãos e a constância na formulação aplicada na extensão da largura de trabalho de uma máquina distribuidora a lanço com dois fertilizantes. Foram efetuadas análises químicas do produto depositado em coletores dispostos transversalmente e analisadas as distribuições individuais dos elementos das fórmulas. Os resultados evidenciam que os fertilizantes apresentaram diferenças na sua formulação ao longo da largura, sendo que o fertilizante que continha...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aplicação a lanço; Deposição transversal; Adubadora.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400011

ERRATUM
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100121

Physical-chemical characterization and wet milling yield of four maize hybrids
Provedor de dados: 70
Autores: Mussolini,Renata C.; Lopes Filho,José F.; Duarte,Aildson P.
The influence of physical-chemical characteristics of maize grains and lactic acid concentrations on byproduct yields, generated by conventional wet milling, was studied during steeping, for four maize hybrids and two lactic acid concentrations (0.55 and 1.00%). For physical-chemical characterization, grain dimensions (length, thickness, and width) were determined, as well as mass of 100 grains, percentage of floating grains, volumetric mass, and centesimal composition. Statistical differences were found for percentage of floating grains (2.33 to 24.67%), volumetric mass (0.814 to 0.850 kg.L-1), mass of 100 grains (0.033 to 0.037 kg), water content (11.86 to 12.20%), proteins (8.21 to 9.06%), lipids (3.00 to 4.77%), and ashes (1.07 to 1.26%). There were no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays L.; Physical-chemical properties; Starch recovery; Steeping.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300015

Sequências de dias chuvosos: fator de risco à colheita em Goiás
Provedor de dados: 70
Autores: Mesquita,Wilson O.; Griebeler,Nori P.; Correchel,Vladia.
O objetivo deste trabalho foi estabelecer sequências de dias chuvosos como fator de risco à colheita no Estado de Goiás. Para isso, foram utilizadas séries históricas pluviométricas, com período de base de, no mínimo, 17 anos referentes a 36 estações pluviométricas localizadas neste Estado. As sequências de dias chuvosos foram separadas por uma rotina computacional para os meses de dezembro, janeiro, fevereiro e março. Para o estudo de probabilidade destas sequências, utilizou-se a Distribuição Binominal Negativa Truncada (DBNT). A aderência da distribuição às sequências de dias chuvosos foi verificada, utilizando-se do teste de Qui-quadrado (χ²). Os resultados foram espacializados, de modo a facilitar a visualização da distribuição espacial das sequências...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Distribuição binominal; Precipitação; Espacialização; Sequências de precipitações.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300004

MANAGEMENT CLASS DELIMITATION IN A SOYBEAN CROP USING ORBITAL IMAGES
Provedor de dados: 70
Autores: Zanella,Marco A.; Queiroz,Daniel M. de; Valente,Domingos S. M.; Pinto,Francisco de A. de C.; Santos,Nerilson T.
ABSTRACT The delimitation of management classes is critical for successful precision agriculture. This process involves choosing the variables to use and analyzing the spatial variability of the variables. Thus, the objective of this study was to analyze the correlation between management class maps generated from orbital images and yield maps. A 95-hectare area of rainfed grain was evaluated. Yield maps were obtained for the 2015/2016 and 2016/2017 soybean crops. Orbital images were used from two dates for each crop to generate vegetation index maps. The spatial correlation between the vegetation indices and the yield maps was obtained using a bivariate Moran index. The delineated management classes were compared using the Kappa index. This study...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Vegetation index; Yield map.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500676

Adaptação e avaliação do modelo infocrop para simulação do rendimento de grãos da cultura do arroz irrigado
Provedor de dados: 70
Autores: Walter,Lidiane C.; Rosa,Hamilton T.; Streck,Nereu A.; Ferraz,Simone E. T.
Este trabalho teve como objetivo adaptar e avaliar o modelo InfoCrop para simulação do rendimento de grãos da cultura do arroz irrigado, em Santa Maria - RS. O rendimento de grãos da cultura do arroz irrigado foi simulado, considerando-se três versões do modelo InfoCrop com adaptações para cultivares locais. Os rendimentos simulados foram comparados com os rendimentos observados no município de Santa Maria, no período 1996/1997 a 2008/2009, disponibilizados pelo Instituto Riograndense do Arroz (IRGA), e com rendimentos de experimentos realizados na Universidade Federal de Santa Maria (UFSM), entre os anos agrícolas de 1998/1999 e 2005/2006. O modelo InfoCrop capturou a variação interanual do rendimento de grãos de arroz irrigado para o município de Santa...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelagem matemática; Grãos; Produtividade; Oryza sativa.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300010

Development of experimental structure and influence of high CO2 concentration in maize cro
Provedor de dados: 70
Autores: Silva,João B. Lopes da; Ferreira,Paulo A.; Pereira,Eduardo G.; Costa,Luís C.; Miranda,Glauco V.
Maize is a C4 plant that shows few or no response to high [CO2]. Thus, this study aimed to analyze the photosynthetic rate and yield of maize under high [CO2] and develop open-top chambers (OTC) to create an atmosphere enriched with CO2. The experiment was conducted between October 2008 and March 2009. The OTCs were developed in modular scheme. Measurement of photosynthetic rates, transpiration, stomata conductance, grain yield and dry matter were performed. The experimental design was randomized blocks with four replications and three treatments: P1 - plants grown in OTC with 700 ppm [CO2], P2 - plants grown in OTC with environmental [CO2], and P3 - control, cultivated in open field. The results were analyzed by ANOVA and Tukey's test (Pr&lt; 0.05). The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Open-top chambers; Climate change; Zea mays L.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200010

Yield of cotton/cowpea and sunflower/cowpea crop rotation systems during the reclamation process of a saline-sodic soil
Provedor de dados: 70
Autores: Sousa,Carlos H. C. de; Lacerda,Claudivan F. de; Silva,Francisco L. B. da; Neves,Antonia L. R.; Costa,Raimundo N. T.; Gheyi,Hans R.
The objective of this study was to evaluate the use of subsoiling, gypsum and organic matter associated with the cultivation of cotton, sunflower and cowpea in crop rotation, seeking the reclamation and use of a saline-sodic soil. The treatments were arranged in a randomized block design in split plots with four replications, during two crop cycles (2009/2010 and 2010/2011). The plots were formed by the treatments: T1. Subsoiling (S); T2. S + 20 Mg ha-1 of gypsum; T3. S + 40 Mg ha-1 of organic matter; T4. S + 10 Mg ha-1 of gypsum + 20 Mg ha-1 of organic matter; T5. S + 20 Mg ha-1 of gypsum + 40 Mg ha-1 of organic matter and the sub-plots consisted of the cotton-cowpea (C/CP) and sunflower-cowpea (S/CP) crop rotation. The use of gypsum and organic matter...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Salinity; Sodicity; Gossypium hirsutum; Helianthus annuus; Vigna unguiculata.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500006

Experimental evaluation of the performance of a wireless sensor network in agricultural environments
Provedor de dados: 70
Autores: Roccia,Clerivaldo; Teruel,Bárbara; Alves,Elaine C. de S.; Arnold,Francisco; Bravo-Roger,Leonardo; Moretti,Angelo; Gonçalves,Marcos S.
The aim of this study was to perform an experimental study to evaluate the proper operation distance between the nodes of a wireless sensor network available on the market for different agricultural crops (maize, physic nut, eucalyptus). The experimental data of the network performance offers to farmers and researchers information that might be useful to the sizing and project of the wireless sensor networks in similar situations to those studied. The evaluation showed that the separation of the nodes depends on the type of culture and it is a critical factor to ensure the feasibility of using WSN. In the configuration used, sending packets every 2 seconds, the battery life was about four days. Therefore, the autonomy may be increased with a longer...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Maize (Zea mays L); Physic nut (Jatropha curcas); Eucalyptus (Eucalyptus grandis); Precision agriculture; Zigbee technology.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600018

Avaliação do espectro de gotas de pontas de pulverização hidráulicas utilizando a técnica da difração do raio laser
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Teixeira,Mauri M.; Fernandes,Haroldo C.
As pontas de pulverização são os componentes mais importantes dos pulverizadores na aplicação de agrotóxicos. Dessa forma, este trabalho teve como objetivo avaliar o espectro de gotas de pontas de pulverização hidráulicas de jato plano (standard e antideriva) e de jato cônico vazio, disponíveis no mercado, submetidas a diferentes pressões da calda. Em ambiente controlado, avaliou-se o espectro de gotas, por meio de um analisador a laser de gotas em tempo real, nas pressões de 200; 300 e 400 kPa para as pontas de jato plano, e de 400; 500 e 600 kPa para as pontas de jato cônico. Os resultados permitiram concluir que: o espectro de gotas foi influenciado pela vazão nominal das pontas e pela pressão da calda; o potencial de deriva das pontas de jato plano...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Agrotóxicos; Pulverizadores.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200002

Anaerobic-aerobic treatment of swine wastewater in uasb and batch reactors in series
Provedor de dados: 70
Autores: Urbinati,Estevão; Oliveira,Roberto Alves de.
In this work it was evaluated the performance of two systems of swine wastewater treatment consisting of two-stage upflow anaerobic sludge blanket (UASB) reactors, with and without post-treatment in sequencing batch reactor (SBR), fed continuously, with aerobic phase. The UASB reactors in the first stage had 908 L in the sets I and II, and in the second stage 350 and 188 L, respectively. In the set II the post-treatment was performed in a SBR of 3,000 L. The hydraulic detention times in the anaerobic treatment systems were 100, 75 and 58 h in the set I; 87, 65 and 51 h in the set II; and 240 and 180 h in the SBR. The volumetric organic load applied in the first stage UASB reactors ranged from 6.9 to 12.6 g total COD (L d)-1 in the set I and 7.5 to 9.8 g...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coliforms; Methane; Two-stage anaerobic reactors; Nutrients removal; Combined treatment.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100014

GEOCHEMICAL BACKGROUND IN AN OXISOL
Provedor de dados: 70
Autores: Cembranel,Adir S.; Sampaio,Silvio C.; Remor,Marcelo B.; Gotardo,Jackeline T.; Rosa,Pábolla M. Dalla.
ABSTRACT Geochemical background establishment is indispensable to determine the actual state of contamination of soils and sediments. However, no scientific consensus exists regarding the methodology for determining these values. In this context, this study aimed to establish the geochemical background in an Oxisol (Rhodic Hapludox) by means of an integrated method that uses direct and indirect soil analyses to identify the most appropriate calculation methodology. Soil samples were collected in a permanent preservation area of the Cascavel River watershed, PR, Brazil. The elements Cd, Co, Cr, Cu, Fe, K, Mg, Mn, Na, Ni, Pb, and Zn present in soil samples were quantified by flame atomic absorption spectrometry. The use of a permanent preservation area is...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Trace elements; Heavy metals; Sediment; Soil.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300565

Ratoon sugarcane yield integrated drip-irrigation and nitrogen fertilization
Provedor de dados: 70
Autores: Uribe,Raúl A. M.; Gava,Glauber J. de C.; Saad,João C. C.; Kölln,Oriel T.
The aim of this study was to compare the use of water and nitrogen on ratoon sugarcane during irrigated and rain-fed conditions, and to assess the production potential of stalks and sugar with different rates of N-fertilizer on the subsurface drip-irrigated management. The experimental design was a randomized block with four replications for each experiment and treatments: (T1) irrigated, 0kg N ha-1; (T2) irrigated, 70kg N ha-1; (T3) irrigated, 140kg N ha-1; (T4) irrigated, 210kg N ha-1; (T5) not irrigated, 0kg N ha-1, and (T6) not irrigated, 140kg N ha-1. Biometric, technological, dry matter and yield variables were analyzed among the treatments. The irrigation system together with the application of N-fertilizer at 140kg ha-1 presented significant...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertigation; Nitrogen; Water stress; Sacharum spp.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600005

SOIL ATTRIBUTES AND INITIAL CORN DEVELOPMENT AS A FUNCTION OF FERTILIZATION AND INTERCROPPING SYSTEMS
Provedor de dados: 70
Autores: Cortez,Jorge W.; Silva,Rouverson P. da; Furlani,Carlos E. A.; Olszevski,Nelci; Nagahama,Hideo de J.
ABSTRACT Fertilization systems that allow higher sowing speeds have been used in areas of grain production, as well as the use of intercropping to improve soil physical quality and provide better soil cover. This study aimed to evaluate soil attributes and the initial corn development and intercropping (corn + velvet bean, corn + pigeonpea, and corn + bonavist bean) as a function of fertilization systems (pre-sowing and sowing). The experiment was conducted in an Oxisol in a randomized block design in the 2 × 3 factorial scheme, with four replications. The number of days for emergence, plant stand, intercropping dry matter, soil straw cover, soil straw permanence index, penetration resistance, soil moisture, soil density, degree of compaction, and total...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compaction; Vegetation cover; Soil physical quality.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200257

Influence of vinasse application in hydraulic conductivity of three soils
Provedor de dados: 70
Autores: Uyeda,Claudio A.; Miranda,Jarbas H. de; Duarte,Sergio N.; Medeiros,Pedro R. F. de; Dias,Carlos T. dos S.
The potassium ion, present in great amount in the vinasse because it is a monovalent cation, has the characteristic of promoting the dispersion of clay particles, in the same way as the sodium, causing a reduction in the pore space of the soil and, in its turn, reducing its permeability. To evaluate this effect of reduction by application of vinasse to the soil, an experiment was conducted for three different soils, with the objective of evaluating the effect of the application of different doses of vinasse on hydraulic conductivity of saturated soil and verifying its possible chemical changes of these soils. For that, it was used PVC columns (in a scheme of constant head permeameter to obtain the values of hydraulic conductivity of saturated soil), filled...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Clay dispersion; Potassium; Soil permeability.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400008

Spatio-temporal modelling of the duration of the cotton cycle in the State Of Goiás, Brazil
Provedor de dados: 70
Autores: Antonini,Jorge C. dos A.; Silva,Euzebio M. da; Griebeler,Nori P.; Sano,Edson E.
The objective of this work was to develop and validate a mathematical model to estimate the duration of cotton (Gossypium hirsutum L. r. latifolium hutch) cycle in the State of Goiás, Brazil, by applying the method of growing degree-days (GD), and considering, simultaneously, its time-space variation. The model was developed as a linear combination of elevation, latitude, longitude, and Fourier series of time variation. The model parameters were adjusted by using multiple-linear regression to the observed GD accumulated with air temperature in the range of 15°C to 40°C. The minimum and maximum temperature records used to calculate the GD were obtained from 21 meteorological stations, considering data varying from 8 to 20 years of observation. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Growing degree-days; Base temperature; Thermal requirement; Fourier series.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400004

Mensuração da condutividade elétrica do solo por indução e sua correlação com fatores de produção
Provedor de dados: 70
Autores: Molin,José P.; Gimenez,Leandro M.; Pauletti,Volnei; Schmidhalter,Urs; Hammer,Jens.
A condutividade elétrica (CE) do solo, obtida por contato ou por indução eletromagnética, tem sido utilizada como uma variável que se correlaciona com características do solo. Investigaram-se as relações existentes entre a CE medida com um sensor de indução eletromagnética, a granulometria do solo, umidade e fatores da fertilidade, a topografia do terreno e a produtividade de milho e soja, em uma lavoura de 19 ha, conduzida sob semeadura direta, entre 2000 e 2002. A produtividade das culturas foi obtida com monitor comercial, e a CE e os demais parâmetros foram obtidos por amostragem em grade regular. Os dados foram espacializados para a produção dos mapas que serviram para a análise de correlações entre os fatores. O sensor de condutividade elétrica...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Variabilidade espacial; Fatores de produção.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200015

Identification, assessment and ordering of concepts for agro-energy planning and possibilities of spatial analysis
Provedor de dados: 70
Autores: Cervi,Walter R.; Lamparelli,Rubens; Berni,Mauro; Rocha,Jansle.
ABSTRACT The present study aims to present the main concepts of the sugarcane straw to energy planning. Throughout the study, the subject is contextualized highlighting broader aspects of sustainability, which is considered the main driver towards agro-energy modernization. Concerning sugarcane straw, we first evaluated its availability regarding technical and economic aspects, and then it summarized the straw production chain for energy supply purposes. As a proposal to support agro-energy planning, it is presented some spatial tools that have been barely used in the Brazilian energy planning context so far. Therefore, working on straw to electricity associated with supply chain basis, we developed a conceptual model to spatially assess this bioenergy...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sugarcane; Straw; Agro-energy planning; Geographic information system.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601210

Technical and economic analysis of irrigation of asparagus bean in protected environment
Provedor de dados: 70
Autores: Silva,Wellington G.; Carvalho,Jacinto A.; Oliveira,Eduardo C.; Lima Júnior,Joaquim A.; Silva,Buno M.
This experiment was conducted in Lavras - state of Minas Gerais (MG), Brazil, in a protected environment, and aims to estimate the irrigation depths that maximize productivity and economic returns in the cultivation of asparagus bean and analyze the economic viability of irrigation management. The experimental delineation was randomized blocks with five treatments and four replications. The treatments consisted of five drip irrigation depths: 40, 70, 100, 130 and 160% of water replacement depth up to field capacity. The depths of water that maximize productivity and economic returns were obtained from the regression model adjusted to productivity data, cost of product relations and water cost. The economic viability was achieved on the benefit/cost ratio...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vigna unguiculata spp. sesquipedalis; Irrigation management; Economic viability; Benefit/cost ratio.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400007

INFLUENCE OF OPERATIONAL CONDITIONS OF MECHANIZED HARVESTING ON SUGARCANE LOSSES AND IMPURITIES
Provedor de dados: 70
Autores: Martins,Murilo B.; Ruiz,Daniel.
ABSTRACT Operational conditions of mechanized harvesting can affect the quality of harvested sugarcane. Therefore, the aim of this study was to assess the influence of the displacement speed and cutting height on the quality of the raw material during the mechanized harvest of sugarcane. Vegetable losses were accounted for in the field by manual collection of the fractions left after harvest. Vegetable and mineral impurities were determined at the processing stage in the laboratory. Both the displacement speed and cutting height did not affect vegetable losses. However, the increase in vegetal impurities occurred at higher displacement speeds, whereas lower cutting heights resulted in higher amounts of mineral impurities.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural mechanization; Harvest; Quality; Saccharum spp.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300352

OPTIMIZATION OF ANAEROBIC TREATMENT OF CASSAVA PROCESSING WASTEWATER
Provedor de dados: 70
Autores: Fleck,Leandro; Tavares,Maria H. F.; Eyng,Eduardo; Andrade,Minéia A. de M. de; Frare,Laercio M.
ABSTRACT The main contribution of this research is to optimize the operating conditions of an anaerobic reactor applied to the treatment of wastewater from cassava starch production. A 20-L anaerobic reactor was used, operating in a batch system, with temperature control. Temperature and inoculum total volatile solids (TVSi) were controlled for evaluation of effects on the removals of chemical oxygen demand (COD) and reactor total volatile solids (TVSr) by means of a Central Composite Rotational Design (CCRD). Twelve trials were analyzed simultaneously by the desirable function approach. The higher COD removal (96.82%) was obtained at 42 °C and 12.0% TVSi. The largest TVSr removal (69.31%) was registered at 45 °C and 10.0% TVSi. Equations representative of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anaerobic reactor; Biogas; Desirability function; Mathematical modeling.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300574

Técnicas de diagnóstico de influência local na análise espacial da produtividade da soja
Provedor de dados: 70
Autores: Borssoi,Joelmir A.; Uribe-Opazo,Miguel A.; Galea,Manuel.
A modelagem da estrutura de dependência espacial pela abordagem da geoestatística é fundamental para a definição de parâmetros que definem esta estrutura, e que são utilizados na interpolação de valores em locais não amostrados pela técnica de krigagem. Entretanto, a estimação de parâmetros pode ser muito afetada pela presença de observações atípicas nos dados amostrados. O desenvolvimento deste trabalho teve por objetivo utilizar técnicas de diagnóstico de influência local em modelos espaciais lineares gaussianos, utilizados em geoestatística, para avaliar a sensibilidade dos estimadores de máxima verossimilhança e máxima verossimilhança restrita na presença de dados discrepantes. Estudos com dados experimentais mostraram que tanto a presença de valores...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Máxima verossimilhança; Máxima verossimilhança restrita.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200018

Sensoriamento remoto na identificação do uso e ocupação da terra na área do projeto "Conquista da Água", Ilha Solteira - SP, Brasil
Provedor de dados: 70
Autores: Silva,Hélio R.; Altimare,André L.; Lima,Elizete A. C. de Freitas.
A cidade de Ilha Solteira está propondo o projeto "Conquista da Água", visando ao desenvolvimento sustentável do Município, a partir do turismo, da cultura e da ciência e tecnologia. Para atingir esse objetivo, os planejadores do meio físico-ambiental necessitam de dados que possam auxiliá-los na seleção dos melhores locais onde serão instalados as avenidas, o aeroporto e os demais espaços que comporão esse projeto. A elaboração do mapa de uso e cobertura do solo da área de interesse do projeto constitui um dos temas necessários ao banco de dados a ser utilizado pelos planejadores. Neste trabalho, é apresentado o estado de degradação dessa área, o que auxiliará na definição das estratégias de conservação ambiental.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Desenvolvimento sustentável; Geoprocessamento; Mapas.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100035

Crop residues on short-term CO2 emissions in sugarcane production areas
Provedor de dados: 70
Autores: Corradi,Mariana M.; Panosso,Alan R.; Martins Filho,Marcílio V.; La Scala Junior,Newton.
The proper management of agricultural crop residues could produce benefits in a warmer, more drought-prone world. Field experiments were conducted in sugarcane production areas in the Southern Brazil to assess the influence of crop residues on the soil surface in short-term CO2 emissions. The study was carried out over a period of 50 days after establishing 6 plots with and without crop residues applied to the soil surface. The effects of sugarcane residues on CO2 emissions were immediate; the emissions from residue-covered plots with equivalent densities of 3 (D50) and 6 (D100) t ha-1 (dry mass) were less than those from non-covered plots (D0). Additionally, the covered fields had lower soil temperatures and higher soil moisture for most of the studied...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil respiration; Sugarcane management; Green harvest.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400009

Effect of trickle irrigation on root development of the wet bulb and 'pera' orange tree yield in the state of São Paulo, Brazil
Provedor de dados: 70
Autores: Pires,Regina C. de M; Bodine Junior,Décio; Sakai,Emílio; Villar,Heloísa L; Silva,Tonny J. A. da; Arruda,Flávio B.
The aim of this study was to evaluate the effect of different microirrigation designs on root system distribution in wet bulb region, orange orchard yield and quality of orange fruits. The experiment was installed as random blocks with five treatments and four replicates in an orchard of 'Pêra' orange trees grafted on 'Cleopatra' mandarin rootstock. The treatments consisted of: one drip line (T1), two drip lines (T2), four drip lines (T3) per planting row, microsprinkler irrigation (T4) and without irrigation (T5). Irrigation treatments favored yield and ºBrix. The treatment with a single drip line (T1) showed the greatest quantity of roots in relation to the treatments T2 and T3.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Trickle irrigation; Microsprinkler irrigation; Citrus; Water management.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600007

Influência da distância entre passadas de colhedora equipada com monitor de colheita na precisão dos mapas de produtividade na cultura do milho
Provedor de dados: 70
Autores: Bazzi,Cláudio L.; Souza,Eduardo G.; Opazo,Miguel A. Uribe; Nóbrega,Lúcia H. P.; Pinheiro Neto,Raimundo.
Um dos entraves para a maior expansão da agricultura de precisão está, principalmente, no elevado custo dos equipamentos a serem utilizados. A geração de mapas de produtividade é a fase de mais fácil execução na agricultura de precisão. Entretanto, quando várias colhedoras operam simultaneamente em uma determinada área, nem sempre é possível dispor de monitores de colheita em todas as máquinas. Assim, neste trabalho, foi avaliado o decréscimo da precisão em mapas de produtividade obtidos a partir de áreas onde se utilizaram colhedoras não-equipadas com monitor de colheita associadas a colhedoras monitoradas. Também foram comparados os métodos de interpolação "inverso da distância ao quadrado" e "krigagem". Inicialmente, a interpolação do mapa com todos os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Métodos de interpolação; Mapas temáticos.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200016

Efeitos da aplicação de efluente de tratamento de esgoto na fertilidade do solo e produtividade de pepino sob irrigação subsuperficial
Provedor de dados: 70
Autores: Azevedo,Leonardo P. de; Oliveira,Eduardo L. de.
O experimento foi conduzido com o objetivo de avaliar técnicas para a aplicação de águas residuárias na agricultura, proporcionando melhor reutilização de água, recurso natural atualmente escasso e muito mal disponibilizado. Utilizou-se da cultura de pepino (Cucumis sativus L.) em estufa, com oito parcelas irrigadas com efluentes de tratamento de esgoto residencial e oito parcelas irrigadas com água tratada e distribuída pela SABESP (tratamento-testemunha), ambas abastecidas por sistema de irrigação subsuperficial, avaliando-se a produção média por planta, a fertilidade do solo e a disposição de nutrientes na água do solo. Nas análises do solo, verificaram-se maiores teores de P, K e CTC no solo irrigado com efluentes. Nesse mesmo tratamento,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Águas residuárias; Irrigação localizada; Cucumis sativus L.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100028

Fungicide application using a trailing boom in soybean fields
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Fornari,Allison J.; Bauer,Fernando C.; Justino,Altair; Garcia,Luiz C.
The objective of this study was to determine the effects in the yield of soybean crop utilizing a trailing boom sprayer for chemical control of late season diseases. The experimental design was randomized blocks with 04 treatments, which consisted of applying fungicides with a traditional sprayer, trailing boom, the traditional sprayer plus the trailing boom simultaneously and control (without fungicide aerial application) in 05 repetitions per treatment. The variables evaluated were: final plant population, pods per plant, grains per pod, weight of one thousand grains and yield. It was concluded that the control of foliar diseases with fungicides presented weight of one thousand grains and yield significantly higher than the average of plots without...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Late season diseases; Spray boom; Yield components.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400026

BIOPHOTONICS: ACCLIMATION OF PRE-SPROUTED SUGARCANE SEEDLINGS IN PROTECTED ENVIRONMENT
Provedor de dados: 70
Autores: Almeida Neto,Luiz A.; Pandorfi,Héliton; Moraes,Alex S.; Guiselini,Cristiane; C. Júnior,José J. Florentino.
ABSTRACT Sugarcane is considered one of the main alternatives for biofuel production and an important product of Brazilian agriculture, so it is indispensable to adopt new techniques for its cultivation and management. Thus, the present study aimed to evaluate the effect of the quality of supplemental lighting, based on light-emitting diode (LED), on the acclimation of pre-sprouted sugarcane seedlings in a protected environment. The experimental design was completely randomized, consisting of three supplemental LED lighting systems, with light proportions of 90% red + 10% blue (R:B 90/10), 80% red + 20% blue (R:B 80/20) and 70% red + 30% blue (R:B 70/30), and a control, with natural solar radiation, with 5 replicates. Multivariate principal component...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Principal components; Light-emitting diode; Supplemental lighting; Solar radiation.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400410

Method of numerical correction of errors occasioned by delay of records during the monitoring of environmental variables of interest for animal production
Provedor de dados: 70
Autores: Gabriel Filho,Luís R. A.; Pereira,Danilo F.; Barato,Fernando F.; De Magalhães,Marcelo M.
Thermal and air conditions inside animal facilities change during the day due to the influence of the external environment. For statistical and geostatistical analyses to be representative, a large number of points spatially distributed in the facility area must be monitored. This work suggests that the time variation of environmental variables of interest for animal production, monitored within animal facility, can be modeled accurately from discrete-time records. The aim of this study was to develop a numerical method to correct the temporal variations of these environmental variables, transforming the data so that such observations are independent of the time spent during the measurement. The proposed method approached values recorded with time delays...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatistical; Animal precision production; Mathematical methods.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500001

RAINFALL ZONING FOR COCOA GROWING IN BAHIA STATE (BRAZIL) USING FUZZY LOGIC
Provedor de dados: 70
Autores: Franco,Laís B.; Almeida,Ceres D. G. C. de; Freire,Martiliana M.; Franco,Gustavo B.; Silva,Samuel de A.
ABSTRACT Cacao is a species of great economic and social importance. Expanding the area grown with this crop has been limited by its climatic requirements. Agroclimatic zoning for agricultural sector and creation of land suitability maps by fuzzy logic contribute to such production expansion. In this sense, this study aimed to develop rainfall zoning for cacao in Bahia state using the fuzzy logic method. The used data came from rainfall historical series of 519 meteorological stations distributed throughout the state. Geostatistical analyses were used to quantify the spatial dependence degree of studied variable and kriging was used to develop maps representing mean monthly rainfall. These maps were submitted to continuous classification by fuzzy mapping...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Land suitability; Mapping; Spatial dependence; Theobroma cacao L.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800048

Draft prediction models for soil engaging tines in two soils of Rio Grande do Sul, Brazil
Provedor de dados: 70
Autores: Machado,Antônio L. T.; Trein,Carlos R.
The draft forces of soil engaging tines and theoretical analysis compared to existing mathematical models, have yet not been studied in Rio Grande do Sul soils. From the existing models, those which can get the closest fitting draft forces to real measure on field have been established for two of Rio Grande do Sul soils. An Albaqualf and a Paleudult were evaluated. From the studied models, those suggested by Reece, so called "Universal Earthmoving Equation", Hettiaratchi and Reece, and Godwin and Spoor were the best fitting ones, comparing the calculated results with those measured "in situ". Allowing for the less complexity of Reece's model, it is suggested that this model should be used for modeling draft forces prediction for narrow tines in Albaqualf...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chiselling; Draft requirement; Soil dynamics.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100017

Turbidimetry as an alternative method to determine the rating curve of suspended sediments
Provedor de dados: 70
Autores: Poletto,Kayla; Sampaio,Silvio C.; Queiroz,Manoel M. F. de; Gomes,Benedito M.; Soncela,Rosimaldo.
Understanding hydrosedimental behavior of a watershed is essential for properly managing and using its hydric resources. The objective of this study was to verify the feasibility of the alternative procedure for the indirect determination of the sediment key curve using a turbidimeter. The research was carried out on the São Francisco Falso River, which is situated in the west of the state of Paraná on the left bank of ITAIPU reservoir. The direct method was applied using a DH-48 sediment suspended sampler. The indirect method consisted of the use of a linigraph and a turbidimeter. Based on the results obtained, it was concluded that the indirect method using a turbidimeter showed to be fully feasible, since it gave a power function-type mathematical model...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Watershed; Hydrosedimentalogy; Agriculture.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300019

Efeitos de águas residuárias de café no crescimento vegetativo de cafeeiros em seu primeiro ano
Provedor de dados: 70
Autores: Ribeiro,Moisés S.; Lima,Luiz A.; Faria,Fábio H. de S.; Rezende,Fátima C.; Faria,Lucas do A.
Ao utilizar o solo como forma de tratamento e de disposição final de águas residuárias de café (ARC) e essa como fonte de água e de nutrientes para os cafeeiros, solucionam-se problemas ambientais e diminuem-se os custos de produção para o cafeicultor. Este trabalho teve por objetivo avaliar os efeitos de diferentes doses de potássio aplicadas via ARC no crescimento vegetativo de cafeeiros (Coffea arabica L.), Catuaí' e Catucaí', em seu primeiro ano, bem como o incremento de potássio e a condutividade elétrica na solução do solo. O estudo foi desenvolvido em casa de vegetação do Departamento de Engenharia, na Universidade Federal de Lavras, no município de Lavras - MG. Os tratamentos foram definidos por diferentes doses de potássio (K+): 30 mg L-1; 65 mg...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Potássio; Reúso; Coffea arabica L.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400007

Distribuição de fósforo no bulbo molhado, aplicado via fertirrigação por gotejamento com ácido fosfórico
Provedor de dados: 70
Autores: Zanini,José R.; Barreto,Ana K. G.; Foratto,Leticia C.; Natale,William.
Foram investigados a distribuição do fósforo, o pH e a umidade do solo no bulbo molhado em um Latossolo sem vegetação, após fertirrigação com ácido fosfórico, durante 21 dias. O experimento foi instalado na UNESP/Jaboticabal - SP, em blocos casualizados, com cinco repetições. Os tratamentos foram 0; 30; 60; 90 e 120 kg ha-1 de P2O5, dividindo-se as doses em quatro aplicações semanais, via fertirrigação. Após a última aplicação, foram abertas trincheiras nos bulbos molhados e coletadas amostras de solo em quadrículas de 100 cm². O ácido fosfórico provocou aumento da acidez e elevados teores de fósforo no bulbo, principalmente até 30 cm de distância lateral e até 40 cm de profundidade, em relação ao ponto de gotejamento. O aumento da dose de ácido fosfórico...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bulbo úmido; Irrigação por gotejamento; Acidez do solo.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100012

Meso e macrofauna de solo cultivado com milho e irrigado com água residuária da suinocultura
Provedor de dados: 70
Autores: Castaldelli,Ana P. A; Sampaio,Silvio C.; Tessaro,Dinéia; Herrmann,Daniela da R.; Sorace,Mauren.
RESUMO A utilização da fauna edáfica como bioindicadora de alterações antrópicas e ambientais vem crescendo nos últimos anos. No entanto, ainda são poucos os estudos em longo prazo que relacionam esses organismos com aplicação de resíduos orgânicos no solo. O objetivo deste trabalho foi avaliar, em dois ciclos da cultura do milho, os efeitos da aplicação de diferentes doses e tipos de águas residuárias da suinocultura (ARS) combinadas ou não com adubação mineral sobre a meso e a macrofauna de solo. Quatro doses (0; 100; 200 e 300 m3ha-1) de ARS, tratada em biodigestor no primeiro ano de estudo e bruta no segundo ano, associadas ou não com adubação mineral, foram aplicadas em dois ciclos da cultura de milho, totalizando 24 parcelas experimentais, sendo 12...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fauna edáfica; Reúso de efluente; Dejeto líquido de suíno.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500905

Variação espacial e temporal dos fatores limnológicos em riachos da microbacia do rio São Francisco Verdadeiro
Provedor de dados: 70
Autores: Oliveira,Luciano C. de; Gomes,Benedito M.; Baumgartner,Gilmar; Sebastien,Nyamien Y.
Com objetivo de caracterizar espacial e temporalmente os riachos da microbacia do rio São Francisco Verdadeiro, Marechal Cândido Rondon - PR, em função de fatores limnológicos, foram estabelecidas seis estações de coleta em três riachos (Curvado, Ajuricaba e Arroio Fundo), sendo uma estação na foz e outra na nascente. As coletas de água foram obtidas entre junho de 2005 e maio de 2006, totalizando 72 amostras. Foram analisadas as seguintes variáveis: temperatura, pH, condutividade elétrica, oxigênio dissolvido, turbidez, material em suspensão, fósforo total dissolvido, ortofosfato, nitrogênio total e nitrogênio amoniacal. De acordo com a análise de variância, houve baixa variabilidade entre as estações de coleta, porém a variação temporal demonstrou a...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Variáveis físicas e químicas; Limnologia; Material alóctone.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400017

Taxa de emissão de CO2 de um latossolo fertirrigado com ácido fosfórico por gotejamento
Provedor de dados: 70
Autores: Zanini,José R.; Barreto,Ana K. G.; La Scala Júnior,Newton.
A aplicação de fertilizantes fosfatados por meio de fertirrigação com sistemas de irrigação localizada pode causar obstrução de emissores. Para evitar esse problema, pode ser utilizado o ácido fosfórico como fonte de fósforo às plantas. Porém, têm sido pouco investigados os efeitos da irrigação relacionados às perdas de CO2 do solo para a atmosfera, em conseqüência da decomposição do carbono orgânico e da infiltração de água no solo. Neste trabalho, investigou-se, no período de um mês, o efeito da fertirrigação com ácido fosfórico nas taxas de emissão de CO2 de um latossolo desprovido de vegetação, na Área Experimental de Irrigação da UNESP, Câmpus de Jaboticabal - SP. Utilizou-se de um sistema de irrigação por gotejamento, com delineamento experimental em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Respiração do solo; Irrigação localizada; Fertirrigação.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100020

Dimensionamento de motores para o bombeamento de água
Provedor de dados: 70
Autores: Oliveira Filho,Delly; Ribeiro,Marcos C.; Mantovani,Everardo C.; Soares,Antônio A.; Fernandes,Haroldo C.
O dimensionamento de motores com potência acima da necessária acarreta maior custo inicial, menor rendimento e menor fator de potência. Desde 1996, que se fabricam no Brasil motores elétricos com fator de serviço maior do que a unidade, obedecendo a valores prescritos em norma. O fator de serviço informa a potência disponível do motor em regime contínuo para as condições de carga nominal. A literatura técnica de dimensionamento de motores para acionamento de bombas hidráulicas indica a necessidade da adoção de acréscimos na potência dos motores. Tanto o fator de serviço, quanto o acréscimo na potência constituem fatores de segurança para o dimensionamento. Estes fatores de segurança têm a função de suprir maior demanda de potência devido a variações nas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fator de segurança; Motores elétricos; Bombeamento.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600003

Heat pump for thermal power production in dairy farm
Provedor de dados: 70
Autores: Jordan,Rodrigo A.; Cortez,Luís A. B.; Barbin,Douglas F.; Lucas Junior,Jorge de.
ABSTRACT Besides cold for milk cooling, dairy facilities need to produce hot water for cleaning of tools and equipment. Overall, ohmic heating has been used in dairy farms, increasing power consumption and manufacturing costs. Therefore, as an alternative to reduce power consumption, this paper proposed a water-water heat pumping for simultaneous cold and heat generations. Accordingly, operational tests were performed with three heat-pump prototypes designed for dairy farms, in both laboratory and field levels. At laboratory, tests were carried out using electricity and CNG to define a coefficient of performance (COP). Biogas tests were performed in the field to measure its consumption. CNG average consumption was of 1.118 m3/ h, while biogas consume was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal power; Thermal-accumulation; Cooling; Heating.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500779

Análise espacial da precipitação pluviométrica no Estado de São Paulo: comparação de métodos de interpolação
Provedor de dados: 70
Autores: Carvalho,José R. P. de; Assad,Eduardo D.
O objetivo deste trabalho é comparar três interpoladores univariados: inverso do quadrado da distância, curvatura mínima e krigagem ordinária usando observações de precipitação pluvial média anual de 1.027 postos pluviométricos abrangendo todo o Estado de São Paulo, representando área de 248.808,8 km² (2,91% do território nacional), no período de 1957 a 1997. Os mapas de variabilidade espacial não apresentaram grandes diferenças visuais; entretanto, quando a estatística quadrado médio do erro foi calculada para cada técnica, confirmou-se a grande vantagem em usar o interpolador ótimo de krigagem. A diferença entre os valores observados e estimados pela krigagem foi muito menor do que para os outros dois métodos, indicando ser esse o interpolador a ser...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Krigagem ordinária; Geoestatística; Semivariograma.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200011

Avaliação da resistência do solo à penetração em diferentes solos com a variação do teor de água
Provedor de dados: 70
Autores: Assis,Renato L. de; Lazarini,Gilmar D.; Lanças,Kléber P.; Cargnelutti Filho,Alberto.
Com os crescimentos da população e da demanda por alimentos, novas tecnologias têm surgido visando ao aumento da produtividade e à redução nos custos de produção. Se por um lado essas tecnologias elevam a produção e reduzem os custos, por outro o tráfego intenso de máquinas e tratores alteram a estrutura do solo, tornando-o compactado, comprometendo, assim, a produtividade agrícola. Neste trabalho, relacionou-se o teor de água do solo com a sua resistência à penetração, para quatro tipos de solo e quatro condições de umidade, utilizando penetrômetro hidráulico-eletrônico com sistema de navegação DGPS. Os resultados mostraram que ocorreram modificações nas condições de atrito entre o cone e o solo com o aumento do teor de água, facilitando a penetração da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Densidade do solo; Índice de cone; Limites de consistência.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400006

SPRAY DEPOSITION AT TWO GROWTH STAGES OF CATTAIL
Provedor de dados: 70
Autores: Silva,João R. V.; Silva Junior,Antonio C. da; Pereira,Maria R. R.; Martins,Dagoberto.
ABSTRACT Surfactant use in spray solutions has a major advantage of reducing droplet surface tension and increasing deposition. We aimed to evaluate droplet deposition on cattail plants (Typha subulata) using food coloring (Brilliant Blue - FD &amp; C-1) as marker added to spray solution at two different growth stages: vegetative (4 leaves) and flowering (5 leaves). The treatments were arranged in a completely randomized design with four replications and five plants per plot (16.2-L tanks). Treatments consisted of adding into spray solutions Brilliant Blue alone (control), Brilliant Blue + 0.5% v/v Aterbane and Brilliant Blue + 0.01% v/v Silwet. Spraying was performed by a pressurized CO2 sprayer at 220 kPa using two Teejet XR 8002 nozzles at a spray...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aterbane; Droplet; Silwet; Surfactant; Typha subulata.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100194

Desempenho físico-mecânico de minipainéis de terra crua tratada com aditivos químicos
Provedor de dados: 70
Autores: Ferreira,Régis de C.; Freire,Wesley J.
O presente trabalho teve como objetivo pesquisar o efeito da incorporação ao solo de estabilizantes químicos (cal e cimento) associados ao silicato de sódio. Os tijolos foram moldados e assentados na forma de minipainéis que tiveram suas características físico-mecânicas determinadas em laboratório e seu comportamento tecnicamente avaliado por meio de métodos destrutivos e não-destrutivos (método acústico do ultra-som). Foram pesquisados um solo arenoso e outro siltoso. Os teores de cimento e cal adicionados foram de 6% e 10% em relação à massa seca do solo, e o teor de silicato de sódio foi de 4% em relação à massa seca de solo-cimento ou solo-cal. Os tijolos foram prensados e colocados em câmara úmida por 7; 28; 56 e 91 dias. Aos 28; 56 e 91 dias, os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tijolos de terra crua; Propriedades mecânicas; Ultra-som.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300003

Avaliação do uso de identificadores eletrônicos em suínos
Provedor de dados: 70
Autores: Silva,Késia O. da; Nääs,Irenilza de A.
O mercado consumidor, atualmente, exige aumento gradativo do controle da qualidade dos produtos. Os métodos manuais de controle existentes, aplicáveis à produção animal, começam a se mostrar ineficientes para garantir percentual crescente dessa qualidade, pois essa garantia somente pode ser efetiva se houver rastreamento confiável do animal, desde o seu nascimento até o abate. A identificação individual apresenta grande importância nesse enfoque, pois possibilita a coleta de informações inerentes ao animal. A rastreabilidade eletrônica utiliza dispositivo eletrônico, que emite um sinal ativado por um leitor fixo, colocado onde for necessário registrar um determinado evento, ou um leitor manual que permite maior independência do operador. Sabendo-se da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Rastreabilidade; Transponder; Zootecnia de precisão.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100002

Water quality indicators for environmental and resistance profile of Escherichia coli strains isolated in Rio Cascavel, Paraná, Brazil
Provedor de dados: 70
Autores: Souza,Marinêz de; Pinto,Fabiana G. da S.; Fruet,Thomas K.; Piana,Pitágoras A.; Moura,Alexandre C. de.
In this article it was evaluated the quality of water in the Cascavel river, in the city of Cascavel - Paraná using microbiological indicators, physical and chemical pollution and susceptibility / resistance in strains of Escherichia coli isolated antimicrobial trade. The water sampling was conducted between 2010-July and 2011-June at three points: a) near the source, b) urban area, c) rural area. The samples were analyzed for physical, chemical and microbiological variables: temperature, pH, color, turbidity, electrical conductivity, total nitrogen and total phosphorus, total coliforms (CT), fecal coliform (CTe) and Escherichia coli. Tests were also performed to nine antimicrobial commercial resistances. The variables studied indicated that the Cascavel...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water resources physical and chemical parameters water pollution coliforms; Microbiology WQI.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200016

Efeito da aeração no primeiro estágio da compostagem de carcaça de aves
Provedor de dados: 70
Autores: Costa,Mônica S. S. de M.; Costa,Luiz A. de M.; Olibone,Dácio; Röder,Cinthia; Burin,Alcione; Kaufmann,Anderson V.; Ortolan,Mara L.
Avaliou-se o efeito da aeração no primeiro estágio do processo de compostagem em carcaças de aves mediante o monitoramento de parâmetros físicos (temperatura), químicos (reciclagem de nutrientes) e microbiológicos (coliformes fecais, totais, ausência ou presença de Salmonella sp). O processo de compostagem desenvolveu-se em dois estágios, o primeiro em composteiras com e sem aeração e o segundo no pátio de compostagem. A temperatura máxima atingida, considerando a média semanal, no primeiro estágio, foi de 56,1 ºC e 54,1 ºC (com e sem aeração) e 66,2 ºC e 61,9 ºC (com e sem aeração), respectivamente, para o primeiro e o segundo carregamentos realizados nos sistemas, enquanto no segundo estágio foi de 53,6 ºC e 61,1 ºC; 64,6 ºC e 66,3 ºC, respectivamente,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Composição química; Salmonella sp; Colimetria.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200029

Caracterização das perdas e distribuição de cobertura vegetal em colheita mecanizada de soja
Provedor de dados: 70
Autores: Toledo,Anderson de; Tabile,Rubens A.; Silva,Rouverson P. da; Furlani,Carlos E. A.; Magalhães,Stefânia C.; Costa,Beatriz O.
O conceito de controle de qualidade nas operações inserido na agricultura é viabilizado por incidir diretamente nos principais objetivos do processo produtivo: retorno econômico e aumento da produtividade. A colheita mecanizada normalmente é realizada sem que haja controle efetivo para que a variabilidade das perdas fique dentro de padrões aceitáveis. Esta pesquisa teve o objetivo de determinar e caracterizar as perdas e a distribuição da cobertura vegetal após a colheita mecanizada da soja, por meio de ferramenta de controle estatístico de processo (cartas de controle). A média da perda de grãos total foi próxima do limite superior aceitável para a cultura da soja, apresentando alta variabilidade entre os pontos, tornando o processo fora de controle. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cartas de controle; Colheita mecanizada; Controle estatístico; Perdas quantitativas.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400011

STATISTICAL CONTROL OF PROCESSES APLIED FOR PEANUT MECHANICAL DIGGING IN SOIL TEXTURAL CLASSES
Provedor de dados: 70
Autores: Zerbato,Cristiano; Furlani,Carlos E. A.; Silva,Rouverson P. da; Voltarelli,Murilo A.; Santos,Adão F. Dos.
ABSTRACT The digging of peanut, which has the pod production in the subsurface, is directly affected by soil conditions, physical or environmental characteristics, at the time of operation and may be the cause of unwanted losses. Therefore, the quality of the operation is very important for minimizing these losses. Thus, this study aimed to evaluate the quality of mechanized digging operation of peanut according to three soil textural classes (Sandy, Medium and Loamy) and their water content conditions at operation through statistical process control. The experiment was conducted at three locations in the state of São Paulo, Brazil, under sampling scheme arranged in tracks and 40 sampling points for each textural class of soil, using the mechanical digging...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Arachis hypogaea L; Losses; Quality; Soil water content; Water content of the pods.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200315

The design and evaluation of travelling gun irrigation systems: enrolador software
Provedor de dados: 70
Autores: ROLIM,JOÃO; TEIXEIRA,JOSÉ L.
ABSTRACT Travelling gun irrigation systems offer great mobility and operation flexibility with a low investment cost per unit of irrigated area. However, the drawbacks include high operating pressure, low application efficiency, and high rainfall, runoff and erosion. Many of these problems can be minimized if the design and operation of travelling gun irrigation systems are carried out carefully, taking into account several design criteria that will ensure the quality of the irrigation performed by the system. The Enrolador software was developed to meet this goal. The software designs the travelling gun irrigation system, performs its simulation and its performance evaluation. This software was experimentally applied in the Alentejo region, Portugal. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Travelling gun; Irrigation design; Software.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500917

Performance of an anaerobic-aerobic reactor and kinetic study of organic matter removal of cattle slaughterhouse effluent
Provedor de dados: 70
Autores: Kreutz,Cristiane; Passig,Fernando H.; Carvalho,Karina Q. de; Mees,Juliana B. R.; Gomes,Simone D.
This paper sought to evaluate the behavior of an upflow Anaerobic-Aerobic Fixed Bed Reactor (AAFBR) in the treatment of cattle slaughterhouse effluent and determine apparent kinetic constants of the organic matter removal. The AAFBR was operated with no recirculation (Phase I) and with 50% of effluent recirculation (Phase II), with θ of 11h and 8h. In terms of pH, bicarbonate alkalinity and volatile acids, the results indicated the reactor ability to maintain favorable conditions for the biological processes involved in the organic matter removal in both operational phases. The average removal efficiencies of organic matter along the reactor height, expressed in terms of raw COD, were 49% and 68% in Phase I and 54% and 86% in Phase II for θ of 11h and 8h,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Kinetic; Cattle slaughterhouse; Combined treatment system.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200015

Penetration resistance and agronomic characteristics of soybean affected by soil management and sowing speed systems
Provedor de dados: 70
Autores: CORTEZ,JORGE W.; CHAVES,RODRIGO G.; ORLANDO,ROBERTO C.; SOUZA,CRISTIANO M. A. DE; SOUZA,PAULO H. N. DE.
ABSTRACT With the short period of the sowing process, we observed an increase in the seeder speed set in several soil management systems that may result in decreased soybean yield and problems with penetration resistance. We aimed to assess the penetration resistance (PR) and agronomic characteristics of soybean on soil tillage and sowing speed. The randomized block design in split plot with four replications was used. The treatments consisted of six management systems, applied to the plots: no tillage (NT), no tillage and chiseling (NTc), no tillage and cross chiseling (NTcc), conventional tillage (CT), reduced tillage (RT) and conservation tillage (CsT) and four speeds, (4.6; 5.5; 7,3 and 7.8 km h-1) applied in the subplot at the time of soybean seeding....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural mechanization; No tillage; Yield.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400664

Management zones definition using soil chemical and physical attributes in a soybean area
Provedor de dados: 70
Autores: Bazzi,Claudio L.; Souza,Eduardo G.; Uribe-Opazo,Miguel A.; Nóbrega,Lúcia H. P.; Rocha,Davi M.
Several equipments and methodologies have been developed to make available precision agriculture, especially considering the high cost of its implantation and sampling. An interesting possibility is to define management zones aim at dividing producing areas in smaller management zones that could be treated differently, serving as a source of recommendation and analysis. Thus, this trial used physical and chemical properties of soil and yield aiming at the generation of management zones in order to identify whether they can be used as recommendation and analysis. Management zones were generated by the Fuzzy C-Means algorithm and their evaluation was performed by calculating the reduction of variance and performing means tests. The division of the area into...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Spatial variability; Fuzzy clustering; Management zones; Autocorrelation; Cross-correlation.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500007

Estimativa das condições de conforto térmico para avicultura de postura usando a teoria dos conjuntos Fuzzy
Provedor de dados: 70
Autores: Oliveira,Henrique L. de; Amendola,Mariangela; Nääs,Irenilza de A.
Neste trabalho, foi utilizada uma ferramenta matemática promissora na análise de sistemas e/ou processos, particularmente na área de produção animal. Essa ferramenta é a desenvolvida segundo a abordagem da teoria dos Conjuntos Fuzzy e, neste caso específico, permitiu a análise da composição das variáveis climáticas independentes, como temperatura de bulbo seco e umidade relativa do ar, que influenciam na variável dependente denominada conforto térmico das aves. Foi realizada a construção de regras baseadas na intuição humana, segundo o conhecimento de especialistas da área, a partir do que é possível simular cenários distintos para o suporte à decisão de construção de galpões para abrigo a animais. Neste trabalho, foi estimado o conforto térmico para...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Suporte à decisão; Conforto térmico; Aves de postura.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200002

Mobilização do solo e profundidade de semeadura por diferentes mecanismos para o manejo do sulco de semeadura em uma semeadora direta
Provedor de dados: 70
Autores: Brandelero,Evandro M.; Araujo,Augusto G. de; Ralisch,Ricardo.
Na semeadura direta, é fundamental que a mobilização do solo no sulco de semeadura seja a menor possível, visando a reduzir o risco de erosão e de desenvolvimento de ervas infestantes. O objetivo do trabalho foi avaliar o desempenho de diferentes mecanismos para o manejo do sulco de semeadura quanto à mobilização de solo e à profundidade de semeadura empregados em uma semeadora direta. O experimento foi conduzido em solo argiloso, em semeadura direta, com alto volume de palha de sorgo. Os tratamentos consistiam no emprego isolado de dois mecanismos rompedores à frente da haste sulcadora, compostos pelo disco de corte e rodas de varredura, e suas combinações com três mecanismos cobridores atrás do sulcador da semente, executados pelos discos cobridores,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays; Plantio direto; Mecanização agrícola; Sulcadores.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200008

Comparative analysis of different meat traceability systems using multiple criteria and a social network approach
Provedor de dados: 70
Autores: NÄÄS,IRENILZA DE A.; MOLLO NETO,MARIO; VENDRAMETTO,ODUVALDO; CANUTO,SIMONE A.
The adoption of a proper traceability system is being incorporated into meat production practices as a method of gaining consumer confidence. The various partners operating in the chain of meat production can be considered a social network, and they have the common goal of generating a communication process that can ensure each characteristic of the product, including safety. This study aimed to select the most appropriate meat traceability system “from farm to fork” that could be applied to Brazilian beef and pork production for international trade. The research was done in three steps. The first used the analytical hierarchy process (AHP) for selecting the best on-farm livestock traceability. In the second step, the actors in the meat production chain...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Analytic hierarchy process; Food traceability; Social network analysis-SNA.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200340

Utilização de dados georreferenciados na determinação de parâmetros de desempenho em colheita mecanizada
Provedor de dados: 70
Autores: Molin,José P.; Milan,Marcos; Nesrallah,Michel G.T.; Castro,Cesar N. de; Gimenez,Leandro M.
As informações sobre o desempenho e a capacidade de trabalho das máquinas agrícolas são de grande importância no gerenciamento de sistemas mecanizados agrícolas, auxiliando na tomada de decisões. A obtenção de informações sobre o desempenho é normalmente realizada de modo manual, por meio da análise dos tempos e movimentos, consumindo recursos, mão-de-obra e tempo. Considerando-se a importância das informações e o custo envolvido na aquisição, o objetivo deste trabalho é apresentar uma metodologia automática para a determinação da capacidade de trabalho de colhedora de cereais. Para tanto, realizou-se o estudo de tempos e movimentos a partir de arquivos de dados obtidos por meio de monitores de produtividade em oito propriedades no Estado do Paraná. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Mecanização; Gerenciamento.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300013

Pré-filtração em pedregulho e filtração lenta com areia, manta não tecida e carvão ativado para polimento de efluentes domésticos tratados em leitos cultivados
Provedor de dados: 70
Autores: Paterniani,José E. S.; Silva,Marcelo J. M. da; Ribeiro,Tulio A. P.; Barbosa,Melina.
O presente trabalho teve como objetivo comparar sistemas de filtragem, composto de pré-filtro de pedregulho seguido de filtro lento com o meio filtrante areia e no topo manta sintética não tecida e pré-filtro de pedregulho seguido de filtro lento com meio filtrante areia e carvão ativado granular e no topo manta sintética não tecida, para polimento de efluentes domésticos tratados em leitos cultivados, visando à aplicação na fertirrigação. Na comparação dos sistemas de filtragem, avaliou-se a eficiência de remoção dos parâmetros: sólidos em suspensão, turbidez, cor aparente, demanda química de oxigênio, oxigênio dissolvido, ferro, manganês, coliformes totais e E. coli. Os dois sistemas operavam 24 horas por dia, com a mesma taxa de aplicação, tratando uma...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saneamento rural; Tratamento de esgotos; Reúso de água; Fertirrigação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400018

EFFECT OF THE DOWNWASH FLOW FIELD OF A SINGLE-ROTOR UAV ON DROPLET VELOCITY IN SUGARCANE PLANT PROTECTION
Provedor de dados: 70
Autores: Zhang,Ping; Zhang,Wei; Sun,Haitian; Fu,Haiba; Liu,Jiansheng.
ABSTRACT Protecting against the main sugarcane diseases and insect pests requires good control at the base of the plant; therefore, higher droplet penetration is required during plant protection. The objectives of this research were to explore the movement mechanism of droplets in a sugarcane protection operation using a single-rotor unmanned aerial vehicle (UAV) and establish the connection between the UAV downwash flow field and droplet penetration. By considering the downwash flow field of a single-rotor UAV in layers, a theoretical model of the vertical velocities of droplets was established, and verification experiments were carried out in a sugarcane field. The results showed that the velocity of the UAV downwash flow was the main factor affecting...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Numerical solution; Droplet motion law; Droplet penetration; Vertical velocity; Droplet diameter.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200235

Quantificação do erro na determinação da perda contínua de carga em tubos elásticos
Provedor de dados: 70
Autores: Rettore Neto,Osvaldo; Botrel,Tarlei A.; Frizzone,José A.; Pinto,Marinaldo F.; Camargo,Antônio P.
A indústria de plásticos e derivados, com o auxílio da engenharia, tem aprimorado a qualidade do material destinado à fabricação de tubos, principalmente os de polietileno. A elasticidade desses tubos permite que ocorra aumento do diâmetro interno com o aumento da pressão, o que não é levado em consideração pelos equacionamentos matemáticos utilizados para a determinação da perda de carga. O objetivo deste trabalho foi quantificar os erros na determinação da perda de carga em tubos elásticos, em função da pressão de entrada na linha lateral, comparando valores observados e estimados pelas equações recomendadas na literatura técnica. Avaliaram-se 3 amostras de tubo de polietileno sob 9 pressões de entrada e 3 vazões, sendo estas correspondentes às...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Perda de carga contínua; Irrigação localizada; Tubos de polietileno.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600023

Avaliação do microclima de instalações para gado de leite com diferentes recursos de climatização
Provedor de dados: 70
Autores: Martello,Luciane S.; Savastano Júnior,Holmer; Pinheiro,Maria das G.; Silva,Saulo da L. e; Roma Júnior,Luiz C.
Este trabalho foi realizado no verão de 2002 e teve como objetivo avaliar a influência de alguns recursos de climatização no microclima interno das instalações. Foram utilizadas três instalações: i) controle; ii) com aspersão associada à ventilação, e iii) com tela de sombreamento. Os dados climáticos de cada instalação foram registrados e, posteriormente, calculados os índices de temperatura e umidade, do globo negro e umidade e a entalpia. Foram selecionados e analisados 26 dias com entalpia elevada. Os índices de temperatura e umidade (ITU) e de temperatura do globo e umidade (ITGU), nos horários mais quentes do dia, diferenciaram-se para a instalação climatizada (ii), que apresentou melhor desempenho em relação às demais. A entalpia menor foi observada...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Estresse calórico; Gado de leite; Índice de conforto térmico.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200004

Homogeneous Pinus sp. particle boards reinforced with laminated composite materials
Provedor de dados: 70
Autores: Christoforo,André L.; Nascimento,Maria F. do; Panzera,Tulio H.; Ribeiro Filho,Sérgio L. M; Lahr,Francisco A. R.
ABSTRACT This study aimed to evaluate the mechanical performance of laminated composite materials (fiberglass, carbon, sisal, palm fiber) in epoxy matrix as reinforcement in wood particleboards of Pinus sp. with bicomponent polyurethane resin from castor oil. Modulus of elasticity (MOE) and modulus of rupture (MOR) were investigated using a three-point bending test. Single-layered laminated plates were used to reinforce traction of specimens obtained from boards. MOE and MOR of materials developed without reinforcements exceeded limits in ABNT standards both NBR 12810-2:2002 and A208.1:199, proving therefore their feasibility. In all investigated cases, inclusion of reinforcements led to higher values for both MOE and MOR. Composites in fiberglass...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Particleboard; Laminated composites; Structural reinforcement.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300558

STARCH EXTRACTION FROM THE PEACH PALM (Bactris gasepaes Kunth.) FRUIT: A MODEL APPROACH FOR YIELD INCREASE
Provedor de dados: 70
Autores: Melo Neto,Biano A. de; Bonomo,Renata C. F.; Franco,Marcelo; Almeida,Paulo F. de; Pontes,Karen V.
ABSTRACT The objective was to study the starch extraction process of the peach palm (Bactris gasipaes Kunth.) fruit focused on increasing yield and in preserving the quality characteristics the extracted product. Two experimental designs are carried out in order to investigate the effects of NaOH and NaHSO3 concentrations, as well as the decantation time, on the yield of starch and on product color. Firstly, a 23 full factorial design provided a linear model with 95% of confidence, indicating major tendencies for optimization. Secondly, a 22 central composite design rendered a quadratic model which allowed the maximization of yield (it 9.0% higher) without compromising the color of the product. The maximum yield of 23.90%, validated with triplicate...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Design of experiments; Response surface methodology; Native starch.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100148

Utilização de energia elétrica em diferentes sistemas de aquecimento para leitões desmamados
Provedor de dados: 70
Autores: Sarubbi,Juliana; Rossi,Luiz A.; Moura,Daniella J. de; Oliveira,Rafael A. de; David,Eduardo.
A eficiência do uso de energia elétrica no aquecimento de leitões em fase de creche e maternidade pode ser viabilizada sem prejudicar o conforto térmico dos suínos. Neste trabalho, foram comparadas três tecnologias de aquecimento de leitões em fase de creche, quanto ao uso de energia elétrica e ao ambiente térmico. Estudaram-se três tratamentos: resistências elétricas suspensas (TR), piso aquecido (TP) e aquecimento por convecção (TA). Os critérios de comparação foram: consumo de energia elétrica (kWh), demanda máxima de potência (kW), consumo específico (kWh/kg de suíno vivo produzido), a quantidade de energia elétrica consumida (kWh) para o aumento de 1ºC em 1m³ de ar, a temperatura de bulbo seco (ºC) e o Índice de Temperatura e Umidade (ITU). O sistema...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Suinocultura; Creche; Racionalização de energia elétrica; Piso aquecido.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600002

RELATIONSHIP BETWEEN COFFEE CROP PRODUCTIVITY AND VEGETATION INDEXES DERIVED FROM OLI / LANDSAT-8 SENSOR DATA WITH AND WITHOUT TOPOGRAPHIC CORRECTION
Provedor de dados: 70
Autores: Nogueira,Sulimar M. C.; Moreira,Maurício A.; Volpato,Margarete M. L.
ABSTRACT The reflectance values of a coffee crop are influenced by several factors such as planting direction, crop spacing, time of the year, plant age and topography which reduces the accuracy of the estimates derived from remote sensing data. In this context were evaluated the relationships between coffee productivity and values of NDVI, SAVI and NDWI vegetation indexes with and without topographic reflectance correction for different coffee phenological phases for the crop years 2013/2014 (low productivity) and 2014/2015 (high productivity). The evaluations were made through the standard deviation of vegetation indices (VIs), linear relationship between the cosine factor and the VIs and between VIs and coffee productivity. The best phenological phases...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffee; NDVI; NDWI; Yield; SAVI; Remote sensing.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300387

DRYING KINETICS OF PEANUT KERNELS IN THIN LAYERS
Provedor de dados: 70
Autores: Goneli,André L. D.; Araujo,Willian D.; Hartmann Filho,Cesar P.; Martins,Elton A. S.; Oba,Guilherme C.
ABSTRACT: The aim of this study was to adjust mathematical models to the experimental data on the peanut kernels drying in thin layer, as well as to determine the effective diffusion coefficient and the main thermodynamic properties involved in drying of the grains under different air conditions. The peanut kernels, with a water content of 0.59 ± 0.002 (dry basis, d.b.), were dried in a forced air ventilation oven with different temperature levels (40, 50, 60 and 70 °C) until reaching a water content of 0.04 ± 0.001 (d.b.). For the experimental data, eight mathematical models traditionally used to represent the drying kinetics of thin layer of agricultural products were adjusted, also being determined the effective diffusion coefficient and the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Arachis hypogaea L.; Effective diffusivity; Activation energy; Page model; Thermodynamic properties.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500994

Magnetic susceptibility in the prediction of soil attributes in two sugarcane harvesting management systems
Provedor de dados: 70
Autores: Peluco,Rafael G.; Marques Júnior,José; Siqueira,Diego S.; Cortez,Lucas A.; Pereira,Gener T.
This study aimed to investigate the potential use of magnetic susceptibility (MS) as pedotransfer function to predict soil attributes under two sugarcane harvesting management systems. For each area of 1 ha (one with green sugarcane mechanized harvesting and other one with burnt sugarcane manual harvesting), 126 soil samples were collected and subjected to laboratory analysis to determine soil physical, chemical and mineralogical attributes and for measuring of MS. Data were submitted to descriptive statistics by calculating the mean and coefficient of variation. In order to compare the means in the different harvesting management systems it was carried out the Tukey test at a significance level of 5%. In order to investigate the correlation of the MS with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pedotransfer; Indirect quantification; Oxisol.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600006

Caracterização e biodigestão anaeróbia dos dejetos de caprinos
Provedor de dados: 70
Autores: Orrico,Ana C. A.; Lucas Júnior,Jorge de; Orrico Júnior,Marco A. P.
Quantificar e caracterizar os dejetos gerados por cabras Saanen em quatro categorias de idade e alimentadas com três dietas e na seqüência, e promover a biodigestão anaeróbia dos dejetos constituíram os objetivos deste trabalho. Para a produção de dejetos, foram utilizadas 36 cabras Saanen, com idades entre 2 e 4 (C1), 4 e 8 (C2), 8 e 12 (C3) e acima de 12 meses (C4), alimentadas com as dietas 1 (D1: 80% volumoso (Vol) e 20% concentrado (Con)); 2 (D2: 60% Vol e 40% Con) e 3 (D3: 40% Vol e 20% Con). Foram quantificadas as produções diárias de fezes e urina e seus teores em N, P, K, Ca, Mg, Na, Fe, Cu, Zn e Mn. Com a mistura das fezes e urina de todas as categorias, separadas segundo as dietas, foram abastecidos biodigestores batelada, com capacidade para 4...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogás; Sólidos totais; Sólidos voláteis.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400006

Caracterização espacial do ambiente termoacústico e de iluminância em galpão comercial para criação de frangos de corte
Provedor de dados: 70
Autores: Yanagi Júnior,Tadayuki; Amaral,Adriana G. do; Teixeira,Vitor H; Lima,Renato R. de.
A presente pesquisa teve o objetivo de avaliar e espacializar as variáveis termoacústicas e de iluminância no interior de um galpão comercial, com sistema de ventilação convencional e resfriamento evaporativo, destinado à produção de frangos de corte. Os frangos de corte Hybro foram alojados em um galpão subdividido em três regiões (refugos, fêmeas e machos), sendo criados a uma densidade aproximada de 20 aves m-2. O ambiente produtivo foi avaliado por meio do índice de conforto térmico, nível de ruído e de iluminância. Mapas de distribuição espacial destas variáveis foram gerados para o interior do galpão, usando o método da krigagem. Com base nos resultados, pode-se concluir que as aves, de forma geral, estiveram submetidas a condições ambientais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avicultura; Ambiente de produção; Distribuição espacial.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100001

Avaliação de índices de firmeza para abacaxi minimamente processado em fatias tratadas com soluções de sais de cálcio
Provedor de dados: 70
Autores: Eduardo,Marisa de P.; Benedetti,Benedito C.; Ferraz,Antonio C. O.
Produtos minimamente processados estão prontos para o consumo imediato e devem apresentar qualidade sensorial semelhante à do produto fresco. Embora a maioria dos estudos seja com hortaliças, constata-se o grande potencial de comercialização de frutas minimamente processadas, principalmente aquelas que oferecem alguma dificuldade para a comercialização ou até mesmo para o preparo, sendo o abacaxi um ótimo exemplo disso. O objetivo deste trabalho foi avaliar o efeito de diferentes sais de cálcio (cloreto, sulfato e lactato), nas concentrações de 1% e 3%, utilizando-se de medidas de pH , sólidos solúveis totais e da firmeza, em fatias de abacaxi minimamente processadas. Dois tipos de ponteiras de penetração (cilíndrica e anel vazador) e três índices de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Propriedades mecânicas; Energia de deformação; Vida útil; Textura.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100016

HYDROPHOBIC MEMBRANE TECHNOLOGY FOR AMMONIA EXTRACTION FROM WASTEWATERS
Provedor de dados: 70
Autores: KUNZ,AIRTON; MUKHTAR,SAQIB.
ABSTRACT Total Ammoniacal Nitrogen - TAN (NH3 + NH4+) in wastewaters cause environmental degradation concerns due to their negative impacts on air, soil and water. Several technologies are available for TAN removal from the wastewaters. One emerging technology is the use of hydrophobic membrane as non-destructive NH3 extraction. In this paper the authors discuss the uses of gas permeable membrane (GPM) and its physicochemical characteristics that influence gas mass transfer rate, diffusion and recovery mechanisms of NH3 from liquid sources (e.g. animal wastewater). Several aspects of NH3 extraction from liquid manure and other TAN generation sources using GPM technology as well as its applicability for NH3 mitigation from liquid effluents and possible...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ammonia; Separation; Wastewater; Nutrient recovery.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200377

Parcelamento da adubação e da fertirrigação na produção de palmito pupunha no Noroeste Paulista
Provedor de dados: 70
Autores: Alves Júnior,José; Hernandez,Fernando B. T.; Santos,Ronaldo A.; Lopes,Adriano S.
O palmito é um alimento muito apreciado na culinária brasileira e mundial, e entre as várias espécies de palmeira produtora, a pupunha se destaca por apresentar precocidade de produção, perfilhamento, rusticidade e boas características de processamento. Introduzida no Noroeste Paulista em 1994, a cultura da pupunha é vista por técnicos e produtores como bastante promissora na região, porém carente de informações técnicas, entre as quais a maneira e a época de aplicação de fertilizantes. Face a isso, foi instalado um experimento na UNESP, Câmpus de Ilha Solteira - SP, em área irrigada por microaspersão, com pupunheiras espaçadas de 2 x 1 m entre linhas e entre plantas, respectivamente. Os tratamentos foram assim constituídos: adubação manual na linha de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bactris gasipaes; Microaspersão; Fertirrigação.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300014

Outlining precision boundaries among areas with different variability standards using magnetic susceptibility and geomorphic surfaces
Provedor de dados: 70
Autores: Matias,Sammy S. R.; Marques Júnior,José; Siqueira,Diego S.; Pereira,Gener T.
There is an increasing demand for detailed maps that represent in a simplified way the knowledge of the variability of a particular area or region maps. The objective was to outline precision boundaries among areas with different accuracy variability standards using magnetic susceptibility and geomorphic surfaces. The study was conducted in an area of 110 ha, which identified three compartment landscapes based on the geomorphic surfaces model. To determinate pH, organic matter, phosphorus, potassium and magnesium, the total sand and clay, 514 soil samples were collected at depths of 0-0.20 m and 0.60-0.80 m. The sum of base, cationic exchange capacity and base saturation were calculated and the magnetic susceptibility was evaluated in the laboratory using...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Detailed mapping; Pedometrics; Accuracy boundaries.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400009

Zoning of environmental conditions inside a wean-to-finish pig facility
Provedor de dados: 70
Autores: Massari,Juliana M.; Moura,Daniella J. de; Curi,Thayla M. R. de C.; Vercellino,Rimena do A.; Medeiros,Brenda B. L.
ABSTRACT Using geostatistics, this study aimed to analyze environmental conditions for wean-to-finish swines at 3 pm, during the most sensitive phases to thermal stress (growth/ finishing and finishing). To this end, dry-bulb temperature, relative humidity, air speed, ammonia and carbon dioxide concentrations were measured at 81 equidistant points within the barn. Descriptive statistics was used to classify attribute variability, generating mean, median, variation coefficient, asymmetry and kurtosis, through the normality of Kolmogorov-Smirnov (KS). For that, it was used Minitab 15 software. Moreover, semivariograms were used to assess spatial dependence using the GS+ software, and through Surfer, spatial distribution maps were designed. Dry-bulb...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Welfare; Geostatistics; Pig farming.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500739

VERTICAL PRESSURES AND COMPRESSIVE FRICTION FORCE IN A LARGE SILO
Provedor de dados: 70
Autores: Fank,Marivone Z.; Nascimento,José W. B. do; Cardoso,Décio L.; Meira,Ariadne S.; Willrich,Fábio L.
ABSTRACT The grain flow is a dynamic phenomenon of high non-linearity, responsible for the occurrence of a high index of structural problems in silos, assuming particular interest in Brazil because the country does not have a standard of design of these structures. In order to determine the transfer of loads to the foundations, a silo in true magnitude was instrumented through pressure cells in the reinforced concrete slab of the bottom and through load cells under two of its column. The experiment was conducted during the period from December 2016 to February 2017 in Entre Rios do Oeste-PR. The profiles of vertical and the compression friction pressures were obtained during the loading, storage and unloading phases of corn grains. The vertical pressure...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Metal silos; Grain storage; Instrumentation.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400498

ALTERATIONS ON THE EVAPOTRANSPIRATION OF SUGARCANE CULTIVARS UNDER DISTINCT SALINITY LEVELS APPLIED IN THE FERTIGATION
Provedor de dados: 70
Autores: Toledo,João V.; Zolnier,Sérgio; Silva,Thieres G. F. da; Boehringer,Davi; Steidle Neto,Antonio J.
ABSTRACT: The aim of this research was to evaluate the effect of distinct levels of salinity on the evapotranspiration of the RB867515, RB855453, RB92579 and RB928064 sugarcane cultivars. The evapotranspiration was monitored during daytime period under meteorological conditions influenced, mainly by cloud variations. The salinity values were established by addition of 0, 50, 100 and 150 mM of Sodium Chloride (NaCl) to the nutrient solution, which was applied by fertigation, in such way that the electrical conductivity (EC) of the leached solution was near 3, 6, 10 and 13 dS m−1, respectively. The increase of the NaCl concentration in the nutrient solution affected, significantly and in a linear manner, the evapotranspiration of all sugarcane cultivars,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Efficient water use; Saccharum officinarum; Saline stress; Salinization.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500940

CHARACTERIZATION OF CLOGGING MATERIAL FROM HORIZONTAL SUBSURFACE FLOW CONSTRUCTED WETLAND SYSTEMS
Provedor de dados: 70
Autores: Miranda,Suymara T.; Matos,Antonio T.; Matos,Mateus P.; Borges,Alisson C.; Baptestin,Gheila C. F.
ABSTRACT This study aimed to characterize the material composition responsible for clogging the porous medium of horizontal subsurface flow constructed wetland (HSSF–CW) systems, which is detrimental to a proper system operation. Six completely clogged HSSF–CWs were used after treatment of swine wastewater. Operating conditions of these systems were named CW–C (HSSF– CW 1 and HSSF–CW 4, non-cultivated, i.e. controls), CW–T (HSSF–CW 2 and HSSF–CW 5, cultivated with Tifton 85 (Cynodon spp.)), and CW–A (HSSF–CW 3 and HSSF–CW 6, cultivated with alligator weed (Alternanthera philoxeroides)). The results showed that most of the clogging material was composed of total fixed solids (95, 84, and 82% in CW–C, CW–T, and CW–A, respectively). However, total volatile...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Constructed wetlands; Clogging; Porous medium.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300463

ADJUVANTS IN FUNGICIDE SPRAYING IN WHEAT AND SOYBEAN CROPS
Provedor de dados: 70
Autores: Garcia,Luiz C.; Machado Júnior,Carlos R.; Bochnia,Giovana P.; Weirich Neto,Pedro H.; Raetano,Carlos G.
ABSTRACT The objective of this study was to determine whether the combination of adjuvants to fungicides significantly alters the spray physicochemical characteristics, and potentiates the chemical control of foliar diseases, in that it may affect yield components in wheat (Triticum aestivum) and soybean (Glycine max). The experimental design was completely randomized for the spray physicochemical characteristics, and randomized blocks for the culture variables analyzed, with four treatments and five replications. Treatments consisted of control (no fungicide spraying in the shoot), with fungicides only in plant shoots, fungicides + 0.25% of the spray with adjuvant of methyl ester base of soybean oil, and fungicides + 0.05% of the spray with adjuvant...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Disease; Glycine max; Application technology; Triticum aestivum.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601110

Eficiência de sistemas alagados construídos na remoção de poluentes de águas residuárias de indústria de laticínios
Provedor de dados: 70
Autores: Matos,Antonio T.; Abrahão,Sérgio S.; Lo Monaco,Paola A. V.
Objetivou-se avaliar a eficiência de sistemas alagados construídos (SACs), cultivados com dois diferentes capins e cinco taxas de carregamento orgânico (TCOs) na remoção de poluentes de águas residuárias de indústria de laticínios (ARL). Para isso, unidades experimentais foram constituídas por um SAC sem vegetação (SV), cinco SACs cultivados com capim-elefante (SACs-CF) e cinco SACs cultivados com capim-tifton 85 (SACs-CT), com escoamento subsuperficial horizontal. A ARL foi aplicada numa vazão média de 60 L d-1 e tempo de residência hidráulica de 4,8 dias e TCOs de 66; 130; 190; 320 e 570 kg ha-1 d-1 de DBO5. Os SACs mostraram-se eficientes na remoção da DBO, DQO e dos SSTs, STs e NTKs, porém foram pouco eficientes na remoção de P-total, K e Na da ARL. As...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tratamento de resíduos; Leitos cultivados; Sistemas wetlands.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600016

Consumo de água pela cultura do crisântemo cultivada em ambiente protegido
Provedor de dados: 70
Autores: Pereira,Joelma R. D.; Carvalho,Jacinto de A.; Miguel,Douglas S.; Santana,Márcio J. de.
Com o objetivo de determinar o consumo de água pela cultura do crisântemo, ao longo do seu ciclo de desenvolvimento, conduziu-se um experimento em ambiente protegido, na Universidade Federal de Lavras - MG, com as cultivares Kátia e Bi Time. O delineamento experimental foi o inteiramente casualizado, em esquema fatorial, com duas cultivares e duas freqüências de irrigação, com oito repetições, sendo o manejo da irrigação feito utilizando-se do método da pesagem. O consumo de água entre irrigações foi obtido pela pesagem dos vasos. Instalou-se na área experimental um tanque Classe A, para obter a evaporação e posterior correlação com o consumo hídrico das cultivares. Verificou-se que não houve diferença significativa do consumo quando as cultivares foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manejo da irrigação; Necessidade hídrica; Dendranthema grandiflora.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300010

Eficiência e qualidade da aplicação de misturas em tanque com adjuvantes na dessecação de corda-de-viola
Provedor de dados: 70
Autores: Maciel,Cleber D. de G.; Neto,Antonio M. de Oliveira; Guerra,Naiara; Justiniano,Wagner.
O objetivo do trabalho foi avaliar se a utilização de adjuvantes nas misturas em tanque de glyphosate + chlorimuron-ethyl e glyphosate + carfentrazone-ethyl influenciam na qualidade da aplicação e eficiência de controle de Ipomoea grandifolia. Treze tratamentos, dispostos em delineamento inteiramente casualizado, foram constituídos pelas misturas em tanque de glyphosate + chlorimuron-ethyl (1.440 + 12,5 g ha-1) e glyphosate + carfentrazone-ethyl (1.440 + 10 g ha-1) isoladas e associados aos adjuvantes Nimbus®, Joint Oil®, Naturl'Oil®, Triunfo 515® e All Fix ®, e uma testemunha sem aplicação. Os adjuvantes utilizados foram eficientes na redução da tensão superficial das caldas; no entanto, não influenciaram nos valores de deposição e na eficiência do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Glyphosate; Chlorimuron-ethyl; Carfentrazone-ethyl.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400009

Sustentabilidade na produção de leite: balanço energético em sistema intensivo de produção com visão focada nos processos
Provedor de dados: 70
Autores: Ramos,Marcelo C.; Campos,Alessandro T.; Y. Júnior,Tadayuki; Silva,Karen C. P. da.
O objetivo deste trabalho foi analisar as atividades de produção de leite em sistema intensivo, classificá-las em processos de produção e projetá-las em valores energéticos em Mapa de Fluxo de Valores Energéticos (MFVE). Na pesquisa, realizada em uma fazenda do município de Córrego Fundo-MG, foi feito um estudo dos fluxos energéticos na produção, sendo todo o sistema dividido em processos de produção de milho para silagem, alimentação do rebanho, ordenha, sanidade animal, manejo sanitário e controle de produção. Foram levantados os empregos de energia direta e indireta nos processos produtivos em 2011. O valor unitário da energia empregada na produção de um litro de leite foi de 7,42 MJ kg-1, com eficiência energética de 34,56%. Por meio do Mapa de Fluxo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Indicadores energéticos; Fluxos energéticos; Eficiência energética; Bovinocultura; Construções rurais.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300011

Temperatura da água em bebedouros utilizados em instalações para aves de postura
Provedor de dados: 70
Autores: Klosowski,Elcio S.; Campos,Alessandro T.; Gasparino,Eliane; Campos,Aloíso T. de; Amaral,Daniele F.
A temperatura da água exerce influência sobre o seu consumo pelas aves e sobre a produtividade das mesmas. Entretanto, existe carência de informações comparando a temperatura da água entre os bebedouros mais comumente empregados em aviários de postura no Brasil. Neste trabalho, avaliou-se a variação da temperatura da água para dois tipos de bebedouro: "nipple" e calha. O experimento foi conduzido em uma instalação comercial de postura, localizada na região Oeste do Paraná. Para a determinação da temperatura da água, das 8 às 18 h, foram instalados termômetros de mercúrio com o bulbo inserido no interior da água em bebedouros tipo "nipple" e calha, em dois galpões idênticos. Foi estimado o ITGU do ambiente a partir de dados obtidos de termômetros de globo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas de fornecimento de água; Desempenho térmico; Aves de postura.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300002

ESTIMATION OF MAIZE BIOMASS USING UNMANNED AERIAL VEHICLES
Provedor de dados: 70
Autores: Calou,Vinícius B. C.; Teixeira,Adunias dos S.; Moreira,Luis C. J.; Rocha Neto,Odílio C. da; Silva,José A. da.
ABSTRACT Unmanned aerial vehicles (UAVs) are a promising tool for technology development and transfer and for the economic success of the agricultural sector. The objective of this study is to assess the validity of biomass estimation in a commercial maize plantation using aerial images obtained by a UAV. The proposed methodology involved analyzing images acquired in scheduled flights, processing orthophoto (georeferenced image) data, evaluating digital terrain elevation models, and assessing the quality of dense point clouds. Data were collected using two cameras, one with a 16-megapixel flat lens and the other with a 12-megapixel fish-eye lens coupled to a UAV, at two flight altitudes (30 and 60 meters) over hybrid maize (AG1051) crop irrigated by center...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Structure from Motion; Unmanned aerial vehicles; Zea mays L.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600744

Padrões de distribuição volumétrica de pontas de pulverização de jato plano 11002, com e sem indução de ar, sob diferentes espaçamentos e alturas
Provedor de dados: 70
Autores: Bauer,Fernando C.; Raetano,Carlos G.; Pereira,Francisco de A. R.
O presente trabalho teve como objetivo avaliar a distribuição volumétrica de pontas de pulverização hidráulica de jato de uso ampliado 11002, com e sem indução de ar, em laboratório, bem como o padrão de deposição da pulverização, por meio da estimativa do coeficiente de variação (C.V.) obtido pela simulação da sobreposição de jatos adjacentes. As pontas foram posicionadas, isoladamente, no centro da mesa de teste, a 30; 40 e 50 cm de altura da mesa e a 300 e 500 kPa de pressão. Foram avaliadas 20 unidades de cada tipo de ponta, e a deposição média foi utilizada para a simulação da deposição ao longo da barra pulverizadora, com as pontas espaçadas em 30; 40; 50 e 60 cm entre si. A uniformidade da distribuição foi estimada pelo cálculo do C.V. resultante da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Pulverizador de barra; Indução de ar.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200024

Management strategies of saline water on morphometric characteristics of melon cultivars
Provedor de dados: 70
Autores: Medeiros,José F. de; Terceiro Neto,Cícero P. Cordão; Gheyi,Hans R.; Dias,Nildo da S.; Souza,Mariana S. de M.; Souza,Rauny O. de.
It was to aimed it to investigate effects of various saline water use strategies on melon production and quality of two cultivars (Cucumis melo L., Sancho - C1 and Medellín - C2. The plants were irrigated with water of low (S1 = 0.61 dS m-1) and high (S2 = 4.78 dS m-1) salinity levels, during each crop stage: S1S1S2S2 - T1; S2S1S2S2 - T2; S2S2S1S2 - T3. The 1st, 2nd, 3rd and 4th terms of these sequences correspond to initial growth, flowering, fruit ripening and harvest phenological stages, respectively. Additionally, there was irrigation rotation during all cycle, with water S1 during two days followed by S2 for one day (S1 2 dias + S2 1 dia - T4) and irrigation with non-salt water S2 during all cycle - T5. Moreover, we used as control, the irrigation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cucumis melo L.; Irrigation water quality; Growth analysis.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400005

CALIBRATION AND TESTING OF CS-CROPGRO MODEL FOR COMMON BEANS
Provedor de dados: 70
Autores: Santos,Miquéias G. Dos; Faria,Rogério T. De; Palaretti,Luiz F.; Dantas,Geffson De F.; Dalri,Alexandre B.; Lopes,Adriano Da S.
ABSTRACT: Simulation models of crop growth enable estimating crop yield and water balance components with low cost and high precision. This study aimed to calibrate and evaluate the performance of the CS-CROPGRO model for common beans under the conditions of Jaboticabal city (SP), Brazil. The model was calibrated and tested with data previously collected from two experiments conducted in 2002 and 2003. In these experiments, treatments corresponded to two irrigation scheduling methods (tensiometers and class A pan evaporation) and two cropping systems (conventional and no-till). For calibration, data from the experiment carried out in 2002 were used. For testing, we used data from the experiment conducted in 2003. By using the genetic coefficients...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulation; DSSAT; Phaseolus vulgaris; Irrigation; Planting system.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601239

ESTIMATING VEGETATION VOLUME OF COFFEE CROPS USING IMAGES FROM UNMANNED AERIAL VEHICLES
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Sirqueira Neto,Matheus A.; Hurtado,Sandro M. C.
ABSTRACT Tree crops, such as Arabica coffee (Coffea arabica L.), present enormous technical challenges in terms of pesticide application. The correct deposition and distribution of the active ingredient throughout the aerial part of these plants depends on knowledge of the canopy volume, but manually determining this volume is time consuming and imprecise. The objectives of this study were to develop a method to determine the vegetation volume of coffee crops from digital images captured by camera onboard unmanned aerial vehicles and to compare this approach with traditional vegetation volume estimation (tree row volume (TRV) method). Manual measurements of the canopy volume of four coffee cultivation areas were compared with data obtained using the method...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Unmanned aircraft system; Digital image processing; Canopy volume.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800041

LONG-TERM EFFECTS OF SWINE wastewater AND MINERAL FERTILIZER ASSOCIATION ON SOIL MICROBIOTA
Provedor de dados: 70
Autores: MOURA,ALEXANDRE C. DE; SAMPAIO,SILVIO C.; REMOR,MARCELO B.; SILVA,ADRIANA P. DA; PEREIRA,PAMELA A. M.
ABSTRACT Swine wastewater (SW) application in agricultural soils may affect its microbial community in a long term. The objective of this study was to evaluate prospective changes in soil bacterial community after eight years continuous application of swine wastewater. The wastewater doses tested were 0; 100; 200 and 300 m3 ha-1, being applied from the beginning of the experiment and with or without recommended fertilization. Three soil samples were taken from each plot for determinations of basal respiration, microbial biomass and metabolic quotient. We also performed DGGE analysis and made a correlation between soil chemical conditions and microbial activity. Microbial community underwent significant structural changes from swine wastewater applications....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pig manure; Soil bacterial diversity; Water reuse; Soil microbial biomass; Basal respiration.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200318

INFLUENCE OF DIFFERENT TEMPERATURES AND AIRFLOWS ON DRYING OF NATURAL AND PULPED COFFEE
Provedor de dados: 70
Autores: Alves,Guilherme E.; Borém,Flávio M.; Andrade,Ednilton T.; Isquierdo,Éder P.; Siqueira,Valdiney C.; Dias,Camila de A.
ABSTRACT This study aimed to evaluate drying kinetics for natural and pulped coffee, using different temperatures and drying airflows. For the conduction of the experiment, coffee fruits (Coffea arabica L. cv. Topázio) were harvested manually, selecting only ripe fruits and subsequent to the hydraulic separation. For drying the coffee, use a mechanical dryer with two temperatures (40 and 45°C) and four drying air streams (24; 60; 96 and 132 m3.min-1.m-2). Twelve models for employees to describe the drying kinetics of coffees. Among the models used to describe the drying process of natural coffee and pulped coffee, according to the results of the coefficient of determination, relative mean error, standard deviation of estimates and distribution of waste...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica L.; Mathematical modeling; Drying rate.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200192

PERFORMANCE OF ANALYSIS METHODS OF SLOPE STABILITY FOR DIFFERENT GEOTECHNICAL CLASSES SOIL ON EARTH DAMS
Provedor de dados: 70
Autores: Pereira,Tonismar Dos S.; Robaina,Adroaldo D.; Peiter,Marcia X.; Braga,Fabiano De V. A.; Rosso,Ricardo B.
ABSTRACT The aim of this study was to evaluate the performance of less accurate analysis methods of slope stability, in order to reduce the number of operations used by the most accurate methods available in the literature. The study evaluated four methods for calculating slope stability. Fellenius (FELLENIUS, 1936), Bishop (BISHOP, 1955), Simplified Bishop (BISHOP &amp; MORGENSTERN, 1960) and Simplified Janbu (JANBU, 1973) were compared with the Spencer method (SPENCER, 1967), which is considered an accurate method for calculating the factor of safety (FS). The procedure was performed in scenarios with different soil groups according to the Unified Soil Classification System (USCS) (ASTM 2011), heights and slope inclinations, and under conditions of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fellenius; Bishop; Simplified Bishop; Simplified Janbu; Spencer.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601027

Fuzzy rule-based system for evaluation of uncertainty transaction in cassava chain
Provedor de dados: 70
Autores: GABRIEL FILHO,LUÍS R. A; PIGATTO,GIULIANA A. S.; LOURENZANI,ANA E. B. S.
A fuzzy ruled-based system was developed in this study and resulted in an index indicating the level of uncertainty related to commercial transactions between cassava growers and their dealers. The fuzzy system was developed based on Transaction Cost Economics approach. The fuzzy system was developed from input variables regarding information sharing between grower and dealer on “Demand/purchase Forecasting”, “Production Forecasting” and “Production Innovation”. The output variable is the level of uncertainty regarding the transaction between seller and buyer agent, which may serve as a system for detecting inefficiencies. Evidences from 27 cassava growers registered in the Regional Development Offices of Tupa and Assis, São Paulo, Brazil, and 48 of their...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuzzy system; Transactions; Cassava; Uncertainty.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200350

Medidas radiométricas em casas de vegetação com cobertura plástica na região de Campinas - SP
Provedor de dados: 70
Autores: Costa,Edilson; Leal,Paulo A. M.
Com o objetivo de caracterizar as relações e alterações radiométricas em três casas de vegetação, cobertas com filme transparente de polietileno de baixa densidade (PEBD) de camada simples com 150µm de espessura, tratado contra raios ultravioleta, sob ambientes distintos, foram realizados os experimentos durante o cultivo hidropônico de alface, cultivar Vera, na região de Campinas - SP, em diferentes períodos do ano, visando ao uso de dados experimentais de postos meteorológicos em substituição à necessidade de adquirir equipamentos de radiação para medições internas. As casas de vegetação eram de estrutura metálica de aço, de forma e volume idênticos. Coletaram-se a radiação solar global interna e externa (RSGI e RSGE, W m-2), a radiação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiente protegido; Climatização; Polietileno de baixa densidade; Radiação solar.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300005

SAMPLING DENSITY FOR CHARACTERIZING THE PHYSICAL QUALITY OF A SOIL UNDER COFFEE CULTIVATION IN SOUTHWESTERN MINAS GERAIS
Provedor de dados: 70
Autores: Silvero,Nélida E. Q.; Marques Júnior,José; Siqueira,Diego S.; Gomes,Romário P.; Costa,Milene M. R.
ABSTRACT The elaboration of maps to characterize the spatial variability of soil attributes assists in the strategic planning and decision making of agricultural managers. Precision and accuracy of maps are related to the ideal sampling density to characterize the variability pattern. This study was conducted with the aim of identifying the sampling density to represent the variability of soil physical quality using attributes with different magnitudes of variation in an area cultivated with coffee. Three approaches were used to find the most adequate sampling density (geostatistical analysis, percentage of error associated with the sampling density, and coefficient of variation). A total of 145 soil samples were collected at a depth of 0-0.20 m at the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Coffea arabica; Sampling error; Geostatistics.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500718

Degradação ambiental da bacia hidrográfica do rio Uberaba: uma abordagem metodológica
Provedor de dados: 70
Autores: Candido,Humberto G.; Galbiatti,João A.; Pissarra,Teresa C. T.; Martins Filho,Marcílio V.
O presente estudo trata da avaliação da degradação ambiental da bacia do Rio Uberaba, situada no triângulo mineiro, com área de 241.904,30 ha, abrangendo os municípios de Uberaba, Veríssimo, Conceição das Alagoas e pequena porção de Planura. Neste estudo, foi produzido o mapa de degradação ambiental contendo quatro níveis: baixo, moderado, acentuado e severo. Os parâmetros utilizados nesta avaliação foram: vegetação, topografia, solo/geologia, potencial natural de erosão, mecanização, área agrícola, densidade populacional, pecuarização e área de conflito, aos quais foram atribuídos pesos. Para o nível de degradação "baixo", foram definidos valores ≤ 13 pontos. Para o nível "moderado", valores situados no intervalo de 14 a 16. Entre 17 e 19 pontos para o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistema de informação geográfica; Geoprocessamento; Vulnerabilidade.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100019

TECHNICAL EFFICIENCY AND IMPLEMENTATION COSTS OF SHEEP IDENTIFICATION SYSTEM
Provedor de dados: 70
Autores: Bezerra,Alan C.; Pandorfi,Héliton; Carvalho,Francisco F. R. E; Guiselini,Cristiane; Lima,Thiago A. S. de.
ABSTRACT: The objective of this research was to characterize the efficiency and convenience of sheep identification system and its implementation costs. Therefore we quantified the time for implementation, reading and data transfer to a management program in a manual system (earrings) and electronic system (subcutaneous transponders). Furthermore, it was evaluated the implementation costs of the traceability systems by analysis of the absorption costs and comparison between systems. It was observed that the implementation time for the manual system was shorter (2.2 s animal−1) than the electronic system (4.67 s animal−1). As for reading time, the electronic system presented shorter time (2.89 s animal−1) than the manual system (4.67 s animal−1). As for the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal identification; Sheep production; Traceability.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000501073

STORAGE POTENTIAL OF PEELED CRAMBE FOR OIL QUALITY
Provedor de dados: 70
Autores: Santos,Silas da S.; Biaggioni,Marco A. M.; Monteiro,Iara M. C.; Sartori,Maria M. P.; Brandão,Fernando J. B.
ABSTRACT Peeling of crambe fruits, besides increasing the yield of mechanical oil extraction, can increase its apparent specific mass from about 330 to 700 kgm−3, reducing transport and storage operating costs, as well as increasing cake protein content. However, there is no information on the quality of the oil extracted from the stored unpeeled crambe. This study aimed to assess the possible effects of peeling fruits submitted to different storage systems. For nine months, peeled and unpeeled crambe fruits were stored in conventional (permeable) and hermetic packages and water content, fatty acid, and acidity and oil peroxide indices were monitored. The experimental design was a completely randomized design in a 2 x 2 x 3triple factorial, with three...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hermetic storage; Biofuel; Biodiesel; Oilseeds.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400518

DECREASE IN OFF-PEAK ELECTRICAL ENERGY DEMAND BY AGROINDUSTRIES DUE TO PHOTOVOLTAIC SOLAR GENERATION
Provedor de dados: 70
Autores: Viana,Lucas de A.; Oliveira Filho,Delly; Toledo,Olga M.; da Silva,Samuel C.; Dalvi,Giovanni G.
ABSTRACT The largest energy losses and voltage variations from electricity suppliers occur at times of peak demand. Daytime peaks are mainly influenced by large industrial and commercial consumers. The installation of photovoltaic systems without energy storage to supply part of the demand can contribute to stabilize the voltage and reduce losses. These and other benefits constitute the so-called externality of the decrease in off-peak demand due to photovoltaic generation. The objective of this study was to investigate the role of this externality in agroindustry, as a consumer of electrical energy, in order to better understand its effects on the consumer and the utility. The implementation of photovoltaic systems was simulated with the objective to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Load curve; Demand curve; Cost reduction; Load factor; Photovoltaic system externality.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400537

Controle automático do fluxo de água na etapa de limpeza em unidades de beneficiamento de tomate de mesa
Provedor de dados: 70
Autores: Ferreira,Marcos D.; Benicio,Rafael P.; Umezu,Cláudio K.
A água é um recurso cada vez mais escasso e também de alto custo em várias regiões. O beneficiamento de frutas e hortaliças, em geral, apresenta elevado consumo de água durante o processo de limpeza. A linha de beneficiamento e de classificação do tomate de mesa é constituída de: recebimento, limpeza, seleção, classificação e embalagem. Normalmente, o recebimento dos tomates em uma linha de beneficiamento ocorre com taxa de alimentação constante, porém com interrupções frequentes dos operadores, ocasionando desperdício de energia e água, e a eficiência de limpeza dos frutos. O objetivo deste trabalho foi avaliar um sistema de limpeza dos frutos, equipado com um controle automático de fluxo de água, visando ao uso racional de água. Para a avaliação da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: CLP; Limpeza; Água; Lycopersicon esculentum Mill.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500020

SENSITIVITY OF EVAPOTRANSPIRATION ESTIMATED BY ORBITAL IMAGES UNDER INFLUENCE OF SURFACE TEMPERATURE
Provedor de dados: 70
Autores: Filgueiras,Roberto; Mantovani,Everardo C.; Althoff,Daniel; Dias,Santos H. B.; Cunha,Fernando F. da.
ABSTRACT Surface temperature (Ts) is a determining factor to obtain energy balance parameters, being relevant to understand the influence of this variable on the estimation of evapotranspiration. Thus, the objective of this study was to simulate errors in Ts estimation to verify the consequences of actual evapotranspiration (ETa) estimated by the SAFER (Simple Algorithm for Evapotranspiration Retrieving) model. For this, an image of the Landsat-8 satellite was used to induce errors from 0.2K to 10K in the variable Ts, allowing verifying the consequences in the ETa data. After the estimations of Ts and ETa, the quantitative consequences and dynamics of Ts impact on the ETa data were verified along the different land uses in the study area. The results...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy balance; Irrigated areas; Remote sensing; NDVI.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800023

CHEMICAL CHANGES IN BEAN GRAINS DURING STORAGE IN CONTROLLED CONDITIONS
Provedor de dados: 70
Autores: Almeida,Ana J. B. de; Coelho,Silvia R. M.; Schoeninger,Vanderleia; Christ,Divair.
ABSTRACT Bean (Phaseolus vulgaris L.) is a traditional food in the diet of Brazilians, due to its low fat content and it is rich in vitamins, protein, fiber, carbohydrates and minerals. One of the major problems related to this product is storage without temperature and humidity control, causing quality reduction of this legume. This study aimed to evaluate the effects suffered by cooking time parameters, seed coat color, phytate and minerals (P, Ca, Mg and Mn) content during storage. The grain varieties: BRS Madrepérola, BRS Estilo, BRS Pontal and CNFC 10467, from the pinto group, were stored in hermetic acrylic containers with humidity and temperature controlled for a period of 108 days. All varieties had better results of the parameters studied when...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cooking time; The integument color; Content of phytates.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300529

PHYSICAL AND MECHANICAL PROPERTIES OF PARTICLEBOARD FROM Eucalyptus grandis PRODUCED BY UREA FORMALDEHYDE RESIN WITH SiO2 NANOPARTICLES
Provedor de dados: 70
Autores: Valle,Ana C. M.; Ferreira,Bruno S.; Prates,Glaucia A.; Goveia,Danielle; Campos,Cristiane I. de.
ABSTRACT The use of nanoparticles appears to be a feasible option for improving the quality of a range of wood-based products. Studies show that they can improve both the physical and mechanical properties of wood and wood-based products. This preliminary study aimed to analyze the influence of SiO2 nanoparticles on the physical and mechanical properties of wood particleboard. To this end that, panels were produced without the addition of SiO2 nanoparticles and with the addition of 4% by mass of the urea formaldehyde adhesive used for its production. The results showed that panels produced with the nanoparticles 42% reduction in thickness swelling of the panel. Therefore, the dimensional stability of the panels without decreasing mechanical properties,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thickness swelling; Wood-based products; Adhesives.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300289

Vocalization data mining for estimating swine stress conditions
Provedor de dados: 70
Autores: Moi,Marta; Nääs,Irenilza de A.; Caldara,Fabiana R.; Paz,Ibiara C. de L. Almeida; Garcia,Rodrigo G.; Cordeiro,Alexandra F. S.
This study aimed to identify differences in swine vocalization pattern according to animal gender and different stress conditions. A total of 150 barrow males and 150 females (Dalland® genetic strain), aged 100 days, were used in the experiment. Pigs were exposed to different stressful situations: thirst (no access to water), hunger (no access to food), and thermal stress (THI exceeding 74). For the control treatment, animals were kept under a comfort situation (animals with full access to food and water, with environmental THI lower than 70). Acoustic signals were recorded every 30 minutes, totaling six samples for each stress situation. Afterwards, the audios were analyzed by Praat® 5.1.19 software, generating a sound spectrum. For determination of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sound intensity; Sound attributes; Animal welfare.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300008

Queda de pressão estática por meio de uma coluna de noz macadâmia
Provedor de dados: 70
Autores: Biaggioni,Marco A. M.; Toledo Piza,Pedro L. B.; Ferreira,Widsney A.
As unidades de beneficiamento de macadâmia adotam silos secadores distintos, para cada etapa de secagem, a fim de garantir a manutenção da qualidade do produto pela redução da umidade a níveis desejáveis. Diante da necessidade de quantificar a resistência apresentada pelas nozes, submetidas a diferentes fluxos de ar durante a secagem, bem como avaliar a possibilidade de utilização de modelos empíricos, que estimem o gradiente de pressão a partir da vazão de ar, conduziram-se vários testes em laboratório para obtenção de dados experimentais e ajuste de modelos. Frutos de macadâmia (M. integrifolia), com umidade de 0,11 b.s., após limpeza e classificação, foram colocados no interior de um protótipo constituído por uma coluna de chapa galvanizada (com tomadas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gradiente de pressão estática; Modelos empíricos; Macadâmia.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200024

Light emitting diode (LED) use in artificial lighting for broiler chicken production
Provedor de dados: 70
Autores: Santana,Mayara R. de; Garcia,Rodrigo G.; Naas,Irenilza de A.; Paz,Ibiara C. de L. A.; Caldara,Fabiana R.; Barreto,Bruna.
Light emitting diode (LED) has been used in commercial poultry industry by presenting superior energy savings and providing feasibility on production process. The objective of this research was to evaluate performance and carcass yield of broiler chickens exposed to different LED colors compared with fluorescent lamps. For that, two experiments (E1 and E2) were performed and 2,646 Cobb® chickens were used. In experiment E1, male birds were exposed to 20 lux artificial lighting with red, yellow, blue, and white LED bulbs; and fluorescent bulb. In experiment E2, male and female birds were exposed to 15 lux artificial lighting with red and blue LED bulbs; and fluorescent bulb. Cumulative weight gain (kg), feed intake (kg), feed conversion, hot carcass weight...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry; Production; Artificial lighting.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300005

Predição da configuração de sombras de árvores em pastagens para bovinos
Provedor de dados: 70
Autores: Silva,Roberto G. da.
São propostas equações para a determinação da orientação, comprimento e área da sombra projetada por árvores destinadas ao plantio em pastagens para bovinos, considerando o local, a época do ano e a hora do dia. As equações abrangem árvores com os seguintes formatos de copa: esférica, lentiforme, cilíndrica, elipsóide, cônica e cônica invertida. Um exemplo é apresentado, discutindo-se a aplicação no sombreamento de pastagens.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sombra; Climatologia animal; Bovinocultura.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100029

Sistematização do dimensionamento técnico e econômico de sistemas fotovoltaicos isolados por meio de programa computacional
Provedor de dados: 70
Autores: Marini,José A.; Rossi,Luiz A.
Uma das principais questões referentes à energia solar é como compará-la, técnica e economicamente, com outras fontes de energia, tanto alternativas quanto com as convencionais (como a rede elétrica). O propósito deste trabalho foi desenvolver um programa computacional que reúne os principais dados técnicos e econômicos, para identificar, por meio de métodos de análise microeconômica, a viabilidade comercial no dimensionamento de sistemas fotovoltaicos, além de considerar os benefícios provenientes da própria geração energética. Na análise microeconômica da energia solar, foram identificados os custos da energia proveniente da rede convencional durante o período de vida útil dos componentes do sistema gerador de eletricidade fotovoltaica, pelo estudo dos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energia solar; Programa computacional; Sistema fotovoltaico.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100008

Biodiesel de mamona no diesel interior e metropolitano em trator agrícola
Provedor de dados: 70
Autores: Tabile,Rubens A.; Lopes,Afonso; Dabdoub,Miguel J.; Camara,Felipe T. da; Furlani,Carlos E. A.; Silva,Rouverson P. da.
A demanda de recursos energéticos pelos sistemas de produção, aliada à escassez dos combustíveis fósseis, tem motivado a produção do Biodiesel, que é um combustível obtido de fontes renováveis. O objetivo deste trabalho foi realizar dois ensaios: o primeiro dinâmico, para avaliar o desempenho operacional utilizando como parâmetro o consumo de combustível, e o segundo, estático, para mensurar a opacidade da fumaça (material particulado) do motor de um trator agrícola, operando com diesel metropolitano e interior misturados ao Biodiesel de mamona, em sete proporções. O trabalho foi conduzido no Departamento de Engenharia Rural da UNESP/Jaboticabal - SP. Os resultados mostraram que o tipo de diesel influenciou no consumo de combustível e na opacidade da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biocombustível; Desempenho operacional; Mecanização agrícola; Ricinus communis L.; Opacidade da fumaça.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300008

Qualidade de águas subterrâneas captadas em fontes em função da presença de proteção física e de sua posição na paisagem
Provedor de dados: 70
Autores: Rheinheimer,Danilo dos S.; Gonçalves,Celso S.; Bortoluzzi,Edson C.; Pellegrini,João B. R.; Silva,José L. S. da; Petry,Cláudia.
No meio rural, a água de consumo humano é frequentemente captada por meio de sistemas precários. O objetivo do trabalho foi o de monitorar parâmetros físicos, químicos e microbiológicos da qualidade de água subterrânea captada em fontes para uso doméstico, relacionando suas posições na paisagem e à presença de proteção física. Trinta e cinco fontes de água subterrânea, localizadas na pequena bacia hidrográfica-PBH do Arroio Lino, área rural do Município de Agudo - RS, foram amostradas e classificadas quanto à proteção física e à posição na paisagem. Monitoraram-se, de janeiro a agosto de 2002, os seguintes parâmetros da água: pH, cor, carbono orgânico solúvel total (COST), N-NO3, N-NH3 e fósforo total (PT), Escherichia coli e coliformes totais. Em geral,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Abastecimento rural; Manejo do solo; Saúde pública; Contaminação da água.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500016

Produção de mudas de mamoeiro utilizando diferentes substratos, ambientes de cultivo e recipientes
Provedor de dados: 70
Autores: Costa,Edílson; Santos,Léia C. R. dos; Vieira,Laura C. R.
No Estado de Mato Grosso do Sul, a fruticultura é limitada de informações consistentes, referentes ao potencial de produção de mudas para exploração a campo. Este trabalho avaliou a produção de biomassa em mudas de mamoeiro em diferentes ambientes de cultivo, recipientes e substratos na Universidade Estadual de Mato Grosso do Sul, Aquidauana - MS, de setembro a novembro de 2006. Utilizaram-se os ambientes de cultivo: estufa com filme de polietileno de baixa densidade; viveiro com tela de monofilamento preta; viveiro com tela aluminizada e viveiro com palha de coqueiro nativo. Os substratos "solo + composto orgânico + vermiculita", "solo + composto orgânico + pó de serra" e "solo + composto orgânico + vermiculita + pó de serra" preencheram as sacolas de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carica papaya L.; Estufa; Sacolas; Bandejas.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400003

Análise de imagens para a caracterização das atividades de vacas leiteiras dentro do galpão de confinamento
Provedor de dados: 70
Autores: Souza,Silvia R. L. de; Nääs,Irenilza de A; Moura,Daniella J. de.
A produção atual de animais necessita do emprego de tecnologias de informação automatizadas, inerentes ao ambiente em que os animais estão inseridos, para que se possa analisar a interferência dos mesmos na produção e no bem-estar. O objetivo desta pesquisa foi comparar a eficiência de duas metodologias de análise de imagens, utilizadas para avaliar a presença de vacas leiteiras em locais específicos no galpão de confinamento. O experimento foi realizado em uma fazenda comercial, e as vacas foram monitoradas através de seis microcâmeras. Foram usadas duas formas de análise da presença das vacas nos locais pré-selecionados (camas, bebedouros e comedouros): imagens analisadas visualmente da tela do computador (T1) e automaticamente, pelo software...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Comportamento; Análise de imagens; Zootecnia de precisão.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600001

Mathematical models to describe the volumetric shrinkage rate of red beans during drying
Provedor de dados: 70
Autores: Corrêa,Paulo C.; Resende,Osvaldo; Garin,Silvia A.; Jaren,Carmen; Oliveira,Gabriel H. H. de.
The present study aimed to determine the volumetric shrinkage rate of bean (Phaseolus vulgaris L.) seeds during air-drying under different conditions of air, temperature and relative humidity, and to adjust several mathematical models to the empiric values observed, and select the one that best represents the phenomenon. Six mathematical models were adjusted to the experimental values to represent the phenomenon. It was determined the degree of adjustment of each model from the value of the coefficient of determination, the behavior of the distribution of the residuals, and the magnitude of the average relative and estimated errors. The rate of volumetric shrinkage that occurred in bean seeds during drying is between 25 and 37%. It basically depends on the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus vulgaris L.; Moisture content; Volume; Air-drying; Physical property.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400010

Evaluation of the effect of the seed extract of Moringa oleifera Lam over the efficiency of organic filters in wastewater treatment of dairy cattle breeding
Provedor de dados: 70
Autores: Francisco,João P.; Silva,Jonathas B. G.; Roque,Odir C. C.; Nascentes,Alexandre L.; Silva,Leonardo D. B.
This study aimed to evaluate the effect of Moringa oleifera Lam extract on the removal of total solids (TS), total suspended solids (TSS) and chemical oxygen demand (COD), in different filter media for treating wastewater of dairy cattle breeding (DCW). The moringa seed extract was obtained by grinding 50 g of seeds in one liter of distilled water and, after passing the solution through a quantitative paper filter of 25 microns, 60 mL of the extract were added to wastewater from cattle breeding before the filtration process in organic filters made of thin coal, bamboo leaves, eucalyptus leaves, gliricidia branches and sawdust. This was followed by the completely randomized experimental design, adopting a factorial of 5 x 2. Aliquots of filtered effluent...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coagulant; Fertigation; Water treatment.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100015

Desenvolvimento e testes de uma semeadora-adubadora modular para pequenas propriedades rurais
Provedor de dados: 70
Autores: Arend,Lucas; Forcellini,Fernando A.; Weiss,Augusto.
O trabalho apresenta o desenvolvimento e testes de campo de equipamento agrícola modular. Para o desenvolvimento do equipamento, foi utilizada metodologia de projeto para sistemas modulares. O objetivo principal foi desenvolver um sistema modular que contribuísse para melhorar o atual quadro de mecanização agrícola da pequena propriedade rural, enfocando alguns dos equipamentos destinados às atividades conservacionistas de cultivo. Por ser modular, o equipamento atende às funções de semear-adubar, escarificar e sulcar o solo. Para a função semear-adubar, podem ser usados cinzéis e disco duplo para a semeadura; já para as funções de escarificação e sulcagem, podem ser usadas ferramentas específicas, facilmente intercambiadas em um chassi tubular principal....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semeadora-adubadora modular; Plantio direto; Testes de campo.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300027

Variabilidade espacial da textura de um latossolo vermelho eutroférrico sob cultivo de cana-de-açúcar
Provedor de dados: 70
Autores: Souza,Zigomar M.; Marques Júnior,José; Pereira,Gener T.; Barbieri,Diogo M.
Estudos regionais mais detalhados, utilizando modelos de paisagem e geoestatística, têm demonstrado que, em áreas consideradas homogêneas, sob uma única classe de solo, existe dependência espacial de atributos granulométricos. Visando a avaliar a variabilidade espacial de atributos granulométricos em Latossolo Vermelho eutroférrico, foram feitas amostragens do solo em intervalos regulares de 50 m, em forma de malha, totalizando 306 pontos de amostragem. Foram coletadas amostras nas profundidades de 0-0,2 m e 0,6-0,8 m para a determinação da argila, silte, areia total (AT), areia grossa (AG), areia média (AM), areia fina (AF) e areia muito fina (AMF). Os dados foram submetidos à análise estatística descritiva, geoestatística e interpolação por krigagem. Os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Krigagem; Atributos físicos.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200009

Condutância estomática como indicador de estresse hídrico em feijão
Provedor de dados: 70
Autores: Oliveira,Alexsandra D. de; Fernandes,Edemo J.; Rodrigues,Teresinha de J. D.
O objetivo do trabalho foi verificar os indicadores de estresse hídrico, bem como seu efeito na cultura do feijão, por meio da condutância estomática. O experimento foi realizado na Área Experimental de Irrigação da Universidade Estadual Paulista - Jaboticabal, no ano agrícola de 2000. Foram estudados quatro tratamentos de irrigação com níveis crescentes de ETm: (T1) ETm acumulada = 22 mm; (T2) ETm acumulada = 33 mm; (T3) ETm acumulada = 44 mm; (T4) ausência de irrigação. Nas plantas com suprimento adequado de água, os maiores valores de condutância estomática ocorreram por volta do meio-dia solar, atingindo cerca de 159 e 174 mmol m-2 s-1, para T1 e T2, respectivamente, enquanto nos tratamentos T3 e T4, os maiores valores encontrados foram de 83 e 52 mmol...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus vulgaris; Parâmetros fisiológicos; Irrigação.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100010

Produtividade de soja em semeadura direta influenciada por profundidade do sulcador de adubo e doses de resíduo em sistema irrigado e não irrigado
Provedor de dados: 70
Autores: Herzog,Ricardo L. da S.; Levien,Renato; Trein,Carlos R.
O experimento foi conduzido na EEA-UFRGS, em Argissolo Vermelho distrófico típico, com o objetivo de quantificar o volume de solo mobilizado e a produção total de biomassa de soja em uma área de campo nativo, anteriormente cultivada com aveia-preta. Após a colheita, o resíduo de aveia foi distribuído nas parcelas, nas doses de 0; 2; 3; 4; 5 e 6 Mg ha-1, que constituíram os tratamentos principais, os quais, por sua vez, foram subdivididos em função de profundidades (0,06 m e 0,12 m) de atuação dos sulcadores de adubo, tipo facão, da semeadora-adubadora. O delineamento foi o de blocos casualizados, com três repetições. Os tratamentos foram conduzidos em áreas distintas, com e sem irrigação. O volume de solo mobilizado pelos sulcadores de adubo foi 53% maior...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biomassa; Mobilização do solo; Plantio direto.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300031

Errata: volume 32, número 6
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100021

GÁLIA MELONS PRODUCTION IN PROTECTED ENVIRONMENT UNDER DIFFERENT IRRIGATION DEPTHS
Provedor de dados: 70
Autores: Lima,Elvis M. de C.; Carvalho,Jacinto de A.; Viol,Miguel A.; Almeida,Rodrigo C. de; Rezende,Fátima C.
ABSTRACT The study aimed to evaluate the “Gália” melons productive characteristics grown in greenhouse under different irrigation levels, and conducted with and without soil cover by plastic mulching. Experiments I (WC) and II (WtC) were conducted simultaneously in a protected environment, using a completely randomized design (CRD), where plants of Gália melons (Hybrid Nectar cv.) received five levels of water depth defined by 50, 75, 100, 125 and 150% of evapo-transpiration (water requirement), with four replications, differing only by utilization (WC) or not (WtC) of plastic mulching. The results showed that the variables productivity, average weight, length and diameter of the fruits were affected by different levels of water replacement in the soil...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation management; Protected environment; Productivity.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100075

Crescimento e componentes de produção da mamoneira sob estresse salino e adubação nitrogenada
Provedor de dados: 70
Autores: Lima,Geovani S. de; Nobre,Reginaldo G.; Gheyi,Hans R.; Soares,Lauriane A. dos A.; Silva,Alexsandro O. da.
Esta pesquisa foi realizada com o propósito de avaliar o crescimento e os componentes de produção da mamoneira cv. BRS Energia sob diferentes níveis de salinidade da água de irrigação e de doses de nitrogênio em condições de campo, no Neossolo Regolítico eutrófico típico de textura franco-arenosa, no município de Pombal - PB, em delineamento de blocos ao acaso, testando-se cinco níveis de salinidade da água de irrigação-CEa (0,4-controle, 1,4; 2,4; 3,4 e 4,4 dS m-1) e cinco doses de N (50; 75; 100; 125 e 150 mg kg-1), em esquema fatorial 5 x 5, com três repetições. O aumento da CEa, a partir de 0,4 dS m-1, promoveu redução do número de folhas (NF), da altura de planta (AP), do diâmetro de caule (DC), da massa seca da parte aérea (MSPA), do comprimento do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ricinus communis; Água salina; Nitrogênio.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500005

Variabilidade espacial da umidade de um Latossolo Vermelho-Amarelo sob plantio direto
Provedor de dados: 70
Autores: Sampaio,Fabrício de M. T.; Ferreira,Mozart M.; Oliveira,Marcelo S. de; Almeida,Alberto C.; José,Marcos R.
O estudo da dependência espacial de atributos do solo é importante para aprimorar as práticas de manejo e de amostragem. Este trabalho teve o objetivo de estudar a variabilidade espacial da umidade de um Latossolo Vermelho-Amarelo sob plantio direto, cultivado com milho, e sua relação com o carbono orgânico total do solo, macroporosidade e microporosidade. A pesquisa foi conduzida em uma área localizada no município de Lavras - MG. Na avaliação dos atributos do solo, foi delineada uma malha experimental com dimensões iguais a 90 x 90 m (0,81 ha de área), com espaçamento entre os pontos de amostragem de 15 x 15 m. Para obter maior detalhamento da dependência espacial dos dados, realizou-se a implantação de mais duas malhas (zoom) dentro de um quadrante da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Manejo do solo; Reflectometria no domínio do tempo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500008

STABILITY OF PARTIAL NITRITATION OF POULTRY SLAUGHTERHOUSE WASTEWATER IN A SEQUENTIAL BATCH REACTOR
Provedor de dados: 70
Autores: Assis,Tatiane M. de; Schilichting,Marcos V.; Lopes,Carla L.; Kunz,Airton; Gomes,Simone D.
ABSTRACT The aim of this study was to monitor the stabilization of a sequential batch reactor (SBR) regarding the partial nitritation of poultry slaughterhouse wastewater, aiming at preparing it for a reactor with bacteria that promote anaerobic ammonia oxidation (anammox). A cylindrical reactor with a useful volume of 3.5 L, mechanical agitation (50 rpm), and suspended biomass was used in the experiment. The strategies adopted for nitrite-oxidizing bacteria (NOB) inhibition were cycle time (CT: 24, 16, 6, 5, 4 h and real-time monitoring), free ammonia accumulation, alkalinity restriction and low concentrations of dissolved oxygen (DO). The ammonification process, observed at all experimental phases, negatively influenced the control of partial nitritation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anammox; Deammonification; Nitrite; Nitrate; Nitrafying.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200323

Análise da adequação ambiental e manejo dos dejetos de instalações para suinocultura em propriedades na região oeste do Paraná
Provedor de dados: 70
Autores: Daga,Jacir; Campos,Alessandro T.; Feiden,Armin; Klosowski,Elcio S.; Câmara,Roberto J.
Os dejetos de suínos são resíduos altamente poluidores, que prejudicam o meio ambiente, em especial a qualidade da água e o desenvolvimento de peixes e outros organismos aquáticos. Com isso, o objetivo deste trabalho foi verificar o perfil da suinocultura, a análise da adequação das instalações, os sistemas de manejo dos dejetos, bem como a adequação à legislação ambiental das propriedades agrícolas localizadas na microbacia do Córrego Ajuricaba, selecionada e localizada na bacia hidrográfica do Rio São Francisco Verdadeiro, na região Oeste do Paraná. Os resultados apresentados neste trabalho referem-se a dez propriedades das 110 analisadas. O perfil da suinocultura é de 80% dos suinocultores com sistema de criação em terminação e 20% em ciclo completo;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resíduos; Sustentabilidade; Construções para suínos.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400001

WEAR QUANTIFICATION OF BASAL CUTTING KNIVES IN SUGARCANE HARVESTING
Provedor de dados: 70
Autores: Paixão,Carla S. S.; Voltarelli,Murilo A.; Oliveira,Luan P. de; Bernache,Leonardo; Silva,Rouverson P. da.
ABSTRACT The mechanized harvesting of sugarcane has increased exponentially in recent years because of the gradual prohibition of burning on the cane fields in mechanizable and non-mechanizable areas. This study aimed to evaluate the wear of the basal cutting knives in two different mechanized sugarcane harvesters, through statistical process control. The experiment was conducted in Cravinhos, São Paulo, in an agricultural area, on July 25, 26, and 27, 2016. Two harvesters with different basal cutting mechanisms were evaluated: harvester A—Model BE1035e (conventional type knife), and harvester B—Model A8800 (racket type knife). The experimental design was completely randomized with two treatments. The wear was quantified by measuring the thickness increase...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Basal cutting; Control charts; Mechanized harvesting; Quality indicator; Statistical process control.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400498

Umidade e temperatura de argissolo amarelo em sistemas de preparo e estádios de desenvolvimento do milho
Provedor de dados: 70
Autores: Cortez,Jorge W.; Nagahama,Hideo de J; Olszevski,Nelci; Patrocinio Filho,Antonio P; Souza,Elder B.
RESUMO Os sistemas de preparo do solo afetam a quantidade de resíduo vegetal sobre a superfície do solo e, consequentemente, sua umidade e temperatura. Objetivou-se avaliar a temperatura e a umidade do Argissolo Amarelo em estádios de desenvolvimento da cultura do milho sob sistemas de preparo mecanizado. O experimento foi conduzido no delineamento em blocos inteiramente casualizados, com quatro repetições, em Petrolina - PE. Os sistemas de preparo do solo foram: sem preparo primário, grade off-set de discos de 0,56 m, grade off-set de discos de 0,61 m, escarificador e arado de aivecas. As leituras de umidade e temperatura foram realizadas ao longo do dia, nos horários de 6; 9; 12; 15 e 18 h, nos estádios de desenvolvimento V3, V8, R3 e R6 do milho. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanização agrícola; Semiárido Nordestino; Variação térmica.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400699

USE OF GROUND PENETRATING RADAR TO STUDY SPATIAL VARIABILITY AND SOIL STRATIGRAPHY
Provedor de dados: 70
Autores: Campos,José R. da R.; Vidal-Torrado,Pablo; Modolo,Alcir J.
ABSTRACT Ground Penetrating Radar (GPR) is a geophysical method that uses electromagnetic waves to study subsurface structure in different fields such as geology, agriculture and civil engineering. The wave penetration in the soil is strongly controlled by the electrical conductivity of soil components such as clay, organic matter, and water. In this study, tests were conducted in a floodplain in the Elizabeth Creek watershed (New Jersey – USA). We established one transect where measurements were completed using two techniques, common mid point (CMP) and constant offset profile (COP), both with 100- MHz frequency antennas. Measurements were also completed using 250 and 500 MHz shielded antennas. GPR showed good accuracy to study soil spatial variability...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geophysics; Soil stratigraphy; Agricultural engineering.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300358

Sistema fuzzy para predição do desempenho produtivo de frangos de corte de 1 a 21 dias de idade
Provedor de dados: 70
Autores: Ponciano,Patrícia F.; Yanagi Junior,Tadayuki; Schiassi,Leonardo; Campos,Alessandro T.; Nascimento,José W. B. do.
Um sistema de inferência fuzzy foi desenvolvido baseado em dados da literatura para predição do consumo de ração, ganho de peso e conversão alimentar de frangos de corte com idade variando de 1 a 21, dias submetidos a diferentes condições térmicas. O sistema fuzzy foi estruturado com base em três variáveis de entrada: idade das aves (semanas), temperatura (°C) e umidade relativa (%) ambientes, sendo que as variáveis de saída consideradas foram: ganho de peso, consumo de ração e conversão alimentar. A inferência foi realizada por meio do método de Mamdani, que consistiu na elaboração de 45 regras e a defuzzificação por meio do método do Centro de Gravidade. Com base nos resultados, ao se compararem os dados da literatura com os obtidos pelo sistema fuzzy...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelagem; Inferência fuzzy; Conforto ambiental.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300004

Ajuste de parâmetros de transporte de solutos no solo utilizando Matlab 6.5
Provedor de dados: 70
Autores: Souza,Anderson L. de; Matsura,Edson E; Miranda,Jarbas H. de; Colombo,Alberto.
O sucesso na utilização de modelos matemáticos no estudo do transporte de íons no solo está intimamente ligado à precisão com que os parâmetros de transporte envolvidos neste processo são estabelecidos. De maneira geral, tais parâmetros são determinados mediante a resolução de um problema de otimização não linear em que os dados experimentais, obtidos em ensaios de deslocamento miscível, são ajustados a um modelo teórico. Neste sentido, a utilização de softwares de alta performance no ajuste destes parâmetros mostra-se vantajosa, uma vez que, além da consistência e da disponibilidade de ferramentas numéricas preexistentes, possibilita a incorporação de novas rotinas de acordo com o fenômeno que se queira simular. Sendo assim, este trabalho teve como...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Curva de distribuição de efluentes; Rotina computacional; Dinâmica de solutos.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600004

Concentration of injetion solution and its effects on soil and on yield of fertirrigated banana cv. Terra Maranhão
Provedor de dados: 70
Autores: Coelho,Eugênio F.; Andrade Neto,Torquato M. de; Barros,Damiana L.
The Fertigation is the combined application of water and nutrients to a crop. It can be adapted to all types of agricultural crops. The objective of this study was to evaluate the effect of urea concentration in irrigation water on electrical conductivity of the soil solution and saturation extract along the first cycle of banana cv. Terra Maranhão. The experiment followed a completely randomized design with six treatments and ten replications. Treatments regarded for using three urea concentrations (1.0; 2.5 and 4.0 g L-1) in irrigation water applied by two micro irrigation systems (microsprinkler and drip). Results showed that there was a linear elevation of electrical conductivity of saturation extract and soil solution with the increase on...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Urea; Salinity; Fertirrigation.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600007

Variations on the expertise of two attributes of physical soil due to differences in the method of global satellite navigation
Provedor de dados: 70
Autores: CRISTIANO,ZERBATO; COMPAGNON,ARIEL M.; VOLTARELLI,MURILO A.; ROSALEN,DAVID L.; FURLANI,CARLOS E. A.
ABSTRACT The mechanical resistance to penetration when related to the water content is an indicator often used of soil compaction, the use of positioning methods for greater accuracy of this review is important. In this context, this study aimed to determine the variability of positioning methods provided by GPS receivers to determine the spatial behavior of physical attributes related to soil compaction. The study area is located in the municipality of Jaboticabal, around the latitude 21º15’22”S and longitude 48º18’58”W, being characterized with a clayey Oxisol. The variables used as parameters of soil physical properties were the mechanical resistance to penetration and water content, using a sampling grid of 20 x 20 m, totaling 60 points. We used six...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: GPS; Penetrometer; Soil compaction; Soil water content.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400696

BOVINE WELLFARE HANDLED IN ADAPTED CORRAL WITH UNCONVENTIONAL MATERIALS
Provedor de dados: 70
Autores: Sartori,Diogo de L.; Nakanishi,Erika Y.; Cravo,Julio C. M.; Martello,Luciane S.; Fiorelli,Juliano.
ABSTRACT This study aimed at evaluating bovine behavioral parameters managed in crowding pens built with modular panel of reforestation wood and homogeneous particle sheets of sugarcane bagasse and in conventional wooden crowding pens. The animals treated had their body surface temperature measured by the infrared thermography method and the behavior evaluated through the flight time parameters and the behavior score in the crowding pens. The results indicated that the animals managed in these buildings showed no difference in the behavioral parameters, but the mean and maximum superficial body temperatures were lower in the animals managed in the crowding pens of modular panel.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Particle sheet; Rural buildings; Animal reactivity; Body surface temperature.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300272

Economic analysis of cashew early dwarf Crop BRS - 189 depending on water levels and doses of potassium fertilization
Provedor de dados: 70
Autores: Leite,Kelly N.; Costa,Raimundo N. T.; Crisótomo,João R.; Frizzone,José A.; Marinho,Albanise B.
Water and fertilizer among the production factors are the elements that most restrict the production of cashew. The precise amount of these factors is essential to the success of the crop yield. This research aimed to determine the best factor-product ratio and analyze technical and economic indicators, of productivity of the cashew clone BRS 189 (Anacardium occidentale) to production factors water and potassium. The experiment was conducted from May 2009 to December 2009 in an experimental area of 56.0 m x 112.0 m in the irrigated Curu - Pentecoste, located in the municipality of Pentecoste, Ceará, Brazil. Production factors water (W) and potassium (K) were the independent variables and productivity (Y), the dependent variable. Ten statistical models that...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anacardiun occidentale; Irrigation; Potassium.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400013

Evaluation of alternative containers to determining the working width of fertilizer spreaders
Provedor de dados: 70
Autores: Primo,Marcelo A.; Gurgacz,Flavio; Kunz,Vilson L.; Primo,Lucas I.; Furlan,Fernando; Silva,Suedêmio L.; Gabriel Filho,Antonio.
Farmers have difficult of determining the evenness of transverse distribution and the working width, due the tests with this aim require equipments and complex methodologies. So, this study evaluates some alternative containers with the aim to allow a more accessible adjustment of the full width of the solid fertilizer spreaders. Four different containers were tested: i) standard container constructed in accordance with ISO 5690/1; ii) container of polyethylene (plastic trays) with screen shading to prevent the ricochet of material; iii) containers composed by boxes of long-life milk, and iv) containers composed by flowerpots (number 3.5). Also, three different spreaders were used for the tests. Alternative containers showed greater retention of particles...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertilization at throw; Agricultural machines; Agricultural mechanization.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300013

As, Cu AND Zn CONCENTRATION IN SANITARY SEWAGE SLUDGE FERTILIZED SOIL AND IN CRAMBE AND CORN GRAINS
Provedor de dados: 70
Autores: Cardoso,Paulo H. S.; Sousa,Izabelle de P.; Junio,Geraldo R. Zuba; Gonçalves,Paula W. B.; Sampaio,Regynaldo A.
ABSTRACT This study aimed to evaluate the total contents of As, Cu and Zn in the profile of a Haplic Cambisol cultivated with crambe and corn and fertilized with sanitary sewage sludge and to compare them with those obtained in other forms of fertilization, as well as the content of metals in the grain of these crops. Two experiments were carried out in the field, one with maize cultivation and another with crambe, both were delineated as randomized blocks with four treatments and six replicates, which were: without fertilization, fertilization with sewage sludge dewatered and dried in the sun, with dry sewage sludge and with mineral fertilizers. At the end of the experiments soil samples were collected at 15, 50, 100, 150 and 200 cm depth for analysis of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biosolid; Crambe abyssinica; Organic fertilization; Zea mays.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300426

Comparison between hydrographically conditioned digital elevation models in the morphometric charaterization of watersheds
Provedor de dados: 70
Autores: Guedes,Hugo A. S.; Silva,Demetrius D. da.
The aim of this study was to compare the hydrographically conditioned digital elevation models (HCDEMs) generated from data of VNIR (Visible Near Infrared) sensor of ASTER (Advanced Spaceborne Thermal Emission and Reflection Radiometer), of SRTM (Shuttle Radar Topography Mission) and topographical maps from IBGE in a scale of 1:50,000, processed in the Geographical Information System (GIS), aiming the morphometric characterization of watersheds. It was taken as basis the Sub-basin of São Bartolomeu River, obtaining morphometric characteristics from HCDEMs. Root Mean Square Error (RMSE) and cross validation were the statistics indexes used to evaluate the quality of HCDEMs. The percentage differences in the morphometric parameters obtained from these three...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digital elevation models; Water resources; Remote sensing; Morphometry.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500012

APPLICATION EFFECT OF DIFFERENT RATES OF WASTEWATER FROM GELATIN PRODUCTION IN THE CHEMICAL ATTRIBUTES OF THE SOIL
Provedor de dados: 70
Autores: Silvano,Caroline; Freitas,Paulo S. L.; Rezende,Roberto; Mioto,Liliane S.; Dallcort,Rivanildo.
ABSTRACT The gelatin industry wastewater has nutrients in its composition, allowing its use in agriculture as an alternative to disposal and recycling of this residue. However, high application rates can cause the accumulation of elements such as sodium in the soil, and generate negative impacts on the environment. This study aimed to evaluate the effects of the application of rates up to 600 m3ha-1 of gelatin industry wastewater in soil columns, on soil chemical attributes in five depths. The experiment was conducted in a greenhouse, in PVC tube columns (0.20 m diameter) filled with distroferric Red Nitosol soil, of very clayey texture. The treatments consisted of increasing rates of wastewater equivalent to 0, 150, 300, 450 and 600 m3 ha-1, with a single...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertirrigation; Leaching; Sodium; Soil fertility.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400606

Metodologia para obtenção do hidrograma de escoamento superficial em encostas e canais. Parte I: desenvolvimento e avaliação
Provedor de dados: 70
Autores: Silva,José M. A.; Pruski,Fernando F.; Silva,Demetrius D.; Cecílio,Roberto A.
Desenvolveu-se uma metodologia que permite obter o hidrograma de escoamento superficial e a vazão máxima para qualquer posição ao longo de uma encosta e para seções transversais de canais utilizando o modelo de ondas cinemáticas. A área da encosta é dividida num sistema matricial composto por 100 linhas e 100 colunas. Na encosta, considera-se que o escoamento ocorre na direção da declividade e que a vazão de cada pixel é a soma da vazão produzida nesse com a vazão advinda dos pixels que contribuem com o escoamento superficial para o pixel em análise. No canal, a vazão é calculada pela soma dos hidrogramas advindos das colunas do sistema reticulado. A comparação entre os valores de lâmina e vazão máxima de escoamento superficial obtidas experimentalmente e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelagem hidrológica; Conservação de água e solo.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300005

Aerodinâmica de leitos vibrofluidizados: uma revisão
Provedor de dados: 70
Autores: Park,Kil J.; Brod,Fernando P. R.; Oliveira,Rafael A. de.
Aplicações da vibração mecânica com o intuito de facilitar a fluidização e aumentar as transferências de calor, massa e quantidade de movimento são processos comumente utilizados nas agroindústrias, que atualmente encontram suas aplicações no processamento de partículas difíceis de fluidizar. Equações e dados experimentais encontrados na literatura das características aerodinâmicas de leitos vibrofluidizados são apresentados e discutidos, ressaltando o efeito da vibração no leito.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Perda de carga; Velocidade mínima de fluidização; Porosidade do leito.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300023

Thermal comfort in reduced models of broilers' houses, under different types of roofing materials
Provedor de dados: 70
Autores: Almeida,Eduardo A. de; Passini,Roberta.
The research was developed to evaluate the use of different types of roofing materials regularly used in poultry houses. Measurements of thermal comfort were made through the use of techniques such as the Black Globe and Humidity Index (BGHI), the Thermal Heat Load (THL) and Enthalpy (H). Conducted in the State University of Goiás, during the months of April and May, 2011, the experiment was composed of five different treatments: AC - Asbestos cement tiles, BA -Bamboo tiles, BAP - Bamboo tiles painted in white, FB -Vegetable fiber tiles and bitumen, FBP -Vegetable fiber tiles and bitumen painted in white. The experiment consisted in 15 repetitions, which were considered the different days of measurements taken. Throughout the studied period, the time of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Alternative roofing material; Poultry production.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100003

Desempenho de válvulas antigotas e microaspersores
Provedor de dados: 70
Autores: Sandri,Delvio; Bessa,Kady S. E.; Mesquita,Márcio; Prado,Lazaro C. R. A.
Nos últimos anos, foram introduzidos novos modelos de dispositivos para cultivo em ambiente protegido, como as válvulas antigotas e microaspersores, necessitando-se avaliar o desempenho dos mesmos. Assim, o objetivo deste trabalho foi avaliar o desempenho hidráulico de válvulas antigotas novas e usadas, sob baixa e alta pressão, em microaspersores do grupo modular e modelo Hadar. O CVf e CVq do conjunto microaspersor e válvula antigotas de baixa pressão e somente o microaspersor modular foram classificados como ruins ou inaceitáveis e a válvula anti-gotas modular de alta pressão nova como inaceitável. A válvula Hadar apresentou o melhor desempenho para todas as pressões de serviço. As válvulas avaliadas abriram em pressões inferiores às indicadas pelos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Equação vazão x pressão; Microaspersor; Estufa; Irrigação.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400007

DEFICIT IRRIGATION OF SUBSURFACE DRIP-IRRIGATED GRAPE TOMATO
Provedor de dados: 70
Autores: Mendonça,Thaís G.; Silva,Marília B. da; Pires,Regina C. de M.; Souza,Claudinei F.
ABSTRACT Agriculture is one of the segments that most uses water and developments have been made to save irrigation water. Deficit irrigation is a technique that can contribute to production and water saving in agriculture. This study aimed to evaluate the viability of deficit irrigation in tomato production irrigated by subsurface drip in a greenhouse and estimate water saving. The experiment was conducted at the CCA/UFSCar, in Araras, São Paulo, Brazil, with grape tomato cultivation. It consisted of three treatments, 100 % water depth and deficit irrigation (75 and 50 % of water depth), with a randomized block design. Irrigation management was performed using mean soil moisture data collected through TDR probes installed in each treatment. Tomato plants...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: TDR; Water resources; Irrigation management; Water content.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400453

LOW-COST AUTOMATION OF FERTIGATION WITH PROGRAMMABLE LOGIC CONTROLLER AND GAS-FILLED SENSORS
Provedor de dados: 70
Autores: Bezerra,Ricardo de S.; Evangelista,Adão W. P.; Vellame,Lucas M.; Alves Júnior,José; Casaroli,Derblai.
ABSTRACT The aim of this study was to develop and evaluate a low-cost automation system for management of different fertigation regimes in tomato plants (Solanum lycopersicum L.) grown in a protected environment. The system consisted of an irrigation controller coupled to substrate moisture sensors and to a programmable logic controller (PLC). Four water regimes and nutrient supply levels were considered during evaluations. While developing, functional tests were performed to the automation system. Moreover, a cost-benefit analysis for the assembling of the system was carried out. As result, we noted that the automation system was efficient for controlling fertigation. It showed no problems regarding malfunction, still presenting a lower cost if compared...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water management; Microcontroller; Matrix potential.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200394

Desenvolvimento de software e hardware para irrigação de precisão usando pivô central
Provedor de dados: 70
Autores: Queiroz,Tadeu M. de; Botrel,Tarlei A.; Frizzone,José A.
O presente trabalho teve por objetivo desenvolver softwares e hardwares para aplicação ao monitoramento e controle automático para a irrigação de precisão usando sistemas do tipo pivô central. O trabalho foi desenvolvido no Departamento de Engenharia Rural - LER, da Escola Superior de Agricultura "Luiz de Queiroz" - ESALQ, da Universidade de São Paulo - USP, em Piracicaba - SP. Foram utilizados componentes eletrônicos discretos, circuitos integrados diversos, módulos de radiofreqüência, microcontroladores da família Basic Step e um microcomputador. Foram utilizadas as linguagens Delphi e TBasic. O hardware é constituído de dois circuitos eletrônicos, sendo um deles para "interface" com o computador e o outro para monitoramento e transmissão da leitura de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Automação; Eletrônica; Manejo da irrigação.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100005

Soil physical attributes in chemigated banana plantation with wastewater
Provedor de dados: 70
Autores: Alves,Pablo F. S.; Santos,Silvânio R.; Kondo,Marcos K.; Pegoraro,Rodinei F.; Araújo,Edcássio D.
ABSTRACT The feasibility of using sewage wastewater as a water and nutrient source for plants is an alternative to harness agricultural natural resource, observing its influence on the organic matter dynamics and soil energy. Our objective here was to evaluate the effects of applying different doses of effluent from a sewage treatment plant, in Janaúba – MG, Brazil, over the physical attributes of a soil grown with “Prata Anã” banana. From soil sample collection at depths of 0-20, 20-40, and 40-60 cm, we determined the following soil properties: soil density, total porosity, macroporosity, microporosity, organic matter, clay dispersed in water and stability of soil aggregate. The experimental design was in randomized blocks with four repetitions....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Musa spp; Agricultural reuse of effluents; Environmental sanitation; Semi-arid.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000600998

K-NEAREST NEIGHBORS METHOD FOR PREDICTION OF FUEL CONSUMPTION IN TRACTOR-CHISEL PLOW SYSTEMS
Provedor de dados: 70
Autores: Al-Dosary,Naji Mordi Naji; Al-Hamed,Saad Abdulrahman; Aboukarima,Abdulwahed Mohamed.
ABSTRACT Most important farm operations require a significant amount of energy, and this consumes a major portion of the farm's budget. Consequently, analyzing the fuel consumption of agricultural machinery for farm operations of different sizes makes it possible to predict fuel consumption to set an appropriate budget for energy. The main purpose of this study was to determine the ability of the k-nearest neighbors (KNN) algorithm to predict the fuel consumption of tractor–chisel plow systems correctly. A training-set design of 139 points of 173 data points obtained from the literature was utilized, and the remaining 34 data points were applied as a test set. The input parameters were tractor power, plowing width, depth and speed of plowing, soil...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Machine-learning algorithms; Tillage; Prediction; K-nearest neighbors; Fuel consumption; Chisel plow.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600729

Evaluation of tractive performance of four agricultural tractors in laterally inclined terrain
Provedor de dados: 70
Autores: Leite,Fabricio; Santos,João E. G. dos; Lanças,Kleber P.; Leite Júnior,João B.
The present work aimed to evaluate the tractive performance of four agricultural tractors with auxiliary front traction in function of six lateral inclinations in a lateral track of trials, which belongs to the Agronomic Sciences Faculty from the São Paulo State University, Campus of Botucatu. The lateral inclinations were 0; 5; 10; 15; 20 and 25 degrees. In all of these situations, the tractors operated with predetermined load of an imposed traction to the pulled tractor of 40 kN in the inclination of 0 degrees. Hence a delineation in random blocks was used, considering six inclinations and four tractors, and with three repetitions for each treatment. The analyzed variables were slippage, tractive force, hourly fuel consumption, and speed. It was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tractive force; Slippage; Lateral steepness.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500010

Evaluation of cotton stalks destroyers
Provedor de dados: 70
Autores: Bianchini,Aloisio; Borges,Pedro H. de M.
The destruction of the cotton crop residues (cotton stalks) is a mandatory procedure in Brazil for prophylactic issues, but is a subject unexplored by the research and there are few studies that deal with this issue. However, this is not encouraged in recent decades, studies aimed at developing and evaluating equipment for this purpose. The present study had the objective to evaluate six methods for mechanical destruction of cotton crop residues. Each method was defined based on the principle of operation of the active parts of the equipment, which were tested in medium texture soil and in a clayey one. The variables used to evaluate the efficiency of the equipment were the regrowth rate, the theoretical field capacity and energy demand. The equipment with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cotton stalk; Machine performance; Uprooting cotton stalks; Cotton stalk puller.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500008

METHODOLOGY EVALUATION OF PIN MICRORELIEF METER
Provedor de dados: 70
Autores: Melo,Mariana C.; Tavares,Laene F.; Oliveira,Thaísa F.; Silva,Rodrigo R.; Carvalho Filho,Alberto.
ABSTRACT: The effects of natural weathering and different managements performed in agriculture may best be understood by studying the soil roughness. The aim of this study was to evaluate the optimization of the use of pin microrelief meter, an instrument used to determine the soil surface roughness, as the number of readings collected over traditional methodology proposed in the bibliography. The study was conducted in Rio Paranaiba (MG), in a Haplustox soil. The experimental design was completely randomized in a 2×3 factorial design with four replications. There were combined two types of primary tillage: conventional tillage with disc plow (PCAD) and harrow (PCGA), and three amounts of readings (100, 200, and 300 reading points) sampled in each...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mobilization; Pin microrelief meter; Roughness; Soil tillage.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000501056

Physical properties of soils and soybean yields after planting cover crops
Provedor de dados: 70
Autores: SANTOS,DIEGO DOS; SOUZA,EDUARDO G. DE; NÓBREGA,LÚCIA H. P.; BAZZI,CLAUDIO L.; QUEIROZ,FERNANDO N. DE.
Cover crops are important for improving soil quality. However, soil properties usually have some spatial dependence. Thus, this study aimed to evaluate the effect of winter cover crops on physical properties of soil and soybean yields using thematic maps. Five winter treatments were used: black oats; intercropping 1 (forage turnips and black oats); intercropping 2 (forage turnips, black oats and common vetch); wheat; and control. Macroporosity, microporosity, total porosity, bulk density and water content of the soil from 0 - 0.1 m depths were evaluated after the winter cover crop management. Soybeans were sown over the entire area in the summer after the winter cover crop management, and the soybean yield was determined for each treatment. Maps for each...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil porosity; Bulk density; Crop rotation.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200280

Mecanismos de transferência de massa na desidratação osmótica de goiaba em soluções de sacarose, sucralose e açúcar invertido
Provedor de dados: 70
Autores: Queiroz,Valéria A. V.; Berbert,Pedro A.; Molina,Marília A. B.; Gravina,Geraldo A.; Queiroz,Luciano R.
O objetivo deste trabalho foi avaliar o efeito da concentração de soluções de sacarose, sucralose e açúcar invertido sobre a cinética da desidratação osmótica de pedaços de goiaba. Frações de 1/12 do fruto foram imersas em soluções de sacarose a 0,5 e 0,4 g mL-1; de sacarose a 0,3 g mL-1 + sucralose a 0,2 g L-1 e em xarope de açúcar invertido, a 50 ºC, por 2 h, sob agitação de 60 min. A solução de açúcar invertido promoveu maior perda de água e redução de massa nas amostras de goiaba submetidas à desidratação osmótica. O melhor desempenho foi obtido para o tratamento em solução de sacarose a 0,4 g mL-1; com perda de água e redução de massa semelhantes aos valores obtidos na imersão em solução de sacarose a 0,5 g mL-1 e ganho de sólidos similar ao observado...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Psidium guajava; Desidratação por imersão-impregnação.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400015

Tratamento de efluentes de sala de ordena de bovinocultura: lagoas de estabilização seguidas de leito cultivado
Provedor de dados: 70
Autores: Silva,Edu M. da; Roston,Denis M.
No Brasil, o destino dos efluentes dos confinamentos de animais foi e continua sendo os cursos de água, usando o ultrapassado método da diluição para eliminar os resíduos das instalações, o que pode resultar na eutrofização de rios, riachos, lagos e lagoas. As lavagens diárias da sala de ordenha, da Unidade Educativa de Produção (UEP) de Bovinocultura de Leite da Escola Agrotécnica Federal de Inconfidentes -MG (EAFI/MG), gerou 4,7 vezes mais efluentes poluentes do que a produção de leite, entre os meses de junho de 2006 e maio de 2007. Uma unidade-piloto composta por lagoa anaeróbia, lagoa facultativa e leito cultivado (“constructed wetland”) foi projetada para testar a eficiência no tratamento do resíduo líquido gerado pela sala de ordenha. Após o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bovinocultura leiteira; Tratamento de efluente.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100007

Analysis of land use and occupancy in permanent preservation areas according to the hydrography of Ribeirão Água Fria - Bofete, SP - Brazil
Provedor de dados: 70
Autores: Nardini,Rafael C.; Campos,Sérgio; Gomes,Luciano N.; Moreira,Katiuscia F.; Piza,Mariana W. de T.
The use conflicts are determined by the inadequate occupations of the soil, as it is the case of soil occupation inside of permanent preservation areas. This study aimed to determine the classes of the soil use and if there are conflicts inside of permanent preservation areas along the drainage network of the Água Fria Stream watershed, located in Bofete city - São Paulo, Brazil. It locates geographically between the coordinates: 48°09'30" to 48°18'30" longitude WGr., 22°58'30" to 23°04'30" latitude S, with an area of 15242.84 ha. The map of soil use was elaborated through the interpretation directly in the computer screen of satellite digital image. In the orbital data, the study area is inserted in the quadrant A, of image TM/Landsat - 5, orbit 220,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Watershed; Geographic information systems; Soil use.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500013

A multicriteria model to assess tractors used in family agriculture
Provedor de dados: 70
Autores: Reis,Ângelo V. dos; Machado,Antônio L. T.; Gomes,Mário C.; Andersson,Norberto L. M.; Machado,Roberto L. T.
In recent years, public policy has been offering subsidized credit for machine purchase to family farmers. However, there is no methodological procedure to select a suitable tractor for these farmers' situation. In this way, we aimed to develop a selection model for smallholder farmers from Pelotas city region in the state of Rio Grande do Sul. Building a multicriteria model to aid decisions is divided into three main stages: structuring stage (identifying stakeholders, decisional context and model creation), evaluation stage (stakeholder preference quantification) and recommendation stage (choice selection). The Multicriteria method is able to identify and value the criteria used in tractor selection by regional family farmers. Six main evaluation areas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Machine selection; Small farms; MCDA; PRONAF.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400012

Coeficiente de cultura da lima-ácida tahiti no outono-inverno determinado por lisimetria de pesagem em Piracicaba - SP
Provedor de dados: 70
Autores: Barboza Júnior,Cícero R. A.; Folegatti,Marcos V.; Rocha,Fábio J.; Atarassi,Roberto T.
O Brasil é o maior produtor mundial de citros, com destaque para o Estado de São Paulo, maior produtor nacional. Recentes estudos mostram que a área irrigada de citros em São Paulo tem aumentado significativamente nos últimos anos. Porém, a falta de informações sobre o manejo eficiente da irrigação na cultura de citros é uma das principais dificuldades enfrentadas pelos produtores. Com o intuito de atender a essa necessidade, este trabalho teve como objetivos determinar a evapotranspiração de uma planta adulta de limeira-ácida 'Tahiti' (Citrus latifolia Tan.) e o coeficiente de cultivo (Kc) no período seco (outono-inverno), utilizando a técnica de lisimetria de pesagem. O experimento foi realizado na ESALQ/USP em Piracicaba - SP, em área irrigada por...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação localizada; Evapotranspiração da cultura; Coeficiente de cultivo.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400009

Evapotranspiração e coeficientes de cultura do mamoeiro para a região litorânea do Ceará
Provedor de dados: 70
Autores: Montenegro,Afrânio A. T.; Bezerra,Francisco M. L.; Lima,Raimundo N. de.
O objetivo deste trabalho foi estimar a evapotranspiração da cultura do mamoeiro (Carica papaya L.), bem como seus coeficientes de cultura, sob irrigação, utilizando-se de uma linha de emissores para duas linhas de plantio, com um emissor para quatro plantas. Foi utilizada a variedade "Sunrise Solo", no espaçamento 2,5 m x 2,5 m x 3,5 m, em fileira dupla. A evapotranspiração da cultura foi estimada por meio do método do balanço hídrico, adotando-se um volume de controle de solo com profundidade de 0,6 m. A evapotranspiração de referência (ETo) foi medida em área adjacente, utilizando-se do lisímetro de pesagem e estimada pelo método de Penman-Monteith FAO. A taxa de evapotranspiração média da cultura para o período foi de 3,3 mm dia-1, sendo 2,2 mm dia-1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carica papaya L; Tensiômetro; Condutividade hidráulica.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200027

USE OF PROTECTION SCREEN IN CONVENTIONAL AVIARIES (CALIFORNIAN TYPE) FOR LAYING HENS
Provedor de dados: 70
Autores: Lourençoni,Dian; Yanagi Junior,Tadayuki; Oliveira,Daniela D. de; Lima,Renato R. de; Pena,Mariela R. da S.
ABSTRACT The objective of this work was to evaluate the thermal environment inside conventional cages for laying hens, with and without the use of protective screens. This research was conducted in two conventional cages (open cage), where each cage had half of its area surrounded by high density polyethylene mesh (HDPE) with a diameter of 2.0 cm, and the other half was kept fully open. Hyline W-36 and Dekalb Brown laying hens were housed in these cages. The wind speed, dry bulb temperature (tdb), black globe temperature, humidity index (BGHI), and enthalpy (H) were analyzed. The results indicate that the use of the screen reduced the wind speed inside the cage by 0.22 m s−1. The presence of the screen affected tdb, BGHI, and H in some of the evaluated...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry farming; Animal welfare; Ambience; Thermal comfort index.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100048

EFFECT OF THE DISTANCE BETWEEN THE CUTTING DISC AND FURROW OPENERS EMPLOYED IN ROW CROP PLANTING ON SOIL MOBILIZATION
Provedor de dados: 70
Autores: Francetto,Tiago R.; Alonço,Airton dos S.; Becker,Rafael S.; Scherer,Vitor P.; Bellé,Mateus P.
ABSTRACT The objective of this study was to determine the effect of the longitudinal distance between a cutting disc and a fertilizer furrow opener on the operational performance of the furrow opener working at different forward speeds during soil mobilization. The soil in the experimental area was classified as Typic Hapludalf with a loam soil texture. The experiment involved 24 treatment combinations in a 2 × 3 × 4 factorial scheme. These combinations were formed by the interaction of the following factors: furrow opening mechanisms, longitudinal distance from the center of the cutting mechanism to center of the furrow opener, and forward speeds. The effects of the tools on the soil mobilization variables were characterized in three phases: analysis of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural engineering; Machinery-soil relation; Agricultural machinery; Field test; Direct planting.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200148

Impacto da irrigação sobre os solos de perímetros irrigados na Bacia do Acaraú, Ceará, Brasil
Provedor de dados: 70
Autores: Lopes,José F. B.; Andrade,Eunice M. de; Chaves,Luiz C. G.
Para avaliar o risco de salinidade e de sodicidade do solo pelo manejo da irrigação, desenvolveu-se estudo comparativo entre os valores de CEes e RAS de área irrigada com os da mata nativa. A investigação ocorreu nos Distritos Irrigados Baixo Acaraú (DIBAU) e Araras Norte (DIPAN), localizados na Bacia do Acaraú. As amostras de solo foram coletadas bimestralmente, de maio/2003 a set./2005, nas camadas de 0-0,30 m; 0,30-0,60 m; 0,60-0,90 m e 0,90-1,20 m, sendo as análises efetuadas no Laboratório de Solo e Água da Embrapa Agroindústria Tropical. Para identificar se os incrementos dos parâmetros estudados eram estatisticamente significativos, aplicou-se o teste de Wilcoxon. Os incrementos de CEes foram maiores no DIPAN, com média de 250%, enquanto no DIBAU, a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Salinidade; Lixiviação; Adsorção de sódio.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100004

Impacto técnico e econômico das perdas de solo e nutrientes por erosão no cultivo da cana-de-açúcar
Provedor de dados: 70
Autores: Andrade,Nilo S. F. de; Martins Filho,Marcilio V.; Torres,José L. R.; Pereira,Gener T.; Marques Júnior,José.
O objetivo geral foi demonstrar o impacto técnico e econômico das perdas de solo e nutrientes por erosão no cultivo da cana-de-açúcar. Propôs-se avaliar as perdas de nutrientes por erosão (P, K, Ca e Mg), o custo de reposição de nutrientes e o de produção da cana em dois sistemas de colheita (cana crua e queimada) em Catanduva - SP, em área de 100 ha para cada sistema, formadas e colhidas no mesmo período (2002 a 2007), com similaridade quanto ao tipo de solo, variedade, topografia e numero de cortes. A metodologia baseou-se na equação universal da perda de solos e teoria dos custos de produção e de reposição de nutrientes. A maior perda de solo e de nutrientes por erosão ocorreu nas áreas de cana queimada; a cana queimada (corte manual), na média dos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas de colheita; Erosão do solo; Retorno técnico e econômico.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300014

GAUSSIAN SPATIAL LINEAR MODEL OF SOYBEAN YIELD USING BOOTSTRAP METHODS
Provedor de dados: 70
Autores: Dalposso,Gustavo H.; Uribe-Opazo,Miguel A.; Johann,Jerry A.; Galea,Manuel; Bastiani,Fernanda De.
ABSTRACT This study aims to quantify the uncertainties associated to the parameters of a Gaussian spatial linear model (GSLM) and the assumption of normality residuals in the modeling of the spatial dependence of the soybean yield as a function of soil chemical attributes. The spatial bootstrap methods were used to determine the point and interval estimators associated with the model parameters. Hypothesis tests were carried out on the significance of the model parameters and the quantile-quantile probability plot was elaborated to verify the data normality. The uncertainties associated to the parameters of the spatial dependence structure were quantified and the potassium content, phosphorus content and soil pH covariates were significant to explain the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geostatistics; Spatial resampling; Spatial variability.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100110

Uso de mesa vertical como parâmetro para regulagens de turboatomizadores
Provedor de dados: 70
Autores: Mion,Renildo L.; Sombra,Weberte A.; Duarte,José M. de L.; Nascimento,Elivânia M. S.; Viliotti,Carlos A.; Lucas,Fidel C. B.; Monte,Clesson A.
O consumo excessivo de agrotóxicos na agricultura brasileira é preocupante, e um dos fatores que contribuem para este excesso é o uso incorreto dos equipamentos de aplicação, causando grandes problemas de contaminação ambiental. O sucesso de uma aplicação agrícola somente é efetivado quando se consegue atingir o alvo com a menor contaminação ambiental possível. O objetivo deste trabalho foi comparar o perfil da distribuição vertical de um turboatomizador com e sem fluxo de ar e o número de bicos utilizados nos ramais, utilizando-se de uma mesa vertical como parâmetro de avaliação. O conjunto utilizado foi um trator marca VALTRA, modelo BM-120 4x2 TODA, e um turboatomizador da marca Jacto, modelo ARBUS 400 GOLDEN, com pontas do tipo J5-2, pressão de 1378...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mesa vertical; Acurácia; Tecnologia de aplicação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200015

Levantamento e identificação dos símbolos gráficos utilizados para a caracterização de controles e comandos em máquinas agrícolas
Provedor de dados: 70
Autores: Alonço,Airton dos S.; Balestra,Mônica R. G.; Dias,Vilnei de O.; Medeiros,Fabrício A.
Os símbolos gráficos utilizados para indicar a função dos comandos e controles das máquinas agrícolas tornam a operação mais segura. Logo, este trabalho teve por objetivo identificar a simbologia existente nas máquinas agrícolas disponíveis nas quatro principais concessionárias de Santa Maria - RS. No levantamento, foram utilizados como parâmetros os símbolos gráficos recomendados pelas normas técnicas, sendo os existentes nas máquinas estudadas fotografados e posteriormente anotados em planilha. O resultado encontrado foi, em média, de 86%, em relação à utilização dos símbolos gráficos recomendados pelas normas, porém existe também a utilização de símbolos gráficos criados pela própria empresa, o que pode gerar dúvidas no operador da máquina agrícola,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ergonomia; Normas; Símbolos gráficos.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200013

Validation study of an overall radiation balance estimation method under Ponta Grossa (PR) Brazil weather conditions
Provedor de dados: 70
Autores: Beruski,Gustavo C.; Pereira,André B.
Radiation balance is the fraction of incident solar radiation upon earth surface which is available to be used in several natural processes, such as biological metabolism, water loss by vegetated surfaces, variation of temperature in farming systems and organic decomposition. The present study aimed to assess and validate the performance of two estimation models for Rn in Ponta Grossa city, Paraná State, Brazil. To this end, during the period of 04/01/2008 to 04/30/2011, from radiometric data collected by an automatic weather station set at the Experimental Station, of the State University of Ponta Grossa. We performed a linear regression study by confrontation between measurements made through radiometric balance and Rn estimates obtained from Brunt...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Overall radiation balance; Bowen ratio; Global solar radiation; Modeling; Solar radiometry.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300010

Desempenho operacional de semeadura-adubadora em diferentes manejos da cobertura e da velocidade
Provedor de dados: 70
Autores: Furlani,Carlos E. A.; Pavan Júnior,Álvaro; Lopes,Afonso; Silva,Rouverson P.; Grotta,Danilo C.C.; Cortez,Jorge W.
O presente trabalho teve como objetivo avaliar o desempenho de uma semeadora-adubadora no sistema plantio direto. Os fatores estudados foram três manejos das culturas de cobertura, selecionados em função do tamanho de fragmentos da vegetação, triturador de palhas (palha totalmente triturada), roçadora (palha parcialmente picada) e rolo-facas (palha acamada), combinados com três velocidades do conjunto trator-semeadora-adubadora, sendo 4,0; 5,0 e 6,0 km h-1. O delineamento experimental foi em blocos casualizados, em esquema fatorial 3 x 3, com nove tratamentos e oito repetições, totalizando 72 observações. Para comparar os tratamentos, avaliaram-se a capacidade de campo operacional, a força de tração e a potência na barra, o consumo horário e por área, e a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Força de tração; Consumo de combustível; Plantio direto.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300014

Simulation of the energy performance of maize production integrated to pig farming
Provedor de dados: 70
Autores: Perin,Márcio L.; Martins,Gilberto; Bueno,Osmar de C.
The study evaluated the energy performance of pig farming integrated with maize production in mechanized no-tillage system. In this proposed conception of integration, the swine excrement is used as fertilizers in the maize crop. The system was designed involving the activities associated to the pig management and maize production (soil management, cultivation and harvest). A one-year period of analysis was considered, enabling the production of three batches of pigs and two crops of maize. To evaluate the energy performance, three indicators were created: energy efficiency, use of non-renewable resources efficiency and cost of non-renewable energy to produce protein. The energy inputs are composed by the inputs and infrastructure used by the breeding of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pig farming; Integrated agroecosystems; Energy analysis.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500004

Comparison of maps of spatial variability of soil resistance to penetration constructed with and without covariables using a spatial linear model
Provedor de dados: 70
Autores: Bastiani,Fernanda de; Uribe-Opazo,Miguel A.; Dalposso,Gustavo H.
A study about the spatial variability of data of soil resistance to penetration (RSP) was conducted at layers 0.0-0.1 m, 0.1-0.2 m and 0.2-0.3 m depth, using the statistical methods in univariate forms, i.e., using traditional geostatistics, forming thematic maps by ordinary kriging for each layer of the study. It was analyzed the RSP in layer 0.2-0.3 m depth through a spatial linear model (SLM), which considered the layers 0.0-0.1 m and 0.1-0.2 m in depth as covariable, obtaining an estimation model and a thematic map by universal kriging. The thematic maps of the RSP at layer 0.2-0.3 m depth, constructed by both methods, were compared using measures of accuracy obtained from the construction of the matrix of errors and confusion matrix. There are...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geostatistics; Maximum likelihood; Error matrix.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200019

PRODUCTIVITY AND NUTRITIVE VALUE OF TIFTON 85 IN SUMMER, WITH AND WITHOUT IRRIGATION UNDER DIFFERENT NITROGEN DOSES
Provedor de dados: 70
Autores: Sanches,Arthur C.; Gomes,Eder P.; Rickli,Max E.; Friske,Elcio; Fasolin,Julia P.
ABSTRACT The pasture irrigation has expanded, mostly in small areas in order to boost the production system, along with the use of soil improvement techniques and high-productivity grasses. Thus, this study, carried out on a small dairy farm property, aimed to evaluate the productivity, botanical composition and nutritive value of Tifton 85 with different nitrogen (N) doses, in the presence and absence of irrigation. The experimental design was a randomized block in a split-plot design with four replications, plots Non-irrigated and Irrigated. The subplots consisted of nitrogen doses: 25 kg ha−1 cycle−1 of N, 50 kg ha−1 cycle−1 of N, 75 kg ha−1 cycle−1 of N and 100 kg ha−1 cycle−1 of N. The irrigation increased the productivity in an average of 3,626.5 kg...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Neutral detergent fiber; Acid detergent fiber; Tensiometry; Cynodon ssp.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200246

OUTDOOR CULTIVATION OF Scenedesmus obliquus BR003 IN STIRRED TANKS BY AIRLIFT
Provedor de dados: 70
Autores: Pereira,Emanuele G.; Martins,Marcio A.; Mendes,Mariana dos S. A.; Mendes,Leonardo B. B.; Nesi,Adriano Nunes.
ABSTRACT: The use of microalgae as a source of raw material for biofuel production has been highly targeted. Compared to other biological options for the capture and use of CO2, microalgae crops have the following advantages: high productivity, lack of competition with feed and food-based products, use of unproductive and non-arable land, and allowance of the use of wastewater for its cultivation. The use of wastewater from industrial, agricultural, and domestic sewage has been indicated as an alternative means to reduce the cost of crops, since such waste is generally released into the environment without previous treatment. This work addresses the use of petrochemical wastewater (ARP) from effluent produced at the Gabriel Passos Refinery (Petrobrás...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wastewater treatment; Microalgae; Biofuel.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000501041

MORPHOGENIC AND STRUCTURAL CHARACTERISTICS OF MARANDU GRASS AFFECTED BY FERTIGATION WITH TREATED SEWAGE EFFLUENT AND CUTTING HEIGHT
Provedor de dados: 70
Autores: Dantas,Geffson de F.; Faria,Rogério T. de; Costa,Natã R.; Santos,Gilmar O.; Ferraudo,Antonio S.
ABSTRACT The response of biomass flow components of forage from the interaction between fertigation with wastewater and cutting height during the year is little known. The objective of this work was to verify the responses of morphogenic and structural characteristics of Urochloa brizantha as a function of fertigation application strategies with sewage treatment plant effluent (TSE), complemented with urea (U), associated with harvest with two plant heights during the dry and rainy periods. The forage cutting heights were 30 cm (H1) and 40 cm (H2), and nitrogen fertilization doses were 9.1 (D1), 12.1 (D2), 22.5 (D3), 26.6 (D4), and 34.0 (D5) kg of N per Mg−1 of dry matter (DM) produced, applied by TSE via fertigation, plus 7.5 kg N per Mg−1 of DM produced,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Defoliation; Nitrogen; Water reuse.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600692

IDENTIFICATION OF SUITABLE AREAS FOR IRRIGATED RICE CROPPING USING MODIS IMAGES AND HAND MODEL
Provedor de dados: 70
Autores: MENGUE,VAGNER P.; FONTANA,DENISE C.
ABSTRACT One of the most relevant activities of Brazilian economy is agriculture. Among the main crops in Brazil, rice is one of high relevance. The state of Rio Grande do Sul, in Southern Brazil, is responsible for 68.7% of domestic production (IBGE, 2013). The goal of this study was to develop a low-cost methodology with a regional scope to identify suitable areas for irrigated rice cropping in this state, using spectro-temporal behavior of vegetation index by means of MODIS images and HAND model. The rice-cropped area of this study was the southern half of the State. Using the HAND model, flood areas were mapped to identify irrigated rice cultivation. We used multi-temporal images of vegetation index from MODIS sensor, covering the period from August...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: HAND Model; EVI; MODIS; Irrigated rice; Mapping.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200329

CROP COEFFICIENT REGIONALIZATION FOR IRRIGATED AGRICULTURE PLANNING IN MARANHÃO STATE -BRAZIL
Provedor de dados: 70
Autores: Silva,Wilson A. Da; Santana,Jhonata S.; Silva,Cristiane M. Da; Nunes,Acassio A.
ABSTRACT: Irrigated agriculture has emerged as a necessary technology to achieve greater productivity, mainly by supplying the water requirements of agricultural crops in critical periods, especially for those regions where natural rainfall is insufficient to meet these requirements. The daily water consumption of crops is strongly influenced by local weather conditions, which justifies the need for regionalized studies of the parameters influencing the water depth to be applied. The crop coefficient (Kc) is perhaps the most important parameter because it interferes directly with the crop water requirements. This index must be determined for each region, thus avoiding the use of reference values meant for other climatic conditions, causing loss of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water requirements; Irrigation; Zea mays L.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500953

‘Sweet grape’ tomato post harvest packaging
Provedor de dados: 70
Autores: Sandri,Delvio; Rinaldi,Maria M.; Ishizawa,Taís A.; Cunha,Ananda H. N.; Pacco,Honorato C.; Ferreira,Rafael B.
ABSTRACT This paper aims at evaluating the shelf life of mini tomatoes (Lycopersicum esculentum Mill.) cultivar ‘Sweet Grape’, grown in hydroponics, and stored under environmental and refrigerated conditions inside different packages. We adopted a completely randomized design, in which treatments were combinations of storage conditions: environment (e) and refrigerated (r) with packaging: polyvinyl chloride film (PVC); low-density polyethylene (LDPE); biofilm of tomato fruit of Solanum lycocarpum A.St.-Hil (lobeira) (TFB); cassava starch biofilm (CSB); carnauba wax (Copernicia prunifera) (CW), and without packaging - control (C). Physicochemical and sensory tests were carried out at the beginning (day zero), and at 8, 19, and 33 days of storage (DS). Fruit...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lycopersicon esculentum Mill; Storage; Shelf life; Lifespan; Expiration; Expiry date.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601093

FUZZY MODELING OF THE EFFECTS OF IRRIGATION AND WATER SALINITY IN HARVEST POINT OF TOMATO CROP. PART I: DESCRIPTION OF THE METHOD
Provedor de dados: 70
Autores: Viais Neto,Daniel dos S.; Cremasco,Camila P.; Bordin,Deyver; Putti,Fernando F.; Silva Junior,Josué F.; Gabriel Filho,Luís R. A.
ABSTRACT It was used statistical techniques for the evaluation of agricultural experiments, but there are mathematical theories that allow finer adjustments, highlighting among them, the fuzzy logic. The objective of the study was characterizing a method of fuzzy modeling from an agronomic experiment. For this study it was used data from an experiment conducted at the School of Agriculture of São Paulo State University (UNESP) in Botucatu-SP. The system input variables based in fuzzy rules were soil water tension and doses of water salinity, being defined three fuzzy sets. The output variables was elected from the biometric and productivity analysis that showed statistically significant differences, namely, plant height, stem diameter, leaf area, green...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuzzy logic; Drought; Salt stress; Crop management.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300294

Colheita de cana-de-açúcar com auxílio mecânico
Provedor de dados: 70
Autores: Braunbeck,Oscar A.; Oliveira,Julieta T. A.
As demandas legais da sociedade civil e dos produtores de cana-de-açúcar em áreas inclinadas colocam em evidência deficiências tecnológicas dos processos de colheita que ameaçam a produção de cana-de-açúcar em extensas regiões canavieiras. O estudo analisa o sistema de colheita mecânica atual, comparativamente a uma proposta de colheita semimecanizada, com base em 11 características consideradas determinantes para a disseminação rápida da colheita da cana sem queima prévia, em áreas declivosas, com menor impacto sobre a demanda de mão-de-obra agrícola e sobre a capacidade de investimento dos produtores.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Investimento; Declividade; Emprego agrícola.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100032

Efeitos do Organosuper® e do ambiente protegido na formação de mudas de mamoeiro
Provedor de dados: 70
Autores: Costa,Edilson; Leal,Paulo A. M; Mesquita,Viviane do A. G; Sassaqui,Adriano R.
Com o objetivo de avaliar doses de composto orgânico e ambiente protegido na formação de mudas de mamoeiro, foi conduzido um experimento no período de setembro a dezembro de 2007. Utilizaram-se seis ambientes protegidos: estufa plástica com pé-direito de 2,5 m; viveiro telado com Sombrite® 50%, com pé-direito de 2,5m; viveiro telado de tela termorrefletora Aluminet® 50%, com pé-direito de 2,5m; viveiro coberto com palha de coqueiro, com pé-direito de 1,8 m; estufa plástica com pé-direito de 4,0 m, possuindo abertura zenital e tela termorrefletora 50% sob o plástico e viveiro telado de tela de sombreamento 50%, com pé-direito de 3,5 m. Foram utilizados cinco substratos com doses de 0; 7; 14; 21 e 28% de composto orgânico Organosuper® (oriundos de resíduos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carica papaya; Fruticultura; Estufas; Substratos.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100005

Nitrogen fertilization by deep-bedding swine production and its effects on the properties of a Quartzarenic Neosol
Provedor de dados: 70
Autores: Campos,Alessandro T.; Veloso,Alessandro V.; Silva,Enilson de B; Yanagi Junior,Tadayuki; Klosowski,Elcio S.
The objective of this study was to evaluate the effects of the nitrogen fertilization in the form of swine deep bed in the properties of a quartz-sand neosol. The organic compound used was the deep bed made with rice hulls, from a commercial swine finishing system farm. Deep bed samples have been collected at various points in the installation in order to obtain a representative composite sample which has been fractionated in a 2.0 mm sieve and submitted to a 50-day maturation period. Then, agronomic value analyses were done. The experimental design was completely randomized. The treatments consisted of 0; 75; 150 and 300 mg dm-3 of N doses of deep bed as well as an additional treatment with ammonium sulfate at a 150 mg dm-3 of N. The experimental period...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Swine production; Swine buildings; Alternative management; Waste treatment; Organic fertilizer; Quartz-sand neosol.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400015

Rendimento de motor elétrico como parâmetro de dimensionamento de bitola de alimentador conectado diretamente ao transformador
Provedor de dados: 70
Autores: Oliveira Filho,Delly; Teixeira,Carlos A.; Lacerda Filho,Adílio F.; Martins,José H.; Queiroz,Josué M.
O dimensionamento de condutores de energia elétrica não leva em consideração critérios de racionalização do uso de energia elétrica. O estudo abrangeu uma avaliação sobre o dimensionamento de condutores alimentadores de energia elétrica de motores conectados diretamente a transformadores utilizados na eletrificação rural. No dimensionamento dos condutores alimentadores, indica-se que, além do atendimento à norma técnica (dimensionamento em função da capacidade de corrente do condutor e da queda de tensão admissível), também sejam considerados: (i) o número de horas de funcionamento; (ii) as características elétricas e preço de condutores; (iii) as características da instalação, como comprimento do ramal e potência do motor. Provou-se que, em algumas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Motor elétrico; Qualidade da energia; Dimensionamento de condutores.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500005

Performance impact of the application of castor oil biodiesel in diesel engines
Provedor de dados: 70
Autores: Monteiro,Leonardo de A.; Pianovski Júnior,Guilherme; Velásquez,José Antonio; Rocha,Danilo S.; Bueno,André V.
The use of renewable fuels, such as the biodiesel, can ease the demand of fossil fuel for the power generation and transportation fields in rural area. In this work, the performance impact of the application of castor oil biodiesel is evaluated with an automotive and a stationary diesel engine. The application of B20 and B10 biodiesel blends and pre-heated net biodiesel is considered. The viability of the employment of B10 and B20 blends to mobility and power generation was observed from dynamometric bench tests, where this blends performed similar to fossil diesel. With the pre-heated net biodiesel, however, a brake torque loss and a specific consumption increase were observed with relation to diesel fuel.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biodiesel; Castor Oil; Diesel Engine; Dynamometric Bench Tests.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600009

Calibração de extratores providos de cápsula porosa para monitoramento da salinidade e da concentração de íons
Provedor de dados: 70
Autores: Oliveira,Francisco de A. de; Medeiros,José F. de; Duarte,Sergio N.; Silva Júnior,Manoel J. da; Campelo,Charlles M.
Os resultados satisfatórios obtidos no monitoramento da salinidade e concentração de íons na solução do solo, usando extratores de cápsulas porosas, motivaram a realização deste trabalho, o qual teve como objetivo a obtenção de curvas de calibração para estes extratores monitorarem a condutividade elétrica e a concentração de nitrato e de potássio na solução de dois tipos de solo (Latossolo Vermelho-Amarelo Argissólico franco arenoso, e o outro como Cambissolo Eutrófico), em Mossoró - RN. As concentrações de nitrato utilizadas foram as mesmas nos dois solos (0; 84; 168; 252; 336; 420 e 504 mg L-1); quanto ao potássio, foram utilizadas concentrações diferentes no solo arenoso (0; 117; 234; 351; 468; 585 e 702 mg L-1) e no argiloso (0; 117; 234; 351; 468;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solução do solo; Condutividade elétrica; Potássio; Nitrogênio.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300012

Efeito de subdoses de 2,4-D na produtividade de uva itália e suscetibilidade da cultura em função de seu estádio de desenvolvimento
Provedor de dados: 70
Autores: Oliveira Júnior,Rubens S. de; Constantin,Jamil; Brandão Filho,José U. T.; Callegari,Osni; Pagliari,Paulo H.; Cavalieri,Sidnei D.; Framesqui,Vagner P.; Carreira,Sílvio A. M.; Roso,Ana C.
Durante os anos agrícolas de 2002-2003 e 2003-2004 foram conduzidos trabalhos no município de Maringá - PR, com o objetivo de avaliar o dano potencial de subdoses de 2,4-D sobre plantas de uva, imitando depósitos decorrentes de deriva. No primeiro experimento, a aplicação foi realizada cerca de 30 dias após a poda de inverno, num pomar de uva Itália. As doses utilizadas foram de 6,72; 13,44; 26,88; 53,76 e 107,52 g de equivalente ácido (e.a.) por hectare de 2,4-D, equivalentes a depósitos de 1,0%; 2,0%; 4,0%; 8,0% e 16,0%, assumindo-se uma aplicação de 1 L ha-1 (670 g e.a. ha-1). Nessa data, as plantas encontravam-se na fase de emissão de cachos e florescimento (estádio 15). O surgimento de sintomas visuais de fitointoxicação foi imediato e proporcional às...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vitis vinifera; Herbicidas fenóxicos; Subdoses.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200006

Comportamento espacial da demanda energética em semeadura de amendoim em latossolo sob preparo convencional
Provedor de dados: 70
Autores: Toledo,Anderson de; Furlani,Carlos E. A.; Silva,Rouverson P. da; Lopes,Afonso; Dabdoub,Miguel J.
A mecanização desempenha papel fundamental na produção agrícola e, consequentemente, na composição dos custos. Os adequados planejamento e gerenciamento dos sistemas mecanizados contribuem para a racionalização e redução dos gastos e melhoria do produto final. O objetivo deste trabalho foi estudar e caracterizar a variabilidade espacial da resistência mecânica do solo à penetração, da demanda energética e do desempenho operacional do conjunto trator-semeadora-adubadora em semeadura de amendoim, atuando com 5% de biodiesel etílico destilado de amendoim, em solo sob preparo convencional. As variáveis avaliadas neste estudo foram: força e potência requeridas na barra de tração, capacidade de campo efetiva, consumo de combustível, consumo de energia,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Consumo de combustível; Geoestatística; Desempenho operacional; Penetrógrafo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300010

DESIGN OF ELECTRONIC CONTROL GOVERNOR FOR A SINGLE CYLINDER GASOLINE ENGINE BASED ON AN INTELLIGENT SENSING ALGORITHM
Provedor de dados: 70
Autores: Sun,Lixiang; Yang,Yan; Ma,Fang; Jing,Wen; Zheng,Yibo; Wu,Hao.
ABSTRACT At present, most large machinery and vehicle engines are electronically controlled but their electronic control systems are too expensive to be popularised and applied in small gasoline engines with relatively low prices. Therefore, small gasoline engines still use mechanical speed regulators. Mechanical speed regulators not only have the defects of inertia lag, friction resistance, inherent speed regulation and the like, but also have the disadvantage that dynamic performance and steady performance cannot be combined, which is not suitable for the increasingly improved speed regulation performance of gasoline engines. This paper describes the design of an electronically controlled intelligent governor for small gasoline engines. Starting from a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Electronic control; Intelligent perception; Dynamic and steady state performance; Power; Hunting.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400495

Avaliação do efeito do estresse hídrico no crescimento de cultivares de cana-de-açúcar usando um sistema automático de fertirrigação
Provedor de dados: 70
Autores: BATISTA,EVANDRO L. DA S.; ZOLNIER,SÉRGIO; RIBEIRO,ARISTIDES; LYRA,GUSTAVO B.; SILVA,THIERES G. F.; BOEHRINGER,DAVI.
O objetivo desta pesquisa foi identificar o efeito de diferentes níveis de estresse hídrico no crescimento das cultivares RB92579, RB855453, RB867515 e RB928064, utilizando um sistema automático de controle dos eventos de fertirrigação, durante o período de formação da cana-de- -açúcar. No período experimental, as plantas foram submetidas a períodos alternados de estresse e de reposição hídrica, por meio de fertirrigações periódicas, cujos limites do potencial matricial de água (Y) foram aqui denominados, para propósitos comparativos, como ausência de estresse, estresse leve, moderado e severo, respectivamente, para os valores críticos de Y de −10, −60, −90 e −120 kPa. Para avaliação do efeito do estresse hídrico no crescimento da cana-de-açúcar, foi...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelos de crescimento; Saccharum officinarum; Disponibilidade hídrica; Irrigação.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200215

Desenvolvimento e validação de um modelo matemático para o cálculo da área superficial de frangos de corte
Provedor de dados: 70
Autores: Silva,Eberson; Yanagi Júnior,Tadayuki; Braga Júnior,Roberto A.; Lopes,Marcos A.; Damasceno,Flávio A.; Silva,Gleice C. A. E.
A área superficial de frangos de corte é importante parâmetro de entrada em modelos de transferência de calor e massa. Dessa forma, o presente trabalho teve o objetivo de desenvolver e validar modelo matemático empírico para estimar a área superficial (As) de frangos de corte. Para a realização desta pesquisa, foram utilizadas 84 aves de corte da linhagem Ross, sendo 37 machos e 47 fêmeas, com animais abrangendo todo o período da fase de criação. Em cada teste realizado em laboratório, uma ave, aleatoriamente selecionada, teve as suas dimensões (comprimento, largura e altura) e massa corporal avaliadas. A pele com penas da ave foi retirada para a determinação da As. Parte dos dados foi usada para ajuste da equação para a determinação da As e parte para a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Frangos de corte; Área superficial; Modelo empírico; Análise de imagens.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100001

Uso de tela termorrefletora em ambientes protegidos para cultivo do tomateiro
Provedor de dados: 70
Autores: FERRARI,DIEGO L.; LEAL,PAULO A. M.
O emprego de telas termorrefletoras, como forma de limitar o aumento da temperatura do ar em ambientes protegidos, deve ser manejado, a fim de evitar a redução excessiva da radiação solar, dada sua importância sobre o desenvolvimento e a produção de hortaliças como o tomateiro. Nesse contexto, os objetivos do trabalho foram comparar os microclimas entre ambientes protegidos cultivados com tomateiro, sendo um coberto somente com polietileno de baixa densidade (PEBD) reforçado e outro coberto com PEBD reforçado associado a uma tela termorrefletora aluminizada retrátil, sob condições de manejo, e avaliar sua adequação às condições climáticas recomendadas à cultura do tomateiro pela bibliografia consultada. O experimento foi conduzido no município de Rio das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tela termorrefletora; Manejo; Tomateiro.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200180

SPATIAL VARIABILITY OF THE MICROCLIMATE IN DIFFERENT SMALL RUMINANT HOUSE LOCATED IN THE SEMIARID OF PERNAMBUCO, BRAZIL
Provedor de dados: 70
Autores: Gonçalves,Indira C. M.; Turco,Sílvia H. N.; Leitão,Mário de M. Vilas Boas R.; Oliveira,Leane N.; Amorim,Danielle M.
ABSTRACT The spatial variability in meteorological conditions was evaluated in two small ruminant house with different constructive aspects, based on the variables of dry bulb temperature, relative humidity, wind speed and temperature humidity index (THI), through the generation of maps using the Kriging interpolation method. The experiment was conducted in two seasons, winter and summer, and the small ruminant house were denominated as: FNRG (facility at ground level with no ridge vent) and FWRG (facility at ground level and with ridge vent). The studied parameters were recorded by portable digital sensors, thermo-anemometers and thermo-hygrometers, with data collections at 9 am and 3 pm. With the analysis of the spatial variability of the data, it was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environment; Animal production; Welfare.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300300

TOPOGRAPHIC ASPECTS IN THE SPATIAL AND TEMPORAL DYNAMIC OF NET RADIATION
Provedor de dados: 70
Autores: Filgueiras,Roberto; Nicolete,Donizeti A. P.; Carvalho,Tânia M. de; Cunha,Antonio R. da; Zimback,Célia R. L.
ABSTRACT: The measurements obtained by remote sensing are influenced by issues related to relief. Based on that, this paper aims to analyze the spatial and temporal dynamics of the net radiation (Rn), considering the influence of topographic parameters on it, in Edgárdia Experimental Farm (FEE). It was used the methodology based on the SEBAL algorithm (Surface Energy Balance Algorithm for Land) to estimate the net radiation by orbital images. In order to assess the topographic influence on the computing of net radiation, three methodologies were applied: without topographic correction (RnSem), cosine correction (RnCos) and C correction (RnC). These methodologies were applied on 21 images of the orbital platform Landsat-5/TM, from 1985 up to 2010. Due to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Topographic correction; SEBAL; Biophysical parameters.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000501028

Marketing in the pre-development process of agricultural machines: a reference model
Provedor de dados: 70
Autores: Oliveira,Alexandre S. de; Dallmeyer,Arno U.; Romano,Leonardo N.
The theme of the research is the development of the domain of marketing knowledge in the design of agricultural machinery. It is developed throughout the design of agricultural machinery in order to identify the corporate and customers needs and to develop strategies to satisfy these needs. The central problem of the research questions which marketing tools to apply on pre-development process of farm machinery, in order to increase the market value of the products and of the company and, consequently, generate competitive advantage to the manufacturers of agricultural machinery. As methodology, it was developed bibliographical research and multicase study of the development process of agricultural machinery developed by small, medium and large companies...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Product design; Agricultural mechanization; Marketing techniques.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400014

Cultura da soja em função da profundidade de semeadura e da carga vertical sobre a fileira de semeadura
Provedor de dados: 70
Autores: Grotta,Danilo C. C.; Furlani,Carlos E. A.; Silva,Rouverson P.; Santos,Leonardo dos; Cortez,Jorge W.; Reis,Gustavo N. dos.
A análise do efeito da profundidade de semeadura e carga vertical visando a melhorar o aproveitamento, e a integração entre o solo e a cultura é muito difícil. O objetivo do presente trabalho foi avaliar cargas verticais (0; 98; 196 e 294 N) sobre as rodas compactadoras das semeadoras, combinando com profundidades de semeadura (0,03; 0,05 e 0,07 m) para a cultura da soja. O trabalho foi realizado no DER/UNESP - Jaboticabal, na pista de ensaio do Laboratório de Máquinas e Mecanização Agrícola (LAMMA), utilizando o delineamento experimental em blocos casualizados, no esquema fatorial (4 x 3), com 12 tratamentos e três repetições, totalizando 36 observações. Foram analisados: emergência de plântulas, estandes inicial e final, índice de sobrevivência, área...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Estande de plantas; Área mobilizada; Rendimento de grãos.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300018

Eficiência de utilização de água e nutrientes em plantas de feijão-de-corda irrigadas com água salina em diferentes estádios de desenvolvimento
Provedor de dados: 70
Autores: Lacerda,Claudivan F. de; Neves,Antonia L. R.; Guimarães,Francisco V. A.; Silva,Francisco L. B. da; Prisco,José T.; Gheyi,Hans R.
O objetivo deste trabalho foi investigar os efeitos do uso de água salina em diferentes estádios de desenvolvimento de plantas de feijão-de-corda sobre a eficiência de utilização de água e de nutrientes. O experimento foi conduzido no campo e obedeceu ao delineamento em blocos ao acaso, com cinco tratamentos e cinco repetições. Os tratamentos empregados foram: T1 - água de poço com condutividade elétrica (CEa) de 0,8 dS m-1 durante todo o ciclo; T2 - água salina (CEa de 5,0 dS m-1) durante todo o ciclo; T3, T4 e T5 - água salina de 0 a 22 dias após o plantio (DAP), de 23 a 42 DAP e de 43 a 62 DAP, respectivamente. As plantas dos tratamentos T3, T4 e T5 foram irrigadas com água de poço nas demais fases do ciclo. Aos 8; 23; 43 e 63 DAP, as plantas foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vigna unguiculata; Salinidade; Eficiência no uso de água; Eficiência de utilização de nutrientes.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200005

Importância relativa dos íons na salinidade de um cambissolo na Chapada do Apodi, Ceará
Provedor de dados: 70
Autores: D'Almeida,Deborah M. B. A.; Andrade,Eunice M.; Meireles,Ana C. M.; Ness,Ricardo L. L.
Este trabalho foi realizado com o objetivo de desenvolver e validar modelos em que a ordem de influência dos íons nos valores da condutividade elétrica do extrato de saturação do solo (CEes) fosse identificada. As coletas foram realizadas em duas áreas com bananeiras cultivadas sob irrigação (água subterrânea e superficial) e em áreas de vegetação nativa localizadas na Chapada do Apodi, Ceará, sendo uma em Quixeré e a outra no Distrito de Irrigação Jaguaribe Apodi (DIJA), em Limoeiro do Norte. A pesquisa ocorreu no período de dezembro de 1999 a dezembro de 2000 e setembro a dezembro de 2001. Foram retiradas 312 amostras de solo e, por meio das análises do extrato de saturação do solo, foram determinados as CEes e os íons Na+, Cl-, Ca2++Mg2+ e K+....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Salinidade no solo; Modelos estatísticos.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300006

PRAPRAG: software para planejamento racional de máquinas agrícolas
Provedor de dados: 70
Autores: Mercante,Erivelto; Souza,Eduardo G. de; Johann,Jerry A; Gabriel Filho,Antonio; Uribe-Opazo,Miguel A.
O software PRAPRAG é uma ferramenta de escolha de máquinas e implementos agrícolas que apresentam o menor custo por área ou por quantidade produzida, bem como, faz o planejamento de aquisição das máquinas para a propriedade agrícola, do ponto de vista técnico e econômico. Foi utilizada a linguagem de programação Borland Delphi 3.0 e, a partir de prospectos das máquinas e implementos, criou-se um banco de dados onde o usuário pode cadastrar e modificar suas características de uso. O software mostrou-se uma ferramenta útil e uso amigável. O software proporciona maior rapidez, segurança e confiabilidade ao processo produtivo e econômico das propriedades, na seleção e aquisição de conjuntos mecanizados agrícolas, e na determinação de custos com a mão de obra...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Custos e seleção; Desempenho; Sistema computacional.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200015

DRYING KINETICS OF BARU FRUITS (Dipteryx alata Vogel)
Provedor de dados: 70
Autores: Resende,Osvaldo; Oliveira,Daniel E. C. de; Costa,Lílian M.; Ferreira Júnior,Weder N.
ABSTRACT This study aimed to fit different mathematical models to the experimental data on drying of baru fruits (Dipteryx alata Vogel), determine and assess the effective diffusion coefficient, as well as obtain the activation energy and thermodynamic properties for the drying process under different air temperature conditions. Baru fruits with an initial moisture content of 0.429 ± 0.044 (dry basis, db) were dried in a forced air ventilation oven under four temperature conditions (40, 60, 80, and 100 °C) until reaching a moisture content of 0.065 ± 0.018 (decimal db). These data were fitted to mathematical models frequently used to represent the drying of vegetal products. The Logarithmic model presented the best fit to describe the phenomenon. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mathematical modeling; Liquid diffusivity; Logarithmic.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100103

Transferência de massa e secagem em leitos vibrofluidizados: uma revisão
Provedor de dados: 70
Autores: Park,Kil J.; Brod,Fernando P. R.; Oliveira,Rafael A. de.
O desenvolvimento de tecnologias de processamento e equipamentos requer a utilização de novos métodos e melhor qualidade do produto processado. Dentro do processo de secagem contínua, a utilização de equipamentos que promovem incremento nos coeficientes de transferência, é a de maior interesse. O uso de energia vibracional tem sido recomendado para materiais dispersos. Assim, uma revisão da literatura sobre a transferência de massa e a secagem em leitos vibrofluidizados foi realizada, envolvendo resultados experimentais e modelagem matemática.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Taxa de secagem; Parâmetro vibracional; Transferência de massa.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300022

TEMPORAL VARIABILITY IN ACTIVE REFLECTANCE SENSOR-MEASURED NDVI IN SOYBEAN AND WHEAT CROPS
Provedor de dados: 70
Autores: Beneduzzi,Humberto M.; Souza,Eduardo G.; Bazzi,Claudio L.; Schenatto,Kelyn.
ABSTRACT: Optimization of N management is one of the great challenges to be overcome in grain production, as it is directly related to productivity and can also cause environmental damage. Precision agriculture aims to solve this problem by applying nitrogen fertilizer at varying rates. Reflectance sensors are instruments capable of estimating N needs in various crops, including grain crops. However, it is not clear how these sensors perform under varying solar radiation and cloud cover, due to a lack of research on their temporal variability. Thus, this study examined the temporal variability of the NDVI (normalized difference vegetation index), as measured by an active reflectance sensor, in both soybean and wheat crops. The NDVI data were collected...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Remote sensing; Vegetation index; NDVI.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400771

Caracterização do perfil de deposição e do diâmetro de gotas e otimização do espaçamento entre bicos na barra de pulverização
Provedor de dados: 70
Autores: Fernandes,Ana P.; Parreira,Renata S.; Ferreira,Marcelo C.; Romani,Gustavo N.
A escolha e o uso adequado de pontas de pulverização são essenciais para a correta aplicação de produtos fitossanitários, sendo, portanto, indispensável o conhecimento de suas características. Este trabalho teve o objetivo de caracterizar o perfil de distribuição e o diâmetro de gotas, oferecendo dados para otimizar o espaçamento entre bicos na barra de pulverização. Foram avaliados os perfis de distribuição da ponta de jato plano Teejet XR 110015 VS, a 0,50 m da altura da mesa de deposição, nas pressões de 200 e 300 kPa, e o diâmetro das gotas pelo método de difração de raios laser. As distâncias máximas foram de 0,85 m, calculadas para um coeficiente de variação (C.V.) aceitável para as pressões de 200 e 300 kPa , com os respectivos valores de 9,52 e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ponta de jato plano; Pressão de trabalho; Tecnologia de pulverização.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400016

ARTIFICIAL NEURAL NETWORK-BASED METHOD TO IDENTIFY FIVE VARIETIES OF EGYPTIAN FABA BEAN ACCORDING TO SEED MORPHOLOGICAL FEATURES
Provedor de dados: 70
Autores: Aboukarima,Abdulwahed; El-Marazky,Mohamed; Elsoury,Hussien; Zayed,Moamen; Minyawi,Mamdouh.
ABSTRACT One of the new crop varieties that have been adopted for high yield is the Egyptian faba bean. However, poor-quality faba bean has reduced economic value. Quality evaluation is thus important and can be performed using computational intelligence. We developed a robust method based on morphological features and artificial neural network for quality grading and classification of Egyptian faba-bean seeds, covering five varieties: Giza3, Giza461, Misr1, Nobarya1, and Sakha1. Fifteen seed morphological features were then calculated, and artificial neural networks classified faba beans into different varieties. The results indicated an overall classification accuracy of 77.5% was achieved in training phase and it was 100% when testing dataset was used....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Faba bean; Quality; Classification; Artificial neural network; Features.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600791

Evaluation of five sugar cane planters
Provedor de dados: 70
Autores: Rípoli,Marco L. C.; Rípoli,Tomaz C. C.
Brazil is the world biggest producer of sugar cane with an area of 7x10(6) hectares. Mainly the system used for planting is the semi-mechanized one, which consists in opening the furrows with a machine, manually allocating the fractioned stalks and then covering the furrows done by the machines. The great amount of human labor used in the semi-mechanized system is becoming harder to find and also more expensive, indicating the need of a fully mechanized operation. Currently in Brazil these agriculture machines industries offers six different types of fully mechanized sugar cane planters (two types of whole stalks for planting and four using mechanized harvested stalks known as billets). All of them plant in two furrows simultaneously in 1.5 m row spacing....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sugar cane; Planters; Performance; Costs.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600012

Efeitos da cobertura do solo com filme de polietileno azul no consumo de água da cultura da alface cultivada em estufa
Provedor de dados: 70
Autores: Gonçalves,Alexandre O.; Fagnani,Maria A.; Peres,José G.
A cobertura do solo é uma prática agrícola que visa, principalmente, a controlar as plantas invasoras, a diminuir as perdas de água por evaporação do solo e a facilitar a colheita e a comercialização, uma vez que o produto se torna mais limpo e sadio. Porém, ao se cobrir o solo, também são alterados parâmetros importantes do microclima e, conseqüentemente, a germinação das sementes, o crescimento das raízes, a absorção de água e nutrientes, a atividade metabólica das plantas e o armazenamento de carboidratos. O objetivo do presente trabalho foi avaliar o efeito da cobertura do solo com filme de polietileno azul no consumo de água da cultura da alface (Lactuca sativa L.). O experimento foi instalado em uma estufa convencional, no município de Araras - SP, e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Consumo de água; Lisímetro de pesagem; Plástico.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300007

Avaliação das câmaras frias usadas para o armazenamento de frutas e hortaliças no entreposto terminal de São Paulo (CEAGESP): CEAGESP
Provedor de dados: 70
Autores: Ferreira Neto,Josué; Ferreira,Marcos D.; Neves Filho,Lincoln de C.; Andreuccetti,Caroline; Gutierrez,Anita de S. D.; Cortez,Luis A. B.
O tempo de vida pós-colheita de frutas e hortaliças está diretamente relacionado à temperatura de armazenamento do produto. Em condições controladas de temperatura e umidade relativa do ar, as reações metabólicas podem ser retardadas, proporcionando melhor conservação do produto. Foram realizadas avaliações das câmaras frias destinadas à estocagem de frutas e hortaliças na Companhia de Entrepostos e Armazéns Gerais de São Paulo, CEAGESP - São Paulo - SP, com o objetivo de identificar a situação das câmaras frias utilizadas nesse entreposto. As condições de estocagem dos produtos foram avaliadas por meio dos parâmetros: temperatura do ar, umidade relativa, isolamento, equipamento frigorífico (condensador, compressor, evaporador), piso, dimensões da câmara e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Frutas; Hortaliças; Câmaras frias; Estocagem.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300021

ESTIMATES OF MONTHLY AND ANNUAL EVAPORATION RATES AND EVAPORATED VOLUMES PER UNIT TIME IN THE TUCURUÍ-PA AND LAJEADO-TO HYDROELECTRIC POWER PLANT RESERVOIRS BASED ON DIFFERENT METHODS
Provedor de dados: 70
Autores: Coelho,Clívia D.; Silva,Demetrius D. da; Sediyama,Gilberto C.; Moreira,Michel C.; Pereira,Silvio B.; Lana,Ângela M. Q.
ABSTRACT Evaporation rates in reservoirs influence the volume of water available for multiple uses. Thus, the objective of this study was to estimate the evaporation rates and the evaporated volumes per unit time in the Tucuruí-PA and Lajeado-TO reservoirs based on the methods in Linacre (1993), Kohler et al. (1955), Morton (1983), Bruin &amp; Keijman (1979) and Penman (1948) method was adopted as the standard. The mean annual evaporation rates in the Tucuruí and Lajeado reservoirs, estimated by the Penman method, were similar, with values of 1,784 mm and 1,882 mm, respectively. None of the alternative analyzed methods could be used to estimate the mean annual evaporation in the Tucuruí and Lajeado reservoirs and could not replace the Penman method....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lake evaporation; Multiple water uses; Water resources.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100038

CLIMATE CHANGE IMPACTS ON WATER DEMAND OF MELON PLANTS IN JAGUARIBE-APODI REGION, BRAZIL
Provedor de dados: 70
Autores: Gondim,Rubens S.; Evangelista,Sílvio R. M.; Maia,Aline de H. N.; Duarte,Aryberg de S.
ABSTRACT The aim of this study was to evaluate the impacts of climate change on irrigation water demand of melon plants grown in Jaguaribe-Apodi Irrigation District (DIJA), which is located between the states of Ceará and Rio Grande do Norte, in Northeastern Brazil. Future scenarios were developed using the Eta-CPTEC/HadCM3 climate change projections, after being submitted to downscaling method. We used a set of climate data from the same model for the period of 1961 through 1990, and further projections after bias correction. Local geographic coordinates were interpolated using GIS techniques. Reference evapotranspiration (ETo) was estimated from the monthly minimum and maximum mean temperatures, using a limited data method. The rainfall, temperature,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiration; GIS techniques; Irrigation; Cucumis melo L.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300591

CORN FERTILIZATION USING SWINE WASTEWATER AND SOIL-WATER ENVIRONMENTAL QUALITY
Provedor de dados: 70
Autores: Rosa,Danielle M.; Sampaio,Silvio C.; Pereira,Pâmela A. M.; Reis,Ralpho R. Dos; Sbizzaro,Mariana.
ABSTRACT: Soil application of swine wastewater for nutrient cycling may represent a correct destination of these residues and reduction in production costs. However, when applied to soil, such residue may cause environmental impacts. This study aimed to analyze the chemical characteristics of the soil, corn, and leachate after successive swine wastewater applications associated with mineral fertilization. The experiment was developed in drainage lysimeters under field conditions. Wastewater doses applied were 0, 100, 200, and 300 m3 ha−1 with and without mineral fertilization. The results were submitted to analysis of variance and Tukey's test. After nine years of application, a special attention should be taken regarding water quality from a dose of 200...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Liquid residue of swine; No-tillage; Water reuse.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400801

Uso de geossintéticos como reforço em estradas não pavimentadas
Provedor de dados: 70
Autores: Oliveira,Lorena A.; Viana,Paulo M. F.; Santos,Divina C. R.; Reis,Elton F.
RESUMO O trabalho teve como objetivo avaliar o comportamento de estradas não pavimentadas construídas sobre solos moles reforçadas com diferentes geossintéticos. Foram selecionadas três estradas não pavimentadas que apresentassem um trecho com baixa capacidade de suporte de carga. A flecha foi medida pelo método fotográfico para cada número de passadas, nas condições com e sem reforço, e submetido à análise de variância, pelo teste de F, a 5% de probabilidade, e quando houve diferença significativa entre os tratamentos, suas médias foram comparadas pelo teste de Tukey. Posteriormente, realizou-se o cálculo da razão de benefício de tráfego fornecida pela inclusão do reforço. O geossintético não tecido, quando inserido no interior do solo, contribui de modo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Capacidade de suporte de carga; Trilha de roda; Simulador de tráfego.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300546

Perfomance evaluation of a direct injection engine using different blends of soybean (Glycine max) methyl biodiesel
Provedor de dados: 70
Autores: Nietiedt,Gustavo H.; Schlosser,José F.; Russini,Alexandre; Frantz,Ulisses G.; Ribas,Rodrigo L.
Diesel fuel is used widely in Brazil and worldwide. On the other hand, the growing environmental awareness leads to a greater demand for renewable energy resources. Thus, this study aimed to evaluate the use of different blends of soybean (Glycine max) methyl biodiesel and diesel in an ignition compression engine with direct injection fuel. The tests were performed on an electric eddy current dynamometer, using the blends B10, B50 and B100, with 10; 50 e 100% of biodiesel, respectively, in comparison to the commercial diesel B5, with 5% of biodiesel added to the fossil diesel. The engine performance was analyzed trough the tractor power take off (PTO) for each fuel, and the best results obtained for the power and the specific fuel consumption,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dynamometer; Power; Specific consumption.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500009

Analysis of the relationship intensity, duration, frequency of disaggregated daily rainfall in southern Rio Grande do Sul, Brazil
Provedor de dados: 70
Autores: Damé,Rita de C. F.; Teixeira-Gandra,Claudia F. A.; Villela,Francisco A.; Santos,Jacira P. dos; Winkler,Antoniony S.
The intensity, duration, and frequency relationship (IDF) of rainfall occurrence may be done through continuous records of pluviographs or daily pluviometer values . The objective of this study was to estimate the intensity-duration-frequency relationships of precipitation, using the method of daily rainfall disaggregation, at weather stations located to the southern half of the state of Rio Grande do Sul; comparing them with those obtained by rain gauge records, in places considered homogeneous from the meteorological point of view. The IDF equation parameters were estimated from daily rainfall disaggregation data, using the method of nonlinear optimization. To validate the equations confidence indices and efficiency and the "t" Student test, among...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydrology; Daily rainfall disaggregation; Heavy rain.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400006

Análise de um sistema de aquecimento de água para residências rurais, utilizando energia solar
Provedor de dados: 70
Autores: Basso,Luiz H.; Souza,Samuel N. M. de; Siqueira,Jair A. C.; Nogueira,Carlos E. C.; Santos,Reginaldo F.
A conscientização da importância do meio ambiente tem incentivado o estudo de novas fontes energéticas renováveis e menos poluentes. Dentre essas fontes, a energia solar destaca-se por ser perene e limpa. A utilização da energia solar em sistemas de aquecimento de água residencial rural pode colaborar com a economia de energia elétrica, base da matriz energética brasileira. Conhecer os fatores que influenciam na operação de um sistema de aquecimento de água por energia solar é importante na determinação de sua viabilidade técnica, visando a sua difusão em residências rurais. Para tanto, construiu-se um protótipo, no câmpus da Faculdade Assis Gurgacz, em Cascavel - PR, com características similares a um equipamento utilizado em residências para dois...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água quente; Circulação natural; Termossolar.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100002

Modelo dinâmico de simulação e otimização da força normal de reação do solo para um mecanismo de corte basal
Provedor de dados: 70
Autores: Volpato,Carlos E. S.; Braunbeck,Oscar A.; Oliveira,Carlos A. A. de.
O modelo físico foi baseado no método de Newton-Euler, sendo o mesmo desenvolvido utilizando o programa computacional científico Mathematica®. Realizaram-se várias simulações, nas quais se procurou obter a força normal de reação do solo variando velocidades de avanço (0,69; 1,12; 1,48; 1,82 e 2,12 m s-1); perfis de solo (senoidal, rampa ascendente e descendente) e altura do camalhão (0,025 e 0,05 m). Após as simulações iniciais, o mecanismo foi otimizado utilizando o programa computacional científico Matlab®, tendo como critério (função-objetivo) a minimização da força normal de reação do perfil (F N) e como variáveis de projeto os comprimentos das barras (L1y, L2, l3 e L4), altura da operação (L7), o comprimento inicial da mola (Lmo) e a constante...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanismo de quatro barras; Colheita mecânica; Forragem.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200017

Relação entre índice de área foliar e frações de componentes puros do modelo linear de mistura espectral, usando imagens ETM+/Landsat
Provedor de dados: 70
Autores: Xavier,Alexandre C.; Vettorazzi,Carlos A.; Machado,Ronalton E.
O índice de área foliar (IAF) é uma das mais importantes variáveis biofísicas da vegetação, estando relacionado diretamente com a evapotranspiração, com a produtividade da vegetação e com a interceptação da chuva pelo dossel. O objetivo deste trabalho foi analisar a relação do IAF de diversos tipos de cobertura do solo com Frações de Componentes Puros (FCPs) do Modelo Linear de Mistura Espectral (MLME). A área de estudo foi a microbacia hidrográfica do Ribeirão dos Marins, localizada no município de Piracicaba - SP. O IAF foi medido, no campo, com o equipamento LAI-2000, em 32 áreas com diferentes coberturas vegetais. A imagem utilizada foi do sensor ETM+ a bordo do satélite Landsat-7. No MLME, foram considerados três componentes puros (vegetação, solo e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensoriamento remoto; Modelo Linear de Mistura Espectral; LAI-2000.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200022

Variabilidade espacial de fatores de erosão em Latossolo Vermelho eutroférrico sob cultivo de cana-de-açúcar
Provedor de dados: 70
Autores: Souza,Zigomar M. de; Martins Filho,Marcílio V.; Marques Júnior,José; Pereira,Gener T.
Visando a avaliar a variabilidade espacial de fatores de erosão em Latossolo Vermelho eutroférrico, foram obtidas amostras do solo em intervalos regulares de 50 m, em forma de grid, totalizando 206 pontos de amostragem. Foram coletadas amostras nas profundidades de 0,0-0,2 m para a determinação da composição granulométrica e do conteúdo de matéria orgânica. Os fatores de erosão locais, como erosividade (R), erodibilidade (K), relevo (LS), perda de solo (A), potencial natural de erosão (PNE), risco de erosão (RE) e expectativa de erosão (EE), foram avaliados. A variabilidade do solo medida pelo coeficiente de variação registrou-se média para K, alta para o RE e EE e muito alta para A, LS e PNE. As variáveis estudadas apresentaram estrutura de dependência...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Semivariograma; Krigagem.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100012

EVALUATION OF THE RADIOMETRIC ACCURACY OF IMAGES OBTAINED BY A SEQUOIA MULTISPECTRAL CAMERA
Provedor de dados: 70
Autores: Teixeira,Alison A. D.; Mendes Júnior,Cláudio W.; Bredemeier,Christian; Negreiros,Marcelo; Aquino,Robson dos S.
ABSTRACT Geometric and radiometric corrections of images obtained by remotely piloted aircraft systems (RPAS) are required for the measurement of the spectral reflectance and calculation of vegetation indices. This study aimed to determine which radiometric calibration procedures allow obtaining suborbital images with more accurate reflectance data and spectral indices based on data collected by a Sequoia multispectral camera coupled to a RPAS on black oat cultivations at the flowering stage located in Eldorado do Sul, RS, Brazil. The orthophoto mosaics were processed without and with radiometric corrections by reflectance calibration ground target and/or solar irradiance sensor of the camera, and the radiometric accuracy of these images was evaluated...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: NDVI; NDRE; Sequoia camera; Radiometric correction.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600759

PERFORMANCE OF AN AGRICULTURAL DIESEL ENGINE USING DIFFERENTS FUELS
Provedor de dados: 70
Autores: Perin,Gismael F.; Schlosser,José F.; Galon,Leandro; Rodrigues,Fabrício A.; Frantz,Ulisses G.
ABSTRACT The use of fuels for agricultural Diesel engines cycle, both of mineral origin (Diesel) or vegetable and animal origin (biodiesel) can significantly alter its performance. Therefore, the aim of this study was to quantify the change in torque, power and consumption of agricultural Diesel engine fuel using minerals and vegetables fuels. It was used a tractor power take-off coupled to a magnetic brake dynamometer (for measuring speed and torque for subsequent calculation of power), and a flow meter (for measuring the hourly fuel consumption and specific fuel consumption calculation). Eleven different fuels (S10 mineral diesel with 5%, 10%, 15%, 20% and 50% biodiesel and mineral diesel S500 with 5%, 10%, 15%, 20% and 50% biodiesel, have been used pure...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Test; Dynamometer; Tractor; Torque; Power.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100091

NITROGEN, PHOSPHORUS AND POTASSIUM ACCUMULATION IN WATERMELON CULTIVARS IRRIGATED WITH SALINE WATER
Provedor de dados: 70
Autores: Costa,Andréa R. F. C. da; Medeiros,José F. de.
ABSTRACT The use of saline water in agriculture has increased in the Brazilian semiarid due to low availability of good quality water for irrigated agriculture, being the selection of salt tolerant hybrids an alternative to reduce the effect of salinity on nutritional status of plants. So, the objective of this work was to evaluate the effect of salinity of irrigation water in the accumulation and partition of nutrients in the vegetable tissue of watermelon cultivars, in the region of Mossoro in the State of Rio Grande do Norte, Brazil. The treatments studied consisted of applying irrigation water with five electrical conductivities (EC1 = 0.57, EC2 = 1.36, EC3 = 2.77, EC4 = 3.86 and EC5 = 4.91 dS m-1), two watermelon cultivars and four samplings times...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrullus lanatus; Plant nutritional status; Water management.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300343

SPRAYING QUALITY OF CROP PROTECTION PRODUCTS USING TWO DROPLET SPECTRA IN THREE PERIODS OF THE DAY
Provedor de dados: 70
Autores: Graziano,Carlos E. P. L.; Alves,Karina A.; Gandolfo,Marco A.; Dario,Gustavo; Oliveira,Rone B.
ABSTRACT: Spraying of crop protection products can be affected by weather conditions and spray nozzles, altering deposition patterns and coverage of the target surface. The objective of this research was to analyze the quality of sprayings performed in three periods of the day (9:00 am, 2:00 pm, and 6:00 pm), using two different droplet sizes (fine and coarse) in soybeans. Coverage and deposition were evaluated in the upper, middle, and lower portion of soybean canopy. Spraying the products at 2:00 pm increased leaf coverage in the medium portion but also increased losses to the soil. Spray nozzles with fine droplet sizes provided greater coverage and deposition in the medium and upper portion of the crop for the sprayings performed in the morning. If...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coverage; Deposition; Endo-drift; Spraying time; Application technology.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601183

Atributos físicos de um latossolo cultivado com cana-de-açúcar após aplicações de lodo de esgoto e vinhaça
Provedor de dados: 70
Autores: Camilotti,Fábio; Andrioli,Itamar; Marques,Marcos O.; Silva,Alysson R. da; Tasso Júnior,Luiz C.; Nobile,Fabio O. de.
O objetivo deste trabalho foi avaliar se a aplicação anual de lodo de esgoto e vinhaça, resíduos empregados com a finalidade exclusiva de fornecer a quantidade necessária de N e K para cana-de-açúcar, causaria alteração em alguns atributos físicos de um Latossolo Vermelho distroférrico argiloso, após as colheitas do 3º e 4º cortes da cultura. O experimento foi conduzido em blocos ao acaso, com três repetições. Os tratamentos foram: (i) dose de lodo de esgoto para suprir 100% do N exigido pela cultura; (ii) dose de lodo de esgoto para suprir 200% do N exigido; (iii) dose de vinhaça para suprir 100% do K exigido; (iv) dose de vinhaça para suprir 200% do K exigido; (v) combinação dos tratamentos (i) e (iii); (vi) combinação dos tratamentos (ii) e (iv); (vii)...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Matéria orgânica do solo; Resíduos orgânicos; Saccharum.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300010

Produtividade e qualidade de frutos de mamão cultivar 'Golden' sob diferentes lâminas de irrigação e doses de potássio no norte de Espírito Santo
Provedor de dados: 70
Autores: Marinho,Albanise B.; Bernardo,Salassier; Sousa,Elias F. de; Pereira,Messias G.; Monnerat,Pedro H.
Este trabalho teve como objetivo estudar os efeitos de diferentes lâminas de irrigação e de doses de potássio sobre a produtividade e a qualidade dos frutos do mamoeiro cultivar Golden. O experimento foi realizado em área de produção agrícola comercial, localizada em Linhares - ES. O delineamento experimental foi em blocos casualizados, com arranjo em parcela subdividida, com três repetições. Os tratamentos foram compostos por cinco lâminas de irrigação, na parcela, e quatro doses de potássio, na subparcela, totalizando 20 tratamentos. As cinco lâminas de irrigação programadas foram de 50; 70; 90; 110 e 130% da ETo, e as quatro doses de potássio foram de 30; 42; 54 e 66 g de K2O por planta ao mês. Os elevados índices pluviométricos no período experimental...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Produção; Nutrição de plantas.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300003

PROCESSING IN THE QUALITY OF TANZANIA GRASS SEEDS
Provedor de dados: 70
Autores: Melo,Lilian F. De; Martins,Cibele C.; Silva,Givanildo Z. Da; Sanches,Mauricio F. G.
ABSTRACT The available research concerning the processing of grass seeds is scarce, despite its fundamental importance for national and international agribusiness. The objective of this project was to evaluate the effects of processing phases on the physical and physiological quality of tanzania grass seeds for commercialization purposes. Seeds were sampled before processing and after leaving the air and screen machine (upper and intermediate screens and bottom); first gravity table (drift, upper and intermediate spouts); treating machine; second gravity table (upper, intermediate, and lower spouts). Seeds were evaluated as to water content, physical quality (purity and 1,000 seeds weight) and physiological (germination, first count of germination,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Germination; Panicum maximum; Pastures; Tropical grass; Vigor.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601157

Desempenho da sonda de dissipação térmica na medida da transpiração de plantas jovens de Lima Ácida
Provedor de dados: 70
Autores: Delgado-Rojas,Juan S.; Angelocci,Luiz R.; Folegatti,Marcos V.; Coelho Filho,Maurício A.
Devido à dificuldade de se quantificar o consumo individual de água de uma árvore, tem surgido uma série de técnicas de medida do fluxo de seiva que passa por meio do caule, o qual é relacionado diretamente com a transpiração da planta. Este trabalho teve como objetivo avaliar o desempenho de uma dessas técnicas, denominada método da sonda de dissipação térmica (SDT), na medida de fluxo de seiva em plantas de lima ácida ‘Tahiti’. O experimento foi instalado em pomar de plantas jovens, localizado na fazenda experimental de irrigação, do Departamento de Engenharia Rural da ESALQ, em Piracicaba - SP, sendo a avaliação feita utilizando dois lisímetros de pesagem. Os resultados indicaram que o método estudado pode ser utilizado para essa finalidade em condições...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citros; Fluxo de seiva; Sonda de Granier.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300009

Energy demand in citrus production under varied operational efficiency values
Provedor de dados: 70
Autores: Franco Junior,Nelson C.; Milan,Marcos; Romanelli,Thiago L.
Citrus orchards are very important in Brazil, especially in São Paulo State, where occupy an area of 600,000 ha approximately. To identify sustainability degree of citrus production system, an energy analysis allows evaluating efficiency of direct and indirect applied inputs. Thus, this study aimed to evaluate citrus production system under energetic point of view, in which invested energy is paid back with citrus production; being compared within three scenarios for operational field efficiency. As result, by sensitivity analysis was determined that fuel was the main energy demander, followed by pesticides and fertilizers. In operational work capacity analysis, all combinations between efficiency (minimum, typical and maximum) and yield levels became...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy balance; EROI; Machinery management; Sustainability.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400014

Proposta de um sistema de medição de desempenho aplicado à mecanização agrícola
Provedor de dados: 70
Autores: Peloia,Paulo R.; Milan,Marcos.
As organizações líderes dos mais diferentes setores têm como característica medir o próprio desempenho de modo sistêmico, porém nas empresas agrícolas ainda não é comum o emprego desse conceito, incluindo o setor de mecanização. A mecanização tem um forte impacto na composição dos custos de produção, e conhecer o seu desempenho é primordial para o sucesso de empresa agrícola. A importância que as medidas de desempenho têm no auxílio à gestão e o que a mecanização representa para os custos de produção justificaram o desenvolvimento deste trabalho, que tem como objetivo propor um sistema de medição de desempenho integrado para dar suporte à gestão da mecanização agrícola. A metodologia foi dividida em duas etapas: adaptação de um modelo conceitual sistêmico,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Máquinas agrícolas; Mecanização agrícola; Sistemas de informação; BSC.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400012

Hymenaea courbaril SEEDLINGS IN PROTECTED ENVIRONMENTS AND SUBSTRATES
Provedor de dados: 70
Autores: Sanches,Cássio F.; Costa,Edilson; Costa,Geany G. S. da; Binotti,Flávio F. da S.; Cardoso,Eliana D.
ABSTRACT The Brazilian copal is a tree fruit species that can be used for various purposes. The study evaluated protected environments and substrates in forming Brazilian copal seedlings (Hymenaea courbaril), at the State University of Mato Grosso do Sul, Cassilândia-MS, from January to March, 2014. Two greenhouses were used: (A1) agricultural greenhouse covered with aluminized thermal reflector screen of 50% shading and (A2) agricultural greenhouse covered with black screen of 50% shading. Inside the greenhouses, substrates derived from mixtures of cattle manure, soil, medium vermiculite, super fine vermiculite and washed fine sand were tested. For each cultivation environment, a completely randomized experimental design was used. The environments were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hymenaea courbaril; Solar radiation; Reflective covered; Cattle manure; Vermiculite; Humus; Sand.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100024

SPATIAL VARIABILITY OF THE WATER DEPTH APPLIED BY FIXED SPRINKLER IRRIGATION SYSTEMS
Provedor de dados: 70
Autores: Tamagi,Jorge T.; Uribe-Opazo,Miguel A.; Vilas Boas,Marcio A.; Johann,Jerry A.; Guedes,Luciana P. C.
Abstract The uniformity of water application is an important factor in the evaluation of sprinkler irrigation systems. This uniformity depends on the type of sprinkler and its operating conditions, such as the arrangement and spacing between the sprinklers in the area; velocity and wind direction during the period of water application and the pressure variation of the irrigation system. The objective of this study was to model, analyze and compare the structure of spatial dependence, as well as the spatial variability of the water depths applied by a sprinkler irrigation system with compensating and non-compensating sprinklers, using geostatistical methods and measurements of accuracy or similarity between the applied water depth maps. The experiment was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compensating sprinklers; Noncompensating sprinklers; Spatial dependence.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200188

Modelos matemáticos para ajuste das isotermas de dessorção da polpa de banana da variedade prata
Provedor de dados: 70
Autores: Gouveia,Josivanda P. G. de; Nascimento,Jucilene do; Almeida,Francisco de A. C.; Silva,Manassés M. da; Farias,Eliana da S.; Silva,Flávio L.H. da.
O presente trabalho teve por objetivo estudar as isotermas de dessorção da polpa de banana nos estádios madura e semiverde (Musa acuminata L.) da variedade Prata, para as temperaturas de 20; 30 e 40 ºC pelo método gravimétrico estático, na faixa de atividade de água de 0,48 a 0,81. Os dados experimentais obtidos foram ajustados por regressão não linear, pelos modelos de BET, GAB, Halsey e Oswin, escolhendo-se o melhor, mediante o valor do coeficiente de determinação (R²) e erro médio relativo (E). Os modelos que apresentaram o menor erro relativo (E) e o maior coeficiente de determinação (R²), foram os de Oswin e GAB, respectivamente. O de GAB foi escolhido por ser triparamétrico, o que permite melhor ajuste dos dados até a atividade de água de 0,9.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Musa acuminata; Isotermas de dessorção; Atividade de água.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300034

Calibration of angles of nozzles and deposition of an axial-flow sprayer on dwarf cashew
Provedor de dados: 70
Autores: Mion,Renildo L.; Sousa,Beatriz M. de; Cordeiro,Igor M.; Sombra,Weberte A.; Duarte,José M. de L.; Lucas,Fidel C. B.
The study aimed to determine an optimum angle for the nozzles axial-flow sprayers a deposition for better vertical distribution focused on cashew. In laboratory tests were conducted adjusting the angle of the nozzle axial-flow sprayers. The experimental design was randomized blocks in a 2x3 factorial with four replications. The treatment for this test were two settings (with and without the adjustment of the angles of the nozzles ) and tree application volumes 273, 699 and 954 L ha-¹.The study was conducted in an orchard of dwarf cashew, with eight years of age. It was concluded that the volumetric distribution profile showed better vertical distribution uniformity when the angles of the nozzles were regulated for the canopy, the adjustment of the angles...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fruit; Deposition; Vertical patternator.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400020

Validação de um modelo de cálculo por elementos finitos do chassi de uma semeadora de quatro linhas
Provedor de dados: 70
Autores: Niemczewski,Bóris K.; Reis,Ângelo V. dos; Machado,Roberto L. T.; Machado,Antônio L. T.
O comportamento estrutural estático de um chassi experimental de semeadora de quatro linhas para agricultura familiar foi testado, utilizando-se da técnica numérica de Análise de Elementos Finitos, onde se levou em consideração os esforços a que a máquina em questão estaria sujeita, quando suspensa do chão, pelos três pontos de engate do trator. Para a validação do modelo usado pelo software SolidWorks Simulation, submeteu-se um protótipo em escala real do chassi a carregamentos de forças verticais, a fim de comparar os deslocamentos reais da estrutura com os deslocamentos calculados pelo software. Dois estudos foram feitos do modelo para o cálculo dos deslocamentos da estrutura: no primeiro, não foram incluídos os suportes dos engates dos três pontos no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanização; Agricultura familiar; Deslocamentos; Métodos numéricos.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100017

Physical, chemical and microbiological properties of a Dystrophic Yellow Latosol using manipueira
Provedor de dados: 70
Autores: Silva Júnior,João J. da; Coelho,Eugênio F.; Sant'Ana,José A. do V.; Accioly,Adriana M. de A.
The study aimed to evaluate chemical, microbiological and hydro-physical changes of a Dystrophic Yellow Latosol, receiver of different levels of manipueira (cassava wastewater) application, in the cultivation of 'Terra Maranhão' banana. The experimental design was a randomized block with three replications in a factorial scheme 3 x 4, in which it was considered three soil depths and four levels of manipueira. It was evaluated the weighted mean diameter of the aggregate, the percentage of aggregation at different periods, soil density, particle density, porosity and soil saturated hydraulic conductivity, in addition to pH of P (mg dm -3), K (mg dm-3), Ca (cmolc dm-3), Mg (cmolc dm-3), Ca+Mg (cmolc dm-3), Al (cmolc dm-3), Na (cmolc dm -3), H+Al (cmolc dm-3),...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertirrigation; Water reuse; Musa spp.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400013

The influence of the season of the year and of dilution on the development of swine manure and wood shaves co-composting
Provedor de dados: 70
Autores: Higarashi,Martha M.; Sardá,Luana G.; Oliveira,Paulo A. V.
The objective of this research was to study the influence of factors related to the proper management of pig manure (lower dilution) and the season of the year in the progress of the co-composting of pig manure with wood shavings and in the final quality of the compost resulting from the treatments. In the first experiment, two types of swine manure were used: a diluted one (2% Dry Matter - DM), typical from the management usually used in Brazil, and a more concentrated one (6% DM). The manures were incorporated into the wood shavings (6L:1kg) over the course of four weeks. The development of composting was accompanied by monitoring of temperatures inside the piles and the emission of CO2 and CH4 gases during 65 days, including the period of incorporation....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pig farming; Manure management; Compost; Gas emission.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200004

Use of interactive performance optimization for identifying the ideal profile of swine finishing producers
Provedor de dados: 70
Autores: SANGOI,LUIZ F.; KESSLER,ALEXANDRE M.; SILUK,JULIO C. M.; RIBEIRO,ANDREA M. L.; NEUENFELDT JÚNIOR,ALVARO L.
The present research aimed to develop a modeling capable of identifying the ideal profile of swine finishing producers using the interactive performance optimization, which began by verifying qualitative the criteria considered most relevant to the decision-making, generating a closed structured diagnosis that covers the socioeconomic aspects about the activity, until the design of a mathematical model able to translate the data obtained in quantitative information. For the verification, it was proposed a practical study for a universe of 120 members of a cooperative in the state of Rio Grande do Sul, Brazil. The results showed that, from the application and the definition of the ideal profile, it was possible to verify that 82 producers are in the group...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Swine production; Performance optimization; Competitiveness; Agribusiness.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200197

Errata: volume 24, número 1
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/report
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300036

Mathematical model to estimate of the deterioration of wooden poles in contact with soil used in rural areas
Provedor de dados: 70
Autores: Molina,Julio C.; Calil Júnior,Carlito; Freitas,Roberto R. de.
In São Paulo State, mainly in rural areas, the utilization of wooden poles is observed for different purposes. In this context, wood in contact with the ground presents faster deterioration, which is generally associated to environmental factors and, especially to the presence of fungi and insects. With the use of mathematical models, the useful life of wooden structures can be predicted by obtaining "climatic indexes" to indicate, comparatively among the areas studied, which have more or less tendency to fungi and insects attacks. In this work, by using climatological data of several cities at São Paulo State, a simplified mathematical model was obtained to measure the aggressiveness of the wood in contact with the soil.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Durability of wood; Decay of wood; Wooden poles.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500019

Response of young 'Tahiti' lime trees to different irrigation levels
Provedor de dados: 70
Autores: Alves Júnior,José; Folegatti,Marcos V.; Silva,Cláudio R. da; Silva,Tonny J. A. da; Evangelista,Adão W. P.
The aim of this study was to evaluate the effect of different irrigation levels on canopy and root growth, productivity, and fruit quality of young ‘Tahiti’ acid lime trees. The experiment was installed in Piracicaba, Brazil in a 1.0-ha orchard plot with ‘Tahiti’ acid lime trees, grafted on ‘Swingle’ citrumelo rootstock and carried out from August of 2002 to May 2005. Each treatment was assigned to a drip irrigation level, based on ETc as follows: T1) non-irrigated, T2) 25%, T3) 50%, T4) 75% and T5) 100% of ETc determined by weighing lysimeter presented in the orchard plot. Trunk diameter and tree height were evaluated monthly. The roots were evaluated when the trees were 30 and 48 months old. The yield and fruit quality was evaluated in 2004 and 2005. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation scheduling; Citrus latifolia Tan.; Evapotranspiration; Root distribution.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200010

OPERATOR EFFORT ON THE OPERATION OF THE KNAPSACK SPRAYER PUMPING LEVER
Provedor de dados: 70
Autores: Lambrecht,Edson; Rosa,Douglas S. da; Machado,Roberto L. T.; Machado,Antônio L. T.; Reis,Ângelo V. dos.
ABSTRACT Several equipments are used in the application of agrochemicals by small scale farmers, with emphasis on the knapsack hand sprayer due to the low cost of acquisition and viability of use in different operating conditions. Although it is an equipment widely used, few studies have been developed in order to ascertain its functional characteristics. This study has the objective of presenting a methodology to measure the effort to which the operator is subjected in the activation of the pumping lever of knapsack hand sprayer verifying if these machines fit within the limitations foreseen by the Brazilian laws and international regulations. The methodology used was adequate to measure the operator's required efforts for the activation of knapsack hand...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ergonomics; Upper limb effort; Effort in sprayers.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200238

THERMODYNAMIC PROPERTIES OF TAMARIND SEEDS (Tamarindus indica L.)
Provedor de dados: 70
Autores: Ferreira Junior,Weder N.; Resende,Osvaldo; Silva,Ligia C. de M.; Pinheiro,Gleyce K. I.; Sousa,Kelly A. de.
ABSTRACT Tamarind is used in the food and pharmaceutical industry, and its seed is the main means for the reproduction of this species, thus justifying studies that ensure its post-harvest viability. This research aimed to study the thermodynamic properties of tamarind seeds as a function of the equilibrium moisture content. The experimental data of the water activities were obtained by the indirect static method. The Cavalcanti Mata model was used to determine the thermodynamic properties of tamarind seeds, as it was the model that best fitted the experimental data of the desorption isotherms. The results showed that the thermodynamic properties are influenced by the moisture content and temperature, with an increase in the energy required to remove water...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Equilibrium moisture content; Enthalpy; Gibbs free energy.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600740

Produtividade e qualidade da brachiaria irrigada no outono/inverno
Provedor de dados: 70
Autores: Dantas,Geffson de F.; Faria,Rogério T. de; Santos,Gilmar O.; Dalri,Alexandre B.; Palaretti,Luiz F.
RESUMO Um dos fatores que determinam os baixos índices zootécnicos na pecuária brasileira é a estacionalidade da produção das plantas forrageiras tropicais. A irrigação pode proporcionar aumento e estabilização da produtividade durante o outono e o inverno. Objetivou-se pelo presente estudo avaliar: a) a produtividade de massa seca e qualidade de forragem de Brachiaria brizantha, em função de lâminas de irrigação, no período do outono e do inverno; b) a umidade do solo e a temperatura do ar a fim de determinar seus efeitos na produtividade de forragem. O experimento foi conduzido na Fazenda Experimental da FCAV-Unesp, em Jaboticabal-SP. Utilizou-se de um sistema de aspersão em linha para estabelecer tratamentos com cinco lâminas de irrigação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brachiaria brizantha; Forragem; Irrigação.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300469

LIQUID DIFFUSION DURING DRYING OF SORGHUM GRAINS UNDER DIFFERENT CONDITIONS
Provedor de dados: 70
Autores: Silva,Lígia C. de M.; Resende,Osvaldo; Oliveira,Daniel E. C. de; Ferreira Junior,Weder N.; Rodrigues,Gabrielly B.
ABSTRACT Drying is the most widely used process to ensure the quality and stability of plant products. Therefore, this study aimed to determine the effective water diffusivity and activation energy in grain sorghum during drying at different temperatures and initial moisture contents. Sorghum grains (cultivar DeKalb 640) were harvested with an initial moisture content of 0.49 kg water kg−1 dry matter. The effective diffusion coefficient was determined from different initial moisture contents of approximately 0.49, 0.40, 0.31, and 0.23 kg water kg−1 dry matter. Grains with different moisture contents were dried under four temperature conditions of 40, 60, 80, and 100 °C on perforated trays. The spherical geometry model was used for liquid diffusion. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Diffusion coefficient; Activation energy; Sorghum bicolor L.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600737

Ammonia nitrogen desorption from sanitary landfill leachate in filling towers
Provedor de dados: 70
Autores: Leite,Valderi D.; Barros,Aldre J. M.; Lopes,Wilton S.; Sousa,José T. de.
Sanitary landfill leachates present high concentrations of carbonaceous and nitrogenous materials. The crucial point is that carbonaceous materials are of difficult biodegradation, what compromises the performance of biological treatment processes, while nitrogenous materials, such as ammonia nitrogen, probably preclude the use of biological treatments. Therefore, the aim of this work was to study the desorption process of ammonia nitrogen from sanitary landfill leachate in filling towers. Desorption was carried out in filling towers of 35 L capacity. The leachate was collected from a sanitary landfill located in João Pessoa, Paraíba State, Brazil. Desorption efficiency for the pH values ​​adopted in four treatments was 93% minimum and 95.5% maximum, with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Leachate; Ammonia nitrogen; Filling tower; Desorption.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300017

QUALITY OF SUGARCANE MECHANIZED PLANTING
Provedor de dados: 70
Autores: CORTEZ,JORGE W.; Missio,Camilla; Barreto,Ana K. G.; Silva,Marcelei D. Da; Reis,Gustavo N. Dos.
ABSTRACT: The quality of the sugarcane plantation affects the plantation longevity, yield and production costs. Therefore, this study aimed to evaluate the quality of sugarcane mechanized planting in day and night shifts. The mechanized planting was carried out in Ivinhema, MS, Brazil. For the evaluation of pre-planting seedlings, were collected 40 billets in the seedling area with 10 repetitions for each shift. For the other variables, it was held sampling, totaling 60 points, 30 points assessed for each shift. The variables evaluated were: total of natural damage and total of mechanized damage in pre-planting, shoot per meter, viable shoots per meter, total of unviable shoots, seedlings consumption and failures percentage. Data were analyzed with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Statistical process control; Saccharum spp; Control charts.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601136

Solar drying of jack fruit almonds
Provedor de dados: 70
Autores: Queiroz,Alexandre J. de M; Dantas,Hermeval J; Figueirêdo,Rossana M. F. de; Melo,Karla dos S.
Dryers heated by solar energy have been constructed and used in drying whole and half jack fruit almonds. The samples were dried during the day in direct sun and in the conventional solar dryer prepared for this purpose. Another piece of equipment was built for reception and accumulation of sun energy in a body of water, which was used as a heat source for night drying. The drying with the sun energy was compared with artificial drying. The jack fruit almonds were dried whole, half, with pellicle and without it. The storage of solar energy in water was technically viable for use in night drying. The drying by combining solar dryers in the day and night periods were completed in approximately 35 hours, and were equivalent to artificial drying between 40ºC...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Artocarpus heterophyllus; Solar dryer; Agricultural residues.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600012

THE TOPPLING OF AN IRRIGATION CENTER PIVOT SUBMITTED TO WIND ACTION EFFECTS
Provedor de dados: 70
Autores: Schmidt,Edomir M.; Meira Junior,Agenor D. de; Pedrali,Patricia C.; Valdiero,Antonio C.; Thesing,Nelson J.
ABSTRACT This research aims to improve the study about the stability of truss structures used in pivot irrigation, widely used due to the growing demand for food production, when submitted to wind effects. Specifically, it aims to verify the maximum wind speed supported by an irrigation center pivot structure when submitted to the load effects caused by wind gusts perpendicular to the equipment. In order to determine these forces and their effects on the irrigation equipment, computational numerical investigations were carried out using finite element bar models validated by measuring the natural frequency of the equipment in the field. A span was designed based on the existing standards in Brazil and the dynamic response of the structure was examined...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Toppling; Stability; Wind; Pivot; Irrigation.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200150

VALIDATION OF A HEATING SYSTEM IN THE FARROWING HOUSE USING A CFD APPROACH
Provedor de dados: 70
Autores: Damasceno,Flávio A.; Oliveira,Carlos E. A.; Saraz,Jairo A. O.; Schiassi,Leonardo; Oliveira,Jofran L. de.
ABSTRACT The current heating system for piglets in the farrowing usually uses incandescent lamps and, in some cases, heated floors with electric resistances, which in most cases generates a high energy cost. Thus, the implantation of systems that use renewable energies in the heating of piglets can allow the thermal comfort of the animals without reducing the productive development. The objective of this research was to evaluate a computer model in Computational Fluid Dynamics (CFD), which predicts surface temperature in the heating system of a farrowing house. The study was conducted during the summer season on the swine sector of Federal University of Lavras, Brazil. For this study, a prototype solar heater using alternative materials (ASWH) was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Swine; Computational modelling; Simulation.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400471

Modelo para estimativa do potencial produtivo em trigo e cevada por meio do sensor GreenSeeker
Provedor de dados: 70
Autores: Grohs,Daniel S.; Bredemeier,Christian; Mundstock,Claudio M.; Poletto,Naracelis.
Áreas com diferentes potenciais de rendimento dentro de uma lavoura necessitam ser manejadas separadamente, para fins de aplicação da adubação nitrogenada em cobertura. O equipamento baseado em sensoriamento remoto terrestre (GreenSeeker) é um dos instrumentos utilizados para separar diferentes zonas de manejo. Para fazer isso, o sensor permite a definição de classes para estimar o potencial produtivo de forma ágil, precisa e em tempo real. Com o instrumento, foi desenvolvido um modelo para estimativa do potencial produtivo em trigo e cevada, correlacionando o Índice de Vegetação por Diferença Normalizada (NDVI) com a biomassa seca acumulada na parte aérea, por ocasião da emissão da sexta folha do colmo principal. A base do modelo foi a formação de classes...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Adubação nitrogenada em taxa variável; NDVI.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100011

Emergence of corn according to the sowing depth of the seed and loads on press wheels
Provedor de dados: 70
Autores: Neto,Pedro H. Weirich; Lopes,Angelo R. C.
The seeding process was the operation that suffered the most changes in no-tillage system due the cover crop soil and new particle soil arrangement. The objective of this study was to verify the effects of loads applied to the wheels and adjustments of sowing depth on seedling emergence of corn in no-tillage system. The experimental design was completely randomized with a factorial arrangement 5x4, with five loads applied to the wheels and four theoretical sowing depth adjustments. The real sowing depth increased in the lower theoretical depth and decreased in the higher theoretical depth, due to the compaction loads. Regarding the time of emergence, loads applied had not influence at the greater depths. Emergence time decreased with the load increase in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Seeding process; No-tillage; Farm mechanization.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200012

Carbon footprint of the colombian cocoa production
Provedor de dados: 70
Autores: Ortiz-Rodríguez,Oscar O.; Villamizar-Gallardo,Raquel A.; Naranjo-Merino,Carlos A.; García-Caceres,Rafael G.; Castañeda-galvís,María T.
ABSTRACT Cocoa is an important commercial crop in the tropics; and estimating the carbon emissions in the producing-areas is a worthwhile effort. The main goal of the current paper was to evaluate the carbon footprint (CF) per kilogram of Colombian cocoa bean produced under conventional and agroforestry managements, following the methods proposed by PAS 2050. In this research, we compared our results to other worldwide researches, showing an overview of the current limitations and challenges involving the CF researches. Our results showed that all calculated environmental burdens were lower for the conventional management. In the agroforestry practice, composting of cocoa pod husks contributed with approximately 34.00E+00 g methane and 2.55E+00 g nitrous...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carbon footprint; Climate changes; Global warming potential; Theobroma cacao L.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200260

BIOGAS YIELD AND PRODUCTIVENESS OF SWINE MANURE FOR DIFFERENT REACTOR CONFIGURATIONS
Provedor de dados: 70
Autores: Lins,Marcos A.; Steinmetz,Ricardo L. R.; Amaral,André C. do; Kunz,Airton.
ABSTRACT The progression of the organic loading rate (OLR) up to a certain limit increases biogas production. The limit and operation range vary according to the configuration of the reactor and are associated with other variables that generate different results with respect to biogas yield (BY) and biogas productiveness (BP). The aim of this study was to investigate the effect of the OLR on the BY and BP from swine manure in continuous stirred tank reactors (CSTRs) and upflow anaerobic sludge blanket reactors (UASBs). In the assay with the CSTR, the best operational condition was at an OLR of 0.7 gVS add L−1 reactor d−1 and a hydraulic retention time (HRT) of 18 days. At this operational condition, 0.8 LN biogas gVS add−1 of BY and 0.6 LN biogas L−1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bioenergy; Sustainability; Swine farms.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600664

Doses de composto orgânico comercial na composição de substratos para a produção de mudas de maracujazeiro em diferentes tipos de cultivo protegido
Provedor de dados: 70
Autores: Costa,Edilson; Leal,Paulo A. M.; Sassaqui,Adriano R.; Gomes,Viviane do A.
Doses de composto orgânico comercial misturado ao solo foram utilizadas como substrato na produção de mudas de maracujazeiro amarelo. O experimento foi conduzido no Campus de Aquidauana, da Universidade Estadual de Mato Grosso do Sul, de setembro a dezembro de 2007. Utilizaram-se seis ambientes protegidos: estufa plástica com pé-direito de 2,5m; viveiro telado com Sombrite® 50%, com pé-direito de 2,5m; viveiro telado de tela termo-refletora Aluminet® 50%, com pé-direito de 2,5m; viveiro coberto com palha de coqueiro, com pé-direito de 1,8m; estufa plástica com pé-direito de 4,0m, possuindo abertura zenital e tela termo-refletora 50% sob o plástico e, viveiro telado de tela de sombreamento 50%, com pé-direito de 3,5m. Foram utilizados cinco substratos com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Passiflora edulis Sims f. flavicarpa Deg.; Estufas; Viveiros; Substratos.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500001

Low cost driver device for microclimate maintenance in the pre-milking of dairy cattle
Provedor de dados: 70
Autores: Silva,Irenilson M. da; Pandorfi,Héliton; Vasconcelos,Ângelo J. S. de; Laurenti,Renato; Guiselini,Cristiane.
Due to the importance of the environment on animal production and thus environmental control, the study aims to build a system for monitoring and control the meteorological variables, temperature and relative humidity, low cost, which can be associated with an evaporative cooling system (ECS). The system development included all the stages of assembly, test and laboratory calibration, and later the validation of the equipment carried in the field. The validation step showed results which allowed concluding that the system can be safely used in the monitoring of these variables. The controller was efficient in management of the microclimate in the waiting corral and allowed the maintenance of the air temperature within the comfort range for dairy cattle in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dairy cattle; Thermal comfort; Instrumentation.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100001

FUZZY MODELING IN ORANGE PRODUCTION UNDER DIFFERENT DOSES OF SEWAGE SLUDGE AND WASTEWATER
Provedor de dados: 70
Autores: Putti,Fernando F.; Lanza,Marcio H.; Filho,Hélio G.; Cremasco,Camila P.; Souza,Angela V.; Gabriel Filho,Luís R. A.
ABSTRACT The present work aimed to develop mathematical fuzzy models to evaluate the effects of different doses of sewage sludge and irrigation with wastewater and potable water. Such models were elaborated from an experiment carried out at the Faculty of Agronomic Sciences, in the Department of Soil and Environmental Resources, from the Sao Paulo State University, in Brazil. The experiment was carried out in a randomized block design, in a 6 × 2 factorial scheme, with 6 doses of sewage sludge (0, 25, 50, 75, 100 and 125 of the recommended dose of N), and in the presence and absence of wastewater. In the development of the fuzzy model, the Mamdani method was used for the defuzzification. As input variables, the doses of sewage sludge and the types of water...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuzzy logic; Organic matter; Biosolid; Reuse water; Mamdani method.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200204

Desempenho operacional de um protótipo "aerossolo"
Provedor de dados: 70
Autores: Lopes,Afonso; Camara,Felipe T. da; la Scala Júnior,Newton; Furlani,Carlos E. A.; Silva,Rouverson P. da; Barbosa,Ana L. P. B.
O desempenho operacional de máquinas e equipamentos agrícolas é de fundamental importância para o conhecimento do comportamento desses em condições de trabalho. O presente estudo teve por objetivo avaliar o desempenho operacional de um protótipo "Aerossolo", tracionado por um trator Valtra BM100 4x2 TDA, com potência no motor de 73,6 kW (100 cv). O equipamento é de arrasto, constituído por comando hidráulico, cabeçalho com luva telescópica para regulagem longitudinal, duas seções dispostas lateralmente, contando com 28 lâminas em cada uma delas, lastros de concreto, rodas de transporte e rolo destorroador. O trabalho foi conduzido no Departamento de Engenharia Rural da UNESP -Jaboticabal, em delineamento em blocos casualizados, no esquema fatorial 3 x 3,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Força de tração; Velocidade de deslocamento; Consumo de combustível.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100009

Tarifa binômia para o custo de água pressurizada em perímetros irrigados
Provedor de dados: 70
Autores: Ribeiro,Marcos C.; Oliveira Filho,Delly; Soares,Antônio A.; Martins,José H.; Mantovani,Everardo C.
Nos distritos de irrigação, a tarifa de custo variável tem dependido exclusivamente da quantidade de água consumida e não, da energia e da demanda de potência elétrica para o fornecimento de água na pressão e na vazão recomendadas pelo sistema de irrigação. Essa forma de tarifação da água de irrigação é um contrassenso em que os irrigantes mais eficientes subsidiam os irrigantes menos eficientes. Este trabalho propõe que as tarifas de água considerem não somente a quantidade de água consumida no mês, mas também a pressão, já que a demanda de potência hidráulica é função do produto da vazão pela pressão de serviço. O estudo comparou o custo de água de irrigantes que consomem o mesmo volume mensal para a situação atual e pela metodologia proposta....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tarifa; Distribuição de água; Perímetro irrigado.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400002

Avaliação da transmissão de dados de temperatura no sistema 1-wireTM
Provedor de dados: 70
Autores: Steidle Neto,Antonio J.; Baêta,Fernando C.; Martins,José H.; Zolnier,Sérgio; Monteiro,Paulo M. B.
A necessidade de sistemas de monitoramento automático versáteis e de baixo custo que possam auxiliar o produtor agrícola na otimização dos processos produtivos, é evidente. Este trabalho foi realizado com o objetivo de pesquisar as limitações e as potencialidades de aplicação do sistema 1-wireTM na transmissão de dados de temperatura em instalações agrícolas. O sistema 1-wireTM é uma rede de transmissão de dados que possibilita a comunicação digital entre um computador e dispositivos da série 1-wireTM, tais como os sensores de temperatura DS1820. A transmissão de dados de temperatura nesse sistema foi avaliada em função do tipo dos condutores e do número de sensores DS1820. Com base nos resultados, concluiu-se que o aumento do número de sensores de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas de aquisição de dados; Sensores de temperatura; Instalações agrícolas.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100004

SOIL PHYSICAL ATTRIBUTES BEFORE AND AFTER MANAGEMENT UNDER SOWING FORWARD SPEED
Provedor de dados: 70
Autores: Cortez,Jorge W.; Armando,Egas J.; Motomiya,Anamari Viegas de A.; Rodrigues,Sonia A.; Gonçalves,Eduardo A.
ABSTRACT The soil management system affects physical attributes, and the forward sowing speed can increase or decrease its results. Thus, this work aimed to evaluate management systems before and after soil mobilisation and forward sowing speed on soil physical attributes. Thus, an experiment was conduct in a completely randomized block design with four replications and six soil management systems: no tillage (NT), medium harrowing (MH), subsoiling operation (S), subsoiling and medium harrowing operations (S+MH), cross-subsoiling and medium harrowing (S+MH), and ploughing and two medium harrowing (P+2MH), and four forward sowing speeds: 3.1, 5.1, 5.8, and 7.9 km h−1, applied in the subplots. Soil management affects soil penetration resistance (PR) values,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Subsoiling; Conventional tillage; No-tillage.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500607

Espacialização da precipitação e erosividade na Bacia Hidrográfica do Rio Dourados - MS
Provedor de dados: 70
Autores: Arai,Fabiane K.; Gonçalves,Geula G. G.; Pereira,Silvio B.; Comunello,Éder; Vitorino,Antônio C. T.; Daniel,Omar.
A distribuição da precipitação numa bacia hidrográfica durante o ano é um dos fatores determinantes para quantificar a necessidade de irrigação de culturas e de abastecimento de água doméstico e industrial, além de estudos para o controle de inundações e da erosão do solo. O potencial da chuva em causar erosão hídrica pode ser avaliado por meio de índices que se baseiam nas características físicas das chuvas de cada região, entre os quais se destacam índice de erosividade. Analisaram-se, neste trabalho, a espacialização da precipitação pluvial e o índice de erosividade médio anual e mensal na Bacia Hidrográfica do Rio Dourados. Analisando os resultados obtidos, foi possível concluir que: o regime de precipitação apresenta oscilação unimodal, com período...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precipitação média; Índice de erosividade; Perda de solo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500014

REPRODUCTIVE EFFICIENCY AND BEHAVIOR OF PREGNANT SOWS HOUSED IN CAGES AND COLLECTIVE PENS WITH OR WITHOUT BEDDING
Provedor de dados: 70
Autores: Zotti,Maria L. A. N.; Miranda,Késia O. da S.; Vieira,Afrânio M. C.; Demsk,Joana B.; Romano,Gislaine G.
ABSTRACT This study aimed to evaluate the effect of wood shaving bedding on pregnant sows under two housing conditions. Sixty-four animals were distributed into four treatments, each treatment included 54 sows split into three replicates. A 2 × 2 factorial design was used (two types of housing, collective pens (CP) and combined housing (cages + CP [CCP]); and two types of floor, concrete floor without wood shavings (CFWS-) and concrete floor with wood shavings (CFWS+), allowing establishing the following treatment combinations: CP+CFWS+, CP+CFWS-, CCP+CFWS+, and CCP+CFWS-. Animal behavior, body injuries, reproductive efficiency, and abiotic variables were evaluated. The sows kept on wood shaving bedding presented a higher frequency of standing postures...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal welfare; Environmental enrichment; Pigs.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200166

Condutância estomática em folhas de feijoeiro submetido a diferentes regimes de irrigação
Provedor de dados: 70
Autores: Paiva,Auricleia S.; Fernandes,Edemo J.; Rodrigues,Teresinha J. D.; Turco,José E. P.
O controle estomático é importante propriedade fisiológica por meio da qual as plantas limitam a perda de água, ocasionando reduções na condutância estomática e, geralmente, reduzindo as trocas gasosas como forma de resposta das plantas a diversos fatores, incluindo o estresse hídrico. O objetivo deste trabalho foi determinar a condutância estomática em folhas de feijoeiro submetido a diferentes regimes de irrigação. O experimento foi conduzido no Departamento de Engenharia Rural da Faculdade de Ciências Agrárias e Veterinárias de Jaboticabal - SP. As irrigações nos tratamentos foram determinadas em função do esgotamento de água no solo: T1 - irrigado quando esse atingiu 40% da capacidade de água disponível (CAD); T2 - quando atingiu 60% da CAD; T3 -...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Estresse hídrico; Água no solo; Phaseolus vulgaris L.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100018

Isolation of microorganisms of cheese whey with lipolytic activity for removal of COD
Provedor de dados: 70
Autores: Hermes,Eliane; Rocha,Dayane C. da; Orssatto,Fábio; Lucas,Juliana F.R.; Gomes,Simone D.; Sene,Luciane.
The aim of this study was to isolate microorganisms that produce lipase and to assess the efficiency of COD removal intreatment of cheese whey under different operating conditions. The microorganisms were isolated from cheese whey and a commercial product; it was selectedthreemicroorganisms that obtained the best response to the lipolytic activity test through the enzyme index. Then, the microorganisms were inoculated in sterilized cheese whey samples, for two pH values (6.2 and 7.0), incubated at 35 °C and 150 rpm in shaker and the lipolityc activity and the efficiency of COD removal were measured in two time periods (24 and 48h). After incubation, it was observed that the treatments showed a good removal efficiency of COD for the pre-treatment and the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Waste treatment; Dairy industry; Lipases.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200016

Soil water evaporation under densities of coverage with vegetable residue
Provedor de dados: 70
Autores: Gava,Ricardo; Freitas,Paulo S. L. de; Faria,Rogério T. de; Rezende,Roberto; Frizzone,José A.
This study was conducted at the Agronomic Institute of Paraná (IAPAR) in Londrina, State of Paraná (PR), Brazil (latitude 23º18'S, longitude 51º09'W and average altitude of 585 m). The local climate, according to the classification of Köeppen, is Cfa type, i.e., humid subtropical climate, with rain in all seasons and can occur dry seasons during the winter. It was determined soil evaporation (E) under different coverage densities with residue from the wheat crop. The treatments were installed in weighting lysimeters of 2.66 m² and 1.3 m deep, which allows to determine E by the mass difference with measuring precision of 0.1mm at one hour intervals. Treatments consisted of 0; 2.5; 5 and 10 t ha-1 of wheat crop residues, placed evenly over each lysimeter. In...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wheat straw; Soil coverage; Water losses.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100010

EFFECT OF DRYING METHODS ON CRAMBE (Crambe abyssinica HOCHST) SEED COAT PIGMENTATION AND ON OIL AND BIODIESEL QUALITY
Provedor de dados: 70
Autores: Silva,Magnun A. P. Da; Biaggioni,Marco A. M.; Sperotto,Felipe C. S.; Macedo,Ana C.; Brandão,Fernando J. B.
ABSTRACT The objective of this study was to evaluate the effect of different drying methods on seed coat pigmentation and quality of oil and biodiesel extracted from crambe. The experimental design was completely randomized with five treatments and four replications, totaling 20 plots. The treatments consisted of drying with heated air, natural air, ground, in the shade and in the plant. Physical and chemical analyzes were performed to verify the quality of grain, oil and biodiesel. The largest amounts of chlorophyll a and b and green beans and the lowest oil content were found in artificial drying with heated air. It was concluded that the drying in the plant presented grains and oil of better quality, but do not interfering in the quality of biodiesel,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chlorophyll; Biofuels; Oilseed.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601167

Avaliação de meios filtrantes primários em filtro contínuo de tambor rotativo a vácuo para lodo de caldo de cana
Provedor de dados: 70
Autores: Polonio,Walter L.; Gonçalves,Eliete M.; Razuk,Paulo C.
Este estudo teve o objetivo de avaliar o comportamento de treze tipos de meios filtrantes primários desenvolvidos para uso na filtração a vácuo de lodo de caldo de cana, simulando as operações de formação e desidratação da torta em filtros contínuos de tambor rotativo a vácuo, empregados nas indústrias de açúcar e álcool do Brasil. Para tanto, foi desenvolvida uma planta-piloto anexa ao filtro de tambor rotativo a vácuo, na qual foram realizados todos os ensaios, com o objetivo de refletir a realidade das variáveis operacionais durante uma safra sucroalcooleira. Os resultados são apresentados, comparando-se as taxas de filtração, variando a pressão de formação da torta, temperatura e concentração de auxiliar filtrante, mostrando ao usuário um novo caminho...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chapa perfurada; Filtração a vácuo; Indústria sucroalcooleira.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100019

Application of fuzzy logic for the evaluation of livestock slaughtering
Provedor de dados: 70
Autores: Gabriel Filho,Luís R. A.; Cremasco,Camila P.; Putti,Fernando F.; Chacur,Marcelo G. M.
The fuzzy logic admits infinite intermediate logical values between false and true. With this principle, it developed in this study a system based on fuzzy rules, which indicates the body mass index of ruminant animals in order to obtain the best time to slaughter. The controller developed has as input the variables weight and height, and as output a new body mass index, called Fuzzy Body Mass Index (Fuzzy BMI), which may serve as a detection system at the time of livestock slaughtering, comparing one another by the linguistic variables "Very Low", "Low", "Average ", "High" and "Very High". For demonstrating the use application of this fuzzy system, an analysis was made with 147 Nellore beeves to determine Fuzzy BMI values for each animal and indicate the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Corporal index; Controlling mass fuzzy; Quantitative method.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400019

Image analysis for assessing broiler breeder behavior response to thermal environment
Provedor de dados: 70
Autores: Nääs,Irenilza de A.; Laganá,Marcus; Mollo Neto,Mario; Canuto,Simone; Pereira,Danilo F.
The research proposes a methodology for assessing broiler breeder response to changes in rearing thermal environment. The continuous video recording of a flock analyzed may offer compelling evidences of thermal comfort, as well as other indications of welfare. An algorithm for classifying specific broiler breeder behavior was developed. Videos were recorded over three boxes where 30 breeders were reared. The boxes were mounted inside an environmental chamber were ambient temperature varied from cold to hot. Digital images were processed based on the number of pixels, according to their light intensity variation and binary contrast allowing a sequence of behaviors related to welfare. The system used the default of x, y coordinates, where x represents the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal welfare; Image processing; Clusters analysis.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400001

Seeder-fertilizer machine: energetic demand as a function of vegetal covering handling and manure deposition shank depth in no-tillage system
Provedor de dados: 70
Autores: Grotta,Danilo C. C.; Furlani,Carlos E. A.; Silva,Rouverson P. da; Lopes,Afonso; Reis,Gustavo N. dos.
The purpose of this work was evaluating the energetic demand of a seeder-fertilizer machine as a function of the type and handling of vegetal covering culture and of the fertilizer deposition shank depth. A Valtra BM100 tractor was used implemented to pull a high precision seeder-fertilizer machine with four ranks of seeding, spaced 0.9 m for maize culture. Experiment was conducted with design in randomized blocks in factorial plots, in the Laboratory of Machines and Agricultural Mechanization experimental area (LAMMA) of UNESP-Jaboticabal, using two covering cultures (black-mucuna and crotalaria), three handlings of this covering, two mechanical (straw crusher and roller knife) and one chemical (pulverization of herbicide), performed 120 days after...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuel consumption; Knife roller; Traction force.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200007

Profundidade de deposição de semente de milho na região dos Campos Gerais, Paraná
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Schimandeiro,Adriana; Gimenez,Leandro M.; Colet,Marcelo J.; Garbuio,Paulo W.
O sistema plantio direto encontra-se hoje plenamente incorporado à região dos Campos Gerais no Paraná. A acurácia e a precisão no processo de semeadura são itens de grande importância para que tal sistema alcance sucesso. Sendo assim, foram selecionadas 50 propriedades e, em 38, determinou-se a profundidade de deposição da semente de milho. A área experimental era formada por quatro ou cinco linhas de semeadura, onde se avaliaram dez plântulas por linha. A profundidade ficou em torno de 46 mm, observando-se diferenças significativas entre as linhas, em 21 áreas. O coeficiente de variação médio ficou em torno de 20%, limite estatístico entre médio e alto. Conforme análise de outros parâmetros, tais coeficientes podem representar diferentes tipos de erro no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantio direto; Processo de semeadura; Mecanização agrícola.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400022

Estimativa da condutividade elétrica da solução do solo a partir do teor de água e da condutividade elétrica aparente do solo
Provedor de dados: 70
Autores: Santana,Gessionei da S.; Coelho,Eugênio F.; Silva,Tibério S. M. da; Ramos,Márcio M.
O crescente uso da técnica de fertirrigação não tem sido acompanhado com pesquisas para disponibilizar informações capazes de proporcionar o correto manejo dessa técnica. A reflectometria no domínio do tempo (TDR) possibilita o monitoramento simultâneo e contínuo do teor de água (teta) e da condutividade elétrica aparente do solo (CEa). A literatura apresenta diversos modelos que relacionam teta e CEa com a condutividade elétrica da solução do solo (CEw), com vistas à predição da CEw a partir de dados de teta e CEa obtidos por meio da técnica da TDR. Porém, muitas pesquisas demonstram a necessidade de avaliação e calibração desses modelos para solos de diferentes classes texturais. Neste trabalho, foram avaliados seis modelos com o objetivo de conhecer a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: TDR; Modelos matemáticos; Manejo de fertirrigação.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300003

INTEGRATED ENVIRONMENTAL FOOTPRINT INDEX (IEFI): MODEL DEVELOPMENT AND VALIDATION
Provedor de dados: 70
Autores: Silva,Vicente De P. R. Da; Aleixo,Danilo De O.; Campos,João H. B. Da C.; Araújo,Lincoln E.; Souza,Enio P.
ABSTRACT: Freshwater is a valuable resource worldwide given the growing demand of the global population. This study aimed to develop and validate an integrated assessment model by means of environmental footprint indices (water, ecological, and carbon), which measure the environmental sustainability of heterogeneous communities, people, and countries. An environmental footprint was firstly defined as a set of indicators to track human pressure on planet Earth under different angles, being a multidimensional index of environmental sustainability. A Delphi survey was used to bring together opinions from a diverse set of experts. The participants of this study consisted of 120 experts from several fields of knowledge belonging to the best-known research and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water footprint; CO2 emissions; Natural resources.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500918

COMPOSTING TIME REDUCTION OF AGRO-INDUSTRIAL WASTES
Provedor de dados: 70
Autores: Costa,Mônica S. S. De M.; Carneiro,Leocir J.; Costa,Luiz A. De M.; Pereira,Dercio C.; Lorin,Higor E. F.
ABSTRACT The agro-industrialization of animal products has led to a significant waste generation, which has been stabilized by composting process in specialized plants. Waste stabilization time on composting depends on the handling used. 12 treatments were performed, three frequency turnings combined with two environmental conditions (with and without coverage of the composting area) and with and without commercial inoculant, whose results were submitted to multiple regression analysis. Windrows turned twice a week in the first month had adequate temperature control and stabilization time of 83.5 and 95.5 days for uncovered and covered windrows, respectively. Uncovered windrows have accelerated the process in 10 days on average, with the disadvantage of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environmental conditions; Inoculation; Turnings.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601206

Compactação de solos cultivados com cana-de-açúcar: II -quantificação das restrições às funções edáficas do solo em decorrência da compactação prejudicial
Provedor de dados: 70
Autores: Severiano,Eduardo da C.; Oliveira,Geraldo c. de; Dias Júnior,Moacir de S.; Castro,Matheus B. de; Oliveira,Luiz F. C. de; Costa,Katia A. de P.
A redução do período de entressafra canavieiro pode levar à disseminação da compactação do solo, em decorrência da colheita mecanizada da cana-de-açúcar na estação chuvosa. Dessa forma, faz-se necessário definir estratégias que visem a minimizar a esse processo. O presente estudo objetivou modelar o processo de compressão do solo com base na pressão crítica. Avaliou também os efeitos da colheita mecanizada da cana-de-açúcar em diferentes épocas da safra em um Latossolo Vermelho-Amarelo (LVA) e em um Cambissolo Háplico (CX). Determinaram-se em amostras indeformadas a macroporosidade do solo, a pressão de preconsolidação em diferentes conteúdos de água no solo e a densidade do solo. A partir da incorporação da densidade do solo crítica na modelagem do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum sp.; Degradação estrutural; Pressão crítica; Colheita mecanizada de cana-de-açúcar.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300006

Resistência à compressão e remoção de folhas da cana-de-açúcar visando à colheita mecânica
Provedor de dados: 70
Autores: Magalhães,Paulo S. G.; Braunbeck,Oscar A.; Pagnano,Natasha B.
A cultura de cana-de-açúcar ocupa um papel importante na economia brasileira, sendo sua colheita ainda em grande parte realizada manualmente, pelo método tradicional de colheita de cana-de-açúcar inteira. As colhedoras existentes no mercado adotaram uma tecnologia de picar a cana-de-açúcar em rebolos de 200 a 300 mm, para permitir sua transferência para o veículo de transporte que acompanha a colhedora, contradizendo o método tradicional de colheita. Para viabilizar a colheita mecânica de cana-de-açúcar inteira, uma das barreiras tecnológicas a ser vencida é a remoção da palha mecanicamente. Projetar um mecanismo que realize essa operação depende diretamente do conhecimento de propriedades mecânicas da cana-de-açúcar. Este trabalho teve por objetivo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Propriedades mecânicas; Saccharum officinarum; Cana crua.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100020

CAN BASAL CUTTING BLADE WEAR AFFECT SUGARCANE REGROWTH?
Provedor de dados: 70
Autores: Bernache,Leonardo; Tedesco-Oliveira,Danilo; Oliveira,Luan P. de; Corrêa,Ligia N.; Silva,Rouverson P. da.
ABSTRACT Sugarcane harvester cutting blade wear increases ratoon damages and losses, impairing sugarcane regrowth. This study aimed to evaluate the quality of basal cut using ratoon damage and loss indexes and correlating them with effects on sugarcane regrowth. Harvest parameters such as plant height and position, damage and loss indexes, and stem length were evaluated every 30 min, following statistical process control (SPC) assumptions. Blade wear was examined during three harvesting shifts (0-8 h, 8-16 h, and 16-24 h). Sugarcane regrowth was assessed by counting number of tillers and measuring plant height and stem diameter. The second harvesting shift showed better quality in terms of damage and loss indexes, and plant height and stem diameter....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mechanized harvesting; Sugarcane; SPC; Harvester.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100053

Índice geométrico e perda de carga localizada em conexões de emissores "online"
Provedor de dados: 70
Autores: Cardoso,Gabriel G. de G.; Klar,Antônio E.
O objetivo deste artigo é apresentar um estudo envolvendo uma relação entre a perda de carga localizada em conexões de emissores em tubulações, com diferentes diâmetros, utilizados em irrigação localizada, com a geometria dos conectores de emissores "online", que permite a fácil quantificação dessas perdas de carga, uma vez conhecida a dimensão dos conectores. O experimento foi conduzido para Números de Reynolds no intervalo de fluxo turbulento, obtidos pela variação da vazão nos tubos a uma temperatura constante da água. Para os tubos considerados, os resultados da investigação indicaram que o fator de atrito da equação de Darcy-Weisbach pode ser estimado pela Equação de Blasius com os coeficientes b = 0,300 e m = 0,25 para a determinação da perda de...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Perda de carga localizada; Equação de Blasius; Número de Reynolds.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600008

WIND EFFECTS ON FOUNDATIONS OF SILOS AND LIGHT STRUCTURES: SOLUTION BY USE OF STEEL PILES IN DIABASIC SOIL
Provedor de dados: 70
Autores: Carvalho,David de; Fujii,Armando K.; Paschoalin Filho,João A.; Cury Filho,Dirney; Silva,Marccella B. M.
ABSTRACT Wind solicitations generate horizontal, tensile, and compressive stresses on building foundations. In empty light structures, such as agricultural greenhouses and, in the specific case of silos and elevated structures such as metal water tanks, the consideration of these loads becomes important because the lack of the weight component due to the storage load significantly influences the balance of forces. This study focused on the behavior of metallic steel profiles, aiming at its application as a foundation element for the pile, considering the soil of Diabasic origin common to the Center-South region of Brazil. Load tests in real scale were carried out on three steel profiles, type I, gauge W 250 mm x 32.7 kg m-1, drilled in the ground up to 12m...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Foundations; Piles; Wind effect; Light structures; Load tests; Diabasic soil.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300370

COMPARISON OF ARROWROOT (Maranta arundinacea) AND CASSAVA STARCH EXTRACTION IN SEPARATION, CONCENTRATION, AND PURIFICATION USING A ROTATING SIEVE UNDER WATER
Provedor de dados: 70
Autores: Fabiano,P. Branco; Marney,P. Cereda; Marco,H. Naka.
ABSTRACT Brazil is home to several plant species that exhibit potential for starch extraction. The arrowroot plant stands out owing to its South American origin. Arrowroot starch is especially important for fine confectionery, which is a high-value niche market. Thus, a small producer could benefit from the high prices of arrowroot starch. However, to have consistent production, the extraction should be performed using simple, safe, and inexpensive equipment. Starch extraction involves disintegration of the raw material under water, followed by the separation of fibrous bagasse from the starch–water suspension. This study presents an equipment design based on the concept of appropriate technology that is suitable for small producers to extract starch. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Efficiency; Yield; Machine project; Water consumption; Granulometry.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100090

Estado térmico de produtos armazenados em silos com sistema de aeração: estudo teórico e experimental
Provedor de dados: 70
Autores: Oliveira,Fabiane A. de; Khatchatourian,Oleg A.; Bihain,Anderson.
O resfriamento de grãos por ventilação de ar ambiente aplica-se amplamente nas etapas finais de secagem e para controle posterior da temperatura de grãos armazenados. O objetivo deste trabalho é realizar estudo teórico-experimental sobre o estado térmico de massa de grãos de soja sujeita à aeração. Foram obtidos dados experimentais sobre a dinâmica de resfriamento de massa pré-aquecida de grãos de soja para diferentes alturas da coluna de grãos e velocidades do ar. A análise dos resultados mostrou que a taxa de resfriamento varia significativamente durante todo o processo e em todo o domínio e a difusividade térmica das camadas não poderia ser considerada constante. Para simular a dinâmica de resfriamento, foram apresentados dois modelos matemáticos. No...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Armazenamento; Aeração; Resfriamento.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100019

Avaliação de parâmetros da biodigestão anaeróbia de dejetos de suínos alimentados com dietas à base de milho e sorgo
Provedor de dados: 70
Autores: Orrico Júnior,Marco A. P.; Orrico,Ana C. A.; Lucas Júnior,Jorge De.
O objetivo deste trabalho foi avaliar a interferência da dieta à base de sorgo em substituição à de milho na composição e no tratamento dos dejetos. Foram utilizados 24 biodigestores batelada de bancada, dos quais 12 foram abastecidos com dejetos de suínos alimentados com dieta á base de milho, e o restante, com dieta á base de sorgo. A cada 30 dias foram esvaziados três biodigestores dentro de cada dieta, em um total de quatro tempos de retenção hidráulica (TRH) 30; 60; 90 e 120 dias. Para avaliar a eficiência do processo de biodigestão anaeróbia, foram avaliadas as reduções de sólidos totais, sólidos voláteis totais, demanda química de oxigênio, demanda bioquímica de oxigênio, número mais provável (NMP) de coliformes totais e termotolerantes, além dos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Suinocultura; Tanino; Metano; Coliformes.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400004

MULTICRITERIA DECISION AID TO IMPLEMENT AN ON-FARM STORAGE SYSTEM FOR SOYBEANS
Provedor de dados: 70
Autores: Bocca,Lucas S.; Galves,Maria L.
ABSTRACT: Implementing an on-farm storage system for agricultural products becomes a complex decision problem when considering risks, benefits, uncertainties and alternatives. This study aimed at applying the multicriteria decision aid (MCDA) approach to select the infrastructure to be implemented, taking into account variables and farmer's goals. As a result, we concluded that the adopted approach was useful since it allowed a better understanding of the problem and provided decision-making support.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Grain storage; Investment; Multicriteria decision aid.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601250

Qualidade de aplicação de herbicida em lavoura de trigo
Provedor de dados: 70
Autores: Suguisawa,Jorge M.; Franco,Fabiana N.; Silva,Saulo S. S.; Peche Filho,Afonso.
O objetivo deste trabalho foi analisar a operação de aplicação de herbicida em lavoura de trigo utilizando ferramentas estatísticas da qualidade e tecnologia de sistema de informação geográfica, sendo os dados coletados em propriedade agrícola situada no Paraná. Foram considerados dois indicadores: percentagem de cobertura de gotas e densidade de gotas. Foram utilizadas, para avaliação dos resultados, técnicas da estatística descritiva, de controle de qualidade e do sistema de informação geográfica. Os resultados mostram que o processo de aplicação de defensivo avaliado apresenta irregularidade e grande variabilidade, necessitando de melhorias. Entretanto, tendo em vista a característica dos produtos utilizados (sistêmicos), pode-se considerar como...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avaliação; Pulverização; Variabilidade.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200007

Estudo cinético da remoção de matéria orgânica de águas residuárias da suinocultura em sistemas alagados construídos cultivados com diferentes espécies de vegetais
Provedor de dados: 70
Autores: Matos,Antonio T. de; Freitas,Wallisson da S; Borges,Alisson C.
Com a realização deste estudo, teve-se o objetivo de obter valores dos coeficientes de remoção da matéria orgânica de águas residuárias da suinocultura (ARS), quando em tratamento em sistemas alagados, construídos (SACs) e cultivados com diferentes espécies vegetais e em condições climáticas tropicais. Em tanques de 24,0 x 1,1 x 0,7 m, impermeabilizados com lona de PVC e preenchidos com uma camada de 0,4 m de brita zero (altura útil), foram plantados taboa (SAC1), tripa-de-sapo (SAC2) e capim-tifton 85 (SAC3). No SAC4 (multivegetado), foi plantado, no primeiro terço, tripa-de-sapo; no segundo terço, taboa, e no último terço, capim-tifton 85. A ARS foi previamente tratada em filtros orgânicos constituídos por bagaço de cana-de-açúcar, sendo aplicada numa...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Efluentes suinícolas; Zona de raízes; Cinética de remoção; Fitorremediação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600015

Eficiência no uso da água na cana-de-açúcar sob diferentes lâminas de irrigação e níveis de zinco no litoral paraibano
Provedor de dados: 70
Autores: Farias,Carlos H. A.; Fernandes,Pedro D.; Dantas Neto,José; Gheyi,Hans R.
Esta pesquisa foi conduzida em área experimental da Fazenda Capim II, localizada no Município de Capim - PB, com o intuito de determinar a eficiência no uso da água (EUA) pela cana-de-açúcar (Saccharum officinarum L.), cultivar SP 79-1011. O delineamento experimental consistiu em blocos casualizados, com três repetições, em esquema fatorial 5 x 5. Os tratamentos referentes à lâmina de irrigação foram: sequeiro; 25; 50; 75 e 100% da ETc (1.026,57 mm) com as respectivas precipitações efetivas de 780,06; 713,31; 487,54; 243,71 e 194,51 mm; os níveis de zinco estudados foram 0; 1; 2; 3 e 4 kg ha-1. O equipamento de irrigação utilizado foi do tipo pivô central, com turno de rega de nove dias. A eficiência no uso da água (EUA) na produção de colmos e de açúcar...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum officinarum; Otimização; Zinco; Evapotranspiração.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300010

HYBRID SOLAR HEAT PUMP SYSTEM FOR WATER HEATING
Provedor de dados: 70
Autores: Jordan,Rodrigo A.; Yamasaki,Johnny T.; Silveira Júnior,Vivaldo; Dória,Eduardo C. B.
ABSTRACT A comparative test of water heating between the hybrid system - solar collector with heat pump - and a system with conventional supplementary heating - with high electric power - was performed. For this, a small capacity heat pump was installed, which was later installed together with a solar heating system, composed of a 250 L thermal reservoir and three thermoplastic collector plates. Tests were carried out to evaluate the COP of the heat pump and the energy consumption of the solar heating system operating with the heat pump and with an electrical resistance of 3000 W. In the laboratory tests, the heat pump presented an average COP of 2.15. In the field tests, the energy consumption of the solar system with heat pump was 54.9% lower when...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Heat pump; Solar collector; Thermal energy.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400419

Perda de carga em microtubos e conectores utilizados em microaspersão
Provedor de dados: 70
Autores: Zitterell,Danieli B.; Frizzone,José A.; Rettore Neto,Osvaldo; Ullmann,Mario N.
Este trabalho foi desenvolvido com o objetivo de ajustar equações que estimam a perda distribuída de carga em microtubos utilizados em microaspersão e a perda localizada de carga na passagem lateral do fluxo por meio dos conectores na linha lateral. A perda distribuída de carga foi determinada em quatro diâmetros de microtubos com nove a dez repetições para 15 vazões, por meio da aplicação do teorema de Bernoulli. O fator de atrito (f) foi estimado fixando-se o valor de m = 0,25 e calibrando-se o valor do parâmetro c (0,290). A perda localizada de carga foi determinada por diferença entre perda de carga no microtubo mais conector e perda de carga no microtubo. Dois modelos de conectores foram utilizados e caracterizados quanto ao diâmetro interno e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Perda localizada de carga; Perda distribuída de carga; Comprimento equivalente; Coeficiente de carga cinética.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400009

Qualidade da água para irrigação de um córrego após receber efluente tratado de abate bovino
Provedor de dados: 70
Autores: Thebaldi,Michael S.; Sandri,Delvio; Felisberto,Alberto B.; Rocha,Marco S. da; Avelino Neto,Sebastião.
A qualidade da água de irrigação é de fundamental importância para não comprometer a qualidade dos produtos e o funcionamento dos equipamentos de irrigação, especialmente quando são diluídos outros compostos. O objetivo deste trabalho foi avaliar a influência do lançamento de efluente de abate de bovinos tratado sobre a qualidade da água para fins de irrigação do Córrego Jurubatuba, Anápolis-GO. As amostras de efluente e água foram obtidas em seis diferentes dias e nos seguintes locais: na descarga do efluente tratado antes do lançamento no córrego -P1, 50 m a montante do ponto de descarga -P2, 50 m a jusante do ponto de descarga -P3 e 120 m a jusante do ponto de descarga -P4. Analisaram-se os sólidos dissolvidos, pH, ferro, dureza, sódio, cálcio,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reúso da água; Entupimento de emissores; Toxicidade.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100012

Utilização da TDR para monitoramento da solução de nitrato de potássio em Latossolo Vermelho-Amarelo
Provedor de dados: 70
Autores: Lopes,Leonardo do N.; Souza,Claudinei F.; Santoro,Bruno de L.
O conhecimento da distribuição e armazenamento da solução no solo é de grande importância para a agricultura, pois a interação entre os nutrientes e a água é um dos fatores que influenciam diretamente no rendimento das culturas. Das várias técnicas utilizadas para o monitoramento da solução no solo, a reflectometria no domínio do tempo (TDR) vem sendo bastante difundida entre os pesquisadores por apresentar inúmeras vantagens, dentre as quais a mensuração em tempo real e a possibilidade de leituras automatizadas. O principal objetivo desta pesquisa foi avaliar a distribuição da solução de KNO3 no perfil de um Latossolo Vermelho-Amarelo. Sondas de Reflectometria no Domínio do Tempo (TDR) foram utilizadas para monitorar a distribuição de solução no solo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reflectometria no domínio do tempo; Umidade do solo; Condutividade elétrica do solo; Volume de solo molhado.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500015

Probabilistic structure of an annual extreme rainfall series of a coastal area of the State of São Paulo, Brazil
Provedor de dados: 70
Autores: Blain,Gabriel C.; Camargo,Marcelo B. P. de.
This study aimed to describe the probabilistic structure of the annual series of extreme daily rainfall (Preabs), available from the weather station of Ubatuba, State of São Paulo, Brazil (1935-2009), by using the general distribution of extreme value (GEV). The autocorrelation function, the Mann-Kendall test, and the wavelet analysis were used in order to evaluate the presence of serial correlations, trends, and periodical components. Considering the results obtained using these three statistical methods, it was possible to assume the hypothesis that this temporal series is free from persistence, trends, and periodicals components. Based on quantitative and qualitative adhesion tests, it was found that the GEV may be used in order to quantify the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Extreme values; Adhesion tests; Time series.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300014

Mathematical analysis of maximum power generated by photovoltaic systems and fitting curves for standard test conditions
Provedor de dados: 70
Autores: Gabriel Filho,Luís R. A.; Viais Neto,Daniel dos S.; Cremasco,Camila P.; Seraphim,Odivaldo J.; Caneppele,Fernando de L.
The rural electrification is characterized by geographical dispersion of the population, low consumption, high investment by consumers and high cost. Moreover, solar radiation constitutes an inexhaustible source of energy and in its conversion into electricity photovoltaic panels are used. In this study, equations were adjusted to field conditions presented by the manufacturer for current and power of small photovoltaic systems. The mathematical analysis was performed on the photovoltaic rural system I-100 from ISOFOTON, with power 300 Wp, located at the Experimental Farm Lageado of FCA/UNESP. For the development of such equations, the circuitry of photovoltaic cells has been studied to apply iterative numerical methods for the determination of electrical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Rural electrification; Photovoltaic cells; Numerical methods.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400004

Análise econômica baseada em funções de resposta da produtividade versus lâminas de água para o mamoeiro no Norte Fluminense
Provedor de dados: 70
Autores: Almeida,Frederico T. de; Bernardo,Salassier; Sousa,Elias F. de; Marin,Sérgio L. D.; Grippa,Sidney.
A potencialidade de um pólo de fruticultura irrigada no Norte Fluminense é enorme, dada a região apresentar muitas vantagens. Entretanto, a viabilidade de um sistema de produção dependerá do adequado manejo do mesmo, carecendo de análises econômicas dos insumos aplicados e dos resultados obtidos para estabelecer uma diretriz. Baseado nessas premissas, o objetivo deste trabalho foi avaliar o manejo da água a aplicar por meio de análises econômicas das funções de resposta (água x produção) e, ainda, considerando os diferentes mercados a atingir, nacional e internacional. Foi montado um experimento com diferentes lâminas de irrigação na cultura do mamão, com a cultivar "Improved Sunrise Solo 72/12", plantada em fileiras duplas, com espaçamento 3,6 x 2,0 x 2,0...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Análise econômica; Manejo de irrigação; Mamão.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300019

Identification of grain areas replaced by sugarcane and analysis of the relationship with family farming production in the state of Goiás
Provedor de dados: 70
Autores: Petrini,Maria A.; Rocha,Jansle V.
In Brazil, the State of Goiás is one of sugarcane expansion's frontiers to meet the growing demand for biofuels. The objective of this study was to identify the municipalities where there were replacement of annual crops (mainly grains) by sugarcane in the state of Goiás, as well as indicate correlations between the sugarcane expansion and the family farming production, in the period between 2005 and 2010. For this purpose, grains crop mask and sugarcane crop mask, obtained from satellite images, were intersected using geoprocessing techniques. It was also used IBGE data of sugarcane production and planted area, and data of family farming production linked with the National Food Acquisition Program (PAA), in relation to the number of cooperatives and...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Geoprocessing; Ethanol; National Food Acquisition Program (PAA).
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600023

Influência da pressão interna dos pneus e da velocidade de deslocamento nos parâmetros operacionais de um trator agrícola e nas propriedades físicas do solo
Provedor de dados: 70
Autores: FEITOSA,JARDÊNIA R.; FERNANDES,HAROLDO C.; TEIXEIRA,MAURI M.; CECON,PAULO R.
O tráfego intenso de tratores ocasiona alterações na qualidade física do solo, desencadeando processos de compactação e erosão. O presente trabalho teve como objetivo avaliar a influência da alteração da pressão interna dos pneus e da velocidade de deslocamento de um trator agrícola 4 x 2 com tração dianteira auxiliar (TDA), em propriedades físicas de um solo usadas como parâmetros para a avaliação da compactação e em parâmetros operacionais do trator relacionados ao seu desempenho. Para tanto, foram determinadas a densidade do solo, a porosidade total e o índice de cone de amostras de solo coletadas antes e após a passagem do trator. Determinou-se, ainda, o avanço cinemático do trator, a patinagem dos rodados, a área de contato entre o pneu e o solo, e a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compactação; Densidade do solo; Patinagem dos rodados; Porosidade.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100117

Aplicação de métodos numéricos para estimativa de variáveis psicrométricas
Provedor de dados: 70
Autores: Miranda,Jarbas H. de; Angelocci,Luiz R.; Silva,Késia O. da; Duarte,Sergio N.; Villa Nova,Nilson A.
O ar atmosférico é formado por uma composição de ar seco e vapor d'água, cujos valores da quantidade de vapor, em termos quantitativos, são variáveis em função dos elementos climáticos, tais como: temperatura e pressão. Portanto, para estimar os valores de umidade relativa do ar, são necessárias informações completas de séries de dados de temperatura do ar (Tar), pressão atual de vapor (e a) e temperatura de bulbo úmido (Tu). O trabalho apresenta como objetivo a elaboração de rotina computacional para encontrar valores da temperatura do termômetro de bulbo úmido (Tu) em função de outras variáveis, para uma série de dados obtidos, mediante a aplicação de métodos numéricos (Método de Newton-Raphson e Método da Secante), para fins de complementação de uma...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Métodos numéricos; Temperatura de bulbo úmido; Umidade relativa.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300004

EFFECT OF HEIGHT, TILT AND TWIST ANGLES OF AN ACTIVE REFLECTANCE SENSOR ON NDVI MEASUREMENTS
Provedor de dados: 70
Autores: Stocker,Vinícius; Souza,Eduardo G. de; Johann,Jerry A.; Beneduzzi,Humberto M.; Silva,Franciléia de O. e.
ABSTRACT The application of nitrogen (N) fertilizer is complex and expensive, so its correct management has financial and environmental benefits. The use of optical proximity sensors is a promising technique. However, the movement of the agricultural machinery or of the person carrying the sensor will result in height differences and/or different tilt and twist angles with respect to the canopy. We considered whether these variations would affect the reflectance measurement. In this study, we took normalized difference vegetation index (NDVI) readings of a wheat canopy, to which 90 kg ha-1 of urea had been applied in stage 5, and observed the NDVI in stages 6, 8 and 10.5. We also tested soybeans, to which 90 kg ha-1 of urea had been applied in stage R1,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrogen fertilization; Precision agriculture; GreenSeeker; NDVI.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800096

EVALUATION OF THE Peltophorum vogelianum Benth. WOOD SPECIES FOR STRUCTURAL USE
Provedor de dados: 70
Autores: Christoforo,André L.; Aquino,Vinicius B. de M.; Wolenski,Anderson R. V.; Araujo,Victor A. De; Lahr,Francisco A. R.
ABSTRACT Wood is a material used for various purposes since ancient times and is mainly used in civil and rural construction and industry. Due to the predatory exploitation of known trees, it is necessary to characterize new species for use in urban and rural structures as alternatives of species commonly used. This study aimed to determine the physical and mechanical properties of Guarucaia wood (Peltophorum vogelianum Benth.) based on the Brazilian standard ABNT NBR 7190 (1997) and estimate the strength and stiffness as a function of apparent density using the analysis of variance and also estimate stiffness as a function of its strength. The mechanical properties of P. vogelianum were considered compatible for structural use when compared with others...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Peltophorum vogelianum; Characterization; Apparent density; Regression models; Analysis of variance (ANOVA).
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600763

Modelos estatísticos indicadores de comportamentos associados a bem-estar térmico para matrizes pesadas
Provedor de dados: 70
Autores: Salgado,Douglas D.; Nääs,Irenilza de A.; Pereira,Danilo F.; Moura,Daniella J. de.
O estudo de reprodutoras de frangos de corte é de grande importância para o País, uma vez que o frango de corte é um dos maiores itens agropecuários em exportação, sendo o Brasil o segundo maior exportador mundial dessa carne. O comportamento animal é conceituado como reflexo do efeito da interação de diversos fatores, entre os quais o ambiental. Dessa forma, o ambiente interno do galpão de produção constitui um dos elementos que fornecem indicações sobre o conforto térmico das aves. O comportamento de matrizes expressa, sob a forma de padrões específicos, a saúde e o bem-estar dessas aves. Este trabalho teve como objetivo a aplicação dos modelos estatísticos preditivos, por meio da construção de cenários, apresentando resultados do conforto animal perante...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avicultura; Bem-estar; Modelos estatísticos.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400004

Using an aerial system of remote sensing to detect different nutritional status in Brachiaria decumbens
Provedor de dados: 70
Autores: Silva Júnior,Mário C. da; Pinto,Francisco de A. De C.; Queiroz,Daniel M. de; Vieira,Luciano B.; Resende,Ricardo C. de.
The aim of this study was to use digital images acquired by cameras attached to a helium balloon to detect variation of the nutritional status in Brachiaria decumbens. The treatments consisted of five doses of nitrogen (0, 50, 100, 150 e 200kg ha-1) with six replications each, evaluated in a completely randomized statistical design. A remote sensing system composed of digital cameras and microcomputers was used for image acquisition, and a helium balloon lifted the cameras to the heights of 15, 20, 25 and 30m. A portable chlorophyll meter and analyses of leaf nitrogen content were used to make comparisons with data obtained by the remote sensing system. Data was acquired in two phases, in different climatic conditions. At the end of each phase, dry matter...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digital images; Vegetation indices; Nitrogen.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500016

Seedlings of Acrocomia aculeata in diferent substrates and protected environments
Provedor de dados: 70
Autores: Costa,Edilson; Martins,Roberta F.; Faria,Tatiane A. C.; Jorge,Marçal H. A.; Leal,Paulo A. M.
The seedling production stage is the key to achieve uniformity in tree breeding stage. This study evaluated "bocaiúva" (Acrocomia aculeata) seedling formation, with pre-germinated seeds in different substrates and protected environments, in the University of Mato Grosso do Sul State, Aquidauana, MS. As substrates, we used 100% cattle manure (M), 100% cassava branches (CB), 100% vermiculite (V), 50% cattle manure + 50% cassava branches, 50 % cattle manure + 50% vermiculite, 50% cassava branches + 50% vermiculite and ⅓ cattle manure + ⅓ cassava branches + ⅓ vermiculite. These substrates were tested in a greenhouse covered with 150 µm low density polyethylene (LDPE) film under thermo-reflective screen with 50% shading under film; black screen with 50% shading...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bocaiúva; Cattle manure; Cassava branches; Vermiculite; Protected cultivation.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300002

Produção de chapas de partículas com resíduos de madeira Cordia goeldiana
Provedor de dados: 70
Autores: CHRISTOFORO,ANDRÉ L.; SILVA,SÉRGIO A. M. DA; BARBOSA,JULIANA C.; RIBEIRO FILHO,SÉRGIO L. M.; PANZERA,TÚLIO H.; LAHR,FRANCISCO A. R.
O objetivo deste trabalho consistiu no aproveitamento de resíduos de madeira tropical de baixa densidade (Cordia goeldiana) para confecção de chapas de partículas com resinas poliuretanas monocomponente e bicomponente derivadas de óleo de mamona, gerando subsídios como aplicação nas construções rurais e civis, assim como na indústria moveleira. As propriedades físicas e mecânicas investigadas foram: densidade; teor de umidade; módulo de resistência na flexão estática e adesão interna, ambas obtidas segundo os procedimentos de cálculo propostos pela norma Brasileira NBR 14810:2002. As chapas foram confeccionadas com 15% de resina (uma parte de poliol para uma parte de pré-polímero), 4MPa de pressão de compactação, temperatura de prensagem de 90oC e tempo de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Painéis de partículas; Resina poliuretana; Resíduos de madeiras tropicais.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200368

Avaliação de sensor capacitivo para o monitoramento do teor de água do solo
Provedor de dados: 70
Autores: Cruz,Tadeu M. L.; Teixeira,Adunias Dos S.; Canafístula,Francisco J. F.; Santos,Clemilson C. Dos; Oliveira,Antonio D. S. De; Daher,Sérgio.
Este trabalho teve como objetivo avaliar sensores capacitivos desenvolvidos para monitorar o teor de água do solo. Os sensores foram submetidos a testes para avaliar o efeito da temperatura, o tempo de resposta, obter a equação de calibração e determinar a sua sensibilidade. Foram analisados em diferentes situações (solo, água e ar) e temperaturas (25 ºC; 20 ºC; 15 ºC; 10 ºC; 5º C e 0 ºC). A calibração foi efetuada com um dos sensores capacitivos instalado em uma coluna de solo (indeformada) contida em um tubo de PVC (0,015066 m³) e suspensa em um dos lados de uma balança de braços. Na outra extremidade da balança, havia uma célula de carga conectada a um sistema de aquisição de dados. Os resultados indicaram redução na frequência do sensor capacitivo com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Automação; Irrigação; Capacitância; Constante dielétrica.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100004

Characterization and use of swine deep bedding ashes in cementitious composites
Provedor de dados: 70
Autores: Oliveira,Débora C. G. de; Rodrigues,Michelle S.; Santos,Sérgio F. dos; Savastano Junior,Holmer.
The deep bedding is a swine alternative production, especially in the finishing phase, whose byproduct can be recycled, reducing the environmental impact. The objectives of this study were to characterize the ash coming from the controlled burning of the swine deep bedding (SDBA) based on rice husk, and to evaluate their performance in composites as a partial substitute for Portland cement (PC). To measure the differences between SDBA and rice husk ash (RHA) as a reference, we have characterized: particle size distribution, real specific density, x-ray diffraction, electrical conductivity, scanning electron microscopy, chemical analysis and loss on ignition. Samples were prepared for two experimental series: control, and another one with the partial...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Composite; Rural construction; Residues; Swine production; Sustainability.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500001

Comportamento aerodinâmico e efeito de enrijecimento externo em silos cilíndricos sob a ação do vento
Provedor de dados: 70
Autores: Andrade Júnior,Luciano J. de; Calil Júnior,Carlito.
Os silos metálicos, quando vazios, são suscetíveis ao amassamento das chapas do corpo cilíndrico pela ação do vento. Este trabalho compara os efeitos do enrijecimento interno e externo com colunas, no comportamento aerodinâmico de silos cilíndricos com telhado cônico. Os estudos teóricos conduziram a ensaios em túnel de vento, que foram realizados em dois tipos de modelos reduzidos: um com superfície lisa (enrijecimento interno) e o outro com superfície nervurada (enrijecimento externo), ambos em duas relações geométricas de altura/diâmetro do cilindro (0,5 e 1,0) e inclinação da cobertura cônica de 27º. Com base nos ensaios, foram obtidos os coeficientes de pressão externa e os coeficientes de arrasto nos cilindros, bem como os coeficientes de arrasto e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coeficientes aerodinâmicos; Silos cilíndricos; Enrijecimento externo.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300004

CHARACTERIZATION AND EVALUATION OF THE POTENTIAL USE OF SLUDGE FROM STP AND WTP IN PAVING
Provedor de dados: 70
Autores: Lucena,Leda C.; Juca,José F. T.; Soares,Jorge B.; Barroso,Suelly H. A.; Portela,Manoel G.
ABSTRACT Water and sewage treatment plants (STP and WTP) generate as byproduct a significant amount of sludge with environment harmful elements. Sending to landfills or depositing on the ground or rivers are respectively expensive and dangerous alternatives. In this scenario, the use of this waste in paving processes is a promising alternative for disposal thereof. In this study, we focused on characterizing sludge and evaluating its use in paving, which showed satisfactory results for use in base and sub-base floors.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Stabilization; Chemical constituents; Soil.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100166

Spatial variability of apparent electrical conductivity and soil properties in a coffee production field
Provedor de dados: 70
Autores: Valente,Domingos S. M.; Queiroz,Daniel M. de; Pinto,Francisco de A. de C.; Santos,Fábio L.; Santos,Nerilson T.
Precision agriculture based on the physical and chemical properties of soil requires dense sampling to determine the spatial variability of these properties. This dense sampling is often expensive and time-consuming. One technique used to reduce sample numbers involves defining management zones based on information collected in the field. Some researchers have demonstrated the importance of soil electrical variables in defining management zones. The objective of this study was to evaluate the relationship between the spatial variability of the apparent electrical conductivity and the soil properties in the coffee production of mountain regions. Spatial variability maps were generated using a geostatistical method. Based on the spatial variability results,...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Geostatistical; Management zone; Sensors.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600017

Computational modeling for irrigated agriculture planning. Part II: risk analysis
Provedor de dados: 70
Autores: Borges Júnior,João C. F.; Ferreira,Paulo A.; Andrade,Camilo L. T.; Hedden-Dunkhorst,Bettina.
Techniques of evaluation of risks coming from inherent uncertainties to the agricultural activity should accompany planning studies. The risk analysis should be carried out by risk simulation using techniques as the Monte Carlo method. This study was carried out to develop a computer program so-called P-RISCO for the application of risky simulations on linear programming models, to apply to a case study, as well to test the results comparatively to the @RISK program. In the risk analysis it was observed that the average of the output variable total net present value, U, was considerably lower than the maximum U value obtained from the linear programming model. It was also verified that the enterprise will be front to expressive risk of shortage of water in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Risk simulation; Monte Carlo method; Irrigation requirement.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300009

Comparação entre métodos de amostragem do solo para recomendação de calagem e adubação do cafeeiro conilon
Provedor de dados: 70
Autores: Oliveira,Rone B. de; Lima,Julião S. de S.; Xavier,Alexandre C.; Passos,Renato R.; Silva,Samuel de A.; Silva,Alessandra F. da.
O objetivo deste trabalho foi comparar a metodologia convencional de amostragem de solo com a análise espacial para a recomendação de calagem e adubação de nitrogênio, fósforo e potássio em solo cultivado com café conilon. O experimento foi realizado nas safras de 2004/2005 e 2005/2006, em área de 1,0 ha, com as amostras retiradas na profundidade de 0-0,20 m. No método convencional, coletaram-se 15 subamostras em caminhamento ziguezague, constituindo uma amostra composta, e, no método espacial, construiu-se uma malha amostral de 109 pontos georreferenciados. Com os resultados das análises, foi calculada a necessidade de calagem e adubação em função do teor do elemento no solo e da produtividade esperada das plantas. Os dados foram analisados por meio da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Geoprocessamento; Manejo do solo.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100018

BEHAVIORAL RESPONSES OF PIGS FINISHED IN DEEP BEDDING AND CONVENTIONAL BED SYSTEMS
Provedor de dados: 70
Autores: Amaral,Pedro I. S.; Campos,Alessandro T.; Esteves Junior,Roberto da C.; Esteves,Gabriella F.; Yanagi Junior,Tadayuki; Leite,Maria E. C. R.
ABSTRACT The objective of this study was to characterize the thermal environment and evaluate the behavior of finishing pigs housed in deep bedding and conventional systems. The work was carried out in the Department of Animal Science of the Federal Institute of Education, Science and Technology of Southeast Minas Gerais, Rio Pomba campus. Three pens were used in an installation for breeding pigs in their finishing phase. Two pens contained deep bedding, with wood shavings and rice husks. The remaining pen was a conventional system. The behavior of the piglets was observed from 8 a.m. to 5:30 p.m., noting the behaviors with the use of an ethogram, while data relating to the thermal environment in the stalls were automatically collected using data loggers....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal welfare; Animal behavior; Swine breeding; Breeding systems.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100025

THE USE OF VOCALIZATION SIGNALS TO ESTIMATE THE LEVEL OF PAIN IN PIGLETS
Provedor de dados: 70
Autores: Cordeiro,Alexandra F. da S.; Nääs,Irenilza de A.; Baracho,Marta dos S.; Jacob,Flávia G.; Moura,Daniella J. de.
ABSTRACT Pain is considered a condition that most affect the welfare of animals and its measurement is seen as a difficult task. This research aimed to determine the level of pain in pigs by their vocalization. It was recorded the vocalizations of 20 male piglets under normal circumstances (I), marking by Australian method (II), tail trimming management (III), and castration (IV). A unidirectional microphone and a digital recorder were used to record the sound signals. The results suggested that Pitch frequency (Hz), the maximum amplitude (Pa), and intensity (dB) increased from pain-free pigs to the marking procedure; and from marking to both tail trimming and castration The tail trimming and castration vocal response did not differ.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Stress; Caudectomy; Castration; Marking; Swine; Sound signals.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400486

Spatial variability of the rainfall erosive potential in the State of Mato Grosso do Sul, Brazil
Provedor de dados: 70
Autores: Oliveira,Paulo T. S.; Rodrigues,Dulce B. B.; Sobrinho,Teodorico A.; Carvalho,Daniel F. de; Panachuki,Elói.
Information about rainfall erosivity is important during soil and water conservation planning. Thus, the spatial variability of rainfall erosivity of the state Mato Grosso do Sul was analyzed using ordinary kriging interpolation. For this, three pluviograph stations were used to obtain the regression equations between the erosivity index and the rainfall coefficient EI30. The equations obtained were applied to 109 pluviometric stations, resulting in EI30 values. These values were analyzed from geostatistical technique, which can be divided into: descriptive statistics, adjust to semivariogram, cross-validation process and implementation of ordinary kriging to generate the erosivity map.Highest erosivity values were found in central and northeast regions of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water erosion; Rainfall erosivity index; Geostatistics.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100008

Semeadura de milho com dois mecanismos sulcadores sob diferentes intensidades de pastejo
Provedor de dados: 70
Autores: Modolo,Alcir J.; Franchin,Marcia F.; Trogello,Emerson; Adami,Paulo F.; Scarsi,Marina; Carnieletto,Ricardo.
A integração lavoura-pecuária pode ser definida como o sistema que integra duas atividades, visando a maximizar racionalmente o uso da terra e a minimizar os custos de produção. O trabalho teve como objetivo avaliar a semeadura de milho com dois mecanismos sulcadores, em área de pastagem submetida a diferentes manejos, no sistema de integração lavoura-pecuária. O experimento foi conduzido em delineamento de blocos ao acaso, com quatro repetições, e os tratamentos foram compostos pela combinação de quatro intensidades de pastejo (0,25-0,05; 0,30-0,10; 0,35-0,15 m e sem pastejo, para as alturas de entrada e saída dos animais dos piquetes, respectivamente) e dois mecanismos sulcadores (haste e disco duplo). Foram avaliadas a densidade e a macroporosidade do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Integração lavoura-pecuária; Densidade do solo; Produtividade do milho.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600013

COMPARING A SINGLE-SENSOR CAMERA WITH A MULTISENSOR CAMERA FOR MONITORING COFFEE CROP USING UNMANNED AERIAL VEHICLES
Provedor de dados: 70
Autores: Gomes,Amanda P. A.; Queiroz,Daniel M. de; Valente,Domingos S. M.; Pinto,Francisco de A. de C.; Rosas,Jorge T. F.
ABSTRACT There exist two options for digital cameras that can capture the near-infrared (NIR) band. Conventional red–green–blue (RGB, visible bands) cameras with a single sensor provide NIR band visibility based on the removal of the internal NIR-blocking filter. Alternatively, multisensor cameras exist that have a specific sensor for each band. The modified RGB cameras are of a lower price. In this context, the objective of this study was to compare the performance of a modified RGB camera with that of a multisensor camera for obtaining the normalized difference vegetation index (NDVI) in an area with coffee cultivations. A multispectral camera with five sensors and another camera with only one sensor were used. The NDVI of the coffee field was also...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; UAV; Radiometric calibration; Modified RGB camera.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100087

Nutrient loss in composting of agroindustrial residues
Provedor de dados: 70
Autores: Carneiro,Leocir J.; Costa,Mônica S. S. de M.; Costa,Luiz A. de M.; Martins,Marcos F. L.; Rozatti,Marcos A. T.
The management of composting may influence the characteristics of the produced compounds. The experiment used three frequencies of plowing, combined with the conditions: with and without coverage of the composting patio, with and without the use of commercial inoculant, resulting in 12 furrows, installed on the Experimental Center of Agricultural Engineering (NEEA), of the STATE UNIVERSITY OF WEST PARANÁ (UNIOESTE), Campus of Cascavel city - state of Paraná (PR), in Brazil. The waste and quantities used in kg were: corn cob (7.5); hatchery residue (5); floater sludge (31); ash (1); wheat cleaning residue (120); wheat pre-cleaning residue (120); corn peel (7.5); solid fraction of wash trucks used to transport chickens (2); solid fraction of pig manure (1)...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Volatilization; Leaching; Inoculation; Turn of plowing.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400019

Natural shading and productivity index of broiler chickens
Provedor de dados: 70
Autores: Souza,Fernando A.; Milani,Adhemar P.
The appropriate use of natural resources in the design of broiler houses provides a reduction in farming operating costs and optimization of production conditions. Therefore, the natural shading around the broiler house can be an alternative for improving internal conditions of comfort. This study verified the efficiency of natural shading in the broiler productivity index (PI) in East-West oriented commercial housings. The PI of 32 commercial broiler houses in five flocks divided throughout a year was compared. The sheds had the same management, density and the same structural features, except from tree shading: on the North face; on the South face; on both faces and without shading. It was observed that broiler house in East-West direction with shading...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tree-shading; Ambience; Broiler houses; Broiler industry.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300601

Uncertainties of the 137Cs technique for validation of soil redistribution modelling in a semiarid meso-scale watershed
Provedor de dados: 70
Autores: Medeiros,Pedro H. A.; Araújo,José Carlos de; Andrello,Avacir C.
Scarcity of long-term series of sediment-related variables has led watershed managers to apply mathematical models to simulate sediment fluxes. Due to the high efforts for installation and maintenance of sedimentological gauges, tracers have been pointed out as an alternative to validate soil redistribution modelling. In this study, the 137Cs technique was used to assess the WASA-SED model performance at the Benguê watershed (933 km²), in the Brazilian semiarid. Qualitatively, good agreement was found among the 137Cs technique and the WASA-SED model results. Nonetheless, quantitatively great differences, up to two orders of magnitude, were found between the two methods. Among the uncertainties inherent to the 137Cs technique, definition of the reference...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: 137Cs; Soil redistribution; Sediment modelling; Semiarid.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200004

Comparison of metering mechanisms of corn seed
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Justino,Altair; Namur,Rodrigo T.; Domingues,José; Garcia,Luiz C.
It was compared the performance of the metering mechanism of corn seeds (Zea mays) in direct seeding in an area of ​​200 ha, a property in Piraí do Sul, State of Paraná - PR, in Brazil. It was seeded 4 maize hybrids, 50 ha of each, with seeds of different sieves. The experiment was conducted in a randomized block design (RBD), with 3 treatments and 9 repetitions for each corn hybrid. The treatments were the pneumatic seed of metering mechanisms, horizontal perforated disc with and without ramp®. The plots were 40 m² and were distributed at the early, middle and late sowing. The variables analyzed in each corn hybrid were initial population, faulty spacing, multiple spacing, acceptable spacing, and yield components. As there were no significant differences...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pneumatic system; Horizontal seed plate; Disc with ramp®.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500017

Determining the concrete stiffness matrix through ultrasonic testing
Provedor de dados: 70
Autores: Gonçalves,Raquel; Giacon Júnior,Milton; Lopes,Igor M.
The determination of the modulus tangent (Eci ) and of the modulus secant (Ecs) of the concrete can be done using compression test but, to be simpler, it is used relations with characteristic strength (f ck). Relations are also used to determine the transversal modulus (Gc) and, in the case of the Poisson's ratio (ν), a fixed value 0.20 is established. The objective of this research was to evaluate the use of the ultrasonic propagation waves to determine these properties. For the tests were used specimens with f ck varying from 10 to 35 MPa. For the ultrasonic tests were used cylindrical and cubic specimens. The modulus of deformation obtained by ultrasound was statistically equivalent to the obtained by compression tests. The results of modules obtained...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compressive strength; Modulus of deformation; Mechanical properties.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300003

Processo da retrolavagem em filtros de areia usados na irrigação localizada
Provedor de dados: 70
Autores: Salcedo,Juan C; Testezlaf,Roberto; Mesquita,Márcio.
O processo da retrolavagem consiste na passagem da água através do filtro em sentido contrário ao fluxo de filtragem com o objetivo de remover partículas orgânicas e inorgânicas retidas no meio filtrante. O projeto de filtros de areia com configurações ineficientes e a ocorrência de condições operacionais inadequadas contribuem para limitar o desempenho desse processo, causando deficiências na limpeza dos meios filtrantes e comprometendo o funcionamento dos sistemas de irrigação localizada. O objetivo do presente trabalho é proporcionar uma revisão sobre os conceitos associados ao processo da retrolavagem nos filtros de areia, relacionando informações existentes na literatura com experiências de laboratório. Foi gerado um texto básico com informações...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Filtração; Fluidização; Camada filtrante.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600020

TRANSITION FROM SYSTEMATIC TO DIRECTED SOIL SAMPLING DESIGNS IN AN AREA MANAGED WITH PRECISION AGRICULTURE
Provedor de dados: 70
Autores: Pias,Osmar H. de C.; Cherubin,Maurício R.; Santi,Antônio L.; Basso,Claudir J.; Bayer,Cimélio.
ABSTRACT In agricultural areas with a historical of systematic soil sampling, alternative methodologies such as directed sampling design based on management zones (MZ) have been proposed to reduce sampling costs. The aim of this study was to evaluate the technical and economic impacts of replacing a dense systematic soil sampling design (cell size of 0.5 ha) by a systematic sampling with a smaller number of samples (cell size ranging from 1 to 4.5 ha), directed or conventional sampling design on the mapping of soil plant-available phosphorus (P), exchangeable potassium (K), and pHwater. The study was carried out in an agricultural area of 120 ha with soil classified as an Oxisol. The directed sampling designs were based on MZ delimited from data of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sampling costs; Sampling grids; Spatial variability; Management zones.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300400

Acúmulo de matéria seca e óleo em sementes de pinhão-manso irrigado e de sequeiro
Provedor de dados: 70
Autores: Evangelista,Adão W. P.; Alves Júnior,José; Souza,Jorge L. M.; Bezerra,Ricardo de S.; Domingos,Marcus V. H.
RESUMO Avaliou-se o efeito da irrigação e de fases de maturação dos frutos sobre o rendimento em massa de matéria seca e de óleo de sementes de pinhão-manso. O experimento foi conduzido na área experimental do departamento de Agricultura da Universidade Federal de Lavras - UFLA, em Lavras-MG, em uma lavoura de pinhão-manso irrigada por gotejamento, com três anos de idade. Frutos de pinhão-manso foram classificados em quatro fases de maturação, assim denominadas: F1 (frutos totalmente verdes e sementes brancas); F2 (20% de frutos verdes e o restante amarelos, marrons e secos); F3 (frutos amarelos com partes marrons, com início de deiscência e sementes pretas); e F4 (frutos marrons escuros, secos e deiscentes). As sementes foram extraídas para a determinação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Jatropha curcas L.; Maturação fisiológica; Manejo de água.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500829

Avaliação do tensiômetro eletrônico no monitoramento do potencial matricial de água no solo
Provedor de dados: 70
Autores: Coelho,Silvana L.; Teixeira,Adunias dos S.
O presente trabalho apresenta o monitoramento do potencial de água no solo obtido por meio do uso de um tensiômetro eletrônico. Os testes foram conduzidos no Laboratório de Mecânica e Eletrônica do Departamento de Engenharia Agrícola da UFC, tendo sido utilizados nove exemplares de tensiômetro eletrônico e três exemplares de tensiômetro convencional de mercúrio. Durante o período de um mês, os dados foram armazenados a uma freqüência de 2 Hz, sendo possível obter detalhes quanto ao monitoramento do potencial da água do solo, o efeito das flutuações de temperatura nas leituras do tensiômetro e a realização de testes de tempo de resposta e de sensibilidade. O efeito das flutuações de temperatura acentuou-se à medida que o potencial matricial diminuiu, sendo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensor de pressão; Tempo de resposta; Sensibilidade.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300006

Avaliação de um circuito eletrônico para medição da condutividade elétrica de soluções nutritivas
Provedor de dados: 70
Autores: Steidle Neto,Antonio J.; Zolnier,Sérgio; Marouelli,Waldir A.; Carrijo,Osmar A.; Martinez,Herminia E. P.
Nos sistemas de cultivo hidropônicos ou que utilizam a fertirrigação, a quantidade total de sais dissolvidos na solução nutritiva tem grande impacto na produtividade da cultura. A concentração adequada ao crescimento e desenvolvimento da cultura sofre variações marcantes ao longo do seu ciclo, podendo ser avaliada indiretamente por meio do monitoramento da condutividade elétrica da solução nutritiva. O objetivo deste trabalho foi avaliar um circuito eletrônico de baixo custo para a medição da condutividade elétrica, cujo princípio se baseia na medida de freqüência. O circuito eletrônico foi conectado a um computador via porta paralela, sendo calibrado utilizando-se de 16 soluções de KCl. A temperatura das soluções foi mantida nos níveis desejados por meio...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Condutivímetros; Hidroponia; Fertirrigação.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200016

Desenvolvimento de um dispositivo eletrônico para calibração de sensores de umidade do solo
Provedor de dados: 70
Autores: Leão,Raimundo A. de O.; Teixeira,Adunias dos S.; Canafístula,Francisco J. F.; Mesquita,Paulo E. G.; Coelho,Silvana de L.
Com o advento da eletrônica e a disponibilidade de "software" de processamento, vários tipos de transdutores têm sido testados, visando à determinação da umidade do solo. O uso desses transdutores tem por objetivo a otimização do consumo de água e o conseqüente retorno econômico da atividade da agricultura irrigada. No Laboratório de Hidráulica do Departamento de Engenharia Agrícola da Universidade Federal do Ceará, construiu-se um dispositivo para calibração de sensores de umidade do solo, a sua calibração e a determinação de suas principais propriedades, como precisão e cargas mínima e máxima. O dispositivo consistiu numa torre em aço 1020, com 3,0 m de altura, no topo da qual se montou uma balança de braços. Em um dos braços da balança, colocou-se uma...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Célula de carga; Instrumentação eletrônica; Curva característica do solo.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100024

NUTRIENT CONTENTS IN ‘TOMMY ATKINS’ MANGO LEAVES AT FLOWERING AND FRUITING STAGES
Provedor de dados: 70
Autores: Faria,Leandro N.; DONATO,Sergio L. R.; Santos,Marcelo R. Dos; Castro,Luciana G.
ABSTRACT The objective of this study was to evaluate the nutrient contents in ‘Tommy Atkins’ mango leaves at the flowering and fruiting stages under different strategies to reduce irrigation levels during flower induction. Five irrigation level reduction strategies, based on crop evapotranspiration (ETc) were used in the plots: T1 (0% ETc), T2 (25% ETc), T3 (50% ETc), T4 (75% ETc) and T5 (100% ETc); two production cycles in the split-plots; and in two development stages, flowering and harvest, in the split-split plots. The content of N, P, K, Ca, Mg, and S, as well as B, Cu, Fe, Mn, Zn, and Na was determined and leaf chlorophyll index was measured during the second cycle. The content of P, K, Mg, and Cu in the ‘Tommy Atkins’ mango trees leaves varied...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mangifera indica L.; Water deficit; Nutritional status.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601073

Thermal efficiency of individual shelters for girolando calves in brazilian semi-arid regions
Provedor de dados: 70
Autores: Almeida,Gledson L. P. de; Pandorfi,Héliton; Baptista,Fátima; Guiselini,Cristiane; Barnabé,Janice M. C.
ABSTRACT The objective of this research was to evaluate the thermal efficiency of roofs used on individual shelters during milk-feeding stage of Girolando calves. The research was conducted at a farm located in a dry region of Pernambuco state, Brazil. The experimental design was completely randomized, with 27 Holstein × Gir dairy crossbred calves housed in shelters with three roofing materials (fibre cement tile, recycled tile, and thatched roofs). The recycled tiles and thatched roofs provided reductions of 18.7 and 14.6% in radiant thermal load, respectively. Regardless the roofing material, all animals increased their respiratory rate to maintain thermal equilibrium.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Dairy cattle; Roofing materials; Thermography.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100013

Static tests of constructive tires using hydraulic press on the soil
Provedor de dados: 70
Autores: Machado,Thiago M.; Lanças,Kléber P.; Oliveira Junior,Mauro B. de; Artioli,José A.; Marasca,Indiamara.
ABSTRACT The power consumption and load capacity of agricultural machines have grown and the effects of pressure on the soil by tires have been still little investigated. In concern with sustainable development, the relationship machine-tire-soil must be in balance to give more consistency on the best use of tires for a given load. This study aimed to evaluate four tires of two constructive types, the bias belted tires and radial tires, both with respective rim diameters of 22.5 and 26.5 inches with variables measuring the footprint, elastic deformation, sinkage and resistance to penetration. A hydraulic press with an attachment shaft for tire mounting and a box of soil in which the tire has been imposed on a load of 53.00 kN using nominal pressures...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compaction; Footprint; Pressure; Elastic deformation; Sinkage.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500886

Influência do processo de secagem na qualidade do cogumelo shiitake
Provedor de dados: 70
Autores: Sampaio,Sara M.; Queiroz,Marlene R. de.
Os cogumelos comestíveis são alimentos altamente perecíveis. A secagem apresenta-se como alternativa de proporcionar armazenagem segura e livre do desenvolvimento de microrganismos. Neste trabalho, foram investigados os efeitos dos fatores geometria da matéria-prima (cogumelos inteiros e fatiados), temperatura de secagem (50 °C e 70 ºC) e umidade final (5% e 15% bu) sobre a qualidade de cogumelos Shiitake, após a secagem. Curvas experimentais de secagem foram levantadas e análises de cor e textura foram realizadas no produto fresco e no produto depois de seco e reidratado. O efeito desses parâmetros foi avaliado mediante análise de variância acompanhada de teste de comparações múltiplas. A secagem ocorreu no período decrescente, e os cogumelos fatiados e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cor; Textura; Temperatura de secagem.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200027

NUGGET EFFECT INFLUENCE ON SPATIAL VARIABILITY OF AGRICULTURAL DATA
Provedor de dados: 70
Autores: Guedes,Luciana P. C.; Bach,Raquel T.; Uribe-Opazo,Miguel A.
ABSTRACT Spatial variability description of soil chemical properties by thematic maps depends substantially on suitable geostatistical models. One of the parameters composing a geostatistical model is nugget effect. This study aimed to evaluate the simultaneous influence of nugget effect and sampling design on geostatistical model estimation and estimation of soil chemical properties at unsampled sites, considering simulated data. Our results will be used as scientific basis for spatial variability analyses of soil chemical properties in agricultural areas. Given the simulation results and agricultural data, we concluded that the high nugget effect values obtained here reduced spatial estimation efficiency. Moreover, a systematic sampling design promoted...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geostatistics; Spatial Dependence Index (SDI); Relative Nugget Effect (RNE); Spatial Estimation.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100096

Avaliação de risco à produção de frango de corte do Estado de São Paulo em função da temperatura ambiente
Provedor de dados: 70
Autores: Salgado,Douglas D.; Nääs,Irenilza de A.
As perdas produtivas na avicultura de corte, provenientes de climas com temperaturas diárias elevadas, são potencialmente de grande magnitude, pois abrangem perdas diretas e indiretas. Esta pesquisa teve a finalidade de apontar os municípios localizados onde há mais risco de temperaturas extremas diárias. Os dados históricos meteorológicos de temperaturas diárias, máximas e mínimas, fornecidos pelo CEPAGRI-UNICAMP, foram adaptados para análise estatística, descritiva e exploratória. As temperaturas diárias foram categorizadas em forma binária, estimando-se probabilidades condicionais (riscos) por meio das frequências relativas, obtidas em tabelas de contingência. Utilizando o software Minitab 15®, foi realizada análise descritiva, análise de risco e, por...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bem-estar animal; Temperaturas extremas; Risco.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300001

Spatial statistics applied to soybean production data from Paraná State for 2003-04 to 2009-10 crop-years
Provedor de dados: 70
Autores: Prudente,Victor H. R.; Souza,Carlos H. W. de; Mercante,Erivelto; Johann,Jerry A.; Uribe-Opazo,Miguel A.
In the current study, we performed a soybean production spatial distribution analysis in Paraná State. Seven crop-year data, from 2003-04 to 2009-10, obtained from the Paraná Department of Agriculture and Supply (SEAB) were used to develop a Boxmap for each crop-year, show soybean production throughout this time interval. Moran's index was used to measure spatial autocorrelation among municipalities at an aggregate level, while LISA index local correlation. For each index, different contiguity matrix and order were used and there was a significance level study. As a result, we have showed spatial relationship among cities regarding the production, which allowed the indication of high and low production clusters. Finally, identifying main soybean-producing...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spatial correlation; Moran's Index; LISA index.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400015

A decision support system for cost determination in grain storage facility operations
Provedor de dados: 70
Autores: Valente,Domingos S. M.; Queiroz,Daniel M. de; Corrêa,Paulo C.; Silva,Luis C. da; Vale,Sônia M. L. R. do.
Many research works have being carried out on analyzing grain storage facility costs; however a few of them had taken into account the analysis of factors associated to all pre-processing and storage steps. The objective of this work was to develop a decision support system for determining the grain storage facility costs and utilization fees in grain storage facilities. The data of a CONAB storage facility located in Ponta Grossa - PR, Brazil, was used as input of the system developed to analyze its specific characteristics, such as amount of product received and stored throughout the year, hourly capacity of drying, cleaning, and receiving, and dispatch. By applying the decision support system, it was observed that the reception and expedition costs were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Costs; Modeling; Software.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400012

Operational characteristics of four metering systems for agricultural fertilizers and amendments
Provedor de dados: 70
Autores: Camacho-Tamayo,Jesus H.; Barbosa,Angela M.; Pérez,Nancy M.; Leiva,Fabio R.; Rodríguez,Gonzalo A.
The use of fertilizers and solid amendments in agriculture generates special interest for their effect on crop productivity, as well as for their environmental impact. The efficient use of these products demands knowing their physical and mechanical properties, the storing conditions effect and the operational characteristics of the metering systems used in the fertilizing equipment. In this context, the present study was developed with the purpose of evaluating the operational characteristics of different fertilizing metering systems and to determine the adequate metering system-product operational parameters, using powder lime, powder gypsum, granular 10-30-10 (N-P-K), and granular urea. Operational differences were established among four types of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertilizer metering system; Agricultural machinery; Granular material.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400010

Curvas de distribuição de efluentes do íon nitrato em amostras de solo deformadas e indeformadas
Provedor de dados: 70
Autores: Rossi,Paulo; Miranda,Jarbas H.; Duarte,Sérgio N.
Devido à grande importância em se avaliar o destino e o transporte de íons no solo, o presente trabalho teve o objetivo de obter os parâmetros de transporte do nitrato no solo, como a velocidade da água nos poros (v), o fator de retardamento (R), a dispersividade (lambda) e o coeficiente de dispersão (D), em solos de diferentes texturas e em amostras deformadas e indeformadas. O ensaio foi conduzido empregando as amostras deformadas e indeformadas oriundas de dois perfis distintos de solos, coletadas à profundidade de 0-20 cm, com aplicação de solução de nitrato de cálcio contendo 50 mg L-1 de NO3-. Após a obtenção dos parâmetros de transporte, ajustados pelo programa computacional CXTFIT, notou-se que as curvas de efluentes preparadas com solos a partir...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dinâmica de solutos; Amostras de solo; Parâmetros de transporte.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400010

Technical and economic analysis of replacing artificial lighting system to induction of photoperiod effect in begonia's seedlings in greenhouse
Provedor de dados: 70
Autores: David,Eduardo; Rossi,Luiz Antonio; Pagliardi,Odail.
The type of artificial light used for inducing photoperiod effect in begonia's seedlings at greenhouse has fundamental importance in the growth and development of these plants and directly reflects in the electrical energy consumption used in this production process. The objective of this research was to analyze the technical and economic feasibility of replacing the current technology of artificial lighting used by the producers (incandescent lamps), by the technology of discharge lamps with the purpose of inducing photoperiod in a greenhouse. The analysis results indicate that the discharge lamp of 32 W Tubular Fluorescent discharge lamp was the one that presented the lower peak demand and lower average energy consumption of 85.01% compared to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy efficiency; Artificial lighting; Rural energy; Photoperiod induction.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400005

BASIC UNIT COST SIMULATION FROM FREE-STALL DESIGN TO DAIRY CATTLE CONFINEMENT USING DIFFERENT CONSTRUCTION TECHNIQUES
Provedor de dados: 70
Autores: Ramos,Marcelo C.; Barbosa,Jackson A.
ABSTRACT The ascendancy of milk production in Brazil is due to mainly to the adoption of confinement systems, however, construction quality of these systems impact on milk production. This study aimed to simulate the Basic Unit Cost (BUC m-2), referring to a free-stall design with capacity for 80 animals and different construction techniques, with a database for various budget analysis and investment plans. A budgetary spreadsheet was modeled, allowing simulating the BUC m-2 for different combinations of roof pillars (metallic, wood or reinforced concrete), covering structure (metallic or wood), coverage model (with or without ridge vent), roof tiles (aluminum, cement or ceramic) and masonry (concrete block, ceramic or solid brick). The techniques used...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cost breakdown; Construction techniques; Dairy farms; Milk production; Rural buildings.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000600972

Intensity-Duration-Frequency relationships: stochastic modeling and disaggregation of daily rainfall in the lagoa Mirim watershed, Rio Grande do Sul, Brazil
Provedor de dados: 70
Autores: Damé,Rita de C. F; Teixeira-Gandra,Claudia F. A.; Guedes,Hugo A. S.; Silva,Gisele M. da; Silveira,Suélen C. R. da.
ABSTRACT This study aimed to investigate information gain by using rainfall intensity-duration-frequency (IDF) relationships, with data gathered within N+M years from seven rain gauge stations located in the Lagoa Mirim Watershed (South Atlantic basin). After N years of daily rainfall, the transition probabilities of a time homogeneous two-state Markov chain were defined to simulate rainfall occurrence, as well as gamma distribution to measure it; for that, daily rainfall series were composed of N+M years, with M being the generated series. The series were adjusted to Gumbel distribution, being used in annual maximum daily rainfall disaggregation for durations of 10, 20, 30, 40, 50, 60, 120, 360, 720 and 1440 min. Daily rainfall disaggregation was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Intense rainfall; Hydrologic modeling; Pluviographic records; Hydrological series.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300492

Control of ammonia emissions in naturally ventilated dairy cattle facilities in Portugal
Provedor de dados: 70
Autores: Pereira,José; Trindade,Henrique.
We conducted a study of the processes associated to NH3 emission in naturally ventilated dairy cattle facilities, having described factors that regulate NH3 emission, as well as methodologies for measuring these emissions at these facilities. Appropriate techniques to mitigate NH3 emission in facilities located in regions with warm climates were also identified. The most effective mitigation techniques with simple implementation include strategies associated to: (i) installation design and flooring, which lead to reduced emissions, (ii) excreta pre-excretion, namely the use of diets with optimized crude protein content and increased milk production at farm level; and (iii) excreta post-excretion, particularly by changing the conditions of environmental...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Facilities; Gases; Methods; Floors; Mitigation techniques.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300022

Série histórica secular de brilho solar e suas relações com os modos de variabilidade ENOS e ODP em Santa Maria-RS
Provedor de dados: 70
Autores: Paula,Gizelli M. de; Streck,Nereu A.; Langner,Josana A.; Barbosa,Daniele C.; Heldwein,Arno B.; Ferraz,Simone E. T.; Buriol,Galileo.
Os objetivos neste trabalho foram testar a homogeneidade, recalcular a média climatológica e determinar possíveis tendências e variabilidade interanual e interdecadal na série histórica secular mensal e sazonal de brilho solar, em Santa Maria - RS. Os dados de brilho solar foram obtidos na Estação Climatológica Principal (ECP) do Instituto Nacional de Meteorologia (8o DISME), no período de 1912 a 2011. Foram usados os testes de Sequência, de Mann-Kendall e Pettitt para análise de homogeneidade e tendência, respectivamente. As séries históricas na escala mensal e sazonal são estacionárias e homogêneas, exceto para o mês de dezembro e para a estação de outono. Há variabilidade interanual e interdecadal nas séries, devido aos fenômenos El Niño-Oscilação Sul...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Homogeneidade; El niño-oscilação sul; Oscilação decadal do pacífico; Mann- Kendall.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300494

SPECTRUM, VELOCITY AND DRIFT OF DROPLETS SPRAYED BY NOZZLES WITH AND WITHOUT AIR INDUCTION AND MINERAL OIL
Provedor de dados: 70
Autores: França,Jorge A. L.; Cunha,João P. A. R. da; Antuniassi,Ulisses R.
ABSTRACT The aim of this study was to evaluate the spectrum, the velocity and the potential drift risk of droplets sprayed by nozzles with and without air induction, with the addition of mineral oil to the spray solution. The experiment was conducted in a completely randomized design with five replications; in a factorial model 2 × 2 (two spray nozzles and spray solution with and without mineral oil Assist®). Spray nozzles with and without air induction were evaluated, with nominal flow rate of 1.14 L min−1 and pressure of 300 kPa. The spectrum and the velocity of droplets were evaluated directly, using a droplet analyzer (VisiSize D30) in real time based on the analysis of high-resolution images. The drift potential was evaluated in an open circuit wind...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adjuvants; Droplet size; Application technology.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300502

SURFACE ENERGY BALANCE SYSTEM (SEBS) AND SATELLITE DATA FOR MONITORING WATER CONSUMPTION OF IRRIGATED SUGARCANE
Provedor de dados: 70
Autores: Ferreira,Elizabeth; Mannaerts,Christiaan M.; Dantas,Antonio A.; Maathuis,Bernardus H.
ABSTRACT The objective of this research was to evaluate the water consumption of irrigated sugarcane areas using the Surface Energy Balance System (SEBS) driven by products derived from Meteosat Second Generation (MSG), SPOT/VEGETATION, Terra/MODIS satellite data and meteorological observations data from Minas Gerais State, Brazil. The actual evapotranspiration from SEBS model (ET-SEBS) was compared against crop evapotranspiration under standard conditions (ETc), which was obtained from weather data based on reference evapotranspiration (ET0) and the crop coefficient (Kc) values from FAO. Results showed that there was a good agreement between ET-SEBS and ETc when sugarcane was at maximum development stage under center pivot irrigation and the Kc value...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Crop coefficient; Evapotranspiration; Irrigation; Remote sensing; Vegetation indices.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601176

AN EVALUATION OF THE THERMAL AND LUMINOUS ENVIRONMENT OF LAYING HEN AVIARIES EQUIPPED WITH LIGHT-EMITTING DIODE AND COMPACT FLUORESCENT LAMPS AND THEIR EFFECTS ON PRODUCTION AND EGG QUALITY
Provedor de dados: 70
Autores: Ribeiro,Priscilla A. P.; Yanagi Junior,Tadayuki; Lima,Renato R. de; Oliveira,Daniela D. de; Abreu,Lucas H. P.
ABSTRACT The thermal and luminous conditions in aviaries affect the production and quality of eggs. Thus, the aim of the present study was to evaluate the thermal and luminous environment of commercial laying hen aviaries equipped with compact fluorescent (CF) and light-emitting diode (LED) lamps and their influence on egg production and quality. The study was carried out in two commercial laying hen facilities with similar construction features and management. The first facility was illuminated with CF lamps and the second with LED lamps. The thermal environment was assessed via air temperature, air relative humidity, and enthalpy. The evaluated lamps provided a similar thermal environment in both facilities. The aviary equipped with LED lamps showed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal environment; Artificial lighting; Laying hens.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100001

RELATIONSHIP BETWEEN SAMPLE DESIGN AND GEOMETRIC ANISOTROPY IN THE PREPARATION OF THEMATIC MAPS OF CHEMICAL SOIL ATTRIBUTES
Provedor de dados: 70
Autores: Guedes,Luciana P. C.; Uribe-Opazo,Miguel A.; Ribeiro Junior,Paulo J.; Dalposso,Gustavo H.
ABSTRACT Spatial variability depends on the sampling configuration and characteristics associated with the georeferenced phenomenon, such as geometric anisotropy. This study aimed to determine the influence of the sampling design on parameter estimation in an anisotropic geostatistical model and the spatial estimation of a georeferenced variable at unsampled locations. Datasets were simulated with geometric anisotropy, considering five values for the anisotropic ratio (1, 2, 3, 4, 5), and three sampling designs: lattice, random and lattice plus close pairs. The simulation results were used as a reference to select anisotropic models to describe the spatial dependence structure in chemical soil properties. For each dataset (with either simulated or chemical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bootstrap; Directional trend; Geostatistics; Spatial variability; Tests of isotropy.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200260

Caracterização física e mecânica de argamassas à base de cimento Portland e cinza de casca de arroz residual
Provedor de dados: 70
Autores: Rodrigues,Michelle S; Beraldo,Antonio L.
A casca de arroz, utilizada como fonte de energia em indústrias de beneficiamento de arroz, converte-se, depois da queima, em uma cinza residual. Esse resíduo, ainda sem um destino adequado, é muitas vezes depositado em grandes áreas abertas e provoca elevado impacto ambiental. Este trabalho teve como objetivo avaliar a viabilidade de utilização da cinza de casca de arroz (CCA) residual na produção de argamassas, como substituta parcial do cimento. A caracterização da CCA foi realizada por meio da análise de fluorescência de raios-X (composição química), análise do teor de carbono e difração de raios-X; também foi realizada análise granulométrica a laser. Os corpos de prova foram submetidos a dois tipos de exposição: ambientes externo e interno, com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cimento Portland; Cinza de casca de arroz (CCA); Argamassa.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200001

Technical-economic analysis of different lighting systems for broiler poultry
Provedor de dados: 70
Autores: Ribeiro,Priscilla A. P.; Yanagi Junior,Tadayuki; Silva,Joaquim P. da; Yanagi,Sílvia de N. M; Campos,Renato S.
ABSTRACT Broiler poultry is highly dependent on artificial lightening. Power consumption costs of artificial lighting systems is the second largest expense related to broiler industry, second only to feed expenses. Therefore, the current study focused to analyze technical and economic feasibility of replacing incandescent lamps already used in aviaries with other lamp types. Costs related to power consumption, implementation and maintenance of the lighting systems were evaluated with the aid of financial mathematics using net present value, return over investment and payback. Systems composed of six lamp types were analyzed in two different configurations to meet the minimum illuminance of 5 and 20 lux and for use in conventional sheds and dark house. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Economic analysis; Poultry farming; Energy efficiency; Artificial lighting.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200242

DYNAMIC OF PRESSURE-DEFORMATION CURVE IN UNIAXIAL COMPRESSION TEST IN DIFFERENT LOAD TIMES
Provedor de dados: 70
Autores: Mazurana,Michael; Levien,Renato; Zulpo,Lucas; Passos,Gabrielle M.; Kerpen,Hyran S.
ABSTRACT: The loading application time by machinery tires and agricultural tires is one of the factors of soil compaction. We evaluated the effect of loading reduction time in uniaxial compression test, in laboratory, in some physical and mechanical parameters, approaching the loading field condition time by machinery with laboratory tests. Soil samples of two Oxisol and one Paleudult under different years of implementation of no tillage system (NT) and of different layers were collected and subjected to uniaxial compression tests, two times of loading application, 300 seconds per load, according to actual methodology and 30 seconds per load in the laboratory. We analyzed the soil deformation to each load, bulk density, pre-compression stress, recompress...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Loading bearing support; Compaction; Recompression index.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500973

IDENTIFICATION OF NAVEL ORANGE LESIONS BY NONLINEAR DEEP LEARNING ALGORITHM
Provedor de dados: 70
Autores: Yang,Guoliang; Xu,Nan; Hong,Zhiyang.
ABSTRACT It is difficult for humans to recognize recessive diseases in navel oranges. Therefore, deep neural networks are applied to plant disease identification. To improve the feature extraction ability of convolutional neural networks, the Parameter Exponential Nonlinear Activation Unit (PENLU) is proposed to replace the activated function of the neural network. This function not only adds multiple parameters but also brings better generalization ability to the neural network. In addition, the proposed function parameters can be updated by the inverse Stochastic Gradient Descent (SGD) algorithm, which has unparalleled advantages over the existing activated functions. The Residual Network (ResNet), improved by PENLU, is applied to navel orange lesion...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Neural networks; Activation function; Plant image classification; Lesion detection.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500783

Potential of adjuvants to reduce drift in agricultural spraying
Provedor de dados: 70
Autores: Oliveira,Rone B. de; Antuniassi,Ulisses R.; Mota,Alisson A. B.; Chechetto,Rodolfo G.
The reduction of pesticide spraying drift is still one of the major challenges in Brazilian agriculture. The aim of this study was to evaluate the potential of different adjuvant products, such as surfactants, drift retardants, mineral oil and vegetable oil for reducing drift in agricultural spraying. The experiment consisted of quantifying drift of sprayings of 18 adjuvants dissolved in water under controlled conditions in a wind tunnel. Tests were performed in triplicates with spraying nozzles type Teejet XR8003 VK, pressure of 200kPa and medium drops. Solutions sprayed were marked with Brilliant Blue dye at 0.6% (m v-1). The drift was collected using polyethylene strips transversally fixed along the tunnel at different distances from the nozzle and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wind tunnel; Drift retardant; Mineral oil; Vegetable oil; Surfactant.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500010

THE PERFORMANCE OF EXPLICIT FORMULAS FOR DETERMINING THE DARCY-WEISBACH FRICTION FACTOR
Provedor de dados: 70
Autores: Minhoni,Renata T. de A.; Pereira,Francisca F. S.; Silva,Tatiane B. G. da; Castro,Evanize R.; Saad,João C. C.
ABSTRACT The Darcy-Weisbach equation is the most recommended equation for determining the pressure loss in pressurized pipes because of its wide applicability. However, one of the largest obstacles to implementing this equation is the friction factor (f) calculation. This factor can be precisely determined using the Colebrook equation, which is implicit. Thus, the objective of this study was to compare six explicit equations for calculating the Darcy-Weisbach friction factor with the implicit Colebrook equation based on the relative error. Based on the results, the equations of Vatankhah and Offor &amp; Alabi were the most highly recommended. These six explicit formulas showed a mean relative error of less than ± 1% compared to the Colebrook equation,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Absolute roughness; Colebrook equation; Forced conduits; Head loss; Hydraulic load; Reynolds number.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200258

Condições ambientais em galpão convencional telado para galinhas poedeiras hyline W-36
Provedor de dados: 70
Autores: LOURENÇONI,DIAN; YANAGI JUNIOR,TADAYUKI; OLIVEIRA,DANIELA D. DE; CAMPOS,ALESSANDRO T.; LIMA,RENATO R. DE.
Devido às ocorrências dos vírus de influenza aviária (H5N1 e H7N2), estudos relacionados à biosseguridade têm-se intensificado, e uma das soluções discutidas é o uso de tela para cercar completamente o perímetro dos galpões, visando a evitar o contato das galinhas poedeiras alojadas com outras aves. Desta forma, o presente trabalho teve como objetivo avaliar e comparar a utilização de tela cercando o perímetro de galpões convencionais de poedeiras, sobre o ambiente acústico e aéreo no interior da instalação. A pesquisa foi realizada em uma granja comercial para produção de ovos, localizada no sul do Estado de Minas Gerais, e foi conduzida em um galpão aberto, que teve a metade de sua área cercada por tela e a outra metade mantida totalmente aberta. Foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biosseguridade; Ruído; Amônia; Dióxido de carbono; Poedeiras.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100001

Comparação de bancadas simuladoras do processo de semeadura em milho
Provedor de dados: 70
Autores: Jasper,Roberto; Justino,Altair; Morgado,Carlos B.; Dyck,Rogério; Garcia,Luiz C.
No sistema de disco perfurado horizontal, há cerca de 180 opções para a distribuição das peneiras de milho disponibilizadas pelas empresas produtoras de semente. A utilização de bancadas simuladoras do processo de semeadura tem sido a ferramenta empregada por empresas produtoras de sementes e discos para indicar a melhor opção para cada lote de sementes de milho. O objetivo deste trabalho foi avaliar a bancada simuladora do processo de semeadura em dois formatos, revestida com feltro e revestida com graxa. Os tratamentos foram efetuados com base no projeto de norma da ABNT (1996) e foram montados com as combinações das velocidades 3; 5; 7 e 9 km h-1; densidades 4,0; 4,8 e 5,6 sementes por metro e nível de sementes cheio, médio e ¼ do reservatório. O...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Velocidade de semeadura; Densidade de sementes; Nível do reservatório; Distribuição.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400012

Produtividade da cana-de-açúcar fertirrigada com N e K via gotejamento subsuperficial
Provedor de dados: 70
Autores: Dalri,Alexandr B.; Cruz,Raimundo L.
O objetivo deste trabalho consistiu no estudo da fertirrigação por gotejamento subsuperficial na produtividade da cana-de-açúcar, no segundo e terceiro ciclos de cultivo, e os efeitos nos índices tecnológicos na cultura. O experimento foi desenvolvido na área experimental da Faculdade de Ciências Agronômicas, FCA/UNESP - Botucatu. O tubo gotejador foi instalado a 30 cm de profundidade e sob a fileira de plantio da cana-de-açúcar. A variedade cultivada foi a RB 72454. O tratamento com a aplicação da maior dose de NK via fertirrigação foi o que respondeu melhor, apresentando produtividade de colmos de 190,01 t ha-1 e 168,80 t ha-1 para o segundo e terceiro ciclos, respectivamente. A fertirrigação não alterou a qualidade tecnológica da cana-de-açúcar nos dois...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertirrigação; Saccharum spp.; Irrigação por gotejamento.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300012

Umidade do solo na zona radicular do maracujazeiro cultivado sob irrigação localizada
Provedor de dados: 70
Autores: Sousa,Valdemício F.; Folegatti,Marcos V.; Frizzone,José A.; Corrêa,Rodrigo A. L.; Viana,Thales V. A.
O objetivo deste trabalho foi avaliar o efeito de níveis de irrigação aplicados por gotejamento no perfil de umidade do solo na zona de concentração radicular do maracujazeiro-amarelo (Passiflora edulis Sims f. flavicarpa Deg). O experimento foi realizado no período de julho de 1999 a janeiro de 2000, no Campo Experimental da Fazenda Areão, em Piracicaba - SP (22º42'30"S e 47º38'00"W). Os níveis de irrigação, aplicados por um sistema de irrigação por gotejamento, foram: L1 = 0,25 L; L2 = 0,50 L; L3 = 0,75 L, e L4 = 1,00 L, em que L é a lâmina de água média medida em lisímetros. Os níveis de irrigação influenciaram nos perfis de distribuição temporal do potencial matricial, apresentando comportamento diferenciado na oscilação e na manutenção dos teores de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Potencial matricial; Irrigação por gotejamento; Manejo de água.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200004

BIOMECHANICAL PROPERTIES OF WOLFBERRY PLANT ORGANS
Provedor de dados: 70
Autores: Ma,Fulong; Li,Lekai; Wang,Yutan; Li,Ping; Zhu,Chaowei.
ABSTRACT To improve the picking rate and reduce the wrong picking rate of the existing wolfberry harvesting machinery, in this study, the binding force and physical appearance of the immature fruit stalk, mature fruit stalk, flower, and leaf were studied to guide the designing of new-generation wolfberry harvesting machinery and lay theoretical foundation for further studies on biomechanical properties of wolfberry. By preprocessing the experimental data with the Pauta criterion, the distribution range of the binding force and physical appearance of stalk were obtained; the binding force was not influenced by the picking temperature, mass of the fruit, and location of the branch of the fruit. The length-diameter ratio of mature fruit was confirmed by image...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Binding force; Biomechanical characteristics; Constitutive equation; Dynamic model; Vibrating wolfberry harvesting machinery.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200162

Cobre e zinco no material percolado e no solo com a aplicação de água residuaria de suinocultura em solo cultivado com soja
Provedor de dados: 70
Autores: Smanhotto,Adriana; Sousa,Antônio de P; Sampaio,Silvio C; Nóbrega,Lúcia H. P; Prior,Maritane.
O objetivo deste trabalho foi avaliar possíveis efeitos da aplicação de taxas de água residuária de suinocultura (ARS), quanto às concentrações de cobre e zinco, tanto no solo quanto na água percolada de lisímetros de drenagem, durante o ciclo da cultura da soja. O experimento foi conduzido em ambiente protegido, onde havia 24 lisímetros de drenagem. Semeou-se soja cultivar CD 202, e foram aplicadas ARS nas seguintes dosagens: 0; 100; 200 e 300 m³ ha-1 no ciclo, combinadas com duas adubações na semeadura (com e sem adição da adubação recomendada na semeadura), em três repetições por tratamento. Foram feitas seis coletas do material percolado durante o ciclo da cultura e realizadas determinações de cobre e zinco. No solo, foram feitas três coletas em cada...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reúso de água; Lixiviação; Lisímetros.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200017

Crop coefficient and water consumption of eggplant in no-tillage system and conventional soil preparation
Provedor de dados: 70
Autores: Carvalho,Daniel F. de; Lima,Marcio E. de; Oliveira,Alexsandra D. de; Rocha,Hermes S. da; Guerra,José G. M.
Under organic management in Seropédica-RJ, Brazil, using a weighing lysimeter, the crop coefficients (kc), the maximum evapotranspiration and the productivity of eggplant cultivation under two cropping systems (no tillage with straw plus soil with conventional preparation) were determined. A whole randomized layout with two treatments (no tillage and conventional) and five replicates during 134 days of cultivation were adopted. There were no significant differences in the eggplant cultivation in the two cropping systems, with a maximum commercial productivity obtained from 47.42 Mg ha-1 for the no-tillage system, and 47.91 Mg ha-1 for the conventional tillage. The accumulated ETc was 285.15 and 323.44 mm for the no-tillage and conventional, respectively....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solanum melongena L.; Weighing lysimeter; Irrigation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400018

Planejamento energético rural assistido por computador
Provedor de dados: 70
Autores: Borges Neto,Manuel R.; Carvalho,Paulo C. M. de.
Este trabalho traz o desenvolvimento de ferramenta computacional de auxílio ao planejamento energético na eletrificação rural, tendo como referência os principais softwares disponíveis no mercado mundial e citados na literatura científica. Após identificar as principais limitações dos mesmos, obteve-se um produto em português, que compara a extensão da rede convencional de energia elétrica às principais modalidades de geração elétrica de pequeno porte em uso no Brasil. Traz a inovação do dimensionamento e do uso da geração de energia elétrica a partir da produção de biogás no local. Para validação do programa, foram comparados os resultados obtidos pela mesma em dois estudos de casos reais de eletrificação rural.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energia; Fontes renováveis; Geração descentralizada.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200001

Partida de um reator anaeróbio horizontal para tratamento de efluentes do processamento dos frutos do cafeeiro
Provedor de dados: 70
Autores: Borges,Alisson C.; Pereira,Priscila dos A.; Matos,Antonio T. de.
O presente estudo teve o objetivo de avaliar a partida e a adaptação de um reator anaeróbio horizontal de leito fixo (RAHLF) no tratamento de águas residuárias do processamento primário dos frutos do cafeeiro (ARC). O reator foi construído com tubos de PVC de 0,2 m de diâmetro e 3,2 m de comprimento. O sistema foi preenchido com cubos de espuma de poliuretano para imobilização de biomassa ativa. O reator apresentou volume total de 0,1 m³ e volume útil equivalente a 0,04 m³. Em média, houve remoção de 49% da matéria orgânica, com o reator trabalhando sob carga orgânica volumétrica média de 2,66 kg m-3 d-1, medida como DQO. A suplementação de alcalinidade, somada à inoculação prévia de biomassa, proporcionou partida estável do RAHLF, confirmada pelo consumo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biomassa imobilizada; Digestão anaeróbia; Efluentes agroindustriais; Cafeicultura.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400016

Assistência de ar e volumes de aplicação na deposição de calda e no controle do arroz vermelho (Oryza sativa L.)
Provedor de dados: 70
Autores: Vigano,Leopoldo L. S.; Raetano,Carlos G.
O trabalho teve como objetivo avaliar o efeito da assistência de ar junto à barra pulverizadora e de três volumes de pulverização na dessecação e deposição da calda em arroz vermelho, sob cultivo de nabo forrageiro, em áreas de recuperação de várzeas, utilizando o herbicida paraquat e o corante Azul Brilhante, respectivamente. Os volumes de pulverização foram 100; 200 e 300 L ha-1 da solução aquosa, contendo corante alimentício (1.500 mg L-1). Com ou sem a assistência de ar junto à barra, foram utilizadas pontas de pulverização de jato plano tipo AXI 110015 à pressão de 117,3 kPa, AXI 11002 e AXI 11003 a 276 kPa. A avaliação da deposição da pulverização deu-se em folhas de plantas de arroz vermelho. Os maiores volumes (200 e 300 L ha-1) pulverizados com a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Controle químico; Herbicida.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400017

Internal ambience of bee colonies submitted to strengthening management by adding broods
Provedor de dados: 70
Autores: Brasil,Daniel de F.; Guimarães,Michelle de O.; Barbosa Filho,José Antonio D.; Freitas,Breno M.
This study aimed to investigate the ideal brood area to be introduced for strengthening Apis mellifera colonies, considering variations in the hive's internal ambience. Therefore, eight colonies were equipped with data loggers for recording variations in temperature and humidity inside the hives. Then, these colonies were split in four treatments involving the swapping of four, three, two and one brood comb between strong and weak colonies. Growth in the amount of brood and food stores to the four colony strengthening treatments was assessed counting the comb cells to record changes in the brood and food area. The colonies tended to restore their normal thermoregulation within four hours after they had been manipulated and the hive cover had been closed,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Colony homeostasis; Thermal comfort; Colony management.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500002

Using data mining to identify factors that influence the degree of leg injuries in broilers
Provedor de dados: 70
Autores: Cordeiro,Alexandra F. da S.; Baracho,Marta dos S.; Nääs,Irenilza de A.; Nascimento,Guilherme R. do.
Locomotor problems prevent the bird to move freely, jeopardizing the welfare and productivity, besides generating injuries on the legs of chickens. The objective of this study was to evaluate the influence of age, use of vitamin D, the asymmetry of limbs and gait score, the degree of leg injuries in broilers, using data mining. The analysis was performed on a data set obtained from a field experiment in which it was used two groups of birds with 30 birds each, a control group and one treated with vitamin D. It was evaluated the gait score, the asymmetry between the right and left toes, and the degree of leg injuries. The Weka ® software was used in data mining. In particular, C4.5 algorithm (also known as J48 in Weka environment) was used for the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Decision tree; Poultry; Gait score.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400003

Desenvolvimento do feijoeiro sob o uso de biofertilizante e adubação mineral
Provedor de dados: 70
Autores: Galbiatti,João A; Silva,Flávia G. da; Franco,Claudenir F; Caramelo,Anaira D.
A produção intensiva de alimentos exige manejo adequado do solo para garantir a produtividade e a sustentabilidade ambiental. Uma das alternativas é a utilização de resíduos orgânicos no desenvolvimento das culturas, diminuindo a dependência de adubos minerais. Com o objetivo de avaliar o desenvolvimento da cultura de feijão (Phaseolus vulgaris L.), utilizando biofertilizante e adubação mineral, conduziu-se o experimento com seis tratamentos dispostos ao acaso, em esquema fatorial, em quatro blocos, com parcelas de 8,0 x 5,0 m. Os tratamentos sob solo cultivado com a cultura de feijão caracterizaram-se como: com e sem biofertilizante (CB e SB, respectivamente) e para a adubação mineral foram utilizadas a dose recomendada no plantio, ½ dose de adubação e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biofertilizante; Adubação orgânica; Feijão; Phaseolus vulgaris.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100017

ERRATUM
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601275

Nutrientes no solo e na solução do solo na citricultura fertirrigada por gotejamento
Provedor de dados: 70
Autores: Souza,Thais R. de; Bardiviesso,Diógenes M.; Andrade,Thomas F. de; Villas Bôas,Roberto L.
A análise da solução do solo vem mostrando-se um método promissor de diagnóstico da fertilidade de solo, principalmente em sistemas de fertirrigação. O objetivo deste estudo foi avaliar o comportamento dos nutrientes no solo e na solução do solo, quando fornecidas cinco doses de N, P2O5 e K2O (0; 25; 50; 100 e 200% da dose recomendada) via fertirrigação. O experimento foi conduzido por três safras em laranjeiras Valência enxertadas sobre citrumelo Swingle. O solo e a solução do solo foram coletados ao final do período de fertirrigação de cada safra. As doses de N, P2O5 e K2O aplicadas proporcionaram redução nos valores de pH do solo e da solução do solo, porém a variação dos valores de pH da solução do solo foi 3,5 vezes maior que a observada no solo. Para...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrus sinensis; Extrator de solução do solo; Fertilidade do solo.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300484

CLASSIFICATION OF ROBUSTA COFFEE FRUITS AT DIFFERENT MATURATION STAGES USING COLORIMETRIC CHARACTERISTICS
Provedor de dados: 70
Autores: Costa,Anderson G.; Sousa,Daniela A. G. de; Paes,Juliana L.; Cunha,João P. B.; Oliveira,Marcus V. M. de.
ABSTRACT Coffee growers who produce the robusta species (Conilon) have sought to increase productivity and drink quality by improving production techniques. Artificial vision systems can assist in increasing the efficiency of operations associated with crop management. This study aimed to obtain colorimetric characteristics of robusta coffee fruits at different stages of maturity and use them for classifying fruits from digital images. A digital camera with spectral resolution in the visible was used to acquire images from 60 samples of coffee fruits at the green, cherry, and over-ripe stages of maturity. Colorimetric variables were extracted from the RGB, HIS, and L*a*b* color models and correlated with the physicochemical attributes of the fruits. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Artificial vision systems; Coffea canephora; Principal component analysis.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400518

Discriminação entre estágios nutricionais na cultura do trigo com técnicas de visão artificial e medidor portátil de clorofila
Provedor de dados: 70
Autores: Sena Júnior,Darly G. de; Pinto,Francisco de A. de C.; Queiroz,Daniel M. de; Santos,Nerilson T.; Khoury Júnior,Joseph K.
O ajuste da adubação nitrogenada é um tema que suscita preocupações econômicas e ambientais em todo o mundo. Isso decorre da elevada resposta das culturas, especialmente gramíneas, ao nitrogênio e da falta de métodos adequados de quantificação de sua disponibilidade no solo. Com o objetivo de avaliar a discriminação de três estágios nutricionais na cultura do trigo, foram utilizadas imagens digitais e um medidor portátil de clorofila (SPAD -502). Os dados foram coletados em três épocas (8; 14 e 20 dias após a adubação nitrogenada em cobertura - DAA), em parcelas de trigo submetidas a três doses de N (0; 30 e 60 kg ha-1). As imagens foram processadas para desenvolvimento dos classificadores multivariados, utilizando-se de nove índices espectrais com as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Taxas variáveis; Processamento de imagens.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100019

Effect of a simulated heat wave in thermal and aerial environment broiler-rearing environment
Provedor de dados: 70
Autores: Vale,Marcos M. do; Moura,Daniella J. de; Nääs,Irenilza de A.; Curi,Thayla M. R. C.; Lima,Karla A. O.
ABSTRACT Global warming increases the occurrence of events such as extreme heat waves. Research on thermal and air conditions affecting broiler-rearing environment are important to evaluate the animal welfare under extreme heat aiming mitigation measures. This study aimed at evaluating the effect of a simulated heat wave, in a climatic chamber, on the thermal and air environment of 42-day-old broilers. One hundred and sixty broilers were housed and reared for 42 days in a climatic chamber; the animals were divided into eight pens. Heat wave simulation was performed on the 42nd day, the period of great impact and data sampling. The analyzed variables were room and litter temperatures, relative humidity, concentrations of oxygen, carbon monoxide and ammonia...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ammonia; Gas production; Animal welfare; Oxygen; Litter temperature.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200271

Geometry and head loss in Venturi injectors through computational fluid dynamics
Provedor de dados: 70
Autores: Manzano,Juan; Palau,Carmen V.; Benito,M. de Azevedo; Guilherme,V. do Bomfim; Vasconcelos,Denise V.
ABSTRACT To determine the influence of geometry on the hydrodynamic behavior of Venturi injectors, using computational fluid dynamics techniques, we studied, at the Universitat Politècnica de València, Valencia, Spain, the geometric parameters that exert the most influence on head losses: the relationship between throat diameter and nozzle (β), nozzle angle (α1) and diffuser angle (α2). In addition, three throat morphologies (B1: nozzle-throat and throat-diffuser with a sharp edge; B2: nozzle-diffuser with a zero-length, sharp-edge throat; B3: nozzle-throat and throat-diffuser with rounded edge). We analyzed their influence on the velocity distribution and differential pressure between inlet and throat (DP/γ), throat and outlet (Δhv/γ), and outlet and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chemigation; Fertirrigation; DFC.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300482

MERCURY IN THE SEDIMENT OF THE UPPER PARNAÍBA RIVER
Provedor de dados: 70
Autores: Remor,Marcelo B.; Sampaio,Silvio C.; Rosa,Danielle M.; Model,Kathleen J.; Paloschi,Cristiane L.; Conceição,Fagner G. da.
ABSTRACT The contamination of aquatic environments with chemical trace elements can be evaluated by their accumulation in sediments of the water body. Studies on mercury require the use of exclusive extraction techniques that have relatively high costs when compared to the analysis of other trace elements. This study was conducted aiming at determining the mercury concentration in sediments of the Upper Parnaíba River basin, located in a region of agricultural expansion between the states of Piauí and Maranhão. The sediment was collected at 12 sites in the basin. After drying, the quantification of total mercury was performed by the Zeeman atomic absorption spectrometry coupled to a pyrolysis reactor. Mercury concentrations in sediments of the Parnaíba...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Trace elements; Agricultural frontier; Heavy metal.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500760

SOIL COMPACTION AND THE STABILITY OF LEVEES OF AQUACULTURE PONDS
Provedor de dados: 70
Autores: Magalhães,Esner R. S.; Freitas,Carlos E. de C.; Neves Junior,Afrânio F.; Silva Filho,Francisco C. da.
ABSTRACT The aim of this work was to evaluate the effects of variations in soil compaction on the stability of the slope embankments of fish farms used in aquaculture. Computational modeling was performed using the RocScience Slide 6.0 program, simulating filling scenarios, fast lowering and stationary regimes for the full operation of the fish farms. The data used in these simulations were obtained from soil characterization tests in the laboratory. The geometry of the levees, the inclination of the slopes and the crest width and height, also necessary for modeling, were obtained from field data and technical projects. The modeling generated a safety factor (SF) for the upstream and downstream slopes of the levees, considering different upstream slopes,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aquaculture; Fish farming; Soils; Levees; Stability.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500555

EFFECTIVE POWER AND HOURLY FUEL CONSUMPTION DEMANDED BY SET TRACTOR- COFFEE HARVESTER IN FUNCTION OF ADEQUACY TRACTOR BALLASTING
Provedor de dados: 70
Autores: Tavares,Tiago de O.; Damasceno,André F.; Voltarelli,Murilo A.; Silva,Rouverson P. da; Furlani,Carlos E. A.
ABSTRACT: The mechanized gathering process of sweeping coffee is extremely important to reduce the losses of fruit not used in the harvesting operation. But this operation usually has a low operational performance and a high cost per unit collected in this way any measures that can effectively reduce costs increase the viability of the operation. In this sense, studies on adequacy tractor mass for each operation show improvement in energy use, reducing fuel consumption. So, this study aimed to quantify the fuel consumption and effective power along the process of a tractor 4x2 FWD pulling the coffee harvester. I was used as treatments three ballasting settings, these being equivalent the relations power to weight of 36, 39 and 42 kg hp-1 working with and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dynamic mass equilibrium; Power-weight ratio; Front wheel assist.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400699

Environmental adaptation of the source of the subbasin of Rico Stream, Monte Alto - SP, Brazil
Provedor de dados: 70
Autores: Pissarra,Teresa C. T.; Marcussi,Aline B.; Leão,Gilberto da R.; Galbiatti,João A.; Borges,Mauricio J.; Campos,Sergio.
The aim of this study was to define the photographic patterns that represent the use and occupation of the landcover of the "spring" of the Rico Stream subbasin, located at Monte Alto, state of São Paulo (SP), Brazil, for environmental adaptation regarding the Brazilian Forest Law. The mapping was performed using remote sensing techniques and visual interpretation of the World View image, followed by the digitalization of the net of drainage and vegetation (natural and agricultural) at the AutoCad software with documents and field work. The study area has 2141.53 ha and the results demonstrated that the main crop is sugarcane with 546.34 ha, followed by 251.22 ha of pastures, 191.71 ha of perennial crops, 57.31 ha of Eucalyptus and 49.52 ha of onion,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mapping; Land use and occupation; Vegetal coverage.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200009

USING SOUNDS PRODUCED BY PIGS TO IDENTIFY THERMONEUTRALITY ZONES FOR THERMAL ENVIRONMENT ASSESSMENT RATIOS
Provedor de dados: 70
Autores: Amaral,Pedro I. S.; Campos,Alessandro T.; Yanagi Junior,Tadayuki; Cecchin,Daiane; Leite,Evandro M.; Dias e Silva,Nhayandra C.
ABSTRACT Although dry bulb temperature (T) is the environmental variable most commonly used to classify thermal comfort in pigs, environmental assessment ratios provide more accurate information. The objective of this study was to correlate the sound pressure levels (SPL) produced by piglet vocalization with the thermal environment observed during the nursery phase, and subsequently establish thermoneutrality ranges. The experiment was conducted on a pig farm where T, relative humidity (RH), and SPL data were recorded between 9 am-5 pm for 42 days. The association between SPL and T in nursery phase piglets was verified; for thermal comfort to be possible, SPLs were 56.3 to 60.3 dB. The SPLs were subsequently used in predictor equations of ratios, and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Animal welfare; Nursery; Rearing; Thermal comfort.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300266

PHOTOCHEMICAL AND PRODUCTIVE PERFORMANCE OF YELLOW PASSION FRUIT IRRIGATED IN THE BRAZILIAN SEMIARID
Provedor de dados: 70
Autores: Dutra,Alexson F.; Melo,Alberto S. de; Brito,Marcos E. B.; Suassuna,Janivan F.; Dutra,Wellison F.
ABSTRACT The drought stress is an important factor for crops in areas with low rainfall as in the semiarid regions and affects immediately the physiological processes and plant production. However, irrigation is an essential practice to minimize effects of drought stress since the appropriate management is done it can increase the farm income. This study aimed to analyze the photochemical and productive performance of passion fruit (Passiflora edulis) hybrid ‘BRS Gigante Amarelo' irrigated in a Brazilian semiarid region. It was studied four water replacement rates (33, 66, 100 and 133% of ETo) at field conditions. A randomized block design was used with five replications and the fluorescence of chlorophyll a, yield and fruit quality were evaluated. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Passiflora edulis; Drought stress; Chlorophyll fluorescence; Production.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600901

Performance of spray nozzles in land applications with high speed
Provedor de dados: 70
Autores: Zaidan,Samir E.; Gadanha Jr,Casimiro D.; Gandolfo,Marco A.; Pontelli,Cristiano O.; Mosquini,Walter W.
The aim of this study was to evaluate different spray nozzles for land applications in high speed on the coverage and deposit in soybean plants pulverization. It was evaluated the AXI 110 04 plane jet nozzles operated at speed of 4.17m.s-1 (control), the grey APE and the AXI 110 08 plane jets, and the TD HiSpeed 110 06 and AXI TWIN 120 06 twin jets, at speed of 9.72m.s-1. The application volume was fixed in 120L ha-1. The application efficiency was evaluated by two different methods: analysis of the coverage area using fluorescent pigment and UV light and analysis of deposits through the recovery and quantification of FD&amp;C N°1 brilliant blue marker by spectrophotometry. Both analyses were done in samples collected from top, middle and bottom parts of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spray nozzles; Speed; Soybean; Pulverizer.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600014

Coverage mobilization in the sowing line and its influence on temperature and water content and on maize emergence
Provedor de dados: 70
Autores: BRANDELERO,EVANDRO M.; ARAÚJO,AUGUSTO G. DE; RALISCH,RICARDO.
Straw on sowing line modifies seed germination environment regarding temperature and water content. Given these considerations, the aim of this study was to evaluate different mechanisms for coverage mobilization on the sowing line and their effect on germination environment of maize seeds, mainly in relation to the dynamics of straw in the seedbed, water content and soil temperature. Treatments consisted on the combination of two mechanisms at front of furrow opener, composed of cutting disc and row cleaners, with three mechanisms behind the seed furrower for returning the soil, consisting of three covering mechanisms, commercial and prototype models. It was found that straw presence on the surface of sowing line contributed to germination of maize seeds,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: No-tillage planting; Germination environment; Furrowers; Soil coverage.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100098

Portable flow board for storage of fruits and vegetables in mini-chambers with controlled atmosphere
Provedor de dados: 70
Autores: Carmelo,Luis G. P.; Becaro,Aline A.; Ferreira,Marcos D.; Calbo,Adonai G.
ABSTRACT A portable flow board system was developed in the present study with the aim to facilitate lab-scale experiments of controlled atmosphere (CA) with fruits and vegetables. This sturdy flow board combines ease fabrication, low cost and gas economy. Its functionality is provided by manifolds and gas mixers. Each gaseous component is supplied by a gas cylinder through a differential valve of adjusted pressure control, generally at 6 kPa, and forced through 13 standardized restrictors coupled to each manifold output. Controlled atmospheres are then formed with one, two or three gases in 13 gas mixers affixed to the flow board base, which are further conducted through flexible tubes to storage mini-chambers that can also be used to study metabolic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Flow-board; Flux control; Gas flow; Method; Gas mixer; Restriction.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601105

Quality of beans stored under hermetic conditions
Provedor de dados: 70
Autores: Freitas,Romenique da S; Faroni,Lêda R. DA; Sousa,Adalberto H; Cecon,Paulo R; Carvalho,Marcela S.
This study aimed to evaluate the quality of beans (Phaseolus vulgaris L.) stored with different moisture contents under hermetic conditions. Beans with 12.3%, 15.7%, and 17.8% moisture content were used in the experiment. They were packed in bag type silos (3 kg), PET bottles (1.5 L), and glass containers (3 L), covered with organza fabric (control), and stored at 25 ºC and 70±5% relative humidity, for 120 days. The evaluated characteristics included moisture content, apparent density, electrical conductivity, germination percentage, cooking time, and bean classification, every 30 days. Except for the electrical conductivity and cooking time, the other characteristics were kept for 120 days in the stored product with moisture contents of 12.3% and 15.7% in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus vulgaris L; Modified atmosphere; Bag silo; PET bottles.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600011

AMBIENCE OF SHEEP SUBMITTED TO DIFFERENT BREEDING ENVIRONMENTS AND GLOBAL TEMPERATURES
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Santos,Luana de Fátima D. dos; Nascimento,José W. B. do; Lopes,Fernanda F. M.; Costa,José H. S.
ABSTRACT The aim is to characterize and to compare the black (TBG) and gray (TGG) globe temperatures in the production of sheep in the Brazilian semi-arid, using Santa Inês and Doper breeds, distributed in two thermal environments (exposed to the sun and shaded), containing 10 animals in each picket. The experimental design was completely random, 2 x 2 factorial scheme (shaded environment and sun x black and gray globe) in 46 replicates (evaluation days). There was an increase of the TBG in relation to the TGG during the evaluation times, with maximum temperature (48.1°C) at 1p.m. in the environment exposed to the sun, concomitantly with elevation of the black globe temperature and humidity index - BGHI (96.7). The result was distinct for TGG, with a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Heat absorption; Surface coloring; BGHI.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600829

Rotina computacional para a determinação da velocidade de sedimentação das partículas do solo em suspensão no escoamento superficial
Provedor de dados: 70
Autores: Oliveira,Luiz F. C. de; Martinez,Mauro A.; Pruski,Fernando F.; Griebeler,Nori P.; Oliveira,Geraldo C. de.
O presente trabalho teve como objetivo desenvolver uma rotina computacional para a determinação da velocidade de deposição de partículas em suspensão no escoamento superficial, verificar sua aplicação por intermédio de modelo de transporte de sedimentos e comparar os resultados obtidos com dados experimentais. Empregou-se na rotina o processo iterativo de Newton-Rapshon para a solução das equações empregadas na determinação da velocidade de deposição de partículas em suspensão no escoamento superficial, e na solução da equação do transporte de sedimentos empregou-se a técnica das diferenças finitas. Essas rotinas foram empregadas na implementação do modelo MTSES (Modelo para Transporte de Solutos no Solo e no Escoamento Superficial). As velocidades de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão; Escoamento superficial; Modelagem.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100014

Tratamento das águas do processamento dos frutos do cafeeiro em filtro anaeróbio seguido por sistema alagado construído: II - remoção de nutrientes e compostos fenólicos
Provedor de dados: 70
Autores: Fia,Ronaldo; Matos,Antonio T. de; Lambert,Túlio F.; Fia,Fátima R. L.; Matos,Mateus P. de.
Seis sistemas de tratamento foram compostos por três filtros anaeróbios com escoamento descendente, seguidos por seis sistemas alagados construídos (SACs), sendo avaliados, sob o ponto de vista operacional, no tratamento da água residuária do processamento dos frutos do cafeeiro (ARC). Os filtros foram confeccionados em PVC (1,5 m de altura e 0,35 m de diâmetro) e preenchidos com brita nº 2 e os SACs foram constituídos por caixas de madeira (1,5 m de comprimento, 0,4 m de altura e 0,5 m de largura), sendo impermeabilizados e preenchidos com brita "zero". A ARC teve o pH corrigido com cal até valores próximos a 7,0, e a concentração de nutrientes alterada, com a adição de fertilizantes, de forma a se obter uma relação DBO/N/P igual a 100/5/1. Em metade dos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tratamento anaeróbio; Wetlands construídos; Água residuária agroindustrial; Compostos fenólicos; Café.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600020

Stabilization of confined beef cattle manure: characteristics of produced fertilizers
Provedor de dados: 70
Autores: LORIN,HIGOR E. F.; COSTA,MÔNICA S. S. DE M.; COSTA,LUIZ A. DE M.; PEREIRA,DERCIO C.; CARNEIRO,LEOCIR J.
ABSTRACT The growing demand for animal protein is directly related to the feedlot system of animals and their assumptions, such as the waste management. The characterization of the final products becomes an important factor in decision making by one or by other process. The objective was highlight characteristics that fertilizers present due to the used of stabilization process, by the principal component analysis. For the manure stabilization we realized three aerobic processes, composting, vermicomposting and natural decomposition, and one anaerobic, the anaerobic digestion. These processes produced the compost, the vermicompost, the decomposed manure and the biofertilizer. Fertilizers produced were analyzed by means of seventeen chemical and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biofertilizer; Cattle manure; Compost; Vermicompost; Stability.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500877

Intensity-duration-frequency ratios obtained from annual records and partial duration records in the locality of Pelotas - RS, Brazil
Provedor de dados: 70
Autores: Teixeira,Claudia F. A.; Damé,Rita de C. F.; Rosskoff,José L. C.
The intensity-duration-frequency occurrence ratio (IDF) is a tool commonly used for precipitation-runoff data transformation, which is established from observations of intense precipitations over a period sufficiently long as to allow the occurrence of extremes at the observation site. This study focused on verifying the existence or absence of new data, in terms of IDF ratio, by using partial duration records produced from data on maximum daily disaggregated rainfall for pre determined durations. The partial duration records considered a base value of 55 mm, totaling 279 values. After the rainfall series were established, their independence and seasonality were assessed. Using the Student's t-test statistics, it was established that no new data, as IDF...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Maximum rainfall; Daily disaggregated precipitation; Probability models.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400007

Atividade respiratória, produção de etileno e vida útil de repolho (Brassica oleracea, var. capitata) minimamente processado em atmosfera controlada
Provedor de dados: 70
Autores: Rinaldi,Maria M.; Benedetti,Benedito C.; Moretti,Celso L.
Com o objetivo de avaliar a atividade respiratória e a produção de etileno do repolho inteiro e minimamente processado e a vida útil do repolho mimimamente processado em atmosfera controlada, realizaram-se dois experimentos em etapas seqüenciais. Na primeira etapa, avaliaram-se a atividade respiratória e a produção de etileno do repolho inteiro e minimamente processado, em sistema fechado, nas temperaturas de 5 ºC e 10 ºC. Na segunda etapa, avaliou-se a vida útil do repolho minimamente processado em atmosfera controlada. O produto foi submetido a fluxo contínuo de misturas gasosas ternárias, com concentrações de 2% a 10% de O2 e de 3% a 10% de CO2, previamente umidificadas, na temperatura de 5 ºC por 10 dias. Como controle, foi utilizado o ar atmosférico....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Processamento mínimo; Armazenamento; Temperatura.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300018

Padrão de distribuição de K+, Ca++, Mg++ e P no solo de um pomar de citros em função da fertirrigação
Provedor de dados: 70
Autores: Laurindo,Valério T.; Silva,Guilherme O.; Pavani,Luiz C.; Quaggio,José A.
Em solos tropicais, a distribuição dos nutrientes no solo em função da fertirrigação realizada por meio de irrigação localizada (gotejamento e/ou microaspersão), na cultura de citros, é pouco conhecida. Este trabalho teve por objetivo avaliar os padrões de distribuição de potássio, cálcio, magnésio e fósforo em solo tropical, em função da fertirrigação, aplicada por dois sistemas de irrigação localizada (microaspersão e gotejamento), sendo que o sistema por gotejamento era composto por uma e duas linhas laterais por linha de plantas, e o de microaspersão por apenas uma linha, e com três dotações hídricas (100%, 75% e 50%) da evapotranspiração da cultura (ETc), em um pomar de laranjeira. As fontes de fertilizantes utilizadas na fertirrigação foram o nitrato...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Macronutrientes; Lixiviação; Gotejamento; Microaspersão.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500013

Alteração do campo visual em função do uso de cabinas em tratores agrícolas
Provedor de dados: 70
Autores: Schlosser,José F.; Dallmeyer,Arno; Debiasi,Henrique; Menegas,Mauro T.; Nietiedt,Gustavo H.
Com o objetivo de avaliar a alteração do campo visual de um trator, ocasionada pela instalação de uma cabina, foram determinadas as áreas de visibilidade nula em função da presença ou não da mesma, para cada campo visual. Os procedimentos adotados basearam-se na norma ISO 5721-1981 - Agricultural tractors - Operator's field of vision. A cabina aumentou em 34,42% a área de visibilidade nula. A relação área de projeção do trator/área total sombreada foi de 0,075 para o trator sem cabina, e 0,057 para o trator com cabina, indicando as melhores condições de visibilidade do primeiro em relação ao segundo. No que se refere aos campos visuais, a maior redução ocorreu no campo visual dos olhos e no obtido com o movimento da cabeça, em função dos suportes da cabina...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Campo visual; Tratores agrícolas; Ergonomia.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200016

Recycling of nutrients with application of organic waste in degraded pasture
Provedor de dados: 70
Autores: Silva,Adriane de A.; Costa,Adriana M. da; Lana,Regina M. Q.; Lana,Ângela M. Q.
The utilization of organic wastes represents an alternative to recover degraded pasture. The experiment aimed to assess the changes caused by the provision of different organic waste (poultry litter, turkey litter and pig manure) in a medium-textured Oxisol in Brazilian Savanna under degraded pasture. It was applied different doses of waste compared to the use of mineral fertilizers and organic mineral and evaluated the effect on soil parameters (pH, organic matter, phosphorus and potassium) and leaf of Brachiariadecumbens (crude protein, phosphorus and dry mass production). It was observed that application of organic waste did not increase the level of soil organic matter and pH in the surface layer, and the application of turkey litter caused...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry litter; Swine manure; Soil chemistry; Nutrient uptake.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200020

Mapeamento multitemporal da cobertura de terra, por meio de árvore de decisão, na bacia hidrográfica do rio Marombas-SC
Provedor de dados: 70
Autores: Caten,Alexandre Ten; Safanelli,José L.; Ruiz,Luis F. C.
RESUMO O conhecimento sobre a cobertura da terra é fundamental como informação para o planejamento e o estudo dos efeitos da substituição de paisagens naturais por paisagens antropizadas. Este estudo objetivou analisar a dinâmica da cobertura da terra entre os anos de 1989 e 2011, na bacia hidrográfica do rio Marombas (SC), empregando o classificador árvore de decisão (AD). Foram utilizadas bandas espectrais do satélite Landsat 5, índices de vegetação e atributos de terreno extraídos do modelo digital de elevação. Esses dados foram utilizados como atributos de classificação da cobertura da terra, nos anos de 1989, 1991, 1993, 1997, 2001, 2004 e 2011. A qualidade do classificador AD foi avaliada por um conjunto de 500 pontos aleatórios e independentes,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensoriamento remoto; Classificação supervisionada; Uso da terra; Mineração de dados.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601198

Conhecimento da disponibilidade hídrica natural para a gestão dos recursos hídricos
Provedor de dados: 70
Autores: Pruski,Fernando F; Rodriguez,Renata del G; Souza,João F; Silva,Bruno M. B. da; Saraiva,Isabel S.
O uso da vazão natural permite representar as condições naturais existentes na bacia e sua evolução ao longo dos anos; entretanto, por ser este um assunto de preocupação recente, pouco se conhece sobre o impacto do uso dessas vazões em estudos hidrológicos. Tendo em vista a importância do conhecimento das vazões naturais, o presente trabalho teve como objetivo avaliar o efeito do uso destas vazões em relação às vazões observadas para a bacia do Paracatu. O impacto do uso das vazões naturais foi estimado para as vazões média de longa duração e as mínimas (Q7,10 e Q95), sendo feitas uma análise pontual e uma espacial. A análise pontual foi feita nas seções onde se localizam as estações fluviométricas; já a espacial engloba toda a hidrográfica da bacia do Rio...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recursos hídricos; Ações antrópicas; Vazão natural.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100007

USE OF AIC AND BIC IN DESORPTION ISOTHERMS OF TAMARIND SEEDS (Tamarindus indica L.)
Provedor de dados: 70
Autores: Ferreira Junior,Weder N.; Resende,Osvaldo; Pinheiro,Gleyce K. I.; Silva,Ligia C. de M.; Costa,Eduarda R.
ABSTRACT The knowledge of hygroscopicity is essential for the storage of tamarind seeds, but there is a limitation of a judicious statistical parameter to define the best mathematical model to adjust the isotherms of plant products. Therefore, this study aimed to determine the desorption isotherms of tamarind seeds and test the Akaike information criterion (AIC) and Schwarz Bayesian information criterion (BIC) for choosing the best mathematical model. Seeds with an initial moisture content of 21.00 ± 0.10% dry basis (db) were dried at 45 °C until they reached moisture contents of 17.27 ± 0.10, 15.04 ± 0.16, 14.14 ± 0.06, 12.41 ± 0.17, and 10.52 ± 0.12% db. The water activity of the product was determined by the static-indirect method at temperatures of 10,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water activity; Hygroscopicity; Cavalcanti Mata.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400511

Estimativa da demanda de água nas áreas irrigadas da bacia do rio Paracatu
Provedor de dados: 70
Autores: Rodriguez,Renata del G.; Pruski,Fernando F.; Novaes,Luciano F. de; Ramos,Márcio M.; Silva,Demetrius D. da; Teixeira,Alessandro de F.
A irrigação apresentou expressivo crescimento na bacia do Paracatu na década de 1970, sendo que, como conseqüência da grande expansão da agricultura irrigada, sérios conflitos têm surgido em várias partes da bacia. Tendo em vista esses conflitos, o presente trabalho teve como objetivo analisar a demanda de água pela irrigação e sua sazonalidade para as condições climáticas da bacia do Paracatu. A demanda de água pela irrigação foi realizada com base nas condições climáticas e nas áreas irrigadas de cada cultura, sendo essas obtidas com base nos dados do censo agropecuário do Instituto Brasileiro de Geografia e Estatística. A vazão média anual retirada pela irrigação na bacia do Paracatu, em 1996, foi de 0,15 L s-1 ha-1, sendo a vazão média retirada no mês...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiração; Precipitação efetiva; Vazão retirada pela irrigação.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100011

Determinação em tempo real da magnitude de danos físicos por impacto em linhas de beneficiamento e em condições de laboratório e seus efeitos na qualidade de tomate
Provedor de dados: 70
Autores: Ferreira,Marcos D.; Camargo,Gustavo G. de T.; Andreuccetti,Caroline; Moretti,Celso L.
O tomate de mesa é uma das principais hortaliças consumidas no Brasil e apresenta elevados índices de perdas pós-colheita. O objetivo deste trabalho foi avaliar a magnitude dos impactos verificados em linhas de beneficiamento para tomate de mesa, bem como determinar, em laboratório, as alterações na qualidade de tomates submetidos a danos físicos controlados em diferentes superfícies. Para a avaliação dos pontos críticos e registro da magnitude dos impactos, foi usada uma esfera instrumentada. Os pontos críticos de transferência demonstraram valores de aceleração entre 30 e 129 G (m s-2). Os testes laboratoriais evidenciaram que superfícies acolchoadas reduziram em até 31% a magnitude de impacto. A incidência de danos físicos internos foi crescente e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lycopersicon esculentum; Esfera instrumentada; Aceleração (G).
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400013

Influence of irrigation on wheat crop
Provedor de dados: 70
Autores: Flumignan,Danilton L.; Lena,Bruno P.; Faria,Rogério T. de; Scholz,Maria B. dos S.; Medina,Cristiane de C.
The use of irrigation has been increased significantly in wheat crops in Brazil. This study aims to evaluate the effect of irrigation on the productivity, on flour technological quality and on the wheat root system. In a field experiment conducted at IAPAR, in Londrina -state of Paraná (PR), Brazil, the IPR 118 cultivar was grown under sprinkler irrigation (Irrigated Treatment) and without irrigation (Non-irrigated Treatment). The productivity was determined by harvesting three samples of 25 m² per treatment. The same samples were used to evaluate the flour technological quality, considering, among other parameters, gluten strength (W). The evaluation of the root system was performed after the harvest, considering a profile of 0 to 45 cm of soil depth, and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Triticum aestivum L.; Spinkler; Productivity; Alveograph; Root system.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100009

Efeito das mudanças climáticas na disponibilidade hídrica da bacia hidrográfica do Rio Paracatu
Provedor de dados: 70
Autores: Mello,Eloy L. de; Oliveira,Fernanda A.; Pruski,Fernando F.; Figueiredo,Juliana C.
O aumento da demanda pelo uso da água na bacia do Rio Paracatu vem ocasionando sérios problemas ambientais e conflitos entre os usuários. Para a gestão mais eficiente dos recursos hídricos, é importante o conhecimento do comportamento hidrológico da bacia hidrográfica, no presente e no futuro, devido às fortes evidências de mudanças climáticas no planeta. O objetivo deste trabalho foi estimar a tendência de variação da disponibilidade hídrica na bacia hidrográfica do Rio Paracatu, até o final deste século, considerando dois cenários contrastantes de mudanças climáticas, um para altas emissões de CO2 (A2) e outro para baixas (B2). Para atingir esse objetivo, foi realizado o downscaling das precipitações mensais para os anos de 2001 a 2099, simulados pelo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Downscaling; Recursos hídricos; Vazões mínimas.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400003

Avaliação de classificadora de cilindros divergentes para tomate "Carmen"
Provedor de dados: 70
Autores: Atarassi,Márcia E; Ferreira,Marcos D; Braunbeck,Oscar A; Moretti,Celso L.
As normas de classificação garantem o mesmo padrão para produtores, atacadistas e consumidores finais, facilitando a comercialização, agregando valor ao produto e diminuindo as perdas. O objetivo deste trabalho foi avaliar uma classificadora de tomates in natura por diâmetro, por meio de cilindros rotativos divergentes com diferentes velocidades de rotação. Foram realizados ensaios para avaliar a eficiência da classificação, conformidade da classificação por diâmetro com a norma do PROGRAMA BRASILEIRO PARA A MODERNIZAÇÃO DA HORTICULTURA (2003) e incidência de danos mecânicos em tomates "Carmen". Os cilindros divergentes apresentaram conformidade de mistura na classificação por diâmetro, nas classes 60 e 80. Entretanto, para a classe 70, nenhum tratamento...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pós-colheita; Classificação; Lycopersicon esculentum Mill; Qualidade; Atividade respiratória.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200016

Water storage in wetted strips under irrigated coffee trees with different criteria of irrigation management
Provedor de dados: 70
Autores: Colombo,Alberto; Alvarenga,Lívia A.; Scalco,Myriane S.; Ribeiro,Randal C.; Abreu,Giselle F.
The increasing demand for water resources accentuates the need to reduce water waste through a more appropriate irrigation management. In the particular case of irrigated coffee planting, which in recent years presented growth with the predominance of drip irrigation, the improvement of drip irrigation management techniques is a necessity. The proper management of drip irrigation depends on the knowledge of the spatial pattern of soil moisture distribution inside the wetted strip formed under the irrigation lines. In this study, grids of 24 tensiometers were used to determine the water storage within the wetted strip formed under drippers, with a 3.78 L h-1 discharge, evenly spaced by 0.4 m, subjected to two different management criteria (fixed irrigation...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigated coffee planting; Tensiometers; Soil water storage.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200004

Ambiência aérea em alojamento de frangos de corte: poeira e gases
Provedor de dados: 70
Autores: Nääs,Irenilza de A.; Miragliotta,Miwa Y.; Baracho,Marta dos S.; Moura,Daniella J. de.
A qualidade do ar em ambientes de produção animal vem sendo referenciada como ponto de interesse em estudos de sistema de controle ambiental, focando tanto a saúde dos animais que vivem em total confinamento, quanto a dos trabalhadores. O objetivo do trabalho foi determinar a variação da qualidade da ambiência aérea em dois tipos de galpões criatórios de frangos de corte: convencional (Gc) e tipo túnel (Gt). Os valores de poeira total, em ambos os galpões, ofereceram condições adequadas às aves; entretanto, as concentrações de poeira respirável no ar estiveram acima do limite recomendado para humanos. A concentração de monóxido de carbono, na fase de aquecimento, esteve acima dos 10 ppm máximos recomendados, no período avaliado, sendo superior na época de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avicultura de corte; Poluentes aéreos; Saúde do trabalhador.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300001

SOWS AND PIGLETS THERMAL COMFORT: A COMPARATIVE STUDY OF THE TILES USED IN THE FARROWING HOUSING
Provedor de dados: 70
Autores: Machado,Sivanilza T.; Nääs,Irenilza De A.; Reis,João G. M. Dos; Caldara,Fabiana R.; Santos,Rodrigo C.
ABSTRACT The global animal production is increasing as expected to meet world demand for food, especially for meat products. This research aimed to investigate the effect of two types of roofs (clay and fiber-cement tiles) in a tropical area on the thermal comfort of farrowing sows and piglets. Twelve sows and forty-eight piglets were observed during summer in the Southeast region of Brazil. Climate variables, thermal comfort and surface temperature (sows and piglets) were assessed. The type of roofs clearly affected the piglets' surface temperature during all studied periods, but the results were not similar in the sows' surface temperature. Temperature and humidity index found was high in the building with fiber-cement tiles. The pen location in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pig production; Roof material; Surface temperature; Thermal comfort; Tropical conditions.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000600996

Aplicação da análise harmônica por séries de Fourier para a previsão de produtividade da cultura do café no Estado de Minas Gerais
Provedor de dados: 70
Autores: Carvalho,Luiz G. de; Sediyama,Gilberto C.; Cecon,Paulo R.; Alves,Helena M. R.
O objetivo deste trabalho foi obter um modelo de previsão de produtividade para a cultura do café, em sete municípios do Estado de Minas Gerais. Submeteram-se à análise harmônica por séries de Fourier, séries de produtividades representativas de cada município, das quais se extraíram os coeficientes até o sétimo harmônico, submetendo-os à regressão linear múltipla nos três primeiros componentes principais de um conjunto de 33 variáveis inerentes à produção cafeeira. Essas variáveis foram médias de 15 anos correspondentes aos mesmos anos das produtividades e subdivididos em quatro períodos trimestrais, ao longo do ciclo produtivo da cultura (julho a junho). O modelo mostrou-se inconsistente, apresentando erros das estimativas bastante discrepantes,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelagem agrometeorológica; Componentes principais; Balanço hídrico.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300019

EFFECT OF NOZZLES, APPLICATION RATES, AND ADJUVANTS ON SPRAY DEPOSITION IN WHEAT CROPS
Provedor de dados: 70
Autores: Machado,Willian A.; Silva,Sérgio M.; Carvalho,Stephan M.; Cunha,João P. A. R. da.
ABSTRACT The use of insecticides is common in pest management in wheat crops but may lead to higher production costs and environmental contamination. Therefore, a more comprehensive and uniform distribution of plant protection products in the desired target is recommended. The objective of this study is to evaluate the effect of different spray nozzles, application rates, and adjuvants on droplet spectrum and spray deposition in wheat crops. The physicochemical characteristics of the spray mixture, droplet spectrum, and spray deposition in wheat plants were evaluated. The lower application rate (75 L ha−1) combined with the use of the twin flat fan tip AS7030 and the adjuvant sodium lauryl ether sulfate (SLES) yielded droplets with a larger diameter....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Triticum aestivum; Application technology; Spray mixture volume; Droplet spectrum; Insecticide drift.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100083

Estimativa de parâmetros biofísicos de plantios de café a partir de imagens orbitais de alta resolução espacial
Provedor de dados: 70
Autores: Ramirez,Gláucia M.; Zullo Júnior,Jurandir.
O uso de recursos de sensoriamento remoto orbital constitui um grande avanço no levantamento de dados sobre a cafeicultura, sobretudo por seu caráter temporal e baixo custo. Sendo assim, o objetivo do trabalho foi avaliar a utilização da imagem do satélite QUICKBIRD na determinação de parâmetros biofísicos importantes para a cultura cafeeira. Foram utilizados 25 talhões com plantios de café localizados entre os municípios de Ribeirão Corrente, Franca e Cristais Paulista (SP). Os parâmetros biofísicos utilizados foram os espaçamentos entre linhas e plantas, altura, IAF, diâmetro da copa, porcentagem de cobertura vegetal, rugosidade, variedade e biomassa. Foram utilizados valores de refletância real das bandas espectrais do satélite QUICKBIRD e os índices de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Quickbird; IAF; Biomassa; Altura; Modelo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300011

Computational modeling for irrigated agriculture planning. Part I: general description and linear programming
Provedor de dados: 70
Autores: Borges Júnior,João C. F.; Ferreira,Paulo A.; Andrade,Camilo L. T.; Hedden-Dunkhorst,Bettina.
Linear programming models are effective tools to support initial or periodic planning of agricultural enterprises, requiring, however, technical coefficients that can be determined using computer simulation models. This paper, presented in two parts, deals with the development, application and tests of a methodology and of a computational modeling tool to support planning of irrigated agriculture activities. Part I aimed at the development and application, including sensitivity analysis, of a multiyear linear programming model to optimize the financial return and water use, at farm level for Jaíba irrigation scheme, Minas Gerais State, Brazil, using data on crop irrigation requirement and yield, obtained from previous simulation with MCID model. The linear...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation requirement; Financial return; Simulation model.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300008

Unidades combinadas RAFA-SAC para tratamento de água residuária de suinocultura – parte II nutrientes
Provedor de dados: 70
Autores: Amorim,Fabiana; Fia,Ronaldo; Silva,Juliano R. M.; Chaves,Camila F. M.; Pasqualin,Pedro P.
RESUMO Neste trabalho, avaliou-se o efeito combinado de duas unidades de tratamento na remoção de nitrogênio total Kjeldahl (NTK) e fósforo total (PT). As unidades avaliadas receberam alimentação contínua, sendo um reator anaeróbio de manta de lodo e fluxo ascendente tipo RAFA, com volume útil de 96 L, seguido de um sistema alagado construído (SAC) com capacidade para 237 L. O experimento foi conduzido em três fases, variando o tempo de detenção hidráulica (TDH) no reator anaeróbio de: 59 h, 19,5 h e 5 h, e no SAC 146 h, 48 h e 13 h, respectivamente, nas fases I, II e III. A carga orgânica volumétrica (COV) aplicada foi de 1,2; 1,3 e 13,0 kg m-3 d-1 de DQO no RAFA, e as taxas de aplicação superficial (TAS) no SAC foram de 120, 130 e 464 kg ha-1d-1 de NTK e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carga orgânica; Nutrientes; Taxa de aplicação superficial; Tratamento biológico; Wetlands.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500931

Teores de micronutrientes no solo e foliar com aplicação de fontes quelatadas e sulfatadas em feijão
Provedor de dados: 70
Autores: Silva,Adriane de A.; Couto Junior,Pedro A.; Lana,Angela M. Q.; Lana,Regina M. Q.
As fontes de micronutrientes apresentam, em geral, baixa disponibilidade no solo, e espera-se que o uso de fontes quelatadas aumente a absorção destes elementos. Objetivou-se comparar formulações de fertilizantes quelatizados e sulfatados, na absorção dos micronutrientes, zinco e cobre, com aplicação de diferentes doses na cultura do feijão. O experimento foi conduzido, na casa de vegetação da Universidade Federal de Uberlândia. Os fertilizantes utilizados foram fontes quelatadas e sulfatadas, nas doses de 0; 20; 40; 60 e 80 mg dm-3. Instalaram-se, em vasos com 3 kg de solo, os 2 ensaios independentes em DIC, em esquema fatorial 5 X 2, em que foi semeado feijão da variedade Pérola, sendo que, após 15 dias após emergência (DAE), realizou-se o desbaste,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus vulgaris L.; Cu e Zn; Quelato EDTA.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100004

SPRAY DRIFT AND PEST CONTROL FROM AERIAL APPLICATIONS ON SOYBEANS
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Barizon,Robson R. M.; Ferracini,Vera L.; Assalin,Marcia R.; Antuniassi,Ulisses R.
ABSTRACT Pesticide drift is an issue in modern farming, mainly for crops under constant spraying as soybeans. This study aimed at assessing drift and pest control for aerial applications in soybean crops. Hydraulic nozzles and rotary atomizers, regulated to a wide spectrum of droplet sizes, sprayed thiamethoxam plus lambda-cyhalothrin using an agricultural aircraft Ipanema 202A at volume rate of 20 L ha−1. Treatments consisted of testing two devices: a rotary cage atomizer (Micronair AU 5000) with blade angles of 65° for larger droplets, and with angle of 55° for smaller ones; and a set of adjustable nozzles (Stol model) with deflector angle of 90° for smaller droplets, and with angle of 30° for larger ones. Drift was evaluated through quantification of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural aviation; Crop protection; Exodrift; Glycine max.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300493

Utilização de 1-metilciclopropeno e resfriamento rápido na conservação de pêssegos
Provedor de dados: 70
Autores: Pinto,Lucia C. de B.; Jorge,José T.
As perdas pós-colheita variam entre os diversos produtos vegetais, porém, de modo geral, entre as frutas e hortaliças, têm-se perdas da ordem de 30 a 50%. Assim, este trabalho teve como objetivo a aplicação de 1-metilciclopropeno (1-MCP) e de resfriamento rápido com ar forçado (RR) em pêssegos, a fim de avaliar seus efeitos no processo de amadurecimento dessa fruta. Foram feitas análises fisiológicas: perda de massa fresca, firmeza, pH, acidez titulável, sólidos solúveis, razão SS/AT e produção de CO2, e análises sensoriais: cor, textura e sabor. O experimento foi dividido em duas etapas. Na primeira, testaram-se as concentrações de 30; 60 e 90 nL L-1 de 1-MCP aplicadas nas temperaturas de 0 ºC e 20 ºC. As frutas não-tratadas com 1-MCP foram denominadas de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fruta; Armazenamento; Qualidade.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100018

CALIBRATION OF THE THERMAL DISSIPATION PROBE FOR ATEMOYA: (Annona squamosa x A. cherimola)
Provedor de dados: 70
Autores: Santos,Irai M. S.; Vellame,Lucas M.; Araújo,Jairton F.; Marinho,Lígia B.
ABSTRACT When determining plant transpiration (TR) using the thermal dissipation probe method, it is necessary to calibrate the sap flow (SF) estimation equation for each species under study, and thus obtain reliable information about the water demand of crops. This study aims to calibrate the equation used to determine SF using the thermal dissipation probe for atemoya cultivation. The experiment was conducted in the experimental field of the Universidade do Estado da Bahia, Juazeiro, Northeast Brazil. Atemoya plants in the initial phase of development were transplanted into 21.5-l pots arranged on weighing platforms that acted as lysimeters. The SF was determined by the thermal dissipation probe method using 1-cm-long probes. The angular coefficient of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Annonaceous; Sap flow; Lysimeter; Granier method.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400545

Leaf concentrations of nitrogen and phosphorus in phaseolus vulgaris l. Plants under high CO2 concentration and drought stress
Provedor de dados: 70
Autores: Silva,João B. L. da; Ferreira,Paulo A.; Justino,Flávio; Pires,Luanna C.; Toledo,Amanda S.
This study aims to evaluate the leaf concentration of nitrogen and phosphorus correlated to the production of photoassimilates in beans plants (Phaseolus vulgaris L.) under high [CO2] and drought stress. The experiment was conducted in Viçosa (Brazil), during the period from April to July 2009, by using open-top chambers equipped with CO2 injection system. The drought stress was applied, through the irrigation suspension, during the period from flowering to maturation. The experimental design was randomized blocks in split-plot scheme with four replication, where the plots with plants grown in [CO2] of 700 mg L-1 and [CO2] environment of 380 mg L-1 and the subplots with plants with and without drought stress. The results were submitted to ANOVA and Tukey...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Beans; Mineral nutrition; Photosynthesis; Climatic changes.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500012

Utilização de biomassa na secagem de produtos agrícolas via gaseificação com combustão adjacente dos gases produzidos
Provedor de dados: 70
Autores: Silva,Jadir N.; Cardoso Sobrinho,José; Saiki,Emílio T.
Este estudo determinou a viabilidade do uso de um gaseificador/combustor que utiliza tocos de eucalipto, resíduos de serraria, cavacos de lenha e sabugo de milho como combustível na secagem de produtos agrícolas. Utilizou-se o gaseificador desenvolvido por SILVA (1988) com modificações na câmara de gaseificação; área da grelha reduzida de 0,21 para 0,06 m²; adição de um revestimento envolvendo a parte superior do gaseificador, e foi colocado um registro tipo borboleta na saída da câmara de combustão. O ar aquecido no combustor foi enviado para um secador que possuía câmaras metálicas que eram removíveis, içadas por um sistema de roldanas, facilitando a homogeneização da secagem. Como teste do sistema, secou-se café com umidade inicial de 54,5% bu até 11,1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Secagem; Café; Alternativas energéticas.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200020

Diagnóstico das áreas de preservação permanente na bacia hidrográfica do Rio Tijuco, Ituiutaba - MG, utilizando tecnologia SIG
Provedor de dados: 70
Autores: Valle Júnior,Renato F. do; Pissarra,Teresa C. T.; Passos,Andréa de O.; Ramos,Tiago G.; Abdala,Vera L.
O presente trabalho teve como objetivo elaborar o mapa de uso da terra e cobertura vegetal da bacia hidrográfica do Rio Tijuco, município de Ituiutaba - MG, com base nas imagens digitais obtidas do satélite CBERS 2, através de delimitação automática das áreas de preservação permanente, seguindo-se a identificação de ocorrência de conflito de uso, tendo como referência legal o Código Florestal Brasileiro (Lei nº. 4.771/1965) e a resolução nº 303/02, do Conselho Nacional do Meio Ambiente. Este artigo analisa, por meio de parâmetros quantitativos e uso do Sistema de Informação Geográfica, a manutenção de faixas de preservação permanente de larguras recomendadas pela legislação ao longo dos corpos d'água. Os resultados mostraram um déficit de áreas preservadas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reserva legal; Geoprocessamento; Uso da terra; Sensoriamento remoto.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300013

Formation of beetroot seedlings in different protected environments, substrates and containers in Aquidauana region, State of Mato Grosso do Sul, Brazil
Provedor de dados: 70
Autores: Oliveira,Letícia C. de; Costa,Edilson; Cortelassi,Julissandra A. da S.; Rodrigues,Edson T.
This study with beetroot seedlings, cultivar Top Tall Early Wonder, was carried out at the State University of Mato Grosso do Sul (UEMS/Aquidauana), from October to November 2008. Three environments of cultivation were used: greenhouse; nursery with monofilament screen of 50 % of shading; and nursery with aluminized thermal reflective screen of 50% of shading. In these environments, three polystyrene trays of 72, 128 and 200 cells, filled with four substrates, were tested: soil; Plantmax®; coconut fiber and vermiculite. There were no replication environments and then each one was considered an experiment alone. For each environment, it was adopted a completely randomized design in factorial scheme 3x4 (three trays x four substrates), with four...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Beta vulgaris; Protected cultivation; Propagation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300001

Comparação de classificadores de imagens digitais na determinação da cobertura do solo
Provedor de dados: 70
Autores: Cruz,Eleandro S.; Carvalho,Daniel F.; Varella,Carlos A. A.; Silva,Leonardo D. B.; Souza,Wanderley J.; Pinto,Francisco A. C.
Com o objetivo de comparar dois classificadores de imagens para a estimativa da cobertura vegetal do solo, foram avaliadas as coberturas proporcionadas pela semeadura de leguminosas e de gramíneas, sob diferentes espaçamentos, preparo do solo e condições de céu com e sem nuvens. O experimento foi conduzido em quatro parcelas experimentais de perda de solo, com 22 m x 3,5 m, instaladas em um Argissolo Vermelho-Amarelo. Os tratamentos consistiram: a) mucuna-cinza (Mucuna pruriens) em nível; b) crotalária (Crotalaria juncea) em sulcos dispostos em nível; c) milho (Zea mays L.) em sulcos dispostos em nível, e d) milho semeado no sentido do declive. Foram tomadas fotografias das parcelas dos 15 aos 85 dias após a semeadura para posterior análise, utilizando o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão do solo; Plantas de cobertura; Manejo do solo; Processamento de imagens.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200004

Substrate with Organosuper® for cucumber seedlings formation in protected environments and polystyrene trays
Provedor de dados: 70
Autores: Costa,Edilson; Vieira,Laura C. R.; Leal,Paulo A. M.; Jara,Murillo C. de S.; Silva,Priscilla N. de L.
Culture environments, trays and doses of organic compost were evaluated in the formation of cucumber seedlings (Cucumis sativus L.). Five environmental conditions were tested: (A1) a greenhouse with height of 2.5 m, covered with polyethylene film, (A2) nursery with height of 2.5 m, monofilament fabric, 50% shading, (A3) nursery with height of 2.5 m, heat-reflective screen, 50% shading, (A4) nursery with a height of 1.8 m, covered with coconut tree straw and (A5) greenhouse with height of 4.0 m, covered with polyethylene film, with zenith opening and thermo-reflective cloth under the plastic. Trays of 72 (R1) and 128 (R2) cells were filled with 93% soil and 7% organic compound (S1), 86% soil and 14% organic compound (S2) and 79% soil and 21% organic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environments of cultivation; Containers; Substrates; Cucumis sativus.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200003

Influence of data acquisition geometry on soybean spectral response simulated by the prosail model
Provedor de dados: 70
Autores: Breunig,Fábio M.; Galvão,Lênio S.; Formaggio,Antonio R.; Epiphanio,José C. N.
View angle and directional effects significantly affect reflectance and vegetation indices, especially when daily images collected by large field-of-view (FOV) sensors like the Moderate Resolution Imaging Spectroradiometer (MODIS) are used. In this study, the PROSAIL radiative transfer model was chosen to evaluate the impact of the geometry of data acquisition on soybean reflectance and two vegetation indices (Normalized Difference Vegetation Index - NDVI and Enhanced Vegetation Index -EVI) by varying biochemical and biophysical parameters of the crop. Input values for PROSAIL simulation were based on the literature and were adjusted by the comparison between simulated and real satellite soybean spectra acquired by the MODIS/Terra and hyperspectral...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Leaf area index; NDVI; EVI; Reflectance; MODIS; Remote sensing.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100018

Qualidade da classificação do tomate de mesa em unidades de beneficiamento
Provedor de dados: 70
Autores: Ferrari,Paulo R.; Ferreira,Marcos D.
A avaliação da qualidade da classificação foi realizada em duas unidades de beneficiamento de tomates de mesa, com equipamentos de classificação eletrônica e mecânica, e em dois períodos de produção, safras de verão e inverno. O objetivo deste trabalho foi avaliar a conformidade de classificação por diâmetro e coloração dos equipamentos com o proposto pelo Programa Brasileiro para a Modernização da Horticultura (PBMH), e verificar a classificação obtida por diâmetro com os equipamentos, na regulagem programada pela unidade de beneficiamento, sendo utilizados tomates da cultivar Carmen. Os resultados obtidos mostraram que não houve conformidade entre a classificação por diâmetro e a coloração feita com os equipamentos, com o proposto nas normas de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Unidade de beneficiamento; Classificação eletrônica; Classificação mecânica.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300029

SIMULATION OF SODIUM AND POTASSIUM DYNAMICS BY THE HYDRUS 2D MODEL IN A HAPLIC PLANOSOL VIA RESIDUE WATER
Provedor de dados: 70
Autores: Andrade,Carolyne W. L. de; Montenegro,Suzana M. G. L.; Miranda,Jarbas H. de; Montenegro,Abelardo A. de A.; Assis,Fred M. C. V. de.
ABSTRACT The application of chemical substances to the soil together with little attention given to the possible environmental impacts, transformed the environment into a recipient of waste. The aim of this study was to simulate the movement of water and solutes (sodium and potassium together) using the STANMOD and HYDRUS-2D models in a typical Haplic Planosol under the application of wastewater via surface irrigation under different flow rates. The experiment was conducted in the laboratory by miscible displacement tests, first using columns with deformed soil under saturation and steady water flow conditions, at a rate of 11.7 cm3 min-1, to obtain transport parameters of sodium and potassium ions, and in the applied residual water, the values of 475 and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modeling; Nutrients; Soil physical properties; Water reuse.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600874

Desempenho de processo anaeróbio em dois estágios (reator compartimentado seguido de reator UASB) para tratamento de águas residuárias de suinocultura
Provedor de dados: 70
Autores: Fernandes,Gracie F. R.; Oliveira,Roberto A. de.
Avaliou-se o efeito das águas residuárias de suinocultura com concentrações de sólidos suspensos totais em torno de 6.000 mg L-1 (DQOtotal variando de 7.557 a 11.640 mg L-1) no desempenho de processo anaeróbio em dois estágios compostos por reator compartimentado (ABR) e reator de fluxo ascendente com manta de lodo (UASB), instalados em série, em escala-piloto (volumes de 530 e 120 L, respectivamente), submetidos a tempos de detenção hidráulica (TDH) de 56 a 18 h no primeiro reator e de 13 a 4 h no segundo reator. As eficiências médias de remoção de DQOtotal variaram de 71,1 a 87,5% no reator ABR e de 41,5 a 50,1% no reator UASB, resultando em valores médios de 86,8 a 94,9% para o sistema de tratamento anaeróbio em dois estágios com carga orgânica...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digestão anaeróbia; Reator anaeróbio de chicanas; Resíduos de suínos.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100027

SENSOR SYSTEMS FOR MAPPING SOIL FERTILITY ATTRIBUTES: CHALLENGES, ADVANCES, AND PERSPECTIVES IN BRAZILIAN TROPICAL SOILS
Provedor de dados: 70
Autores: Molin,José Paulo; Tavares,Tiago Rodrigues.
ABSTRACT Soil fertility attributes have different scales and forms of spatial and temporal variations in agricultural fields. Adequate spatiotemporal characterization of these attributes is fundamental to the successful development of strategies for variable rate application of fertilizers, enabling the classic benefits of precision agriculture (PA). Studies on Brazilian soil have shown that at least 1 sample ha-1 is required for the reliable mapping of key fertility attributes. However, this sampling density is difficult owing to the operational challenges of sample collection and the cost of laboratory analyses. Given this limitation, soil sensors have emerged as a practical and complementary technique for obtaining information on soil attributes, at...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spatial variability; Spectroscopy; On-the-go sensing; Hybrid laboratory.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800126

DETERMINATION OF XARAÉS GRASS QUALITY SUBMITTED TO IRRIGATION WATER LEVELS AND NITROGEN AND POTASSIUM DOSES
Provedor de dados: 70
Autores: Oliveira,Ednaldo M. de; Oliveira Filho,Jair da C.; Oliveira,Rubens A. de; Oliveira,Reginaldo M. de; Cecon,Paulo R.
ABSTRACT In the correct pasture management, nutritional factors such as nitrogen and potassium fertilization play an important role in the forage production and quality. The aim was to evaluate the effects of the application of water levels, nitrogen and potassium doses in the Xaraés grass in the south of the State of Tocantins. For this, Xaraés grass was cultivated in the experimental field of the Federal University of Tocantins, municipality of Gurupi, TO. We used a mixture of fertilizer, combinations of N and K2O following the 1 N: 0.8 K2O ratio. To evaluate the effect of irrigation water levels and combinations of N and K2O doses in Xaraés grass, the plant height, the crude protein content and neutral detergent fiber were determined. The greatest...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigated pasture; Brachiaria brizantha; Forage production.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100064

Use of data mining and spectral profiles to differentiate condition after harvest of coffee plants
Provedor de dados: 70
Autores: Lamparelli,Rubens A. C.; Johann,Jerry A.; Santos,Éder R. dos; Esquerdo,Julio C. D. M.; Rocha,Jansle V.
This study aimed at identifying different conditions of coffee plants after harvesting period, using data mining and spectral behavior profiles from Hyperion/EO1 sensor. The Hyperion image, with spatial resolution of 30 m, was acquired in August 28th, 2008, at the end of the coffee harvest season in the studied area. For pre-processing imaging, atmospheric and signal/noise effect corrections were carried out using Flaash and MNF (Minimum Noise Fraction Transform) algorithms, respectively. Spectral behavior profiles (38) of different coffee varieties were generated from 150 Hyperion bands. The spectral behavior profiles were analyzed by Expectation-Maximization (EM) algorithm considering 2; 3; 4 and 5 clusters. T-test with 5% of significance was used to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Crop monitoring; Spectral behavior; Management; Orbital remote sensing.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100019

Efeito residual de quatro aplicações anuais de lodo de esgoto e vinhaça na qualidade tecnológica da cana-de-açúcar
Provedor de dados: 70
Autores: Có Júnior,Caramo; Marques,Marcos O.; Tasso Júnior,Luiz C.
O principal objetivo deste trabalho foi avaliar os efeitos residuais, por quatro anos seguidos, de diferentes tipos de resíduos, aplicados de formas e em doses distintas, sobre a qualidade tecnológica da cana-de-açúcar de quinto corte (cultivar SP 81-3250). Os tratamentos testados são combinações de dois tipos de resíduos (lodo de esgoto; vinhaça; lodo de esgoto + vinhaça) com dois modos de aplicação (ao lado da linha de cultivo e em área total) e com duas doses (100 e 200%), e um tratamento-testemunha. O delineamento experimental foi em blocos casualizados, com três repetições, totalizando 39 parcelas. As variáveis analisadas foram: percentagem de sólidos solúveis no caldo extraído (Brix % C.E.), percentagem aparente de sacarose no caldo extraído (Pol %...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resíduos; Uso agrícola; Saccharum spp.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100020

Prototype for soil mechanical resistance measurement with chisel plow automated control
Provedor de dados: 70
Autores: MACHADO,THIAGO M.; LANÇAS,KLÉBER P.
ABSTRACT In Brazil, there are several available models and systems to measure soil compaction; however, the data generated by such equipment have to be processed and interpreted, making the process expensive. Our study aimed to evaluate a prototype of instrumented rods to identify soil compacted layers and control chiseling depth, and compared it to a conventional system at a fixed depth of 0.35 m. In order to compare them, we assessed the following parameters: hourly fuel consumption, operational fuel consumption, drawbar power, average power, average speed, slipping, tractor effective field capacity and response time. Our results showed that mechanical chiseling at variable depths reduced in 26% the operational fuel consumption and increased in 14% the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Soil compaction; Chiseling.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400646

Detection of soybean planted areas through orbital images based on culture spectral dynamics
Provedor de dados: 70
Autores: Mercante,Erivelto; Lima,Luiz E. P. de; Justina,Diego D. D.; Uribe-Opazo,Miguel A.; Lamparelli,Rubens A. C.
The soybean is important to the economy of Brazil, so the estimation of the planted area and the production with higher antecedence and reliability becomes essential. Techniques related to Remote Sensing may help to obtain this information at lower cost and less subjectivity in relation to traditional surveys. The aim of this study is to estimate the planted area with soybean culture in the crop of 2008/2009 in cities in the west of the state of Paraná, in Brazil, based on the spectral dynamics of the culture and through the use of the specific system of analysis for images of Landsat 5/TM satellite. The obtained results were satisfactory, because the classification supervised by Maximum Verisimilitude - MaxVer along with the techniques of the specific...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Image analysis; Landsat 5/TM; Estimate of planted area.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500011

POTENTIAL OF REDUCTION IN THE EMISSION OF METHANE AND NITROUS OXIDE FROM SWINE WASTEWATER AFTER TREATED BY TWO DIFFERENT SYSTEMS
Provedor de dados: 70
Autores: Inoue,Keles R. A.; Souza,Cecília De F.; Matos,Antonio T.; Sousa,Marilú S.; Vieira,Maria De F. A.
ABSTRACT Swine wastewater have high pollution load, requiring treatment before its disposal into the environment. Methane (CH4) potentially emitted for such waste is considered 21 times more polluting than Carbon dioxide (CO2), and the nitrous oxide (N2O) is considered 310 times. In this way, projects of the Clean Development Mechanism (CDM) and energy use related to the CH4 are worldwide diffused. It was evaluated the potential greenhouse gas emissions in the influent and effluent from digesters and stabilization ponds used to treat the swine wastewaters in two commercial farms operating in full cycle, located in the municipality of Oratorios-MG, Brazil. Using the methodology “AM0006” to estimate the average potential of greenhouse gases, it was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Greenhouse gases; Air pollution; Swine; Waste management.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601198

Variáveis biométricas da cana-de-açúcar fertilizada com resíduos orgânico e industrial e irrigada com água servida e potável
Provedor de dados: 70
Autores: Nobile,Fabio O. de; Galbiatti,João A; Muraishi,Reginaldo I; Araujo,José R.
O uso agrícola de resíduos orgânicos e industriais é uma alternativa de aproveitamento como fertilizante e fonte de matéria orgânica ao solo. Neste sentido, o objetivo deste trabalho foi avaliar o uso do composto de lixo e biofertilizante como fonte de nutrientes, e o resíduo do processamento da bauxita como corretivo da acidez do solo, para a cultura da cana-de-açúcar (cana-planta), irrigada com água potável e servida. Para tanto foi conduzido experimento em vaso, utilizando-se de solo Argissolo Vermelho-Amarelo distrófico, cultivado com a variedade RB855536. Foram avaliadas variáveis biométricas da planta, tais como: altura de plantas, diâmetro do colmo, perfilhamento, número de folhas, matéria seca de raiz e parte aérea. Os dados obtidos evidenciaram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adubação orgânica; Matéria seca; Diâmetro de colmo; Altura de plantas; Raiz.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100019

Viabilidade econômica de tecnologias de manejo da irrigação na produção do feijão-caupi, na região dos cocais-MA
Provedor de dados: 70
Autores: Castro Júnior,Wady L.; Oliveira,Rubens A. de; Silveira,Suely de F. R.; Andrade Júnior,Aderson S. de.
O feijão-caupi é uma cultura de grande relevância socioeconômica nas regiões Norte e Nordeste do Brasil. No entanto, apresenta baixa produtividade. A irrigação é uma técnica que possibilita aumentos na produtividade e na rentabilidade dos cultivos, principalmente quando bem manejada. Para tanto, existem diversas tecnologias de manejo. Assim, objetivando avaliar economicamente diferentes tecnologias de manejo da irrigação na produção do feijão-caupi (Vigna unguiculata (L.) Walp.), em duas épocas de cultivo (primavera e outono), na região dos cocais, no Estado do Maranhão, conduziu-se um experimento no Campo Experimental do Instituto Federal do Maranhão, em Codó-MA, no delineamento em blocos casualizados, com sete tratamentos e quatro repetições. Deste modo,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vigna unguiculata; (L.) Walp.; Rentabilidade; Custo de produção.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300406

Desempenho de reatores anaeróbios de fluxo ascendente com manta de lodo em dois estágios tratando águas residuárias de suinocultura
Provedor de dados: 70
Autores: Santana,Adriana M. de; Oliveira,Roberto A. de.
Avaliou-se o desempenho de dois reatores anaeróbios de fluxo ascendente com manta de lodo (UASB) em escala-piloto com volumes de 908 L e 188 L, instalados em série, alimentados com águas residuárias de suinocultura com concentrações médias de sólidos suspensos totais (SST) variando de 2.216 mg L-1 a 7.131 mg L-1 e submetidos a tempos de detenção hidráulica (TDH) de 62,3 e 31,1 h, no primeiro reator, e de 12,9 e 6,5 h, no segundo reator. As eficiências médias de remoção de DQOtotal variaram de 74,0% a 89,6% no Reator 1 e de 34,3% a 45,1% no Reator 2, resultando em valores médios de 86,6% a 93,1% para o sistema de tratamento em dois estágios com carga orgânica volumétrica (COV) na faixa de 3,40 a 14,44 kg DQOtotal m-3 reator d-1 no Reator 1. As concentrações...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digestão anaeróbia; Reator UASB; Resíduo de suínos.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300029

Uso da geoestatística na avaliação de variáveis ambientais em galpão de suínos criados em sistema "wean to finish" na fase de terminação
Provedor de dados: 70
Autores: Medeiros,Brenda B. L.; Moura,Daniella J. de; Massari,Juliana M.; Curi,Thayla M. R. de C.; Maia,Ana Paula de A.
O "wean to finish" é um sistema de criação de suínos que ainda é novo no Brasil, e não existem muitos estudos a respeito do ambiente onde estes animais são criados. Assim, o objetivo deste trabalho foi avaliar o ambiente térmico e aéreo por meio da técnica da geoestatística em galpão de suínos criados no sistema "wean to finish", na fase de terminação, nos horários das 09h, 12h e 15h. A variabilidade dos atributos foi baseada na estatística descritiva dos dados de temperatura, umidade relativa, velocidade do ar, concentrações de amônia e dióxido de carbono, obtendo-se: média, mediana, coeficiente de variação, assimetria e curtose, com o teste de normalidade de Kolmogorov-Smirnov, através do programa estatístico Minitab 15. Para a determinação da existência...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência; Distribuição espacial; Mapas; Suínos.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500001

GRANULOMETRY AND ENERGY CONSUMPTION AS INDICATORS OF DISINTEGRATION EFFICIENCY IN A HAMMER MILL ADAPTED TO EXTRACTING ARROWROOT STARCH (Maranta arundinacea) IN COMPARISON TO STARCH EXTRACTION FROM CASSAVA
Provedor de dados: 70
Autores: Branco,Fabiano P.; Naka,Marco H.; Cereda,Marney P.
ABSTRACT The commercial sector of starch extraction has fully automated plants with a minimum scale of 200 ton.day–1, which extracts starch from maize and cassava in Brazil. Although these starches are commodities, the market demands starches with special properties obtained without chemical modifications. A higher-priced starch can compensate for small-scale extraction, as in the case of arrowroot starch, which would correspond to an alternative income for the producer. As a small-scale equipment was not available in Brazil, it was necessary to adapt a hammer mill for arrowroot starch extraction, which should have a performance similar to that obtained from cassava roots using industrial grinders. The degree of disintegration and energy consumption were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Appropriate Technology; Small producers; Mechanization; Agribusiness.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300341

Geoestatística para a avaliação do controle ambiental do sistema de ventilação em instalações comerciais para frangos de corte
Provedor de dados: 70
Autores: Curi,Thayla M. R. de C.; Vercellino,Rimena do A.; Massari,Juliana M.; Souza,Zigomar M.; Moura,Daniella J. de.
O sistema de ventilação e de resfriamento utilizado em instalações para frangos de corte desempenha um papel importante no controle ambiental, possibilitando que a ave expresse seu potencial máximo de produção. Nesse sentido, o objetivo deste trabalho foi avaliar, por meio da geoestatística, a influência do sistema de ventilação e das diferentes tipologias construtivas em relação ao ambiente térmico e aéreo em aviários de frangos de corte na fase final de criação. Os aviários avaliados com sistema de ventilação artificial de pressão negativa, por meio de exaustores, foram: Blue House com nebulizadores na entrada de ar e vedação de cortinas; Dark House com painel evaporativo (tijolo cerâmico) e vedação de cortinas e Solid Wall com painel evaporativo...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Avicultura; Conforto térmico; Qualidade do ar; Sistema de ventilação.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600004

Compostagem da fração sólida da água residuária de suinocultura
Provedor de dados: 70
Autores: Orrico Júnior,Marco A. P.; Orrico,Ana C. A.; Lucas Júnior,Jorge de.
Avaliar o desenvolvimento do processo de compostagem utilizando como substrato à fração sólida da água residuária de suinocultura foi o objetivo deste trabalho. Para a obtenção da fração sólida, a água residuária de suinocultura foi submetida ao peneiramento, utilizando-se de peneira com malha de 1 milímetro. Após separação, a fração sólida foi utilizada para a confecção de três leiras de compostagem, em pátio com piso de concreto e cobertura plástica. Durante a compostagem da fração sólida da água residuária de suinocultura, foram avaliados: temperatura, reduções de sólidos totais (ST), sólidos voláteis (SV), demanda química de oxigênio (DQO), carbono orgânico, matéria orgânica compostável (MOC), matéria orgânica resistente à compostagem (MORC), números...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coliformes; Temperatura; Redução de sólidos.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300015

Technical and economic indicators of the yellow passion fruit tree irrigated with underground water supply
Provedor de dados: 70
Autores: Araújo,Haroldo F. de; Costa,Raimundo N. T.; Crisóstomo,João R.; Saunders,Luís Carlos U.; Moreira,Olavo da C.
The research aimed to quantify technical and economic indicators of yellow passion fruit tree irrigated with fractions of irrigation with underground source of water, to generate information that helps farmers in decision making on the implementation of investment in irrigated fruit growing (yellow passion fruit). For this purpose, we used the passion fruit crop irrigated with Microjet type irrigation system, with conducting system in simple espaliers. The treatments consisted of five hours of application of the depth of water required by the crop with irrigation frequency of two days. The results showed that the highest yield (16660kg ha-1) was obtained with the fractionation of irrigation twice a day (50% to 7h and 50% to 21h30), which provided an...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Passiflora edulis; Productivity; Night irrigation; Profitability analysis.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500006

Uso de traçador salino para avaliação da colmatação e das condições hidrodinâmicas em sistemas alagados construídos de escoamento horizontal subsuperficial
Provedor de dados: 70
Autores: Matos,Mateus P.; Sperling,Marcos V.; Matos,Antonio T.; Passos,Ricardo G.
RESUMO A colmatação é um fenômeno intrínseco aos sistemas alagados construídos (SACs) utilizados no tratamento de esgotos, sendo decorrente dos mecanismos de remoção de poluentes. Dentre os métodos disponíveis para a avaliação da colmatação, destaca-se o uso de traçadores para a obtenção das condições hidrodinâmicas dos SACs. No entanto, não há um traçador ideal; os salinos, por exemplo, são passíveis de absorção, mecanismo influenciado pelo estádio no qual a planta se apresenta. Assim, objetivou-se, com a realização do trabalho, avaliar a utilização do NaCl para caracterização do grau de colmatação e das condições hidrodinâmicas de SACs de escoamento horizontal subsuperficial, plantado e não plantado, verificar a confiabilidade do uso desse traçador em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cloreto de sódio; Eficiência volumétrica; Esgotos; Obstrução; Plantas; Wetlands construídos.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601137

Estimativa do conforto de matrizes de frango de corte baseada em análise do comportamento de preferência térmica
Provedor de dados: 70
Autores: Pereira,Danilo F.; Nääs,Irenilza de A.
Considerando o comportamento social, é sugestivo que a freqüência e a intensidade de interações agressivas, o total de coesão social e compreensão da extensão de vícios sociais possam ser utilizados para avaliação de bem-estar. Este trabalho propõe que a freqüência de utilização de determinados locais dentro do galpão possa ser usada como variável para monitorar estados de bem-estar térmico e/ou estresse das aves alojadas. A partir de dados registrados no verão de 2000-2001, esta pesquisa identificou as temperaturas críticas máximas (tc máx) de matrizes pesadas, individualmente, por meio de análise estatística da freqüência de uso de locais previamente estabelecidos, utilizando a tecnologia de identificação eletrônica. Os valores das tc máx individuais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avicultura; Zona de termoneutralidade; Identificação eletrônica.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200004

KNOWLEDGE ON ADJUVANT PROPERTIES, DISPOSAL OF PESTICIDERESIDUES AND SPRAY DRIFT OCCURRENCE IN THE STATE OF MATO GROSSO
Provedor de dados: 70
Autores: CARVALHO,FERNANDO K.; ANTUNIASSI,ULISSES R.; MOTA,ALISSON A. B.; CHECHETTO,RODOLFO G.; CARVALHO,LÍDIA R. DE.
ABSTRACT This paper aimed at investigating the knowledge level of people working on pesticide spraying activities concerning spray adjuvant properties, as well as collecting information on disposal locations for residues from internal spray tank cleaning, and finally the understanding of pesticide spray drift occurrence in the state of Mato Grosso, Brazil. The information was gathered through a questionnaire answered by participants of a rural extension program in application technology located in nineteen grain and fiber producing regions of Mato Grosso state. Among the mentioned adjuvants, 49.0% belonged to the mineral oil class and 17.9% of participants did not know the functions performed by such products. In addition, 58.5% of the participants...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pesticides; Spraying; Environmental safety; Application technology.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200352

USING PASSIVE AND ACTIVE MULTISPECTRAL SENSORS ON THE CORRELATION WITH THE PHENOLOGICAL INDICES OF COTTON
Provedor de dados: 70
Autores: Souza,Heloisa B.; Baio,Fabio H. R.; Neves,Danilo C.
ABSTRACT: The investment in precision agriculture technologies has been growing as well the investment in vegetation index sensors with different types of data collection. This study aimed to evaluate the NDVI potential use obtained from passive and active multispectral sensors as phenological parameters indicator of cotton growth. The experiment was conducted in cultivated cotton fields during the harvest seasons of 2013/14 and 2014/15. The phenological variables analyzed in the field, were cotton plant height and number of branches per sampled cotton plant. The active sensors Crop Circle and Green Seeker were mounted on a manual support. The passive sensor Tetracam was installed on a support positioning the sensor at 4 m height from the ground. NDVI...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vegetation index; Variability; Multispectral sensors.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400782

TILLAGE INTERFERENCE IN THE QUALITY OF PEANUT MECHANIZED HARVEST
Provedor de dados: 70
Autores: Ormond,Antonio T. S.; Dos Santos,Adão F.; Alcantara,Aline S.; Zerbato,Cristiano; Furlani,Carlos E. A.
ABSTRACT In Brazil, a large portion of peanut production is found under conventional soil preparation. Due to the fact that there is a lack in studies related to the cultivation of peanuts in conservationists soil preparation, mainly in the field of losses and mechanized harvesting. Thus, it was aimed to assess the quality of digging and gathering operation of peanut, based on losses, using statistical process control techniques in two tillages. The sowing was carried out under conventional and conservationist preparation, revolving only the sowing line. Losses were evaluated in the digging and gathering operation, being that in the gathering it was evaluated the harvest losses in three displacement speeds (4, 6 and 8 km h-1) in two tillages. The quality...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digging; Statistical process control; Losses; Gathering.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200251

Influência local em um modelo espacial linear da produtividade da soja utilizando distribuição t-Student
Provedor de dados: 70
Autores: Prado,Naimara V. do; Uribe-Opazo,Miguel A.; Galea,Manuel; Assumpção,Rosangela A. B.
O uso das ferramentas da geoestatística, aliadas à agricultura de precisão permitem o acompanhamento das áreas agrícolas produtoras de soja, estabelecendo as relações de dependência espacial entre os pontos amostrados. A modelagem da estrutura de variabilidade espacial possibilita a construção de mapas temáticos dos atributos estudados, utilizando como método de interpolação a krigagem. Porém, a presença de valores atípicos entre os elementos amostrais pode influenciar na construção e interpretação desses mapas. A distribuição de probabilidades t-Student tem sido utilizada na tentativa de diminuir a influência dos valores atípicos durante a estimativa dos parâmetros de dependência espacial, por ter caudas mais pesadas que a distribuição normal. A detecção...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Máxima verossimilhança; Variabilidade espacial; Diagnósticos.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500012

SHIFTS AND HARVESTING SYSTEMS ON QUALITY OF IMPURITIES SAMPLES IN SUGARCANE
Provedor de dados: 70
Autores: Alcantara,Aline S.; Ormond,Antonio T. S.; Sousa Júnior,Paulo R. de; Silva,Rouverson P. da; Kazama,Elizabeth H.
ABSTRACT Semi-mechanical and mechanical harvesting methods may influence the content of impurities in harvested sugarcane. This study aimed to evaluate the quality of three mechanical methods of sugarcane harvesting: one semi-mechanical, and two mechanical ones - self-performed and outsourced, during three working shifts. As quality indicators, both mineral and vegetal impurities were accounted. About 50 random samples were collected in the studied area during 35 harvest days and in three working shifts, for each harvesting method. Mineral impurities showed similar behavior for both self-performed and outsourced mechanical harvesting, thus displaying a low variability. On the other hand, vegetal impurities showed to be unstable for all three shifts....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mechanical harvesting; Agricultural machinery; Statistical process control; Saccharum officinarum.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300510

CASTOR BEANS QUALITY SUBJECTED TO DIFFERENT STORAGE TEMPERATURES AND PERIODS
Provedor de dados: 70
Autores: Goneli,André L. D.; Corrêa,Paulo C.; Oliveira,Ana P. L. R.; Hartmann Filho,Cesar P.; Oba,Guilherme C.
ABSTRACT The control of the temperature of the storage air have the ability to improve a better preservation of some types of agricultural products. However, the most effective temperature for storage as well as the duration of storage varies between products. Therefore, special attention should be concentrated on the storage temperature and its effects on the integrity and longevity of the produce. The objective of the present study was to evaluate the effects of storage temperature and storage period on the quality of castor beans. Castor seeds with a water content of approximately 6.1% (w.b.) were stored for 180 days at temperatures of 15, 25 and 35 °C. The quality of the seeds was evaluated every 45 days throughout the study period by measuring dry...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Armazenability; Ricinus communis L.; Post-harvest.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300361

INFRARED THERMOGRAPHY FOR DETERMINING TRAY TEMPERATURE IN LETTUCE PRODUCTION
Provedor de dados: 70
Autores: Cavalcanti,Sávio D. L.; Pandorfi,Héliton; Guiselini,Cristiane; Menezes,Dimas; Neto,Luiz A. de A.
ABSTRACT This research was carried out in Recife, PE, Brazil, and aimed to assess the variation of the surface temperature of trays and substrate in the production of lettuce seedlings and its influence on the final product. Trays consisted of expanded polystyrene, conventional polyvinyl chloride, polyvinyl chloride painted white, and polyvinyl chloride painted gray. Two cultivars (Solaris and Vanda) were used to register crop biometric variables from seedling stage to the final product (46 days). Tray and substrate temperatures were recorded by means of an infrared thermal imager. The experimental design was a completely randomized design in a 4 × 2 factorial scheme with three replications. The conventional polyvinyl chloride tray presented the highest...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Protected cultivation; Lactuca sativa L.; Seedlings.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100041

Custo de energia elétrica em cultura do feijoeiro irrigado por pivô central, afetado pelo manejo da irrigação e sistemas de cultivo
Provedor de dados: 70
Autores: Turco,José E. P.; Rizzatti,Gilcileia dos S.; Pavani,Luiz C.
O objetivo deste trabalho foi analisar o consumo e o custo de energia elétrica em cultura do feijoeiro irrigado por pivô central, cultivar IAC-Carioca, submetida a dois manejos de irrigação: TENS - tensiometria; TCA - balanço hídrico-climatológico, baseado no tanque "Classe A"; e dois sistemas de cultivo em Latossolo Vermelho: PD - plantio direto; PC - plantio convencional, no ano de 2002. A pesquisa foi desenvolvida na Área Demonstrativa e Experimental de Irrigação - ADEI da FCAV/UNESP, Câmpus de Jaboticabal - SP. O consumo de energia elétrica do sistema de irrigação foi monitorado, e seu custo, analisado para dois grupos tarifários: A e B, sendo os preços do kWh dos sistemas tarifários de energia elétrica obtidos na CPFL (Companhia Paulista de Força e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas tarifários de energia elétrica; Tensiômetro; Tanque "Classe A"; Plantio direto e convencional.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200014

Fuzzy modeling in the prediction of climate indices and productive performance of quails kept in climate chamber
Provedor de dados: 70
Autores: MARQUES,JORDÂNIO I.; LOPES NETO,JOSÉ P.; LOPES,FERNANDA F. DE M.; FURTADO,DERMEVAL A.; ARAÚJO,TIAGO G. P.
ABSTRACT With the demand in the production at large-scale food, confinement of animals has become a necessity of the productive process because of the increase in production capacity and optimization of the spaces reserved for creations. In this context, the aim of this study was the development and validation of models using fuzzy logic for predicting climate indices and productive performance of European quails kept in a climatic chamber. The model developed was analyzed from two points of view; the first one took into account the prediction of climate indexes where the input variables were the temperature (°C) and relative humidity (%) of the air. In the second, related to the prediction of productive performance, the input variables were air...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coturniculture; Fuzzy logic; Productivity; Environmental quality.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400604

ERRATA
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400737

Reatores anaeróbios operados em batelada sequencial, seguidos de lagoas de polimento, para o tratamento de águas residuárias de suinocultura. Parte I: produção de metano e remoção de DQO e de sólidos suspensos
Provedor de dados: 70
Autores: Duda,Rose M.; Oliveira,Roberto A. de.
Neste trabalho, avaliou-se o desempenho de dois reatores anaeróbios operados em batelada sequencial (ASBR), instalados em série, em escala-piloto (R1 e R2 com volumes de 280 L e 140 L, respectivamente), no tratamento de águas residuárias de suinocultura com concentrações de sólidos suspensos totais (SST) em torno de 10.000 mg L-1. Para o pós-tratamento do efluente do sistema de tratamento com os reatores anaeróbios, utilizaram-se duas lagoas de polimento (L1 e L2 com volume de 1.000 L, cada) em série. As cargas orgânicas volumétricas (COV) aplicadas no primeiro ASBR variaram de 4,43 a 12,75 g DQOtotal (L d)-1. As eficiências médias de remoção da demanda química de oxigênio total (DQOtotal) e de SST variaram de 52 a 86% e de 54 a 87%, respectivamente, no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digestão anaeróbia; Carga orgânica volumétrica; Dois estágios; Pós-tratamento.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100013

Influência de diferentes materiais de cobertura no conforto térmico de instalações para frangos de corte no oeste paulista
Provedor de dados: 70
Autores: Fiorelli,Juliano; Fonseca,Ricardo da; Morceli,José A. B.; Dias,Antonio A.
Este trabalho apresenta um estudo da influência de diferentes materiais de cobertura no conforto térmico de instalações destinadas à criação de frangos de corte. A pesquisa foi desenvolvida no Câmpus Experimental da UNESP de Dracena - SP. Quatro protótipos em escala real foram construídos, com área de 28 m² cada, cobertos com telha reciclada à base de embalagens longa vida, telha cerâmica, telha cerâmica pintada de branco e telha de fibrocimento. Os dados foram coletados durante o período de inverno de 2007, totalizando 90 dias. Com esses dados, foram calculados os índices de conforto térmico Carga Térmica Radiante (CTR) e a variável ambiental (Ta). Uma análise estatística por inferência e descritiva foi realizada com os valores do índice de conforto...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência; Frango de corte; Instalações; Cobertura.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500020

COIL SPRING FOR TORQUE REDUCTION IN TRACTOR FOLDABLE ROPS
Provedor de dados: 70
Autores: Araujo,Guilherme de M.; Teixeira,Marcos A.; Voltarelli,Murilo A.; Orlando Junior,Wilson de A.; Tavares,Leticia C. M.
ABSTRACT Studies conducted by the international labor organization have shown that operations involving agricultural machinery are among the three activities with the highest risk of accidents to workers. Among the possible causes, rollover is the most common, accounting for 33% of fatal accidents. Despite this, there are standards that provide for the use of safety devices to ensure the physical integrity of the operator, among these equipment stand out rollover protection structures, which can be foldable or not. In this sense, the objective of this study was to perform an ergonomic study in order to analyze the torque required for lowering and lifting a foldable rollover protection structure attached to an agricultural tractor, developing...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tractor accidents; Tractor rollover; Torsion coil springs; Agricultural tractors.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500680

Conformidade de acessos e de saídas de postos de operação em tratores agrícolas segundo norma NBR/ISO 4252
Provedor de dados: 70
Autores: Mattar,Danielle M. P.; Dallmeyer,Arno U.; Schlosser,José F.; Dornelles,Marçal E.
Este trabalho teve como objetivo avaliar a conformidade dos acessos e de saídas dos postos de operação em tratores agrícolas, por meio de população amostral dos tratores fabricados no Brasil. Para a avaliação, diversos itens referentes aos acessos e às saídas dos postos de operação foram analisados qualitativa e quantitativamente com base nos padrões da Norma NBR/ISO 4252. Ao final do trabalho, foi observado que os tratores classificados na Classe III, quanto à potência nominal do motor, atendem ao maior número de requisitos da Norma em comparação a tratores da Classe II. Dentre os itens avaliados, a altura da plataforma até o teto dos postos de operação foi atendida por todos os modelos. As presenças de batentes de proteção sobre os degraus e de corrimão...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ergonomia; Máquinas agrícolas; Segurança operacional.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100008

Desenvolvimento e avaliação de uma servoválvula de baixo custo para a aplicação de insumos líquidos
Provedor de dados: 70
Autores: Johann,André L.; Russo,Edison; Cappelli,Nelson L.; Umezu,Claudio K.
O presente trabalho teve o objetivo de desenvolver uma servoválvula de baixo custo, que respondesse a um sinal eletrônico de controle, para a aplicação de insumos líquidos a taxas variáveis. Depois de realizada pesquisa na literatura das opções de válvulas existentes para a dosagem de líquidos a baixas pressões, partiu-se para o desenvolvimento de uma válvula proporcional com acionamento mecânico por intermédio de um servomotor controlado eletronicamente. Uma vez desenvolvida a servoválvula, o sistema foi submetido a um conjunto de testes, realizados em bancada desenvolvida especificamente para esse fim, onde se procurou avaliar seu comportamento em termos de repetitividade, histerese e linearidade. Como resultados, obtiveram-se três curvas de vazão em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Taxa de aplicação; Válvula proporcional.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100016

Performance of UASB reactors in two stages followed by post-treatment with activated sludge in wastewater batch of wet-processed coffee
Provedor de dados: 70
Autores: Bruno,Marcelo; Oliveira,Roberto A. de.
In this study it was evaluated the efficiency of the treatment of wet-processed coffee wastewater in upflow anaerobic sludge blanket (UASB) reactors in two stages, in bench scale, followed by post-treatment with activated sludge in batch. The first UASB reactor was submitted to an hydraulic retention time (HRT) of 6.2 d and organic loading rates (OLR) of 2.3 and 4.5g CODtotal (L d)-1, and the second UASB reactor to HRT of 3.1 d with OLR of 0.4 and 1.4g CODtotal (L d)-1. The average values of the affluent CODtotal increased from 13,891 to 27,926mg L-1 and the average efficiencies of removal of the CODtotal decreased from 95 to 91%, respectively, in the UASB reactors in two stages. The volumetric methane production increased from 0.274 to 0.323L CH4 (L...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anaerobic digestion; Methane; Nitrogen; Phosphorus; Phenols.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400020

HEAT-APPLICATOR MACHINE FOR WEED CONTROL
Provedor de dados: 70
Autores: Spagnolo,Roger T.; Custódio,Tiago V.; Morais,César S. de; Reis,Ângelo V. dos; Machado,Antônio L. T.
ABSTRACT Pesticide environmental risks and increased weed resistance have encouraged studies for alternatives to herbicides. Among these are weed thermal control methods by controlled heat application machines. Thus, this study aimed to test a prototype of heat-applicator machine as a function of changes in gas pressure, travel speed, and tire traffic effect on plants. Then, three experimental factors were tested: gas pressure (98, 196, and 245 kPa), travel speed (0.56, 0.78, and 1.17 m s−1), and tire traffic effect on plants (with and without traffic). The results showed that tire traffic effect on plants and subsequent heat application had no effect on control rate. Weed control rates reached levels considered satisfactory using a heat application speed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal control; Agricultural machinery; Organic production.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500595

Internal ambience of beehives Apis mellifera with different colors and roofing materials in the sub middle of the São Francisco Valley
Provedor de dados: 70
Autores: Souza,Maria de F. P; Turco,Silvia H. N.; Silva,Eva M. S; Costa,Daniel dos S; Freire,Murilo S.
ABSTRACT The current study aimed to evaluate the influence of three colors and two types of roofing materials under the internal temperature of bee colonies Apis mellifera. The experiment was conducted at the Agricultural Sciences Campus at the Federal University of Sao Francisco Valley located in Petrolina-PE, in November and December 2013, using 24 colonies housed in Langstroth hives. The experiment was a completely randomized factorial design (3x2) with three colors of box (blue, white, and traditional) and two types of cover (with and without the use of plaster) with six treatments and four replications. The internal temperature dates of the colonies were hourly recorded, during 24 hours, and surface temperatures were hourly recorded between 08h00 and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal comfort; Insects; Temperature.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400625

Simulação da uniformidade da irrigação de sistemas convencionais de aspersão operando sob diferentes condições de vento
Provedor de dados: 70
Autores: Faria,Lessandro C.; Colombo,Alberto; Oliveira,Henrique F. E.; Prado,Giuliani do.
A uniformidade de aplicação de água é um importante fator a ser considerado na avaliação dos sistemas de irrigação por aspersão. A uniformidade em sistemas convencionais de aspersão depende de fatores como: o tipo de aspersor e suas condições operacionais, a disposição e o espaçamento entre aspersores no campo, e a velocidade e a direção do vento durante o período de aplicação de água. Tendo em visa que as complexas relações entre esses fatores e a uniformidade podem ser caracterizadas de forma mais eficiente com o auxílio da modelagem matemática, neste estudo, foram avaliadas simulações, fornecidas pelo modelo semiempírico de RICHARDS &amp;amp; WEATHERHEAD (1993), da distribuição espacial da água aplicada pelo canhão PLONA-RL250, operando sob diferentes...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: PLONA-RL250 canhão hidráulico Richard &amp;amp; Weatherhead.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100003

ORGANOCLORATED AND ORGANOPHOSPHORUS PESTICIDES IN THE PELOTAS RIVER SEDIMENT
Provedor de dados: 70
Autores: Model,Kathleen J.; Sampaio,Silvio C.; Remor,Marcelo B.; Mercante,Erivelto; Boas,Márcio A. Vilas.
ABSTRACT Aquatic sediments are widely used for the evaluation of anthropogenic contamination due to their ability to adsorb particles and contaminants, making them historical environmental archives. Therefore, the objective was to evaluate the contamination of the Pelotas River sediments, at the border between the states of Santa Catarina and Rio Grande do Sul, by organochlorine and organophosphorus compounds, determining the ecological risk. The evaluation was carried out with quarterly sediment collections in 8 points, totalizing four campaigns within one year, with the aid of the Peterson dredger. Among organochlorines, p'p'DDT stands out regarding environmental persistence, representing 53.23% of the contaminated samples, with values varying up to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural pesticides; Disulfoton; P'p'-DDT.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100124

Avaliação de modelo matemático para estimar a radiação solar incidente sobre superfícies com diferentes exposições e declividades
Provedor de dados: 70
Autores: Turco,José E. P.; Rizzatti,Gilcileia S.
Este trabalho teve por objetivo avaliar modelo matemático para estimar a radiação solar global diária sobre superfícies com diferentes exposições e declividades, no período de março de 2002 a março de 2003. A pesquisa foi desenvolvida em uma estrutura denominada "Bacia Hidrográfica Experimental" do Departamento de Engenharia Rural da UNESP, Câmpus de Jaboticabal - SP. Nessa estrutura, foram utilizadas superfícies caracterizadas como H, 10N, 10S, 20N, 20S, 10E, 10W, 20E e 20W. O sensor utilizado para medir a radiação solar global incidente nas superfícies estudadas foi um piranômetro da marca Kipp &amp;amp; Zonnen, modelo CM3. Para calcular a radiação solar incidente nas superfícies estudadas, foi utilizado o modelo de Kondratyev. As análises dos resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelo; Radiação global; Superfícies inclinadas.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100028

PRICE AND QUALITY OF COFFEE (COFFEA ARABICA L.) DRIED USING AIR DEHUMIDIFIED BY CONVECTION
Provedor de dados: 70
Autores: Konopatzki,Evandro A.; Christ,Divair; Coelho,Silvia R. M.; Demito,Angélica; Werncke,Ivan; Camicia,Rafaela G. da M.
ABSTRACT Grain drying processes have been improved to reduce costs and losses of coffee beverage quality. The objectives of this study were to evaluate the quality of coffee dried using air partially dehumidified before entering drying units (DUs) in four coffee-producing farms, as well as the effects of such process on coffee commercial value. The method consisted of obtaining three samples (triplicates) of coffee dried in both DUs and concrete terraces (control) for mean multiple comparisons. The following variables were analyzed for sieve #13 and hand-picked beans: defect number, cupping test, and pricing. Evaluations were carried out by three professional graders. The results showed that coffee dried in the DUs presented fewer broken grains, higher...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Air dehumidifier; Artificial drying; Coffee dryers; Electric dryer.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500649

Mathematical modeling applied to the growth of tilapia in net cages in the sub middle of the São Francisco river
Provedor de dados: 70
Autores: Sousa Júnior,José de A. de; Garrido,Marlon da S.; Carvalho,Paulo G. S. de; Rocha,Luciano G. da; Campeche,Daniela F. B.
This study aimed to apply mathematical models to the growth of Nile tilapia (Oreochromis niloticus) reared in net cages in the lower São Francisco basin and choose the model(s) that best represents the conditions of rearing for the region. Nonlinear models of Brody, Bertalanffy, Logistic, Gompertz, and Richards were tested. The models were adjusted to the series of weight for age according to the methods of Gauss, Newton, Gradiente and Marquardt. It was used the procedure "NLIN" of the System SAS® (2003) to obtain estimates of the parameters from the available data. The best adjustment of the data were performed by the Bertalanffy, Gompertz and Logistic models which are equivalent to explain the growth of the animals up to 270 days of rearing. From the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Economy; Equations; Oreochromis niloticus.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500019

Mapeamento das áreas de cana-de-açúcar na região norte fluminense - RJ por uso de técnicas de sensoriamento remoto
Provedor de dados: 70
Autores: Mendonça,José C.; Freitas,Ramon M. de; Aguiar,Daniel A. de; Sousa,Elias F. de; Muniz,Rodrigo de A.; Esteves,Barbara dos S.
Este trabalho teve por objetivo avaliar a dinâmica da ocupação do uso do solo cultivado com a cultura da cana-de-açúcar nos seis principais municípios produtores da região Norte Fluminense - RJ, entre o período de 1984 a 2007. Foram utilizadas 18 imagens do sensor TM-Landsat, técnicas de interpretação visual e de Modelo Linear de Mistura Espectral (MLME), para gerar mapas temáticos das áreas ocupadas com a cultura. Com base nesses mapas, foi possível analisar a espacialização das áreas de cana e quantificá-las em cada município. Dos resultados obtidos, pode-se concluir que, entre os anos de 2004 a 2007, ocorreu um decremento total na área ocupada com a cultura, em 43.308,33 ha. A partir do ano de 2000 até 2007, houve um incremento de 24.422,72 ha,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelo linear de mistura espectral; Uso do solo; Landsat.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300016

Imagens de sensoriamento remoto no monitoramento da colheita da cana-de-açúcar
Provedor de dados: 70
Autores: Aguiar,Daniel A. de; Rudorff,Bernardo F. T.; Adami,Marcos; Shimabukuro,Yosio E.
A prática agrícola da queima da palha da cana-de-açúcar tem por finalidade facilitar a colheita manual. No Estado de São Paulo, essa prática está submetida a uma rigorosa legislação ambiental devido ao impacto negativo para o meio ambiente. Está previsto que a queima da cana deve ser gradativamente eliminada até 2017. O presente trabalho tem por objetivo avaliar a área de cana colhida com e sem queima em todo o Estado de São Paulo. Para tal, foram utilizadas as imagens disponíveis do sensor TM a bordo do satélite Landsat-5. As imagens foram adquiridas de abril a dezembro de 2006, que corresponde ao período de colheita da cana. Essas imagens foram analisadas por meio de técnicas de processamento digital e interpretação visual. A área de cana colhida sem...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Queima da cana; Modelo linear de mistura espectral; Cana crua.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300011

Aplicação de efluente tratado de suinocultura para diluição de dejeto suíno e remoção de nitrogênio por desnitrificação
Provedor de dados: 70
Autores: Nunes,Matheus A. G.; Kunz,Airton; Steinmetz,Ricardo L. R.; Paniz,José N. G.
Este trabalho avaliou o efeito da diluição do dejeto de suíno com o efluente tratado a 50% (v/v), com vistas a aumentar a desnitrificação via fornecimento de carbono ao processo. Considerando-se a diluição estudada, a concentração média de N-NO3- na mistura foi de 47,9 + 14,5 mg L-1, e a DQO da mistura, na faixa de 17.543 + 675 mg L-1, resultando numa relação DQO/N-NO3- de 366, extremamente favorável à ocorrência da atividade desnitrificante no tanque de homogeneização da mistura. A concentração de N-NO3- foi reduzida biologicamente a 0,5 mg L-1 (cerca de 1% da concentração inicial). O procedimento testado promoveu, ainda, uma melhora na etapa de separação sólido-líquido, empregando coagulantes naturais, onde foi observado um consumo de tanino inferior ao...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tratamento de efluentes; Dejeto de suíno; Remoção de nitrogênio.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200019

Demanda energética de uma semeadora-adubadora para soja sob diferentes velocidades de deslocamento e coberturas do solo
Provedor de dados: 70
Autores: Bortolotto,Virindiana C.; Pinheiro Neto,Raimundo; Bortolotto,Marciano C.
O objetivo deste trabalho foi avaliar a demanda energética requerida por uma semeadora-adubadora disponível comercialmente para plantio direto, submetida a quatro velocidades de deslocamento e três condições de cobertura do solo na implantação da cultura da soja. O experimento foi conduzido no Sítio Cazarotto, localizado no Distrito de Iguatemi, município de Maringá - PR, em Latossolo Vermelho distrófico. Utilizou-se de delineamento de blocos ao acaso, em arranjo de parcelas subdivididas, em que os tratamentos principais foram três condições de cobertura do solo (vegetação espontânea, aveia dessecada e aveia dessecada + rolada) e as secundárias, quatro velocidades de deslocamento (4,7; 5,4; 6,5 e 7,2 km h-1). As variáveis estudadas foram: força na barra de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Força de tração; Potência requerida; Consumo de combustível.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100014

Produtividade de híbridos de milho em função da velocidade de semeadura
Provedor de dados: 70
Autores: Mello,Adilson J. R.; Furlani,Carlos E. A.; Silva,Rouverson P.; Lopes,Afonso; Borsatto,Edinan A.
O presente trabalho foi conduzido na área experimental do Laboratório de Máquinas e Mecanização Agrícola da UNESP - Jaboticabal, em um Latossolo Vermelho eutroférrico, em preparo convencional. Avaliaram-se o desenvolvimento e os componentes de produção de dois híbridos de milho (DKB 390, simples e DKB 435, duplo) em função de três velocidades do conjunto trator-semeadora-adubadora (5,4; 6,8 e 9,8 km h-1), totalizando seis tratamentos, com quatro repetições, em delineamento em blocos ao acaso, em esquema fatorial 2 x 3. Os resultados evidenciaram que o aumento da velocidade do conjunto trator-semeadora-adubadora reduziu a produtividade de grãos para o híbrido simples e não interferiu na produtividade do híbrido duplo. Apenas na menor velocidade (5,4 km...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Componentes da produção; Distribuição longitudinal; Tipos de híbridos.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300017

A STUDY OF THE IMPACT OF LAND USE AND OCCUPATION ON BASIN WATER QUALITY THROUGH MULTIVARIATE STATISTICS
Provedor de dados: 70
Autores: Santos,Gilmar O.; Hernandez,Fernando B. T.; Ferraudo,Antonio S.; Vanzela,Luiz S.; Santos,Duílio J. O.
ABSTRACT Without effective actions to improve environmental management, water resources tend to become scarce. Thus, this study aimed to understand the processes influencing the physical, chemical, and biological properties of the water due to land uses and occupation in the Ipê stream basin, in Ilha Solteira - SP (Brazil), regarding the dependence of the analyzed variables. Monitoring of chemical, physical, and biological water quality was performed from 2006 to 2011, and the records of land use and occupation in 2011. A factorial multivariate analysis allowed us to understand that the processes in densely populated areas increased degradation of water by the input of organic loads, yet those of farming areas enhanced the degradation of the chemical and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Factor analysis; Irrigation; Land use and occupation; River basin.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300453

Calor específico e densidade da polpa de cajá (Spondias lutea L.) com diferentes concentrações de sólidos solúveis sob baixas temperaturas
Provedor de dados: 70
Autores: Mata,Mario E. R. M. Cavalcanti; Duarte,; Zanini,Helen L. H. T.
A polpa de cajá tem sido exportada da região Nordeste para todo o Brasil, e uma das maneiras de conservá-la é processando-a e armazenado-a na forma congelada. Durante o processamento, existem dois fatores que favorecem a qualidade do produto a ser armazenado: a rapidez com que o produto é congelado e a adição de açúcar como forma de dificultar a ação microbiológica. Na linha de processo, algumas propriedades termofísicas, como o calor específico e a densidade, se alteram com as temperaturas negativas e com o teor de sólidos solúveis totais; dessa forma, para o dimensionamento adequado de máquinas e equipamentos, torna-se necessário conhecer essas propriedades, principalmente quando se operam equipamentos criogênicos, onde as temperaturas podem chegar a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Propriedades termofísicas; Criogenia; Congelamento.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200023

Potential of utilization of rain water excess for irrigation of green roofs in Mato Grosso, Brasil
Provedor de dados: 70
Autores: Vieira,Nathan L.; Queiroz,Tadeu M. de; Fagundes,Minéia C.; Dallacort,Rivanildo.
The aim of this study was to identify the relation between the evapotranspirometer demand and the supply of water from local rainfall, evaluating the possibility of using water excess for irrigation of Green Roofs in the State of Mato Grosso, in Brazil. The study was done using a series of historical data provided by the National Institute of Meteorology (INMET - Instituto Nacional de Meteorologia) which has official climatological stations in 12 cities and regions of the State. The evapotranspiration values were obtained by the Penman-Monteith method and by the Climatic Water Balance (CWB) by the Thornthwaite and Mather method using Available Water Capacity (AWC) of 12mm. With the CWB the excess and deficit were calculated, which were used for the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water balance; Rainfall and sustainability.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400024

Qualidade da água de nascentes com diferentes usos do solo na bacia hidrográfica do córrego rico, São Paulo, Brasil
Provedor de dados: 70
Autores: Donadio,Nicole M. M.; Galbiatti,João A.; Paula,Rinaldo C. de.
Com o objetivo de verificar a influência de remanescentes de vegetação ciliar e da ação antrópica na qualidade da água, estudaram-se quatro nascentes, sendo duas com a presença de vegetação natural remanescente e duas com predominância de atividades agrícolas. Essas nascentes fazem parte da bacia hidrográfica do Córrego Rico, estando localizadas nos municípios de Taquaritinga e de Guariba - SP, em duas classes de solo: Argissolo e Latossolo, respectivamente. Definiram-se pontos de coleta da água nas nascentes e ao longo dos cursos d'água (entre 0 a 50 m da nascente), em dois períodos (chuvoso e seco). Foram analisadas as seguintes variáveis: cor, pH, temperatura, turbidez, alcalinidade, dureza total, dureza em magnésio, dureza em cálcio, fósforo,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Microbacia; Recursos hídricos; Uso do solo.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100013

Estruturas automáticas para controle de água nos canais em lavoura de arroz irrigado
Provedor de dados: 70
Autores: Amaral,Luís G. H. do; Righes,Afranio A.
O Rio Grande do Sul apresenta a maior área irrigada do Brasil, devido principalmente à lavoura de arroz irrigado por inundação. Um dos fatores que contribuem para reduzir a eficiência de irrigação nessas lavouras é o baixo grau de controle exercido pelas estruturas de distribuição de água. Os objetivos deste trabalho foram projetar e construir dois protótipos de estruturas hidráulicas para controle automático de vazão em canais de irrigação e comparar sua sensibilidade de controle de vazão com a sensibilidade de duas comportas fixas. Os protótipos construídos - uma comporta hidromecânica automática e um regulador automático de vazão - foram instalados à entrada de um canal secundário, juntamente com uma comporta-gaveta e uma comporta-vertedor, que são as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Comporta hidromecânica; Regulador automático de vazão; Hidrometria.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100030

Avaliação do desempenho de um aquecedor para aves adaptado para utilizar biogás como combustível
Provedor de dados: 70
Autores: Santos,Tânia M. B.; Lucas Júnior,Jorge de; Silva,Fábio M. da.
Desenvolveu-se ensaio para avaliar a adaptação (diâmetro do injetor) e o desempenho (consumo e eficiência de aquecimento) de um aquecedor tipo campânula, adaptado para queimar biogás. Foi testado um aquecedor comum que, queimando gás liquefeito de petróleo (GLP), opera à baixa pressão (28 cm.c.a.), com capacidade calorífica de 5.024 kJ h-1 e recomendado para 500 aves. O aquecedor foi avaliado com o combustível original (GLP), sem qualquer modificação no injetor de gás, e após adaptação para o funcionamento a biogás. Na adaptação, foi mantida a mesma grelha do queimador principal, aumentando-se a perfuração do injetor para permitir o funcionamento e a avaliação. Foram avaliados cinco injetores com perfurações de 1,0053; 1,5080; 1,5708; 1,7672 e 1,980 mm²....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aquecimento de ar; Aquecedores; Frangos de corte.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400008

ESTIMATION ON THE CONCENTRATION OF SUSPENDED SOLIDS FROM TURBIDITY IN THE WATER OF TWO SUB-BASINS IN THE DOCE RIVER BASIN
Provedor de dados: 70
Autores: Oliveira,Amanda R. M. de; Borges,Alisson C.; Matos,Antonio T.; Nascimento,Moysés.
ABSTRACT Knowing the relationship between the total suspended solids concentration (TSS), turbidity in the waters, and that turbidity analysis can be done faster and in less expensive way, this study aimed to obtain mathematical model to estimate the total suspended solids (TSS) concentration from the turbidity values for waters of Doce river basin. For this purpose, it was used the water quality database of the Minas Gerais Institute of Water Management (IGAM). The data were pre-treated using the adjusted boxplot technique followed by adjustment of curves for the different management units and rainfall regime period. It was verified the possibility of a single curve through the dummy variable technique, subsequently. With the results it was observed that...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adjusted boxplot; Water quality monitoring; Variables dummy.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500751

Influência de centrífuga no processamento do mel de abelha
Provedor de dados: 70
Autores: Costa,Cleber C. da; Pereira,Roberto G.; Prata Filho,Dario de A.
Neste trabalho, estudou-se a influência do tipo de centrífuga utilizado no processamento do mel de abelha sobre os parâmetros reológicos, físico-químicos e sensoriais. Para a análise sensorial, trabalhou-se com 58 provadores que constataram mudanças no sabor das amostras. Na análise reológica, foi utilizado um reômetro RS50 conectado a um banho termostático K20-DC5, ambos da HAAKE, com um sensor de geometria cone-placa. Ocorreram diferenças significativas nos valores da viscosidade entre as duas amostras obtidas por meio dos respectivos modelos de centrífugas. O valor da viscosidade do mel obtido da centrífuga radial foi, aproximadamente, o dobro do valor do mel processado na centrífuga facial. Nenhuma alteração foi observada nos níveis de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reologia; Análise físico-química; Análise sensorial.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300028

CONSUMPTION, EFFICIENCY AND WATER CONTENT OF ARUGULA UNDER DIFFERENT MANAGEMENT OF BRACKISH NUTRITIONAL SOLUTIONS
Provedor de dados: 70
Autores: Campos Júnior,José E.; Santos Júnior,José A.; Silva,Ênio F. de F. e; Martins,Juliana B.; Rolim,Mário M.
ABSTRACT The need to use strategies for using brackish water in agriculture, especially in semi-arid conditions, is evident. Based on this information, this study was developed with the aim of evaluating the consumption, efficiency and water content, as well as the dry mass of the arugula plants (cv. Broad Leaf) exposed to brackish nutrient solutions as a function of replacement strategies and circulation frequencies. The treatments consisted of six salinity levels of the nutrient solution (1.5, 3.0, 4.5, 6.0, 7.5 and 9.0 dS m-1) and two circulation frequencies (twice a day 8 a.m. and 4 p.m., and three times a day at 8 a.m., 12 p.m. and 5 p.m.). In Experiment I, the evapotranspiration line was replaced with the respective brackish water used in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eruca sativa; Cultivation without soil; Salinity.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600885

CROP DATA RETRIEVAL USING EARTH OBSERVATION DATA TO SUPPORT AGRICULTURAL WATER MANAGEMENT
Provedor de dados: 70
Autores: Rolim,João; Navarro,Ana; Vilar,Pedro; Saraiva,Cátia; Catalao,Joao.
ABSTRACT Accurate crop data are essential for reliable irrigation water requirements (IWR) calculations, which can be acquired during the crop growth season for a given region using earth observation (EO) satellite time series. In addition, a relationship between crop coefficients and the NDVI can be established to allow for crop evapotranspiration estimation. The main objective of the present work was to develop a methodology, and its implementation in an application software, to extract crop parameters from EO image time series for a set of parcels of different types of crops, to be used as input data for a soil water balance model to compute IWR. The methodology was tested at two distinct test sites, the Vila Franca de Xira (site I) and Vila Velha de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Remote sensing; Irrigation; Software; NDVI; Crop phenology; Crop coefficient.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300380

Logistic regression to estimate the welfare of broiler breeders in relation to environmental and behavioral variables
Provedor de dados: 70
Autores: Pereira,Danilo F; Oliveira,Sandra C. de; Penha,Nárima L. J.
The increasing demand of consumer markets for the welfare of birds in poultry house has motivated many scientific researches to monitor and classify the welfare according to the production environment. Given the complexity between the birds and the environment of the aviary, the correct interpretation of the conduct becomes an important way to estimate the welfare of these birds. This study obtained multiple logistic regression models with capacity of estimating the welfare of broiler breeders in relation to the environment of the aviaries and behaviors expressed by the birds. In the experiment, were observed several behaviors expressed by breeders housed in a climatic chamber under controlled temperatures and three different ammonia concentrations from...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry production; Animal welfare; Statistical model; Animal precision.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100004

Mechanical damage during harvest and loading affect orange postharvest quality
Provedor de dados: 70
Autores: MIRANDA,MARCELA; SPRICIGO,POLIANA C.; FERREIRA,MARCOS D.
Brazil is the world’s largest orange producer; however, part of this production is lost during postharvest. This loss can be minimized by controlling incidence of physical damage throughout the harvest and loading operations. Impacts can negatively modify quantitative and qualitative fruits aspects. The main goal of this study was to measure the impact magnitude in two types of harvest (manual and detachment) and during all steps from picking into bags until loading for transport to the processing industry and additionally evaluating, in laboratory, the physico-chemical quality of the fruit subjected to various impacts, similar to those found in the field. In order to evaluate the impact magnitude, an instrumented sphere was used (760 mm, Techmark, Inc,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrus sinensis instrumented sphere manual; Detachment; Soluble solids.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100154

Geostatistics and remote sensing methods in the classification of images of areas cultivated with citrus
Provedor de dados: 70
Autores: Silva,Alessandra F.; Barbosa,Ana Paula; Zimback,Célia R. L.; Landim,Paulo M. B.
This study compares the precision of three image classification methods, two of remote sensing and one of geostatistics applied to areas cultivated with citrus. The 5,296.52ha area of study is located in the city of Araraquara - central region of the state of São Paulo (SP), Brazil. The multispectral image from the CCD/CBERS-2B satellite was acquired in 2009 and processed through the Geographic Information System (GIS) SPRING. Three classification methods were used, one unsupervised (Cluster), and two supervised (Indicator Kriging/IK and Maximum Likelihood/Maxver), in addition to the screen classification taken as field checking.. Reliability of classifications was evaluated by Kappa index. In accordance with the Kappa index, the Indicator kriging method...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Indicator Kriging; Cluster; Maxver; CBERS-2B satellite; Spatial classification.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600017

Uso de água residuária de origem urbana no cultivo de gérberas: efeito nos componentes de produção
Provedor de dados: 70
Autores: Medeiros,Salomão de S.; Soares,Frederico A.L.; Gheyi,Hans R.; Fernandes,Pedro D.
Com este trabalho, teve-se o objetivo de determinar a viabilidade de quatro lâminas de águas residuárias de origem urbana (75; 100; 125 e 150% da evapotranspiração da cultura) na produção de gérbera (Gerbera jamesonni), tipo comercial Rambo, comparando-se os resultados com os obtidos por meio da adoção do manejo convencional (adubação orgânica, química e irrigação com água de abastecimento equivalente a 100% da evapotranspiração). O experimento foi realizado em casa de vegetação, na Universidade Federal de Campina Grande, de fevereiro a julho de 2006, abrangendo um ciclo completo de produção. O delineamento experimental foi em blocos casualizados, com três repetições, e as variáveis monitoradas foram: número de botões florais emitidos e intervalo de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Flores; Fertirrigação; Gerbera jamesonni.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300028

EFFECT OF DRYING KINETICS ON COLOR OF “DEDO DE MOÇA” CHILI PEPPERS (Capsicum baccatum)
Provedor de dados: 70
Autores: Andrade,Ednilton T. de; Figueira,Vitor G.; Teixeira,Luciana P.; Martinazzo,Ana Paula; Araujo,Kátia G. de L.
ABSTRACT This study aimed to assess the drying kinetics of red and yellow chili peppers, “dedo-de-moça” variety, at different temperatures (35, 45, 55, and 70 °C) and model this phenomenon mathematically. We also evaluated the effect of these drying air temperatures on pepper fruit color. Pepper fruits were dried in a forced-air circulation dryer. Ten mathematical models were fitted to the experimental data by nonlinear regression analysis. After drying, pepper samples were analyzed for the following colorimetric parameters: lightness (L*), chroma or saturation (c), and hue angle (h), in order to determine the influence of drying air temperature on fruit coloration. Our findings showed that the higher the air temperature, the faster the drying process....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dehydration; Hue angle; Quality; Midilli model.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500659

SEASONAL DYNAMICS OF AGRICULTURAL SOIL COVER IN RUNOFF GENERATION
Provedor de dados: 70
Autores: Aguiar,Wagner de; Sampaio,Silvio C.; Paisani,Julio C.; Remor,Marcelo B.; Reis,Ralpho R. dos.
ABSTRACT Seasonal changes in agricultural soil use due to agroclimatic conditions affect the water cycle in watersheds. This study aimed to understand the temporal variation of runoff inherent to the seasonal occupation dynamics of the agricultural soil in the basin that drains the upper valley of the Marrecas River, upstream of the urban perimeter of Francisco Beltrão, PR. The effects of runoff were verified through flow peaks simulated by the HEC-HMS model in twelve monthly soil use scenarios, under seven precipitation return periods. The results indicated a strong relationship between bare soil and flow peaks, temporally delimiting April and March as the largest runoff generators and January and August as the smallest ones. The ratio quantified by rates...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Flood; Flow peak; Hydrological simulation; Agricultural soil use.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500592

Initial development of two eucalyptus hybrid submitted to irrigation
Provedor de dados: 70
Autores: Oliveira,Gabriel Q. de; Lopes,Adriano S.; Jung,Leandro H.; Rego,Norton H.; Oliveira,Jean C. L. de.
The eucalyptus offers several advantages compared to other forestry species and, by using the irrigation can increase productivity and decrease production time. The objective of the present study was to evaluate two hybrid eucalyptus (Grancam and Urograndis), no irrigation, dripping and micro sprinkler irrigated at 90, 120, 150 and 180 days after transplanting (DAT). The experiment was conducted at the experimental irrigation area in the State University of Mato Grosso do Sul, in the municipality of Aquidauna - State of MS, Brazil. The experimental design was randomized blocks, split plot with four blocks and two replications within each block, and the plots were composed by irrigation treatments (dripping, micro sprinkler irrigate and dry) and the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eucalyptus spp.; Sprayer; Dripping irrigation; Evapotranspiration.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600003

Racionalização do uso de força motriz em fábrica de ração
Provedor de dados: 70
Autores: Teixeira,Carlos A.; Oliveira Filho,Delly; Lacerda Filho,Adílio F. de; Martins,José H.
A falta de investimento no setor energético, aliada à sazonalidade de recursos naturais necessários para a geração de energia hidroelétrica, faz da racionalização do uso de energia elétrica uma ferramenta de apoio imprescindível para o crescimento do País. A ração animal pode representar entre 70 e 80% do custo de produção da criação de animais. Sendo assim, é importante o estudo da racionalização do uso de energia em processos que utilizam intensivamente força motriz, tais como as fábricas de ração. Na fábrica de ração estudada, os motores elétricos são utilizados principalmente para moagem e mistura de granulados e transporte. Com o objetivo de racionalizar o uso da energia elétrica, foi realizado estudo de adequação de força motriz dos equipamentos da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gerenciamento do lado da demanda; Motor elétrico; Energia elétrica.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200006

PRODUCTIVITY OF IRRIGATED JAMBU UNDER SOIL-WATER STRESSES AND NITROGEN DOSES
Provedor de dados: 70
Autores: Aviz,William L. C. de; Lima Junior,Joaquim A. de; Silva,André L. P. da; Oliveira,Pedro D. de; Gama,Cândido M. P.
ABSTRACT Jambu (Acmella oleracea (L.) R.K.) is a short-cycle leafy vegetable from the Amazon region, which needs an adequate availability of water and nutrients, mainly nitrogen, to obtain a rapid mass increase. This research aimed to study the effect of different soil-water stresses and nitrogen doses on jambu cultivation in the state of Pará. The experiments were conducted at the Igarapé-Açu experimental farm of the Federal Rural University of Amazonia (UFRA). The Jamburana variety was used in a 10 × 10 cm spacing, using a randomized block design in a 4 × 4 factorial scheme with three replications. Each plot had a dimension of 0.4 × 0.5 m (0.2 m2), totaling 20 plants in 4 rows, but only the plants of the central rows were useful. Treatments consisted of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Acmella oleracea (L.) R.K.; Tensiometry; Dripping; Nitrogen fertilization.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100016

Environmental comfort in constructions for Sindi and Guzera calves in the agreste region of the State of Paraiba, Brazil
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Peixoto,Adriana P.; Nascimento,José W. B. do; Regis,Jonh E. F.
The objective of this study was to evaluate the quality of air, bioclimatic indexes of facilities and physiological indices of Guzera and Sindhi calves, reared in climatic conditions of Agreste. The study was conducted at the experimental station of Alagoinha, PB, Brazil, using 16 calves of Sindi and Guzerá races. The average concentration of oxygen (20.85%), ammonia (1.99 ppm), carbon monoxide (&lt;0.01 ppm), methane (0.13 ppm) and hydrogen sulfide (&lt;0.01) within facilities, were within the limits established by the Brazilian and international standards, for both animals and workers. The bioclimatic index of temperature and humidity and the temperature of the black globe and humidity index were within the thermal comfort zone for cattle in most of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environment; Cattle; Adaptability; Physiological responses.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100001

ISOSTERIC HEAT, ENTROPY, AND GIBBS FREE ENERGY OF PUMPKIN SEEDS (Cucurbita moschata)
Provedor de dados: 70
Autores: Teixeira,Luciana P.; Andrade,Ednilton T. de; Devilla,Ivano A.
ABSTRACT To maintain seed and soil quality of pumpkin, energy knowledge associated with processing and storage stages is strategic for the optimization of the thermodynamic processes needed for product stabilization. Thus, the objective of this study was to determine isosteric heat, differential entropy, and Gibbs free energy within a temperature range from 20 to 70° C, and relative air humidity levels between 10.75 and 85.11%. The study was based on empirical data for water activity determination. As a result, we verified that as moisture content decreased, the integral isosteric heat of the product increased from 2502.35 to 6231.17 kJ kg-1, differential entropy raised from 1.18 to 12.43 kJ kg-1 K-1, and Gibbs free energy ranged from -243.84 to -432.59 kJ...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Quality; Energy; Thermodynamic properties; Oil.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100097

THE PHOTOVOLTAIC ELECTRIFICATION IN ISOLATED COMMUNITIES OF CARDOSO ISLAND STATE PARK - SP
Provedor de dados: 70
Autores: Baschiera,Luciene M.; Fagnani,Maria A.
ABSTRACT This study concerns a research conducted in 2014, in isolated communities of Cambriú and Foles belonging to the Cardoso Island State Park-SP, in order to establish a link between electrification through isolated photovoltaic systems type SIGIFI 30 (30 kWh/month) with the existing demands, interactions and changes in traditional communities studied. The energy in this case is presented as a structure component to these demands regarding to the labor, agriculture, fishing, health, education, comfort of buildings and income generation. The objective was to conduct an analysis of the implementation of photovoltaic electrification process, and to establish a relationship with the surveyed communities. The results demonstrated that electrification...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solar energy; Energy demand; Implantation process.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400536

Qualidade física e fisiológica de semente de soja colhida com sistema de trilha axial sob diferentes velocidades de operação e rotações do cilindro trilhador
Provedor de dados: 70
Autores: Vieira,Bruno G. T. L.; Silva,Rouverson P. da; Vieira,Roberval D.
A colheita mecanizada é ferramenta fundamental no processo produtivo das grandes culturas; se não for realizada adequadamente, poderá resultar em danos mecânicos severos às sementes, acarretando, prejuízos significativos na colheita, particularmente devido à redução da qualidade. Visando a avaliar os danos causados na colheita mecanizada de soja, o presente trabalho teve como objetivo estudar o efeito do sistema de trilha axial sobre a percentagem de bandinhas, impurezas e sementes quebradas de soja cv. M-Soy 8001, em função da velocidade de trabalho e rotação do cilindro trilhador. O delineamento experimental utilizado foi o inteiramente casualizado, em parcelas subdivididas, avaliando-se duas rotações do cilindro trilhador (400 e 500 rpm) e três...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Perdas na colheita; Vigor; Qualidade.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200016

Gases e ruídos em edificações para suínos: aplicação das normas NR-15, CIGR e ACGIH
Provedor de dados: 70
Autores: Sampaio,Carlos A. de P.; Nääs,Irenilza de A.; Nader,Alexandre.
A produção de suínos representa importante setor da economia brasileira, e a possibilidade de crescimento na produção é iminente, principalmente se considerar o baixo consumo de carne suína comparado ao de outras carnes e com outros países. As transformações e exigências de mercado que vêm ocorrendo no cenário mundial mostram que, num futuro muito próximo, as barreiras serão baseadas no bem-estar dos animais, na proteção ao meio ambiente e na legislação trabalhista. Pouco conhecimento está disponível sobre as normas relacionadas ao trabalho com agentes ambientais nas atividades rurais, assim como as condições de qualidade do ar nas instalações brasileiras. Os objetivos deste trabalho foram aplicar as principais normas relacionadas a ruído e gases, e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Suíno; Ruído; Qualidade do ar.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100002

Impact of the substitution of reference annual streamflow by monthly streamflow on the potential use of water resources
Provedor de dados: 70
Autores: Pruski,Fernando F.; Bof,Luiz H. N.; Silva,Luciano M. C. da; Silva,José M. A. da; Rego,Fernando S.; Justino,Flavio B.
The consideration of the streamflow seasonality has a high potential to improve the water use. In order to give subsidies to the optimization of water use, it was evaluated the impact of the change of reference annual streamflow by the monthly streamflows in the potential water use throughout the hydrography of Paracatu sub-Basin. It was evaluated the impact on Q7,10 (lowest average streamflow during a 7-day period with an average recurrence of 10 years) and on Q95 (permanent flow present 95% of the time). The use of monthly streamflow to substitute the annual streamflow had a high potential of improvement of water resources use in the sub-Basin studied. The use of monthly Q 7,10 in substitution of annual Q 7,10 increases the potential water use that vary...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Seasonality of streamflow; Planning and management of water resources.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300013

EVOLUTION OF CERRADO VEGETAL COVER ON A RIVER ISLAND BASED ON ORBITAL IMAGING DATA
Provedor de dados: 70
Autores: Carvalho,Daniel C. De; Pessoa,Mayara M. De L.; Pereira,Marcos G.; Delgado,Rafael C.
ABSTRACT This study aimed to assess vegetal cover evolution on a river island within the Ecological Station of (EEP), by remote sensing. For this purpose, Normalized Difference Vegetation Indexes were generated for Landsat 1 (1973) and Landsat 5 (1984, 1990, 2000 and 2011) images. Five landscape units were identified in the field: bare soil, Rough savanna, Typical savanna, Forested savanna and Evergreen dry woods. Only Forested savanna and Evergreen dry woods showed poor spectral splitting, being thus considered as a forestry complex. Changes throughout time have occurred in all units, with decreasing in bare soil areas (-2.56 ha year−1), Rough savanna (-0.66 ha year−1) and Typical savanna (-0.94 ha year−1) and with an increase in the Forested savanna...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Remote sensing; Environmental monitoring; Vegetation index.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601186

Estudos sobre a mensuração da condutividade elétrica do solo
Provedor de dados: 70
Autores: Molin,José P; Rabello,Ladislau M.
A condutividade elétrica é a capacidade que um material possui em conduzir corrente elétrica, e uma das suas utilidades na agricultura provém do fato de que a massa do solo com sua variabilidade na composição físico-química apresenta diferentes níveis de condutividade elétrica (CE). O objetivo do presente trabalho foi estudar o comportamento da CE no solo e avançar no entendimento dos fatores que regem seus níveis de variação e desenvolver sistemas que permitam a mensuração contínua da CE do solo para a geração de mapas. Construiu-se um sistema com várias configurações de mensuração da CE e, nas avaliações em campo, os resultados foram parcialmente satisfatórios. Num estudo detalhado utilizando apenas um sistema comercial para sua mensuração, obteve-se a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Sensores; Indicador qualitativo de solo.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100009

Sowing performance by a metering mechanism of continuous flow in different slope conditions
Provedor de dados: 70
Autores: CORREIA,TIAGO P. DA S.; SOUSA,SAULO F. G. DE; SILVA,PAULO R. A.; DIAS,PATRÍCIA P.; GOMES,ANDERSON R. A.
ABSTRACT One of the reasons for the success of a productive culture is the correct sowing. Therefore, the seeds must be properly dosed, deposited and not damaged by the metering mechanism of the seed drill. So, the aim of this study was to evaluate in a simulator the sorghum seed deposition by a metering mechanism with continuous flow in different conditions of slope and sowing speed, and evaluate the quality of the deposited seeds assessing mechanical damage and germination. The experiment was carried out at the College of Agricultural Sciences, UNESP in Botucatu-SP, being used a simulator equipped with seed metering mechanism of helical channelled rotor type. The experimental design was randomized in a 3 x 2 factorial arrangement with six replications....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Deposition; Germination; Mechanical damage; Sowing.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500839

Compostaje de biosólidos de plantas de tratamiento de águas residuales
Provedor de dados: 70
Autores: Torres,Patricia; Pérez,Andrea; Escobar,Juan C.; Uribe,Iris E.; Imery,Ricardo.
Foi avaliada a compostagem dos biossólidos gerados na Estação de Tratamento de Esgotos - ETE, de Cañaveralejo, da cidade de Cali - Colômbia. Ainda que o processo se mostrasse viável, a incorporação de materiais de suporte e emenda foi favorável ao mesmo e à qualidade do produto final ao melhorar as condições de manejo, estrutura e porosidade do biossólido (B), além de melhorar as relações carbono/nitrogênio. Dos materiais avaliados, os que apresentaram melhor desempenho como materiais de suporte (MS) e Emenda (ME), foram os resíduos de poda e a cachaça, respectivamente; a relação ótima B:MS:ME, em percentagem, foi 72:10:18. Do ponto de vista da gestão dos resíduos e considerando o crescente incremento no número de ETEs municipais, este estudo mostrou que o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compostagem; Gestão de biossólidos; Materiais de emenda e suporte.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100021

Bem-estar na produção de frango de corte em diferentes sistemas de criação
Provedor de dados: 70
Autores: Nazareno,Aérica C; Pandorfi,Héliton; Guiselini,Cristiane; Vigoderis,Ricardo B; Pedrosa,Elvira M. R.
Esta pesquisa foi conduzida com o objetivo de avaliar diferentes sistemas de criação para frangos de corte, caracterizando o ambiente térmico, os parâmetros fisiológicos e o comportamento animal. O experimento foi realizado no decorrer de um ciclo produtivo de 42 dias, no município de Carpina, Estado de Pernambuco, na Estação Experimental de Pequenos Animais da Universidade Federal Rural de Pernambuco (UFRPE). A pesquisa foi desenvolvida em um módulo de produção dividido em 15 boxes, com 10 aves por Box, e densidade de 10 aves por m², totalizando 150 aves, submetidas a três sistemas de criação: semiconfinado com 3 m² por ave de área de piquete (SC 3), semiconfinado com 6 m² por ave de área de piquete (SC 6) e confinamento total (CONF). O delineamento...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avicultura; Conforto térmico; Comportamento; Instalações agrícolas.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100002

Código Florestal brasileiro: impactos econômicos e sociais no município de Bandeirantes – PR
Provedor de dados: 70
Autores: Reis,Luiz C.; Reis,Teresinha E. da S.; Saab,Otávio J. G. A.; Reis,Amanda S.; Batista,Bruno G.
RESUMO O trabalho teve como objetivo analisar os impactos econômicos e sociais provocados pela recomposição florestal do município de Bandeirantes – PR, considerando dois cenários: o Código Florestal vigente e a proposta de alteração. No município, 83,63% dos imóveis rurais enquadram-se na categoria de agricultura familiar, com predomínio de minifúndios e pequenas propriedades, nos quais, problemas sociais poderão surgir caso as alterações na legislação ambiental não apresentem alternativas justas e viáveis economicamente. Se aprovada a proposta, as áreas de mata ciliar ao longo dos córregos serão reduzidas de 4.270,74 ha para 2.122,18 ha; enquanto nas nascentes e nos rios principais, que não sofrerão alteração, serão de 434,17 ha e 1.152,32 ha,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mata ciliar; Reserva legal; SIG; Agricultura familiar.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400778

Characterization of water availability in a hydrographic basin
Provedor de dados: 70
Autores: Arai,Fabiane K.; Pereira,Silvio B.; Gonçalves,Geula G. G.
The quantitative knowledge of hydrological parameters (rainfall and flow) and their spatial and temporal variability on the regions or basins should be understood as essential to the efficient planning and management of water resources. Because the Ivinhema Basin, located in the state of Mato Grosso do Sul, Brazil, represents an important inductor on the region agricultural development, characterized as a major producer of grains and meat, it was used to characterize the hydrological study. Knowing the rainfall, flow and drainage area of each of the studied affluent, it was calculated the proportion of contribution of the affluent. To that end, it was proposed the concepts of potential and real contributions, aiming to identify the proportion of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: River discharge; Water resources; Rainfall.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300018

Spatial variability of soil physical properties in two management systems in sugarcane crop
Provedor de dados: 70
Autores: Carvalho,Laércio A. de; Meurer,Ismael; Silva Junior,Carlos A. da; Centurion,José F.
The aim of this study was to characterize the spatial variability of soil bulk density (Bd), soil moisture content (θ) and total porosity (Tp) in two management systems of sugarcane harvesting, with or without burning, in a Haplustox soil, in the 0-0.20 m layer. The study area is located in Rio Brilhante, state of Mato Grosso do Sul, Brazil, in Eldorado Sugar Mill. The plots have presented 180 m length, and 145.6 m width, totaling 90 points distributed in the form of a grid of nine rows by ten columns, with points spaced 20 m from its neighbor. Soil samples were collected at 0-0.20 m layer in 2007/2008 and 2008/2009 crops. The harvest with burning system had a higher density compared to mechanized harvest, in the two study periods. The moisture content as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mechanized harvesting; Bulk density; Saccharum spp.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100007

Receptores GPS de três precisões e estação total na caracterização de cotas básicas para projetos rurais
Provedor de dados: 70
Autores: Rodrigues,Vilmar A.; Cardoso,Lincoln G.; Gomes,Luciano N.; Barros,Zacarias X. de; Campos,Sérgio.
O objetivo deste estudo foi comparar cotas de vértices de uma poligonal, considerando dados coletados por três diferentes receptores GPS, usando como testemunha uma estação total. Os dados foram obtidos em uma poligonal fechada, sendo posteriormente tratados pelo software Topograph. As cotas obtidas pelos três receptores foram confrontadas com aquelas calculadas a partir do levantamento com a estação total, mediante a aplicação do teste "t", constatando-se que as mesmas foram satisfatórias para o equipamento GPS Trimble® 4600 LS. Para o equipamento GPS Trimble® modelo PRO XR, as cotas não foram totalmente satisfatórias, mas possíveis de serem consideradas em anteprojetos. Para o equipamento GPS Garmin® de navegação 12 XS, as cotas mostraram-se inaceitáveis...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cotas; Estação total; GPS.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100023

Avaliação de estrutura de bambu como elemento construtivo para casa de vegetação
Provedor de dados: 70
Autores: Mary,Wellington; Kenmochi,Claudio S.; Cometti,Nilton N.; Leal,Paulo M.
O uso da tecnologia do cultivo protegido no Brasil, para a produção de hortaliças e plantas ornamentais, passou por diversas fases de adaptação, visando a atender às necessidades de oferta e de qualidade dos produtos, com a preocupação de minimizar os custos de produção e os efeitos negativos do clima. A grande maioria dessas adaptações partiu da iniciativa dos próprios agricultores, utilizando-se de diferentes materiais e de outros artifícios para contornar problemas cotidianos. O experimento foi realizado na área da Faculdade de Engenharia Agrícola/UNICAMP, no período compreendido entre dezembro de 2002 e janeiro de 2003, com o objetivo de avaliar as deformações do sistema construtivo de estrutura de bambu para utilização em casa de vegetação, em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Material alternativo; Estufa; Cultivo protegido.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100003

BIOGAS PRODUCTION FROM DAIRY CATTLE MANURE, UNDER ORGANIC AND CONVENTIONAL PRODUCTION SYSTEMS
Provedor de dados: 70
Autores: Matos,Camila F.; Paes,Juliana L.; Pinheiro,Érika F. M.; Campos,David V. B. De.
ABSTRACT The purpose of this study was to evaluate the production of biogas, as well as the biogas production potential resulting from the anaerobic biodigestion of dairy cattle manure under organic (CMOS) and conventional (CMCS) production system. Also, the concentration of thermotolerant coliforms was evaluated after the biodigestion process. Therefore, bench biodigesters prototypes were supplied with CMOS and CMCS for 30 weeks. The experimental design was completely randomized with four repetitions for each treatment. Analysis of total solids (TS), volatile solids (VS), biogas production potential, most probable number (MPN) of thermotolerant coliforms were made. The cumulative biogas production was 6.18 L and 11.15 L, when using the CMOS and CMCS,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anaerobic biodigestion; Biodigester; Agricultural waste.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601081

Horizontal pressures in cylindrical metal silos and comparison with different international standards
Provedor de dados: 70
Autores: Nascimento,José W. B. do; Lopes Neto,José P.; Montross,Michael D.
The focus of this research was to evaluate the horizontal pressures on a cylindrical metal silo of corrugated walls and flat bottom with 1.82m diameter and 5.4m high, and to compare the values with those obtained theoretically by the ISO 11697, EP 433 and AS 3774 standards. The silo was symmetrically filled and constant speed with wheat cv. soft red for two different height/diameter ratios (H/D) and was unloaded through three orifices with a diameter of 71.6mm, one concentric and two eccentrics. Horizontal pressures were measured on the walls of the silo at three positions using hydraulic type pressure cells. The results showed that shortly after the start of the unloading, there was a mass flow above the quota of H/D = 1.2, whereas below this quota funnel...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Horizontal pressures in silos; Eccentric unloading; Mixed flow.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400002

GREEN ROOF: SIMULATION OF ENERGY BALANCE COMPONENTS IN RECIFE, PERNAMBUCO STATE, BRAZIL
Provedor de dados: 70
Autores: Omar,Aline; Vigoderis,Ricardo; Pandorfi,Héliton; Moura,Geber; Guiselini,Cristiane.
ABSTRACT Green roof is a technology that consists of the use of soil and vegetation installed in the roof of buildings, being a great solution to combat heat islands. Thus, this study aimed to compare micrometeorological changes and their effect on the energy balance of non-vegetated (slab) and vegetated building roofs by means of a simulation model calculated as a function of the reference evapotranspiration (ETo), determined by the Penman-Monteith method. This research was developed between February 1 and September 30, 2016, in the Charles Darwin Building's Parking Garage, Rio Ave Empreendimentos, Recife, PE, Brazil. For this, a weather station was installed on the external building slab. On the slab, sensible, latent, and soil heat fluxes corresponded...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Radiation balance; Urban climate; Energy fluxes.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300334

Drought resistance of sugar-cane crop for different levels of water availability in the soil
Provedor de dados: 70
Autores: Barbosa,Fernando da S.; Coelho,Rubens D.; Maschio,Rafael; Lima,Carlos J. G. de S.; Silva,Everaldo M. da.
Soil water availability is the main cause of reduced productivity, and the early development period most sensitive to water deficit. This study aimed to evaluate the drought resistance of the varieties of sugar-cane RB867515 and SP81-3250 during the early development using different levels of water deficit on four soil depths. The experiment was conducted at the Department of Biosystems at Escola Superior de Agricultura "Luiz de Queiroz" (ESALQ/USP) in a greenhouse in soil classified as Oxisol, sandy loam texture (Series "Sertãozinho"). Once exhausted the level of available water in the soil, the dry strength of the studied strains are relatively low. Water balance with values less than -13 mm cause a significant decrease in the final population of plants,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Plant population; Saccharum spp.; Drought tolerance.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200002

Designing and manufacturing of a soybean harvest residue picker
Provedor de dados: 70
Autores: Schöffel,Rubem; Boller,Walter; Walber,Márcio.
ABSTRACT Soy harvest matches seasons with shortage of dry matter supply for ruminant feeding in most Brazilian soy-growing areas. Agricultural machinery-producing companies must have market perception, observing new opportunities and developing equipment to meet costumers’ needs. This paper aims to design, build, and test a device to collect soybean crop residues from the combine cleaning mechanism, consisting mainly of vegetable straw (chaff), and the other plant parts (stems) remain being deposited onto the ground. For equipment designing, we made use of the architectural design methodology proposed in the reference model for the agricultural machinery development process. The equipment was designed and built following the proposed methodology, then...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ruminant feeding; Soy chaff; Agricultural machinery designing.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601053

Estimativa do custo de implantação da agricultura irrigada, utilizando o sistema de informação geográfica
Provedor de dados: 70
Autores: Carvalho,Daniel F. de; Silva,Wilson A. da; Ceddia,Marcos B.; Tanajura,Elmo L. X.; Villela,André L. O.
A proposta deste trabalho foi utilizar o Sistema de Informações Geográficas (SIG) com o objetivo de indicar áreas agroeconomicamente mais aptas para a implantação da cultura do coqueiro irrigado. Foram utilizadas informações referentes ao assentamento rural Antonio Farias, localizado no município de Campos dos Goytacazes, região Norte do Estado do Rio de Janeiro. O software IDRISI 32 gerou informações que técnicos, extensionistas e produtores rurais podem utilizar no planejamento da agricultura em áreas irrigadas. Foram utilizados mapas digitais de solo e planialtimetria, além de mapas temáticos com informações de drenagem, estradas e limite dos lotes. A partir de operações de sobreposição dos temas solo, clima e relevo, foram criados novos mapas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Planejamento da irrigação; Mapas de custo de implantação; SIG.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200013

Volume of polyethylene bags for development of papaya seedlings in protected environments
Provedor de dados: 70
Autores: Faria,Tatiane A. C.; Costa,Edilson; Oliveira,Letícia C. de; Santo,Tiago L. do Espírito; Silva,Arthur P. da.
The objective of this study was to test container of polyethylene bags and protected environments on the papaya seedlings production, from May to August of 2008, in Aquidauana state of Mato Grosso do Sul (MS), Brazil. Five bags of polyethylene were used: 7.5 cm x 11.5 cm, 205.9 cm³; 8.4 cm x 10.6 cm, 238.1cm³; 10.0 cm x 16.5 cm, 525.2 cm³; 12.0 cm x 12.0 cm, 550.0 cm³ and 15.0 cm x 21.5 cm, 1539.8 cm³. These containers were placed in three protected environments: greenhouse; screened nursery with Sombrite® and screened nursery with Aluminet®. Because there is no replication of growing environment, each one was considered an experiment. For each cultivation environment, it was adopted a completely randomized design with eight replications of two plants...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sunrise solo; Containers; Seedlings production.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100002

Software para o planejamento e a racionalização do uso de sistemas de terraceamento em nível
Provedor de dados: 70
Autores: Griebeler,Nori P.; Pruski,Fernando F.; Teixeira,Alessandro F.; Oliveira,Luiz F. C. de.
O desenvolvimento de técnicas que permitam o aumento da eficiência de práticas de conservação do solo é necessário frente aos grandes prejuízos causados pela erosão. Nesse sentido, elaborou-se um software que utiliza bases de dados geradas em um Sistema de Informações Geográficas e que permite o dimensionamento de sistemas de terraceamento em nível de maneira mais racional, considerando as variações espaciais existentes no terreno. Como dados de entrada ao software, devem ser fornecidas imagens de elevação e declividade e, ainda, características de tipo, uso e manejo do solo, a metodologia para o cálculo do espaçamento entre terraços e a recomendação para a escolha do tipo de terraço mais aconselhado. Como resultados, o software fornece uma imagem com o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Conservação do solo; SIG; Planejamento integrado.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300031

Potentials of biogas production from young bulls manure fed with different diets
Provedor de dados: 70
Autores: Costa,Mônica S. S. de M.; Costa,Luiz A. de M.; Lucas Junior,Jorge de; Pivetta,Laércio A.
Physical and chemical characteristics of manure are modified by different animal production systems. In cattle feeding system for young bulls there is an inversion of the proportion between forage and concentrate. In other words, the animals receive a smaller amount of forage compared to the traditional system. These changes in the manure characteristics involve changes in the treatment systems. The aim of this study was to determine the potential production of biogas of batch digesters fed with manure from young bulls that received two diets containing different proportions between forage and concentrate, with or without inoculums and submitted to three levels of temperature (25, 35 and 40(0)C). The evaluated parameters were total solids (TS) and volatile...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Batch digesters; Temperature levels; Inoculums.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600002

MODELING OF PHOSPHORUS LOSSES BY WATER EROSION
Provedor de dados: 70
Autores: Farias,Vera L. da S.; Martins Filho,Marcílio V.; Paula,Daniela T. de; Siqueira,Diego S.
ABSTRACT Phosphorus losses in runoff water and eroded sediment may increase the risk of eutrophication. Erosion prediction models can be used to assess and quantify nutrient losses and transport in different soil management scenarios. This study aimed to assess the performance of models to estimate the losses of available phosphorus in eroded sediments and assess their spatial variability pattern. The experiment was installed on a eutrophic Red Ultisol located in Tabapuã, northwestern São Paulo State, São Domingos Stream Watershed. Aiming at estimating and validating the models, measurements were made from 2007 to 2015 at 17 observation points (slopes), determining soil phosphorus content (Psoil), eroded sediments (Psed), and enrichment rate (ERsed). The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: WEPP model; Enrichment rate; Spatial variability.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100149

Variação temporal do comportamento hidrológico na bacia do Rio Dourados no período de 1973 a 2002
Provedor de dados: 70
Autores: Pereira,Silvio B.; Alves Sobrinho,Teodorico; Fedatto,Euclides; Peixoto,Paula P. P.; Bonacina,Raquel.
A bacia do Rio Dourados localiza-se na sub-bacia do Rio Ivinhema que, por sua vez, se insere na Bacia Hidrográfica do Rio Paraná. A região é de grande potencial para o desenvolvimento agrícola e, com o crescimento da agricultura irrigada, o conhecimento das características hidrológicas dessa bacia é de grande importância para que o aproveitamento de suas águas possa ser otimizado com menor impacto ambiental. Neste trabalho, procedeu-se à análise do comportamento hidrológico na Bacia do Rio Dourados, tomando-se, para tanto, dados observados na estação Porto Wilma, situada próxima à foz da bacia. Foram obtidas a precipitação média anual, a vazão média anual, a vazão máxima anual, a vazão mínima anual de sete dias de duração, a vazão associada à permanência...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Disponibilidade hídrica; Recursos hídricos; Irrigação.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300027

ERRATA
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400736

Estimativa da evapotranspiração a partir de variação de nível estático de aquífero
Provedor de dados: 70
Autores: Barreto,Carlos E. A. G.; Wendland,Edson; Marcuzzo,Francisco F. N.
A quantificação da evapotranspiração é uma tarefa essencial para o gerenciamento dos recursos hídricos em uma bacia hidrográfica, já que é variável importante no ciclo hidrológico. Entretanto, estimar a evapotranspiração real é uma tarefa difícil, e os pesquisadores usam, geralmente, mais de um método a fim de validar os resultados. Este trabalho apresenta um método para a determinação da evapotranspiração real com base na variação da precipitação, do escoamento de base e do nível de água subterrânea medidas na bacia hidrográfica. Usando o método proposto em uma bacia hidrográfica piloto, a evapotranspiração real foi estimada em 900 mm por ano. Esse resultado foi comparado com a evapotranspiração potencial, calculada pelos métodos empíricos e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gerenciamento de recursos hídricos; Balanço hídrico; Água subterrânea.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100006

Evapotranspiration and crop coefficients of melon plants measured by lysimeter and estimated according to FAO 56 methodology
Provedor de dados: 70
Autores: Melo,Talyana K. de; Medeiros,José F. de; E. Sobrinho,José; Figueiredo,Vladimir B.; Souza,Paulo S. de.
Aiming at contributing to an adequate management of water resources, this study aimed to analyze and compare evapotranspiration (ETc) and crop coefficients (Kc) of melon plants measured by a lysimeter and estimated according to the FAO 56 methodology, in the city of Mossoró, state of Rio Grande do Norte (RN), Brazil. In order to measure ETc, weighing lysimeters with an area of 2.25m² were used, with two repetitions. The Penman-Monteith equation parameterized by FAO was used to estimate the reference evapotranspiration, and crop coefficients were those recommended in FAO-56 Bulletin adjusted to local climatic conditions. The required climatic data and lysimeter measurements were collected by an automatic weather station installed at the site. The results...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cucumis melo L.; Irrigation management; Climatic data.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500005

Water application uniformity and fertigation in a dripping irrigation set
Provedor de dados: 70
Autores: Borssoi,Adilson L.; Vilas Boas,Marcio A.; Reisdörfer,Marcelo; Hernández,Ricardo H.; Follador,Franciele A. C.
The purpose of this study was to evaluate the uniformity of distribution coefficient (UDC) and coefficient of variation (CV) of a familiar set of irrigation, classifying it the ASAE standard. The irrigation and fertigation are determined by two methods the KELLER &amp;amp; KARMELI and DENÍCULI . The two experiments were subjected to varying pressures: 12, 14, 16 and 18 kPa, in a completely randomized design of twenty samples composed of flows with three replications. Urea, potassium chloride (KCl) and ammonium phosphate (MAP) were the elements used for fertigation. The system consisted of a 200 L tank, which supplied another container of 30 L, it was moved vertically to control the pressure. The data was statistically compared between treatments for each...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Emitter; Hydraulic performance; Low head; Drip irrigation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400011

Determinação do "status" nutricional de nitrogênio no feijoeiro utilizando imagens digitais coloridas
Provedor de dados: 70
Autores: Baesso,Murilo M.; Pinto,Francisco de A. de C.; Queiroz,Daniel M. de; Vieira,Luciano B. de; Alves,Enrique A.
Este trabalho teve como objetivo avaliar o uso de índices espectrais, retirados de imagens digitais, para discriminar diferentes doses de N no feijoeiro. O trabalho, conduzido em vasos de 8 dm³, teve cinco tratamentos (0; 50; 100; 150 e 200 kg de N ha-1), com dez repetições. As imagens foram adquiridas aos 30; 40 e 50 dias após a emergência. Foram desenvolvidas funções discriminantes quadráticas, tendo como vetores de entrada as médias dos "pixels" de diferentes combinações dos quatro índices espectrais testados. Três diferentes tamanhos de blocos de imagem foram testados 9 x 9; 20 x 20 e 40 x 40 "pixels". Os melhores resultados foram alcançados pelos blocos de 9 x 9 e 20 x 20 "pixels", apresentando classificação 94; 96 e 96% superior à classificação ao...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Processamento de imagens digitais; Classificador estatístico.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300022

MODELING YIELD, SOIL WATER BALANCE, AND ECONOMIC RETURN OF SOYBEAN UNDER DIFFERENT WATER DEFICIT LEVELS
Provedor de dados: 70
Autores: Petry,Mirta T.; Basso,Laudenir J.; Carlesso,Reimar; Armoa,Maria S.; Henkes,Jonas R.
ABSTRACT Evaluating the impacts of water stress on crop yield allows comparing irrigation management alternatives, aiming to ensure an economic return for the irrigated farms. Thus, the main objectives of this study were to model the soil water balance, deriving the crop coefficients, grain yield prediction, and economic return of soybean grown at different levels of water deficit and price quotations. The experiment was carried out under a rainout shelter, using four irrigation water managements. Irrigations were applied when the soil available water in the root zone reached 75%, 64%, 60%, and 50% of the total available water (TAW). Crop and soil parameters were monitored throughout the crop season. The SIMDualKc model was used to simulate the soil water...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycine max; Soil water balance; SIMDualKc model; Economic return.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400526

Indicadores de produção e qualidade da fibra do algodoeiro fertirrigado com água residuária sanitária
Provedor de dados: 70
Autores: Santos,Silvânio R. dos; Soares,Antônio A.; Kondo,Marcos K.; Matos,Antonio T.; Maia,Victor M.
RESUMO Problemas decorrentes da descarga de esgoto sanitário em rios são fatores preocupantes, por reduzir a qualidade da água, principalmente na região semiárida. Como alternativa viável, a utilização agrícola de águas residuárias pode minimizar problemas ambientais e fornecer nutrientes bem como parte da exigência hídrica de plantas cultivadas. Assim, objetivou-se verificar a influência da água residuária sanitária tanto na forma bruta (ARB) quanto na tratada, em nível terciário (ART), em substituição à adubação potássica mineral em cobertura, sobre os indicadores de produção e qualidade tecnológica da fibra do algodoeiro NuOpal BG RR®. O experimento foi conduzido em Janaúba - MG, no delineamento em blocos casualizados, constituído por 5 tratamentos (T0:...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Algodão em pluma; Produtividade; Tecnologia da fibra; Esgoto bruto; Esgoto de tratamento terciário.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300525

Variabilidade espacial e temporal da precipitação pluvial na bacia hidrográfica do Ribeirão João Leite-GO
Provedor de dados: 70
Autores: Santos,Eduardo H. M. dos; Griebeler,Nori P; Oliveira,Luiz F. C. de.
A precipitação pluvial constitui-se na principal variável hidrológica de entrada do ciclo hidrológico e para conhecimento da variabilidade espacial e temporal como informação básica para estudos hidrológicos, manejo de bacias hidrográficas, gestão de recursos hídricos, dentre outros. Os recursos hídricos superficiais produzidos nessa bacia são essenciais ao desenvolvimento do eixo Goiânia-Anápolis-Brasília e, recentemente, com o aumento da demanda hídrica, tem sido relatados conflitos pelo uso da água. Dessa maneira, tem-se que o desenvolvimento de estudos hidrológicos visando ao melhor entendimento e aproveitamento dos recursos hídricos é estratégico para o desenvolvimento da região. Nesse sentido, objetivou-se com este estudo mapear a precipitação média...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Meio ambiente; Hidrologia.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100008

CHANGES IN SOIL CHEMICAL PROPERTIES PROMOTED BY FERTIGATION WITH TREATED SANITARY WASTEWATER
Provedor de dados: 70
Autores: Santos,Silvânio R.; Ribeiro,Danilo P.; Matos,Antonio T.; Kondo,Marcos K.; Araújo,Edcássio D.
ABSTRACT We evaluate the application of treated sanitary wastewater (TSW) to provide potassium for crops and reduce demand for fresh water and mineral nutrients. The field experiment was arranged in randomized block design with four replications and five treatments: 50, 100, 150 and 200% of potassium requirements and a control with conventional fertilizer. The TSW was applied to maize (November 2012 to February 2013), cotton (June to November 2013) and bean (April to June 2014). After bean, soil chemical properties were evaluated until 0.8 m depth. Fertigation with TSW to potassium fertilization provided about 50% of water, nitrogen and phosphorus to the bean. The soil nutrient availability and soil organic matter did not increase, whereas sodium had...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Effluent; Fertilization; Irrigation; Sewage; Sodium.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200343

Compostagem de resíduos da indústria de desfibrilação de algodão
Provedor de dados: 70
Autores: Costa,Mônica S. S. de M.; Costa,Luiz A. de M.; Sestak,Marcelo; Olibone,Dácio; Sestak,Diego; Kaufmann,Anderson V.; Rotta,Sandra R.
O processo de compostagem foi avaliado por meio do monitoramento diário da temperatura em leiras confeccionadas com o resíduo da indústria de desfibrilação de algodão e tipos de inóculo. Foram avaliadas seis leiras, divididas em dois sistemas: com aeração e sem aeração, sendo estudados, em cada sistema, três tipos de inóculo: esterco bovino diluído em água; esterco bovino, e conteúdo ruminal. Avaliou-se, também, a porcentagem de redução de volume nas leiras quando se intensificaram os revolvimentos, visando a obter informações para fins de dimensionamento do pátio de compostagem. Os compostos produzidos foram transferidos para minhocário e amostras do produto após a compostagem e após a vermicompostagem foram analisadas quimicamente com o objetivo de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aeração; Inóculo; Vermicompostagem.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200028

Soil CO2 emission as related to incorporation of sugarcane crop residues and aggregate breaking after rotary tiller
Provedor de dados: 70
Autores: Teixeira,Luis G; Fukuda,Adrian; Panosso,Alan R; Lopes,Afonso; Scala Jr,Newton La.
Soil tillage is a process that accelerates soil organic matter decomposition transferring carbon to atmosphere, mainly in the CO2 form. In this study, the effect of rotary tillage on soil CO2 emission was investigated, including the presence of crop residues on the surface.Emissions were evaluated during 15 days after tillage in 3 plots: 1) non-tilled and without crop residues on soil surface (NTwo), 2) rotary tiller without the presence of crop residues on soil surface (RTwo), and 3) rotary tiller with the presence of crop residues in soil surface (RTw). Emissions from the RTw plot were higher than the other plots, (0.777 g CO2 m-2 h-1), with the lowest emissions recorded in the NTwo plot (0.414 g CO2 m-2 h-1). Total emission indicates that the difference...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil respiration; Soil tillage; Carbon dioxide; Temporal variability of soil CO2 emission.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600005

Análise do resfriamento da solução nutritiva para cultivo hidropônico do morangueiro
Provedor de dados: 70
Autores: Villela Júnior,Luiz V. E.; Araújo,Jairo A. C. de; Factor,Thiago L.
Este trabalho teve como objetivo a produção hidropônica de morangos com resfriamento da solução nutritiva, em Jaboticabal - SP. O experimento foi conduzido no Setor de Plasticultura do Departamento de Engenharia Rural da FCAV/UNESP, Câmpus de Jaboticabal, em casa de vegetação coberta com filme de polietileno, sendo o transplantio realizado em 9-1-2002. Foram avaliadas duas variedades de morango: Campinas e "Sweet Charlie", cultivadas em sistema hidropônico tipo NFT, com ou sem resfriamento da solução nutritiva. A solução nutritiva resfriada foi mantida à temperatura de aproximadamente 12 ºC, por meio de um trocador de calor. A variedade "Sweet Charlie" apresentou melhores resultados para peso médio dos pseudofrutos, diâmetro médio longitudinal, diâmetro...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fragaria x ananassa Duch.; NFT; Hidroponia.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200012

Desempenho de um trator operando em solo com diferentes tipos de cobertura vegetal
Provedor de dados: 70
Autores: Gabriel Filho,Antonio; Silva,Suedêmio de L.; Modolo,Alcir J.; Silveira,João C. M. da.
A eficiência de um trator para desenvolver esforço tratório depende da interação entre o rodado e o solo, envolvendo um complexo conjunto de fatores: característica do rodado, patinagem, transferência de peso do trator, tipo de solo, umidade, estado de compactação, tipo de cobertura do solo, entre outros, que proporcionam diferentes condições de trabalho e interferem no desempenho do trator. Assim, conduziu-se o presente trabalho com o propósito de avaliar alguns desses fatores no desempenho de um trator agrícola, em área coberta com diferentes tipos de cobertura vegetal (aveia, ervilhaca, nabo, aveia e nabo e sem cobertura). O trator foi submetido a cargas por meio do acoplamento a um escarificador de arrasto e instrumentado para a obtenção da força de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eficiência tratória; Potência; Patinagem.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300032

THE SUCCESS OF THE BRAZILIAN ALCOHOL PROGRAM (PROÁLCOOL) - A DECADE-BY-DECADE BRIEF HISTORY OF ETHANOL IN BRAZIL
Provedor de dados: 70
Autores: Stolf,Rubismar; Oliveira,Ana Paula Rodrigues de.
ABSTRACT The National Alcohol Program (Proálcool) was a strategic policy of the Brazilian government to replace petroleum-based fuels with alcohol (ethanol). Based on the review, we can choose the 1960s as a start point for a leap in development. Over the 500 years of sugarcane history in Brazil, the crop enters the second decade of the 21st century with extraordinary strength and prestige, reaching its highest production in history. This made Brazil a leader in sugar and ethanol productions worldwide, with an energy-independent agribusiness. Moreover, effluents and polluting wastes were transformed into high-value inputs (e.g., vinasse, filter cake, and others). Environmentally friendly actions included developing organic cane production technology,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Strategies; Development; Agribusiness; World leadership.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200243

Análise do investimento em climatização para bovinos de leite em sistema de alojamento free-stall
Provedor de dados: 70
Autores: Souza,Silvia R. L.; Nääs,Irenilza A.; Karasawa,Simone; Romanini,Carlos E. B.
A dificuldade de adaptação das raças leiteiras européias no Brasil afeta diretamente o setor produtivo de leite. As condições climáticas do País são desfavoráveis, e o desenvolvimento de novas tecnologias é imprescindível para que o potencial genético e a capacidade de conversão alimentar sejam evidenciados nos animais. Dessa forma, a análise econômica do investimento na climatização de instalações do tipo free-stall torna-se necessária para estimar os aspectos relacionados à rentabilidade, capacidade de pagamento e tempo necessário para recuperar o capital investido. O objetivo deste trabalho foi o de avaliar a influência da climatização no processo produtivo de bovinos de leite e realizar uma análise econômica do investimento. Foram utilizadas 470 vacas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bovinos de leite; Análise econômica; Climatização.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200003

Deposição de calda na aplicação aérea e terrestre de fitossanitário na cultura da batata
Provedor de dados: 70
Autores: Bueno,Mariana R.; Cunha,João Paulo A. R. da; Alves,Guilherme S.
O objetivo deste trabalho foi avaliar a deposição de calda pulverizada na cultura da batata e o espectro de gotas promovidos pela aplicação aérea e terrestre. O experimento foi repetido em duas épocas, em lavouras comerciais de batata, no delineamento inteiramente casualizado, em esquema fatorial 6 x 2, sendo seis formas de aplicação (aérea, a 15 e 30 L ha-1 com atomizador rotativo, e terrestre, a 200 e 400 L ha-1, com pontas de jato plano duplo, com indução de ar e jato cônico vazio); e duas composições de calda (água e água mais o adjuvante fosfatidilcoline + ácido propiônico). Avaliaram-se deposição de calda no dossel da cultura, perdas para o solo e deriva, pela técnica da adição de traçador para quantificação por espectrofotometria, e espectro de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aviação agrícola; Deriva; Ponta de pulverização; Espectro de gotas.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600014

Otimização da eficiência de limpeza em equipamento de beneficiamento de tomate de mesa
Provedor de dados: 70
Autores: Silva,Michele C.; Franco,André T. O.; Ferreira,Marcos D.; Magalhães,Ana M. de; Testezlaf,Roberto.
A etapa de limpeza no sistema de beneficiamento do tomate de mesa é essencial para a aceitação do produto pelo consumidor, pois o grau de limpeza dos frutos está diretamente relacionado com a qualidade do produto. Entretanto, a etapa de lavagem, nos atuais equipamentos de limpeza, utilizada em unidades comerciais de beneficiamento, demanda volume excessivo de água, trazendo sérias preocupações ambientais. Este trabalho teve como objetivo comparar a eficiência de limpeza em dois sistemas, avaliando diferentes configurações operacionais relacionadas com a rotação de escovas, vazão do sistema e tempo de permanência do fruto sobre o jato. Comparou-se o sistema convencional utilizado em equipamentos comerciais com o sistema composto por um bocal de spray do...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Lycopersicum esculentum; Sistemas de limpeza; Consumo de água.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400015

METHANE PRODUCTION FROM CASSAVA STARCH WASTEWATER IN PACKED-BED REACTOR AND CONTINUOUS FLOW
Provedor de dados: 70
Autores: Araujo,Izabela R. C.; Gomes,Simone D.; Tonello,Tamiris U.; Lucas,Shaiane Dal'Maso; Mari,Angelo G.; Vargas,Rodrigo J. de.
ABSTRACT The aim of this study was to evaluate the behavior of an anaerobic reactor of packed-bed and continuous flow, in relation to the biogas and methane production and the removal of organic load, from the wastewater of cassava starch extraction. For this purpose, were tested, in a reactor with a useful volume of 2.82 L and support mean of polypropylene filled with polyethylene foam, the organic loading rate (OLR) of 2.5, 5.0, 8.0 and 10.0 g L-1d-1. It was evaluated the removal of COD, the pH, the VA/TA ratio, the biogas and the methane production. It was concluded from this study that it is possible to produce biogas with methane percentages higher than 80% (maximum) and remove the organic load more than 90% under the tested conditions. In relation to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Methanogenic reactor; Anaerobic biodigestion; Biogas.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200270

INFLUENCE OF SUBSTRATE AND SPECIES ARRANGEMENT OF CULTIVATED GRASSES ON THE EFFICIENCY OF HORIZONTAL SUBSURFACE FLOW CONSTRUCTED WETLANDS
Provedor de dados: 70
Autores: Saraiva,Claudety B.; Matos,Antonio T.; Matos,Mateus P.; Miranda,Suymara T.
ABSTRACT We aimed to evaluate the efficiency of six different horizontal subsurface flow constructed wetlands (HSSF-CWs), with different substrates (gravel and crushed PET bottles), which also varied in relation to the presence and arrangement of plant species (elephant grass and Tifton 85 bermudagrass) in the removal of pollutants from a bulk milk cooling tank (MTWW). Each bed was fed at a flow rate of 0.18 m3 d-1 and average organic load rate (OLR) of 318 kg ha-1 d-1 of BOD5, with hydraulic detention time (HRT) of 1.84 days in the gravel-filled HSSF-CWs (CWS-G) and 2.97 days in the PET-filled HSSF-CWs (CWs-P). The CWs-P were as efficient as the CWs-G in the removal of BOD5, COD, Total-P, and K-Total, being in some cases even more effective (turbidity,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wastewater; Elephant grass; Tifton 85 bermudagrass; Plants; Porosity.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300417

Aplicação do modelo CERES-maize na análise de estratégias de irrigação para milho "safrinha" em Londrina-PR
Provedor de dados: 70
Autores: Cardoso,Célio O.; Faria,Rogério T. de; Folegatti,Marcos V.
Usando-se a capacidade do modelo CERES-maize de simular o crescimento do milho sob várias condições de ambiente e manejo, foram analisadas estratégias de irrigação para o milho "safrinha", em diferentes épocas de semeadura, em Londrina - PR. Os tratamentos simulados constituíram-se no cultivo da cultivar de milho XL-520, em 12 épocas de semeaduras, no período de janeiro a abril, adotando-se cinco critérios para aplicação de irrigação, além de um nível sem irrigação e outro de produção potencial. Para as simulações, foram utilizados os dados meteorológicos da série histórica disponível para o local, características do solo predominante da região e manejo, seguindo as recomendações técnicas regionais para o cultivo. Os resultados revelaram que a irrigação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulação; Modelo matemático; Viabilidade.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100005

Reúso de águas residuárias da piscicultura e da suinocultura na irrigação da cultura da alface
Provedor de dados: 70
Autores: Baumgartner,Dirceu; Sampaio,Silvio C.; Silva,Tatiana R. da; Teo,Carla R. P. A.; Vilas Boas,Márcio A.
Este trabalho teve o objetivo de avaliar o desenvolvimento, a produção e a qualidade sanitária da cultura da alface irrigada com águas residuárias originadas da suinocultura e da piscicultura. Os tratamentos avaliados foram: T1 - alface irrigada com água de origem subterrânea e adubação suplementar; T2 - alface irrigada com água residuária de viveiro de peixes alimentados com ração; T3 - alface irrigada com água residuária originária de lagoa de estabilização de dejetos de suínos, e T4 - água de lagoa de cultivo de algas, alimentada com resíduo de biodigestor de dejeto de suíno. Os tratamentos não apresentaram diferenças significativas para altura da alface, diâmetro da cabeça, comprimento da raiz, massa da raiz, massa total da planta, massa fresca e massa...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Efluente; Irrigação; Lactuca sativa L.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100009

Computational Fluid Dynamics (CFD) simulating heated air from wood burning inside a poultries barn
Provedor de dados: 70
Autores: Coradi,Paulo C.; Martins,Márcio A.; da Costa,Douglas R.; Vigoderis,Ricardo B.; Tinôco,Ilda de F. F.
ABSTRACT Animal welfare is essential for livestock yield gains, which has been ethically justifiable and socially acceptable. Thus, our research aimed to test computational fluid dynamics model (CFD) to simulate heated air within a poultry barn. Data were simulated in CFD software based on Navier-Stokes equations (geometry of 3 m x 6 m, considering a symmetric mesh). As boundary conditions, a temperature of 38ºC was considered for walls where heating pipe outlets are, to the west side, besides a heat flow of zero, in symmetry to the same side. As for the sides east, south and north, walls were taken as isolated, i.e. heat flow equals to zero. The aviary heating system did not achieve a homogeneous temperature distribution, heat flow, heated air pressure...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environment; Animals; Thermal comfort; Airflow.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500768

AN INDEX TO EVALUATE THE ACCEPTANCE OF SPECIALTY COFFEES IN CONSUMER GROUPS
Provedor de dados: 70
Autores: Resende,Mariana; Cirillo,Marcelo Â.; Borém,Flávio M.
ABSTRACT Numerous factors are related to the individual sensory perception of consumers, which makes it impossible to adapt a model that explains their behavior. In this context and given the scarcity of statistical indexes that evaluate preferences for specialty coffees, new statistical methods should be studied. To this end, our study aimed to create an index that measures the acceptance of specialty coffees. The index was built considering the fit of regression models as a function of principal component scores. Validation was done by significance tests, whose probabilities were obtained by bootstrapping, considering the main measures used in diagnosing outliers as weights, with application to real data from different consumer groups. The coffee...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Models; Quality; Bootstrap; Acaia; Bourbon.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500624

PHYSICAL ANALYSIS OF REGIONALIZED FLOW AS AN AID IN THE IDENTIFICATION OF HYDROLOGICALLY HOMOGENEOUS REGIONS
Provedor de dados: 70
Autores: Calegario,Arthur T.; Pruski,Fernando F.; Ribeiro,Rayssa B.; Ramos,Maria C. A.; Rego,Fernando S.
ABSTRACT Regionalization is an important technique for estimating the flow of hydrographic sections with a lack of data. First, it is necessary to identify hydrologically homogeneous regions (HHRs), which are commonly validated via statistical analyses. Because this step is understood to be subjective, studies that contribute to a greater reliability in identifying regions are needed. In this context, the objective was to evaluate the inclusion of a physical analysis of the average regionalized flow rates as an aid to identify HHRs. The groupings were defined on the basis of geographical convenience methods and cluster analysis. For the assessment of regionalized flows, six statistical indices were used with a physical analysis that was performed via a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Regionalization; Long-term average streamflow; Planning and management of water resources; Cluster analysis; Geographical convenience.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300334

Análise dos ciclos de tensões em colhedoras de forragens
Provedor de dados: 70
Autores: Borges,Pedro H. M.; Niiyama,Orlando K.; Braga Júnior,Roberto A.; Volpato,Carlos E. S.; Ravelo,Giovanni F.; Santos,Luciano M. dos.
O estudo das tensões em colhedoras de forragens é imprescindível, uma vez que as condições de operação são muito variáveis e severas. Utilizou-se um sistema "datalogger" devidamente calibrado para medir as tensões, em função do tempo, numa colhedora de forragem. Foram desenvolvidos modelos matemáticos para obter a variação periódica dessas tensões, considerando-se a influência da roda de apoio e da velocidade angular do rotor de corte. O ajuste dos modelos foi verificado pelo coeficiente de determinação (R²). A variação periódica das tensões, em função do tempo, para os valores experimentais e teóricos, foi representada graficamente, utilizando-se da planilha eletrônica EXCEL. Observou-se que as menores amplitudes de tensões e os maiores períodos do ciclo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Colhedora de forragem; Tensões; Modelos matemáticos.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300022

METROLOGICAL BEHAVIOUR OF BULK WATER METERS UNDER DIVERSE INSTALLATION CONFIGURATIONS
Provedor de dados: 70
Autores: Palau,Carmen V.; Peralta,Iban B.; Manzano,Juan; Azevedo,Benito M. de; Bomfim,Guilherme V. do.
ABSTRACT As the correct measurement is an essential part of water management, this study describes the metrological behaviour of a range of bulk water meters under different installation configurations. The meters analysed included the horizontal and vertical Woltman, singlejet, tangential and proportional. Configurations included straight pipe lengths; gate and butterfly valves at different degrees of closure, rotations and distances from the meter; meter with volumetric and reducing valves; reverse installation; and meter rotated 90° from the horizontal setting. The metrological behaviour under different flow conditions was analysed by comparison with electromagnetic and volumetric meters (ISO-4064). The horizontal Woltman showed no permissible errors...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydrometry; Water consumption; Pressurised irrigation.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600893

Effect of adjuvants on the amount of air included in droplets generated by spray nozzles
Provedor de dados: 70
Autores: Mota,Alisson A. B.; Antuniassi,Ulisses R.; Chechetto,Rodolfo G.; Oliveira,Rone B. de; Silva,Anne C. A. e.
The air included in droplets generated by spray nozzles directly int0erferes in transport, deposition and retention of the droplets after its impact on the target. The objective of this study was to analyze the interference of adjuvants in the amount of air included in droplets generated by spray nozzles. The treatments were composed by four spray solutions containing mineral oil, vegetable oil, surfactant and water, and three spray nozzles, two air induction type and one pre-orifice. The air included was calculated by the difference between the volume of spray mix (air plus liquid) and only the liquid, which was made by means of sprayed samples captured in a funnel and collected in a graduated cylinder. The surface tension was estimated by the gravimetric...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Air induction; Pre-orifice; Surface tension.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600020

Efeito de níveis de água, coberturas do solo e condições ambientais na temperatura do solo e no cultivo de morangueiro em ambiente protegido e a céu aberto
Provedor de dados: 70
Autores: Pires,Regina C. de M.; Folegatti,Marcos V.; Pedro Júnior,Mário J.; Sakai,Emílio; Passos,Francisco A.; Arruda,Flávio B.; Calheiros,Rinaldo de O.
A temperatura do solo é um importante parâmetro no cultivo do morangueiro, pois interfere no desenvolvimento vegetativo, na sanidade e na produção. O objetivo do presente trabalho foi avaliar o efeito de diferentes níveis de água, coberturas de canteiro em campo aberto e em ambiente protegido, na temperatura máxima do solo no cultivo do morangueiro. Foram realizados dois experimentos: um em cultivo protegido e outro a campo aberto, em Atibaia - SP, em esquema fatorial 2 x 3 (coberturas do solo e níveis de irrigação), em blocos ao acaso, com cinco repetições. As coberturas de solo utilizadas foram filmes de polietileno preto e transparente. A irrigação localizada foi aplicada por gotejo sempre que o potencial de água no solo atingisse -0,010 (N1), -0,035...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Cobertura de solo; Morango.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300018

Tensões aplicadas no solo pelas diferentes pressões do pneu de um trator agrícola
Provedor de dados: 70
Autores: Mion,Renildo L.; Holanda,Áurea S. de; Barroso,Suelly H. de A; Silva,Samuel de A. T. E.
RESUMO A distribuição das tensões provocadas por rodados das máquinas agrícolas é dependente da carga da roda e da pressão interna do pneu, bem como das condições do solo. O objetivo do presente trabalho consistiu em avaliar numericamente a distribuição dos deslocamentos e das tensões atuantes em um solo coletado no Estado do Ceará, provocada pela passagem de um trator agrícola. O peso individual do pneu traseiro (dimensões 18.4-34 R1) em que foi medida a área de contato do pneu com o solo era de 17,1 kN. Nas análises numéricas, baseadas no método dos Elementos Finitos, foram considerados diferentes valores da pressão interna do pneu (96,5 kPa, 124,0 kPa, 151,0 kPa e 179,0 kPa) com suas respectivas áreas de contato (0,2256 m2, 0,1660 m2, 0,1522 m2 e 0,1393...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Método dos elementos finitos; Módulo resiliente; Compactação; Pneus.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100063

Effect of the application of different water depths and nitrogen and potassium doses on quality of Tanzania grass
Provedor de dados: 70
Autores: Oliveira Filho,Jair da C.; Oliveira,Rubens A. de; Oliveira,Ednaldo M. de; Cecon,Paulo R.; Martins,Carlos E.
The objective of this study was to evaluate the effects of the application of different water depths and nitrogen and potassium doses in the quality of Tanzania grass, in the southern of the state of Tocantins. The experiment was conducted on strips of traditional sprinklers, and used, as treatments, a mixture of fertilizer combinations of N and K2O always in the ratio of 1 N:0.8 K2O. This study determined throughout the experiment: plant height (PH), the crude protein (CP) and neutral detergent fiber (NDF). The highest plant height obtained was 132.4 cm, with a fertilizer dose of 691.71 kg ha-1 in the proportion of N:0.8 K2O, in other words, 384.28 kg ha-1 of N and 307.43 kg ha-1 of K2O, and water depth of 80% of the ETc. The highest crude protein content...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrogen fertilizer; Irrigated pasture; Panicum maximum.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400007

Modelling head loss along emitting pipes using dimensional analysis
Provedor de dados: 70
Autores: Perboni,Acácio; Frizzone,Jose A.; Camargo,Antonio P. de; Pinto,Marinaldo F.
Local head losses must be considered in estimating properly the maximum length of drip irrigation laterals. The aim of this work was to develop a model based on dimensional analysis for calculating head loss along laterals accounting for in-line drippers. Several measurements were performed with 12 models of emitters to obtain the experimental data required for developing and assessing the model. Based on the Camargo &amp; Sentelhas coefficient, the model presented an excellent result in terms of precision and accuracy on estimating head loss. The deviation between estimated and observed values of head loss increased according to the head loss and the maximum deviation reached 0.17 m. The maximum relative error was 33.75% and only 15% of the data set...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Microirrigation; Lateral line; Maximum length.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300442

Benefits of automated acclimatization during the pre-milking phase of lactating girolando cows
Provedor de dados: 70
Autores: Silva,Irenilson M. da; Pandorfi,Héliton; Almeida,Gledson L. P.; Guiselini,Cristiane; Henrique,Hugo M.
The aim of this paper was to evaluate the automated acclimatization effects during pre-milking of cows on thermal conditioning, physiology, milk production and cost-benefit of the automated adiabatic evaporative cooling system (AECS). The treatments 20; 30; 40 min and control consisted of exposure time of pre-milking cows to the automated AECS. Sixteen cows were used with an average daily milk yield of 19 kg, distributed in a 4 x 4 Latin square design. The Tukey's test (P&lt;0.05) was used to compare the means. The environmental variables, dry bulb temperature (DBT, ºC) and relative humidity (RH, %), were recorded every minute, which allowed the determination of the system efficiency through the Temperature and Humidity Index (THI). The respiratory rate...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal comfort; Automation; Dairy cattle; Evaporative cooling system.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500002

Water transfer from São Francisco river to semiarid northeast of Brazil: technical data, environmental impacts, survey of opinion about the amount to be transferred
Provedor de dados: 70
Autores: Stolf,Rubismar; Piedade,Sonia M. de S; Silva,Jair R. da; Silva,Luiz C. F. da; Maniero,Miguel Â.
The transposition of the São Francisco River is considered one of the greatest engineering works in Brazil of all time since it will cross an extensive agricultural region of continental dimensions, involving environmental impacts, water, soil, irrigation, water payment and other multidisciplinary themes. Taking into account its importance, this subject was incorporated into a discipline of UFSCar (Federal University of São Carlos - Brazil) named "Pollution and Environmental Impacts". It was noted strong reaction against the project, even before the presentation. To allow a critical analysis, the first objective was to compile the main technical data and environmental impacts. The second objective was to detect the three most important aspects that cause...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Integration; Water transfer; Volume; Technical data; Northeast; Semiarid.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600001

Swine effluent treatment using anaerobic digestion at different loading rates
Provedor de dados: 70
Autores: Amaral,André C. do; Kunz,Airton; Steinmetz,Ricardo L. R.; Cantelli,Fábio; Scussiato,Lucas A.; Justi,Karin C.
The industrial swine production is characterized by generation of significant effluent amounts that require treatment. The most adopted practices by Brazilian swine farmers have been wastewater storage in lagoons and its subsequent use as a biofertilizer. Nutrient accumulation in soil and water creates the need for an effective management of these residues. The anaerobic digestion process is an important alternative and low-cost treatment for organic matter reduction. However, its efficiency is limited by the digester capacity of solid degradation, especially at low hydraulic retention times. Thus, the present study aimed to verify the behavior of an upflow anaerobic digester by increasing the organic loading rate. This was accomplished in three stages...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydraulic retention time; Biogas production; Animal wastewater.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300019

IMPACT OF LAND USE CHANGE ON THE WATER BALANCE IN A REPRESENTATIVE WATERSHED IN THE SEMIARID OF THE STATE OF PERNAMBUCO USING THE SWAT MODEL
Provedor de dados: 70
Autores: Fontes Júnior,Robertson; Montenegro,Abelardo.
ABSTRACT The Brazilian semiarid region present high rainfall variability and long dry periods. Thus, the main springs and streams are generally intermittent, and both native vegetation and human activities have a strong influence on hydrological processes and the water yield in the watershed. The aim of this study was to investigate the impacts of reforestation of the arboreal Caatinga on the availability of water in a representative basin of the Northeast semiarid with strong anthropic influence, considering a period of severe water scarcity from 2012 to 2015, using the SWAT model as a management tool. The SWAT model successfully simulated the flow hydrograph for the period from 2000 to 2015, with Nash-Sutcliffe (NS) efficiency coefficient of 0.77 and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environmental services; Water resources management; Hydrological modeling.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100110

Índice de capacidade do processo na avaliação da irrigação por aspersão
Provedor de dados: 70
Autores: Justi,André L; Vilas Boas,Marcio A; Sampaio,Silvio C.
Analisar a qualidade da irrigação, além de avaliar seu bom funcionamento, é uma forma de verificar a viabilidade de sua implantação e operação. Como a uniformidade de distribuição é um dos parâmetros mais utilizados para essa avaliação, este trabalho objetivou utilizar técnicas de engenharia de qualidade, usando o índice de capacidade do processo (Cpl) para avaliar a uniformidade de distribuição de água em um sistema de irrigação por aspersão convencional. Os ensaios foram conduzidos no Núcleo Experimental de Engenharia Agrícola, UNIOESTE, com dois aspersores modelo Super10, marca NAANDAN, espaçados 9 m entre si, durante 25 irrigações de 1 h cada. Os dados climáticos foram coletados a cada 10 min, por uma estação meteorológica sem fio. Encontraram-se um...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Controle de qualidade; Velocidade do vento; Uniformidade de distribuição.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200008

Caracterização reológica das diferentes fases de extrato de inulina de raízes de chicória, obtidas por abaixamento de temperatura
Provedor de dados: 70
Autores: Leite,Juliana T. C.; Park,Kil J.; Ramalho,João R. P.; Furlan,Davi M.
A inulina é um ingrediente funcional, geralmente empregado na indústria alimentícia como substituto do açúcar ou da gordura. Esse ingrediente pode ser encontrado em diversos produtos vegetais, incluindo as raízes de chicória. Por ser um produto com solubilidade variável com a temperatura, a inulina sofre uma separação de fases ao ser resfriada, originando uma fase precipitada, mais viscosa, e uma fase sobrenadante, de menor viscosidade. O estudo das propriedades reológicas das diferentes fases do extrato de inulina é importante para o projeto de equipamentos, como misturadores e bombas. Neste trabalho, foi estudado o comportamento reológico, para três condições distintas de temperatura (25; 40 e 50 ºC), das fases sobrenadante e precipitada do extrato...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Viscosidade; Resfriamento; Ingrediente funcional.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100023

Hydrological Modeling of Tributaries of Cantareira System, Southeast Brazil, with the Swat Model
Provedor de dados: 70
Autores: Pontes,Lucas M.; Viola,Marcelo R.; Silva,Marx L. Naves; Bispo,Diêgo F. A.; Curi,Nilton.
ABSTRACT The lack of hydrological data in Brazil is the main limitation for structuring hydrological models, which are able to assist water resources management. Therefore, studies are needed to evaluate the performance of models without on-site calibration. Within this context, the aim of this study was to calibrate the SWAT hydrological model for the Camanducaia River Basin and to evaluate the performance of this calibration in a contiguous drainage basin, one of the Jaguarí River. For the calibration and validation steps, the SWAT-CUP program was utilized. Uncertainty analysis and calculation of efficiency indexes were carried out through the SUFI-2 algorithm. The SWAT adjustment in the Camanducaia River Basin obtained adequate results, with a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Calibration; Model transfer; Uncertainty analysis; Water security.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601037

Production of baruzeiro seedling in different protected environments and substrates
Provedor de dados: 70
Autores: Costa,Edilson; Oliveira,Letícia C. de; Santo,Tiago L. do Espírito; Leal,Paulo A. M.
The high seedlings quality is essential for deployment of homogeneous orchards. This study evaluated the baruzeiro (Dipteryx alata Vog) seedlings formation on different substrates within protected environments. It was used substrates with100% of cattle manure; 100% of cassava stems; 100% of vermiculite; 50% of cattle manure + 50% of cassava stems; 50% of cattle manure + 50% of vermiculite; 50% of cassava stems + 50% of vermiculite; and + ⅓ of cattle manure + ⅓ of cassava stems + ⅓ of vermiculite. These substrates were tested in protected areas: greenhouse; black shade net of 50% shading; and aluminized thermo-reflective screen of 50% shading. A completely randomized experimental design with five replicates of four plants was adopted. Initially, data were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dipteryx alata; Cattle manure; Cassava stems; Vermiculite; Protected cultivation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400002

Análise de aspectos socioeconômicos e tecnológicos da agropecuária na Bacia Hidrográfica do Rio Mogi Guaçu
Provedor de dados: 70
Autores: Zibordi,Marianna S.; Cardoso,João L.; Vilela Filho,Luís R.
Atualmente, com a ocorrência de problemas ambientais e a necessidade de conservação e preservação, a gestão dos territórios de Bacias Hidrográficas apresenta extrema importância. O objetivo do trabalho é levantar e analisar dados socioeconômicos e tecnológicos da Bacia Hidrográfica do Rio Mogi Guaçu - SP, bem como fornecer subsídios para a gestão agropecuária, agrupando os municípios com características semelhantes para os dados levantados, o que poderá orientar ações conjuntas na gestão da Bacia Hidrográfica. Foram levantados dados primários e secundários, sendo utilizados os métodos da análise fatorial em componentes principais e da classificação automática hierárquica, bem como um Sistema de Informações Geográficas para representar os dados por meio de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agropecuária; Bacia hidrográfica; Análise fatorial.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200035

Prediction of free-stall occupancy rate in dairycattle barns through fuzzy sets
Provedor de dados: 70
Autores: Campos,Alessandro T.; Castro,Jaqueline de O.; Schiassi,Leonardo; Yanagi Junior,Tadayuki; Pires,Maria de Fátima Á.; Mattioli,Cristiano C.
The goal of this study was to develop a fuzzy model to predict the occupancy rate of free-stalls facilities of dairy cattle, aiding to optimize the design of projects. The following input variables were defined for the development of the fuzzy system: dry bulb temperature (Tdb, °C), wet bulb temperature (Twb, °C) and black globe temperature (Tbg, °C). Based on the input variables, the fuzzy system predicts the occupancy rate (OR, %) of dairy cattle in free-stall barns. For the model validation, data collecting were conducted on the facilities of the Intensive System of Milk Production (SIPL), in the Dairy Cattle National Research Center (CNPGL) of Embrapa. The OR values, estimated by the fuzzy system, presented values of average standard deviation of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Confinement systems; Bovine facilities; Design; Stalls; Dairy cattle.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600001

Distribution pattern, surface tension and contact angle of herbicides associated to adjuvants on spraying and control of Ipomoea hederifolia under rainfall incidence
Provedor de dados: 70
Autores: Calore,Ricardo A.; Ferreira,Marcelo da C.; Rodrigues,Nara E. L.; Otuka,Alessandra K.
ABSTRACT Scarlet Morning Glory is considered to be an infesting weed that affects several crops and causes serious damage. The application of chemical herbicides, which is the primary control method, requires a broad knowledge of the various characteristics of the solution and application technology for a more efficient phytosanitary treatment. Therefore this study aimed to characterize the effect of rainfall incidence on the control of Ipomoea hederifolia, considering droplet size, surface tension, contact angle of droplets formed by herbicides liquid on vegetal and artificial surfaces, associated to adjuvants and the volumetric distribution profile of the spray jet. The addition of the adjuvants to the herbicide spraying liquid improved the application...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Scarlet morning glory; Glyphosate; Paraquat.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400756

Relações granulométricas no processo de brunimento de arroz
Provedor de dados: 70
Autores: Luz,Carlos A. S.; Luz,Maria L. G. S. da; Bizzi,Luciano T.; Falk,César L.; Isquierdo,Eder P.; Loregian,Rudimar.
O brunimento é uma das etapas de beneficiamento do arroz que tem grande importância sobre o rendimento de engenho. Neste trabalho, analisaram-se relações granulométricas de frações de grãos na massa de arroz e seus efeitos sobre o rendimento de engenho, durante o processo de brunimento. As amostras usadas foram 78 g de arroz descascado, tendo essas partido de amostras originais de 100 g. Foram testadas cinco relações de composição de amostras a serem brunidas, variando as quantidades de grãos quebrados e de quirera que acompanhavam a massa de grãos inteiros, que foram: 1) somente grãos inteiros; 2) 6,16 g de quebrados e 1,04 g de quirera, conforme amostra original; 3) 3,60 g de quebrados e 3,60 g de quirera adicionados aos inteiros; 4) 7,20 g de quebrados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Teste de engenho; Arroz; Grãos quebrados.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100024

CHEMICAL CHANGES OF SOIL AND WATER IN HILLSIDE AREAS UNDER INTENSIVE HORTICULTURE
Provedor de dados: 70
Autores: Silva,Laércio S.; Galindo,Izabel C. de L.; Gomes,Romário P.; Campos,Milton C. C.; Souza,Edivan R. de; Cunha,José M. da.
ABSTRACT Inadequate and intensive management of soils can promote changes in their chemical attributes and impair the quality of surface and groundwater, especially in hillside areas. Therefore, the aim of this study was to identify possible changes in soil and water chemical composition of hillside areas cultivated with horticulture. For this, chemical attributes of three soil depths (0-10, 10-30, and 30-60 cm) were determined in three hillside positions (upper, middle, and lower thirds) of five hillside and adjacent forest areas, as well as water from reservoirs for agricultural use and human consumption. Compared with the forest area, horticultural areas present soil with lower organic matter content and CEC, but higher values of pH, base saturation,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Landscape; Environmental contamination; Management practices; Irrigation water.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300351

Dry months in the agricultural region of Ribeirão Preto, state of São Paulo-Brazil: an study based on the extreme value theory
Provedor de dados: 70
Autores: Blain,Gabriel C.
The application of the Extreme Value Theory (EVT) to model the probability of occurrence of extreme low Standardized Precipitation Index (SPI) values leads to an increase of the knowledge related to the occurrence of extreme dry months. This sort of analysis can be carried out by means of two approaches: the block maxima (BM; associated with the General Extreme Value distribution) and the peaks-over-threshold (POT; associated with the Generalized Pareto distribution). Each of these procedures has its own advantages and drawbacks. Thus, the main goal of this study is to compare the performance of BM and POT in characterizing the probability of occurrence of extreme dry SPI values obtained from the weather station of Ribeirão Preto-SP (1937-2012). According...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Extreme Value distribution; Pareto distribution; Goodness-of-fit tests.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500018

FERTILIZER METERING MECHANISM WITH HELICAL CONIC CYLINDRICAL THREAD FOR FAMILY AGRICULTURE
Provedor de dados: 70
Autores: Galvão,Cezario B.; Albiero,Daniel; Garcia,Angel P.; Monteiro,Leonardo de A.
ABSTRACT Small rural farms are important for Brazilian agribusiness, but equipment suitable for distributing fertilizers on these properties is scarce. We studied a new fertilizer metering mechanism for use on the family farm. It combines a helical conic thread with a conventional fertilizer meter in a cylindrical section. The experimental plan was created using a 24 factorial design. An analysis of variance (ANOVA) was also conducted. The mechanism showed a positive result with respect to the uniformity of fertilizer flow (with a coefficient of variation of 3.1-5.8%), longitudinal distribution (with a coefficient of variation of 4%), and different types of fertilizers (in which variations between 2.7 and 3.5% were found).
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Distribution of fertilizers; Family agriculture; Helical conic thread.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600934

Environment in poultry production covered with thermal and aluminum roofing tiles
Provedor de dados: 70
Autores: OLIVEIRA,FERNANDO G. DE; GODOI,WANESSA M.; PASSINI,ROBERTA.
Brazil is a country of tropical climate, a fact that hinders the poultry production in the aspect of thermal comfort. Thus, we aimed to evaluate the thermal environment in commercial poultry houses with different covers during the months of December 2012 to May 2013, in the municipality of Rio Verde, Goiás. The experimental design was completely randomized in split plots with factorial arrangement of treatments 2x3, being two shed models (thermal and aluminum roof tiles) and three sections within each shed (initial, central and final) for 182 days, having the days as replicates. The thermal environment was assessed through thermal comfort indices: Temperature and Humidity Index, Black Globe Temperature and Humidity Index, Radiant Heat Load and Enthalpy....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal environment; Bioclimatic indices; Roofs.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200206

Physiological responses of caprines raised under different types of covering
Provedor de dados: 70
Autores: Kawabata,Celso Y.; Jesus,Lindalva de A. de; Silva,Ana Paula V. da; Sousa,Thiago V. R. de; Cruz,Luis F. B. da.
Thermal discomfort inside facilities is one of the factors responsible for low productivity of caprines in the Brazilian Northeast region, because inadequate weather conditions can cause elevated rectal temperature, increased respiratory rate, decreased food ingestion and reduced production. The present paper aimed to study the behavior of physiological thermoregulation of the animals (respiratory rate - RR and rectal temperature - RT) at four different times of the day (8 a.m., 11 a.m., 2 p.m. and 5 p.m.) and their relation to bioclimatic indexes (Temperature Humidity Index - THI, Black Globe Humidity Index - BGHI and Radiant Heat Load - RHL) in order to determine whether the type of covering used in the animals facilities (ceramic covering - CC, asbestos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Respiratory rate; Rectal temperature; Thermoregulation.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500003

Fundações de construções submetidas a esforços de tração em solo de alta porosidade da região de Campinas - SP
Provedor de dados: 70
Autores: Paschoalin Filho,João A; Carvalho,David de.
Considerando-se que a maior parte de construções rurais utiliza fundações por estacas escavadas, pequisou-se, neste trabalho, o comportamento à tração de três estacas , submetidas a esforços verticais de tração. O comportamento à tração foi pesquisado, por ser esta situação bastante comum em estruturas leves, como silos, galpões, caixas d'água elevadas, etc. As estacas foram executadas no Campo Experimental para Estudos de Mecânica dos Solos e Fundações da Unicamp, localizado na cidade de Campinas - SP. O subsolo do local é constituído por um solo poroso de Diabásio, cuja primeira camada de 6,5 m é constituída de argila silto-arenosa, seguida de uma camada de silte argilo-arenoso e nível do lençol freático a 17 m de profundidade. Para a verificação do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Construções rurais; Estacas escavadas; Esforços de tração.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200002

Adaptation of "Niagara Rosada" grape must to winemaking by partial cluster dehydration
Provedor de dados: 70
Autores: Santiago,Wesley E.; Teruel,Bárbara J.; Oliveira,Rafael A. De; Silva,João C. T. R. Da.
This study aimed to verify the influence of partial dehydration of "Niagara Rosada" grape clusters in physicochemical quality of the pre- fermentation must. In Brazil, during the winemaking process it is common to need to adjust the grape must when the physicochemical characteristics of the raw material are insufficient to produce wines in accordance with the Brazilian legislation for classification of beverages, which establishes the minimum alcohol content of 8.6 % for the beverage to be considered wine. Therefore, given that the reduction in the water content of grape berries allows the concentration of chemical compounds present in its composition, especially the concentration of total soluble solids, we proceeded with the treatments that were formed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chemical Composition; Must; Drying.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100010

Calibração da Reflectometria no Domínio do Tempo (TDR) para a estimativa da concentração da solução no solo
Provedor de dados: 70
Autores: Souza,Claudinei F.; Folegatti,Marcos V.; Matsura,Edson E.; Or,Dani.
A Reflectometria no Domínio do Tempo (TDR) é um método confiável para medidas in situ da umidade e da concentração da solução no mesmo volume de solo. Entretanto, a interpretação precisa da medida de condutividade elétrica do solo (e umidade do solo) pode requerer uma curva de calibração específica. O objetivo principal deste ensaio foi estabelecer um procedimento de calibração para usar a TDR no cálculo de concentrações de nitrato de potássio (KNO3) em solução do solo. Uma equação que relaciona a condutividade elétrica medida pela TDR e a concentração de KNO3 foram encontradas viabilizando o uso da técnica da TDR na estimativa da umidade e da concentração da solução do solo para o manejo eficiente da fertirrigação.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Concentração de íons; Fertirrigação; Nitrato de potássio.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100030

DEVELOPMENT OF SOFTWARE FOR ANALYSIS OF BEHAVIOR AND WELFARE OF BROILERS
Provedor de dados: 70
Autores: Rodrigues,Tatiana P. N. da S.; Pandorfi,Héliton; Stosic,Borko; Lucena,Aline C. de; Rodrigues,Diogo F. B.
ABSTRACT The objective of this study was to develop a software based on image processing and computer vision techniques for monitoring the feeding/collective behavior of broilers (Cobb) and validate it based on the results obtained from the visual analysis of an expert. The visual analysis was performed based on the observation and quantification of behaviors in the interval of 10 min at each hour of the day, in the period of 24 hours, totaling 1728 frames/day, for males and females. The software was developed using the Hoshen-Kopelman algorithm, for labeling clusters, which would basically be the grouping of similar pixels. This software is written in the 1999 standard of the C language. After this stage of programming, the Hoshen-Kopelman algorithm...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Broiler farming; Image processing; Lighting system; Computer vision.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600657

Test for alternative indicator of soybean sowing depth
Provedor de dados: 70
Autores: SOUZA,NÁTALI M.; WEIRICH NETO,PEDRO H.
Among studies focused on increasing soybean grain yield, the ones related to sowing process are the most significant. Considering that soybean has an epigeal emergence, it becomes difficult to hint at the length covered by hypocotyl up to soil surface, or the actual planting depth. This study aimed to find an indicator that allows the identification of an ideal soybean planting depth. For this purpose, two complementary assays has been carried out in a greenhouse. The first aimed to identify structures that could be indicators of seed planting depth, on a medium-textured soil from Campos Gerais region, in the state of Paraná, Brazil. Spring NK 8350 cultivar seeds were sown at five theoretical depths (1, 2, 3, 4 and 5 cm). As seedlings emerged, the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycine max L.; Planting process; Root.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100128

INCREASED ENERGY COGENERATION IN THE SUGAR-ENERGY SECTOR WITH THE USE OF SUGARCANE STRAW, ELECTRIFICATION OF DRIVES, AND HIGH-DRAINAGE ROLLERS IN THE EXTRACTION
Provedor de dados: 70
Autores: Santos,Paulo S. B. dos; Ramos,Ricardo A. V.
ABSTRACT The sugar-energy sector stands out in the production of electrical energy in the Brazilian energy matrix. The updating of Law 9,427 allowed increasing the limit of power injected in the transmission or distribution systems of existing projects from 30 to 50 MW, encouraging studies of expansion and/or implementation of new cogeneration projects. This study analyzed technologies to enhance energy cogeneration in a plant that sells about 27 MW of surplus power. For this, were studied the use of straw, electrification of drives by steam turbines, and high-drainage rollers (lotus mill roller), which allows reducing bagasse moisture, increasing its lower calorific value (LCV) and, consequently, electrical energy generation. Mass and energy balances in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bioelectricity; Biomass; Combustion; Calorific value; Numerical simulation.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200249

Índices de conforto térmico e respostas fisiológicas de bezerros da raça holandesa em bezerreiros individuais com diferentes coberturas
Provedor de dados: 70
Autores: Kawabata,Celso Y.; Castro,Rafael C. de; Savastano Júnior,Holmer.
Este trabalho avaliou a eficiência de abrigos para bezerros, a partir de índices de conforto térmico (carga térmica radiante, índice de temperatura de globo e umidade e índice de globo negro), pela comparação entre abrigos cobertos por telha de cimento-amianto e telha de cimento- celulose. O experimento foi implantado num sistema de abrigos convencionais, tipo boxe, com cinco tratamentos: telhados de cimento-amianto, cimento-celulose, cimento-celulose pintado de branco e telhado duplo de cimento-celulose, todos expostos ao sol, e telhado de cimento-celulose em área sombreada. Foram realizadas cinco repetições (um bezerro por repetição), de setembro a novembro de 2002, em Pirassununga - SP. As variáveis fisiológicas registradas foram freqüência respiratória...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bovinos; Cimento-amianto; Cimento-celulose.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300004

Water absorbent polymer in sugarcane crop
Provedor de dados: 70
Autores: Marques,Tadeu A.; Marques,Patricia A. A.; Suriani,Marcos W.; Santos,Arleto T. dos; Mendonça,Fernando C.
The water absorbent polymer effect on vegetative growth and production of Theoretical Recovery Sugar (TRS) of sugarcane cv. RB 86 7515 was evaluated on two field tests installed in randomized blocks, with four treatments and five repetitions. The polymer doses were 0; 4; 8 and 12 g m-1 of furrow (test 1) and 0; 1.4; 2.8 and 4.2 g m-1 of furrow (test 2). Test 1 (dec/2007 to may/2009) was implanted in a Distroferric Red Argisol soil in Presidente Prudente - State of São Paulo (SP), Brazil; and the test 2 (Aug/2008 to Aug/2009) was implanted in a Red Yellow Argisol soil in Lucélia - State of São Paulo (SP), Brazil. In test 2, there were no significant differences for any evaluated parameters. In both tests the polymer doses equal to or less than 4 g m-1 of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum spp.; Polymer; Water retention; Polyacrylamide.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100011

Custos da irrigação e receita líquida do feijoeiro em um sistema pivô central sob variação do comprimento da tubulação de recalque e desnível topográfico
Provedor de dados: 70
Autores: Oliveira,Júlio S. de; Zocoler,João L.
Neste trabalho, foi simulado o custo da irrigação de um sistema tipo pivô central com diferentes comprimentos da tubulação de recalque e desníveis topográficos na produção do feijoeiro comum, na região de Ilha Solteira -SP, bem como sua receita líquida. Considerou-se uma área irrigada pelo equipamento de 103,58 ha, sendo sua configuração a mais econômica possível para as variáveis consideradas. A participação da irrigação no custo de produção do feijoeiro variou de 14,8 a 21,5% entre as condições extremas, ou seja, do menor desnível topográfico (40 m) e comprimento da tubulação de recalque (2.000 m) ao maior desnível (80 m) e comprimento (3.000 m). Em todas as configurações do sistema de irrigação e com os preços praticados em agosto de 2008 ou com o preço...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pivô central; Feijoeiro; Custos e lucros.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100013

Viabilidade técnico-econômica do uso de diferentes tecnologias de iluminação para indução de fotoperíodo na produção de mudas de crisântemo
Provedor de dados: 70
Autores: Rossi,Luiz A.; David,Eduardo; Sarubbi,Juliana; Pagliardi,Odail.
Em função de suas características fisiológicas, as mudas de crisântemo necessitam de luz suplementar para evitar formação de botão floral. Isto é feito no período noturno. O presente trabalho visou a analisar a viabilidade técnico-econômica de substituir-se a atual tecnologia de iluminação artificial utilizada pelos produtores (lâmpadas incandescentes) para efeito de indução de fotoperíodo em ambiente protegido, pela tecnologia de lâmpadas de descarga, com o objetivo de reduzir o consumo de energia elétrica utilizada no processo. As lâmpadas de descarga possuem maior vida útil e apresentam menor consumo de energia quando comparadas às lâmpadas incandescentes. Os resultados das análises permitem concluir que a lâmpada fluorescente compacta integrada...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eficiência energética; Iluminação artificial; Energização rural; Indução de fotoperíodo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500004

DISTRIBUTION OF MAIZE SEED IN A SEEDING LINE PROTOTYPE USING MICROCONTROLLED DATA ACQUISITION SYSTEMS
Provedor de dados: 70
Autores: Reis,Elton F. dos; Borges Neto,Antônio C.; Couto,Ródney F.
ABSTRACT: The aim of this study was evaluate the longitudinal distribution of maize seeds using a seeding line prototype, whit a microcontroller data acquisition system, at different speeds and types of horizontal feeder discs. Initially it was constructed a prototype simulator of seeding line, in the laboratory, and mounted two systems of microcontroller data acquisitions with infrared sensors for maize seeds counting. A test was conducted in a completely randomized design in split plots with factorial scheme of treatments 5 x 2 x 2, being the parcel two types of microcontroller data acquisition systems (infrared sensors in parallel and an diffuse infrared sensor), the factors were two feeder discs of maize seeds (inclined and normal) and five sowing...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensor; Microcontroller; Horizontal disc.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601148

Seleção dos indicadores da qualidade das águas superficiais pelo emprego da análise multivariada
Provedor de dados: 70
Autores: Andrade,Eunice M. de; Araújo,Lúcia de F. P.; Rosa,Morsyleide F.; Disney,Walt; Alves,Aurilea B.
Os fatores antrópicos e naturais que determinam a qualidade das águas superficiais na Bacia do Baixo Acaraú foram identificados pelo emprego da técnica de Análise Fatorial/Análise da Componente Principal (AF/ACP). Foram realizadas quatro campanhas no período de fev./2003 a mar./2004, em sete pontos de amostragem localizados ao longo do Rio Acaraú. Foram analisados 25 parâmetros físico-químicos e bacteriológicos. Pelo emprego da AF/ACP, identificou-se que o modelo de melhor ajuste para expressar a qualidade das águas na Bacia do Baixo Acaraú foi aquele composto por quatro fatores, explicando 82,1% da variância total. O primeiro fator representa a componente de sólidos em suspensão, expressando o processo de erosão e escoamento superficial. O segundo fator é...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Análise fatorial; Poluição hídrica; Bacia hidrográfica.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400011

The impact of evaporative cooling on the thermoregulation and sensible heat loss of sows during farrowing
Provedor de dados: 70
Autores: Justino,Eliene; Nääs,Irenilza de A.; Carvalho,Thayla M. R.; Neves,Diego P.; Salgado,Douglas D'Alessandro.
Pigs are more sensitive to high environmental temperatures explained by the inability of sweating and panting properly when compared to other species of farmed livestock. The evaporative cooling system might favor the thermal comfort of animals during exposure to extreme environmental heat and reduce the harmful effects of heat stress. The purpose of this study was to assess the sensible heat loss and thermoregulation parameters from lactating sows during summer submitted to two different acclimatization systems: natural and evaporative cooling. The experiment was carried out in a commercial farm with 72 lactating sows. The ambient variables (temperature, relative humidity and air velocity) and sows physiological parameters (rectal temperature, surface...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Ventilation; Thermal stress; Panting; Surface temperature; Swine; Lactation.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600003

Energy expenditure in vocalizations of pigs under stress
Provedor de dados: 70
Autores: Cordeiro,Alexandra F. da S.; Naas,Irenilza A.; Medeiros,Brenda B.; Maia,Ana Paula de A.; Pereira,Erica M.
Modern swine production faces many challenges nowadays, among which are productivity growth, meat quality improvement, decrease of environmental damage and reduction of cost production. Pigs spend energy to vocalizing, especially when they undergo stress. The waste of energy can increase the cost of production and lead to greater environmental damage. The goal of this study was to estimate the energy spent by pigs under the stress of castration and its effect on the animals' weight gain. Two groups of ten animals each were castrated, being one group with local anesthetic and the other without anesthetic. The piglets' vocalizations were recorded during different stages of the neutering process and then estimated of the amount of energy emitted during each...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal well-being; Signal analysis; Swine production.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500001

Variabilidade espacial de atributos químicos de um argissolo para aplicação de insumos à taxa variável em diferentes formas de relevo
Provedor de dados: 70
Autores: Barbieri,Diogo M.; Marques Júnior,José; Pereira,Gener T.
A agricultura de precisão implica análise da variabilidade espacial de fatores de produção e a aplicação de insumos de forma localizada. Várias são as causas que condicionam a variabilidade espacial dos solos, sendo o relevo um dos fatores mais importantes. O presente estudo teve por objetivo analisar a variabilidade espacial dos atributos químicos do solo e a elaboração de mapas de necessidade de aplicação de insumos de forma localizada, em áreas com diferentes formas de relevo. Duas parcelas de 1 ha cada foram delimitadas em áreas com topografia côncava e convexa. Foram retiradas, em cada área, 242 amostras de solos em 121 pontos, nas profundidades de solo de 0,00-0,20 m e 0,20-0,40 m. Os resultados de análise química foram submetidos às análises da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Geoestatística; Manejo localizado.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400004

Rheological behavior of Chlorella sp. e Scenedesmus sp. cultures in different biomass concentrations
Provedor de dados: 70
Autores: Santos,Michel de O. dos; Martins,Márcio A; Coimbra,Jane S. dos R.; Gates,Richard S.; Corrêdo,Lucas de P.
Studies involving the use of microalgae are increasingly intensifying for the potential they present to produce biofuels, because they are a renewable energy source that does not compete directly with food production, and because they enable the obtaining of a fuel with less environmental impact when compared to fossil fuel. In this context, the use of microalgae is directly associated to its capacity to be produced on a large scale and to be extracted from the culture medium. Rheological studies are important for obtaining the information needed in the elaboration of projects and equipment that will be used in various operations existing in systems of production and extraction of algal biomass. In the evaluation of different levels of dry biomass...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Microalgae; Biomass; Production; Operation.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500017

Consumo de combustível na operação de subsolagem realizada antes e depois de diferentes sistemas de preparo periódico do solo
Provedor de dados: 70
Autores: Salvador,Nilson; Benez,Sérgio H.; Mion,Renildo L.
A subsolagem tem aumentado nos últimos anos de forma indiscriminada, faltando estudos que norteiem os melhores procedimentos para que novos problemas não sejam acrescentados devido a subsolagens inadequadas ou mesmo em solos onde a operação é desnecessária, e principalmente buscar redução no consumo de combustível. Dessa forma, este trabalho teve o objetivo de avaliar o consumo de combustível na operação de subsolagem efetuada antes e depois de diferentes sistemas de preparo periódico do solo, classificado como Nitossolo Vermelho distroférrico. Os preparos foram realizados com arado de discos, arado de discos mais uma gradagem de nivelamento, grade pesada, grade pesada mais gradagem de nivelamento e escarificador. A realização da subsolagem depois dos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Subsolador; Potência; Implementos; Deslizamento das rodas motrizes; Velocidade operacional.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200006

Perdas na colheita mecanizada de soja no estado de Minas Gerais
Provedor de dados: 70
Autores: Campos,Marco A. O.; Silva,Rouverson P. da; Carvalho Filho,Alberto; Mesquita,Hugo C. B.; Zabani,Samir.
O presente trabalho teve por objetivo avaliar as perdas na colheita de soja em função da idade, velocidade de trabalho, sistema de trilha (axial e radial) e condição de propriedade das colhedoras (própria ou alugada), nas regiões do Triângulo Mineiro e Alto Paranaíba - MG, durante a colheita de soja da safra 2002-2003. A velocidade de trabalho das colhedoras e a rotação do cilindro de trilha também foram estudadas, à exceção de quando avaliadas como variável-função. Os resultados obtidos permitiram concluir que as perdas de grãos independem da velocidade das colhedoras e que as colhedoras com até cinco anos, independentemente da sua taxa de utilização anual, tiveram menores perdas do que as colhedoras com mais de seis anos. As colhedoras próprias...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistema de trilha; Colhedoras; Velocidade de trabalho.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100023

Características comportamentais de suínos em crescimento e terminação em sistema “wean to finish”
Provedor de dados: 70
Autores: Massari,Juliana M.; Curi,Thayla M. R. de C; Moura,Daniella J; Medeiros,Brenda B. L.; Salgado,Douglas D'alessandro.
RESUMO O “wean to finish” é um sistema de criação de suínos, no qual os animais permanecem em uma mesma instalação do desmame até à fase de abate. Objetivou-se estudar o comportamento dos animais em alojamento exclusivo de 26 machos suínos (T1), misto (T2), contendo 13 machos e 13 fêmeas, e o tratamento único de fêmeas (T3), com 26 animais. Para isso, utilizou-se da análise multivariada, por meio da análise dos gráficos de componentes principais, por ser um artifício interessante utilizado por diversos pesquisadores para identificar quais variáveis são fortemente ou não correlatas. Assim, indica-se que o aumento da temperatura ambiental predispõe ao comportamento deitado em todos os tratamentos avaliados. No tratamento exclusivo de suínos machos castrados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bem-estar; Comportamento; Instalação animal; Multivariada; Produção comercial; Suinocultura.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400646

Tratamento de efluente de abatedouro de tilápia com adição de manipueira na fase anóxica
Provedor de dados: 70
Autores: Kummer,Ana Carolina B; Andrade,Lidiana de; Gomes,Simone D; Fazolo,Ajadir; Hasan,Salah D. M; Machado,Fabiano.
O objetivo deste trabalho foi avaliar a desnitrificação de efluente de abatedouro de tilápia, em reator em batelada. Para isto, foi avaliado o efluente gerado por uma indústria processadora de mandioca (manipueira) como fonte de carbono. Também foram avaliadas as condições de agitação do sistema. Os experimentos foram conduzidos em escala de laboratório, em que foram testados cinco níveis de agitação (20; 32; 60; 88 e 100 rpm) e cinco níveis de relação DQO/N (0,1; 1,0; 3,2; 5,4 e 6,3), configurando-se um planejamento do tipo Delineamento Composto Central Rotacional (DCCR), com quatro ensaios nos níveis +1 e - 1; quatro ensaios nos níveis dos pontos axiais (-1,414 e +1,414) e mais uma triplicata no ponto central (0), totalizando 11 ensaios. Avaliaram-se o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Remoção biológica; Desnitrificação; Nitrato; Nitrito; Efluente de abatedouro de peixe; Efluente de fecularia.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100015

Determination of the influence of the variation of reducing and non-reducing sugars on coffee quality with use of artificial neural network
Provedor de dados: 70
Autores: Messias,José A. T.; Melo,Evandro de C.; Lacerda Filho,Adílio F. de; Braga,José L.; Cecon,Paulo R.
The present study aimed at evaluating the use of Artificial Neural Network to correlate the values resulting from chemical analyses of samples of coffee with the values of their sensory analyses. The coffee samples used were from the Coffea arabica L., cultivars Acaiá do Cerrado, Topázio, Acaiá 474-19 and Bourbon, collected in the southern region of the state of Minas Gerais. The chemical analyses were carried out for reducing and non-reducing sugars. The quality of the beverage was evaluated by sensory analysis. The Artificial Neural Network method used values from chemical analyses as input variables and values from sensory analysis as output values. The multiple linear regression of sensory analysis values, according to the values from chemical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffee quality; Chemical analysis; Classification; Computer systems.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200015

Manejo da irrigação na cultura do feijoeiro em sistemas plantio direto e convencional
Provedor de dados: 70
Autores: Pavani,Luiz C.; Lopes,Adriano S.; Galbeiro,Rafael B.
O manejo inadequado do solo e da água é limitante à produtividade do feijoeiro irrigado. O objetivo deste trabalho foi avaliar dois métodos de manejo da irrigação, um via solo (tensiometria) e outro via clima (tanque Classe A), conjugados com os sistemas plantio direto e convencional de manejo do solo com a cultura do feijoeiro de "inverno", no segundo ano de plantio direto, em Jaboticabal - SP. Foi medido o potencial mátrico do solo e estimada a variação diária do armazenamento de água no solo, na camada de 0 a 0,40 m de profundidade, e avaliados os componentes de produtividade, além de determinadas a evapotranspiração real média e a eficiência média de uso de água pela cultura. O sistema de preparo convencional do solo com manejo de irrigação pelo tanque...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus vulgaris; Evapotranspiração real; Eficiência de uso de água.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100002

Avaliação do desempenho de dispositivo de corte de base de colhedora de cana-de-açúcar
Provedor de dados: 70
Autores: Salvi,José V.; Matos,Marcos A.; Milan,Marcos.
A utilização da colheita mecanizada na cana-de-açúcar faz surgir preocupações quanto à qualidade do corte e à perda de matéria-prima; para minimizar esses problemas, os fabricantes de colhedoras têm desenvolvido dispositivos para auxiliar o operador no controle da altura de corte. Em vista disso, o objetivo deste trabalho foi avaliar o desempenho qualitativo de um dispositivo semi-automático de controle de altura de corte basal, instalado em uma colhedora de cana picada. Analisou-se em duas situações, com e sem o uso do dispositivo, a variabilidade da altura de corte, tocos arrancados e impureza mineral, por meio de estatística descritiva. Para as condições analisadas, o corte de base não está sob controle estatístico, não sendo possível manter a altura de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanização; Colheita; Controle de qualidade.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100014

Physical characteristics of oily spraying liquids and droplets formed on coffee leaves and glass surfaces
Provedor de dados: 70
Autores: Decaro Junior,Sergio T.; Ferreira,Marcelo da C.; Lasmar,Olinto.
The physical characteristics of a spray liquid are important in getting a good droplet formation and control efficiency over a particular target. As a function of these characteristics, it is possible to decipher which is the best adjuvant based on the respective concentration used during the spray. Therefore, ten spraying liquids were prepared, which varied in concentrations of pesticide lufenuron + profenofos, mineral oil, water and manganese sulfate. Pendant droplets formed from these mixtures were measured to examine their impact on surface tension. Droplets were applied to the surface of coffee leaves and the surface tension, contact angle formed and the leaf area wetted by the droplet, were measured. A smooth glass surface was taken as a comparative...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Surface tension; Contact angle; Wetted area; Oil.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300588

Kinetic behavior of nitrification in the post-treatment of poultry wastewater in a sequential batch reactor
Provedor de dados: 70
Autores: Mees,Juliana B. R.; Gomes,Simone D.; Vilas Boas,Márcio A.; Gomes,Benedito M.; Passig,Fernando H.
A sequential batch reactor with suspended biomass and useful volume of 5 L was used in the removal of nutrients and organic matter in workbench scale under optimal conditions obtained by central composite rotational design (CCRD), with cycle time (CT) of 16 h (10.15 h, aerobic phase, and 4.35 h, anoxic phase) and carbon: nitrogen ratio (COD/NO2--N+NO3--N) equal to 6. Complete cycles (20), nitrification followed by denitrification, were evaluated to investigate the kinetic behavior of degradation of organic (COD) and nitrogenated (NH4+-N, NO2--N and NO3--N) matter present in the effluent from a bird slaughterhouse and industrial processing facility, as well as to evaluate the stability of the reactor using Shewhart control charts of individual measures. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrifying activity; Kinetic constants; Nutrient removal; Quality control; Processing capacity.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500013

SPATIAL CORRELATION OF SOYBEAN PRODUCTIVITY, ENHANCED VEGETATION INDEX (EVI) AND AGROMETEOROLOGICAL VARIABLES
Provedor de dados: 70
Autores: Grzegozewski,Denise M.; Uribe-Opazo,Miguel A.; Johann,Jerry A.; Guedes,Luciana P. C.
ABSTRACT The survey information from growing regions, the interaction with the vegetation index and climatic variables is of great importance in the search for soybean productivity increase. Paraná is the second largest soybean producer in Brazil and presents great spatial variability, both in periods of the crop cycle as in soil and climate. The objective of this study was to analyze the spatial correlation of soybean productivity, the enhanced vegetation index (EVI) and agrometeorological variables (water balance, global radiation and average temperature) in the state of Paraná, on a decendial scale, using the Moran global autocorrelation index between the 2010/2011 and 2012/2013 crop years. Similarity was found in the average productivities in 2010/2011...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Culture cycle; Spatial statistics of areas; Climatic variability.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300541

REFERENCE EVAPOTRANSPIRATION FORECASTING BY ARTIFICIAL NEURAL NETWORKS
Provedor de dados: 70
Autores: Alves,Walison B.; Rolim,Glauco de S.; Aparecido,Lucas E. de O.
ABSTRACT: Evapotranspiration (ET) is the main component of water balance in agricultural systems and the most active variable of the hydrological cycle. In the literature, few studies have used the forecast the day before via Artificial Neural Networks (ANNs) for the northern region of São Paulo state, Brazil. Therefore, this aimed to predict the reference evapotranspiration for Jaboticabal, the major sugarcane-producing region of São Paulo state. We used a historical series of data on average air temperature, wind speed, net radiation, soil heat flux, and daily relative humidity from 2002 to 2012, for Jaboticabal, SP (Brazil). ET was estimated by Penman-Monteith method. To forecast reference evapotranspiration, we used a feed-forward Multi-Layer...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modeling; Multi-Layer Perceptron; Air temperature; Estimate.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601116

FORM OF LAYING HENS EGGS IN THE FUNCTION OF DIFFERENT LAMPS USED IN PRODUCTION
Provedor de dados: 70
Autores: Pereira,Danilo F.; Tavares,Bartira de O.; Lean,Priscilla A. B. Mac.
ABSTRACT: Lighting, either in its intensity or in its luminous spectrum, affects the eggs quality. This study evaluated the effect of four lamps (sodium vapor lamp, mercury vapor lamp, fluorescent lamp and incandescent lamp) that have different luminous spectra in the form of commercial poultry eggs. For this, 60 laying hens of the same age were separated for 63 days in four aviaries with reduced and distorted scale. In each treatment, different lamps were installed which provided similar luminous intensities. At the end of the period, these eggs were taken as samples for the fluorescent, incandescent, mercury vapor and sodium vapor lamps. In this way, images were made of these eggs, using a camera installed on a fixed tripod on a flat table with black...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environment; Image analysis; Precision animal production.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500848

Cloroplast pigments as indicators of lead stress
Provedor de dados: 70
Autores: Gomes,Silvânia M. de S.; Lima,Vera Lucia A. de; Souza,Adailson P. de; Nascimento,Joab J. V. R. do; Nascimento,Everaldo S. do.
Plants respond to environmental adversities, becoming an indicator for assessing the environment quality. In this aspect, chlorophyll contents as well, carotenoids are used as a reliable indicator to associate environmental quality and pollution, mainly regarding the toxicity of heavy metals in higher plants. So, we aimed to evaluate the content of chlorophyll a, b, and total chlorophylls and carotenoids in plants vetiver [Vetiveria zizanioides (L.) Nash], maize (Zea mays L.) cv. AG 1051, sunflower (Helianthus annuus L.) cv. BRS 122/V-2000, and castor beans (Ricinus communis L. ) cv . Northeastern BRS grown in contaminated soil with lead, with and without correction of soil pH, so they were used as indicators of metal stress by the soil. From the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Heavy metal; Pollution; Photosynthesis.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500007

TIMBER BEAM REPAIR BASED ON POLYMER-CEMENTITIOUS BLENDS
Provedor de dados: 70
Autores: Christoforo,André L.; Panzera,Tulio H.; Araujo,Victor A. de; Fiorelli,Juliano; Lahr,Francisco A. R.
ABSTRACT This study aims to manufacture and apply polymer-cementitious blends based on a combination of epoxy polymer and Ordinary Portland Cement (OPC) for timber beam repair. The material was used to repair timber beams of “Maçaranduba” (Manilkara sp.) and “Cedro doce” (Cedrella spp) wood species. A full factorial design was conducted to investigate the effect of cement particle content (0wt%, 30wt%, 40wt% and 50wt %), type of cement (ASTM-II and ASTM-III), and pigment addition (0wt% and 0.2wt%) on the physical and mechanical properties of the blend. The cement content factor affected all properties investigated. The highest elastic modulus was achieved by the blends produced with 50wt% of cement and 0.2wt% of pigment inclusion. This condition was used...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wood; Bending; Beams; Composite section; Connectors.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200366

TIME AVAILABLE FOR SPRAYING AND MECHANIZED SOWING IN THE NORTHEAST OF THE STATE OF MATO GROSSO DO SUL AND SOUTH OF GOIÁS
Provedor de dados: 70
Autores: Gava,Ricardo; Scarpin,Igor M.; Baio,Fabio H. R.; Wassolowski,Carlos R.; Neves,Danilo C.
ABSTRACT The sizing of mechanized agricultural systems depends on the soil and climatic conditions, the crop and the work regime. The aim of this study was to determine the probabilities of time available during an agricultural year for mechanized spraying and sowing in the northeast region of the State of Mato Grosso do Sul and south of Goiás. The meteorological restrictions imposed as unfavorable hours were: ambient temperature above 32°C, relative air humidity below 50%, wind velocity above 15 km h-1 and soil volumetric moisture above 39% (humidity equivalent to 90% of the available water capacity for the studied soil). The mathematical models were elaborated for eight years, based on the historical data of the automatic station of the National...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural machines; Selection of machines; Mechanized systems.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300443

ERRATA
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300614

Emissão de CO2 do solo associada à calagem em área de conversão de laranja para cana-de-açúcar
Provedor de dados: 70
Autores: Silva,Eliton de F.; Moitinho,Mara R.; Teixeira,Daniel de B.; Pereira,Gener T.; La Scala Junior,Newton.
A emissão de CO2 do solo (FCO2) em áreas agrícolas é resultante da interação de diversos fatores, sendo alterada pela prática de manejos do solo e da cultura, além das condições edafoclimáticas locais. Neste estudo, objetivou-se quantificar a FCO2 em função da calagem e posição da aplicação (antiga linha e entrelinha) da cultura da laranja em área de conversão para a cultura da cana-de-açúcar, no município de Frutal-MG. Os tratamentos avaliados foram: Linha/CC (linha com aplicação de calcário); Entrelinha/CC (entrelinha com aplicação de calcário); Linha/SC (linha sem aplicação de calcário), e Entrelinha/SC (entrelinha sem aplicação de calcário). FCO2, temperatura do solo (Ts) e umidade do solo (Us) foram avaliadas durante 12 dias. O maior valor médio da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Calagem; Respiração do solo; Temperatura do solo; Umidade do solo.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500008

Variação de vazão de gotejadores de fluxo normal enterrados na irrigação de café
Provedor de dados: 70
Autores: Faria,Luis F.; Coelho,Rubens D.; Resende,Ronaldo S.
Este trabalho teve como objetivo obter informações sobre o desempenho de gotejadores enterrados (irrigação subsuperficial), quanto ao aspecto de variação de vazão em função da intrusão radicular da cultura do café. As mudas de café foram irrigadas por sete modelos diferentes de gotejadores de fluxo normal, instalados a duas profundidades (15 e 30 cm da superfície do solo) e em dois níveis de depleção de água no solo (tratamentos úmido e seco). O trabalho foi conduzido em vasos e sob ambiente controlado, utilizando mudas de cafeeiro em estágio inicial de desenvolvimento. Concluiu-se que, até os 120 dias do início do experimento, não houve modelo de emissor que se destacasse quanto à penetração de raízes e, a partir daí, diferenças na suscetibilidade dos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gotejamento; Intrusão radicular; Entupimento.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300011

Perda de carga em filtros orgânicos utilizados no tratamento de água residuária de suinoculturas
Provedor de dados: 70
Autores: Matos,Antonio T. de; Magalhães,Marcos A. de; Sarmento,Antover P.
Com a realização deste trabalho, objetivou-se parametrizar a equação de evolução da perda de carga, para descrição do processo de filtração de água residuária da suinocultura. No preenchimento das colunas filtrantes, foram utilizados bagaço de cana-de-açúcar triturado, serragem de madeira e pergaminho de grãos de café. Dados de perda de carga em diferentes profundidades e tempos de operação dos filtros orgânicos foram coletados para ajuste das equações de perda de carga. Para as equações ajustadas, foram obtidos altos coeficientes de determinação, sendo que a significância dos coeficientes da regressão foi, na sua quase totalidade, de 1% de probabilidade, podendo ser utilizada na predição do comportamento dos filtros. As variáveis tempo de operação e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Filtragem; Tratamento de efluentes; Queda de pressão.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300016

Produtividade de plantas forrageiras em função de manejo do solo
Provedor de dados: 70
Autores: Vitória,Edney L. da; Fernandes,Haroldo C.; Teixeira,Mauri M.; Cecon,Paulo R.
O manejo do solo inadequado, aliado a uma baixa fertilidade do solo, constitui um dos principais fatores limitantes da produção pecuária nas regiões tropicais. Objetivou-se neste trabalho avaliar a produtividade de duas espécies de plantas forrageiras submetidas a três sistemas de preparo do solo, obtendo as correlações entre produtividade de matéria seca e índice de área foliar, em função do período de crescimento. O experimento foi instalado em esquema de parcela sub-subdividida, no delineamento em blocos casualizados, com quatro repetições. Somente o manejo do solo, o período e a interação entre o período e a forrageira apresentaram diferença considerada significativa (p &lt; 0,05) em relação à produção de matéria seca e índice de área foliar. Porém,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Preparo do solo; Forragicultura; Propriedades físicas do solo.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500014

Variabilidad espacial de atributos físicos de un Typic Haplustox de los Llanos Orientales de Colômbia
Provedor de dados: 70
Autores: Ramírez-López,Leonardo; Reina-Sánchez,Amparo; Camacho-Tamayo,Jesús H.
O objetivo deste trabalho foi estudar o comportamento da variabilidade espacial da resistência mecânica à penetração (RP), da densidade do solo, da densidade de partículas do solo, da porosidade total e dos teores de areia, silte e argila, e as relações existentes entre as propriedades analisadas. O estudo foi desenvolvido em Puerto López (Meta-Colômbia). As amostras do solo foram coletadas em duas profundidades (0 - 0,10 e 0,10 - 0,20 m), em intervalos regulares de 25 m, em malha regular, compreendendo 42 pontos, sendo a RP medida até 0,42 m de profundidade. A RP não se correlacionou com nenhuma propriedade, na primeira profundidade. De 0,10 - 0,20 m de profundidade, a RP correlacionou-se com os teores de silte e areia. Os semivariogramas da RP não...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compactação; Geoestatística; Oxissol.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100006

Sombreamento arbóreo e orientação de instalações avícolas
Provedor de dados: 70
Autores: Alves,Sulivan P.; Rodrigues,Edmundo H. V.
Este trabalho teve como objetivo estudar a contribuição do sombreamento arbóreo para amenizar a radiação solar em instalações avícolas. Foram analisadas, por meio de simulação gráfica, instalações com dimensões utilizadas em produção avícola, com a cumeeira orientada na direção leste-oeste, bem como na norte-sul, situadas nas latitudes 0; 10; 20 e 30º S e o sombreamento proporcionado por árvores de geometria de forma globosa. A eficiência do sombreamento foi analisada por meio de um Índice de Sombreamento (Isg), em função da localização temporal e espacial da instalação, que considera o efeito sombreador da árvore, interna e externamente. Para condições de verão, foi observado que, para o Norte e Nordeste do Brasil, o uso do sombreamento foi mais eficiente...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sombreamento; Avicultura; Conforto ambiental.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200001

Estimating the most important criteria for hatching eggs as function of broiler breeders age
Provedor de dados: 70
Autores: Baracho,Marta dos S.; Nääs,Irenilza de A.; Neves,Diego P.; Cassiano,Juliano de A.; Lima,Fabiana G.; Moura,Daniella J. de; Garcia,Rodrigo G.
This research aimed to compare two female broiler breeder ages during the incubation period regarding management using the Analytic Hierarchy Process method (AHP). This method is characterized by the possibility of analyzing a multicriteria problem and assists a decision making. This study was carried out on a commercial hatchery located in São Paulo, Brazil. Two ages of broiler breeder (42 and 56 weeks) were compared relative to production rate. Production index data were the same in both ages and were submitted to multicriteria decision analysis using the AHP method. The results indicate that broiler breeders of 42 weeks presented better performance than those of 56 week-old. The setter phase (incubation) is more critical than the hatcher. The AHP method...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Multi-stage incubator; Multi criteria analysis; Broiler breeders' production.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300002

Agregação de um latossolo vermelho submetido a cinco sistemas de preparo do solo em Uberaba - MG
Provedor de dados: 70
Autores: Carvalho Filho,Alberto; Silva,Rouverson P. da; Centurion,José F.; Carvalho,Luís C. C.; Lopes,Afonso.
Visando à obtenção de dados relativos aos efeitos de sistemas de preparo periódico do solo e sua relação com a degradação do solo e a capacidade de incorporação de resíduos, avaliaram-se a distribuição percentual de agregados do solo, o diâmetro médio geométrico, o módulo de finura e a incorporação de resíduos, durante o ano agrícola de 2001-2002. A área em estudo foi classificada como Latossolo Vermelho distrófico, localizada no município de Uberaba - MG. Utilizou-se do delineamento estatístico em blocos casualizados com quatro repetições, tendo como tratamentos o preparo periódico primário do solo com o escarificador, enxada rotativa, arado de aivecas, grade aradora e arado de discos. As análises dos resultados mostraram a enxada rotativa e a grade...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cobertura vegetal; Diâmetro médio geométrico; Distribuição de agregados do solo.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100026

Avaliação da deposição de calda em anteras de trigo, para o estudo do controle químico de giberela (Gibberella zeae)
Provedor de dados: 70
Autores: Panisson,Edivan; Boller,Walter; Reis,Erlei M.
A giberela, causada pelo fungo Gibberella zeae (Fusarium graminearum), é uma importante doença de infecção floral do trigo. Para controlar essa doença, o fungicida deve ser aplicado durante a antese, de modo a proteger as anteras. Os objetivos do presente trabalho foram de construir uma barra de pulverização que permitiu utilizar bicos em diferentes arranjos e quantificar a presença de corante nas anteras quando aplicado com diferentes pontas de pulverização, direções dos bicos na barra e com diferentes volumes de calda. Utilizaram-se pontas de jato plano (XR-11002), jato plano duplo (110DB2) e jato cônico vazio (JA-2), espaçadas em 0,50 m, em uma barra tradicional e numa barra modificada. Na barra modificada, foram utilizados corpos duplos giratórios,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Barras de pulverização; Pontas de pulverização; Anteras soltas e presas.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100013

Desempenho do modelo AcquaNetXL na alocação de água em sistemas de recursos hídricos complexos
Provedor de dados: 70
Autores: Schardong,André; Méllo Júnior,Arisvaldo V.; Roberto,Alexandre N.; Porto,Rubem La L.
Este artigo apresenta uma ferramenta para análise de sistemas complexos de recursos hídricos denominada AcquaNetXL, que foi desenvolvida no formato de planilha eletrônica, na qual foram incorporados dois modelos de otimização, um linear e outro não linear. Essa ferramenta mantém os conceitos e os atributos de um sistema de suporte a decisão, ou seja, possui as características de estreitar a comunicação entre o usuário e o computador, de facilitar o entendimento, a formulação do problema, a interpretação dos resultados de análise e auxiliar no processo de tomada de decisão, tornando-o mais ordenado, objetivo e transparente. O desempenho do algoritmo utilizado na solução dos problemas de alocação de água foi satisfatório, especialmente para o modelo linear.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas de Suporte a Decisões; Simulação hidrológica; Otimização.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400021

Identificação e mapeamento de áreas de milho na região sul do Brasil utilizando imagens MODIS
Provedor de dados: 70
Autores: Yi,José L. R.; Shimabukuro,Yosio E.; Quintanilha,José A.
O presente trabalho teve como proposta avaliar a identificação e o mapeamento das áreas de milho da região noroeste do Estado do Rio Grande do Sul a partir de dados multitemporais do sensor MODIS (Moderate Resolution Imaging Spectroradiometer) a bordo do satélite Earth Observing System - EOS-AM (Terra). O algoritmo de classificação supervisionada Spectral Angle Mapper (SAM) foi aplicado com sucesso em uma série multitemporal de imagens EVI pré-processadas. Verificou-se que as áreas classificadas como milho na imagem coincidiam plenamente com áreas mais extensas ou contínuas (&gt; 90 ha) de milho. Áreas de menor extensão ou localizadas em encostas de morros, ao lado de vegetação arbórea, não foram detectadas pelo classificador devido à baixa resolução...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Índices de vegetação; Classificação supervisionada; Sensoriamento remoto orbital.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400019

SOIL WATER RETENTION CURVE AND S INDEX AS SOIL PHYSICAL QUALITY INDICATORS FOR INTEGRATED PRODUCTION SYSTEMS
Provedor de dados: 70
Autores: Magalhães,Wellington de A.; Freddi,Onã da S.; Wruck,Flávio J.; Petter,Fabiano A.; Tavanti,Renan F. R.
ABSTRACT Assess the physical quality of agricultural soils it is important to establish the management more adequate for plant growth. In this study, the soil water retention curve and S index as indicators of soil physical quality were evaluated in five integrated production systems in the following forestry arrangements: Eucalyptus in a single line, double line and triple line (Eucalyptus I, II and III respectively), Balsa in triple line and Teak triple line. The density and arrangement of forest trees influence the soil physical properties. Less soil water retention was observed in the Teak and Balsa wood systems in the layers 0-0.10 and 0.10-0.20 m. The field capacity, permanent wilting point, and available water were lower under the projection from...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eucalyptus; Pore size distribution; Soil structure; ICLF.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100064

Application of response surface methodology to study the biological removal of nitrogen from effluent of cattle slaughterhouse in a sequencing batch reactor
Provedor de dados: 70
Autores: Lima,Adriana N. de; Gomes,Benedito M.; Gomes,Simone D.; Carvalho,Karina Q. de; Christ,Divair.
The aim of this study was to evaluate the efficiency of a sequencing batch reactor (SBR) on biological removal of nitrogen from cattle slaughterhouse wastewater by nitrification/denitrification processes. The effects of initial concentration of ammoniacal nitrogen were investigated at 100; 150 and 200 mg L-1 and air flow rate at 0.125; 0.375 and 0.625 L min¹ Lreactor-1 on the nitrogen compounds removal, by a Central Composite Rotational Design (CCRD) configuration. There were variations from 9.2 to 94.9%, 4.0 to 19.6% and 20.8 to 92.0% in the conversion of ammoniacal nitrogen to nitrate and nitrite concentration and removal of total nitrogen, respectively. The increase of air flow rate and decrease of the initial concentration of ammoniacal nitrogen...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrification; Denitrification; Central composite rotational design.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200017

Contribuição da estrutura interna na perda de carga de filtros de areia utilizados na irrigação
Provedor de dados: 70
Autores: Mesquita,Marcio; Testezlaf,Roberto; Salcedo,Juan C.; Bizari,Douglas R.
A dinâmica de operação dos filtros de areia afeta o desempenho hidráulico do sistema de irrigação, elevando a perda de carga e alterando a altura manométrica total do sistema. Buscando entender parte dessa dinâmica, o objetivo deste trabalho foi determinar o efeito da estrutura interna de filtros de areia na perda de carga de três modelos de equipamentos fabricados no Brasil, sem a presença do elemento filtrante e utilizando água limpa. Adicionalmente, com o ajuste do modelo matemático exponencial aos dados experimentais, procurou-se estabelecer comparações entre os tipos de estrutura dos filtros avaliados. Os ensaios foram realizados em um módulo experimental construído no Laboratório de Hidráulica e Irrigação da FEAGRI/UNICAMP. Os resultados mostraram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação localizada; Placa difusora; Drenos.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100013

Deposição de calda pulverizada na cultura da soja promovida pela aplicação aérea e terrestre
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Farnese,Alberto C.; Olivet,Juan J.; Villalba,Juana.
Este trabalho teve como objetivo avaliar o efeito da tecnologia de aplicação aérea e terrestre de fitossanitários na deposição de calda, na cultura da soja. Avaliou-se, após a aplicação de um traçador, a deposição nas partes inferior e superior do dossel da cultura, por meio de espectrofotometria. O ensaio foi conduzido no delineamento em blocos ao acaso, com quatro repetições e oito tratamentos (formas de aplicação): 1 - Terrestre (Ponta de jato cônico vazio-TXA 8002 e 180 L ha-1); 2 - Terrestre (Ponta de jato plano defletor duplo com indução de ar-AITTJ 11002 e 150 L ha-1); 3 - Terrestre (Ponta de jato plano defletor com indução de ar-TTI 11002 e 150 L ha-1); 4 - Terrestre (Ponta de jato plano defletor duplo-TTJ60 11002 e 150 L ha-1); 5 - Terrestre...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Aviação agrícola; Pulverização; Glycine max.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200014

Irrigation with domestic treated sewage and nitrogen fertilizing in sunflower cultivation
Provedor de dados: 70
Autores: Bezerra,Francicso M. L.; Freitas,Cley A. S. de; Silva,Alexandre R. A. da; Mota,Suetônio de B.; Aquino,Boanerges F. de.
The objective of this study was to evaluate the productive performance of sunflower plants irrigated with different levels of domestic treated sewage and groundwater well with different doses of nitrogen. It was used randomized blocks design in split-split plots with four replications. In the plots, we evaluated the effect of two types of irrigation water, in the subplots we evaluated the five irrigation levels expressed as 25, 50, 75, 100 and 125% of the Class A pan Evaporation (CAE), and in the sub subplots, we evaluated the effect of four different doses of nitrogen (25, 50, 75 and 100 kg ha-1). The irrigation of sunflower with domestic sewage produced greater yield potential of grain and oil. The use of water from treated wastewater can replace up to...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Helianthus annuus; Recycle; Drip irrigation; Nitrogen fertilization.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600014

Análise Energética da cultura do crambe (Crambe abyssinica hochst) produzida em plantio direto
Provedor de dados: 70
Autores: Jasper,Samir P.; Biaggioni,Marco A. M.; Silva,Paulo R. A.; Seki,André S.; Bueno,Osmar C.
O objetivo deste trabalho foi caracterizar o consumo de energia na implantação e condução da cultura do Crambe abyssinica Hochst, em sistema de plantio direto, na Fazenda Experimental Lageado, pertencente à Faculdade de Ciências Agronômicas - UNESP, localizada no município de Botucatu - SP. Avaliando a sustentabilidade do sistema, estimaram-se, a eficiência energética e a cultura do crambe. Para o levantamento dos componentes da estrutura de dispêndios, foram utilizados coeficientes energéticos preconizados em literaturas especializadas. As estruturas de dispêndios energéticos por tipo, fonte e forma demonstraram que a energia indireta participou com 65,03%; as fontes industrial, fóssil e biológica representaram 68,80%, 23,67% e 11,30%, respectivamente....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eficiência energética; Matérias-primas para biodiesel; Biocombustíveis.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300004

Aplicação da alvenaria estrutural em sistemas de armazenamento de produtos agrícolas a granel
Provedor de dados: 70
Autores: Marques Neto,José F. de A; Silva,Maria C. A. T. da.
O armazenamento de produtos agrícolas cumpre um papel importante no agronegócio. Observa-se uma tendência cada vez maior em se trabalhar com produtos a granel, em grandes volumes. Visando a uma concepção construtiva racional e econômica, o presente trabalho propõe um sistema misto em concreto armado e alvenaria estrutural aplicado a silos para armazenagem de produto agrícola a granel. No projeto proposto, o silo é composto de células em alvenaria estrutural, geminadas duas a duas na largura e com um número variável de células no comprimento, em função do volume desejado de armazenagem. Esse sistema simétrico favorece a racionalidade operacional, garantindo a continuidade entre os fluxos de recebimento e de expedição. O fundo da célula é em forma de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Silos; Produto granular; Alvenaria estrutural; Concreto armado; Sistema estrutural.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100020

Avaliação do módulo de elasticidade da madeira com uso de método não-destrutivo de vibração transversal
Provedor de dados: 70
Autores: Targa,Luiz A.; Ballarin,Adriano W.; Biaggioni,Marco A. M.
Numerosas pesquisas têm estudado os métodos não-destrutivos de avaliação de materiais e sua aplicação àqueles de matrizes complexas, como é o caso da madeira. Um dos primeiros métodos não-destrutivos investigados para aplicação nesses casos foi o da vibração transversal. Apesar de sua concepção simples, e a despeito dos grandes avanços obtidos nessa área com outros métodos, como, por exemplo, o ultra-som, o método de vibração transversal para a determinação do módulo de elasticidade da madeira revela-se como de grande potencial de aplicação, sobretudo pela precisão do modelo matemático a ele associado e pela possibilidade de sua aplicação a peças de dimensões estruturais (in-grade testing). Neste trabalho, apresenta-se o uso desse método na determinação do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ensaios não-destrutivos; Vibração transversal; Eucalyptus sp.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200001

Anaerobic biodigestion of manure from finishing pig supplemented with ractopamine over different periods
Provedor de dados: 70
Autores: Santos,Tânia M. B. dos; Trevizan,Paula S. F.; Xavier,Cristiane A. N.; Kiefer,Charles; Ferraz,André L. J.
ABSTRACT This study aimed to evaluate the efficiency of anaerobic digestion and biogas production by manure from pig supplemented with ractopamine over different periods. We used manure of 50 finishing pigs according to the following diets: without supplementation and supplemented with 20-ppm ractopamine during 7, 14, 21, 28 and 35 days pre-slaughter. Continuous bench biodigesters were used in the experiment. We measured biogas production and made analyses of total (TS) and volatile solids (VS), pH, total phosphorus (total P), total nitrogen (total N) and ammoniacal nitrogen (ammoniacal N) in samples of manure, affluent and effluent from biodigesters. The pH and ammoniacal N as indicator parameters of the process balance and stability were satisfactory....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Β-adrenergic; Biogas; Ractopamine hydrochloride; Environmental impact and nutrient partitioning.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300399

Identificação de requisitos de clientes para o projeto de um dosador de precisão para sementes miúdas
Provedor de dados: 70
Autores: Reis,Ângelo V. dos; Forcellini,Fernando A.
A elevação do custo das sementes miúdas torna necessário o desenvolvimento de semeadoras que tenham controle efetivo sobre a população de plantas, o que pode ser conseguido com a utilização de semeadoras de precisão, as quais, no entanto, não são adequadas aos pequenos espaçamentos entre linhas dessas culturas. Por se tratar de um produto novo, há que se prestar especial atenção ao processo de projeto que será utilizado, de forma a incorporar todos os atributos indispensáveis ao cumprimento da tarefa a que se destina, incluindo-se os de ordem funcional, os de qualidade, os comerciais e os de fabricabilidade. Sendo assim, o presente trabalho tem o objetivo de apresentar os requisitos dos clientes para o projeto de um dosador de precisão para sementes...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semeadora de precisão; Metodologia de projeto; Ciclo de vida.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100033

Eficácia de dados Hyperion/EO-1 para identificação de alvos agrícolas: comparação com dados ETM+/Landsat-7
Provedor de dados: 70
Autores: Tisot,Daniela A.; Formaggio,Antonio R.; Rennó,Camilo D.; Galvão,Lênio S.
O objetivo desta pesquisa foi avaliar o uso de dados hiperespectrais Hyperion/EO-1 na discriminação de alvos agrícolas, comparando a acurácia de classificação obtida pelos dados desse sensor à obtida por dados multiespectrais ETM+/Landsat-7. Para isso, alvos agrícolas da região de Franca - SP, com diferenças espectrais bem definidas e outros alvos com diferenças espectrais sutis, imageados por ambos os sensores, em 16 de julho de 2002, foram discriminados utilizando o classificador supervisionado de Máxima Verossimilhança (MaxVer). Os alvos agrícolas com diferenças espectrais bem definidas foram caracterizados por seis classes de uso e cobertura do solo; já os com diferenças espectrais sutis, por cinco classes de variedades de cana-de-açúcar. Quando os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Classificação digital; Dados hiperespectrais; Dados multiespectrais.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300021

Identification of croplands of winter cereals in Rio Grande do Sul state, Brazil, through unsupervised classification of normalized difference vegetation index images
Provedor de dados: 70
Autores: Junges,Amanda H.; Fontana,Denise C.; Pinto,Daniele G.
This study aimed to propose methods to identify croplands cultivated with winter cereals in the northern region of Rio Grande do Sul State, Brazil. Thus, temporal profiles of Normalized Difference Vegetation Index (NDVI) from MODIS sensor, from April to December of the 2000 to 2008, were analyzed. Firstly, crop masks were elaborated by subtracting the minimum NDVI image (April to May) from the maximum NDVI image (June to October). Then, an unsupervised classification of NDVI images was carried out (Isodata), considering the crop mask areas. According to the results, crop masks allowed the identification of pixels with greatest green biomass variation. This variation might be associated or not with winter cereals areas established to grain production. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wheat; Black oat; Remote sensing; MODIS; NDVI.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400027

Evaluation of covering materials in individual shelters and its effects on physiological responses and performance of dairy calves
Provedor de dados: 70
Autores: Fonseca,Patrícia C. de F; Almeida,Eduardo A. de; Passini,Roberta.
In Tropical regions, the animal performance is often affected by climate conditions. This study aimed to evaluate covering materials in individual shelters, normally used to house dairy calves, and its influence on the calves physiology and performance. The design used was completely randomized, with a 2x3 factorial arrangement to compare the averages of 5% through the Tukey's test, i.e., both genders- and three types of covering in the shelters (Z - zinc; AC - asbestos cement; and WPAC - white-painted asbestos cement). Parameters evaluated included daily weight gain (DWG), dry matter intake (DMI), feed conversion (FC), rectal temperature (RT), and respiratory frequency (RF). Results showed significant differences (P &lt; 0.05) among males (1.04kg/day) and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermoregulation; Weight gain; Feed conversion.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600005

Establishment of Xaraés and Marandu grasses under levels of soil compaction
Provedor de dados: 70
Autores: Bonfim-Silva,Edna M.; Valadão Júnior,Daniel D.; Reis,Rafael H. P. dos; Campos,Jader J.; Scaramuzza,Walcylene L. M. P.
In Cerrado soils under grazing, changes occur in physical attributes, such as increased density, decreasing on the size of water stable aggregates, and macroporosity reduction. Thus, the aim of this study was to study the effect of compaction on the establishment of two forages. It was adopted a completely randomized design with three replications, in 2 x 4 factorial design, and two forages (Xaraés grass and Marandu grass), and four levels of compaction (soil densities of 1.0, 1.2, 1.4, and 1.6 Mg m-3). The following variables were evaluated 48 days after sowing: tiller population, plant height, dry matter production of shoots and components, leaf and stem, as well as the root dry mass. The stem dry mass decreased with soil density in a similar manner for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brachiaria brizantha; Soil density; Forage; Tillering.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400012

Disponibilidade de micronutrientes em cinco solos em função do tempo de incubação de um composto de lixo
Provedor de dados: 70
Autores: Silva,Fábio C. da; Silva,Carlos A.; Bergamasco,Alessandra F.; Ramalho,André L.
O uso agrícola do composto de lixo (CL) nas lavouras constitui a alternativa econômica e ambiental viável, por ser fonte de nutrientes e matéria orgânica. Este estudo foi conduzido em casa de vegetação e teve o objetivo de avaliar a disponibilidade temporal de micronutrientes (Cu, Fe, Mn e Zn) por Mehlich-1, em cinco solos (Latossolo Vermelho-Amarelo distrófico: LVd; Argissolo Vermelho-Amarelo distrófico: PVd; Chernossolo Haplico Órtico: MXo; Planossolo Hidromórfico distrófico: SGd, e Nitossolo Vermelho Eutroférrico: Nvef) incubados com diferentes doses de CL (0; 25; 50 e 100 Mg ha-1), em períodos de incubação (0; 16; 32; 64 e 150 dias). A maioria dos metais pesados teve sua disponibilidade reduzida nos primeiros períodos de incubação, sendo esse efeito...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resíduo sólido urbano; Matéria orgânica; Metais pesados.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100025

OPTIMIZATION MODEL FOR VEHICLE ROUTING AND EQUIPMENT REPLACEMENT IN FARM MACHINERY
Provedor de dados: 70
Autores: Grano,Carolina; Abensur,Eder.
ABSTRACT: An equipment replacement decision takes into account economic engineering models based on discounted cash flow (DCF) such as the Annual Equivalent Cost (AEC). Despite a large number of researches on industrial assets replacement, there is a lack of studies applied to farm goods. This study aimed at assessing an alternative model for economic decision analysis on farm machinery replacement, with no restrictions on the number of replacements and assessed goods during a defined timeline. The results of the hybrid model based on the combination of the vehicle routing problem and the equipment replacement problem (RVPSE) applied to three different farm tractors showed the model reliability, providing a wider range of decisions for management support.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Economic engineering; Annual equivalent cost; Integer linear programming.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500987

Avaliação dos índices de conforto térmico, parâmetros fisiológicos e gradiente térmico de ovinos nativos
Provedor de dados: 70
Autores: Ribeiro,Neyla L.; Furtado,Dermeval A.; Medeiros,Ariosvaldo N.; Ribeiro,Maria N.; Silva,Regina C. B.; Souza,Cicilia M. S.
Esta pesquisa teve o objetivo de determinar os índices de conforto térmico em instalações para ovinos, analisar os parâmetros fisiológicos e o gradiente térmico de quatro grupos genéticos, na região semiárida paraibana. Foram utilizados 40 animais, dez por grupo genético, que foram: Cariri, Morada Nova, Barriga Negra e Cara Curta, todas fêmeas, alojadas aleatoriamente em quatro apriscos. Os índices ambientais dentro das instalações, principalmente das 11 às 15 h, ficaram acima da zona de conforto térmico para ovinos adultos, com exceção da umidade relativa do ar, que ficou com média diária de 67,5%. A temperatura retal dos animais esteve dentro da faixa normal, sendo o grupo genético Morada Nova o que apresentou menor valor (38,6 ºC). A frequência...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência; Conforto térmico; Animais nativos.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400001

Eficiência da estabilização do solo e qualidade de tijolos prensados de terra crua tratada com aditivos químicos, avaliadas pela combinação de testes destrutivos e não-destrutivos
Provedor de dados: 70
Autores: Ferreira,Régis de C.; Freire,Wesley J.
A qualidade de tijolos prensados de terra crua tratada quimicamente é influenciada basicamente pelo tipo de solo, adições químicas e período de cura. O presente trabalho teve como objetivo estudar a combinação de métodos destrutivos e não-destrutivos associados à análise estatística, para a avaliação da qualidade e da eficiência da estabilização de tijolos prensados de terra crua tratada com cimento, cal e silicato de sódio. Os teores de cimento e cal foram 0; 6 e 10%, e a dose de silicato de sódio foi de 4% em relação ao peso seco da mistura solo-aditivo. Após a sua moldagem, os tijolos foram submetidos à cura durante os períodos de 7; 28; 56 e 91 dias. As propriedades físico-mecânicas dos tijolos foram determinadas por meio de testes destrutivos, tais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tijolos de terra crua; Propriedades mecânicas; Material de construção.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300003

ENERGY BALANCE OF IRRIGATED AND RAINFED SORGHUM PRODUCTION
Provedor de dados: 70
Autores: Jordan,Rodrigo A.; Almeida,Alexsandro C. S.; Queiroz,Marcos V. B. M.; Gomes,Eder P.; Rezende,Rodrigo K. S.
ABSTRACT: The objective of this study was to evaluate the yield and energy balance of four sorghum genotypes in irrigated and rainfed crops. The experiment was conducted in an irrigation and drainage unit at the Federal University of Grande Dourados (UFGD), in Dourados, Mato Grosso do Sul state (Brazil). The experimental design was a randomized complete block design with split plots (with and without irrigation), testing four genotypes (BRS 506, CV 007, CV 147, and EJ 7281) with four replicates (32 plots). Irrigation provided yield increase in all four genotypes. The respective yield increases were 85.89%, 71.82%, 64.28%, and 63.36% for genotypes EJ 7281, BRS 506, CV 147, and CV 007. The energy efficiency (produced/ used ratio) was on average 3.5 under...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Productivity; Off-season; Ethanol.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500907

White mold detection in common beans through leaf reflectance spectroscopy
Provedor de dados: 70
Autores: Machado,Marley L.; Pinto,Francisco de A. C.; Paula Junior,Trazilbo J. de; Queiroz,Daniel M. de; Cerqueira,Ozires de A. T.
ABSTRACT This study aimed to identify wavelengths based on leaf reflectance (400-1050 nm) to estimate white mold severity in common beans at different seasons. Two experiments were carried out, one during fall and another in winter. Partial Least Squares (PLS) regression was used to establish a set of wavelengths that better estimates the disease severity at a specific date. Therefore, observations were previously divided in two sub-groups. The first one (calibration) was used for model building and the second subgroup for model testing. Error measurements and correlation between measured and predicted values of disease severity index were employed to provide the best wavelengths in both seasons. The average indexes of each experiment were of 5.8% and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sclerotinia sclerotiorum; PLS regression; Pigments; Spectrum; Absorption.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601117

Modeling and correction of soil penetration resistance for variations in soil moisture and soil bulk density
Provedor de dados: 70
Autores: Silva,Wininton M. da; Bianchini,Aloísio; Cunha,Cesar A. da.
ABSTRACT This study aimed to describe the behavior of models for adjusting data of soil penetration resistance for variations in soil moisture and soil bulk density. The study was carried out in Lucas do Rio Verde, MT, Brazil in a typic dystrophic red-yellow Latosol (Oxisol) containing 0.366 kg kg−1 of clay. Soil penetration resistance measurements were conducted in the soil moistures of 0.33 kg kg−1, 0.28 kg kg−1, 0.25 kg kg−1 and 0.22 kg kg−1. Soil penetration resistance behavior due to variations in soil moisture and soil bulk density was assessed by estimating the soil resistance values by non-linear models. There was an increase of the soil penetration resistance values as soil was losing moisture. For the same edaphic condition studied, small...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Pedotransfer functions; Cone index.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300449

Coverage mobilization by different no-tillage in-line handling mechanisms
Provedor de dados: 70
Autores: BRANDELERO,EVANDRO M.; ARAÚJO,AUGUSTO G. DE; RALISCH,RICARDO.
Vegetation cover on soil acts positively in maintaining temperature and soil moisture, yet, it has been imposing specific operational conditions on seeders. The objective of this study was to evaluate performance of different mechanisms regarding straw mobilization, employed in a no-till seeder. The experimental area was conducted on clayey soil under no-tillage with a large quantity of sorghum residue. The experiment was established in a randomized block design, as the treatments consisted of a combination of two mechanisms at front of the furrow opener composed of cutting disc and row cleaners, and three mechanisms behind the seed furrower, covering discs prototype model M1, Spider and commercial model, with the combination of cutting disc and Spider...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays; Seeder; Furrowers.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100089

VEGETATIVE DEVELOPMENT AND GROWING DEGREE-DAYS OF TROPICAL AND WINTER FORAGES
Provedor de dados: 70
Autores: Sanches,Arthur C.; Souza,Débora P. de; Jesus,Fernanda L. F. de; Mendonça,Fernando C.; Gomes,Eder P.
ABSTRACT One of the limitations to producing irrigated forages is setting suitable biometric parameters to establish the entrance of animals to grazing areas. Such parameters can be measured or even estimated. Estimates are advantageous for being practical and able to be used for grazing optimization. This study aimed to evaluate the correlation among growing degree-days (GDD), canopy height (CH), leaf area index (LAI), and number of cycle days (NCD) of Guinea grass (Panicum maximum cv. Mombaça) and Bermuda grass (Cynodon spp. Tifton 85) single cropped for one year and overseeded with black oat and ryegrass in the autumn-winter season. The study was carried out from February 2016 to February 2017, and forage crops were sprinkle irrigated. LAI and CH were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Lolium multiflorum; Avena strigosa; Base temperature; Grass.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200191

CHEMICAL AND ENERGETIC CHARACTERISTICS OF AFRICAN SWEET SORGHUM AS A SOURCE OF BIOENERGY
Provedor de dados: 70
Autores: Caraschi,José C.; Viana,Ronaldo da S.; Moreira,Bruno R. de A.; Prates,Glaucia A.
ABSTRACT The aim of this study was to evaluate the energetic potential achieved by the application of phyto-regulators to sweet sorghum cultivars. A randomized complete block design was used. Experiments were conducted using two sweet sorghum cultivars (BRS 508 and BRS 509), fourphyto-regulators (ethephon, ethyl-trinexapac, glyphosate, and sulfometuron-methyl), and a control; four replicates were performed 70 days after sowing, at the beginning of the flowering phase of the plants, with the aid of a CO2-pressurized coastal sprayer. The plants were harvested after 40 days, with the stems being cleared at the height of the apical bud, and were subjected to grinding for the extraction of broth. The following analyses were carried out: chemical (total...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Green Energy; Bioenergy; Biofuel; Renewable energy.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400426

Data mining techniques for identification of spectrally homogeneous areas using NDVI temporal profiles of soybean crop
Provedor de dados: 70
Autores: Johann,Jerry A.; Rocha,Jansle V.; Oliveira,Stanley R. de M.; Rodrigues,Luiz H. A.; Lamparelli,Rubens A. C.
The aim of this study was to group temporal profiles of 10-day composites NDVI product by similarity, which was obtained by the SPOT Vegetation sensor, for municipalities with high soybean production in the state of Paraná, Brazil, in the 2005/2006 cropping season. Data mining is a valuable tool that allows extracting knowledge from a database, identifying valid, new, potentially useful and understandable patterns. Therefore, it was used the methods for clusters generation by means of the algorithms K-Means, MAXVER and DBSCAN, implemented in the WEKA software package. Clusters were created based on the average temporal profiles of NDVI of the 277 municipalities with high soybean production in the state and the best results were found with the K-Means...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Annual crop; MODIS; SPOT Vegetation; MAXVER; K-Means.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300008

PHYSIOLOGICAL RESPONSES OF COFFEE TREE UNDER DIFFERENT IRRIGATION LEVELS
Provedor de dados: 70
Autores: Costa,Jéfferson de O.; Coelho,Rubens D.; Barros,Timóteo H. da S.; Fraga Júnior,Eusímio F.; Fernandes,André L. T.
ABSTRACT The plant water potential and the leaf temperature are physiological responses of the coffee tree that can be used as indicative of the irrigation management of this crop. There is a dependence between the leaf water potential with the potential matrix of the soil solution, however, the water potential levels found for the coffee tree show divergent relationships in the literature regarding the matrix potential. The objective of this study is to verify the water potential and leaf surface temperature in the coffee tree when submitted to different irrigation levels. The study was conducted in Piracicaba, SP, Brazil, using Coffea arabica species from Red Catuaí IAC 144 variety, the drip irrigation system was adopted and the management done by...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica; Leaf temperature; Water potential.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500648

MECHANIZED AND INDIVIDUALIZED APPLICATION OF N-P-K IN COMBINED OPERATIONS IN SUGARCANE
Provedor de dados: 70
Autores: Carneiro,Franciele M.; Furlani,Carlos E. A.; Gírio,Lucas A. da S.; Silva,Rouverson P. da; Malheiros,Euclides B.
ABSTRACT: A new concept of fertilizer machine is under development and shows as differential individually fertilizer application, that is sources of N, P and K are applied separately for the purpose of improving the distribution efficiency of the quantities applied. The aim was to compare the quality of the individualized mechanized distribution of N, P and K in combined operations with and without herbicide application, as well as to evaluate the fertilizer application on each side of the fertilizer machine. The experiment was carried out on Cascavel farm, in the municipality of MatãoSP. The experimental design was established according to the criteria of quality control, and variables monitoring carried out in the place during fertilization operation,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Statistical process control; Fertilizer; Operational quality; Fertilizer machine.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400676

Impact of irrigation on yield and energy balance of the production of oil and cake of two sunflower varieties
Provedor de dados: 70
Autores: Jordan,Rodrigo A.; Gomes,Eder P.; Biscaro,Guilherme A.
The energy balance for the production of sunflower oil and cake was carried out during the agricultural and industrial stage phase, where it was considered a cold extraction by hydraulic pressing, with the plant location in a rural area with a radius of 30km range. Data on productivity was used in two varieties of sunflower (Helio 358 and Aguará 04) grown in different seasons (2007/2008, 2008/2009), under different irrigation levels. Data showed that irrigation resulted in an increase in productivity of both varieties, and the best response was observed for Aguará 04 variety. Moreover, the increased intensity of irrigation negatively affected the energy balance, reducing the ratio between energy produced and energy used in the production chain. The most...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bioenergy; Sunflower; Irrigation; Energy balance.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600006

Identification of acoustic parameters for broiler welfare estimate
Provedor de dados: 70
Autores: Pereira,Erica M.; Nääs,Irenilza de A.; Garcia,Rodrigo G.
Estimates of broiler welfare have subjective character. Nowadays, researchers seek non-invasive features or indicators that may describe this condition in animal production. The aim of this study was to identify acoustic parameters to estimate broiler welfare using the following five vocalization acoustic parameters: energy, spectral centroid, bandwidth, first formant, and second formant. The database that generated the model was obtained from a field experiment with 432 broilers, which half were Cobb® and half, Ross® breed, from day 21 to 42, containing bird vocalizations under either welfare or stress conditions. The results of the experiment generated responses to the tested conditions of gender, genetic strain, and welfare. The proposed model was based...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Signal analysis; Broiler production; Algorithm.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300004

Erosion factors and magnetic susceptibility in differet compartments of a slope in Gilbués-PI, Brazil
Provedor de dados: 70
Autores: Santos,Hélio L.; Marques Júnior,José; Matias,Sammy S. R.; Siqueira,Diego S.; Martins Filho,Marcílio V.
The erosion is the degradation of soil with effects on crop productivity and pollution of the environment. To understand the spatial variability of this phenomenon, geostatistical techniques and concepts of soil-landscape can be used to identify landscape compartments with different potential of erosion. The aim of this study was to understand the factors of erosion in landscape compartments and the relations with the magnetic susceptibility (MS) of the soils in a slope in Gilbués, state of Piauí (PI), Brazil. Sampling meshes were set in compartments I and II with 121 points and in compartment III with 99 points spaced every 10 meters. There was significant difference to erodibility (K) and risk of erosion (RE); the spatial variability of MS was lower than...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Indirect quantification; Geostatistics; Conservation planning; Compartments; Topography; Relief; Landscape.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100008

Systems of aerial spraying for soybean rust control
Provedor de dados: 70
Autores: Antuniassi,Ulisses R.; Velini,Edivaldo D.; Oliveira,Rone B. de; Peres-Oliveira,Maria A.; Figueiredo,Zulema N.
The soybean rust caused by Phakopsora pachyrhizi is considered the main soybean disease and consequently the appropriate selection and the use of spraying equipment are vital for its control. The aim of this study was to evaluate the performance of aerial application equipment for soybean rust control. It was used: Micronair AU 5000 at 10 L ha-1 (with oil) and at 20 L ha-1 (without oil); Stol ARD atomizer at 10 and 20 L ha-1 (both with oil) and Spectrum (electrostatic) at 10 L ha-1 (without oil). The adjuvant was cotton oil (1.0 L ha-1) with emulsifier (BR 455) at 0.025 L ha-1. The field trial was set up at the 3rd fungicide application, when f four replications of each treatment. There were no statistical differences among treatments related to fungicide...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application equipments; Agricultural aviation; Fungicides deposits; Phakopsora pachyrhizi.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400008

Determination of physical properties of crambe fruits during drying
Provedor de dados: 70
Autores: Gonçalves,Douglas N.; Resende,Osvaldo; Costa,Lílian M.; Prado,Mariana C.
The Knowledge of the physical properties of agricultural products has great importance for the construction and operation of equipment for drying and storage, to achieve increased efficiency in post-harvest operations. The aim was to determine and analyze the physical properties of crambe fruits during drying at different temperatures. Crambe fruits with an initial moisture content of 0.36 (decimal d.b.) which was reduced by drying at 37.0; 58.8 and 83.5 ºC and relative humidity of 29.4; 11.2 and 3.2%, respectively, to 0.09 ± 1 (decimal d.b.). At different levels of moisture contents (0.36; 0.31; 0.26; 0.21; 0.17; 0.13 and 0.09 decimal d.b.), was evaluated the intergranular porosity, the bulk density, the true density as well as the volumetric shrinkage...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Crambe abyssinica; Moisture content; Dries temperatures.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500016

Aplicação de túnel de vento na avaliação de linhas de fluxo geradas por crepinas de filtros de areia
Provedor de dados: 70
Autores: Santos,Marcelo B. dos; Mesquita,Marcio; Testezlaf,Roberto.
Visando à obtenção de informações técnicas que auxiliem aprimorar a eficiência hidráulica de filtros de areia nos processos de filtragem e retrolavagem, buscou-se avaliar o potencial de utilização de uma bancada didática de túnel de vento como método de visualização e caracterização das linhas de fluxo geradas pela interação da geometria de um modelo de dreno (crepina) com diferentes velocidades de escoamento. Os ensaios foram realizados, instalando-se um modelo comercial de dreno, do tipo cilíndrico, em um módulo experimental construído para ser acoplado a um túnel de vento vertical. Simularam-se as três vazões de escoamento de ar fornecidas pelo módulo, obtendo-se registros fotográficos com uma câmara de alta velocidade, cujas imagens foram tratadas para...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação localizada; Filtração; Retrolavagem.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300011

PERTINENCE CURVES IN FUZZY MODELING OF THE PRODUCTIVE RESPONSES OF BROILERS
Provedor de dados: 70
Autores: Lourençoni,Dian; Abreu,Paulo G. de; Yanagi Junior,Tadayuki; Campos,Alessandro T.; Yanagi,Silvia de N. M.
ABSTRACT The selection of the type of fuzzy systems pertinence curve allows a better representation of the mathematical model and a smaller simulation error. We aimed to study the effect of pertinence curves in fuzzy modeling of broiler performance, created in different production systems. For the development and testing of fuzzy models, three commercial aviaries (conventional, tunnel with negative pressure, and dark house) were evaluated over one year, totaling six lots per system. For the development of the model, the input variables were enthalpy in each rearing phase (initial: phases 1, 2, and 3; growth: phase 4; and final: phase 5) and the output variables were feed intake (FE), weight gain (GP), feed conversion (FE), and the productive efficiency...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry farming; Production performance; Artificial intelligence; Fuzzy logic.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300265

Modelagem de um sistema de informação para rastreabilidade na indústria do vinho baseado em uma arquitetura orientada a serviços
Provedor de dados: 70
Autores: Gogliano Sobrinho,Osvaldo; Cugnasca,Carlos E.; Fialho,Flavio B.; Guerra,Celito C.
Apresenta-se neste trabalho pesquisa científica que levou à modelagem de um sistema de informação para o registro de dados de rastreabilidade destinado à indústria do vinho, segundo os conceitos de uma arquitetura computacional orientada a serviços (service oriented architecture, SOA). Desde 2005, a manutenção de tais registros é obrigatória para todos os produtores que pretendem exportar para países da União Europeia. Ademais, os consumidores finais, inclusive brasileiros, preocupados com a segurança alimentar, apresentam demanda crescente por informações. Buscou-se uma solução que contemple a indústria coletivamente, por meio de consórcios ou associações de produtores, diluindo custos e compartilhando benefícios. A partir do levantamento bibliográfico...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Segurança alimentar; Tecnologia da informação; Internet; Web services; UML.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100011

EVALUATION OF SELF COMPENSATING EMITTERS IRRIGATING WITH SALINE WATER: PART II: PROCESS CAPABILITY INDEX
Provedor de dados: 70
Autores: Silva,Patrícia F. Da; Dantas Neto,José; Lima,VERA L. A. DE; Santos,Delfran B. Dos; Ribeiro,Pedro H. P.
ABSTRACT The use of tools such as process capability index for irrigation aims to observe how this irrigation is adequate in terms of quality. The aim of the study was analyzing the Christiansen uniformity coefficient and the flow of a drip irrigation system with self-compensating emitters under water different salt concentrations, using the process capability index. The research was conducted in a greenhouse at the Federal University of Campina Grande (UFCG). The experimental design was a randomized block in a factorial 5 x 2 with three replications, the factors consisted of five levels of irrigation water salinity (CEw) (0.6, 1.5, 2.5, 3.5 and 4.5 dS m−1 at 25°C) and two running times (0 and 350 hours of operation). The Christiansen uniformity...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Quality engineering; Flow; Quality control; Christiansen uniformity.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601086

Alterações físicas e microbiológicas durante a compostagem dos dejetos de cabras
Provedor de dados: 70
Autores: Orrico,Ana C. A.; Lucas Júnior,Jorge de; Orrico Júnior,Marco A. P.
Avaliaram-se as reduções de massa seca enleirada, volume ocupado pelas leiras e coliformes durante a compostagem dos dejetos gerados por cabras Saanen e F1 (Saanen x Boer), alimentadas com três dietas (dieta 1 = 80% volumoso (V) e 20% concentrado (C); dieta 2 = 60% V e 40% C, e dieta 3 = 40% V e 60% C). As maiores reduções (P&lt;0,05) nas quantidades de massa seca ocorreram em leiras formadas com os dejetos gerados por cabras alimentadas com a dieta 3 (56,2%), em relação aos dejetos gerados quando consumiram as dietas 2 (44,5%) e 1 (40,6%). A maior média da temperatura semanal ocorreu na primeira semana, em leiras formadas a partir dos dejetos de cabras que consumiram a dieta 3. As leiras preparadas com dejetos produzidos por cabras alimentadas com a dieta...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Leiras; Patógenos; Reciclagem.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400020

Dessecação da aveia-preta (Avena strigosa Schreb) com herbicida de contato, em presença ou não de assistência de ar junto à barra do pulverizador, em diferentes volumes de calda
Provedor de dados: 70
Autores: Garcia,Luiz C.; Raetano,Carlos G.; Justino,Altair; Puríssimo,Cláudio.
A tecnologia de aplicação dos produtos fitossanitários na agricultura pode ser aprimorada mediante a redução dos desperdícios. Com o objetivo de contribuir com tal avanço tecnológico, avaliou-se a eficácia de um herbicida com ação de contato, aplicado em pós-emergência com pulverizadores sem e com assistência de ar junto à barra, em diferentes volumes de calda. O experimento foi instalado no município de Ponta Grossa - PR, com a dessecação de aveia-preta (Avena strigosa Schreb) implantada em sistema de plantio direto sob a palha. Empregou-se a mistura herbicida formulada (SC) de dicloreto de paraquate (400 g ha-1) + diuron (200 g ha-1). O delineamento experimental utilizado foi o de blocos casualizados (DBC), em esquema fatorial 2 (pulverizador sem e com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantio direto; Tecnologia de aplicação; Volume de calda.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300029

System for studies of control strategies applied in the refrigerated chambers
Provedor de dados: 70
Autores: Tizzei,Alexandre; Meneghetti,Carlos R.; Cappelli,Nelson L.; Umezu,Claudio K.
The process of cold storage chambers contributes largely to the quality and longevity of stored products. In recent years, it has been intensified the study of control strategies in order to decrease the temperature change inside the storage chamber and to reduce the electric power consumption. This study has developed a system for data acquisition and process control, in LabVIEW language, to be applied in the cooling system of a refrigerating chamber of 30m³. The use of instrumentation and the application developed fostered the development of scientific experiments, which aimed to study the dynamic behavior of the refrigeration system, compare the performance of control strategies and the heat engine, even due to the controlled temperature, or to the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy-saving; PID controller; Fuzzy controller; Cold storage.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500004

Efeito da água disponível do solo no desenvolvimento de dois cultivares de mamona, nos primeiro e segundo ciclos
Provedor de dados: 70
Autores: Formiga,Leoberto de A.; Guerra,Hugo O. C.; Lacerda,Rogério D. de; Silva,José E. Barbosa da; Araujo,Mario S.
A mamoneira é uma oleaginosa de relevante importância econômica e social, de grande relevância para a economia da região Nordeste, por fixar mão de obra, evitando a evasão de divisas. Foram estudados diferentes aspectos do manejo da cultura da mamona, visando à otimização do uso da água e do rendimento da mamona, no primeiro e segundo ciclos de produção, sendo este último obtido após uma drástica poda da planta no final do primeiro ciclo. A pesquisa foi desenvolvida no campo em Lagoa Seca-PB. O delineamento experimental foi o de blocos ao acaso, em esquema fatorial 2 x 4, constituído com duas cultivares de mamona (BRS 149 - Nordestina e o BRS 188 - Paraguaçu) e quatro níveis de água disponível no solo (40; 60; 80 e 100%), distribuídos em três blocos. Os...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Manejo de poda; Manejo da irrigação; Ricinus communis L.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600009

TRACTIVE DEMAND, SOIL MOBILIZATION PARAMETERS, AND CORN YIELD IN COMPACTED OXISOL
Provedor de dados: 70
Autores: Müller,Jônatan; Modolo,Alcir J.; Trentin,Robson G.; Campos,José R. da R.; Baesso,Murilo M.
ABSTRACT Direct seeding systems are characterized by soil disturbance only occurring in the sowing line and the maintenance of the remaining area is achieved by covering with crop residues. Without total area soil mobilization as recommended by the no-tillage system, associated with the increase in the degree of soil compaction caused by the traffic of agricultural machinery, there can be a decrease in crop productivity. This study aimed to evaluate machine parameters, soil mobilization, and corn yield as a function of different furrow opener working depths (0.065, 0.095, 0.125, and 0.150 m) and evaluate the direct seeding of winter ground cover plants (black oat or forage turnip) in compacted Oxisol. The experiment was arranged in strips, in a randomized...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Direct seeding; Ground cover plants; Shank working depth.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100089

Desempenho de uma semeadora-adubadora direta, em função da velocidade de eslocamento e do tipo de manejo da biomassa da cultura de cobertura do solo
Provedor de dados: 70
Autores: Branquinho,Klinger B.; Furlani,Carlos E. A.; Lopes,Afonso; Silva,Rouverson P. da; Grotta,Danilo C.C.; Borsatto,Edinan A.
O objetivo do presente trabalho foi estudar o desempenho de uma semeadora-adubadora, operando em duas velocidades sobre a palhada da cultura do milheto (Pennisetum glaucum (L.) R. Brown), após diferentes manejos, na semeadura direta da cultura da soja (Glycine Max L.). O experimento foi realizado com seis tratamentos, em esquema fatorial, delineados em blocos ao acaso, com quatro repetições. Os tratamentos combinaram três manejos (triturador de palhas tratorizado, rolo- faca e herbicida) com duas velocidades de deslocamento da semeadora-adubadora (5,2 e 7,3 km h-1). Foram analisadas as seguintes variáveis: acúmulo e decomposição de massa seca do milheto, índice de emergência da cultura da soja, uniformidade de distribuição longitudinal de sementes,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Distribuição longitudinal; Velocidade de decomposição; Plantio direto.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200016

Concentração de cátions presentes no lixiviado de solos tratados com vinhaça
Provedor de dados: 70
Autores: Brito,Fábio L.; Rolim,Mário M.; Pedrosa,Elvira M. R.
O presente estudo teve como objetivo avaliar a qualidade do lixiviado de solos que receberam doses de vinhaça em diferentes tempos de incubação. Para isso, em 27 colunas de PVC de 20 x 110 cm (diâmetro x altura), foram reproduzidos três solos classificados como Nitossolo Háplico, Argissolo Amarelo e Espodossolo Cárbico, com horizontes, espessuras e densidades semelhantes à original. Os solos foram tratados com vinhaça em doses equivalentes a 0 (testemunha), 350 e 700 m³ ha-1 e submetidos aos tempos de incubação de 30 e 60 dias. Nos efluentes coletados, foi realizada análise de K, Ca, Mg e Na, e os dados obtidos, submetidos à análise multivariada, a 5% de probabilidade. Os resultados indicaram efeito significativo para as variáveis K, Ca, Mg e Na com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resíduo; Elementos químicos; Percolado.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400021

Influência da suspensão na segurança e no conforto de um pulverizador autopropelido
Provedor de dados: 70
Autores: Ferreira,André L.; Balthazar,José M.; Pontes Júnior,Bento R.
Para avaliar o comportamento da suspensão do pulverizador autopropelido, foram desenvolvidos modelos físicos e matemáticos em função da excitação ocasionada pelas irregularidades do solo. Neste trabalho, estas irregularidades são representadas por obstáculos de uma pista normalizada segundo a norma ISO 5008. As equações do movimento são obtidas a partir dos modelos matemáticos de meio veículo. As simulações numéricas são executadas nos softwares Matlab® e Simulink®. A partir da entrada conhecida, podem-se determinar as características dos elementos da suspensão para obter níveis desejáveis de conforto e segurança. Foram analisadas quatro diferentes configurações do sistema, variando-se a relação de rigidez a partir de um modelo considerado padrão....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Suspensão passiva; Veículos agrícolas; Simulações numéricas.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400019

Manejo da irrigação associada a coberturas mortas vegetais no cultivo orgânico da beterraba
Provedor de dados: 70
Autores: Carvalho,Daniel F. de; Oliveira Neto,Dionizio H. de; Ribeiro,Raul de L. D.; Guerra,José G. M.; Rouws,Janaína R. C.
Práticas agrícolas orgânicas, como a cobertura do solo com palha, foram testadas em área irrigada por gotejamento na Baixada Fluminense, no Estado do Rio de Janeiro. O cultivo de inverno da beterraba nesta região é favorecido por temperaturas mais amenas, coincidindo com a época de maior disponibilidade do produto no Estado. No cultivo da beterraba, foram adotados três tipos de cobertura do solo e seis lâminas de irrigação (0; 29; 48; 78; 100 e 148% da ETc) determinadas com base no balanço de água no solo utilizando a técnica da TDR. O delineamento estatístico adotado foi blocos casualizados, com seis tratamentos e quatro repetições. Sob cobertura morta de Pennisetum purpureum, de Gliricidia sepium e na ausência de cobertura morta, os valores máximos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Beta vulgaris; Gliricidia sepium; Pennisetum purpureum; Olericultura orgânica; Gotejamento; TDR.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200007

DELIMITATION OF HOMOGENEOUS ZONES IN VINEYARDS USING GEOSTATISTICS AND MULTIVARIATE ANALYSIS OF DIFFERENT VEGETATION INDICES
Provedor de dados: 70
Autores: Costa,Bruno R. S.; Oldoni,Henrique; Rocha Junior,Romero C.; Bassoi,Luís H.
ABSTRACT Vegetation indices (VIs) are quantitative measures used to describe the distribution and spatial variability of the vegetation cover of natural or cultivated areas. The aim of this study was to delimit homogeneous zones (HZs) of different VIs using geostatistics and multivariate analysis in order to identify vegetation patterns in Cabernet Franc and Cabernet Sauvignon vineyards. The evaluation was performed in two vineyards in the municipality of Espírito Santo do Pinhal in the state of São Paulo, Brazil. Reflectance (ρ) was measured at three wavelengths of the electromagnetic spectrum (670, 730, and 780 nm) at canopy height in georeferenced points along planting rows using the Crop Circle ACS-430 active sensor. Nine VIs were calculated based on...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vitis vinifera L.; Canopy density; Agricultural instrumentation.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800013

RESIDUE ANALYSIS OF ORGANOCHLORINE AND ORGANOPHOSPHORUS PESTICIDES IN URBAN LAKE SEDIMENTS
Provedor de dados: 70
Autores: Cembranel,Adir S.; Frigo,Elisandro P.; Sampaio,Silvio C.; Mercante,Erivelto; Reis,Ralpho R. Dos; Remor,Marcelo B.
ABSTRACT The knowledge of pesticide residual concentrations in the environment is important to understand the threats to the environment and human health, especially when natural resources are used for human consumption. In this context, this study aimed to assess the potential ecological risk and respective sources of sediment contamination by organochlorine and organophosphorus pesticides. The study site was an urban lake located in Cascavel city, western Paraná state, Brazil, where the history of land use and occupation in the urban environment is typically agricultural. Surface sediment samples were collected every three months from April 2010 to June 2013 at five different collection points, totaling 65 samples. Analyses showed that contamination by...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agrochemicals; Ecological risk; Land use and occupation.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601254

EFFECT OF THE POSTHARVEST PROCESSING METHOD ON THE BIOCHEMICAL COMPOSITION AND SENSORY ANALYSIS OF ARABICA COFFEE
Provedor de dados: 70
Autores: Rodriguez,Yeison F. B.; Guzman,Nelson G.; Hernandez,Joel G.
ABSTRACT The objective of this work was to study the influence of two postharvest processing methods on the biochemical composition and sensory analysis of a Colombian specialty coffee. For this purpose, coffee beans (Coffea arabica) of the Castillo variety were collected and processed using the wet and semi-dry methods, and the drying process was conducted in a sun drier prototype with a plastic parabolic cover, with a maximum drying air temperature of 50 °C; green coffee beans were managed according to the official Specialty Coffee Association cupping protocol and roasted to a medium and dark degree. Physicochemical determinations (pH, color, titratable acidity, caffeine content, and chlorogenic acid quantification) in green coffee and roasted coffee...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Caffeine; Coffee roasting; Coffee processing; Cup quality; Chlorogenic acids.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200177

Modelagem computacional do fluxo unidimensional de água em meio não saturado do solo
Provedor de dados: 70
Autores: Wendland,Edson; Pizarro,Maria de L. P.
O estudo do fluxo de água em zonas não saturadas do solo é de grande importância para pesquisas relacionadas à disponibilidade hídrica para o desenvolvimento das plantas. Devido ao alto custo, ao tempo demandado e ao esforço humano nas investigações de campo, os modelos matemáticos, aliados às técnicas numéricas e avanços computacionais, constituem-se em uma ferramenta importante na previsão desses estudos. No presente trabalho, objetivou-se solucionar a equação diferencial parcial não linear de Richards mediante a aplicação do Método de Elementos Finitos. Na aproximação espacial, foi empregada a adaptatividade com refinamento "h" na malha de elementos finitos e, na derivada temporal, foi aplicado o esquema de Euler Explícito. A função interpolação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zona não saturada; Equação de Richards; Método de elementos finitos.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300007

Regulated deficit irrigation and tommy atkins mango orchard productivity under microsprinkling in brazilian semi arid
Provedor de dados: 70
Autores: Cotrim,Carlos E; Coelho Filho,Maurício A; Coelho,Eugênio F; Ramos,Márcio M; Cecon,Paulo R.
This study aimed to test controlled levels of water deficiency in soil in mango trees, under microsprinkling irrigation, in semi-arid conditions, and to evaluate its effect in the productivity and fruits quality. The deficits were applied in the phases I, II and III of growth of the fruit, during the productive cycles of the mango tree in 2006 and 2007. The experiment in both cases was arranged in an entirely random design with 10 treatments and 3 repetitions, in the year I, and with 8 treatments and 3 repetitions in the year II. The values of soil water potential, of the treatments submitted to regulated deficit irrigation (RDI), were placed in the range of 0 to -0.011 MPa, showing that the soil humidity varied between the saturation and the field...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mango; Irrigation management; Water use optimization.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600003

Monitoramento de variáveis de qualidade da água do Horto Ouro Verde - Conchal - SP
Provedor de dados: 70
Autores: Bueno,Lara F.; Galbiatti,João A.; Borges,Maurício J.
O presente trabalho foi desenvolvido em área do Horto Ouro Verde, de propriedade da International Paper do Brasil, localizado no município de Conchal - SP, tendo por objetivo monitorar algumas variáveis de qualidade da água em duas condições do uso do solo (mata nativa e eucalipto). Para tanto, coletou-se água mensalmente em seis pontos ao longo do curso d'água, de maneira representativa dos diferentes usos do solo. As variáveis analisadas foram temperatura (T), oxigênio dissolvido (OD), matéria orgânica (MO) e potencial hidrogeniônico (pH). Foram encontradas diferenças significativas na matéria orgânica para os pontos P3 (mata nativa) e P6 (eucalipto), e no oxigênio dissolvido para os pontos P1 (mata nativa) e P6 (eucalipto), e quando comparadas às médias...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Qualidade da água; Floresta nativa; Eucalipto.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300020

Uniformidade de aplicação de água de equipamentos autopropelidos de irrigação com aspersores de perfil radial triangular, elíptico e retangular
Provedor de dados: 70
Autores: Prado,Giuliani do; Colombo,Alberto; Oliveira,Henrique F. E. de; Faria,Lessandro C.
Este trabalho apresenta resultados de simulações digitais da uniformidade de aplicação de água de sistemas autopropelidos de irrigação, para a condição de ausência de ventos. Nas simulações foram considerados aspersores com perfis radiais de distribuição de água tipo triangular, elíptico e retangular, operando sob diferentes combinações de ângulo de giro (de 180 até 360º) e espaçamento entre carreadores (de 0 a 100% do diâmetro molhado - DM). Os resultados das simulações foram apresentados em três grupos distintos, cada um representando a mesma forma geométrica do perfil radial de distribuição de água. Independentemente do ângulo de giro, os melhores valores de uniformidade foram obtidos com espaçamentos menores que 45% e entre 55% e 70% do DM para o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulações digitais; Ângulo de giro; Espaçamento entre carreadores.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300011

Distribuição volumétrica e espectro de gotas de bicos hidráulicos de jato plano de faixa expandida XR11003
Provedor de dados: 70
Autores: Camara,Felipe T. da; Santos,José L.; Silva,Elias A.; Ferreira,Marcelo da C.
O presente trabalho teve por objetivos avaliar o espectro de gotas e os perfis de distribuição volumétrica de um bico hidráulico de jato plano de faixa expandida, modelo XR11003. Utilizou-se de analisador de partículas a laser para avaliar o espectro de gotas e de mesa de deposição para análise da distribuição volumétrica. O ensaio do espectro de gotas foi em delineamento inteiramente casualizado, em esquema fatorial 2 x 2 x 3, com três repetições, em que o primeiro fator representa o líquido pulverizado (L1 = água e L2 = água + 0,1% de espalhante adesivo não-iônico), o segundo representa a pressão de pulverização (P1 = 200 kPa e P2 = 400 kPa) e o terceiro representa três bicos hidráulicos XR11003 de jato plano (B1, B2 e B3). No ensaio de distribuição...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Surfactante; Líquido de aplicação; Tecnologia de aplicação.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400014

SWINE WASTEWATER NITROGEN REMOVAL AT DIFFERENT C/N RATIOS USING THE MODIFIED LUDZACK-ETTINGER PROCESS
Provedor de dados: 70
Autores: Giongo,Adelcio; Bortoli,Marcelo; Prá,Marina Celant De; Veruck,Marcos; Kunz,Airton.
ABSTRACT The swine industry has been presented strong growth and thus is producing large volumes of effluents that must be correctly management. Nitritation/denitritation process can be used to improve system performance, saving the energy cost with aeration and with the external source of carbon due to the lower C/N requirement. The aim of this study was to evaluate swine wastewater Nitrification/Denitrification (NDF) and Nitritation/denitritation (NDT) processes at different C/N ratios, using the Modified Ludzack-Ettinger (MLE) process, in order to obtain a system with efficient nitrogen removal and low oxygen and carbon consumption. Four phases were conducted during the experiment: Phase I) DO between 2.0-3.0 mg L−1 of O2 and C/N 1.5 (NDF); Phase II) DO...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitritation/denitritation; Nitrification/denitrification; Biological nitrogen removal; Total organic carbon consumption; Animal production wastewater.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600968

HYPERSPECTRAL SPECTROSCOPY TO DETECT DIFFERENT RESPONSES OF TWO SOYBEAN (GLYCINE MAX) CULTIVARS TO CHARCOAL ROT (MACROPHOMINA PHASEOLINA) TOXIN
Provedor de dados: 70
Autores: Al-Ahmadi,Ameer; Subedi,Arjun; Choudhary,Ruplal; Fakhoury,Ahmad; Watson,Dennis.
ABSTRACT Previous studies have confirmed the potential of hyperspectral spectroscopy (HS) to detect charcoal rot toxin effect on soybean (Glycine max). However, there is no evidence that it can differentiate among difference responses to that effect. This research tested the potential of HS (900–2400 nm) to differentiate different responses to charcoal rot effect caused by the fungal pathogen Macrophomina phaseolina. Known susceptible ‘Pharaoh’ and resistant ‘Spencer’ cultivars of soybean seedlings at the V1 stage were tested, and HS reflectance was measured in each treatment at 0 h (just before toxin treatment), 24 h, and 36 h after toxin treatment. For both cultivars, reflectance generally decreased up to 10% over time for controls and increased for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hyperspectral spectroscopy; Glycine Max; Charcoal rot; Ratio; Reflectance.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100078

FLOW PROPERTIES AND PATTERN FLOW PREDICTION OF FOOD INDUSTRIAL POWDERS
Provedor de dados: 70
Autores: Lopes Neto,José P.; Meira,Ariadne S.; Nascimento,José W. B. do.
ABSTRACT: More and more industries are faced with new products that need to be stored in silos which, in general, require knowledge of their physical properties and, above all, flow. Food industries are among those using powders as raw materials likely to develop functional problems. Thus, the aim of the present study was to investigate the flow properties of six food powders using equipment called Powder Flow Tester, and the results were compared with those recommended by the Eurocode 1 Part 4 international standard. Wide range of variation in the flow properties responses was observed, suggesting that their expression through a single average value may not be suitable for vertical silos. It was concluded that only the bulk density of products is in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Silos; Mass flow; Powder flow tester; Discharge.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400627

Effects of light intensity modification by reflective aluminized screenhouse on sweet pepper growth and yield
Provedor de dados: 70
Autores: Ferreira,Regis de C.; Bezerra,Ricardo de S.; Rosa,Juliano Q. S.
Sweet pepper is one of the ten most consumed vegetables in world. Although it develops better under protected environment, the cultivation in tropical countries is practiced in open field due greenhouse structure higher costs. Unfortunately, such practice has compromised the crop to reach either best yield or fruit quality. Since production and cost are the most important criteria for agricultural production, we aimed to evaluate reflective aluminized polypropylene shading net influence on sweet pepper (Capsicum annuum L.) growth and production as intermediary alternative for low/middle income producers from Brazilian tropical regions. Sweet pepper Magali R hybrid was cultivated in two environments: FC - field conditions (control) and RS - reflective...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Capsicum annuum L.; Shading; Photosynthetically active radiation; Solar radiation use efficiency.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400003

Demanda energética nas operações mecanizadas na silagem de milho no sistema de "silo bag"
Provedor de dados: 70
Autores: Seki,André S.; Benez,Sérgio H.; Silva,Paulo R. A.; Yano,Élcio H.; Mello,Luiz M. M.
Foi avaliado o consumo energético das operações mecanizadas envolvidas na produção de silagem de planta inteira e silagem de "grão úmido" de milho, tendo como referência o processamento seco desse cereal. O ensaio foi conduzido na Fazenda Experimental Lageado, pertencente à Faculdade de Ciências Agronômicas, e nas instalações da Faculdade de Medicina Veterinária e Zootecnia - UNESP, localizada no município de Botucatu - SP. O delineamento experimental foi em blocos ao acaso, com parcelas subdivididas no tempo (três épocas de colheita: silagem de planta inteira, silagem de "grão úmido" e colheita de grãos secos), com 10 repetições. As análises estatísticas foram realizadas por meio do programa ESTAT, pelo teste de média de Tukey, a 5% de probabilidade. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Consumo de energia; Ensilagem; Grão úmido.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300009

Caracterização da água da microbacia do córrego rico avaliada pelo índice de qualidade de água e de estado trófico
Provedor de dados: 70
Autores: Zanini,Helen L. H. T.; Amaral,Luiz A. Do; Zanini,José R.; Tavares,Lucia H. S.
A avaliação do índice de qualidade da água (IQA) e do índice de estado trófico médio (IETm) pode subsidiar a formulação de planos de manejo e gestão de sistemas aquáticos. Neste trabalho, foi avaliada a qualidade da água da microbacia do Córrego Rico, que abastece a cidade de Jaboticabal (SP), utilizando o IQA e IETm. As amostragens de água foram realizadas entre setembro-2007 e agosto-2008, em três pontos: a) em uma das nascentes; b) após a Estação de Tratamento de Esgoto de Monte Alto, e c) na captação de água para abastecimento público de Jaboticabal. As amostras foram analisadas quanto aos parâmetros físicos, químicos e microbiológicos: temperatura, oxigênio dissolvido, pH, DBO5, nitrogênio total, fósforo total, turbidez, resíduo total, ortofosfato,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bacia hidrográfica; Eutrofização; Microbiologia; Variáveis físicas químicas.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400017

ESTIMATION OF TENSILE STRENGTH PARALLEL TO GRAIN OF WOOD SPECIES
Provedor de dados: 70
Autores: Christoforo,André L.; Panzera,Tulio H.; Lahr,Francisco A. R.
ABSTRACT According to the ABNT NBR 7190: 1997 standard, tensile strength of wood samples shall be defined as the ratio between the ultimate strength from a stress test and the specimen cross-sectional area (350 mm2). However, due to the complex wood anatomy and experimental difficulties, the fractured surface in tested samples are not perpendicular to the loading direction; therefore, such fractured surface becomes larger than the sample cross section, overestimating tensile strength by this method. Using an alternative approach, we aimed to determine the approximate fracture surface of wood specimens subjected to tensile test. For this purpose, we used the least square method to estimate tensile strength of four hardwood species, which were equally...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tensile Strength; Wood; Hardwood; Least Square Method.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400533

Desempenho de bomba centrífuga operando com água residuária do processamento do café
Provedor de dados: 70
Autores: Carvalho,Jacinto A.; Aquino,Reinaldo F.; Pereira,Geraldo M.; Rodrigues,Reginaldo C.; Campos,Thiago B.
Este trabalho foi desenvolvido com o objetivo de avaliar o desempenho de bomba centrífuga no recalque de águas residuárias provenientes do processamento do café, especificamente do descascamento e da demucilagem. Montou-se uma bancada, composta por caixas d'água, tubulações, válvulas, medidores de vazão e de pressão, e uma motobomba para a realização dos ensaios. Esses consistiram em aberturas parciais do registro, na saída da bomba, e medições da vazão e da pressão desenvolvida, e da energia consumida. Tais procedimentos foram realizados, primeiro, utilizando água pura, e depois com águas residuárias, em suas concentrações originais e com diversos graus de diluições. Os ensaios mostraram quedas acentuadas de altura manométrica e de rendimento, e aumento...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bomba hidráulica; Rendimento; Potência.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100009

Estudo da adequação do uso do solo, no município de Maringá - PR, utilizando-se de geoprocessamento
Provedor de dados: 70
Autores: Barros,Zacarias X.; Tornero,Marisa T.; Stipp,Nilza A. F.; Cardoso,Lincoln G.; Pollo,Ronaldo A.
O presente trabalho tem por finalidade o estudo da adequação do uso do solo e análise da carta de aptidão agrícola, bem como o mapeamento da ocupação do solo, por meio da criação e estruturação de um banco de dados utilizando-se de Geoprocessamento, visando a atualizações e interações das informações com rapidez e eficiência, permitindo adaptações e/ou confecções de mapas temáticos da área estudada. Por meio da análise conjunta dos mapas de ocupação do solo com a carta de aptidão agrícola, pode-se constatar que: o município de Maringá - PR, apresenta ocupação de suas terras, em sua grande maioria, em acordo com a aptidão agrícola recomendada para a região; a alta porcentagem de mata nativa em terras de boa aptidão para culturas, certamente está vinculada a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aptidão agrícola; Ocupação do solo; SIG.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200024

Sonda de tdr para a estimativa de umidade em bagaço de Cana-de-açúcar
Provedor de dados: 70
Autores: Souza,Claudinei F.; Cirilo,Lucas da S; Bastos,Reinaldo G.; Peres,José G.; Oliveira,Aline F.
RESUMO O bagaço de cana-de-açúcar pode ser utilizado como suporte sólido para cultivo de microrganismos, e apesar de fundamental, o monitoramento da umidade em tempo real nesses processos ainda é pouco pesquisado. Sendo assim, o presente trabalho teve como objetivo propor e validar a TDR para estimar a umidade em bagaço de cana-de-açúcar, visando a seu uso como suporte para cultivo em estado sólido, considerando a produção de ácido cítrico. A sonda de TDR proposta foi analisada fisicamente, e, posteriormente, para a validação dos resultados, realizou-se uma calibração com leituras da constante dielétrica do bagaço de cana-de-açúcar até à saturação do material, os quais foram comparados com o método-padrão e equação universal de Topp. Também, foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: TDR; Monitoramento de umidade; Cultivo em estado sólido; Aspergillus Níger; Constante dielétrica.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100024

Transpiração e temperatura foliar da cana-de-açúcar sob diferentes valores de potencial matricial
Provedor de dados: 70
Autores: Trentin,Roberto; Zolnier,Sérgio; Ribeiro,Aristides; Steidle Neto,Antonio J.
O objetivo deste trabalho foi avaliar a variação diurna da transpiração e da temperatura foliar da cana-de-açúcar, cv. RB867515, sob diferentes potenciais matriciais de água no substrato de cultivo e as condições meteorológicas em ambiente protegido. O efeito do estresse hídrico na transpiração e temperatura foliar foi determinado a partir da suspensão da irrigação, quando foram realizadas três campanhas de medições, iniciadas aos 122; 150 e 185 dias após o plantio (DAP) até que o potencial matricial de água no substrato (Ψ) alcançasse -1.500 kPa, aproximadamente. Sob ausência de estresse hídrico (Ψ&amp;gt;-50 kPa), a transpiração das plantas atingiu o valor máximo entre 10 e 13 h, próximo de 60; 70 e 100 g planta-1 h-1 para 122; 150 e 185 DAP,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum officinarum; Evapotranspiração; Termometria a infravermelho; Estresse hídrico; Irrigação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600006

STATISTICAL CONTROL OF THE PROCESS APPLIED TO THE MONITORING OF THE WATER QUALITY INDEX
Provedor de dados: 70
Autores: Conceição,Ketllin Z. da; Boas,Marcio A. Vilas; Sampaio,Silvio C.; Remor,Marcelo B.; Bonaparte,Danilo I.
ABSTRACT Analyzing the physical-chemical and biological characteristics allows the evaluation of the water quality of a water body. Thus, the objective of this study was to determine the water quality index of the Passaúna and Piraquara rivers, as well as to apply statistical quality control methodologies to evaluate the data resulting from the monitoring of water quality. Therefore, a database with physico-chemical and microbiological parameters of the Passaúna and Piraquara rivers, a watershed of the Iguaçu River, belonging to the cities of Araucária and Piraquara, respectively Paraná, Brazil, was used to carry out the research. The water quality index was determined with the time series and, subsequently, these data were submitted to the statistical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water quality index; Control charts; Capacity of the process.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600951

Poultry carcass decomposition and physicochemical analysis of compounds in different Composter types
Provedor de dados: 70
Autores: Cestonaro,Taiana; Abreu,Paulo G. de; Abreu,Valéria M. N.; Lopes,Letícia dos S.; Coldebella,Arlei.
This study aimed to assess five composter types in poultry carcasses decomposition and to perform a physicochemical analysis of the compounds obtained. Composter types used were six-hole brick, wood, screen, windrow with three PVC pipes with six holes and windrow with three PVC pipes with 10 holes. Composting was followed by four periods using wood shaving like substrate with one bird carcass placed in each composter. Pile turning was performed every 10 days and temperature in each layer was measured on 1st, 7th, 14th, 19th and 29th day, at 3 p.m., as well as room temperature. Temperature during pile turning was also measured at five points per layer and carcass weighing performed to calculate decomposition percentage. Physicochemical parameters evaluated...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Composting; Organic fertilizers; Substrate.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400002

Determinação do fluxo de seiva na cana-de-açúcar pelo método do balanço de energia caulinar
Provedor de dados: 70
Autores: Boehringer,Davi; Zolnier,Sérgio; Ribeiro,Aristides; Steidle Neto,Antonio J.
Medições do fluxo de seiva são importantes não somente no campo da agrometeorologia, mas também em estudos de natureza fisiológica para identificação de doenças vasculares e pesquisas destinadas à quantificação do movimento de água no sistema solo-planta-atmosfera. Este trabalho foi realizado com o objetivo de avaliar o desempenho do método do balanço de energia, a partir da inserção de um minirresistor no centro do colmo de plantas de cana-de-açúcar, visando à determinação do fluxo de seiva sob condições ambientais distintas, utilizando-se de medições gravimétricas como padrão comparativo. O experimento foi conduzido em uma casa de vegetação não climatizada, localizada na área experimental da Universidade Federal de Viçosa, Viçosa - MG. Com base no erro...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Transpiração; Saccharum officinarum; Eficiência do uso de água; Disponibilidade hídrica; Irrigação.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200003

SIMANIHOT: A PROCESS-BASED MODEL FOR SIMULATING GROWTH, DEVELOPMENT AND PRODUCTIVITY OF CASSAVA
Provedor de dados: 70
Autores: Tironi,Luana F.; Streck,Nereu A.; Gubiani,Paulo I.; Benedetti,Rômulo P.; Freitas,Charles P. de O. De.
ABSTRACT The objective of this study was to propose a model, named Simanihot, for simulating growth, development and yield of tuberous roots in cassava, with a choice of two soil water balance models. The model works on a day time step and is calibrated for five cassava cultivars (Fepagro –RS 14, Estrangeira, Cascuda, São José e Paraguaia), with different branching habits and different purpose of use (pasture, food and industry). The model has a graphical interface, where the user can choose one out of two soil water balance models, depending upon the number of known soil variables and details the user wants to know about soil water content.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manihot esculenta; Modeling; Software; Soil water balance.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300471

Influência da temperatura do ar de secagem no calor latente de vaporização de água em feijão macassar (Vigna unguiculata (L.) Walp.), variedade sempre-verde
Provedor de dados: 70
Autores: Silva,Wilton P. da; Silva,Cleide M. D. P. S. e; Precker,Jürgen W.; Silva,Diogo D. P. S. e.
Em cálculos da quantidade de energia requerida em processos de secagem artificial de um produto agrícola, é necessário o conhecimento de uma expressão para a determinação do calor latente de vaporização (H) de água no produto. Normalmente, as expressões para H, encontradas na literatura, são dadas pelo calor latente de vaporização (h) de água livre multiplicado por funções que dependem apenas do teor de água do produto. Isso significa que a relação H/h, para um dado produto, só depende do teor de água, o que é uma simplificação, pois se sabe que tal relação depende também da temperatura. Neste artigo, é apresentada uma expressão para o cálculo de H para feijão macassar, variedade sempre-verde, levando em consideração a dependência de H/h com a temperatura....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energia; Produtos agrícolas; Secagem.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200012

A DISCRETE STOCHASTIC MODEL TO DETERMINE FOOD QUALITY BY USING SIMULATION: A STRAWBERRY CASE STUDY
Provedor de dados: 70
Autores: González-Hernández,Isidro J.; Granillo-Macías,Rafael; Rondero-Guerrero,Carlos; Martínez-Flores,José L.
ABSTRACT The agri-food supply chain (AFSC) sets a series of challenges in the production, storage, distribution, and transportation processes, as the market's requirements for fresh food combine food quality and safety attributes. This research suggests a discrete event modeling to study the behavior of food quality in all supply chains (SCs) in terms of temperature and time variables in a stochastic manner. The ProModel software was used to simulate strawberry quality in the SC, considering a distribution route to export the fruit from Mexico to the United States. The suggested model together with a computer simulation analyzes the fruit quality from two perspectives: with and without a cold chain (CC). The obtained results revealed that in the case of CC...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agri-food supply chain; Discrete and stochastic model; Food quality; Simulation.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600747

Acúmulo de metais pesados em cana-de-açúcar mediante a aplicação de lodo de esgoto e vinhaça
Provedor de dados: 70
Autores: Camilotti,Fábio; Marques,Marcos O.; Andrioli,Itamar; Silva,Alysson R. da; Tasso Junior,Luiz C.; Nobile,Fabio O. de.
O uso de resíduos agroindustriais pode acumular metais pesados no solo e na planta. O objetivo deste trabalho foi avaliar os efeitos do lodo de esgoto e/ou vinhaça, aplicados no solo, disponibilizando Cd, Cr, Ni e Pb ao solo e quantificar as respectivas concentrações em plantas de cana-de-açúcar, após três aplicações anuais sucessivas. O experimento foi conduzido em condições de campo, com parcelas experimentais de cinco linhas espaçadas de 1,5 m e 10 m de comprimento. O delineamento experimental adotado foi o de blocos casualizados, com três repetições. Os tratamentos avaliados foram: 1. Lodo de esgoto com 100% de N; 2. Lodo de esgoto com 200% de N; 3. Vinhaça com 100% de K; 4. Vinhaça com 200% de K; 5. Lodo de esgoto+vinhaça com 100% de N e K; 6. Lodo de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cádmio; Chumbo; Cromo.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100023

Influência da vibração das hastes e da velocidade de deslocamento da colhedora no processo de colheita mecanizada do café
Provedor de dados: 70
Autores: Oliveira,Ezequiel de; Silva,Fábio M. da; Salvador,Nilson; Figueiredo,Carlos A. P.
Hoje, já existem vários estudos sobre a eficiência operacional de colheita mecanizada do café, porém pouco se sabe sobre a influência da vibração das hastes e a velocidade de deslocamento da colhedora nesse processo. Assim, este trabalho teve por objetivo avaliar a influência da vibração das hastes e da velocidade de deslocamento da colhedora no processo de colheita mecanizada do café. O trabalho foi desenvolvido na Fazenda Capetinga, sul de Minas Gerais. Para os ensaios, utilizou-se do delineamento inteiramente casualizado, com quatro repetições, em parcelas aleatórias, contendo, em média, 40 plantas em fileira. Os ensaios foram realizados com duas passadas da colhedora, definidos em função do índice de frutos verdes na planta. A primeira passada foi...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cafeicultura; Mecanização agrícola; Derriça.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400014

ANALYSIS OF ELASTICITY IN WOODS SUBMITTED TO THE STATIC BENDING TEST USING THE PARTICLE IMAGE VELOCIMETRY (PIV) TECHNIQUE
Provedor de dados: 70
Autores: Pereira,Rodrigo A.; Gomes,Francisco C.; Braga Júnior,Roberto A.; Rivera,Fernando P.
ABSTRACT The most important parameter in terms of material mechanical behavior knowledge is the modulus of elasticity, being traditionally obtained through destructive tests. The objective of this study is the verification of the potential use of the particle image velocimetry technique (PIV) as a tool to obtain the modulus of elasticity in sawed wood samples (Pinus oocarpa and Eucaliptus grandis) and wood panels (Plywood, LVL and OSB). The PIV technique has as characteristics the low cost of equipment, fast results, no need for contact with the object tested, accuracy and possibility of application in the field. The application of the PIV technique occurred during the static bending tests where the deformations were also measured with a dial indicator...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Characterization; Nondestructive testing; Modulus of elasticity.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200159

CHARACTERIZATION OF THE THERMAL ENVIRONMENT IN BROILER HOUSES WITH DIFFERENT CLIMATE CONTROL SYSTEMS
Provedor de dados: 70
Autores: Teles Junior,Carlos G. de S.; Gates,Richard S.; Souza,Cecilia de F.; Tinôco,Ilda de F. F.; Vilela,Monique de O.
ABSTRACT The environment control of broiler houses must be done adequately to provide good thermal conditions to broilers without wasting energy. The objective of this study was to characterize the thermal environment in two mechanically ventilated broiler houses with a negative pressure ventilation system, one with a cellulose pad evaporative cooling system and the other with misting nozzles for evaporative cooling. The experiment was conducted in Ervália-MG during winter, spring, and summer. The thermal environment was characterized based on the relationship between the temperature observed inside the broiler houses and the temperatures recommended for the thermal comfort of birds of different ages. The recorded data were evaluated using descriptive...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Broiler thermal demand; Cooling; Heating; Thermal environment management.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500571

Estimation of alluvial recharge in the semiarid
Provedor de dados: 70
Autores: Andrade,Tafnes S.; Montenegro,Suzana M. G. L.; Montenegro,Abelardo A. de A.; Rodrigues,Diogo F. B.
In areas where there is irrigated agriculture, the recuperation of water reserves in alluvial aquifers may occur preferentially due to precipitation. Recharging can be evaluated from variation information of water depth measured in piezometers or observation wells. Thus, the aim of this research is to study the recharge in the alluvial aquifer formed by the Mimoso temporary stream in the semiarid region of Pernambuco (PE), Brazil, using the method of the fluctuation of the water level. This system is typical on the Brazilian Northeast semiarid region, using groundwater for domestic supply and for irrigation on small scale agriculture. Monthly potentiometric levels and rainfall data were used. The selected period for the study, from January 2002 to October...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Recharge factor; Groundwater; Monitoring.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200003

Avaliação dos efeitos da cobertura de palha de cana-de-açúcar na umidade e na perda de água do solo
Provedor de dados: 70
Autores: Peres,José G.; Souza,Claudinei F.; Lavorenti,Norberto A.
No período de 23 de junho a 23 de julho de 2006, nas condições edafoclimáticas da região de Araras - SP, estudou-se a influência da cobertura de palha de cana-de-açúcar colhida mecanicamente nos valores da umidade volumétrica de um Latossolo Vermelho-Escuro, distrófico, A moderado, de textura argilosa. A variação da umidade volumétrica do solo foi avaliada nas camadas de 0 a 0,20 m e 0,20 a 0,40 m de profundidade. Os tratamentos consistiram na cobertura do solo com quantidades de palha de cana-de-açúcar equivalentes a 0 e 1,5 kg m-2 (0 e 1,5 10(4) kg ha-1); o primeiro tratamento representando a condição sem palha, e o segundo, a condição com palha. Os resultados coletados na camada de 0-0,20 m mostraram que, no período estudado houve redução dos valores da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cobertura morta; Palhada de cana-de-açúcar; Umidade do solo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500010

A SPECTRAL AGROMETEOROLOGICAL MODEL FOR ESTIMATING SOYBEAN GRAIN PRODUCTIVITY IN MATO GROSSO, BRAZIL
Provedor de dados: 70
Autores: Sarmiento,Christiany M.; Coltri,Priscila P.; Alves,Marcelo de C.; Carvalho,Luiz G. de.
ABSTRACT This study used spectral data integrated with the agrometeorological model by Doorenbos and Kassam to estimate soybean grain productivity in the state of Mato Grosso, Brazil. In the developed model, spectral data were used instead of meteorological data and biophysical parameters of the crop. For this purpose, the products of real and potential evapotranspiration (MOD16), normalized difference vegetation index – NDVI (MOD13Q1), and leaf area index (MOD15A2H) from the MODIS satellite were used, in addition to sunstroke data obtained by using the visible channel from the satellite GOES IMAGER. The results obtained showed that, with the proposed methodology, it was possible to follow the development of soybean cultivation throughout the cycle and to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geographic Information System; Mathematical Modeling; Remote Sensing; Agrometeorology; Crop Monitoring.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300405

Efeitos da velocidade e da direção do vento na uniformidade de aplicação de água de sistemas autopropelidos
Provedor de dados: 70
Autores: Oliveira,Henrique F. E. de; Colombo,Alberto; Faria,Lessandro C.; Prado,Giuliani do.
A velocidade e a direção de incidência do vento, em relação ao eixo de deslocamento do aspersor, são variáveis apresentadas em vários trabalhos como fatores importantes para a determinação da uniformidade de aplicação de água dos equipamentos autopropelidos de irrigação. No entanto, em razão das dificuldades de se conduzir estudos de campo com canhões hidráulicos sob condições controladas de direção e velocidade do vento, as recomendações de espaçamento entre carreadores, em sua maioria, consideram apenas o efeito da velocidade do vento, sem mencionar a direção de sua incidência. Neste trabalho, a aplicação de coeficientes semiempíricos do modelo Richards &amp;amp; Weatherhead, ajustados com base em ensaios de campo do canhão PLONA RL-250, possibilitou...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulação; Canhão hidráulico; Modelo semiempírico.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400006

Coffee seedlings in different substrates and protected environments
Provedor de dados: 70
Autores: Silva,Arthur P. da; Costa,Edilson; Espírito Santo,Tiago L. do; Silva,Luan E. da; Martins,Roberta F.
The production of high-quality seedlings is a critical factor for successful implementation of a determined crop in the field. In order to evaluate the production of coffee seedlings, experiments were conducted with different substrates and in different protected environments. Treatments consisted of evaluation of the following substrates: 50% cattle manure + 50% commercial substrate, 50% cattle manure + 50% vermiculite, 50% commercial substrate + 50% vermiculite, 1/3 cattle manure + 1/3 commercial substrate + 1/3 vermiculite, 50% cattle manure + 50% sand, 1/3 sand + 1/3 cattle manure + 1/3 commercial substrate and 50% commercial substrate + 50% sand. These substrates were tested in different protected environments: agricultural greenhouse, mesh screen...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffee arabica; Cattle manure; Vermiculite; Commercial substrate; Sand.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400001

Characterization and treatment of sisal fiber residues for cement-based composite application
Provedor de dados: 70
Autores: Lima,Paulo R. L.; Santos,Rogério J.; Ferreira,Saulo R.; Toledo Filho,Romildo D.
Sisal fiber is an important agricultural product used in the manufacture of ropes, rugs and also as a reinforcement of polymeric or cement-based composites. However, during the fiber production process a large amount of residues is generated which currently have a low potential for commercial use. The aim of this study is to characterize the agricultural residues by the production and improvement of sisal fiber, called field bush and refugo and verify the potentiality of their use in the reinforcement of cement-based composites. The residues were treated with wet-dry cycles and evaluated using tensile testing of fibers, scanning electron microscopy (SEM) and Fourier transform infrared (FTIR) spectroscopy. Compatibility with the cement-based matrix was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural residue; Biocomposites; Pull-out test; Fiber treatment; Flexural behavior.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500002

RESISTANCE OF A RED LATOSOL TO PENETRATION: COMPARISON OF PENETROMETERS, MODEL ADJUSTMENT, AND SOIL WATER CONTENT CORRECTION
Provedor de dados: 70
Autores: Duarte,Thiago F.; Silva,Tonny J. A. da; Bonfim-Silva,Edna M.; Fenner,Willian.
ABSTRACT Penetration resistance can be determined directly in the field or in the laboratory. However, data obtained using the two methods are not directly comparable. Considering soil moisture influences penetration resistance, penetration resistance data obtained using the two methods can be corrected based on common moisture values. To enable comparison of the data, the measured data should be adjusted using mathematical models. Consequently, the objective of the present study was to compare soil penetration resistance values measured in a Red Latosol using a static penetrometer and a bench-top electronic penetrometer. The comparison was carried out using samples collected from different soil layers, based on moisture levels ranging from 0.15 to 0.28 kg...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil physics; Soil mechanical; Soil compaction; Modeling.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400462

Influência do auxílio mecânico na colheita de tomates
Provedor de dados: 70
Autores: Sanchez,Augusto C.; Ferreira,Marcos D.; Magalhães,Ana M. de; Braunbeck,Oscar A.; Cortez,Luis A. B.; Magalhães,Paulo S. G.
O objetivo deste trabalho foi avaliar parâmetros que influenciam na colheita auxiliada e comparar a colheita tradicionalmente realizada para tomate de mesa em propriedades agrícolas, no Estado de São Paulo. Para tanto, foi desenvolvido um dispositivo de auxílio à colheita, de estrutura metálica, dotado de rodas e com assentos acoplados para um ou dois colhedores, avaliado em quatro modalidades de colheita: testemunha (colheita-padrão utilizada na Fazenda Santa Luzia, Brotas-SP), colhedor a pé com auxílio, colhedor sentado com auxílio e composição dos dois sistemas, com dois colhedores sentados e um a pé, em diferentes velocidades de deslocamento. Os resultados demonstraram que os tipos de colheita com auxílio mecânico se apresentaram mais eficientes do que...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lycopersicum esculentum; Colhedor; Produtividade.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300011

Evapotranspiration and crop coefficient for potato in organic farming
Provedor de dados: 70
Autores: Carvalho,Daniel F. de; Silva,Dione G. da; Rocha,Hermes S. da; Almeida,Wilk S. de; Sousa,Eraldo da S.
The aim of this study was to quantify the water consumption and the crop coefficients (Kc) for the potato (Solanum tuberosum L.), in Seropédica, Rio de Janeiro (RJ), Brazil, under organic management, and to simulate the crop evapotranspiration (ETc) using the Kc obtained in the field and the ones recommended by the Food and Agriculture Organization (FAO). The water consumption was obtained through soil water balance, using TDR probes installed at 0.15m and 0.30m deep. At the different stages of development, the Kc was determined by the ratio of ETc and reference evapotranspiration, obtained by Penman-Monteith FAO 56. The crop coefficients obtained were 0.35, 0.45, 1.29 and 0.63. The accumulated ETc obtained in the field was 109.6 mm, while the ETc...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solanum tuberosum L.; Time domain reflectometry; Irrigation.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100020

Desempenho de dois equipamentos na colheita semimecanizada da cultura da mandioca
Provedor de dados: 70
Autores: Scalon Filho,Homero; Alves Sobrinho,Teodorico; Souza,Cristiano M. A. de.
Estudou-se o desempenho operacional de dois equipamentos na colheita da mandioca. Um afofador do solo e um arrancador de mandioca foram avaliados. Analisaram-se a patinagem das rodas motoras, as perdas de produto, os danos mecânicos provocados às raízes e a capacidade de campo dos conjuntos trator-equipamento. Depois da passagem dos conjuntos, as raízes inteiras colhidas e que permaneceram no solo e com danos mecânicos, foram separadas e pesadas. O conjunto trator-arrancador apresentou melhor dinâmica de corte, penetração no solo e menor patinagem das rodas. Não foram observadas perdas de raízes para os conjuntos avaliados. Os equipamentos apresentaram semelhantes danos mecânicos às raízes. O conjunto trator-afofador apresentou capacidade de campo 25%...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Arrancador de mandioca; Afofador de solo; Perdas.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200030

Efeito da cobertura nas perdas de solo em um argissolo vermelho-amarelo utilizando simulador de chuva
Provedor de dados: 70
Autores: Silva,Demétrius D.; Pruski,Fernando F.; Schaefer,Carlos E. G. R.; Amorim,Ricardo S. S.; Paiva,Karlos W. N.
O objetivo deste trabalho foi avaliar o efeito da porcentagem de cobertura do solo e da energia cinética decorrente de chuvas simuladas sobre as perdas de solo. O experimento consistiu de seis parcelas experimentais (4 m²), as quais foram mantidas com coberturas de 0; 20; 40; 60; 80 e 100%, utilizando manta de Bidin, simulando condição de manejo de cultivo em contorno. Utilizou-se de simulador de chuva sobre Argissolo Vermelho-Amarelo, com declividade média de 9,5%. Foram utilizadas as intensidades de precipitação de 60; 80; 100 e 120 mm h-1, associadas às durações de 68; 40; 24 e 14 minutos, resultando nos valores de energia cinética de 1.401; 1.122; 841 e 589 J m-2, respectivamente. Para cada uma das intensidades de precipitação, realizaram-se seis...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão hídrica; Intensidade de precipitação; Cobertura do solo.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200014

DAILY RAINFALL DISAGGREGATION COEFFICIENTS FOR THE DOCE RIVER BASIN, BRAZIL: REGIONAL APPLICABILITY AND THE RETURN PERIOD INFLUENCE
Provedor de dados: 70
Autores: Passos,Jéssica B. de M. C.; Silva,Demetrius D. da; Lima,Rafael P. C.
ABSTRACT Alternative methods to the intensity-duration-frequency equations have been used for intense rainfall study in places with no pluviographic data. A pioneering study, by CETESB (1986), established rainfall disaggregation coefficients for Brazil; however, the use of these coefficients take into account neither the rainfall characteristics of the interest locality nor the return period influence in obtaining the precipitation intensities. This study aimed to determine rainfall disaggregation coefficients for Doce river basin; to verify the validity of the regional coefficients use for the entire basin; and to evaluate the return period influence on these coefficients. Data from 19 gauges located in the basin, with rainfall associated with durations...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Daily rainfall disaggregation method; Heavy rainfall; Hydrology; Pluviometric data; Pluviograph gauge station.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200223

Gas emission and efficiency of an engine-generator set running on biogas
Provedor de dados: 70
Autores: SOUZA,SAMUEL N. M. DE; LENZ,ANDERSON M.; WERNCKE,IVAN; NOGUEIRA,CARLOS E. C.; ANTONELLI,JHONATAS; SOUZA,JULIANO DE.
ABSTRACT In Brazil there is a wide availability of residues, which have been used in the production of biogas and biofertilizers. The engine-generator by biogas is grid connected, and produce electricity for self-consumption and the surplus is inserted into the grid. The aim of the present study was to evaluate energetic efficiency and exhaust gas emission of two cases: two engine-generators sets of 100 kVA running on biogas, produced from residues of a poultry slaughterhouse unit (PSU) and swine fattening unit (SFU). Load variation in the engine-generator set was evaluated in the SMCP (system of protection and synchronism). There was an increase in the emission of nitrogen oxide, sulfur dioxide and exhaust gas temperature, in both cases. The elevation in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biofuel; Energy efficiency; Organic waste; Gas emission.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400613

Classificação e padronização dos tomates cv. Carmem e Débora dentro da CEAGESP - SP
Provedor de dados: 70
Autores: Andreuccetti,Caroline; Ferreira,Marcos D.; Gutierrez,Anita S. D.; Tavares,Marcelo.
A criação do Programa Brasileiro para a Modernização da Horticultura pela Secretaria de Agricultura e Abastecimento do Estado de São Paulo, em conjunto com a Companhia de Entrepostos e Armazéns Gerais de São Paulo (CEAGESP), determinou a padronização das hortaliças e frutas comercializadas nos seguintes aspectos: grau de coloração, formato, calibres, defeitos e embalagens, um trabalho iniciado em setembro de 1997. O objetivo deste trabalho foi relacionar a classificação fornecida pelo Programa Brasileiro com a realizada pelos atacadistas no mercado da CEAGESP, verificando se as normas estabelecidas estão sendo cumpridas para os tomates cultivares Carmem e Débora (SAKATA SEED). Os resultados mostraram que, para o tomate cultivar Carmem, a partir da análise...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lycopersicum esculentum Mill.; Normas de padronização; Atacadista.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300033

Fusão de imagens por IHS para melhorar a identificação de uso do solo em elementos amostrais
Provedor de dados: 70
Autores: Adami,Marcos; Deppe,Flavio; Rizzi,Rodrigo; Moreira,Mauricio A.; Rudorff,Bernardo F. T.; Fonseca,Leila M. G.; Faria,Rogério T.
Fotografias aéreas métricas atuais sobre áreas específicas nem sempre estão disponíveis. Esse é um dos principais problemas no Brasil para aplicação de técnicas de amostragem de área para a estimativa de safras. Este trabalho avaliou a técnica de fusão IHS aplicada em imagens Landsat7-ETM+ para a substituição das fotografias aéreas de arquivo, em trabalhos de coleta de dados de campo e delimitação de elementos amostrais para os sistemas de estimativas de área de culturas agrícolas. As bandas 3; 4; 5 e 7 do sensor de ETM+ foram usadas nas diferentes combinações de RGB e fundidas por IHS com a faixa pancromática para produzir imagens com melhor definição espacial. As imagens resultantes foram impressas na escala de 1:25.000 e usadas no trabalho de campo, em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Amostragem; Sensoriamento remoto; Processamento de imagens.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300023

QUALITY OF MECHANICAL SOYBEAN HARVESTING AT TWO TRAVEL SPEEDS
Provedor de dados: 70
Autores: Lima,Felipe B. F. De; Silva,Michel A. F. Da; Silva,Rouverson P. Da.
ABSTRACT: Soybean harvesting is the last operation performed in the field and therefore has high added value. Quantitative losses during this process should therefore be minimized to achieve maximum quality and increase the sustainability of the production system. The aim of the present study was to determine and characterize the quantitative losses and operational characteristics of an axial-flow combine harvester, using tools from Statistical Quality Control to determine the quality of the harvesting operation. The experiment was designed in accordance with the assumptions of statistical process control, with a total of 40 sampling points monitored over time. Quality indicators of harvester performance and crop agronomic characteristics were evaluated at...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Control charts; Variability; Harvesting losses.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601171

Fatores qualitativos da ponta de energia hidráulica ADGA 110015 para pulverização agrícola
Provedor de dados: 70
Autores: Ferreira,Marcelo C.; Costa,Glauberto M.; Silva,Adriana R.; Tagliari,Sônia R. A.
Este trabalho teve o objetivo de caracterizar o diâmetro e a uniformidade das gotas e o perfil de distribuição volumétrica da ponta denominada antideriva de grande ângulo (ADGA) 110015, nas pressões de 207 e 310 kPa, para determinar o seu espaçamento na barra de pulverização. Os perfis de distribuição volumétrica para a altura de 50 cm foram avaliados em mesa de deposição. A partir dos perfis de distribuição, simulou-se o padrão de deposição ao longo da barra de pulverização. O espectro do diâmetro de gotas foi determinado em analisador de tamanho de partículas por difração laser. Pode-se concluir que a ponta ADGA 110015 apresentou perfil de distribuição do jato simétrico nas pressões de trabalho de 207 e 310 kPa. Na maior pressão, pode-se operar com menor...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bico; Padrão de deposição; Tamanho de gotas.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300016

RESIDUAL BIOMASSES IN THE MICRO-REGION OF DOURADOS (MS): ASSESSMENT AND AVAILABILITY FOR ENERGY IN AGRICULTURE THERMAL CONVERSION
Provedor de dados: 70
Autores: Silva,Robson L. da; Paula,Isabele O. de; Patelli Júnior,José R.; Torres,Tainara R. C.; Pereira,Thiago V.
ABSTRACT This research presents results of the assessment of solid biofuels (residual biomasses from agricultural crops) in the state of Mato Grosso do Sul, in the period 2007-2012, for energy in agricultural uses. It is pointed out the available quantity, its geographic location at micro and meso regions and energy conversion potential. The methodology is based on a survey on municipal agricultural production of the Brazilian Institute for Geography and Statistics (quantity and local availability, per year) followed by determination of the amounts of agricultural assessed residues, and then applying equations from the literature to estimate the amount of energy (J) and power (kW) obtained from the thermal conversion of residual biomasses. Results are...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Renewable energy; Solid biofuels; Combustion; Torrefaction; Powerplants.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300433

Avaliação da compostagem de carcaças de frango pelos métodos da composteira e de leiras estáticas aeradas
Provedor de dados: 70
Autores: Paiva,Ed Carlo R.; Matos,Antonio T. de; Azevedo,Mônica A.; Barros,Renata T. P. de; Costa,Tatiana D. R.
Avaliaram-se a compostabilidade de diversos resíduos adequadamente misturados e a eficiência de diferentes processos (leiras estáticas aeradas e composteira) na eliminação de microrganismos e tempo de compostagem. Tratamentos: composteira: palha de café, cama de frango e carcaça de frango, LEA 01: bagaço de cana-de-açúcar, cama de frango e carcaça de frango inteira, LEA 02: bagaço de cana-de-açúcar, cama de frango e carcaça de frango triturada, LEA 03: palha de café, cama de frango e carcaça de frango triturada. Variáveis monitoradas: temperatura, relação C/N, sólidos voláteis (SV), pH e umidade, além de avaliar a eliminação de Salmonella e a redução de coliformes termotolerantes. Os resultados obtidos para redução de SV foram 20,87% (composteira), 25,31%;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carcaça de frango; Compostagem; Composteira; Leiras estáticas aeradas.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500015

Uso de traçadores para avaliação da hidrodinâmica de sistemas alagados construídos operando sob condições climáticas tropicais
Provedor de dados: 70
Autores: Borges,Alisson C.; Matos,Antônio T. de; Calijuri,Maria do C.; Oliveira,Gabriel H. H. de; Roldão,João S. F.
Sistemas alagados construídos (SACs) são, atualmente, importante opção para o tratamento de resíduos e controle da poluição pontual e difusa. O uso de SACs tem aumentado ano a ano, entretanto o nível de entendimento da hidrodinâmica do processo não tem crescido na mesma proporção. Traçadores fluorescentes apresentam-se como opção na determinação de curvas de distribuição de tempos de residência (DTR) e de parâmetros hidrodinâmicos, como número de dispersão e eficiência hidráulica. A pesquisa foi realizada com o objetivo de avaliar dois corantes (rodamina WT e fluoresceína sódica) na determinação das características hidrodinâmicas de SACs com escoamento subsuperficial, operando em região de clima tropical. Os tempos de residência experimentais (τR) para os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Comportamento hidrodinâmico; Distribuição de tempos de residência; Fluoresceína sódica; Número de dispersão; Rodamina WT; Wetlands construídas.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200013

Armazenamento sob condições ambiente e aceitabilidade do melão 'F1 Jangada' produzido em sistema hidropônico
Provedor de dados: 70
Autores: Rinaldi,Maria M.; Sandri,Delvio; Nunes,Dayanna M. C.; Amaral,Adriana G. do.
O objetivo deste trabalho foi determinar o período de armazenamento pós-colheita e a aceitabilidade pelo consumidor de melão híbrido 'F1 Jangada' (Cucumis melo L.), produzido em sistema hidropônico, mantido em condições ambiente (22 ± 2 ºC e umidade relativa de 40 ± 5%). O experimento compreendeu o período de 21-6-2005 a 2-8-2005. Foi utilizado o esquema fatorial 5 x 2, em delineamento experimental inteiramente casualizado, com cinco períodos de armazenamento (0; 7; 21; 28 e 42 dias) e dois tipos de substrato (areia e fibra de coco), com três repetições, em que cada repetição consistiu em cinco frutos de meloeiro. Foram avaliados o pH, a acidez titulável, os sólidos solúveis, a perda de massa fresca, a análise sensorial e a decisão de compra dos melões....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cucumis melo L.; Análise sensorial; Vida útil pós-colheita.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300018

Thermal gradients of container and mean surface temperature of broiler chicks transported on different shipments
Provedor de dados: 70
Autores: NAZARENO,AÉRICA C.; SILVA,IRAN J. O. DA; DONOFRE,ANA C.
ABSTRACT This study aimed to evaluate the thermal gradients between the container environment and the interior of chick boxes and mean surface temperature of broiler chicks during transportation on different shipments. The research was conducted in the state of São Paulo, Brazil, with the accompaniment of nine shipments with different density boxes, using an acclimatized truck with an average capacity of 380 boxes. It was selected 14 chick transportation boxes on each shipment and, subsequently, five chicks per box. It was measured the mean surface temperature of chicks (MST) in shipment (loading and unloading) by using an infrared thermometer. In the container microclimate assessment (center and inside chick boxes), it was recorded the air temperature...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Pre-farm gate practices; Poultry production; Acclimatized truck; Live load.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400581

Rainfall erosivity for the State of Rio de Janeiro estimated by artificial neural network
Provedor de dados: 70
Autores: Carvalho,Daniel F. de; Khoury Júnior,Joseph K.; Varella,Carlos A. A.; Giori,Jacqueline Z.; Machado,Roriz L.
The Artificial Neural Networks (ANNs) are mathematical models method capable of estimating non-linear response plans. The advantage of these models is to present different responses of the statistical models. Thus, the objective of this study was to develop and to test ANNs for estimating rainfall erosivity index (EI30) as a function of the geographical location for the state of Rio de Janeiro, Brazil and generating a thematic visualization map. The characteristics of latitude, longitude e altitude using ANNs were acceptable to estimating EI30 and allowing visualization of the space variability of EI30. Thus, ANN is a potential option for the estimate of climatic variables in substitution to the traditional methods of interpolation.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geographic information system; Interpolation methods; Soil conservation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100020

ESTIMATION OF WOOD TOUGHNESS IN BRAZILIAN TROPICAL TREE SPECIES
Provedor de dados: 70
Autores: Christoforo,André L.; Almeida,Diego H. de; Varanda,Luciano D.; Panzera,Tulio H.; Lahr,Francisco A. R.
ABSTRACT Wood has been used for several purposes such as in civil and rural construction. Knowing wood mechanical behavior under short-term loading is essential for safer structural designs. However, wood toughness is a mechanical property little investigated for this purpose. Thus, this study aimed to evaluate, using exponential and polynomial regression models (linear, quadratic, and cubic), the possibility of estimating toughness as a function of apparent density, compression parallel to grain strength, and modulus of rupture in static bending. Thirty-six Brazilian tropical wood species from south of Roraima, Mato Grosso do Sul, and north and northeast of Mato Grosso were tested. Our results showed the significance and representativeness of all...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Apparent density; Tropical wood species; Modulus of elasticity; Compression parallel to grain strength; Toughness.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200232

Relação de variáveis ambientais em baias cobertas com polietileno e desempenho da rã-touro (Rana catesbeiana)
Provedor de dados: 70
Autores: Teodoro,Sônia M.; Chaves,Modesto A.; Escobedo,João F.; Agostinho,Cláudio A.
Este trabalho visou a relacionar variáveis ambientais em instalação para criação de rãs, com cobertura de polietileno e baias construídas usando material alternativo, com o desempenho de rãs-touro (Rana catesbeiana). No interior das baias, foram medidas as temperaturas do piso, do ar ambiente (bulbo seco), de bulbo úmido, globo negro e da água do reservatório. Foram utilizados 60 animais por baia e três baias por galpão. As variáveis de desempenho estudadas foram peso vivo, ganho de peso e conversão alimentar. Nas condições experimentais, quando a temperatura do ar atingiu valores abaixo de 10 ºC ou superiores a 40 ºC, houve diminuição no consumo de ração pelos animais. Concluiu-se que o estresse predominante, neste tipo de estrutura, para as condições...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência; Instalações zootécnicas; Índices bioclimáticos.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100006

Monitoring of mechanical sugarcane harvesting through control charts
Provedor de dados: 70
Autores: Voltarelli,Murilo A.; Silva,Rouverson P. da; Zerbato,Cristiano; Paixão,Carla S. S.; Tavares,Tiago de O.
ABSTRACT Statistical process control in mechanized farming is a new way to assess operation quality. In this sense, we aimed to compare three statistical process control tools applied to losses in sugarcane mechanical harvesting to determine the best control chart template for this quality indicator. Losses were daily monitored in farms located within Triângulo Mineiro region, in Minas Gerais state, Brazil. They were carried over a period of 70 days in the 2014 harvest. At the end of the evaluation period, 194 samples were collected in total for each type of loss. The control charts used were individual values chart, moving average and exponentially weighted moving average. The quality indicators assessed during sugarcane harvest were the following loss...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Quality; Agricultural mechanization; Moving average; EWMA.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601079

Uso de ardósia na construção de celas de maternidade: I - efeito sobre o ambiente e comportamento de suínos
Provedor de dados: 70
Autores: Castro,Jaqueline de O.; Campos,Alessandro T.; Ferreira,Rony A.; Yanagi Júnior,Tadayuki; Tadeu,Hugo C.
O presente trabalho teve o objetivo de avaliar o uso da ardósia na construção de celas de maternidade, sendo monitoradas 12 matrizes e 139 leitões em celas confeccionadas de alvenaria e ardósia (tratamentos). Imagens digitais foram avaliadas por meio de dois etogramas. As variáveis ambientais foram registradas às 9 h e 15 h. O desempenho dos leitões foi determinado pelo peso ao nascimento e à desmama, ganho de peso diário e final. Na cela de alvenaria, os leitões passaram menos tempo mamando (25,62%) e mais no escamoteador (38,91%) que aqueles mantidos na cela de ardósia (29,22% mamando e 24,90% no escamoteador). As variáveis ambientais e os índices de conforto mostraram que o microclima na cela de ardósia apresentou-se mais confortável aos leitões,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ardósia; Comportamento animal; Instalações para suínos; Material de construção; Suinocultura.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300006

COMPOSTING PROCESS IN THE PRODUCTION OF LETTUCE SEEDLING SUBSTRATES: EFFECT OF COVERING AND TURNING FREQUENCY
Provedor de dados: 70
Autores: Ripp,Paula G.; Gusmão,Ana P.; Lorin,Higor E. F.; Costa,Mônica S. S. de M.; Edwiges,Thiago.
ABSTRACT The composting of waste from a broiler chicken production chain (BCPC) promotes the mitigation of environmental impacts and allows the commercialization of compost as an agricultural input. Both the characteristics and the potential for use of the final compost depends on the operational conditions during composting. The objective of this study was to evaluate the use of organic compounds generated from composting BCPC residues and the pruning debris of urban trees in the germination and initial growth of lettuce seedlings. Six organic substrates obtained under different coverage conditions (presence and absence) and number of turns (8, 12, and 16) were evaluated using the germination index (IG) and Dickson quality index (DQI) for the production...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environmental conditions; Leaching; Seed germination index; Dickson quality index.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500562

Modelagem para a estimativa da orientação de linhas de plantio de cafeeiros
Provedor de dados: 70
Autores: Oliveira,Klerisson M. G.; Carvalho,Luiz G. de; Lima,Luiz A.; Gomes,Raphaela C. C.
A quantidade de radiação solar interceptada por uma cultura é uma importante variável meteorológica que determina o crescimento e o desenvolvimento de uma cultura agrícola e, dentre os sistemas de produção, a orientação das linhas de plantio poderá ser um componente bastante relevante quanto à interceptação da radiação solar direta (Rd) em ambas as faces. Portanto, este trabalho propõe como objetivo um modelo para recomendar a orientação adequada das linhas de cafeeiro na implantação, baseando-se naquela a proporcionar uma uniformidade na quantidade de Rd interceptada e acumulada durante o ciclo agrícola da cultura, em ambas as faces da linha de plantio. Para o teste do modelo, foram coletados dados de produção em uma área experimental de café irrigado por...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Café; Sistema de cultivo; Radiação solar.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200009

Comportamento de um motor de ignição por compressão trabalhando com óleo Diesel e gás natural
Provedor de dados: 70
Autores: Schlosser,José F.; Camargo,Miguel N.; Machado,Paulo R. M.
A previsível escassez de petróleo aliada a uma consciência ecológica está levando pesquisadores a procurar novas fontes de energia e processos de combustão mais eficientes e menos poluentes. Entre os combustíveis menos poluentes está o gás natural, cujo consumo aumenta ano a ano. Os motores de combustão interna são transformadores de energia que têm baixa eficiência de conversão. Este trabalho avaliou um motor Diesel, bicombustível, movido a Diesel e gás natural. Nesse motor, a energia provém, basicamente, da combustão do gás natural. O Diesel tem a função de produzir o início da combustão do gás, que é o combustível principal. Assim, haverá uma substituição parcial de óleo Diesel por gás natural, aumentando o rendimento da combustão. Inicialmente, foi...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Motor bicombustível; Motor Diesel; Gás natural.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300026

SHADING LEVELS AND PLANT GROWTH REGULATOR FOR FORMATION OF SCHIZOLOBIUM AMAZONICUM COMPACT SEEDLINGS
Provedor de dados: 70
Autores: Binotti,Eliana D. C.; Binotti,Flávio F. da S.; Lucheti,Bruna Z.; Costa,Edilson; Pinto,Adriana H.
ABSTRACT Paricá (Schizolobium amazonicum) can be used for rehabilitation of degraded lands, timber manufacturing markets. However, for its planting, high-quality seedlings should be used. Thus, this study aimed to evaluate the effect of different types of paclobutrazol (PBZ) application and two shading levels on high-quality seedling production. As there was no replication of cultivation environments, we considered each one of them as an experiment. For each environment (35 and 50% shading screen), a completely randomized design was adopted, testing combinations of two types of PBZ application (direct seed immersion in 0.005% PBZ solution; substrate hydration with 0.005% PBZ solution; and 50% seed hydration and 50% substrate hydration; plus, a control),...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Protected cultivation; Plant environment; High-quality seedlings; Plant growth reducer; Schizolobium amazonicum.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500586

ELECTRICITY GENERATION FROM BIOGAS ON SWINE FARM CONSIDERING THE REGULATION OF DISTRIBUTED ENERGY GENERATION IN BRAZIL: A CASE STUDY FOR MINAS GERAIS
Provedor de dados: 70
Autores: Antônio,Adriano da S.; Oliveira Filho,Delly; Silva,Samuel C. da.
ABSTRACT The objective of this study was to analyze the feasibility of using agricultural waste from a swine farm to produce biogas, which can be used to generate electricity. For this purpose, the waste production potential was evaluated to determine the biogas production capacity of the farm. This measurement allowed scaling the size of the generator used to the electricity production to meet the needs of the farm as well as surplus electricity. The surplus electricity may be used on the farm when the generator is under maintenance or the electricity consumption is larger than the energy generated. This process is regulated by Normative Resolutions 482 and 687 in Brazil. The results of the analysis of the net present value, internal return rate, payback...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biodigesters; Normative Resolution 482; Swine; Energy credits; Economic viability.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400518

Identificação e avaliação de variáveis críticas no processo de produção da cana-de-açúcar
Provedor de dados: 70
Autores: Campos,Cassiano M.; Milan,Marcos; Siqueira,Luiz F. F.
A cana-de-açúcar é uma das culturas mais importantes economicamente no Brasil, apresentando para os próximos anos perspectiva de expansão da área cultivada. Em razão do aumento da demanda, faz-se necessária a manutenção e o incremento da produtividade no campo, otimizando, assim, os recursos já disponibilizados. O aprimoramento das operações agrícolas envolvidas na produção é uma das alternativas para o aumento da produtividade. É necessário, por questões operacionais e custos envolvidos, identificar aquelas operações de maior importância e estabelecer os padrões a serem atendidos pelas mesmas. Para tanto, o objetivo deste trabalho foi identificar e avaliar as variáveis críticas presentes no processo de produção da cana-de-açúcar. O trabalho foi...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanização; FMEA; Capacidade do processo.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300016

Biodigestão anaeróbia dos resíduos da produção avícola: cama de frangos e carcaças
Provedor de dados: 70
Autores: Orrico Júnior,Marco A. P.; Orrico,Ana C. A.; Lucas Júnior,Jorge de.
O propósito deste trabalho foi avaliar a produção de biogás, bem como os potenciais de produção e a qualidade do biofertilizante obtido com a biodigestão anaeróbia dos resíduos cama de frangos e carcaças de aves pré-compostados. Para tanto, foram pré-compostados cama de frango e carcaças de aves mortas em uma composteira durante um período de 60 dias, período necessário para que ocorresse decomposição prévia das carcaças e assim fosse possível manipular o material para abastecer os biodigestores. Após este período, o material foi utilizado para abastecer os biodigestores batelada de campo com capacidade de 60 litros de material em fermentação. Para o processo de biodigestão anaeróbia, foram efetuadas análises dos teores de sólidos totais (ST), sólidos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Metano; Dejeto; Meio ambiente.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300018

Uso de análise multivariada na classificação das fontes hídricas subterrâneas da bacia hidrográfica do Salitre
Provedor de dados: 70
Autores: Brito,Luiza T. de L.; Silva,Aderaldo de S.; Srinivasan,Vajapeyam S.; Galvão,Carlos de O.; Gheyi,Hans R.
Este estudo teve por objetivo identificar as variáveis responsáveis pela maior variabilidade da qualidade das águas subterrâneas da bacia hidrográfica do Rio Salitre - BA, e detectar as fontes que apresentam características semelhantes, visando a subsidiar medidas de monitoramento e gestão da qualidade das águas da bacia. Para isso, foram utilizadas técnicas de análise multivariada referente à análise fatorial em componentes principais e de agrupamento. A análise fatorial permitiu agrupar as variáveis em três fatores principais que explicaram 86,99%; 72,08% e 68,33% da variância total acumulada em 1984 e 2001, nos períodos de chuvas e sem chuvas, respectivamente. As variáveis priorizadas estão relacionadas com a salinidade das águas. Assim, medidas de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Impactos ambientais; Análise fatorial; Cluster.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100005

EVATUATION SYSTEM OF EXHAUST FANS USED ON VENTILATION SYSTEM IN COMMERCIAL BROILER HOUSE
Provedor de dados: 70
Autores: Silva,Wagner; Moura,Daniella; Carvalho-Curi,Thayla; Seber,Rogério; Massari,Juliana.
ABSTRACT: This study aim to develop a system, called FANS-N, for evaluation the exhaust fans in the ventilation system of broiler facilities. The system is divided into: 1) Mechanical Structure - consisting of two stepper motors for positioning a anemometer sensor in the vertical and horizontal coordinates; 2) Electronic Interface - control of the anemometer positioning and record data of wind speed; 3) Control Programming Module – accountable for the cursor movement, measurement and record the wind speed data with the anemometer at predetermined points; and 4) Analysis Programming Module - responsible for the interpretation of wind speed values at each point. The software uses artificial neural networks (Multi-Layer Perceptron) for images analyses of data...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Broiler; Neural network; Ventilation systems; Air flow.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500887

Water distribuition characteristics and soil loss of LEPA Quad-Spray emitter nozzles
Provedor de dados: 70
Autores: Ribeiro,Moises S.; Lima,Luiz A.; Colombo,Alberto; Caldeira,Ana C. D. M.; Faria,Fabio H. de S.
The objective of this study was to characterize water application rate, water application pattern width, flow rate, water distribution uniformity and soil loss caused by nozzles of the Low Energy Precision Aplication (LEPA) type Quad-Spray emitter. The study was carried out at the Hydraulic and Irrigation Laboratory of the Department of Engineering at the Federal University of Lavras, in Lavras, state of Minas Gerais - MG, Brazil. Twenty-two (22) LEPA Quad-Spray emitter nozzles were evaluated, with nozzle diameter ranging from 1.59 to 9.92 mm. The experimental design used was entirely randomized, with three replications.Increasing values of nozzle flow rate ranging from 77.44 up to 3,044 L h-1, were obtained with increasing nozzle diameter sizes....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Technical characteristics of the Quad-Spray; Resizing of nozzles; Erosive impact.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200002

Pressure compensating microsprinklers using microtube as a flow controller
Provedor de dados: 70
Autores: Almeida,Alexsandro C. dos Santos; Almeida,Ceres D. G. C. de; Botrel,Tarlei A.; Frizzone,José A.
ABSTRACT Microsprinkler non-pressure compensating nozzles usually show water flow variation along the lateral line. This study aimed at adapting microtubes into non-compensating system of microsprinklers previous installed in the field, as a self-compensated nozzle, to improve the flow uniformity along the lateral line. Microtubes were adapted to three types of commercial microsprinklers. Tests were conducted, both in the laboratory and in field, to evaluate the microsprinkler performance at four different flows (40, 50, 60 and 70 L h-1) under pressure head range from 75 to 245 kPa. Nozzles presented coefficient of flow-rate variation (CVq) lower than 5.5% and distribution uniformity (DU) greater than 95%, which are classified as excellent. The original...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Microtube nozzles; Micro-irrigation; Lateral design.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100036

Sistema com aeração, decantação e filtragem para a melhoria da qualidade de água em irrigação localizada
Provedor de dados: 70
Autores: Lemos Filho,Marco A. F.; Zanini,José R.; Silva,Elcides R. S. da; Cazetta,Jairo O.; Ferraudo,Antônio S.
A qualidade da água é muito importante para irrigação por gotejamento, pois ela escoa por pequenos bocais dos emissores, podendo ocorrer obstrução devido à deposição dos sólidos em suspensão. Portanto, antes da instalação do projeto, devem-se avaliar parâmetros de qualidade da água, para adotar medidas preventivas, evitando o risco de entupimento do sistema. Este trabalho teve como objetivo avaliar um sistema composto por aeradores com aspersores, sobre leito de pedra, para a precipitação dos íons Fe+2e Mn+2 em tanque de decantação, e um conjunto de filtragem composto por três filtros de areia e um de disco, em sistema de irrigação localizada. O trabalho foi realizado na Fazenda Alvorada, no município de Nova Granada - SP, no período de março a outubro de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Análises físicas e químicas de água; Tratamento de água; Precipitação dos íons Fe+2e Mn total.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300011

Análise de agrupamento da variabilidade espacial da produtividade da soja e variáveis agrometeorológicas na região oeste do Paraná
Provedor de dados: 70
Autores: Araújo,Everton C. de; Uribe-Opazo,Miguel A.; Johann,Jerry A.
O presente trabalho realizou uma análise de agrupamentos espacial por meio da estatística multivariada, no intuito de investigar a relação entre a produtividade da soja e as seguintes variáveis agrometeorológicas: precipitação pluvial, temperatura média do ar, radiação solar global e índice local de Moran (LISA) da produtividade. O estudo foi realizado com os dados das safras dos anos agrícolas de 2000/2001 a 2007/2008 da região oeste do Estado do Paraná. A identificação do número adequado de clusters para cada ano-safra foi obtida utilizando a minimização de desvios. O estudo mostrou a formação de grupos de municípios utilizando as similaridades das variáveis em análise. A análise de agrupamento foi um instrumento útil para melhor gestão das atividades de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Estatística espacial de área; Similaridade espacial; Estatística multivariada.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400018

HYDROGEN PRODUCTION AND PERFORMANCE OF ANAEROBIC FIXED-BED REACTORS USING THREE SUPPORT ARRANGEMENTS FROM CASSAVA STARCH WASTEWATER
Provedor de dados: 70
Autores: Torres,Douglas G. B.; Lucas,Shaiane Dal' Maso; Andreani,Cristiane L.; Carvalho,Karina Q. de; Coelho,Silvia R. M.; Gomes,Simone D.
ABSTRACT Fixed-bed reactors have been considered promise alternatives for hydrogen production due to their simple construction and increase in the biomass retention. The purpose of this study was to investigate the biological production of hydrogen in anaerobic fixed-bed reactors with cassava starch wastewater used as substrate. Different support materials and arrangements of fixed-bed were used to evaluate the biological production of hydrogen in anaerobic continuous fixed-bed reactors, with cassava starch wastewater as substrate - recycled low-density polyethylene scraps, in packed bed (R1), recycled low-density polyethylene cylinders, in ordained bed (R3) and bamboo stems, in vertical arrangement (R2 and R4). In R1 the initial pH was adjusted for 6.0,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bio-energy; Fermentative processes; Bamboo; Polyethylene; Agro-industrial effluent.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100160

COMPUTATIONAL FLUID DYNAMICS (CFD) APPLICATION FOR VENTILATION STUDIES IN BROILER HOUSES
Provedor de dados: 70
Autores: Curi,Thayla M. R. de C.; Moura,Daniella J. de; Massari,Juliana M.; Mesquita,Márcio; Pereira,Danilo F.
ABSTRACT With the recent increase in the number of acclimatized broiler houses in Brazil, design and adaptation of facilities to withstand the tropical weather conditions enabling the maintenance of ideal conditions without increasing costs have been major challenges. The aim of this study was to evaluate the ventilation system in solid-wall broiler houses using computational fluid dynamics (CFD). The research was carried out in the city of Amparo - SP (Brazil). The facility consisted of a broiler house enclosed by masonry sidewalls with tunnel ventilation equipped with exhaust fans (air outlet) and cooling pads (air inlet). The following variables were collected: wind speed and dry bulb temperature over 27 equidistant points inside the house at bird...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Broiler house; Computational modeling; Environmental control; Poultry; Thermal comfort.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100001

Sistema computacional para aquisição automática e disponibilização de dados meteorológicos
Provedor de dados: 70
Autores: Sousa,Marques M. de; Drumond,Luis C. D.; Naldi,Murilo C.
O objetivo deste artigo é apresentar uma metodologia de automatização do processo de coleta e disponibilização de dados meteorológicos. Esta metodologia faz o uso de uma linguagem de scripts para definir as ações a serem executadas desde a coleta dos dados na estação climática, passando pelo seu processamento e finalizando com o envio dos dados processados para publicação em um site na internet. Os dados meteorológicos temperatura, umidade, velocidade do vento, chuva, radiação e evapotranspiração disponibilizados no site permitem aos produtores e pesquisadores analisar as variações climáticas, auxiliando assim em tomadas de decisão mais eficientes. O resultado obtido é o fornecimento sem custos de informações importantes e de qualidade sobre o clima.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Automatização de sistemas; Meteorologia; Scripts.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300606

Automação em sistema de irrigação tipo pivô central para economia de energia elétrica
Provedor de dados: 70
Autores: Moraes,Maria J.; Oliveira Filho,Delly; Mantovani,Everardo C.; Monteiro,Paulo M. B.; Mendes,André L. C.; Damião,Jorge H. A. C.
A irrigação é de grande importância para a produção de alimentos, e acredita-se que ela seja responsável por boa parte da produção agrícola mundial, mas é grande consumidora de água doce, principalmente na irrigação por aspersão. O objetivo desta pesquisa é avaliar a redução do custo da energia elétrica para irrigação, por meio de sistema automatizado de controle de velocidade em pivô central instalado em encosta. Para tal, foi dimensionado um pivô central com raio de 56,4 metros com 10 emissores com pressão de serviço de 137,8 kPa, representando uma área irrigada de 1,3 ha, e a lâmina bruta de irrigação adotada foi de 10 mm dia-1. Posteriormente, realizaram-se cálculos para determinar as pressões em cada emissor, para as condições de 0; 10; 20 e 30% de...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Motores elétricos; Bombas; Automação em pivô central.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600005

HYDROPONIC CULTIVATION OF CORIANDER USING FRESH AND BRACKISH WATERS WITH DIFFERENT TEMPERATURES OF THE NUTRIENT SOLUTION
Provedor de dados: 70
Autores: Silva,Mairton G. da; Soares,Tales M.; Gheyi,Hans R.; Oliveira,Mateus G. B. de; Santos,Caroline C. dos.
ABSTRACT A large number of studies on salinity in hydroponic systems have been carried out, but few of them have evaluated the interaction between salinity and nutrient solution temperatures. Two experiments were carried out in a randomized block design from January to February (Experiment I) and June to July 2018 (Experiment II). Experiment I consisted of treatments with five combinations, as follows: unheated (control) and heated nutrient solution (NS) at a temperature of 32°C using fresh water with an electrical conductivity (ECw) of 0.3 dS m−1, and unheated and heated NS at temperatures of 30 and 32°C using brackish water with an ECw of 6.5 dS m−1 in the main plots, with two coriander cultivars (Tabocas and Verdão) in the subplots, which were grown in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coriandrum sativum L. abiotic stress shoot fresh matter hydroponics; Salinity.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600674

Performance during post-harvest storage of banana cv. 'prata', 'maçã' and 'nanica' exposed to physical and chemical treatments
Provedor de dados: 70
Autores: Coelho,Silvia R. M.; Werner,Simone S.; Poncio,Anna P.; Ferreira,Letícia; Nóbrega,Lúcia H. P.
Banana is the most consumed fruit in the world and Brazil is the second largest producer. Despite its global position, Brazil has an average of 40% losses during the post-harvest period. So, this experiment aimed at evaluating the efficiency of post-harvest treatments to improve the storage of banana cultivars cv. 'Prata', 'Maçã' and 'Nanica'. The fruits were acquired at CEASA with green peel, and were submitted to six different treatments: T- immersion in drinking water for 3 minutes (control), H3 - hot water (50 °C for 3 minutes), H8 - hot water (50 °C for 8 minutes), HP - immersion in hypochlorite 0.2% for 3 minutes, OS - immersion in soybean oil 10% for 3 minutes, and OM - immersion in mineral oil 10% for 3 minutes. The fruits were stored at room...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Post-harvest loss; Ripening; Musa sp.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400011

Aplicação do modelo de pulsos retangulares de Bartlett-Lewis modificado para estimativa de eventos extremos de precipitação
Provedor de dados: 70
Autores: Back,Álvaro J.; Uggioni,Edison.
Este trabalho teve como objetivo avaliar a modelagem matemática da precipitação pluviométrica horária por meio do modelo de Bartlett-Lewis modificado com seis parâmetros e sua aplicação para estimativa de eventos extremos. Foi utilizada a série de dados pluviográficos do período de outubro de 1980 a dezembro de 2007, da estação meteorológica de Urussanga - SC (latitude 28,31º S, longitude 48,19º W). Foram ajustados os parâmetros mensais do modelo para a precipitação em intervalos de 1 hora, 30 min, 15 min, 10 min e 5 min. Para cada duração estudada, foram simuladas séries com 100 anos de dados. Pode-se concluir que o ajuste dos parâmetros do modelo de Bartlett-Lewis modificado possibilita a simulação de chuvas preservando as propriedades estatísticas da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Probabilidade; Modelos estocásticos; Chuvas intensas.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600005

Eficiência de aeração e consumo de oxigênio no tratamento de água residuária do processamento dos frutos do cafeeiro em sistema de aeração em cascata
Provedor de dados: 70
Autores: Matos,Antonio T.; Eustáquio Júnior,Valdeir; Matos,Mateus P. de.
RESUMO Objetivou-se, com a realização deste trabalho, determinar a eficiência de aeração e a capacidade do sistema de aeração em cascata em remover matéria orgânica da água residuária do processamento dos frutos do cafeeiro (ARC). O sistema de aeração foi constituído por cascata com 4,14 m de altura, distribuída em 23 degraus (altura, largura e comprimento de 0,18; 0,32 e 0,60 m, respectivamente), reservatório para a recepção/detenção da ARC escoada, por três horas, e reservatório de distribuição, de onde era recirculada no sistema. Durante a fase experimental, o sistema de tratamento ficou em operação por trinta dias, sendo a ARC recirculada três vezes por dia, numa vazão constante de 1 L s-1, e substituída a cada dez dias. A cada recirculação, amostras...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tratamento aeróbio; Resíduos orgânicos; Frutos do cafeeiro.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500941

Watermelon fertigation with electrical conductivity and ph monitoring in the soil solution
Provedor de dados: 70
Autores: DA SILVA JÚNIOR,MANOEL J.; VIANA,PAULA C.; MEDEIROS,JOSÉ F. DE; LIMA,JOÃO G. A.; TARGINO,ANA J. DE O.
ABSTRACT In the olericulture, in general, is practiced intensive fertilization, which creates a risk of salinization and change of high pH, ​​which if not well monitored can cause production losses, excessive spending on fertilizers and environmental contamination. We developed this study with the aim of controlling fertigation on watermelon through the behavior of the electrical conductivity (EC) and pH in the soil solution obtained through porous ceramic cups extractors. The EC and pH values ​​were corrected by the current soil moisture for the moisture field capacity, due to different moisture values ​​at the time of extraction. The monitoring comprised 19 assessments during 80 days of cultivation. We can control the pH and EC of the soil and maintain...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrullus lanatus; Fertilization; Solution extractors; Salinity.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400622

SWINE WASTEWATER: IMPACTS ON SOIL, PLANT, AND LEACHATE
Provedor de dados: 70
Autores: Rosa,Danielle M.; Sampaio,Silvio C.; Pereira,Pâmela A. M.; Mauli,Márcia M.; Reis,Ralpho R. Dos.
ABSTRACT: The use of animal-origin residues as a nutrient source without prior and proper investigations on their positive and negative impacts can affect the quality of agricultural soils and the environment into which they are inserted. In this sense, the aim of this study was to assess the impact of swine wastewater and mineral fertilization application on soil, soybean crop, and leachate characteristics. The experiment was developed in drainage lysimeters under field conditions. The following doses of swine wastewater were applied: 0, 100, 200, and 300 m3 ha−1, both with and without mineral fertilization. Swine wastewater application contributed to increasing soil nutrients; however, a special attention should be paid to Cu+ and Zn+ accumulation, which...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pig slurry; Soil fertility; Leachate; Water reuse.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500928

Positioning of fertilizer in corn sowing
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Justino,Altair; Frare,Ivo; Gomes,Jorge N.; Garcia,Luiz C.
The aim of this study was to determine whether the form of placing the fertilizer by the planter during the sowing under mulch in the no till system affects the yield of corn. The treatments consisted of placing the fertilizer during the seeding 0.05 m below and beside the seed, in front of the cutting blade and without fertilizer, in 03 farms during 03 cropping years. The experimental design at each farm was the randomized block, with 08 repetitions, whose plots had 30 m² each. The initial population and yield components were evaluated. Under the experimental conditions it is concluded that base fertilization can affect the yield. Fertilizer placement can affect the initial stand, but not the yield.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tillage; Seeding fertilizer; Yield components.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600010

Experimental dryer design for agricultural products
Provedor de dados: 70
Autores: GONELI,ANDRÉ L. D.; MARTINS,ELTON A. S.; JORDAN,RODRIGO A.; GEISENHOFF,LUCIANO O.; GARCIA,RENATO T.
ABSTRACT This study consisted of designing and building an experimental dryer that allows working with different temperatures and velocities of the air, aiming to perform studies on thin- and thick-layer drying of agricultural products. The project was divided into three stages: heat source designing, dryer geometric parameters, and fan selection to meet operational demand. Heating was made by a set of six electrical resistances totaling 12 kW and the drying bed in thin layer was composed of two trays with diameter of 0.20 m. Operational demands were met using a centrifugal fan with a power rating of 735.5 W. The used methodology was able to size the experimental dryers for thin- and thick-layer drying working at distinct temperatures and air velocities.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thin layer; Electrical resistance; Temperature; Air velocity.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500938

Proposta metodológica para avaliação de controlador automático de seções e pulverização
Provedor de dados: 70
Autores: Reynaldo,Étore F; Molin,José P.
Na aplicação de produtos fitossanitários, a utilização de equipamentos que controlam automaticamente as seções da barra e a pulverização já é realidade; entretanto, ainda não há resultados que demonstrem a sua eficácia. Por esse motivo, este trabalho teve por finalidade desenvolver uma metodologia para a avaliação de um equipamento que controla automaticamente as seções e a pulverização. Avaliou-se um controlador automático de seções e pulverização de mercado, e, para tanto, foram utilizados três níveis de acurácia do sinal de GPS (algoritmo interno, SBAS e RTK), três ângulos para a simulação de entrada e saída da barra de pulverização em relação à borda do talhão (0; 45 e 60º ) e três velocidades de trabalho (1,66; 5,00 e 8,33 m s-1). A metodologia...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Aplicação de produtos fitossanitários; Sistemas eletrônicos.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100011

Uniformidade de distribuição superficial e subsuperficial de água e de água residuária de suinocultura com irrigação por aspersão em malha
Provedor de dados: 70
Autores: Drumond,Luís C. D.; Zanini,José R.; Fernandes,André L. T.; Rodrigues,Guilherme P.
A irrigação por aspersão em malha está sendo bastante utilizada em café, pastagem, cana forrageira e capineiras, por ser sistema de baixo custo, de fácil instalação e manejo e por permitir fertirrigação com água residuária de suinocultura e de bovinocultura. Para determinar a uniformidade de distribuição de água e de água residuária de suinocultura nesse sistema de irrigação, foi conduzido um experimento na Fazenda-Escola da Universidade de Uberaba, empregando-se pluviômetros eqüidistantes, entre quatro aspersores de duas linhas laterais. O coeficiente de uniformidade de Christiansen (CUC) e o coeficiente de uniformidade de distribuição (CUD) foram superiores aos valores mínimos recomendados, mesmo com 200 m³ de água residuária de suinocultura por hectare...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água residuária; Tubos enterrados; Coeficiente de uniformidade.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200009

Evaluation of roof slope and exposure with different roofing materials in reduced models of animal production facilities in spring and summer
Provedor de dados: 70
Autores: Melo,Thiago V.; Furlan,Renato L.; Milani,Adhemar P.; Buzanskas,Marcos E.; Mota,Diego A.
The present study was conducted at the Department of Rural Engineering and the Department of Animal Morphology and Physiology of FCAV/Unesp, Jaboticabal, SP, Brazil. The objective was to verify the influence of roof slope, exposure and roofing material on the internal temperature of reduced models of animal production facilities. For the development of the research, 48 reduced and dissemble models with dimensions 1.00 × 1.00 × 0.50 m were used. The roof was shed-type, and the models faced to the North or South directions, with 24 models for each side of exposure. Ceramic, galvanized-steel and fibro tiles were used to build the roofs. Slopes varied between 20, 30, 40 and 50% for the ceramic tile and 10, 30, 40 and 50% for the other two. Inside the models,...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Ambience; Heat; Shed.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600001

Compostagem dos resíduos da produção avícola: cama de frangos e carcaças de aves
Provedor de dados: 70
Autores: Orrico Júnior,Marco A. P.; Orrico,Ana C. A.; Lucas Júnior,Jorge de.
O propósito deste trabalho foi avaliar a eficiência do processo de compostagem no tratamento e na reciclagem dos resíduos cama de frangos e carcaças de aves. Para tanto, o material foi disposto na composteira em camadas alternadas de cama de frango por 60 dias (pré- -compostagem), tempo necessário para que ocorresse a decomposição prévia das carcaças e assim fosse possível manipular o material e confeccionar as leiras de compostagem. Posteriormente, o material pré-compostado foi transferido para o pátio de compostagem, onde foram avaliados: peso, número mais provável (NMP) de coliformes totais e termotolerantes, sólidos totais (ST), temperatura, pH e os teores de N, P, K, Ca, Na, Mg, Fe, Zn e Cu. Foram observadas reduções elevadas de ST e principalmente de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Composto; Volatilização do nitrogênio; Leiras.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300017

Erratum
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500952

Desempenho de um pulverizador pneumático costal motorizado sob diferentes condições
Provedor de dados: 70
Autores: Gadanha Júnior,Casimiro D.; Costa,Marco A. F. da; Milan,Marcos.
O objetivo do trabalho foi avaliar a uniformidade de vazão de um pulverizador pneumático costal motorizado, utilizado no controle do mosquito vetor da dengue, sob várias condições operacionais de aplicação. O experimento foi planejado como um delineamento inteiramente casualizado, no esquema fatorial 2 x 7, com cinco repetições, sendo os fatores de variação dois diâmetros de orifício do disco dosador e sete ângulos de aplicação em relação ao plano horizontal. Foi avaliado também o efeito das pressões sobre a vazão por meio dos testes de Pearson. A interação dos fatores diâmetro do orifício do disco dosador e ângulo de aplicação foi significativa para a vazão. O disco dosador com diâmetro de 0,42 mm apresentou maior uniformidade entre as vazões médias,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aedes aegypti; Controle químico; Pulverizador.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300023

Spatial variability of yield and other parameters associated with pear trees
Provedor de dados: 70
Autores: Konopatzki,Marcia R. S.; Souza,Eduardo G.; Nóbrega,Lúcia H. P.; Uribe-Opazo,Miguel A.; Suszek,Grazieli.
In the last few years, precision agriculture has become commonly used with many crops, particularly cereals, and there is also interest in precision horticulture. Pear is a seasonal fruit and well appreciated by Brazilian people, although it is mostly imported. Brazilian farmers are nowadays trying to increase pear production. Thus, this research aimed at mapping the yield of pear trees in order to study the spatial variability of yield as well as its comparison with spatial variability of soil and plant attributes. The experimental field had 146 pear trees, variety 'Pêra d'água', distributed on a 1.24 ha. Four harvests were performed according to the fruit ripening and from each tree; only the ripe fruits were harvested. In each harvest, all the fruits...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Thematic maps; Horticulture.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200018

ENERGY PERFORMANCE IN DISC HARROWING OPERATION IN DIFFERENT GRADIENTS AND GAUGES
Provedor de dados: 70
Autores: Oiole,Yasser A.; Kmiecik,Leonardo L.; Parize,Guilherme L.; Silva,Thiago X. da; Jasper,Samir P.
ABSTRACT The operational performance of the agricultural tractor can be increased by adjusting parameters such as tire inflation pressure, axle mass distribution and gauge opening, which is a very divergent factor in controlled-traffic production. The objective of the experiment was to measure the energy performance of a 93 kW agricultural tractor in intermediate grading operation in two slopes (flat and sloping) and three gauge configurations (closed, intermediate and open) in mobilized soil. Energy performance was determined from the following parameters: slip, engine speed, actual effective speed, hourly and specific fuel consumption; strength, power and performance on the drawbar. Turbo pressure and temperature monitoring was also performed at six...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuel consumption; Operating yield; Controlled trafic.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600769

Estimation of climatological water deficit in an experimental watershed in the brazilian cerrado
Provedor de dados: 70
Autores: GOTARDO,JACKELINE T.; RODRIGUES,LINEU N.; GOMES,BENEDITO M.
ABSTRACT This study aimed to estimate the probability of climatological water deficit in an experimental watershed in the Cerrado biome, located in the central plateau of Brazil. For that, it was used a time series of 31 years (1982–2012). The probable climatological water deficit was calculated by the difference between rainfall and probable reference evapotranspiration, on a decennial scale. The reference evapotranspiration (ET0) was estimated by the standard FAO-56 Penman-Monteith method. To estimate water deficit, it was used gamma distribution, time series of rainfall and reference evapotranspiration. The adherence of the estimated probabilities to the observed data was verified by the Kolmogorov-Smirnov nonparametric test, with significance level...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gamma distribution; Penman-Monteith; Rainfall.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400631

Diagnóstico energético de rotas de escoamento do etanol da região Centro-Oeste do Brasil para exportação
Provedor de dados: 70
Autores: Bovolenta,Fábio C.; Biaggioni,Marco A. M.
RESUMO O grande desafio para o agronegócio nos próximos anos é a infraestrutura logística, uma vez que existem muitas dificuldades em escoar a produção. Para o escoamento do etanol, o País possui uma logística que abrange multimodais de transporte, terminais e vias que visam a fortalecer o corredor exportador. Assim, o presente trabalho analisou o fluxo energético, considerando rotas atualmente projetadas, em construção ou operantes, para o escoamento de etanol da região Centro-Oeste do Brasil (Aparecida do Taboado-MS) até o porto de São Sebastião (SP). Foram concebidas quatro rotas para a análise, contemplando a multimodalidade ou a unimodalidade, envolvendo os modais rodoviário, ferroviário, hidroviário e dutoviário. Foram utilizados fatores energéticos,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Logística de transporte; Biocombustível; Dutovia; Consumo energético.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300408

Manejo hídrico em viveiro e uso de hidrogel na sobrevivência pós-plantio de Eucalyptus urograndis em dois solos diferentes
Provedor de dados: 70
Autores: Saad,João C. C.; Lopes,Jane L. W.; Santos,Talita A. dos.
O trabalho teve como objetivo avaliar a sobrevivência do clone H13 de Eucalyptus urograndis sob dois manejos hídricos de viveiro, plantados em dois solos, com e sem a adição de polímero hidroabsorvente (hidrogel). O plantio foi realizado em vasos mantidos em estufa, com dois tipos de solo: um arenoso e outro argiloso. Cada vaso recebeu 2,5 L de solo, um litro de água e o hidrogel na proporção de 0,4 g vaso-1 (120 mL de gel). O delineamento experimental adotado foi o inteiramente casualizado, com três repetições. Os sintomas de estresse, nos vários níveis avaliados, sempre se manifestaram primeiro nas plantas no solo argiloso, de modo mais acentuado naquelas que foram mantidas sem estresse de água na fase de viveiro. Isso garantiu que as plantas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eucalipto; Polímeros hidroabsorventes; Irrigação.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300007

PEDOTRANSFER FUNCTION TO ESTIMATE THE SOIL STRUCTURAL “S” INDEX AND SPATIAL VARIABILITY IN AN OXISOL WITHIN A LIVESTOCK FARMING SYSTEM
Provedor de dados: 70
Autores: Tavanti,Renan F. R.; Montanari,Rafael; Panosso,Alan R.; Freddi,Onã da S.; Paz-González,Antonio.
ABSTRACT Various attributes are often required to build soil quality indicators. However, determining these attributes is time-consuming and requires several specific devices. Thus, it is desirable to develop indexes that express soil quality based on easily determined attributes. The objective of this study was to investigate the spatial variability of the S index and its correlation with other physical and chemical soil attributes to generate a pedotransfer function for estimating the S index. A georeferenced sampling mesh covering 1.4 ha and employing 71 points was installed. The soil samples were collected in 0.00–0.15 m and 0.15–0.30 m deep layers to determine the physical and chemical attributes. The results indicated that the S index was correlated...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil and water management; Geostatistics; Soil quality index; Stepwise procedures.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100034

MONITORING TRACTOR PERFORMANCE USING SHEWHART AND EXPONENTIALLY WEIGHTED MOVING AVERAGE CHARTS
Provedor de dados: 70
Autores: Voltarelli,Murilo A.; Paixão,Carla S. S.; Oliveira,Bruno R. de; Angelo,Eduardo P.; Silva,Rouverson P. da.
ABSTRACT Statistical process control has been widely used in agricultural operations for monitoring and improving process quality. This study aims to evaluate the Shewhart and exponentially weighted moving average (EWMA) control charts to monitor the performance of an agricultural tractor–planter set. The design is completely randomized based on the assumptions of statistical process control and comprises two treatments: day and night shift treatments. The data to assess the performance of the tractor–planter set are collected during the day and night shifts and used to evaluate the operating speed, motor rotation, engine oil pressure and water temperature, and hourly fuel consumption. The dataset comprised 40 samples compiled from the frontal monitor...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Statistical process control; Management operations; Agricultural mechanization.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100062

Indicadores de bem-estar baseados em reações comportamentais de matrizes pesadas
Provedor de dados: 70
Autores: Pereira,Danilo F.; Nääs,Irenilza de A.; Romanini,Carlos E. B.; Salgado,Douglas D.; Pereira,Gracely O. T.
Dada a importância da avicultura de corte para a economia brasileira, este trabalho buscou compreender e identificar novos indicadores de bem-estar inerentes ao animal que contribuíssem para o aumento da eficácia produtiva, estudando-se diferentes reações comportamentais de matrizes de frango de corte, em câmara climática. O experimento foi delineado como um Quadrado Latino 3x3x3, em que as variáveis temperatura do ar, ração e idade das aves foram controladas, sendo as aves de diferentes idades alojadas em boxes distintos. Foram feitas observações do comportamento das aves em dois horários do dia, sendo uma observação na parte da manhã e outra na parte da tarde, durante períodos de 15 minutos cada, por meio de câmeras de vídeo instaladas no teto da câmara...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avicultura; Imagens de vídeo; Bem-estar animal.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200003

Removal of nitrogen, phosphorus, copper and zinc from swine breeding waste water by bermudagrass and cattail in constructed wetland systems
Provedor de dados: 70
Autores: Fia,Ronaldo; Boas,Regina B. Vilas; Campos,Alessandro T.; Fia,Fátima R. L.; Souza,Edson G. De.
This work aimed to study the agronomic performance and capacity of nutrient removal by bermudagrass (Cynodon spp.) and cattail (Typha sp.) when grown in constructed wetlands systems (CWSs) of vertical and horizontal flow, respectively, used in the post-treatment of swine breeding wastewater (ARS). The average yield of dry matter (DM) of bermudagrass in sections of 60-day interval ranged from 14 to 43 t ha-1, while the cultivated cattail produced in a single cut after 200 days of cultivation between 45 and 67 t ha-1 of DM. Bermudagrass extracted up to 17.65 kg ha-1 d-1 of nitrogen, 1.76 kg ha-1 d-1 of phosphorus, 6.67 g ha-1 d-1 of copper and 54.75 g ha-1 d-1 of zinc. Cattail extracted up to 5.10 kg ha-1 d-1 of nitrogen, 1.07 kg ha-1 d-1 of phosphorus, 1.41...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Macronutrients; Micronutrients; Effluent treatment.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100013

Programa computacional para geração de séries sintéticas de precipitação
Provedor de dados: 70
Autores: Zanetti,Sidney S.; Pruski,Fernando F.; Moreira,Michel C.; Sediyama,Gilberto C.; Silva,Demetrius D.
Desenvolveu-se um programa computacional que permite a aplicação da metodologia para geração de séries sintéticas de precipitação desenvolvida por OLIVEIRA (2003). O desenvolvimento do aplicativo foi viabilizado pela elaboração de um algoritmo computacional em ambiente de programação "Borland Delphi 6.0". Os dados de entrada necessários são provenientes de banco de dados no formato padronizado pela Agência Nacional de Águas (ANA) com registros pluviométricos diários provenientes de estações meteorológicas. A partir dessas informações, o programa computacional é capaz de gerar séries sintéticas de precipitação diária contendo o total precipitado em milímetros, a duração do evento em horas, o tempo padronizado de ocorrência da intensidade máxima instantânea...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chuva; Gerador climático; Modelo computacional.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100011

PRODUCTIVE RESPONSES FROM BROILER CHICKENS RAISED IN DIFFERENT COMMERCIAL PRODUCTION SYSTEM - PART II: IMPACT OF CLIMATE CHANGE
Provedor de dados: 70
Autores: Lourençoni,Dian; Yanagi Junior,Tadayuki; Yanagi,Silvia de N. M.; Abreu,Paulo G. de; Campos,Alessandro T.
ABSTRACT Broiler chickens are homoeothermic animals, i.e., animals capable of maintaining their body temperature within quite narrow limits; therefore, climate change poses a great challenge to poultry. With this in mind, this research aims to evaluate the performance of broilers submitted to different commercial production systems and exposed to different future scenarios, taking into account the climate change trends. To achieve this objective, we developed and validated a fuzzy model able to predict the performance of a broiler as a function of enthalpy along its life stages. This model was developed and validated in part I of this article based on experimental data collected for one year in three aviaries: conventional, negative pressure, and dark...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Broiler industry; Artificial intelligence; Climate change; Fuzzy system.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100011

Modelagem de máquina pneumática recolhedora de frutos de café em terreiro usando análise por elementos finitos
Provedor de dados: 70
Autores: Magalhães,Anderson C.; Teixeira,Mauri M.; Couto,Sandra M.; Resende,Ricardo C. de.
Teve-se o objetivo de desenvolver um modelo matemático por meio de análise de elementos finitos, utilizando o programa computacional ANSYS®, versão 5.7, para otimizar o projeto de máquina recolhedora de frutos de café no terreiro. A modelagem da máquina foi realizada com base no levantamento das características aerodinâmicas dos frutos de café e da vazão de ar necessária para o transporte pneumático dos frutos. Foram obtidas, experimentalmente, as pressões estáticas nos dutos da máquina, sendo esses valores comparados com os resultados determinados pelo programa ANSYS, no intuito de validar o modelo. Com base nos resultados numéricos obtidos, concluiu-se que a modelagem desenvolvida apresentou resultados próximos aos determinados experimentalmente, obtendo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Máquina agrícola; Simulação; Projeto.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200017

Entupimento de gotejadores em função da aplicação de superfosfato simples e ácido nítrico
Provedor de dados: 70
Autores: Barros,Allan C.; Coelho,Rubens D.; Medeiros,Pedro R. F.; Melo,Ralini F. de; Barboza Júnior,Cícero R. A.; Dias,Carlos T. dos S.
O superfosfato simples (SS) é uma alternativa aos adubos fosfatados que são utilizados via fertirrigação, como o ácido fosfórico, que provoca acidificação do bulbo úmido no solo, e o monofosfato de amônio purificado, que apresenta maior preço. No entanto, não se conhece o efeito de tal adubo no funcionamento de emissores, principalmente nos gotejadores, nem se é possível controlar o entupimento por SS por meio de aplicações de ácido. Assim, desenvolveu-se este trabalho com o objetivo de avaliar a possibilidade da utilização do superfosfato simples via gotejamento, como alternativa ao uso de outros adubos fosfatados, e a tentativa de controle do entupimento utilizando ácido nítrico. O trabalho foi desenvolvido em bancada de ensaios de gotejadores,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adubos fosfatados; Gotejamento; Obstrução de emissores.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100007

Produtividade e qualidade de cana-de-açúcar cultivada em solo tratado com lodo de esgoto, vinhaça e adubos minerais
Provedor de dados: 70
Autores: Tasso Júnior,Luiz C.; Marques,Marcos O.; Franco,Ademir; Nogueira,Gustavo de A.; Nobile,Fábio O. de; Camilotti,Fábio; Silva,Alysson R. da.
O uso agrícola de resíduos orgânicos, de origem agrícola, urbana ou industrial, é uma interessante alternativa de disposição, permitindo a reciclagem de nutrientes (NPK) nos ecossistemas. Este trabalho avaliou o efeito da aplicação de lodo de esgoto como fonte de N e de vinhaça como fonte de K comparado ao uso de fontes minerais desses nutrientes sobre a produtividade e variáveis agroindustriais da cana-de-açúcar, por dois anos consecutivos (cana-planta e cana-soca). O experimento foi conduzido em Latossolo Vermelho-Amarelo distrófico típico, em Pontal - SP, e a variedade de cana-de-açúcar avaliada foi a SP 81-3250. Utilizou-se de esquema fatorial 3x2x2+1, ou seja, três tipos de resíduos (lodo de esgoto + KCl; vinhaça + uréia, e lodo de esgoto + vinhaça);...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum spp.; Adubação nitrogenada e potássica; Resíduos orgânicos.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100022

CALIBRATION AND VALIDATION OF THE SWAT HYDROLOGICAL MODEL FOR THE MUCURI RIVER BASIN
Provedor de dados: 70
Autores: Almeida,Rafael A.; Pereira,Silvio B.; Pinto,Daniel B. F.
ABSTRACT Hydrological models are becoming more and more widespread, mainly due to their capacity to simulate the impact of environmental changes on water resources. In this way, the aim of this study was to calibrate and validate the SWAT model for the soil and climatic conditions of the Mucuri River Basin, located in the Northeast region of the States of Minas Gerais, Brazil. The SWAT-CUP software module SUFI2 was used to analyze the sensitivity, calibration and validation of the model. The calibration was performed in an intermediate fluviometric station and the validation in five other located: three upstream, one downstream and one independent from the calibration point. It was evidenced for the study area that the parameters referring to the basic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydrological modeling; SWAT-CUP; Flow rate.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100055

Soil penetration resistance analysis by multivariate and geostatistical methods
Provedor de dados: 70
Autores: Medina,Cecilia; Camacho-Tamayo,Jesús H.; Cortés,César A.
The penetration resistance (PR) is a soil attribute that allows identifies areas with restrictions due to compaction, which results in mechanical impedance for root growth and reduced crop yield. The aim of this study was to characterize the PR of an agricultural soil by geostatistical and multivariate analysis. Sampling was done randomly in 90 points up to 0.60 m depth. It was determined spatial distribution models of PR, and defined areas with mechanical impedance for roots growth. The PR showed a random distribution to 0.55 and 0.60 m depth. PR in other depths analyzed showed spatial dependence, with adjustments to exponential and spherical models. The cluster analysis that considered sampling points allowed establishing areas with compaction problem...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compaction; Cluster analysis; Principal components; Andisol.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100010

Avaliação de circuito eletrônico para medição de temperatura em instalações agrícolas por meio da porta paralela de um computador
Provedor de dados: 70
Autores: Steidle Neto,Antonio J.; Zolnier,Sérgio.
Os sistemas de aquisição de dados de temperatura disponíveis comercialmente apresentam alto custo e grande complexidade operacional para a sua utilização em instalações agrícolas climatizadas. Este trabalho teve por objetivos propor, calibrar e validar um circuito eletrônico de baixo custo para a aquisição de dados de temperatura com base na freqüência de oscilação da tensão elétrica (0 a 5 V). O sensor empregado no circuito foi um termistor com resistência ômica de 10 kômega 25 ºC e coeficiente de temperatura negativo. O circuito eletrônico, conectado a um computador via porta paralela, foi calibrado por comparação com um termômetro-padrão de mercúrio em vidro. Após as medições, análises de regressão foram realizadas com os dados experimentais, gerando-se...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas de aquisição de dados; Sensores de temperatura; Instrumentação.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200001

Spatial variability of leaf wetness duration in a 'Niagara Rosada' vineyard
Provedor de dados: 70
Autores: Lulu,Jorge; Sentelhas,Paulo C.; Pedro Júnior,Mário J.; Pezzopane,José R. M.; Blain,Gabriel C.
Despite considerable efforts to develop accurate electronic sensors to measure leaf wetness duration (LWD), little attention has been given to studies about how is LWD variability in different positions of the crop canopy. In order to evaluate the influence of 'Niagara Rosada' (Vitis labrusca) grapevine structure on the spatial variability of LWD, the objective of this study was to determine the canopy position of the Â‘Niagara RosadaÂ’ table grape with longer LWD and its correlation with measured standard LWD over turfgrass. LWD was measured in four different canopy positions of the vineyard (sensors deployed at 45Âº with the horizontal): at the top of the plants, with sensors facing southwest and northeast (Top-SW and Top-NE), and at the grape bunches...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dew; Rain; Flat plate wetness sensor.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100011

Auger-type granular fertylizer distributor: matemathical model and dynamic simulation
Provedor de dados: 70
Autores: Garcia,Angel P.; Cappelli,Nelson L.; Umezu,Claudio K.
The objective of this study was to model mathematically and to simulate the dynamic behavior of an auger-type fertilizer applicator (AFA) in order to use the variable-rate application (VRA) and reduce the coefficient of variation (CV) of the application, proposing an angular speed controller θ' for the motor drive shaft. The input model was θ' and the response was the fertilizer mass flow, due to the construction, density of fertilizer, fill factor and the end position of the auger. The model was used to simulate a control system in open loop, with an electric drive for AFA using an armature voltage (V A) controller. By introducing a sinusoidal excitation signal in V A with amplitude and delay phase optimized and varying θ' during an operation cycle, it is...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Seeder fertilizer drill; Modeling; Precision agriculture.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100016

Obstruction of drippers as a result of application of moisturized whitewash in irrigation water
Provedor de dados: 70
Autores: Barboza Júnior,Cícero R. A.; Lelis Neto,João A.; Hartwig,Marcelo P.; Barros,Allan C.; Coelho,Rubens D.
Plug dynamics of non compensate drip tubes were evaluated, by the precipitation of moisturized whitewash [Ca(OH)2], which is used in the fertigation for the bulb pH control of the trademarks Azud, Amanco, Naandan, Netafim, Petroisa, Queen Gil, with flow rate varying between 0.4 to 3.0 L h-1 usually used in the country. For this matter, increasing doses of Ca(OH)² were applied in the irrigation water, from 0.01 g L-1 to 1.84 g L-1. The flow rate of each drip tube was measured in intervals of time initially of 7 days, later of 15 days of system operation, totaling a time of 100 days of operation, corresponding to nine applications or 432 hours. The coefficient of variation (CV), and relative rate flow (Qr) were evaluated. The results pointed differences...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drip tube; Clogging evaluation; Hydrated lime.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500006

Ambiência aérea em maternidade e creche de suínos
Provedor de dados: 70
Autores: Silveira,Neidimila A.; Nääs,Irenilza de A.; Moura,Daniella J. de; Salgado,Douglas D'Alessandro.
A suinocultura brasileira é uma atividade importante para o agronegócio do País. Embora o uso de tecnologia nos vários segmentos dessa atividade envolva a substituição do trabalho humano pela automatização de tarefas, o uso da mão de obra humana ainda é significativo. O trabalhador no setor suinícola está exposto a uma série de fatores de risco na execução de suas atividades, dentre os quais a exposição a gases nocivos. O presente trabalho teve por objetivo avaliar a qualidade do ar em instalações de maternidade e creche suinícolas, em duas granjas, com diferentes características (G1 e G2). Para tanto, foram avaliadas concentração de gases (NH3, CO2 e CO) e poeira respirável durante o período de atividades dos trabalhadores. As concentrações dos gases...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Suinocultura; Ambiente aéreo; Trabalhador.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300002

Avaliação dos custos de implantação de biodigestores e da energia produzida pelo biogás
Provedor de dados: 70
Autores: Calza,Lana F.; Lima,Cleber B.; Nogueira,Carlos E. C.; Siqueira,Jair A. C.; Santos,Reginaldo F.
RESUMO Este trabalho objetivou avaliar os custos envolvidos na construção de modelos de biodigestores (indiano, chinês e canadense) no município de Cascavel – PR. Determinaram-se os custos de produção de energia a partir do biogás produzido por dejetos de caprinos, bovinos e suínos, para sistemas de semiconfinamento. Foram utilizadas propriedades rurais com 20; 40; 60; 80 e 100 animais de cada um dos três grupos avaliados. A partir do volume de dejetos produzidos por animal, foram dimensionados os biodigestores e calculados os custos para a construção e a implantação de cada modelo, e o custo total da produção anual de energia em função do número de animais. O biodigestor modelo canadense apresentou o menor custo de construção e de implantação, variando de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogás; Esterco; Avaliação econômica.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000600990

Simulação da varredura da superfície por um cortador de base segmentado
Provedor de dados: 70
Autores: Oliveira,Carlos A. A.; Braunbeck,Oscar A.; Volpato,Carlos E. S.
O corte e a alimentação de plantas acamadas da cana-de-açúcar próximas do solo para o interior da colhedora requerem uma varredura eficiente da superfície pelo cortador de base. Essas condições não são conseguidas com o cortador convencional, composto por facas rígidas, além disso, esse mecanismo é responsável pela contaminação e incorporação de terra ao material colhido e causador de danos à soqueira. Este trabalho teve por objetivo simular o desempenho da varredura de um cortador de base segmentado. A modelagem foi desenvolvida por meio das leis da dinâmica, sendo a análise realizada em duas rotações (400 e 600 rpm), duas alturas de trabalho (0,12 e 0,13 m) e duas inclinações do cortador (-10º e -12º). Os resultados de varredura variaram entre 56º e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelagem; Protótipo virtual; Colhedora de cana-de-açúcar.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300024

Estimated production and evapotranspiration of irrigated bean cultivars
Provedor de dados: 70
Autores: Santana,Márcio J. de; Lemos,Leandro B.; Souza,Stefany S. de; Campos,Talita M.; Silva,Flávia M. da; Borges,Rafael D.
The current study intended to determine the optimum water depth, yield and evapotranspiration (ETc) for bean cultivars. The experiment was conducted in the Campus of Unit I of the Triângulo Mineiro Federal Education and Technology Institute in Uberaba, MG, in a completely randomized design with three replications. The treatments consisted of four water-replacing levels in the soil (70, 100, 130 and 160% of the crop evapotranspiration) and four bean cultivars (Pérola, BRSMG Madrepérola, BRSMG Majestoso and IAC Alvorada). The average values of ETc obtained for soil water balance for the cultivars Pérola, BRSMG Madrepérola, BRSMG Majestoso and IAC Alvorada were, respectively, of 5.25 mm day-1, 4.59 mm day-1, 4.54 mm day-1 and 4.77 mm day-1. The water depths...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Irrigation management; ETc; Optimum water depth; Phaseolus vulgaris L.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600006

PHYSIC-CHEMICAL QUALITY OF SECOND CROP CORN AS A FUNCTION OF TIME BETWEEN HARVEST AND DRYING
Provedor de dados: 70
Autores: Andrade,José C. de; Goneli,André L. D.; Hartmann Filho,Cesar P.; Goes,Rafael H. de T. E B. de; Gonçalves,Alexandre A.
ABSTRACT: The gap in the storage industry has brought a series of problems for the agro industrial market today, as its ability to directly infer the quality of newly collected material. The present study was carried out with the objective of evaluating the quality of second crop corn harvested with different water contents depending on the period until drying. The corn grains were harvested with moisture contents of approximately 28.5; 22.4; 21 and 19%, and subjected to temporary storage for ten days, simulating the time between harvest and drying. In the period, every two days the quality was evaluated by determining the specific mass, electrical conductivity, color, crude protein content, ethereal extract, ashes and carbohydrates. Based on the obtained...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays L.; Grain quality; Post-harvest.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000501004

Warning system based on theoretical-experimental study of dispersion of soluble pollutants in rivers
Provedor de dados: 70
Autores: Ribeiro,Celso B. de M.; Silva,Demétrius D. da; Soares,José H. P.; Guedes,Hugo A. S.
Information about capacity of transport and dispersion of soluble pollutants in natural streams are important in the management of water resources, especially in planning preventive measures to minimize the problems caused by accidental or intentional waste, in public health and economic activities that depend on the use of water. Considering this importance, this study aimed to develop a warning system for rivers, based on experimental techniques using tracers and analytical equations of one-dimensional transport of soluble pollutants conservative, to subsidizing the decision-making in the management of water resources. The system was development in JAVA programming language and MySQL database can predict the travel time of pollutants clouds from a point...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Longitudinal dispersion; Water pollution; Computational modeling.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500016

Modelos de regressão lineares para estimativa de produtividade da soja no oeste do Paraná, utilizando dados espectrais
Provedor de dados: 70
Autores: Mercante,Erivelto; Lamparelli,Rubens A. C.; Uribe-opazo,Miguel A.; Rocha,Jansle V.
O trabalho teve o objetivo de avaliar modelos lineares de regressão entre resposta espectral e produtividade em soja, na escala regional. Para isso, foram monitorados 36 municípios do oeste do Paraná, utilizando cinco imagens do satélite Landsat 5/TM da safra de 2004/2005. Foram realizados os procedimentos de transformação radiométrica e correção atmosférica nas imagens, determinando valores físicos das refletâncias aparente e de superfície. Posteriormente, foram calculados os índices de vegetação NDVI e GVI, os quais, por meio de regressões lineares simples e múltiplas, compararam-se com as produtividades oficiais dos municípios, obtidas das estatísticas IBGE. Aplicou-se também uma análise de diagnóstico, para detectar pontos influentes e de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Índices de vegetação; Dados orbitais; Cultura anual; Monitoramento.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300014

BIOHYDROGEN PRODUCTION IN AnSBBR IN FED-BATCH FROM STARCH EFFLUENT: INFLUENCE OF ORGANIC LOAD
Provedor de dados: 70
Autores: Tonello,Tamiris U.; Andreani,Cristiane L.; Mari,Angelo G.; Fernandes,José R.; Gomes,Simone D.
ABSTRACT The hydrogen is a fuel with a high energy density. Studies have sought to verify the potential of different residues and configurations of reactors in the production of biohydrogen. This study evaluated the influence of the organic loading rate on the production of biohydrogen from cassava starch wastewater (CSW) in anaerobic sequencing batch biofilm reactors (AnSBBR) operated in a fed-batch. In the tests, the organic loading rates of 9.0; 13.5 and 18.0 gCT L−1 d−1 were used, at cycle times (CT) of 4; 4 and 2 h (tests I, II and III, respectively). The reactor was inoculated with sludge from a pilot anaerobic reactor used in the treatment of CSW, heat treated (heated at 90°C for 15 min). With the increase of the organic load (condition I to II)...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fed-batch; Fermentative process; Bioenergy; Cassava starch wastewater.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500768

THE TYPOLOGY OF BROILER HOUSE AND THE IMPACT IN THE LOCOMOTION OF BROILERS
Provedor de dados: 70
Autores: Garcia,Rodrigo G.; Lima,Nilsa D. da S.; Naas,Irenilza de A.; Caldara,Fabiana R.; Sgavioli,Sarah.
ABSTRACT The large majority of broiler houses use two types of systems: dark-house system - DHP, and tunnel with curtain system - ATC. The objective of the present study was to evaluate the association and the prevalence of locomotion issues in the broiler commercial farming systems (DHP and ATC). For assessing the thermal environment and the litter quality, a completely random design was adopted using two factors (broiler houses, DHP and ATC) with 12 repetitions. To study the surface temperature of the broiler breast, and the locomotion ability (gait score) a completely randomized design was adopted in a double factorial scheme 2 × 2 (two houses typology vs. sex) with 24 repetitions. To verify whether the type of house and the sex were associated to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Broiler houses; Gait score; Spondylolisthesis; Surface temperature.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300326

Energetic sustainability of three arabica coffee growing systems used by family farming units in Espírito Santo state
Provedor de dados: 70
Autores: Muner,Lúcio H. de; Masera,Omar; Fornazier,Maurício J.; Souza,Cássio V. de; Loreto,Maria Das D. S. de.
Three growing systems of Arabica coffee were evaluated under the energy perspective, in the state of Espírito Santo in Brazil. The systems are conventional cultivation (CC), cultivation with good agricultural practices (CGP) and organic farming (OF). It was made a comparison of the energy flows within these three systems to show sustainable levels of each one based on production average data of several family-farming units. Therefore, we analyzed crop yield, total energy efficiency reverse (TEER), energy efficiency of ripe coffee (EERC) and non-renewable energy efficiency (NREE). OF system had values for TEER, EERC and NREE of 3.3 4.7 and 7.9 respectively. Yet CC showed values of 1.8, 1.9 and 1.6 for TEER, EERC and NREE respectively. Furthermore, CGP...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agroecosystem; Energy analysis; Coffee; Crop yield; Sustainability.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300397

Evaluation of the heating of broilers in shed by means of gas hoods and underfloor heating
Provedor de dados: 70
Autores: Leva,Flávia F. de; Camacho,José R.; Oliveira Filho,Delly.
This study was conducted to evaluate and compare the behavior of the heating inside poultry shed through gas hood and underfloor heating. The experiment was conducted in poultry shed belonging to the Federal Institute of Education, Science and Technology of Triângulo Mineiro Region, Uberlândia city Â– state of Minas Gerais (MG), Brazil. The dimensions of the shed are 24 meters long and 9.6 meters wide and with a ceiling height of 3.2 meters. The temperature was measured with an optical thermometer of Minipa brand, MT 350 model. It was used, to the analysis of temperature behavior, the public domain software FEMM 4.2, which uses finite elements techniques, with data collected from two lots. Underfloor heating is made using hot water flowing through a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy consumption; Underfloor heating; Environment; Thermal comfort; Solar energy.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400023

Variabilidade espacial da força de desprendimento de frutos do cafeeiro
Provedor de dados: 70
Autores: Ferraz,Gabriel A. e S.; Silva,Fábio M. da; Oliveira,Marcelo S. de; Silva,Flavio C. da; Bueno,Rafael de L.
O objetivo deste trabalho foi utilizar técnicas de georreferenciamento e de geoestatística para analisar a variabilidade espacial da força de desprendimento de frutos de cafeeiros por meio de semivariogramas e pela interpolação por krigagem. O trabalho foi conduzido no município de Três Pontas - MG, Brasil. A força de desprendimento dos frutos verdes e de cerejas dos cafeeiros foi obtida por meio de um protótipo de dinamômetro em pontos georreferenciados. A dependência espacial dos dados foi analisada por meio de ajustes de semivariogramas, clássico e robusto, para o método dos mínimos quadrados ordinários e ponderados, e apenas o ajuste clássico, para os métodos da máxima verossimilhança e máxima verossimilhança restrita. Testaram-se, para cada um dos...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Face de exposição solar; Agricultura de precisão; Geoestatística; Colheita mecanizada e seletiva; Café.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600016

Avaliação de tipos de ventilação em maternidade de suínos
Provedor de dados: 70
Autores: Tolon,Yamilia B.; Nääs,Irenilza de A.
As instalações onde os animais fazem o seu ciclo de produção devem ter como característica principal permitir o controle da influência dos fatores climáticos sobre os animais. As variações ambientais podem ser controladas por meio do uso de diferentes sistemas de ventilação. Dessa maneira, o objetivo desta pesquisa foi avaliar a influência de diferentes sistemas de acondicionamento na maternidade de suínos. Foram testados três tratamentos: ventilação natural, ventilação refrigerada e ventilação forçada. Os parâmetros climáticos avaliados foram: temperatura do ar, umidade relativa e temperatura de globo negro. Foram analisados, nas fêmeas, os parâmetros: freqüência respiratória e espessura do toucinho, e nos leitões: número de leitões nascidos vivos, peso...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Suínos; Resfriamento; Índices de conforto térmico.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300001

TECHNICAL FEASIBILITY OF THE ACCLIMATIZATION SYSTEM IN AVIARY OF POSTURE: A CASE STUDY
Provedor de dados: 70
Autores: Pereira,Danilo F.; Kodaira,Vanessa; Bueno,Leda G. de F.; Soares,Nilce M.; Salgado,Douglas D'Alessandro.
ABSTRACT: The objective of this study was to compare the performance of laying hens between automated aviaries, one with and another without acclimatized system. On a daily basis it was registered in each aviary the mortality, the egg production, and the feed consumption. The variables of the dry bulb temperature, relative humidity and black globe temperature were registered every 30 minutes using the thermos hygrometer. Every 28 days ninety eggs from each aviary were collected randomly and the variables egg weight, shell weight, shell thickness and Haugh Unit were registered. The consumption and quality of the electrical energy supply were monitored every 30 minutes using registers of electrical magnitude. The results showed that the acclimatization...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Electrical energy; Mortality; Egg production; Precision animal science.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500855

MATHEMATICAL MODELLING AND IMMEDIATE AND LATENT QUALITY OF NATURAL IMMATURE COFFEE UNDER DIFFERENT DRYING CONDITIONS
Provedor de dados: 70
Autores: Andrade,Ednilton T. de; Lemos,Isabella A.; Dias,Camila de A.; Rios,Paula de A.; Borém,Flavio M.
ABSTRACT This work aimed to study the immediate and latent effects of different relative humidities on the quality of dried coffee fruits, describe the drying kinetics of natural immature coffee (Coffea arabica L.), and evaluate the mathematical model that best fits the experimental drying data. The drying was carried out in a fixed layer dryer coupled to a composite air conditioning system in which the drying air was controlled with an air flow of 20 m3.min1.m−2, at a temperature of 40 °C, and at relative humidities of 10%, 17.5% and 32.5%. Manually harvested coffee fruits were used and dried to a mean water content of 0.120 dry basis (d.b). After drying, the kinetic curve and the physical and physiological properties were determined. The coffee was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drying kinetics; Coffea arabica L.; Post harvest.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500630

SORPTION ISOTHERMS AND ISOSTERIC HEAT OF PERICARP AND ENDOSPERM TISSUES OF ARABICA COFFEE FRUIT
Provedor de dados: 70
Autores: Dias,Camila de A.; Andrade,Ednilton T. de; Lemos,Isabella A.; Borém,Flávio M.; Barros,Ezequiel A.
ABSTRACT The aim of this study was to evaluate and model the hygroscopic equilibrium and isosteric heat curves of pericarp and endosperm tissues of arabica (Coffea arabica) coffee fruit, in different temperature and relative humidity conditions. Sorption isotherms were drawn under temperatures from 20°C to 70°C and relative humidity ranging between 10% and 90% until the product reached the equilibrium water content with the environment. The experiment was set up in a 4 × 4 factorial scheme (four relative humidity of the drying air and three tissues of the coffee cherry pericarp + endosperm [1: exocarp + part of the mesocarp, 2: mesocarp, 3: endocarp, 4: endosperm]), in a completely randomized design, with three repetitions. The results were examined by...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adsorption; Coffea arabica; Desorption; Hygroscopic equilibrium; Mathematical modeling.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100078

Irrigation management in pruned coffee tree crop
Provedor de dados: 70
Autores: Custódio,Anselmo A. de P.; Faria,Manoel A. de; Rezende,Fátima C.; Morais,Augusto R. de; Leite Junior,Maurício C. R.
It was evaluated the effect of irrigation management on the production characteristics of coffee cultivar Acaiá MG-1474, planted in spacing of 3.00 m x 0.60 m, pruned in 2004, and irrigated by drip since the planting, in 1997. The experimental designed used was of randomized blocks with five treatments and four replications. The treatments consisted of irrigation management strategies, applying or not applying controlled moisture deficit in layer of 0 to 0.4m, in dry seasons of the year: A = no irrigation (control), B = irrigation during all year considering the factor of water availability in the soil (f) equal to 0.75, C = irrigation during all year considering f = 0.25, D = irrigation during all year, but in January /February /March /July /October...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drip irrigation; Productivity; Coffee plantation; Coffea arabica L.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100007

Tensão superficial dinâmica e ângulo de contato de soluções aquosas com surfatantes em superfícies artificiais e naturais
Provedor de dados: 70
Autores: Iost,Cristina A. R.; Raetano,Carlos G.
O trabalho objetivou avaliar o efeito de surfatantes em soluções aquosas sobre a tensão superficial dinâmica e ângulo de contato das gotas em diferentes superfícies: artificiais (lâmina de vidro e de óxido de alumínio) e naturais (superfícies adaxiais de folhas de Euphorbia heterophylla, Ipomoea grandifolia e Brachiaria plantaginea). Seis formulações de surfatantes (Antideriva®; Uno®; Pronto 3®; Li-700®; Supersil® e Silwet L-77®), respectivamente nas doses recomendadas do produto comercial (0,050; 0,025; 0,100; 0,250; 0,100 e 0,100 % v v-1) e o dobro delas, foram avaliadas em soluções aquosas. A tensão superficial dinâmica e o ângulo de contato formado sobre as superfícies naturais foram medidos por tensiômetro. Os ângulos de contato formados pelas gotas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adjuvantes; Pulverização; Propriedades físico-químicas; Espécies vegetais.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400011

Uso de piloto automático na implantação de pomares de citros
Provedor de dados: 70
Autores: Oliveira,Tiago C. A.; Molin,José P.
Sistemas de piloto automático vêm sendo utilizados com relativa frequência na agricultura brasileira. Na citricultura, o uso dessa tecnologia vem difundindo-se na operação de abertura de sulcos para o transplantio de mudas. O presente trabalho teve como objetivos avaliar a acurácia de um piloto automático e avaliar possíveis ganhos gerados pela utilização dessa tecnologia de orientação automática em relação ao sistema convencional de abertura de sulcos na implantação de lavoura de citros. A primeira etapa consistiu em georreferenciar as plantas no campo, três meses após o transplantio, com sulcos feitos com as duas tecnologias. Na segunda etapa do trabalho, foi conduzida a avaliação da capacidade operacional da operação de abertura de sulcos, com e sem a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Sistemas guia; GNSS.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200013

Maximização da produção e da receita agrícola com limitações de água e nitrogênio utilizando método de pontos interiores
Provedor de dados: 70
Autores: Carvalho,Daniel F. de; Delgado,Angel R. Sanchez; Oliveira,Rosane F. de; Silva,Wilson A. da; Forte,Vinicius L. do.
Com este trabalho, teve-se o objetivo de pesquisar o desempenho do método de pontos interiores (MPI), tipo trajetória central, na maximização de funções-objetivo associadas à produção e à receita agrícolas, com restrições de água e de nitrogênio. Para isso, foi desenvolvido um procedimento matemático que maximiza a produção e a receita líquida separadamente, em função da água e do nitrogênio aplicados à cultura numa matriz bidimensional de restrições, a partir de funções de produtividade para as culturas da aveia e da laranja-pera. O modelo foi caracterizado e, a partir dele, foram gerados resultados numéricos para diferentes cenários agrícolas. Foi possível concluir que a metodologia utilizada (MPI) foi capaz de maximizar as funções de produtividade e de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Programação não linear; Trajetória central; Concavidade; Função-resposta; Otimização.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200015

Desempenho de colhedoras semimontadas para a colheita direta de milho
Provedor de dados: 70
Autores: Lima,Carlos M. de; Molin,José P.; Araújo,João C. de; del Pino,Miguel A. I. T.
O objetivo do trabalho foi adaptar procedimentos de ensaio existentes para colhedoras autopropelidas e avaliar o desempenho de colhedoras semimontadas, de uma e duas fileiras, operando com três velocidades de deslocamento em dois graus de umidade. Para tanto, foi desenvolvido um dispositivo de coleta do material efluente das máquinas, foram analisadas as perdas de plataforma, de separação e limpeza, de trilha e os parâmetros de qualidade: impureza, danos mecânicos dos grãos e falhas na germinação. O delineamento experimental foi em blocos casualizados, dispostos em esquema fatorial 2 x 3, com seis repetições. Não houve efeito dos tratamentos em relação às perdas na colhedora de uma fileira. Na colhedora de duas fileiras, houve efeito significativo nos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura familiar; Mecanização; Perdas na colheita.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400012

Use of nuclear technique in samples for agricultural purposes
Provedor de dados: 70
Autores: Oliveira,Kerley A. P. de; Menezes,Maria Ângela B. C.; Jacomino,Vanusa M. F.; Sperling,Eduardo Von.
The concern related to environment is growing. Due to this, it is needed to determine chemical elements in a large range of concentration. The neutron activation technique (NAA) determines the elemental composition by the measurement of artificial radioactivity in a sample that was submitted to a neutron flux. NAA is a sensitive and accurate technique with low detection limits. An example of application of NAA was the measurement of concentrations of rare earth elements (REE) in waste samples of phosphogypsum (PG) and cerrado soil samples (clayey and sandy soils). Additionally, a soil reference material of the International Atomic Energy Agency (IAEA) was also analyzed. The REE concentration in PG samples was two times higher than those found in national...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Neutron activation analysis; Multielemental analyses; Phosphogypsum; Rare earth elements.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100006

Adequação de engates rápidos de aspersores como conectores de mangueira para distribuição de água em sulcos de irrigação
Provedor de dados: 70
Autores: Faria,Flaviane F. de; Testezlaf,Roberto.
Como forma de reduzir as perdas de água que ocorrem na irrigação empregada na cultura do tomateiro, agricultores vêm utilizando mangueiras de forma precária na distribuição de água aos sulcos. O presente trabalho teve como objetivo estudar a adequação de engates rápidos de aspersores para serem aplicados como conectores de mangueiras por produtores irrigantes que façam uso desse sistema de distribuição de água. A primeira etapa do estudo foi avaliar, em campo, a operacionalidade do uso de mangueiras por produtores que fazem uso desse sistema. Posteriormente, quatro modelos de engates rápidos, disponíveis no mercado, foram ensaiados em laboratório, determinando-se o coeficiente de resistência, o comprimento equivalente, a curva de perda de carga e a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Equipamento de irrigação; Eficiência do uso da água; Tecnologia de irrigação.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200018

Sistemas de adubação e consórcio de culturas intercalares e seus efeitos nas variáveis de colheita da cultura do milho
Provedor de dados: 70
Autores: Cortez,Jorge W.; Furlani,Carlos E. A.; Silva,Rouverson P. da.
A colheita é a operação final de campo do processo produtivo, e por isso os fatores que interferem na mesma devem ser observados e avaliados atentamente para reduzir ao mínimo as perdas nessa etapa. O objetivo deste trabalho foi avaliar a influência dos sistemas de adubação (em pré-semeadura e na semeadura) e dos consórcios de culturas intercalares (milho+mucuna-cinza-anã, milho+guandu-anão e milho+lablab) nas variáveis de colheita da cultura do milho em sistema plantio direto. O experimento foi realizado na UNESP de Jaboticabal - SP, no período de safra normal, utilizando-se do delineamento em blocos ao acaso, no esquema fatorial (2 x 3), com quatro repetições. Os componentes avaliados na colheita foram: diâmetro do colmo, altura de inserção da primeira...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fluxo de material; Perdas na colheita; Mecanização agrícola.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200011

SOIL SOLUTION DISTRIBUTION IN SUBSURFACE DRIP IRRIGATION IN SUGARCANE
Provedor de dados: 70
Autores: Souza,Claudinei F.; Bizari,Douglas R.
Abstract Given the lack of studies on subsurface drip irrigation in sugarcane plantations, there has been a growing demand for such information, mainly regarding soil solution profile and availability to plants. Thus, this study aimed to evaluate the effects of soil-water solution distribution on qualitative and quantitative traits of sugarcane irrigated by subsurface drip irrigation at two flows (1.6 and 3.5 L h−1). For each application rate, four PVC containers (500 L) were used and filled with sandy soil, where a set of 36 TDR probes was installed. Drippers were placed at a depth of 0.30 m. Irrigation was managed based on TDR daily measurements, maintaining soil moisture within the root zone at field capacity. Sugarcane variety used was RB 845210, being...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertigation; Flow rate; Wetted soil volume; TDR.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200217

ERGONOMIC AND SAFETY CONDITIONS ASSESSMENT OF TRACTORS USED BY SMALLHOLDERS ACCORDING TO BRAZILIAN LEGISLATION AND CURRENT STANDARDS
Provedor de dados: 70
Autores: Reis,Ângelo V. dos; Pereira,Aline S.; Ferreira,Mauro F.; Mackmill,Laurett de Brum; Timm,Márcio W.
ABSTRACT This article aimed to select items with which to evaluate the ergonomic and safety conditions in tractors used by smallholders and family farmers, based on standardization research and legislation for the sector. Brazil has a comprehensive set of technical standards and legislation for the agricultural machinery sector intended to guarantee product standardization and to promote the health and safety of the users. Therefore, the initial step of this research was to review the technical norms and legislation for the product in order to develop instruments to assess their ergonomic and safety conditions. Twenty-eight Brazilian Technical Standards (NBR) and four Regulatory Norms (NRs) were investigated, in addition to CONTRAN (the Brazilian Traffic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Operator's seat; Noise level; Tractor operator.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300391

Integrated multivariate analysis to evaluate effects of pre-slaughter handling on pork quality
Provedor de dados: 70
Autores: Machado,Sivanilza T.; Santos,Rodrigo C.; Caldara,Fabiana R.; Gonçalves,Manoel C.; Nääs,Irenilza de A.
The aim of this study was to investigate the effect of pre-slaughter handling on the occurrence of PSE (Pale, Soft, and Exudative) meat in swine slaughtered at a commercial slaughterhouse located in the metropolitan region of Dourados, Mato Grosso do Sul, Brazil. Based on the database (n=1,832 carcasses), it was possible to apply the integrated multivariate analysis for the purpose of identifying, among the selected variables, those of greatest relevance to this study. Results of the Principal Component Analysis showed that the first five components explained 89.28% of total variance. In the Factor Analysis, the first factor represented the thermal stress and fatiguing conditions for swine during pre-slaughter handling. In general, this study indicated the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Transport operation; Ambience; PSE meat; Multivariate analysis.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300007

The use of infrared thermography in the identification of pododermatitis in broilers
Provedor de dados: 70
Autores: Jacob,Flavia G.; Baracho,Marta dos S.; Nääs,Irenilza de A.; Souza,Rafael; Salgado,Douglas D’Alessandro.
ABSTRACT International trade in broiler’ feet, mainly to Asian markets, has demanded better quality control. The objective of this research was to study the suitability of using chicken footpad surface temperature to determine early lesions of pododermatitis. The project was conducted in two houses A1 and A2) in a commercial farm during one production flock. A1 had reused litter of wood shavings and rice hulls, and A2 had a new litter of sawdust. Both houses had positive pressure ventilation. The inner area of the poultry was virtually divided into three quadrants. The footpads were checked for the feet quality, and a degree of pododermatitis was awarded. Thermal images were made to test the surface temperature of the foot and identify inflammation in a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Rearing ambient; Sub-clinical lesions; Thermal image.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200253

Extrapolation of regionalization equations for long-term average flow
Provedor de dados: 70
Autores: Pruski,Fernando F.; Rodriguez,Renata del Giudice; Pruski,Pedro L.; Nunes,Aline de A.; Rego,Fernando S.
ABSTRACT Knowledge about long-term average flow is essential for planning and managing water resources because it represents the potential water availability. One technique used to determine streamflow is regionalization, but because most gauge stations normally are associated with large drainage areas, the extrapolation of regionalization equations does not accurately represent the water availability; therefore, this method is not recommended. The main objective of the present paper is to propose a new method of estimating water availability that minimizes the risks of extrapolating regionalization equations for long-term average flow. The method is based on the use of a threshold value of the runoff coefficient to obtain the long-term average flow at the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water availability; Planning and management of water resources; Water safety.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500830

Construction and calibration of TDR probes for volumetric water content estimation in a Distroferric Red Latosol
Provedor de dados: 70
Autores: Soncela,Rosimaldo; Sampaio,Silvio C.; Vilas Boas,Marcio A.; Tavares,Maria H. F.; Smanhotto,Adriana.
The determination of volumetric water content of soils is an important factor in irrigation management. Among the indirect methods for estimating, the time-domain reflectometry (TDR) technique has received a significant attention. Like any other technique, it has advantages and disadvantages, but its greatest disadvantage is the need of calibration and high cost of acquisition. The main goal of this study was to establish a calibration model for the TDR equipment, Trase System Model 6050X1, to estimate the volumetric water content in a Distroferric Red Latosol. The calibration was carried out in a laboratory with disturbed soil samples under study, packed in PVC columns of a volume of 0.0078m³. The TDR probes were handcrafted with three rods and 0.20m...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Apparent dielectric constant; Time-domain reflectometry; Soil water content.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500004

MANUFACTURE OF SOIL-CEMENT BRICKS WITH THE ADDITION OF SUGARCANE BAGASSE ASH
Provedor de dados: 70
Autores: Jordan,Rodrigo A.; Costa,Matheus V. Da; Martins,Elton A. S.; Rosa,Maxer A.; Petrauski,Alfredo.
ABSTRACT The objective of this study is to evaluate the effect of sugarcane bagasse ash on the compressive strength and water absorption index of soil-cement bricks. The ash was sieved without chemical and/or physical treatment to reflect the use of this material in real manufacturing processes. The addition of natural ash decreased the quality of the bricks, reducing the compressive strength and increasing the water absorption index.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ash; Compressive strength; Soil-cement.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100026

Simulação do deslocamento de potássio em colunas verticais de solo não-saturado
Provedor de dados: 70
Autores: Miranda,Jarbas H.; Duarte,Sergio N.; Libardi,Paulo L.; Folegatti,Marcos V.
O estudo do transporte de água e potássio em solo não-saturado é importante, tanto do ponto de vista do ambiente quanto do econômico. Assim sendo, o uso da modelagem computacional é importante, pois permite de maneira precisa e rápida o monitoramento do deslocamento de solutos, importante na prevenção de impactos ao ambiente. No presente trabalho, teve-se o objetivo de avaliar a simulação do deslocamento do íon potássio em colunas de solo não-saturado, utilizando o modelo MIDI, bem como apresentar a determinação dos parâmetros de transporte do íon potássio em um Latossolo Vermelho-Amarelo, fase arenosa. Concluiu-se que o modelo foi capaz de simular de maneira satisfatória o perfil de umidade e o deslocamento do íon potássio.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dinâmica de solutos; Modelagem; Curva de eluição.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300013

EFFECTS OF CLAY FRACTION MINERALOGY ON PHYSICAL ATTRIBUTES OF A YELLOW ULTISOL TREATED WITH CHISELING
Provedor de dados: 70
Autores: Nogueira,Deise C. S.; Fernandes,Carolina; Souza,Luma C. de; Camargo,Lívia A.; Ferraudo,Antonio S.
ABSTRACT The objective of this study was to evaluate the influence of minerals in the clay fraction on physical attributes of Yellow Ultisol cultivated with sugarcane and prepared with two different treatments: chiseling across the entire area and chiseling only in planting rows. The samples were collected from four layers of soil at eight months after planting. We assessed the texture of the soil, levels of iron extracted by dithionite-citrate-bicarbonate (DCB) and ammonium acid oxalate (AAO), ratio of kaolinite/(kaolinite + gibbsite), soil bulk density, and soil penetration resistance. The first area showed a higher ratio of kaolinite/(kaolinite + gibbsite) and the second area had greater levels of iron extracted by DCB. Levels of iron extracted by DCB...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Iron oxides; Kaolinite; Soil bulk density; Soil penetration resistance.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400433

SPATIALIZATION OF THE ANNUAL MAXIMUM DAILY RAINFALL IN SOUTHEASTERN BRAZIL
Provedor de dados: 70
Autores: Batista,Marcelo L.; Coelho,Gilberto; Mello,Carlos R. de; Oliveira,Marcelo S. de.
ABSTRACT Extreme rainfall can lead to heavy damage and losses, such as landslides, floods and agricultural productivity as well as the loss of human and animal lives. To mitigate these losses, water resources management policies are needed, among other goals, to study and predict the frequency of such events in a given region to minimize their harmful effects. The present study investigated the Generalized Extreme Value (GEV) probability distribution applied to the annual maximum daily precipitation data from rainfall stations in the southeastern Brazil. A total of 1,921 rainfall stations were considered, among which the stations with at least 15 years of uninterrupted observations were selected. Subsequently, the stationarity and adherence were tested....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Extreme rainfall; GEV; Ordinary kriging.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100097

Swine wastewater associated with mineral fertilization on corn crop (Zea mays)
Provedor de dados: 70
Autores: Kessler,Nathalie C. H.; Sampaio,Silvio C.; Sorace,Mauren; Lucas,Shaiane D.; Palma,Denise.
This study aimed to evaluate the agronomical and environmental aspects in corn, soil characteristics and leachate resulting from the material combination of swine wastewater and mineral fertilizer in the long run. The experimental area has a history of swine wastewater application for experiments conducted since 2006, this being the seventh crop cycle in the area. Four doses of swine wastewater (0; 100; 200 and 300 m³ ha-1) associated with presence and absence of mineral fertilizer were applied, consisting of eight treatments. The results obtained were subjected to variance analysis and means compared by Tukey test at 5% significance. We conclude that the swine wastewater can be partially used as an alternative fertilizer, since the P and Mn are...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manure; Soil fertility; Water reuse.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300018

Yield, specific mass and coloration of azuki seeds after desiccation and storage
Provedor de dados: 70
Autores: TAVARES,CÁSSIO J.; SOUSA,MORGANA S.; ARAÚJO,ALANA C. F.; JAKELAITIS,ADRIANO; RESENDE,OSVALDO.
ABSTRACT Selection and dosage of desiccating herbicides may bring benefits to bean harvesting and its seed quality. This study aimed to assess yield, apparent specific mass and coloration of azuki bean seeds after pre-harvesting desiccation with different herbicides and doses and subsequent storing. In a first trial, we tested paraquat 400 (g ai ha-1), ammonium glufosinate (400 g ai ha-1), glyphosate (720 g ai ha-1), flumioxazin (30 g ai ha-1) and control. In second and third trials, we tested various doses of saflufenacil (0, 50, 75, 100, 150 and 200 g ai ha-1) and flumioxazin (0, 20, 25, 30, 35 and 40 g ai ha-1). All treatments were divided into plots and the dates of evaluation (at harvest and six months after harvest) into subplots with four...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Desiccating herbicides; Post-harvest; Vigna angularis Willd.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500858

Sistema automatizado para aquisição de dados de umidade relativa do ar
Provedor de dados: 70
Autores: Silva,Késia O. da; Moraes,Sergio O.; Miranda,Jarbas H.; Palmieri,Anderson M.
Devido à importância do ambiente na produção animal e vegetal e, portanto, controle ambiental adequado, o trabalho propõe como objetivo a construção de um sistema de aquisição automatizada de dados de umidade relativa do ar, utilizando-se de microcontrolador de dimensões reduzidas e de baixo custo. A calibração do sensor de umidade relativa foi realizada em três etapas de simulação desenvolvidas em laboratório: caixas perfuradas, dessecador sem tampa contendo sílica-gel em seu fundo e psicrometria. As etapas de calibração, utilizando situações naturais e artificiais, bem como as metodologias desenvolvidas, apresentaram resultados que permitem concluir que o sistema pode ser utilizado com segurança no monitoramento dessa variável.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Variáveis climáticas; Monitoramento do ambiente; Instrumentação.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400005

Desiccation time of the spring sorghum as a predecessor crop for summer soybean and autumn bean in a no-tillage system
Provedor de dados: 70
Autores: Denadai,Marcelo S.; Mello,Luiz M. M. de; Chioderoli,Carlos A.; Gazola,Rodolfo de Niro.
ABSTRACT Several authors have been questioned the desiccation interval between the coverage plants and sowing plants for the soybean crop. Therefore, this study aimed to evaluate the desiccation time of the spring sorghum as a predecessor crop for summer soybean and then for autumn bean, focusing on the straw formation for maintenance of the no-tillage system and to evaluate the yield of soybeans and beans grain, as well as analyzing the interference of sorghum straw in these cultures. The experiment was developed in the Teaching and Research Farm of FE/UNESP located in Ilha Solteira/SP where it was used an experimental design of randomized blocks with five treatments and six repetitions. The treatments consisted of five different intervals between sorghum...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Exudates allelochemicals; Soil cover; Desiccation interval for sowing; Crop rotation; Straw production.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100094

Hydrological simulation using SWAT model in headwater basin in Southeast Brazil
Provedor de dados: 70
Autores: Pereira,Donizete dos R.; Martinez,Mauro A.; Almeida,André Q. de; Pruski,Fernando F.; Silva,Demetrius D. da; Zonta,João H.
Hydrological models are important tools that have been used in water resource planning and management. Thus, the aim of this work was to calibrate and validate in a daily time scale, the SWAT model (Soil and Water Assessment Tool) to the watershed of the Galo creek , located in Espírito Santo State. To conduct the study we used georeferenced maps of relief, soil type and use, in addition to historical daily time series of basin climate and flow. In modeling were used time series corresponding to the periods Jan 1, 1995 to Dec 31, 2000 and Jan 1, 2001 to Dec 20, 2003 for calibration and validation, respectively. Model performance evaluation was done using the Nash-Sutcliffe coefficient (E NS) and the percentage of bias (P BIAS). SWAT evaluation was also...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydrological modeling; SWAT; Calibration; Validation.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400018

Tipologia de instalações avícolas na região Agreste de Pernambuco
Provedor de dados: 70
Autores: Silva,Tatiana P. N. da; Pandorfi,Héliton; Guiselini,Cristiane; Almeida,Gledson L. P. de; Gomes,Nicoly F.
RESUMO Este estudo foi conduzido com o objetivo de caracterizar a tipologia das instalações para produção de frangos de corte na região Agreste do Estado de Pernambuco, por meio de levantamento das características construtivas de aviários existentes na região. Foram avaliados 68 galpões, em 27 granjas, no período de maio de 2012 a abril de 2013. Com base nos resultados obtidos, 90% das instalações apresentaram orientação leste - oeste, com pequeno afastamento entre galpões (&lt; 30 m). A maioria dos galpões apresentou cobertura com telhas cerâmicas (93%), ausência de forro (93%) e lanternim (100%), pé-direito abaixo do recomendado (90%), beirais menores que 1,25 m (93%) e muretas com altura superior a 0,2 m (40%). Quanto aos equipamentos, observou-se que a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência; Avicultura de corte; Galpões avícolas.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400789

Efeito de subdoses de 2,4-D na produtividade de fumo e suscetibilidade da cultura em função de seu estádio de desenvolvimento
Provedor de dados: 70
Autores: Constantin,Jamil; Oliveira Júnior,Rubens S. de; Brandão Filho,José U. T.; Callegari,Osni; Pagliari,Paulo H.; Arantes,João G. Z. de.
O presente trabalho teve como objetivo determinar os efeitos de subdoses do herbicida 2,4-D na cultura do fumo. Os experimentos foram conduzidos a campo durante o ano de 2003, no município de Santa Isabel do Ivaí - PR, utilizando-se de fumo tipo Virgínia. No primeiro experimento, foram aplicadas, no estádio de pré-florescimento, doses de 0,84; 1,68; 3,36; 6,72; 13,44 e 26,88 g e.a. ha-1 de 2,4-D, equivalentes à deriva de 0,125; 0,25; 0,5; 1,0; 2,0 e 4,0% de produtos comerciais aplicados a 1,0 L ha-1 (670 g e.a. ha-1). Para o segundo experimento, os tratamentos foram constituídos pela combinação em esquema fatorial de duas doses (6,72 e 13,44 g e.a. ha-1, equivalentes a 1,0 e 2,0% de deriva) e três épocas de aplicação após o transplante para o campo. Nenhum...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Herbicidas fenóxicos; Fitotoxicidade; Subdoses.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200005

Uso de coagulantes naturais à base de moringa oleifera e tanino como auxiliares da filtração em geotêxtil sintético não tecido
Provedor de dados: 70
Autores: Arantes,Camila C.; Ribeiro,Túlio A. P.; Paterniani,José E. S.; Tateoka,Marina S. S.; Silva,Gabriela K. E.
Coagulantes naturais como Moringa oleifera e tanino podem ser usados em sistema de tratamento de água, com a finalidade da remoção de turbidez. Em testes de laboratório, simulou-se uma água bruta com turbidez na faixa de 101 a 110 NTU, que foi tratada utilizando-se de M. oleifera e tanino como coagulantes. Foi feita a filtração direta da água coagulada e floculada com uso de geotêxtil sintético não tecido como meio filtrante. Foram avaliados diferentes métodos para o preparo da solução do coagulante à base de M. oleifera. Também se comparou o comportamento dos dois coagulantes em relação à remoção de turbidez e à influência na variação do pH da água tratada. Os resultados obtidos na comparação entre os coagulantes demonstraram que o tanino (Tanfloc SG),...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tratamento de água; Coagulação-floculação; Polímeros naturais; Remoção de turbidez; Saneamento rural.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400017

Adjust of regression models to estimate the rectal temperature of broilers for the first 14 days of life
Provedor de dados: 70
Autores: Ponciano,Patrícia F.; Yanagi Junior,Tadayuki; Lima,Renato R. de; Schiassi,Leonardo; Teixeira,Vitor H.
The broiler rectal temperature (t rectal) is one of the most important physiological responses to classify the animal thermal comfort. Therefore, the aim of this study was to adjust regression models in order to predict the rectal temperature (t rectal) of broiler chickens under different thermal conditions based on age (A) and a meteorological variable (air temperature - t air) or a thermal comfort index (temperature and humidity index -THI or black globe humidity index - BGHI) or a physical quantity enthalpy (H). In addition, through the inversion of these models and the expected t rectal intervals for each age, the comfort limits of t air, THI, BGHI and H for the chicks in the heating phase were determined, aiding in the validation of the equations and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal environment; Poultry; Thermal comfort; Mathematical modeling; Physiological responses.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100002

Physiological evaluation of heat stress in gestating sows under different housing systems in bedding and concrete floor
Provedor de dados: 70
Autores: Nunes,Maria L. A.; Miranda,Késia O. da S.; Faria,João M. B. A. de; Vieira,Afrânio M. C.; Arcaro Júnior,Irineu.
The purpose of this paper was to observe the use of bedding (wood shavings) in physiological variables that indicate thermal stress in gestating sows. The experiment was conducted in order to evaluate the effect of two types of floor (concrete and wood shavings). Worse microclimatic conditions were observed in bedding systems (P&lt;0.05), with an increase in temperature and enthalpy of 1.14 ºC and 2.37 kJ.kg dry air-1, respectively. The floor temperature at the dirty area was higher in the bedding presence in comparison to its absence. In spite of the worse microclimatic conditions in the bedding, the rectal temperature did not differ significantly (P&amp;gt;0.05) but the skin surface temperature was higher in the bedding systems. The same occurred with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Swine; Thermal regulation; Zootechnical installations.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100001

Yield and quality of elephant grass biomass produced in the cerrados region for bioenergy
Provedor de dados: 70
Autores: Flores,Rilner A.; Urquiaga,Segundo; Alves,Bruno J. R.; Collier,Leonardo S.; Boddey,Robert M.
The objective of this study was to evaluate the performance of two genotypes of elephant grass, fertilized with and without N, for biomass production for energy use under the edaphoclimatic conditions of the Cerrado. The genotypes Roxo and Paraíso, grown in a field experiment in a Latosol in the Cerrado region were evaluated for biomass yield, nitrogen accumulation, C:N and stem:leaf ratios, fibre, ash and P and K contents and calorific value. The accumulated dry biomass ranged from 30 to 42 Mg ha-1 and showed no response to nitrogen fertilization with the lowest biomass obtained by the genotype Paraíso and the highest by Roxo. The total N accumulation followed the same pattern as for dry matter, ranging from 347 to 539 kg N ha-1. C:N and stem:leaf ratio...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pennisetum purpureum; Bioenergy; Nitrogen fertilizer.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500003

Quali/quantitative characterization of biogas produced in batch digesters supplied with six distinct substrates
Provedor de dados: 70
Autores: Galbiatti,João A.; Caramelo,Anaira D.; Chiconato,Denise A.; Araújo,José R.; Girardi,Eliana A. B.
The present research was carried out at the DER/FCAV, São Paulo State University - Brazil, with the purpose of analyzing the quantity and quality of biogas produced by six types of substrates. The substrates used in the anaerobic digestion were characterized as: 1- Litter of broiler (LB); 2- Grinded broiler litter (GBL); 3- Broiler litter with wood shavings (BLWS); 4- Grinded broiler litter with wood shavings (GBLWS); 5- Broiler litter with peanut hulls (BLPH); 6- Grinded broiler litter with peanut hull (GBLPH). It was concluded from the collected data that: the (GBL) substrate showed a superior biogas accumulated production in relation to the other substrates, while the BLWS presented an inferior accumulated production; the grinded substrates showed...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogas; Anaerobic; Organic residue; Digesters.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400017

DEPOSITION AND COVERAGE OF SOYBEAN LEAF SURFACES BY SPRAYS APPLIED USING DIFFERENT ASSISTED BOOM SPRAYER SYSTEMS
Provedor de dados: 70
Autores: Hoffmann,Laercio L.; Roehrig,Rafael; Boller,Walter; Forcelini,Carlos A.
ABSTRACT Maintaining homogeneity in the distribution of fungicidal sprays applied throughout the plant, minimizing the variation between the upper and lower third of the plant, is one of the main challenges for application technologies with regard to soybean crops. To increase the deposition and leaf coverage of sprayed compounds, especially in the middle and lower thirds of the plant, we developed and tested alternative assisted boom sprayer systems. In this study, three assisted boom sprayer systems (Vortex®, Dropleg®, and chain curtain) were evaluated, in addition to the conventional system, in terms of the deposition and coverage of the leaf surface they achieved in the upper, middle, and lower thirds of plants using the fluorescent tracer Helios SC...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Dropleg®; Vortex®.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200198

Mapping of summer crops in the State of Paraná, Brazil, through the 10-day spot vegetation NDVI composites
Provedor de dados: 70
Autores: Araújo,Gleyce K. D.; Rocha,Jansle V.; Lamparelli,Rubens A. C.; Rocha,Agmon M.
The search for low subjectivity area estimates has increased the use of remote sensing for agricultural monitoring and crop yield prediction, leading to more flexibility in data acquisition and lower costs comparing to traditional methods such as census and surveys. Low spatial resolution satellite images with higher frequency in image acquisition have shown to be adequate for cropland mapping and monitoring in large areas. The main goal of this study was to map the Summer crops in the State of Paraná, Brazil, using 10-day composition of NDVI SPOT Vegetation data for 2005/2006, 2006/2007 and 2007/2008 cropping seasons. For this, a supervised digital classification method with Parallelepiped algorithm in multitemporal RGB image composites was used, in order...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Remote sensing; Time series; Crop yield estimates.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400014

Tratamento de águas residuárias de fecularia por meio de lagoas de estabilização
Provedor de dados: 70
Autores: Campos,Alessandro T.; Daga,Jacir; Rodrigues,Emanuel E.; Franzener,Gilmar; Suguiy,Mary M. T.; Syperreck,Vera L. G.
Embora o uso de lagoas de tratamento seja uma tecnologia amplamente conhecida e utilizada para resíduos orgânicos, no caso específico dos resíduos líquidos da industrialização da mandioca, as experiências são reduzidas. Assim, o objetivo deste trabalho foi de avaliar a eficiência na redução da carga poluidora de lagoas de tratamento de resíduos líquidos de fecularia. Para tanto, foram coletadas amostras na entrada do sistema e em cada uma das sete lagoas da Fecularia Horizonte, em Marechal Cândido Rondon - PR, no período de maio a setembro de 2004. Os seguintes parâmetros foram avaliados: Demanda Bioquímica de Oxigênio (DBO), Demanda Química de Oxigênio (DQO), Sólidos Totais (ST), Sólidos Fixos (SF), Sólidos Voláteis (SV), N-NH4+, Condutividade Elétrica...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manipueira; Efluente; Mandioca.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100026

INTEGRATION OF A LOW-COST GLOBAL NAVIGATION SATELLITE SYSTEM TO A SINGLE-BOARD COMPUTER USING KALMAN FILTERING
Provedor de dados: 70
Autores: Silva,Thales M. de A.; Mayrink,Grégory de O.; Valente,Domingos S. M.; Queiroz,Daniel M.
ABSTRACT The global navigation satellite system (GNSS) is the basis for localized crop management by allowing the georeferencing of collected data and the generation of maps by different systems that compose precision agriculture. There is a demand for low-cost navigation systems to enable their use in agriculture. Therefore, the objective of this study is to integrate a low-cost GNSS module to a single-board computer using Kalman filtering to obtain navigation data. The system was evaluated by performing one static and two kinematic experiments, with three repetitions each. In the static experiment, the mean error was 3.25 m with a root mean square error (RMSE) of 3.73 m. In the first kinematic experiment, data variability was lower at a velocity of 1.39...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Georeferencing; Positioning; Beaglebone black; Algorithm.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300323

DEVELOPMENT OF A TRACEABILITY MODEL APPLIED TO GOAT AND SHEEP MEAT PRODUCTION
Provedor de dados: 70
Autores: Bezerra,Alan C.; Pandorfi,Héliton; Gama,Rafael M.; Carvalho,Francisco F. R. de; Guiselini,Cristiane.
ABSTRACT: The goat and sheep meat producer chain has developed in last years, thus, it is imperative to organize and structure the supply chain and to adopt reliable policies for products' traceability, as a tool to achieve these requirements. The study aimed to make a management program with a traceability model for goat and sheep meat production, with emphasis on ensuring product origin and management practices' transparency at the animal production unit. For this purpose, it was made a reference model in order to emit an origin certificate which, in turn, provides specific information concerning the final product from each unit. Secondly, the program was developed using Hipertext Preprocessor (PHP) technology and as for the Database Management System,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Goat and sheep meat production; Traceability; Food safety; Management system.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000501062

Efeito de doses de potássio e da freqüência de irrigação na produção da alface-americana em ambiente protegido
Provedor de dados: 70
Autores: Koetz,Marcio; Coelho,Gilberto; Costa,Claudionor C. da; Lima,Edson P.; Souza,Rovilson J. de.
A produção da alface tipo americana em ambiente protegido, aliada ao emprego de práticas de manejo de irrigação e adubação, pode contribuir para o aumento da produtividade e expansão da cultura na região de Lavras - MG. Em uma estufa modelo capela, foi realizado um experimento com o objetivo de avaliar o efeito de freqüências de irrigação e de doses de potássio sobre a produtividade da alface-americana e a eficiência do uso da água. O experimento foi composto pelos seguintes tratamentos de turnos de rega: (P1) - irrigação diária; (P2) - irrigação de dois em dois dias; (P3) - irrigação de três em três dias, e (P4) - irrigação de quatro em quatro dias. Nas parcelas subdivididas, foram aplicadas quatro doses de cloreto de potássio, via fertirrigação: (D1) -...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Fertirrigação; Manejo de irrigação.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300009

STATISTICAL PROCESS CONTROL APPLIED TO MONITOR LOSSES IN THE MECHANIZED SUGARCANE HARVESTING
Provedor de dados: 70
Autores: Paixão,Carla S. S.; Voltarelli,Murilo A.; Silva,Rouverson P. da; Borba,Mateus A. de P.; Torres,Luma S.
ABSTRACT The mechanized sugarcane harvesting process is considered one of the major economic bottlenecks, with low operational efficiency and, mainly, high losses of stalks left in the field. In order to minimize these problems and assist in the improvement of processes, this study aimed to evaluate the losses in the mechanized sugarcane harvesting using statistical process control. The experimental design was completely randomized, based on the methodology of statistical process control with samples collected on five work fronts during the daytime and nighttime operation. The experiment was carried out in an agricultural area of a sugarcane mill in the municipality of Ribeirão Preto, SP, Brazil, on five sugarcane harvest fronts. Losses were measured using...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Harvester; Visible losses; Saccharum spp.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400473

Emprego de ferramentas numéricas na avaliação do módulo de elasticidade em vigas roliças de madeira
Provedor de dados: 70
Autores: Christoforo,André L.; Zangiácomo,André L.; Panzera,Túlio H.; Silveira,Márcio E.; Lahr,Francisco A. R.
Vigas são elementos estruturais encontrados na maioria das construções civis. Dentre os materiais de engenharia, destaca-se a madeira, por ter resistência mecânica satisfatória aliada a baixa densidade. A madeira roliça apresenta-se como boa solução na confecção de vigas, uma vez que não precisa ser processada, como é o caso da madeira serrada. O projeto de elementos estruturais de madeira requer o conhecimento de suas propriedades físicas e mecânicas, obtidas segundo as premissas de documentos normativos. Em se tratando da madeira roliça, os documentos normativos nacionais que tratam da determinação das propriedades de resistência e rigidez estão vigentes há mais de vinte anos sem revisão técnica. De forma geral, tanto as normas nacionais como as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Madeira roliça; Método dos Elementos Finitos; Método dos Mínimos Quadrados.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500016

Fuel consumption of a tractor in function of wear, of ballasting and tire inflation pressure
Provedor de dados: 70
Autores: Spagnolo,Roger T.; Volpato,Carlos E. S.; Barbosa,Jackson A.; Palma,Marcos A. Z.; Barros,Murilo M. de.
When using appropriate inflation pressures and load capacity (ballast), it may obtain a higher yield and prolongation of the life of the tire, besides it may minimize the problems of loss of traction, increased slippage and fuel consumption. This study aimed to evaluate the fuel consumption of a tractor operating with new and worn tires in three conditions of ballasting and three inflation pressures, when driving on compacted soil with vegetation cover. The experiment was conducted at the experimental unit from the Department of Animal Science, Federal University of Lavras, state of Minas Gerais, Brazil, in an agricultural soil compacted by cattle trampling and with vegetation cover. It was used a tractor 4x2 with front wheel assist, of a 65.62 kW engine...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural machinery; Tractor test; Tractive force.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100014

THERMODYNAMIC PROPERTIES OF BARU FRUITS (Dipteryx alata Vogel)
Provedor de dados: 70
Autores: Resende,Osvaldo; Oliveira,Daniel E. C. DE; Costa,Lílian M.; Ferreira Júnior,Weder N.
ABSTRACT: The objective of this study was to determine and evaluate the thermodynamic properties for different equilibrium moisture contents in baru fruits (Dipteryx alata Vogel), using the direct static method to obtain the experimental data. The Modified Halsey model was used to determine the thermodynamic properties of baru fruits. Results concluded that thermodynamic properties are influenced by moisture content. The water vaporization latent heat increases with the decrease in equilibrium moisture content. The baru fruit desorption process is controlled by enthalpy. Gibbs free energy is positive for the temperatures studied with the increase over desorption, which describes a non-spontaneous process.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Latent heat; Enthalpy; Entropy; Gibbs free energy.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400739

Esterqueiras: avaliação físico-química e microbiológica do dejeto suíno armazenado
Provedor de dados: 70
Autores: Santos,Mônica A. A. dos; Schmidt,Verônica; Bitencourt,Vanessa C.; Maroso,Michele T. D.
Este trabalho avaliou a eficácia do armazenamento de dejetos de suínos por 120 dias, em três esterqueiras de propriedades suinícolas localizadas na bacia do lajeado Suruvi, município de Concórdia, região oeste de Santa Catarina. Os parâmetros analisados foram: decomposição do material carbonáceo, transformação de compostos nitrogenados, adsorção do fósforo e viabilidade de microrganismos patogênicos. Os resultados revelaram que: a) as maiores remoções de material carbonáceo ocorrem entre 30 e 60 dias de armazenamento; b) o ambiente anaeróbio das esterqueiras impossibilitou as remoções de nitrogênio amoniacal por nitrificação/desnitrificação; c) embora as remoções de ortofosfato na fase líquida do dejeto tenham sido significativas, a estocagem por longo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Esterqueiras; Compostos nitrogenados; Indicadores microbianos.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300024

Estimativa da evaporação nos reservatórios de Sobradinho e Três Marias usando diferentes modelos
Provedor de dados: 70
Autores: Vieira,Nayara P. A.; Pereira,Silvio B.; Martinez,Mauro A.; Silva,Demetrius D. da; Silva,Felipe B.
RESUMO Estudos que possibilitem a obtenção de estimativas precisas de evaporação em reservatórios representam uma importante ação para o adequado gerenciamento e manejo dos recursos hídricos. Dessa forma, objetivou-se comparar as estimativas de evaporação, dos reservatórios de Três Marias e Sobradinho, calculadas pelos modelos de Linacre et al. (1993), Kohler et al. (1995), Thornthwaite (1948), CRLE e o método do tanque Classe A com o valor estimado pelo modelo de Penman et al. (1948). Também foram comparados os valores de evaporação estimados a partir de dados de estações meteorológicas situadas no entorno do reservatório com o valor estimado com dados da estação localizada na área da barragem. Os resultados permitiram constatar que, em relação ao modelo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelos evaporimétricos; Parâmetros meteorológicos; Rio São Francisco.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300433

CHEMICAL PROPERTIES OF SOIL FERTIRRIGATED WITH DAIRY AND SLAUGHTERHOUSE WASTEWATER
Provedor de dados: 70
Autores: Oliveira,Jacineumo F. De; Rodrigues,Fernando N.; Fia,Ronaldo; Vilela,Hévelyn S.; Landim,Daniela V.
ABSTRACT The aim of this study was to evaluate the soil chemical properties submitted to fertigation with slaughterhouse (SW) and dairies (DW) wastewater. The experiment was conducted in the Environmental Engineering Center and Sanitary of UFLA/MG in PVC columns filled with Dark Red Latosol (Oxisol) and randomly distributed. The treatments applied with nitrogen based load (300 kg ha years-1 of N) consisted of four doses of SW and DW (100, 200, 300 and 400% of the recommendation) and AQT0 control at random. The soil was collected at a depth of 0.30 m and, subsequently, characterized in terms of physical, chemical and physicochemical. The application of treatment of the largest irrigation of DW provided, after 120 days of monitoring, N concentration of 1.85...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil quality; Fertigation; Plant nutrition; Agroindustrial wastewater.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601244

Produção de matéria seca em pastagem de Tifton 85 irrigada, com diferentes doses de dejeto líquido de suíno
Provedor de dados: 70
Autores: Drumond,Luís C. D.; Zanini,José R.; Aguiar,Adilson de P. A.; Rodrigues,Guilherme P.; Fernandes,André L. T.
O dejeto líquido de suíno (DLS) pode constituir-se em excelente fonte de adubação em pastagem, com aplicação por aspersão, desde que seja assegurada a proteção do meio ambiente. Apesar de seu comprovado potencial para uso em sequeiro, pouco se conhece sobre o comportamento da cultivar Tifton 85 em sistemas sob irrigação e sob aplicação de DLS. Para determinar a produção de matéria seca pré-pastejo de Tifton 85 com DLS, foi conduzido um experimento na Fazenda-Escola da Universidade de Uberaba, irrigado por aspersão em malha, com aplicação de 0; 50; 100 e 200 m³ ha-1 ano-1 de DLS. Houve efeito significativo das doses de DLS em relação à produção de matéria seca pré-pastejo, ocorrendo acréscimos de produção com o aumento das doses. O fornecimento de 200 m³...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação de pastagem; Água residuária; Aspersão em malha.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200010

Tensão superficial estática de soluções aquosas com óleos minerais e vegetais utilizados na agricultura
Provedor de dados: 70
Autores: Mendonça,Cristina G. de; Raetano,Carlos G.; Mendonça,Cristiane G. de.
O trabalho teve como objetivo avaliar a tensão superficial estática de soluções aquosas com formulações de óleos minerais e vegetais emulsionáveis utilizados como adjuvantes na agricultura. Os óleos minerais e vegetais, quando adicionados aos produtos fitossanitários, podem imprimir características desejáveis à calda de pulverização, como reduzir a tensão superficial em soluções aquosas, possibilitar maior contato da calda com a superfície vegetal ou reduzir o potencial de deriva durante as pulverizações. Foram testados os seguintes produtos comerciais: óleos minerais (Assist, Attach, Dytrol, Iharol, Mineral Oil, Spinner, Sunspray-E e Triona) e óleos vegetais (Agrex'oil Vegetal, Crop Oil, Natur'l Óleo, Óleo Vegetal Nortox e Veget Oil), todos com registro...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adjuvante; Tecnologia de aplicação; Tensão superficial.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200003

Características físicas e mecânicas do endocarpo e da amêndoa da castanha de caju 'CCP 76' antes e após tratamento térmico
Provedor de dados: 70
Autores: Araújo,Max C. de; Ferraz,Antonio C. de O.
As características viscoelásticas da casca da castanha de caju in natura dificultam a sua decorticação por compressão. Para facilitar a abertura da casca e a liberação da amêndoa, as castanhas são submetidas à hidratação e tratamento térmico em banho de líquido da casca da castanha (LCC) a 210 ºC. Com o objetivo de conhecer o comportamento do produto, para futuros desenvolvimentos de mecanismos decorticadores, procurou-se caracterizar a castanha do clone 'CCP 76' por meio das principais dimensões, massa, volume e ensaios mecânicos do endocarpo e da amêndoa, antes e após o tratamento térmico. Os tratamentos consistiram em várias combinações de tempo de hidratação e tempo de residência em banho de LCC. Aplicou-se a metodologia de superfície de resposta para...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anacardium ocidentale; Viscoelasticidade; Propriedades mecânicas.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300017

DAMS SAFETY INDEX (DSI): A REASSESSMENT OF THE PARAMETERS OF ANALYSIS
Provedor de dados: 70
Autores: Garcia,Lucas do C.; Martim,André L. S. S.; Dalfré Filho,José G.; Fais,Laura M. C. F.
ABSTRACT Dams provide a water supply, irrigation and power generation. However, the economic, social and environmental impacts are serious when they rupture. It is important that dams continue to function properly and are constantly evaluated for their safety and functionality. Contrary to general belief, small dams are the ones that present the most problems, because they are often built without adequate design and construction methods. One of the methods to evaluate the safety of a dam is through the Dam Safety Index (DSI), which may not entirely avoid subjectivity in dam safety assessment but does propose balanced individual subjectivities in determining the weights of the index criteria. The DSI can also assist managers with preventive maintenance...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dam Safety Index; Small dams; Statistical weighting.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600715

Características espectrais da soja ao longo do ciclo vegetativo com imagens landsat 5/TM em área agrícola no oeste do Paraná
Provedor de dados: 70
Autores: Mercante,Erivelto; Lamparelli,Rubens A. C.; Uribe-Opazo,Miguel A.; Rocha,Jansle V.
O objetivo deste trabalho foi estudar as mudanças no comportamento espectral da cultura da soja, por meio dos perfis espectrais temporais dos índices de vegetação NDVI e GVI, expressos em diferentes valores físicos: fator de reflectância bidirecional (FRB) aparente, de superfície e normalizado derivados de imagens Landsat 5/TM. Foi monitorada área de cultura de soja localizada próxima ao município de Cascavel - PR, utilizando cinco imagens da safra de 2004/2005, sendo realizados nessas imagens os procedimentos de transformação radiométrica, correção atmosférica e normalização, determinando valores físicos dos fatores de reflectância bidirecional aparente, de superfície e normalizado, respectivamente. Com o intuito de caracterizar a resposta espectral da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Imagens orbitais; Correção atmosférica; Normalização de imagens.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200016

Média diária do déficit de pressão de saturação do vapor d'água do ar e sua influência na vapotranspiração de referência pelo modelo de penman-monteith (FAO 56) em Piracicaba - SP
Provedor de dados: 70
Autores: Lyra,Gustavo B.; Pereira,Antonio R.; Sediyama,Gilberto C.; Lyra,Guilherme B.; Santiago,Alailson V.; Folegatti,Marcos V.
Utilizando-se como padrão as medidas lisimétricas de um gramado, avaliaram-se os resultados de estimativas de ETo obtidas com Dar_méd oriundos de 14 métodos para seu cálculo. Tais comparações permitiram separar os métodos de cálculo de Dar_méd em três grupos, ou seja: um grupo resultou sempre em superestimativa de ETo; em outro, a tendência foi de sempre subestimar, e no último a tendência foi de superestimar valores baixos (&lt; 4,5 mm dia-1) e de subestimar valores altos de ETo. Não foram observadas diferenças significativas (teste t; p &lt; 0,05) de ETo, em função dos métodos de Dar_méd ao utilizar a média horária da temperatura e/ou umidade relativa do ar em relação aos determinados com a média dos valores máximo e mínimo desses elementos. Dos métodos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pressão de saturação do vapor d'água; Equação combinada; Análise de sensibilidade.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200011

ECOLOGICAL-ECONOMIC ZONING OF THE CITY OF ALTINÓPOLIS – SP, BRAZIL
Provedor de dados: 70
Autores: Crivelenti,Rafael C.; Bueno,Célia R. P.; Pires,José S. R.; Francisco,José; Lessi,Bruno F.
ABSTRACT: Since colonial times, Brazilian land use has been made under an extractivist model at the expense of deforestation, increasing soil and vegetation depletion, stream siltation, as well as loss of biodiversity. An ecological-economic zoning (EEZ) has been taken as feasible alternative to guide public policies aimed at city land-use planning. This study focused on designing an EZZ for the city of Altinópolis, in São Paulo state (Brazil), by means of geographical information systems (GIS). Information and maps delineated six land-use areas, in which 30% covered areas under environmental protection, 45% over areas with groundwater recharge potential, which should be intended to restoration. Furthermore, around 70% of the territory show potential to be...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geographical information systems; Soil and water preservation; Environmental planning; Land use.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601218

Mathematical simulation parameters for drying of cassava starch pellets
Provedor de dados: 70
Autores: Moreno,Fabian L.; Parra-Coronado,Alfonso; Camacho-Tamayo,Jesus H.
Based on experimental tests, it was obtained the equations for drying, equilibrium moisture content, latent heat of vaporization of water contained in the product and the equation of specific heat of cassava starch pellets, essential parameters for realizing modeling and mathematical simulation of mechanical drying of cassava starch for a new technique proposed, consisting of preformed by pelleting and subsequent artificial drying of starch pellets. Drying tests were conducted in an experimental chamber by varying the air temperature, relative humidity, air velocity and product load. The specific heat of starch was determined by differential scanning calorimetry. The generated equations were validated through regression analysis, finding an appropriate...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Specific heat; Latent heat vaporization; Moisture equilibrium content; Rate drying.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600018

Operational performance of the mechanized and semi-mechanized potato harvest
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Martins,Daniel H.; Cunha,Walter G. da.
Potato is an important crop plant throughout the world. Harvesting is a fundamental step in its production system. Maybe, it is the most complex and expensive operation. Thus, the objective of this work was to compare the cost of the mechanized and semi-mechanized harvest, the operational capacity and the production losses during the potato harvest process. The work was accomplished in a commercial farming, cultivated under pivot system, in the municipal district of Perdizes - MG, Brazil. A completely randomized design with two treatments was used: mechanized and semi-mechanized harvest. The mechanized harvest used a self-propelled harvester. In the semi-automated harvest, a digger mounted on tractor was used and the potato was manually harvested. It was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mechanical harvest; Field efficiency; Operational cost; Solanum tuberosum.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400020

Agricultura de precisão: particularidades de sua adoção no sudoeste de Goiás – Brasil
Provedor de dados: 70
Autores: Soares Filho,Romeu; da Cunha,João P. A. R.
RESUMO A agricultura de precisão tem nos solos do Cerrado Brasileiro um perfeito campo para seu desenvolvimento. Há, entretanto, na região, carência de informações sobre o estado da arte desta nova técnica, já em uso por alguns produtores rurais. Com isso, objetiva-se com este trabalho realizar a análise da adoção e da utilização desta tecnologia na região sudoeste do Estado de Goiás, com informações reais da intensidade e da forma de uso e das condicionantes de sua adoção. Para tanto, foi aplicado um questionário a produtores que utilizavam de alguma forma a agricultura de precisão, analisando os problemas enfrentados com a tecnologia, as fontes de informação e as dificuldades encontradas pelos produtores. Para amostragem, foi utilizado o método não...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia agropecuária; Mecanização agrícola; Distribuidores a lanço.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400689

MODELING SOIL WATER REDISTRIBUTION UNDER SURFACE DRIP IRRIGATION
Provedor de dados: 70
Autores: Arraes,Francisco D. D.; Miranda,Jarbas H. de; Duarte,Sergio N.
ABSTRACT The main objective of this study was to develop a numerical model to simulate water distribution, and the shape of the wetted soil volume, resulting from a point source irrigation at the ground surface (dripper), given soil hydraulic properties and irrigation system parameters. The mathematical model was developed in Fortran 90 at the Department of Biosystems Engineering, at the Luiz de Queiroz College of Agriculture, ESALQ/USP. The computer program was structured to allow the user to input information such as: a) flow and transport related to soil properties, b) information on irrigation type, c) boundary conditions, d) simulation time, and e) water application time through irrigation. Data from another experiment carried out at the Department of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wet Bulb; Finite Differences; Trickle Irrigation.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100055

THERMAL ENVIRONMENT OF TABLE GRAPE PACKING HOUSES IN THE SÃO FRANCISCO VALLEY
Provedor de dados: 70
Autores: Vasconcelos,Osvaldo; Turco,Sílvia; Dacanal,Cristiane; Luz,Simone; Freitas,Sergio.
ABSTRACT The aim of this study was to characterize the thermal environment of the sorting and packing sectors of small, medium and large packing houses in the São Francisco Valley, Northeast of Brazil. Micrometeorological data were monitored every 15 minutes for 20 days during winter 2014 and summer 2015. The parameters evaluated were air temperature (°C), relative humidity (%) and radiant thermal load, RTL,(W/m2). External environmental data were obtained from weather stations close to the packing houses. The data obtained show that packing houses minimum and maximum temperatures were reached at 6am and 3pm, respectively, during winter and summer. Both seasons had air temperatures above 20°C, relative humidity below 90% and radiant thermal load above 450...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal environment; Performance; Agricultural facilities.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100035

IRRIGATION WATER MANAGEMENT TECHNIQUES FOR LOWLAND FURROW-IRRIGATED SOYBEAN IN SOUTHERN BRAZIL
Provedor de dados: 70
Autores: Gollo,Elisa A.; Robaina,Adroaldo D.; Peiter,Marcia X.; Goulart,Rafael Z.; Chaiben Neto,Miguel.
ABSTRACT Different water management strategies should be investigated to ensure adequate water supply to furrow-irrigated soybean plants in lowlands. This study examined the performance and efficiency of furrow irrigation techniques and related them to the soybean yield potential in lowland fields of Southern Brazil in the 2017/18 growing season. An experiment was conducted on raised seedbeds to evaluate furrow irrigation techniques: full irrigation with cutback, irrigation during the advance phase with low inflow, irrigation during the advance phase (cutoff), surge irrigation, and no irrigation. The design parameters, efficiency of the techniques, agronomic characteristics, and the grain yield of the soybean crop, were evaluated. The overall performance...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Surface irrigation; Crop irrigation in raised seedbeds; Design and evaluation of irrigation systems; Soybean yield potential.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200127

Estimativa da batimetria do açude do Saco-PE com auxílio de dados orbitais
Provedor de dados: 70
Autores: Lima,Josimar R. da C.; Shinozaki-Mendes,Renata A.; Almeida,André Q. de.
A batimetria de um corpo d'água pode ser medida em campo, a partir de sondas batimétricas; no entanto, é um processo oneroso e que demanda tempo. Com isso, o objetivo principal deste estudo foi ajustar modelos de estimativa de batimetria de um lago a partir de dados orbitais. O trabalho foi realizado no açude do Saco, localizado na bacia hidrográfica do Rio Pajeú, na cidade de Serra Talhada - PE. Foram ajustados modelos de regressão entre os valores batimétricos, coletados com auxílio de uma sonda, as bandas espectrais verde e infravermelho próximo do satélite Landsat 5 TM e o índice da diferença normalizada da água. A avaliação dos modelos ajustados foi realizada pela análise do coeficiente de determinação, do erro quadrado médio e da eficiência do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Landsat; NDWI; Rio Pajeú; Sensoriamento remoto.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500013

Uso de ardósia na construção de celas de maternidade para suínos: II - ambiente térmico e avaliação dos ruídos
Provedor de dados: 70
Autores: Castro,Jaqueline de O.; Ferreira,Rony A.; Campos,Alessandro T.; Yanagi Junior,Tadayuki; Tadeu,Hugo C.
Este trabalho teve o objetivo de avaliar o ambiente térmico e o ruído em celas de maternidade para suínos com divisórias de alvenaria ou com rochas de ardósia. Para as medidas das variáveis de conforto térmico e de ruídos, utilizaram-se de termômetros e decibelímetro. No interior das celas e para a análise estatística, foram usados doze matrizes e cento e trinta e nove leitões, distribuídos em delineamento em blocos casualizados, em esquema de parcelas subdivididas. Os resultados mostraram que, no período da manhã, em ambos os tratamentos, as condições de conforto térmico foram mais adequadas para as matrizes, enquanto no período da tarde, mais adequadas para os leitões; com relação ao ruído, este foi menor nas celas de alvenaria. De forma geral, o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência; Ruído; Divisórias; Maternidade de suínos.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100005

Comportamento da alface tipo americana sob diferentes tensões da água no solo, em ambiente protegido
Provedor de dados: 70
Autores: Santos,Silvânio R. dos; Pereira,Geraldo M.
Visando a definir critérios para o manejo da irrigação para alface tipo americana, cv. Raider, esse trabalho foi desenvolvido para avaliar o efeito de diferentes tensões da água no solo sobre o comportamento produtivo da cultura, em ambiente protegido, na região de Lavras - MG. O experimento foi instalado em casa de vegetação com delineamento em blocos casualizados, tendo quatro repetições. Os tratamentos foram constituídos de seis tensões de água no solo como indicativas do momento de irrigar. As tensões preestabelecidas foram 15; 30; 45; 60; 75 e 90 kPa, à profundidade de 0,15 m. Os resultados permitiram concluir que, no emprego de tensões em torno de 15 kPa, há tendência em obter plantas mais altas, com maior peso de matéria fresca comercial e menor...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação por gotejamento; Manejo da irrigação; Estresse hídrico.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300009

Correlação linear e espacial entre produtividade de Brachiaria brizantha, densidade do solo e porosidade total em função do sistema de manejo do solo
Provedor de dados: 70
Autores: Vitória,Edney L. da; Fernandes,Haroldo C.; Teixeira,Mauri M.; Cecon,Paulo R.; Lacerda,Elcio Das G.
A densidade e a porosidade são propriedades físicas do solo que são alteradas em função do sistema de manejo utilizado, com consequente influência sobre a produtividade das culturas. A produtividade da planta forrageira, Brachiaria brizantha, em função da densidade do solo e da porosidade total foi analisada em dois sistemas de manejo de solo, em experimento conduzido no segundo semestre de 2009, no município de Santa Teresa, no Estado do Espírito Santo. O objetivo foi estudar a variabilidade e as correlações lineares e espaciais entre os atributos da planta e do solo, visando a selecionar um indicador da qualidade física do solo de boa representatividade para produtividade de forragem. Marcaram-se duas parcelas de 40 m por 50 m a cada 5 m, em duas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Propriedades físicas do solo; Geoestatística; Preparo do solo; Forragicultura.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500010

Caracterização de dois equipamentos de beneficiamento e classificação de tomates para mesa
Provedor de dados: 70
Autores: Franco,André T. O.; Ferreira,Marcos D.; Magalhães,Ana M. de; Ferraz,Antonio C. de O.; Tavares,Marcelo.
No Brasil, nos últimos anos, tem aumentado o beneficiamento e a classificação de frutas e hortaliças em equipamentos. O objetivo deste trabalho foi caracterizar a etapa de limpeza de dois equipamentos de beneficiamento de tomate de mesa, um nacional e outro importado, instalados na região metropolitana de Campinas - SP. A caracterização foi realizada quanto ao número, tipo e velocidade de rotação das escovas, aplicação de água, tempo de permanência dos frutos e eficiência de limpeza. O tempo de permanência foi mensurado com relação ao tamanho dos frutos, segundo os padrões da CEAGESP. Para mensurar a eficiência, foi desenvolvido um equipamento composto de um anel deslizante envolvido por um pano branco. As amostragens foram realizadas antes e após a etapa...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lycopersicon esculentum Mill; Eficiência de limpeza; Tempo de permanência.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400023

Material envoltório na drenagem subterrânea
Provedor de dados: 70
Autores: Almeida,Florício P. de; Lima,Vera L. A. de; Azevedo,Carlos A. V. de; Dantas Neto,José; Pordeus,Roberto V.
Em solos de baixa estabilidade estrutural, o transporte, pela água, de partículas do solo para o interior do tubo drenante pode contribuir para o colapso de sistemas de drenagem, devendo o mesmo ser evitado com o uso adequado de envoltório, considerando a importância da drenagem para uma produção agrícola sustentável. Diante disso, esta pesquisa foi realizada com o objetivo de estudar o comportamento de três materiais envoltórios, sendo dois amplamente utilizados, bidim OP-20 e brita zero, e outro composto de espuma com 5 mm de espessura, que é um material não-convencional. Os tubos drenantes utilizados foram o Drenoflex e o Kananet, com diâmetro nominal de 65 e 75 mm, respectivamente. O desempenho dos envoltórios foi avaliado pela resistência de entrada e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas drenantes; Material não-convencional; Resistência de entrada.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300012

Avaliação da dinâmica do cultivo da cana-de-açúcar no estado de São Paulo por meio de perfis temporais de dados MODIS
Provedor de dados: 70
Autores: Antunes,João F. G.; Lamparelli,Rubens A. C.; Rodrigues,Luiz H. A.
RESUMO As imagens do sensor MODIS fornecem dados que cobrem áreas de grande extensão com alta periodicidade, características fundamentais que possibilitam o monitoramento de culturas agrícolas estratégicas para o Brasil, como as da cana-de-açúcar. Técnicas matemáticas vêm sendo empregadas no estudo de longas séries temporais de índices de vegetação, baseado nas mudanças que acontecem na superfície terrestre, o que facilita o entendimento da dinâmica temporal. O objetivo deste trabalho foi realizar a avaliação da dinâmica do cultivo da cana-de-açúcar no Estado de São Paulo por meio de perfis temporais de dados MODIS, ao longo das safras de 2004/2005 a 2011/2012. A Transformada de Wavelet Daubechies 8 aplicada à série temporal do EVI2 do MODIS mostrou ser...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensoriamento remoto; Processamento de imagens; Índice de vegetação; Séries temporais.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601127

SPATIAL, SEASONAL, AND TEMPORAL VARIATIONS IN RAINFALL AGGRESSIVENESS IN THE SOUTH OF BRAZIL
Provedor de dados: 70
Autores: Back,Álvaro J.; Gonçalves,Fabiane N.; Fan,Fernando M.
ABSTRACT The objective of this study is to evaluate spatial and temporal variations in rainfall aggressiveness in southern Brazil. A total of 181 rain gauge stations located in southern Brazil with rainfall time series from 1976 to 2015 were used. Seasonal and annual rainfall aggressiveness values measured according to the Modified Fournier Index (MFI) were analyzed. The trends in the data series were evaluated using the Mann-Kendall test at a level of significance of 5%. Maps on spatial and seasonal variations in rainfall aggressiveness were prepared. The percentage of rain gauge stations with significant decreasing trends, significant increasing trends, and no significant trends in rainfall aggressiveness between years was 3.3%, 7.7%, and 89.0%,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosivity; Soil conservation; Precipitation; Climatic trends.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400466

Efficiency of water use in sunflower grown in hydroponic system under saline stress
Provedor de dados: 70
Autores: Santos Júnior,José Amilton; Gheyi,Hans R.; G. Filho,Doroteu H.; Soares,Frederico A. L.; Dias,Nildo da S.
In order to identify alternatives for the use of saline water in agricultural production, the effects of the use of brackish water in the preparation of the nutrient solution for the cultivation of sunflower (cv. EMBRAPA 122-V2000) were studied in hydroponic system on consumption and efficiency of water use for the production of achenes and biomass. A completely randomized design was used, analyzed in a 5x2 factorial scheme with three replications. The factors studied were five levels of salinity of nutrient solution (1.7 - control; 4.3; 6.0; 9.0; and 11.5dS m-1) and two plant densities - one or two plants per vessel. It was concluded that the water consumption of sunflower is a variable sensitive to the salinity of the nutrient solution, especially after...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Salinity; Plant density; Soilless culture; Helianthus annuus L.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400011

Avaliação dos comportamentos de aves poedeiras utilizando seqüência de imagens
Provedor de dados: 70
Autores: Barbosa Filho,José A. D.; Silva,Iran J. O.; Silva,Marco A. N.; Silva,Caio J. M.
A grande preocupação com o uso de gaiolas dá-se quanto ao espaço oferecido às aves poedeiras, o qual, certamente, afeta seu bem-estar. Sendo assim, este trabalho teve o objetivo de avaliar aspectos relacionados ao comportamento e bem-estar animal, comparando o sistema de criação alternativo (com cama e ninho) com o sistema convencional em gaiolas. Para isso, dois grupos de 20 aves (10 Hy-Line W36 e 10 Hy-Line Brown) em início de produção foram divididos em dois sistemas de criação (cama+ninho e gaiolas) e colocadas em câmara climática: um grupo a 26 °C e 60% UR (condição de conforto térmico), e outro a 35 °C e 70% UR (condição de estresse térmico), onde eram constantemente monitoradas por câmeras de vídeo. Com base na análise dos comportamentos,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bem-estar animal; Comportamento animal; Análise de imagens.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100002

CARACTERIZAÇÃO DE ESTAÇÕES DE BOMBEAMENTO EM LAVOURAS DE ARROZ DO RIO GRANDE DO SUL
Provedor de dados: 70
Autores: KÖPP,LUCIANA M.; PEITER,MARCIA X.; ROBAINA,ADROALDO D.; TOESCHER,CARLOS F.
Resumo A importância da lavoura de arroz irrigado no contexto nacional e o elevado uso de água e energia motivaram este trabalho, que teve por objetivo caracterizar estações de bombeamento (EB) presentes nos sistemas de irrigação, na fronteira oeste do Rio Grande do Sul (RS). Foram avaliadas 160 EBs e obtidas as seguintes informações: área de cultivo; vazão; altura geométrica de sucção e de recalque; comprimento e diâmetro das tubulações de sucção e de recalque; identificação das peças especiais usadas nas tubulações; potência ativa e identificação da marca e do modelo de bomba e motor. Com estes dados, foram estimados a altura manométrica, o rendimento global e os índices de desempenho. Os resultados mostram médias de 13,2 m de altura manométrica, 57% de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Estações elevatórias; Bombas hidráulicas; Irrigação superficial; Sistemas de bombeamento.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200342

Pastejo e adubação nitrogenada sobre os atributos físicos do solo em sistema de integração lavoura-pecuária
Provedor de dados: 70
Autores: Andreolla,Veruschka R. M.; Moraes,Aníbal de; Bona Filho,Amadeu; Cardoso,Decio L.; Oliveira,Edilson B. de; Bonini,Andreia K.
RESUMO O sistema de integração lavoura-pecuária (SILP) é uma alternativa que vem atraindo grande interesse dos agricultores nas regiões produtoras de grãos, devido ao suporte à pecuária por meio da produção de alimento, além de melhoria nas propriedades físicas do solo. O objetivo deste trabalho foi avaliar o efeito do pastejo e da adubação nitrogenada em atributos físicos do solo e na produtividade da cultura do milho, em um sistema de integração lavoura-pecuária. O delineamento foi em blocos ao acaso, com parcelas subdivididas, sendo as parcelas as doses de nitrogênio, e as subparcelas, a presença e ausência de pastejo. Foram utilizadas três repetições por tratamento. Os tratamentos foram doses de nitrogênio de 0; 75; 150 e 225 kg ha-1 aplicados na...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas integrados; Compactação do solo; Azevém; Aveia; Pastagem.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601019

SEMIAUTOMATIC IRRIGATION MANAGEMENT IN TOMATO
Provedor de dados: 70
Autores: Souza,Claudinei F.; Conchesqui,Maria E. S.; Silva,Marília B. da.
ABSTRACT The use of new technologies to meet the demands of the agricultural market is increasing; however, technical information on application is scarce for some areas of knowledge, including irrigation management. The objective of this study is to evaluate an automatic irrigation system with capacitance sensors connected to a local wireless network for the semiautomatic management of irrigation in tomato crops compared with a manual control system based on time-domain reflectometry (TDR)-type sensors. The experiments were carried out in a protected environment, and the seedlings were transplanted following surface drip lines. The study adopted a completely randomized block design consisting of two treatments and 12 repetitions, totaling 24 subplots. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digital assistant; Irrigation management; TDR; Capacitance; Solanum lycopersicum L.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800118

Influência de variáveis climáticas e hidráulicas no desempenho da irrigação de um pivô central no oeste baiano
Provedor de dados: 70
Autores: Pinto,Jacques M.; Silva,Cícero L. da; Oliveira,Carlos A. da S.
Este trabalho foi conduzido na Fazenda Moreno, localizada no município de Barreiras, oeste baiano, com o objetivo de avaliar o desempenho de um pivô central, em função de variáveis climáticas e hidráulicas ligadas à eficiência de irrigação, em três períodos do ano e duas velocidades de rotação da linha lateral do equipamento. Os três períodos de coletas dos dados foram 12 e 18-5-2002 (primeira época), 27 e 28-7-2002 (segunda época) e 28 e 29-9-2002 (terceira época), respectivamente, para 100 e 50% da velocidade máxima de deslocamento do pivô. Os resultados foram analisados em blocos casualizados para o fator velocidade de deslocamento do pivô, com o fator época do ano em subparcela. O sistema avaliado apresentou pressão no final da linha lateral, menor que...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coeficiente de uniformidade de Christiansen; Eficiência de distribuição; Eficiência de aplicação.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100009

Utilização de sistemas fototérmicos com concentradores para higienização de salas de ordenha
Provedor de dados: 70
Autores: Altoé,Leandra; Oliveira Filho,Delly.
Neste trabalho, analisou-se a viabilidade do uso de concentradores de radiação solar em sistemas fototérmicos para higienização de salas de ordenha. Foram analisadas três opções para aquecimento de água com reservatório de acumulação: sistema com resistência elétrica, sistema solar com concentrador e sistema solar sem concentrador. Calculou-se o custo total dessas alternativas e o valor presente líquido do sistema solar suplementado por lenha de eucalipto comprada, lenha de eucalipto produzida na propriedade rural, energia elétrica e gás liquefeito de petróleo (GLP). Realizou-se uma análise de sensibilidade do sistema fototérmico variando o número de vacas lactantes, o custo da energia elétrica e da lenha, a taxa de juros, o custo dos componentes do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energia solar; Aquecimento de água; Produção de leite.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500003

PHYSICAL-MECHANICAL CHARACTERIZATION OF Eucalyptus urophylla WOOD
Provedor de dados: 70
Autores: Lahr,Francisco A. R.; Nogueira,Marta C. De J. A.; Araujo,Victor A. De; Vasconcelos,Juliano S.; Christoforo,André L.
ABSTRACT: Eucalyptus urophylla consists in a wood-producing species, which offers a natural multiple raw material of good quality for applications in rural and civil constructions. However, Eucalyptus urophylla still has a small utilization as building parts and elements, resulting from the possible ignorance and low diffusion of its structural possibilities. Thereby, the present research aims to measure the main thirteen mechanical properties of Eucalyptus urophylla wood for two different moisture contents, 12% and 30% (green wood). Furthermore, in these two conditions of moisture content evaluation, volumetric mass densities were also evaluated. At the end of this evaluation, which included 2688 determinations, all the obtained results were statistically...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Timor White Gum; Strength modulus; Cracking; Shear stress; Hardness; Density.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500900

INSECTICIDE SPRAYING IN SOYBEAN PLANTS: DIFFERENT NOZZLES MODELS AND AGROMETEOROLOGICAL CONDITIONS
Provedor de dados: 70
Autores: Costa,Lilian L.; Aquino,Nathan C. R. De Moura; Carneiro,Ângela L. C. G.; Almeida,Dieimisson P.; Ferreira,Marcelo Da C.
ABSTRACT The aim of the experiment was to evaluate the quality of the spraying by the spray volume deposit provided by different nozzles models in two agrometeorological conditions of application. Four parameters related to spray quality were evaluated: spray volume deposit, droplet size, surface tension and contact angle. The treatments consisted of three nozzle models (AXI Twin 12002, TTJ 110015 and JAI 120015) and two application times (between 02:00 p.m. and 04:00 p.m. and between 08:00 a.m. and 09:30 a.m.). The spray volume deposit in the upper portion of the soybean plants was similar, but the JAI 120015 nozzle model produces more uniform droplet spectra and is safer than the AXI Twin 12002 and TTJ 110015 due to the highest drift risk. It is...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spray volume deposit; Application time; Phytosanitary product; Application technology.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500673

Simulation of moisture profiles in a Latossol in Dourados region, in the State of Mato Grosso do Sul, Brazil
Provedor de dados: 70
Autores: Scorza Júnior,Rômulo P.; Silva,João P. da; Rigitano,Renê L. de O.
The understanding of unsaturated soil water flow at process-level is essential to develop proper management actions for environmental protection in agricultural systems. One important tool for simulation of soil water flow that has been used worldwide is the SWAP model. The aim of this work was to test and to calibrate the SWAP model by inverse modeling to describe moisture profiles in a Brazilian very clayey Latossol in Dourados, State of Mato Grosso do Sul, Brazil. The SWAP model was tested in an experimental field of 0.09 ha cultivated with soybean and soil profiles were sampled eight times between December 2006 and October 2007. The SWAP input values (i.e. soil water retention curves and meteorological data) were based on in-situ measurements....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil water flow; SWAP; Inverse modeling.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100003

SIMULATION OF VENTILATION SYSTEMS IN A PROTECTED ENVIRONMENT USING COMPUTATIONAL FLUID DYNAMICS
Provedor de dados: 70
Autores: Silva,Roberto C. da; Cordeiro Júnior,José J. F.; Pandorfi,Héliton; Vigoderis,Ricardo B.; Guiselini,Cristiane.
ABSTRACT Computational simulations of mass and energy flow help in implementing alternative cooling systems in protected environments. The aim of this study was to model and simulate the interaction between external and internal environments of a protected environment by means of computational fluid dynamics (CFD) techniques and validate micrometeorological variables for subsequent comparison between natural and indirect ventilation by ground heat exchangers. At the first phase, the micrometeorological variables global solar radiation (Qg), air temperature (Tair), and air relative humidity (RH) were monitored. The second phase consisted of the numerical modeling of finite volumes, with validation through recorded data, as well as simulation and comparison...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Numerical simulation; Micrometeorology; Protected cultivation; Finite elements.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300414

Utilização do tanque Classe A para a estimativa da evapotranspiração de referência dentro de casa de vegetação
Provedor de dados: 70
Autores: Fernandes,Carolina; Corá,José E.; Araújo,Jairo A. C. de.
O trabalho teve como objetivos estimar a evapotranspiração de referência (ETo) dentro e fora de casa de vegetação, pelo método do tanque "Classe A", utilizando-se de dois valores de Kp e estabelecer correlações entre a ETo, dentro e fora da casa de vegetação, buscando evitar a instalação do tanque "Classe A" dentro da mesma. O experimento foi conduzido na Faculdade de Ciências Agrárias e Veterinárias, Câmpus de Jaboticabal - SP. Instalaram-se dois tanques "Classe A", um dentro e outro fora da casa de vegetação. Para o tanque instalado dentro da casa de vegetação, utilizaram-se dois coeficientes de tanque: Kp = 0,7 e Kp = 1,0. Para o tanque instalado fora da casa de vegetação utilizou-se Kp = 0,85. Constatou-se que a ETo dentro da casa de vegetação foi...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiração de referência; Coeficiente de tanque.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100006

EXTRACTION CAPACITY OF GRASSES GROWN IN CONSTRUCTED WETLAND SYSTEMS USING DIFFERENT ARRANGEMENTS AND SUBSTRATES
Provedor de dados: 70
Autores: Saraiva,Claudety B.; Matos,Antonio T.; Matos,Mateus P. de.
ABSTRACT Constructed wetland systems have been used to treat different wastewater; among their essential components are the cultivated plant species and type of substrate used to fill them. The choice of plant species and type of substrate are important for the good system performance in wastewater treatment. This study aimed to evaluate the extraction capacity of Napier and Tifton 85 grasses when cultivated at different positions in horizontal subsurface flow constructed wetlands (HSSF-CWs) filled with different substrates in wastewater treatment from a bulk milk-cooling tank (MTWW). The experimental unit consisted of four HSSF-CWs, in which an average surface organic loading rate of 318 kg ha−1 d−1 of BOD5,20 was imposed and a hydraulic holding time of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wastewater; Forage; Nutrients; Built wetlands.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500668

Effective diffusivity and convective mass transfer coefficient during the drying of bananas
Provedor de dados: 70
Autores: Silva,Cleide M. D. P. da S. e; Silva,Wilton P. da; Farias,Vera S. de O.; Gomes,Josivanda P.
In this article, a methodology is used for the simultaneous determination of the effective diffusivity and the convective mass transfer coefficient in porous solids, which can be considered as an infinite cylinder during drying. Two models are used for optimization and drying simulation: model 1 (constant volume and diffusivity, with equilibrium boundary condition), and model 2 (constant volume and diffusivity with convective boundary condition). Optimization algorithms based on the inverse method were coupled to the analytical solutions, and these solutions can be adjusted to experimental data of the drying kinetics. An application of optimization methodology was made to describe the drying kinetics of whole bananas, using experimental data available in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drying kinetics; Algorithm optimization; Diffusion; Porous media.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200014

Clones, substrates and environments for seedlings of rubber tree rootstocks
Provedor de dados: 70
Autores: Vieira,Noemi C. de S.; Maruyama,Wilson I.; Costa,Edilson; Dias,Pamella M.; Pereira,Amanda C.
ABSTRACT The objective of this study was to evaluate the growth of rubber clones GT1, PR255, RRIM600 grown on different substrates and environments for the production of rubber rootstocks. The experiment was conducted at the Universidade Estadual de Mato Grosso do Sul, Cassilândia University Unit, in Cassilândia-MS. The treatments were conducted in 3 environments: (A1): Sombrite®; (A2) Aluminet® and (A3) full sun, where the clones being tested were: GT1; PR 255 and RRIM 600, grown in substrates: pure soil; soil + cattle manure and commercial substrate usually used for forestry. The experimental design was a randomized block in a factorial 3 x 3 (three substrates x three clones), with 4 replicates with 10 seedlings of rubber trees per plot. The use of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hevea brasiliensis; GT1; PR255; RRIM600; Screens.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500749

Coeficiente de descarga em emissores de pivô central
Provedor de dados: 70
Autores: Silva,Renato M. da; Coelho,Rubens D.; Faria,Lucas do A.; Maschio,Rafael.
Este trabalho foi desenvolvido com o objetivo de determinar, em condições laboratoriais, o coeficiente de descarga (Cd) dos emissores fixos tipo “spray” (Senninger, Nelson e Fabrimar) utilizados em equipamentos pivô central no Brasil. Foram avaliados 45 bocais Senninger, 42 bocais Nelson e 36 bocais Fabrimar, com três repetições, totalizando 369 bocais ensaiados. As pressões de funcionamento variaram entre 6 e 30 PSI (41,37 a 206,84 kPa), com intervalo de leitura a cada 2 PSI (13,79 kPa), totalizando 13 pressões analisadas por bocal. Foram ajustadas as curvas do coeficiente de descarga em função do diâmetro de bocal, para quatro pressões de operação: 10; 15; 20 e 30 PSI (68,95; 103,42; 137,90 e 206,84 kPa). Utilizou-se de dois manômetros de precisão...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Hidráulica agrícola; Pressão de funcionamento; Aplicação de bocais.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300419

Comportamento da cultura do sorgo em função do tipo de rodas compactadoras e cargas verticais impostas na operação de semeadura
Provedor de dados: 70
Autores: Cortez,Jorge W.; Carvalho Filho,Alberto; Silva,Rouverson P.; Furlani,Carlos E. A.; Simonis,Daniel B.
O sorgo pode ser cultivado em áreas e situações ambientais secas e quentes, em que a produtividade de outros cereais é antieconômica. Quando a semeadura do sorgo é realizada de modo eficiente, os benefícios podem ser verificados em sua produtividade. O objetivo deste trabalho foi avaliar o comportamento da cultura do sorgo semeado sob três níveis de carga vertical impostas sobre as rodas compactadoras das semeadoras-adubadoras. O experimento foi conduzido na FAZU - Faculdades Associadas de Uberaba (MG), no delineamento em blocos ao acaso, no esquema de parcelas subdivididas, com três modelos de rodas compactadoras e três cargas verticais, com cinco repetições. Observou-se que não houve efeito dos tratamentos tipo de rodas compactadoras e cargas em relação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Emergência; Mecanização agrícola; Sorghum bicolor.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200014

Comparison of diffusion models for description of osmotic dehydration of radish slices dipped in brine
Provedor de dados: 70
Autores: Silva,Wilton P. da; Silva,Cleide M. D. P. da S. E; Gomes,Josivanda P.
ABSTRACT This paper aims at describing the osmotic dehydration of radish cut into cylindrical pieces, using one- and two-dimensional analytical solutions of diffusion equation with boundary conditions of the first and third kind. These solutions were coupled with an optimizer to determine the process parameters, using experimental data. Three models were proposed to describe the osmotic dehydration of radish slices in brine at low temperature. The two-dimensional model with boundary condition of the third kind well described the kinetics of mass transfers, and it enabled prediction of moisture and solid distributions at any given time.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Inverse method; Analytical models; Cylindrical geometry.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500894

Avaliação de intervenções em unidades de aplicação localizada de fertilizantes e de populações de milho
Provedor de dados: 70
Autores: Molin,José P.; Mascarin,Leonardo S.; Vieira Júnior,Pedro A.
A agricultura de precisão busca gerenciar os recursos disponíveis, enfatizando o aumento na produtividade e mantendo ou reduzindo a quantidade de insumos. Entre as técnicas para a aplicação em taxa variável, está aquela baseada na recomendação de um insumo em função da variabilidade espacial da oferta ambiental. O objetivo deste trabalho é avaliar a metodologia e analisar a viabilidade do uso de unidades de aplicação, variando a população de plantas de milho e a dose de fertilizante formulado na operação de semeadura, comparando a aplicação em taxa fixa e em taxa variável em relação à produtividade de grãos e ao total de insumos gastos. Foram realizados três experimentos: em dois deles, as doses de fertilizante formulado NPK foram aplicadas em taxas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Unidades de gerenciamento; Aplicação de insumos a taxa variada.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200022

Blindagem eletromagnética, aterramento e proteção contra surtos de tensão em equipamentos para monitoramento automático do teor de água no solo
Provedor de dados: 70
Autores: Teixeira,Claudia F. A.; Moraes,Sergio O.
O objetivo do presente trabalho foi implementar um sistema de blindagem eletromagnética, aterramento e proteção contra surtos de tensão na instalação de instrumental para o monitoramento automático do teor de água no solo. O experimento foi instalado em Piracicaba, São Paulo, em que os equipamentos utilizados foram um testador de cabos marca Tektronix, que opera pelo princípio da reflectometria no domínio do tempo e um sistema de aquisição de dados marca Campbell Scientific Inc. (CSI), que controla e analisa as formas de onda produzidas pelo testador de cabos. A umidade volumétrica foi obtida indiretamente por meio de sensores inseridos no solo, os quais medem a constante dielétrica do mesmo. Utilizaram-se tubos galvanizados para a blindagem...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Umidade do solo; Proteção eletrônica; Proteção magnética.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100027

The impact of the law 10,267/2001 in the brazilian rural registration
Provedor de dados: 70
Autores: Rosalen,David L.
The publication of the Law 10,267 of 08/28/2001 changed the paradigm of rural registration in Brazil, because this law known as the "Law of Georeferencing" has created the National Registration of Rural Property, that unifies in a common basis different registrations present in several government agencies, such as the National Institute for Colonization and Agrarian Reform (INCRA), the Secretariat of Federal Revenue, the Brazilian Institute of Environment and Natural Resources, and the National Indian Foundation. Also, this new registration system has a graphical component which has not existed until such date, where the boundaries of rural property are georeferenced to the Brazilian Geodetic System. This new paradigm has resulted in a standardization of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Georeferencing; Registration; Planning.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200018

CLIMATOLOGICAL WATER BALANCE WITH DATA ESTIMATED BY TROPICAL RAINFALL MEASURING MISSION FOR THE DOCE RIVER BASIN
Provedor de dados: 70
Autores: Louzada,Franciane L. R. de O.; Xavier,Alexandre C.; Pezzopane,José E. M.
ABSTRACT The Climatic Water Balance (CLIMWB) is very used in the climatic characterization and can also offer important contribution in the identification of the water demand for irrigation of a region. For this, reliable precipitation data with good spatial coverage is required. The Tropical Rainfall Measuring Mission satellite -TRMM-3B43-v7 is a partnership between NASA (National Aeronautics and Space Administration) and Japan's Aerospace Exploration Agency (JAXA), which estimates rainfall data for the tropics region. The aim of this study is to evaluate the CLIMWB obtained by the Thornthwaite &amp; Mather method (1955), with estimated rainfall data with the 3B43 product versus those generated with rainfall data and to map pixel-by-pixel water...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Orbital data; Rainfall; Water deficit; Water availability.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300376

Eficiência do processo de recobrimento de sementes de brócolos recobertas com polímero em leito de jorro
Provedor de dados: 70
Autores: Almeida,Celina de; Rocha,Sandra C. S.
Neste trabalho, sementes de brócolos foram recobertas em leito de jorro cone-cilíndrico, com suspensão aquosa de hidroxietilcelulose, visando a aprimorar a técnica do recobrimento de sementes, utilizando o processo fluidodinâmico. Foram investigados os efeitos das variáveis operacionais temperatura do ar de jorro, pressão de ar de atomização e vazão de suspensão de recobrimento, na eficiência do processo e na germinação das sementes. Os resultados revelaram que houve influência das variáveis operacionais na eficiência do processo e na germinação. Verificou-se, também, que as sementes recobertas apresentaram de 2 a 10% de umidade a menos que as sementes não-recobertas, quando em ambiente com temperatura controlada e saturado de vapor de água em determinado...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Germinação; Hidroxietilcelulose; Brassica oleracea.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200011

LEAF TEMPERATURE AND TRANSPIRATION OF PEQUI TREES WITH AND WITHOUT WATER RESTRICTION
Provedor de dados: 70
Autores: Miranda,Raiane F.; Alves Júnior,José; Casaroli,Derblai; Evangelista,Adão W. P.; Batisti,Rafael.
ABSTRACT The answers to when and how much to irrigate orchards can be obtained based on the measurements of plants' transpiration and leaf temperature. This study aims to determine the leaf temperature and sap flow of the pequi tree (Caryocar brasiliense Camb.), both with and without water restriction. Further, the leaf temperature was measured by infrared thermometry and estimated transpiration using the Granier method, where the thermal dissipation probes are inserted into the plant stems. The experiment was conducted in a 120-plant orchard located in Goiânia-GO, Brazil, from which seven of the plants (3 irrigated and 4 non-irrigated; aged 6.6–7.4 years) were evaluated for eight months (October 2015 to May 2016). The soil was characterized as a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Caryocar brasiliense Camb.; Water requirement; Water deficit; Brazilian Savannah.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500579

FUZZY MODEL FOR PREDICTING CLOACAL TEMPERATURE OF BROILER CHICKENS UNDER THERMAL STRESS
Provedor de dados: 70
Autores: Abreu,Lucas H. P.; Yanagi Junior,Tadayuki; Campos,Alessandro T.; Lourençoni,Dian; Bahuti,Marcelo.
ABSTRACT Broiler chickens submitted to different intensities and durations of thermal stress are subject to variation in cloacal temperature and, consequently, to a decrease in performance. Given the complexity of these interactions, artificial intelligence is a useful methodology for decision-making. Thus, this study aimed to assess and predict, by means of a fuzzy model, the cloacal temperature of broiler chickens submitted to thermal stress in the second week of life, with varying durations and intensities, in climatized wind tunnels. Mamdani's inference and defuzzification methods by means of the center of gravity were used. One hundred and twenty rules were elaborated. The developed fuzzy model was used to predict the cloacal temperature of broiler...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Physiological response; Thermal environment; Mathematical modeling; Fuzzy logic.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100018

Spatial variability of noise level in agricultural machines
Provedor de dados: 70
Autores: Yanagi Junior,Tadayuki; Schiassi,Leonardo; Rossoni,Diogo F.; Ponciano,Patrícia F.; Lima,Renato R. de.
The knowledge of the spatial variability of noise levels and the build of kriging maps can help the evaluation of the salubrity of environments occupied by agricultural workers. Therefore, the objective of this research was to characterize the spatial variability of the noise level generated by four agricultural machines, using geostatistics, and to verify if the values are within the limits of human comfort. The evaluated machines were: harvester, chainsaw, brushcutter and tractor. The data were collected at the height of the operator's ear and at different distances. Through the results, it was possible to verify that the use of geostatistics, by kriging technique, made it possible to define areas with different levels for the data collected. With...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Human environment; Acoustic comfort; Occupation health; Geostatistics.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200002

Cola à base de PVA e argamassa de solo-cimento como alternativas para o assentamento de alvenaria de tijolos maciços de solo-cimento
Provedor de dados: 70
Autores: Ferreira,Gisleiva C. dos S.; Moreno Júnior,Armando L.
Neste trabalho, foi analisada a viabilidade de emprego de cola à base de PVA e argamassa de solo-cimento no assentamento de paredes de alvenaria de tijolos maciços de solo-cimento, em substituição à argamassa usual (cimento, cal e areia). Pequenos prismas, executados com quatro tijolos maciços de solo-cimento e assentados com as argamassas e a cola de PVA, foram ensaiados à compressão e à flexão. Os resultados dos ensaios dos prismas executados com a argamassa de assentamento usual foram tomados como padrão esperado de comportamento para os outros prismas executados com argamassa de solo-cimento e com cola de PVA. Os resultados obtidos nos ensaios dos prismas indicaram que tanto cola à base de PVA quanto argamassa de solo-cimento podem ser empregadas,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avaliação experimental; Prismas de alvenaria; Resistência de aderência.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200004

BLADE ANGLE EFFECT ON DROPLET SIZE SPECTRUM OF ROTARY ATOMIZERS USED IN BRAZIL
Provedor de dados: 70
Autores: Carvalho,Fernando K.; Antuniassi,Ulisses R.; Chechetto,Rodolfo G.; Mota,Alisson A. B.; Kruger,Greg R.
ABSTRACT The effect of blade angle on droplet size spectrum of five rotary cage atomizers and one rotary disc atomizer used in Brazil was evaluated in a high speed wind tunnel, with an air speed of 180 km h−1. This study included the characterization of the droplet size spectrum, via laser diffraction instrument, generated by three blades angles, of 45, 60 and 75 degrees. The spray solution was composed of Picoxystrobin+ Cyproconazole fungicide (SC), at 20 mL c.p. L−1, and at a flow rate of 6 L min−1. As the angle decreased from 75 to 45 degrees, the rotational speed of the atomizers increased and the volume median diameter (VMD) decreased. However, increasing the rotational speed also increased the percentage of droplets smaller than 100 µm (% &lt; 100...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Atomization; Spray drift; Pesticides.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601118

Use of penetrometers in agriculture: a review
Provedor de dados: 70
Autores: Moraes,Moacir T. de; Silva,Vanderlei R. da; Zwirtes,Anderson L.; Carlesso,Reimar.
Soil physical quality can be easily and quickly evaluated by using simple equipment to identify levels of soil compaction. Hence, it is necessary to know the variables responsible for changes in the soil penetration resistance (SPR). The aim of this review is to identify the main factors related to the various equipment used for assessing SPR as a soil physical quality indicator in agriculture. This literature review describes the different types of equipment used and its relationship with SPR. A wide range of procedures, devices, and equipments are available. Much of variability in SPR results is related to the equipment model, cone angle and diameter, and penetration rate. Usually, restrictions to root growth are correlated with SPR values above 2-3 MPa....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Soil physics; Physical quality; Penetrometry.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100019

ARTIFICIAL NEURAL NETWORKS FOR PREDICTION OF PHYSIOLOGICAL AND PRODUCTIVE VARIABLES OF BROILERS
Provedor de dados: 70
Autores: Abreu,Lucas H. P.; Yanagi Junior,Tadayuki; Bahuti,Marcelo; Hernández-Julio,Yamid F.; Ferraz,Patrícia F. P.
ABSTRACT Due to a number of factors involving the thermal environment of a broiler cutting installation and its interaction with the physiological and productive responses of birds, artificial intelligence has been shown to be an interesting methodology to assist in the decision-making process. For this reason, the main aim of this work was to develop an artificial neural network (ANN) to predict feed conversion (FC), water consumption (Cwater), and cloacal temperature (tclo) of broilers submitted to different air dry-bulb temperatures (24, 27, 30, and 33°C) and durations (1, 2, 3, and 4 days) of thermal stress in the second week of the production cycle. Relative humidity and wind speed were fixed at 60% and 0.2 ms−1, respectively. The experimental data...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry; Thermal stress; Artificial intelligence.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100001

DRYING KINETICS OF NIGER SEEDS
Provedor de dados: 70
Autores: Silva,Fernanda P. Da; Siqueira,Valdiney C.; Quinzani,Guilherme A.; Martins,Elton A. S.; Goneli,André L. D.
ABSTRACT: The objectives of this study were to describe the process of drying niger seeds through the fitting of different mathematical models to the experimental drying data, to select the best model that represents the phenomenon, and to determine the diffusion coefficients and thermodynamic properties of the product. Seeds with an initial moisture content of 0.42 (d.b) were collected and dried at 40°, 50°, 60°, 70°, and 80°C in a fixed bed experimental dryer. After drying, different mathematical models were fitted to determine the diffusion coefficient by applying liquid diffusion theory, which allowed for calculation of the energy activation, enthalpy, entropy, and Gibbs free energy values. The Page model was selected to represent the drying process of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Activation energy; Effective diffusion coefficient; Guizotia abyssinica Cass; Mathematical models.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400727

Perfis temporais NDVI MODIS, na cana-soca, de maturação tardia
Provedor de dados: 70
Autores: Ramme,Fernando L. P.; Lamparelli,Rubens A. C.; Rocha,Jansle V.
Este artigo descreve o desenvolvimento de um banco de dados relacional e de uma ferramenta para a visualização de perfis temporais do NDVI MODIS, a partir dos dados do produto MOD09Q1, referente ao fator de refletância bidirecional de superfície relativa ao comprimento de onda do vermelho e do infravermelho-próximo, composição temporal em mosaicos de 8 dias, e a banda de controle de qualidade, dos talhões de cana-de-açúcar no Estado de São Paulo, para analisar a maturação da cana-soca Tardia. Das fazendas de cana-de-açúcar são obtidos os dados de históricos sobre produtividade, solo, variedade, localização de cada pixel para cada microrregião monitorada. Todos os dados são integrados em um banco de dados desenvolvido em PostgreSQL. O aplicativo foi...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: MODIS; Curvas espectrais; Índice de vegetação; Cana-de-açúcar.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300012

Cadastral maps of irrigated areas by center pivots in the State of Minas Gerais, using CBERS-2B/CCD satellite imaging
Provedor de dados: 70
Autores: Ferreira,Elizabeth; Toledo,Joice H. de; Dantas,Antonio A. A.; Pereira,Rafael M.
Medium-resolution satellite images have been widely used for the identification and quantification of irrigated areas by center pivot. These areas, which present predominantly circular forms, can be easily identified by visual analyses of these images. In addition to identifying and quantifying areas irrigated by center pivot, other information that is associated to these areas is fundamental for producing cadastral maps. The goal of this work was to generate cadastral mapping of areas irrigated by center pivots in the State of Minas Gerais, Brazil, with the purpose of supplying information on irrigated agriculture. Using the satellite CBERS2B/CCD, images were used to identify and quantify irrigated areas and then associate these areas with a database...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigated agriculture; Remote sensing; Geographic information system (GIS); Image visual interpretation.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400015

GRAIN STORAGE SYSTEM IN THE STATE OF PARANÁ, BRAZIL, FROM THE PERSPECTIVE OF MULTIVARIATE ANALYSIS
Provedor de dados: 70
Autores: Cima,Elizabeth G.; Uribe-Opazo,Miguel A.; Guedes,Luciana P. C.; Rocha Junior,Weimar F. da; Johann,Jerry A.
ABSTRACT This study aimed to identify whether there is an association between types of storage and categories of commercialization and use of grains, group the types of storage with the categories of commercialization, and group static and dynamic capacities of the units in the state of Paraná, Brazil. The data were obtained from the Brazilian Registry System of Storage Units for the 2014/2015 season. The association between variables under study was carried out with the chi-square test of independence and correspondence analysis. The cluster analysis consisted of the unweighted pair group method with arithmetic mean and considered a measure of mixed dissimilarity obtained for sets composed of qualitative and quantitative variables. A significant...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agribusiness; Association; Cophenetic correlation coefficient; Category of storage capacity; Clustering; Dissimilarity measures.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300280

Color change and quality response of ‘lane late’ orange submitted to degreening process
Provedor de dados: 70
Autores: MACHADO,FRANCISCA L. DE C.; CAJAZEIRA,JOÃO P.; COSTA,JOSÉ M. C. DA.
This study aimed at evaluating the effects of ethylene on peel color and compositional changes in ‘Lane late’ orange stored under refrigerated and ambient conditions. Physiologically mature, but green-peeled, oranges were exposed to ethylene gas under room temperature and high relative humidity for 24 hours. Storage chamber was ventilated with fresh air after 12 hours to mitigate consequences derived from fruit respiration. Both nondestructive analysis, such as peel color (hue angle, chromaticity, and brightness) and weight loss, and destructive ones (soluble solids, titratable acidity, pH, soluble solids to acidity ratio, and puncture force) were performed upon harvest, after degreening, and every three days during eighteen days in storage. Experiment was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrus sinensis (L.) Osbeck; Peel Color; Ethylene; Fruit Internal Quality.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100144

DAIRY CATTLE BIOGAS USAGE IN MICROTURBINES FOR ENERGY GENERATION AND THERMAL EXPLOITATION
Provedor de dados: 70
Autores: Hirano,Marcio Y.; Silva,Celso L. da.
ABSTRACT The increase in confined cattle breeding reflects the modernization and automation of farming, which has significantly intensified in recent years and caused an increase in the energy demand of rural properties. This study investigated the use of biogas generated from dairy cattle manure confined in gas microturbines on a farm to generate electricity and the energy use of exhaust gases. At the end of the study, 6,195 to 16,077 kWh month-1 of electricity was obtained, which corresponds to 43.3% of the property's self-sufficiency energy demand. By performing an exhaust gas energy exploitation, between 6.8 and 13.6 m3 day-1 of water heated to 368 K can be produced, or between 11,880 and 23,661 kWh month-1 of cooling capacity can be obtained using a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energy exploitation; Biogas; Dairy cattle; Microturbine.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400526

FUZZY SLIDING-MODE TEMPERATURE-CONTROL SYSTEM FOR SOAKING AND GERMINATION OF RICE SEEDS
Provedor de dados: 70
Autores: Zhou,Zheng; Liang,Chunying.
ABSTRACT The soaking and germination process of rice seeds is the starting point in rice cultivation in cold regions and has a significant effect on grain yield. Efficient techniques for controlling the water temperature in the seed tank are required to enhance germination quality. This paper introduces a fuzzy theory for designing a fuzzy logic-based sliding mode controller (SMC) system for a rice seed soaking and germination device. The proposed system was theoretically and experimentally investigated to determine the efficiency of the soaking temperature-control system. A modified fuzzy SMC based on exponent approaching law is also presented for optimizing the proposed controller. A proportional integral derivative (PID) controller was designed to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuzzy sliding-mode control; Temperature controller; Soaking; Germination.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200215

Water treatment by multistage filtration system with natural coagulant from Moringa oleifera seeds
Provedor de dados: 70
Autores: Franco,Monalisa; Silva,Gabriela K. e; Paterniani,José E. S.
This study presents an evaluation of a pilot multistage filtration system (MSF) with different dosages, 131 mg L-1 and 106 mg L-1, of the natural coagulant extracted from Moringa oleifera seeds in pre-filtration and slow filtration stages, respectively. The system was comprised by a dynamic pre-filter unit, two upflow filters in parallel and four slow filters in parallel, and in one of the four filters had the filter media altered. The performance of the system was evaluated by monitoring some water quality parameters such as: turbidity, apparent color and slow filter load loss. The stages that have received the coagulant solution had better treatment efficiency compared with the steps without it. However, the direct application of the coagulant solution...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Multistage filtration system; Slow filtration; Water coagulation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500018

Tratamento de águas residuárias de suinocultura em reatores anaeróbios horizontais seguidos de reator aeróbio em batelada sequencial
Provedor de dados: 70
Autores: Santos,Ariane C. dos; Oliveira,Roberto A. de.
Avaliou-se o desempenho de um sistema combinado anaeróbio-aeróbio para o tratamento de águas residuárias de suinocultura, com concentrações médias de sólidos suspensos totais (SST) de 18.624 e 11.395 mg L-1. Foram utilizados quatro reatores anaeróbios horizontais com volume total de 49,5 L cada, um com manta de lodo (RAHML) e três de leito fixo (RAHLF), instalados em série e seguidos de um reator aeróbio operado em batelada sequencial (RBS) com volume total de 339 L e com alimentação contínua. Nos RAHLF, foram utilizados como meios suporte de anéis de bambu, anéis plásticos de eletroduto corrugado e anéis de bucha (Luffa cillyndrica), respectivamente. Os tempos de detenção hidráulica (TDH) e as cargas orgânicas volumétricas (COV) aplicadas no RAHML foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tratamento anaeróbio-aeróbio-anóxico; Pós-tratamento; Remoção de nutrientes; Tratamento terciário; Nitrogênio.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400016

Sazonalidade de variáveis biofísicas em regiões semiáridas pelo emprego do sensoriamento remoto
Provedor de dados: 70
Autores: Rodrigues,Joseilson O.; Andrade,Eunice M. de; Teixeira,Adunias dos S.; Silva,Bernardo B. da.
Para investigar alterações no albedo, no Índice de Vegetação por Diferença Normalizada (NDVI), no saldo de radiação e no fluxo de calor no solo, em decorrência do regime pluviométrico no semiárido cearense, desenvolveu-se um estudo na bacia do Rio Trussu - Ceará, empregando-se sensoriamento remoto. Foram utilizadas duas imagens Landsat 7 ETM+, datadas de 25-10-2000 e 24-7-2001, sendo as variáveis estimadas pelo emprego do algoritmo SEBAL (Surface Energy Balance Algorithms for Land). Os resultados mostraram que as variáveis investigadas apresentaram alterações entre as duas estações, sendo os maiores valores de albedo registrados na estação seca. O NDVI apresentou maior sensibilidade ao regime hídrico, mostrando alto potencial de recuperação da vegetação ao...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Albedo; NDVI; Sensoriamento remoto; Saldo de radiação.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300012

Locais de implante de microchips de identificação eletrônica de leitões: seleção e validação por análise de imagem
Provedor de dados: 70
Autores: Pandorfi,Héliton; Silva,Iran J. O.; Sevegnani,Kelly B.; Caro,Ivan W.
Nas últimas décadas, a produção de suínos, pressionada por uma crescente demanda por alimentos, tem-se caracterizado pela maior concentração de animais em grandes unidades de produção, dificultando o registro dos dados individuais. Os sistemas automáticos de identificação eletrônica podem auxiliar a detecção de doenças, a avaliação de respostas fisiológicas, o controle de ingestão de alimentos, a atividade física e ainda o impacto ambiental causado pelo sistema de produção, promovendo melhor controle da propriedade. Transponders injetáveis, brincos eletrônicos e o monitoramento por meio da análise de imagem estão sendo utilizados no processo de identificação. O objetivo desta pesquisa foi avaliar os diferentes locais de implante subcutâneo de microchips em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Análise de imagem; Identificação eletrônica; Zootecnia de precisão.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100001

Higroscopicidade das sementes de sorgo-sacarino
Provedor de dados: 70
Autores: Ullmann,Renan; Resende,Osvaldo; Oliveira,Daniel E. C.; Costa,Lílian M.; Chaves,Tarcísio H.
RESUMO Objetivou-se, neste trabalho, determinar as isotermas de dessorção das sementes de sorgo-sacarino para diversas condições de temperatura e atividades de água e obter o calor isostérico de dessorção. As sementes foram submetidas à secagem em estufa com ventilação de ar forçada a 40 °C até atingir os teores de água de aproximadamente 24; 19; 15; 12 e 8 (% b.s.). As isotermas de dessorção das sementes de sorgo-sacarino foram obtidas pelo método estático indireto, sendo a atividade de água (aw) determinada por meio do equipamento Hygropalm Model Aw 1. Para o controle da temperatura, utilizou-se de B.O.D., regulada a 10; 20; 30 e 40 °C. Aos dados experimentais, foram ajustados modelos matemáticos frequentemente utilizados para a representação da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelagem; Calor isostérico; Isotermas.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300515

Balanço de massa de reatores anaeróbicos de fluxo ascendente com manta de lodo (UASB) tratando águas residuárias de suinocultura
Provedor de dados: 70
Autores: Oliveira,Roberto A. de; Foresti,Eugênio.
Foi obtido o balanço de massa, a partir dos valores médios das determinações de demanda química de oxigênio (DQO) e produção de metano (CH4), em dois reatores UASB de bancada com volume de 10,5 L tratando águas residuárias de suinocultura, submetidos a condições operacionais distintas no que diz respeito às concentrações de sólidos suspensos totais do afluente (SST de 500; 1.000; 1.500 e 2.000 mg L-1), tempo de detenção hidráulica (TDH de 30; 20; 12 e 8 h), taxas de carregamento orgânico volumétrico (TCOV de 0,8 a 8,0 kg DQO total (m³ d)-1) e temperatura (ambiente e controlada a 25º e 30ºC). Verificou-se que a DQO total removida convertida em CH4 variou de 28 a 51% e a relação DQO-CH4 por DQO dissolvida removida de 0,94 a 2,07; indicando alta participação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digestão anaeróbia; Tratamento anaeróbio; Resíduos de suinocultura.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300035

Estimativa de bem-estar de frango de corte em função da concentração de amônia e grau de luminosidade no galpão de produção
Provedor de dados: 70
Autores: Owada,Adriana N.; Nääs,Irenilza de A.; Moura,Daniella J. de; Baracho,Marta dos S.
O Brasil é um importante país exportador de carne de frango, e grande parte de seu destino são países com restrições específicas de alojamento, relacionadas ao bem-estar das aves. Um dos poluentes aéreos freqüentemente encontrados em altas concentrações nos aviários, principalmente em ambientes fechados, é a amônia. Existem evidências de que o bem-estar de frangos de corte pode ser comprometido pela exposição contínua a esse poluente dentro dos galpões de alojamento. Este trabalho visou a estimar o bem-estar para frangos de corte alojados, a partir de atributos específicos do ambiente térmico e da densidade de aves, em função da concentração de amônia e luminosidade no ambiente de alojamento, utilizando a Teoria dos Conjuntos Fuzzy. Os resultados mostraram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Qualidade de ar; Ambiente de alojamento; Lógica Fuzzy.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400003

Effect of different substrates in aquaponic lettuce production associated with intensive tilapia farming with water recirculation systems
Provedor de dados: 70
Autores: Geisenhoff,Luciano O.; Jordan,Rodrigo A.; Santos,Rodrigo C.; Oliveira,Fabricio C. de; Gomes,Eder P.
ABSTRACT The integration of fish farming in intensive system and plant production, called "aquaponics" is practiced successfully in countries like the USA, Australia and Europe. In Brazil, this integration has attracted the attention of researchers and producers. In this context, the aim of this study was to evaluate the effect of two substrates (crushed stone number 3, CS III and flexible polyurethane foam, FPF) on the production of aquaponic lettuce, moreover, to show that the residual water from intensive tilapia production provides sufficient qualitative characteristics for competitive production of lettuce without adding commercial fertilizers. The treatment in which FPF was used provided higher concentrations of macro and micronutrients in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soilless cultivation; Water recirculation and aquaponics system.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200291

Mechanical behavior of 'Niagara Rosada' grape berry detachment
Provedor de dados: 70
Autores: Gomes,Daniel; Ferraz,Antonio C. de O.
The 'Niagara Rosada' grape is the main Brazilian table grape belonging to the Labrusca family. It develops medium, cylindrical and compact bunches with berries presenting a pinkish skin and a foxy flavor that is valued in the Brazilian market. These berries are tender and have a pedicel-berry connection provided by the vascular bundles and surrounding skin. This cultivar is very susceptible to berry drop mainly caused by vibration and senescence. The objective of this study was to evaluate the temporal mechanical behavior of the pedicel-berry detachment, using resistance indexes extracted from traction force-deformation curves. Test results showed two different detachment types. In the first one, which exhibited higher average resistance, a considerable...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Postharvest; Viticulture; Mechanical properties; Senescence.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600009

Thermal comfort temperature update for broiler chickens up to 21 days of age
Provedor de dados: 70
Autores: Cassuce,Déborah C.; Tinôco,Ilda de F. F.; Baêta,Fernando C.; Zolnier,Sérgio; Cecon,Paulo R.; Vieira,Maria de F. A.
Due to changes in genetics and nutrition, as well as in acclimatization of broiler chickens to the Brazilian climate, temperature values currently accepted as optimal may be outdated. The objective of this research was to update the environment temperatures that characterize the thermal comfort for broilers chickens from one to 21 days of age, under Brazilian production conditions. This research was conducted with 600 COBB birds, which were distributed in five growth chambers maintained at different temperatures during the first three weeks of age. During the experimental period, temperature values were progressively reduced, consisting in five treatments: T2724/21, T30/27/24, T33/30/27, T36/33/30 and T39/36/33. It was observed that the birds maintained in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal stress; Aviculture; Performance.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100004

WATER HARDNESS AND pH IN THE EFFECTIVENESS OF GLYPHOSATE FORMULATIONS
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Palma,Roxanna P.; Oliveira,Arthur C. de; Marques,Matheus G.; Alvarenga,Cleyton B. de.
ABSTRACT The hardness and pH of the spray water can interfere with the weed control effectiveness with herbicides, but it is not clear the magnitude of this interference, mainly associating different levels of pH and hardness to different glyphosate formulations. This study aimed to evaluate the influence of hardness and pH, in association, of the water used in the application of two glyphosate formulations on the weed control effectiveness. The experiment was conducted in duplicate, in areas with a predominance of Digitaria horizontalis, under a randomized block design with a 4×4×2+1 factorial scheme, composed of four water hardness levels (70, 110, 230, and 430 ppm CaCO3), four pH levels (3.5, 4.5, 5.5, and 6.5), two glyphosate formulations (ammonium...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Herbicide; Water quality; Spraying; Application technology.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400555

Temperaturas superficiais de telhas e sua relação com o ambiente térmico
Provedor de dados: 70
Autores: Sampaio,Carlos A. de P.; Cardoso,Célio O.; Souza,Geovani P. de.
Este trabalho teve como objetivo a análise de temperaturas de telhas de barro, de fibrocimento com pintura branca na face superior e de aço zincado e sua relação com o ambiente térmico, quantificando também os Índices de Temperatura e Umidade (ITU), de Temperatura de Globo e Umidade (ITGU) e Carga Térmica de Radiação (CTR). As análises foram realizadas em modelos de edificações e na área não sombreada. Os resultados mostraram que as telhas cerâmicas e de fibrocimento apresentaram comportamentos térmicos semelhantes, sendo que a opção pela telha de fibrocimento de 5 mm, pintada de branca na sua face superior, é vantajosa economicamente. As telhas metálicas superaram os 53 °C na sua superfície e foram piores no conforto térmico comparado com as outras...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Telhas; Fatores ambientais; Conforto térmico; Índices.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200003

Equipamento microprocessado para geração de sinal de correção diferencial, em tempo real, para GPS
Provedor de dados: 70
Autores: Lima,Thales C. B.; Umezu,Claudio K.; Cappelli,Nelson L.; Nunes,Eduardo F.
Este trabalho apresenta o desenvolvimento de um equipamento microprocessado, de baixo custo, para geração de sinal de correção diferencial para GPS, em tempo real, e configuração e supervisão do receptor GPS base. O equipamento desenvolvido possui um microcontrolador dedicado, display alfanumérico, teclado multifunção para configuração e operação do sistema e interfaces de comunicação. O circuito eletrônico do equipamento tem a função de receber as informações do GPS base e interpretá-las, transformando-as numa sentença no protocolo RTCM SC-104. O software do microcontrolador é responsável pela conversão do sinal recebido pelo GPS base, do formato proprietário para o protocolo RTCM SC-104. A placa processadora principal possui duas interfaces seriais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: DGPS; RTCM SC-104; Microprocessador.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200023

Efeito de diferentes períodos de irrigação no desenvolvimento, produção e qualidade de sementes na cultura do milho (Zea mays L.)
Provedor de dados: 70
Autores: Galbiatti,João A.; Borges,Maurício J.; Bueno,Lara F.; Garcia,Anice; Vieira,Roberval D.
O presente trabalho foi realizado em área demonstrativa de irrigação do Departamento de Engenharia Rural da Faculdade de Ciências Agrárias e Veterinárias, da Universidade Estadual Paulista (FCAV/UNESP), Jaboticabal - SP, tendo como objetivo avaliar os efeitos da deficiência hídrica no desenvolvimento da planta, na produção e na qualidade fisiológica de sementes da cultura do milho (Zea mays L.). O delineamento experimental foi o inteiramente casualizado, com os tratamentos em esquema fatorial 2 x 3, com quatro repetições. Os tratamentos consistiram da utilização de sementes de milho híbrido BR201 e DINA-70, com três períodos de irrigação: 1) durante todo o ciclo; 2) após o período vegetativo (após a emissão da 12ª folha), e 3) até 20 dias após o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Estresse hídrico; Análise de crescimento; Manejo da água.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200008

Produtividade do milho relacionada com a resistência mecânica à penetração do solo sob preparo convencional
Provedor de dados: 70
Autores: Freddi,Onã S.; Carvalho,Morel P.; Veronesi Júnior,Valdenir; Carvalho,Guilherme J.
A resistência mecânica do solo à penetração exerce grande influência sobre o desenvolvimento vegetal, uma vez que o crescimento das raízes e a produtividade das culturas variam de forma inversamente proporcional ao seu valor. O objetivo do trabalho foi estudar a variabilidade espacial e a correlação entre a produtividade do milho (PG) e a resistência mecânica do solo à penetração (RP) de um Latossolo Vermelho sob preparo convencional, em área pertencente à Fazenda Experimental de Ensino e Pesquisa da Faculdade de Engenharia - FE/UNESP - Câmpus de Ilha Solteira. Foram definidos 133 pontos de amostragem no campo, segundo malha com espaçamento regular de 10,0 m, nos quais foram medidas a RP, a umidade gravimétrica (UG), nas camadas de 0-0,10; 0,10-0,20;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Krigagem; Zea mays.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100013

ERRATUM
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500684

DIFFERENT SOYBEAN PLANT POPULATIONS UNDER CENTRAL PIVOT IRRIGATION
Provedor de dados: 70
Autores: Gava,Ricardo; Anselmo,Jefferson L.; Neale,Christopher M. U.; Frizzone,José A.; Leal,Aguinaldo J. F.
ABSTRACT Planting density can influence the competitiveness among plants mainly by water, nutrients and solar radiation, directly affecting yield. The purpose of this study was to evaluate the productivity of different soybean cultivars at different planting populations under irrigated and rainfed conditions. The experiment was conducted during the 2014/15 growing season, under center pivot irrigation in Chapadão do Sul – MS, Brazil. The experimental design was randomized complete block design with split-plot, as follows: Irrigated and Rainfed (plots) x Six cultivars (subplots) x Three Plant Populations (sub-subplots) with 4 replications. The irrigation management was realized by Penman-Monteith-FAO method. The cultivars used were: NA 5909 RR, DM 5958...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plant density; Irrigated Soybean; Deficit irrigation; Soybean Yield.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300441

Análise de imagem aplicada ao estudo do comportamento de leitões em abrigo escamoteador
Provedor de dados: 70
Autores: Pandorfi,Héliton; Silva,Iran J. O.; Moura,Daniella J.; Sevegnani,Kelly B.
O objetivo geral desta pesquisa foi avaliar o comportamento de leitões em diferentes sistemas de aquecimento por meio da análise de imagem. A pesquisa foi desenvolvida na sala da maternidade, com 80 animais entre o nascimento e o desmame. Os tratamentos adotados para a avaliação da eficiência dos diferentes sistemas de aquecimento do abrigo escamoteador foram: piso térmico, lâmpada incandescente, resistência elétrica e lâmpada de infravermelho. Os dados ambientais foram registrados no ambiente externo, na sala da maternidade e no interior de cada abrigo escamoteador avaliado, ao longo de 19 dias. O delineamento experimental foi em blocos casualizados, com quatro tratamentos e 18 blocos, e as médias foram comparadas pelo teste de Tukey (P &lt; 0,01). Os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Comportamento animal; Conforto térmico; Suinocultura.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200005

Depósito e perdas de calda em sistema de pulverização com turboatomizador em videira
Provedor de dados: 70
Autores: Balan,Marcelo G.; Abi Saab,Otavio J. G.; Silva,Cristhiane G.
Grande parte dos viticultores da região Norte do Paraná pratica a condução da videira em caramanchão, com mais de 50 aplicações fitossanitárias em um único ciclo. O objetivo deste trabalho foi avaliar essas aplicações com turboatomizador assistido de ar no sistema de pulverização, por meio do depósito de calda nas folhas e perdas. O trabalho foi desenvolvido utilizando-se de cinco condições de aplicação, variando-se tamanho de gotas e volume de aplicação, com quatro repetições, em blocos casualizados. A avaliação do sistema foi feita com a aplicação de uma calda de cloreto de potássio (5%), sendo o depósito nas folhas medido pela condutividade elétrica, e as perdas, pela comparação entre volumes aplicado e recuperado nas folhas. Para todas as condições, as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Produtos fitossanitários; Deposição; Jato transportado.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200015

Broadcast distribution uniformity of fertilizer with centrifugal spreaders used in variable rate application
Provedor de dados: 70
Autores: CUNHA,JOÃO P. A. R.; SOARES FILHO,ROMEU.
ABSTRACT The quality of fertilizer distribution process is important to the success of agriculture. This research aimed to study the distribution uniformity of fertilizers with spreaders capable of performing variable rate. Evaluations were carried out in different farms, in the Southwest region of the State of Goiás, Brazil. 13 longitudinal and transversal distribution profiles with 11 centrifugal spreaders were evaluated: five with limestone, two with gypsum, two with magnesium oxide, one with monoammonium phosphate (MAP), one with super simple phosphate (SS), one with chloride potassium (KCl) and one with formulated fertilizer (02-20-20). The collectors and the form of distribution followed the ASABE S341.3 standard (2006). The broadcasted distribution...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertilizer distribution; Broadcast spreaders; Precision agriculture.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500928

Evaluation of an indicator for water yield in a watershed of Alto Rio Grande Region, State of Minas Gerais , Brazil
Provedor de dados: 70
Autores: Mattos,Roberto de; Silva,Antônio M. da; Coelho,Gilberto; Mello,Carlos R. de; Rezende,José L. P. de.
The Brazilian Law stipulates that water is a limited natural resource doted of economic value, thus it is necessary to develop mechanisms for its adequate management. Actions that encourage the farmers to apply soil conservation practices with the purpose of increase water yield from springs and to promote improvement of its quality, reducing production of sediment transportation, is being encouraged by governments, even with financial compensation for owners. From these assertions, this study aims to quantify the benefits of the conservation actions of the management units and to characterize a Water Yield Indicator (WYI) to support sustainable actions in the watershed of Alto Rio Grande region, in the state of Minas Gerais (MG). To assess the impact of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Land use and occupation; Water resources management; Water producer program.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000400009

IDENTIFICATION OF MAIZE LODGING: A CASE STUDY USING A REMOTELY PILOTED AIRCRAFT SYSTEM
Provedor de dados: 70
Autores: Acorsi,Matheus G.; Martello,Maurício; Angnes,Graciele.
ABSTRACT A common agricultural problem in many regions of Brazil is maize lodging, as a consequence of strong winds and rain which impacts on crop growth and yield. However, collecting data using ground-based, manual field measurement methods is inefficient. An emerging tool is the Remotely Piloted Aircraft System (RPAS), capable of delivering spatial data with high resolution and flexible periodicity. In this study, the potential to detect the maize lodging using crop surface models derived from RPAS was assessed. Our RPA-based approach uses a quantitative threshold to determine lodging percentage. The threshold values of plant height, used to detect the occurrence of lodging, were based on fixed and variable values. The validation of percentage lodging...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Crop surface model; Structure from motion; Canopy height; RGB.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800066

Modificação de uma barra de pulverização para a aplicação de fungicida em trigo visando ao controle de giberela
Provedor de dados: 70
Autores: Panisson,Edivan; Boller,Walter; Reis,Erlei M.; Hoffmann,Laércio L.
Devido ao aumento da intensidade e da freqüência de ocorrência da giberela, doença causada pelo fungo Gibberella zeae (anamorfo Fusarium graminearum), essa vem sendo apontada como uma das moléstias de maior importância na cultura do trigo no Sul do Brasil. A giberela é uma doença de infecção floral e mesmo os fungicidas sistêmicos recomendados apresentam apenas efeito protetor das anteras. Os objetivos do presente trabalho foram avaliar a eficiência de controle e os efeitos nos grãos colhidos, de diferentes pontas de pulverização (jato plano, jato plano duplo e jato cônico vazio), diferentes arranjos dos bicos na barra de aplicação e dois volumes de calda. Em dois experimentos realizados no ano de 1999, a aplicação dos tratamentos reduziu...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Barra de pulverização; Pontas de pulverização; Volume de calda.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100012

SEED METERING MECHANISMS AND TRACTOR-SEEDER FORWARD SPEED ON CORN AGRONOMIC COMPONENTS
Provedor de dados: 70
Autores: Cortez,Jorge W.; Anghinoni,Matheus; Arcoverde,Sálvio N. S.
ABSTRACT Seed metering system and tractor-seeder forward speed are factors that affect sowing. Therefore, this study aimed to evaluate sowing and agronomic components of corn as a function of seed metering mechanism and tractor-seeder forward speed, in addition to evaluating the yield data obtained from a harvester with a yield monitor. The soil of the area is classified as Distroferric Red Latosol. The experiment was set up in the second crop season of 2018 and treatments consisted of two seed metering mechanisms (M) (pneumatic and mechanical), and tractor-seeder forward speeds (S) (3, 5, 7, and 9 km h−1). The pneumatic system promoted the best longitudinal distribution, with values above 90%, and the increased sowing forward speed reduced normal spacings...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Grain yield; Pneumatic sowing; Sowing forward speed.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100061

Electrically driven fertilizer applicator controlled by fuzzy logic
Provedor de dados: 70
Autores: Garcia,Angel P.; Cappelli,Nelson L.; Umezu,Claudio K.
The present study shows the development, simulation and actual implementation of a closed-loop controller based on fuzzy logic that is able to regulate and standardize the mass flow of a helical fertilizer applicator. The control algorithm was developed using MATLAB's Fuzzy Logic Toolbox. Both open and closed-loop simulations of the controller were performed in MATLAB's Simulink environment. The instantaneous deviation of the mass flow from the set point (SP), its derivative, the equipment´s translation velocity and acceleration were all used as input signals for the controller, whereas the voltage of the applicator's DC electric motor (DCEM) was driven by the controller as output signal. Calibration and validation of the rules and membership functions of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertilizer applicator; Agricultural machinery; Closed-loop control.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300014

Changes in water availability in the soil due to tractor traffic
Provedor de dados: 70
Autores: Gómez-Rodríguez,Katherine; Camacho-Tamayo,Jesús H.; Vélez-Sánchez,Javier E.
Frequent traffic of tractors in agricultural soils, promotes soil compaction and affects the flow and water availability. The aim of this research was to study the effect of compaction induced by tractor traffic on water availability in the soil under different traffic intensities on the same path (0, 1, 3, 6 and 10 passages), to two tractors with 3.3 and 2.6 ton of weights, over three different surface conditions. The study was conducted in an Andisol, representative soil of the study area. It was determined the behavior of the water retention curve, obtaining the gravitational water, available water and hygroscopic water, to 10 and 30 cm of depth. The hygroscopic water is the most prevalent with values ​​of up to 80% of the total water present in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compaction; Soil management; Water retention curve; Andisol.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600008

DEVELOPMENT OF AN EQUIPMENT TO OBTAIN THE RELATION BETWEEN THE HORIZONTAL AND VERTICAL PRESSURE IN SILOS
Provedor de dados: 70
Autores: Ledo,Raul C.; Cheung,Andrés B.; Silva,Josivaldo G. da.
ABSTRACT Silos are essential for sectors such as agriculture, industry, and mining in Brazil, but they are structures with a high degree of complexity in relation to pressure determination. Therefore, new researches on the influence of the product stored in their structure are stimulated. For granular materials, the K coefficient is the factor obtained between the horizontal and the vertical pressure. This study aimed to develop a test device capable of calculating this coefficient based on the recommendations of EN 1991-4 (2006) (Eurocode 1: Actions on structures – Part 4: Silos and tanks). For that, two cylinders of different heights were elaborated to study the influence of the device height in obtaining K coefficient. The results were measured by...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: K coefficient; Granular materials; Silos.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400491

Determination of thermal comfort zone for early-stage broilers
Provedor de dados: 70
Autores: Cândido,Márcia G. L.; Tinôco,Ilda De F. F.; Pinto,Francisco de A. de C.; Santos,Nerilson T.; Roberti,Ricardo P.
ABSTRACT Environmental temperatures currently considered within comfort zone for broiler rearing may be misleading or even obsolete from actual values. Some factors such as animal genetics, nutrition and poultry management, mainly acclimatization to tropical and subtropical conditions, influence in determining the comfort zone for birds. This study aimed to evaluate the effects of five different thermal environments on animal welfare and rearing performance of broiler chickens, setting an ideal temperature range (comfort zone) for each of the first three weeks of poultry breeding. The chicks (375) were randomly placed into five climatic chambers set to distinct thermal conditions, being: one as recommended by the literature, another as stated by Cassuce...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry; Thermal comfort; Animal performance; Cold stress.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500760

Comparação de diferentes metodologias para estimativa de curvas intensidade-duração-freqüência para Pelotas - RS
Provedor de dados: 70
Autores: Damé,Rita de C. F.; Teixeira,Claudia F. A.; Terra,Viviane S. S.
Nos projetos agrícolas de obras hidráulicas, onde não se dispõe de dados observados de vazão, é necessário explorar ao máximo as informações relativas às curvas Intensidade-Duração-Freqüência (IDF). Diante disso, é preciso obter maneira de desenvolver metodologias de estimativas de curvas IDF, em locais que possuam pouco ou nenhum dado pluviográfico. O objetivo do trabalho foi comparar as metodologias de desagregação de precipitações diárias para verificar o ganho de informação em termos de curvas IDF, comparadas àquela obtida a partir de dados observados (histórica). Os métodos utilizados foram: (a) Método das Relações (CETESB, 1979); (b) BELTRAME et al. (1991); (c) ROBAINA &amp;amp; PEITER (1992); (d) Modelo Bartlett-Lewis do Pulso Retangular Modificado...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precipitação máxima; Método das relações; Desagregação de chuva diária.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200005

PERFORMANCE OF HELICAL METERING MECHANISMS IN THE APPLICATION OF MICROGRANULAR FERTILIZER
Provedor de dados: 70
Autores: Spagnolo,Roger T.; Rosa,David P. da; Pinho,Marivan da S.; Schiavon,Cheiner S.; Schmechel,Diego K.
ABSTRACT The use of microgranular fertilizers is currently increasing, with low application rates as an obstacle in the mechanization. This study aimed to verify the performance of helical metering mechanisms using microgranular fertilizer. Four different fertilizer-metering mechanisms were tested at two pre-established dose rates (35 and 50 kg ha−1) and seven longitudinal angles (−15°, −10°, −5°, 0°, +5°, +10°, and +15°). The experiment was carried out according to Brazilian standards. The results showed that the longitudinal inclination affects the actual fertilizer dose in all tested metering systems. Metering mechanisms with a helicoid with longitudinal and lateral overflow presented a similar dose, according to the variation of the longitudinal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural equipment; Longitudinal inclination; Precision agriculture.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400481

PHYSICAL, MECHANICAL AND THERMAL BEHAVIOR OF ADOBE STABILIZED WITH “SYNTHETIC TERMITE SALIVA”
Provedor de dados: 70
Autores: Gandia,Rômulo M.; Corrêa,Andrea A. R.; Gomes,Francisco C.; Marin,Diego B.; Santana,Lucas S.
ABSTRACT Adobe is an efficient construction material for several reasons, such as its thermal comfort, sustainability, and lower energy cost, as well as the simplicity of its production and execution. However, challenges such as water absorption, capillarity, and compressive strength should be investigated to improve its physical and mechanical properties. “Synthetic termite saliva” (STS) is an excellent stabilizer with high cohesive and hydrophobic power. Therefore, the objective of this work was to evaluate the effects of STS incorporation into adobe, analyzing its physical, mechanical and thermal properties. Five treatments were studied: 0 (control); 0.1; 0.2; 0.4 and 0.8% STS by mass. These adobe samples were evaluated according to bulk density, linear...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nonconventional materials; Stabilization; Sustainability; Earth construction; Hydrophobicity.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200139

METHODOLOGY FOR DIMENSIONING OF A CENTER PIVOT IRRIGATION SYSTEM OPERATING WITH DRIPPER TYPE EMITTER
Provedor de dados: 70
Autores: Almeida,Alex N. de; Coelho,Rubens D.; Costa,Jéfferson de O.; Farías,Asdrúbal J.
ABSTRACT: In Brazil, the conventional center pivot is widely used for irrigation of agricultural crops and its use has grown continuously. However, when improperly managed, it facilitates the development of diseases in all parts of the plant, with a direct effect on productivity, besides favoring losses of water by evaporation. The drip may be an alternative, since it minimizes the losses and does not wet the aerial parts of the plants, thereby reducing the incidence of diseases. A new system called localized mobile drip irrigation (IRGMO) is being developed in an attempt to combine the practicality and rusticity of the center pivot with the efficiency and water savings of the dripping irrigation systems. This fusion system is the central pivot with drip...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Design; Drip irrigation; Center pivot.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400828

SODIUM PHYTOREMEDIATION BY GREEN MANURE GROWING IN SOIL IRRIGATED WITH WASTEWATER OF DAIRY INDUSTRY
Provedor de dados: 70
Autores: Donatti,Ramon N.; Gomes,Tamara M.; Menegassi,Luana C.; Tommaso,Giovana; Rossi,Fabrício.
ABSTRACT: Phytoremediation is a technique that uses plants to decontaminate soils containing harmful organic and inorganic elements. The aim of this study was to evaluate the potential of three species of forage green manure in phytoremediation of saline soil irrigated with treated effluent from dairy processing plant. The design used was randomized blocks (3×3) with four replicates. The treatments were three different water sources (anaerobic treated effluent, aerobic treated effluent, and tap water) applied to growing table beets combined with the post-cultivation of three forage green manure: Calopogonium mucunoides Desv (Calopo), Cajanus cajan (L.) Millsp (Pigeon pea), and Pennisetum glaucum (L.) R. Brown (Millet). The treatment with Millet had higher...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reuse water; Phytoextraction; Salinization.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400665

Management zones in agriculture acording to the soil and landscape variables
Provedor de dados: 70
Autores: Delalibera,Hevandro C.; Weirich Neto,Pedro H.; Nagata,Noemi.
The study of spatial variability of soil and plants attributes, or precision agriculture, a technique that aims the rational use of natural resources, is expanding commercially in Brazil. Nevertheless, there is a lack of mathematical analysis that supports the correlation of these independent variables and their interactions with the productivity, identifying scientific standards technologically applicable. The aim of this study was to identify patterns of soil variability according to the eleven physical and seven chemical indicators in an agricultural area. It was used two multivariate techniques: the hierarchical cluster analysis (HCA) and the principal component analysis (PCA). According to the HCA, the area was divided into five management zones: zone...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Multivariate analysis; Precision agriculture; Spatial variability.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600021

GRADIENTE DE PRESSÃO ESTÁTICA DO AR FORÇADO EM CAMADAS DE RESÍDUOS ORGÂNICOS MISTURADOS COM DIFERENTES PROPORÇÕES DE CAMA DE FRANGO
Provedor de dados: 70
Autores: TEIXEIRA,DENIS L.; MATOS,ANTONIO T.; MELO,EVANDRO DE C.
RESUMO Neste trabalho, teve-se como objetivo o ajuste de equações que possibilitassem a estimativa do gradiente de pressão estática do ar, quando insuflado em camadas de resíduos orgânicos misturados com diferentes proporções de cama de frango. As medições do gradiente de pressão estática do ar foram realizadas em um protótipo, submetido a vazões específicas, que variaram de 0,02 a 0,13 m3 s-1 m-2, em camadas de bagaço de cana-de-açúcar, palha de café e serragem de madeira, misturadas com cama de frango, nas proporções de 0; 10; 20; 30 e 40% (base volumétrica). Os dados de gradiente de pressão estática do ar e vazão específica ajustaram-se bem aos modelos de Shedd, Hukill &amp; Ives e Hunter, podendo ser utilizados para predizer o gradiente de pressão...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compostagem; Leiras estáticas aeradas; Queda de pressão estática do ar.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200309

Mapeamento de semeaduras de soja (Glycine max (L.)Merr.) mediante dados MODIS/Terra E TM/Landsat 5: um comparativo
Provedor de dados: 70
Autores: Lamparelli,Rubens A. C.; Carvalho,Waste M. O. de; Mercante,Erivelto.
O objetivo deste trabalho foi comparar mapeamentos de semeadura da cultura da soja na região oeste do Paraná, realizados com imagens MODIS/Terra e TM/Landsat 5. Primeiramente, construiu-se máscara de referência, considerando seis imagens TM ao longo do ciclo da cultura, utilizando-se dos algoritmos Paralelepípedo e MaxVer com posterior análise visual. As imagens MODIS foram classificadas com o algorítimo Paralelepípedo, em quatro passagens referentes ao pico vegetativo. O desempenho das classificações foi avaliado por meio de Matrizes de Erros, calculadas pela análise de 100 pontos amostrais (soja ou não-soja), aleatoriamente distribuídos em cada um dos oito municípios da área de estudo. Os principais resultados mostraram que a Exatidão Global (EG) e o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Monitoramento; Matriz de erros; Previsão de safras; Imagens orbitais; Culturas agrícolas.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200014

INGESTIVE BEHAVIOR OF SANTA INÊS SHEEP UNDER THERMONEUTRALITY AND THERMAL STRESS UPON CONSUMPTION OF SALINE WATER
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Carvalho Júnior,Sebastião B. de; Souza,Bonifácio B. de; Dantas,Nayanne L. B.; Rodrigues,Ladyanne R.
ABSTRACT The consumption of saline water in semiarid regions is a recurrent situation that can affect the ingestive behavior of small ruminants. This study evaluated the ingestive behavior of Santa Inês sheep maintained in a climatic chamber under two air temperatures -25 °C within the thermal comfort zone (TCZ) and 32 °C above the TCZ - and consuming water with three levels of salinity - 2.0, 4.0, and 8.0 dS m-1. The experimental design was completely randomized in 2 × 3 factorial schemes, comprising two air temperatures and drinking water with three levels of salinity, in six replicates (animals). Regardless of air temperature, the consumption of saline water did not affect feed and water intake by the sheep; however, there was a decrease in feed intake...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Climatic chamber; Feed intake; Idleness; Ovis aries; Salinity; Water intake.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100019

Matéria seca e altura das plantas de soja e arroz em função do grau de compactação e do teor de água de dois latossolos
Provedor de dados: 70
Autores: Beutler,Amauri N.; Centurion,José F.
Este trabalho teve o objetivo de avaliar a altura de plantas e a produção de matéria seca da parte aérea e das raízes de soja e arroz em dois teores de água (água retida a 0,05 e a 0,01 MPa) e três de resistência do solo à penetração (entre 0,25 e 6,46 MPa), determinados com o penetrômetro de anel dinamométrico. Foram utilizadas amostras de Latossolo Vermelho, distrófico, textura média (LVd) e Latossolo Vermelho, eutroférrico, textura argilosa (LVef), coletadas na profundidade de 0,0-0,20 m e compactadas em camadas de 0,03 m, em vasos de 0,20 m de altura e 0,25 m de diâmetro. A altura das plantas foi reduzida para valores de resistência à penetração superiores a 3,0 MPa. A menor produção de matéria seca da parte aérea das plantas ocorreu na resistência à...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Matéria seca; Glycine max; Oryza sativa.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100016

Start-up of anaerobic reactors for slaughterhouse wastewater treatment
Provedor de dados: 70
Autores: FIA,RONALDO; PEREIRA,ERLON L.; FIA,FÁTIMA R. L.; EMBOABA,DÉBORA G.; GOMES,EMANUEL M.
This study aimed to evaluate the start-up of a horizontal anaerobic fixed bed reactor (HAFBR) followed by an upflow anaerobic sludge blanket (UASB) for the slaughterhouse wastewater treatment. HAFBR was filled with bamboo rings and had 1.2 m in length, 0.10 m in diameter and volume of 7.5 L. The UASB had the volume of 15 L. The HAFBR and UASB operated at organic loading rate and hydraulic retention time average of 8.46 and 3.77 kg m-3 d-1 of COD and 0.53 and 0.98 days, respectively. During 150 days of monitoring system it was found pH 6.8, relatively high values of bicarbonate alkalinity (&gt; 1000 mg L-1) and reduced values of volatile acids (70 to 150 mg L-1), which afforded average removal efficiencies of COD total and total suspended solids of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: UASB; Anaerobic filter; Slaughterhouse; Organic matter.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200331

Modelagem matemática e difusividade efetiva das sementes de pinhão-manso (Jatropha curcas L.) durante a secagem
Provedor de dados: 70
Autores: Resende,Osvaldo; Ullmann,Renan; Siqueira,Valdiney C; Chaves,Tarcísio H; Ferreira,Lênio U.
O presente trabalho teve o objetivo de ajustar diferentes modelos matemáticos aos dados experimentais da secagem de sementes de pinhão-manso (Jatropha curcas L.), bem como determinar o coeficiente de difusão efetivo e obter a energia de ativação para a faixa de temperatura utilizada. As sementes de pinhão-manso com teor de água de 0,67 (decimal b.s.) passaram por um período de pré-secagem em ambiente natural para reduzir e homogeneizar o teor de água para 0,30 (decimal b.s.). Em seguida, a secagem foi realizada em secador experimental mantendo-se as temperaturas controladas de 30; 40; 50; 60 e 70 ± 1 ºC e umidades relativas de 55,98; 41,44; 35,35; 26,21 e 13,37 ± 3%, respectivamente. Aos dados experimentais foram ajustados onze modelos matemáticos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Curvas de secagem; Modelos matemáticos; Energia de ativação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600010

Desempenho do método de dissipação térmica na medida do fluxo de seiva em seringueira
Provedor de dados: 70
Autores: Delgado-Rojas,Juan S.; Righi,Ciro A.; Karasawa,Shiguekazu; Angelocci,Luiz R.; Bernardes,Marcos S.; Folegatti,Marcos V.
A medida da transpiração de árvores no campo é de difícil consecução. Nas duas últimas décadas, tem-se dado ênfase à medida de fluxo de seiva no caule como indicador da transpiração, principalmente se a escala de tempo usada é igual ou menor que um dia. Para essas medidas, são usados métodos térmicos com fornecimento de calor ao caule. O método de dissipação térmica (MDT) é um deles e vem sendo bastante utilizado pelo seu princípio simples e pela boa sensibilidade às variações de fluxo de seiva. Entretanto, tem-se evidenciado a necessidade de cuidados no seu uso, sendo uma das causas de perda de precisão o efeito da carga radiante sobre a planta, geradora de gradiente térmico natural, que interfere nos resultados. Além disso, o desempenho do método em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hevea brasiliensis; Fluxo de seiva; Transpiração.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300008

CLASSIFICATION OF MACAW PALM FRUITS FROM COLORIMETRIC PROPERTIES FOR DETERMINING THE HARVEST MOMENT
Provedor de dados: 70
Autores: Costa,Anderson G.; Pinto,Francisco de A. de C.; Motoike,Sérgio Y.; Braga Júnior,Roberto A.; Gracia,Luis M. Navas.
ABSTRACT Macaw palm (Acrocomia aculeata) is a promising crop for biofuel production due to the high concentration of its fruit oil, but the harvest date is an issue to be better understood so it could be cultivated on an industrial scale. The aim of this study was to use the colorimetric properties of the macaw palm fruits to develop a neural network classifier to determine the ideal moment for harvesting, based on the oil content of the fruit mesocarp. During nine weeks of maturation were sampled 900 fruits of macaw palm fruits and the colorimetric properties of the RGB, HSI and CIELab color models were used to classify the fruits into immature and mature fruits. Kappa index and the overall accuracy values were used to access the classifier performance....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digital images; Maturation; Neural networks; Oil content.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400634

Remoção de matéria orgânica, de nutrientes e de coliformes no processo anaeróbio em dois estágios (reator compartimentado seguido de reator UASB) para o tratamento de águas residuárias de suinocultura
Provedor de dados: 70
Autores: Abreu Neto,Mário S. de; Oliveira,Roberto A. de.
Neste trabalho, avaliou-se o efeito das águas residuárias de suinocultura, com concentrações médias de sólidos suspensos totais variando de 4.591 a 13.001 mg L-1, no desempenho de processo anaeróbio, em dois estágios, compostos por reator compartimentado (ABR) e reator de fluxo ascendente com manta de lodo (UASB), instalados em série, em escala- -piloto (volumes de 530 e 120 L, respectivamente), submetidos a tempos de detenção hidráulica (TDH) de 60; 36 e 24 h no primeiro reator, e de 13,6; 8,2 e 5,4 h no segundo reator. As eficiências médias de remoção de DQOtotal variaram de 69 a 84% no reator ABR e de 39 a 58% no reator UASB, resultando em valores médios de 87 a 94% para o sistema de tratamento anaeróbio em dois estágios, com carga orgânica volumétrica...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carga orgânica volumétrica; Digestão anaeróbia; Reator anaeróbio de chicanas; Resíduos de suínos; Remoção de metais.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100015

Modelagem de um condicionador de ar de alta precisão para uso em processamento agrícola
Provedor de dados: 70
Autores: Fortes,Mauri; Ferreira,Délcio A.; Ferreira,Wanyr R.; Souza,Antônio C. de.
Apresenta-se neste trabalho, estudo detalhado sobre a modelagem de um condicionador de ar com controle acurado de temperatura e umidade relativa. Desenvolveu-se um programa de computador que permite predizer o comportamento do sistema sob diferentes condições psicrométricas e de vazão do ar de entrada. O modelo global físico-matemático inclui equações de balanço de massa e de energia para três diferentes volumes de controle que compõem o condicionador. Modelaram-se os processos de mistura, evaporação (ou condensação) simultânea de uma superfície d'água e de uma gota e o aquecimento de corrente de ar, separadamente. Propõem-se expressões semi-empíricas simples para os coeficientes de transferência de calor e massa inerentes ao processo de evaporação sobre...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiente controlado; Condicionamento de ar; Câmara climática.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200028

AERIAL AND GROUND APPLICATION OF FUNGICIDE IN CORN SECOND CROP ON DISEASES CONTROL
Provedor de dados: 70
Autores: Menechini,Wagner; Maggi,Marcio F.; Jadoski,Sidnei O.; Leite,Carla D.; Camicia,Ricardo da M.
ABSTRACT The aim was to evaluate the diseases severity on corn second crop. The research was conducted on the agricultural year of 2013 and 2014, evaluating the application quality over the fungicide spraying. The hybrid used was PIONEER 30k75 BT HERCULEX, evaluating the diseases severity previously and after the fungicide spraying, spray deposition on the culture and productivity. The aerial application was carried out with solution volume of 7.5, 13.5, 20 and 30.3 L ha-1, using automatic rotating nozzles, and the ground application with 90, 110, 130 and 150 L ha-1, uniform flat spray tips. As control a non-fungicide treatment was used. The aerial and soil treatment showed diseases control from the corn crop, being the biggest cover of drops acquired at...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Farming plane; Corn productivity; Spraying.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100116

Analyzing the efforts in furrow openers used in low power planters
Provedor de dados: 70
Autores: Troger,Henrique C. H.; Reis,Ângelo V. dos; Machado,Antônio L. T.; Machado,Roberto L. T.
The furrow openers for no-till system should be easy to penetrate the soil, generate low levels of soil mobilization and require a little traction force. Thus, the aim of this research was to compare six hoe-type furrow openers, four of industrial manufacturing and two handcrafted models, which were used in planters in the region of Pelotas, Brazil. The parameters for comparison among these furrow openers were the horizontal (Fh) and vertical (Fv) forces acting on the tip of the hoe and the cross-sectional area mobilized in the furrow. The experimental design was randomized, with six treatments (furrow openers) from T1 to T6, with four repetitions, constituted by their passage through plots of 20 x 3 m. The force data were collected by load cells and a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hoe opener; Traction demand; No-tillage.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600015

Evaluation of protein extraction methods to obtain protein concentrate from cassava leaf
Provedor de dados: 70
Autores: Coldebella,Priscila F.; Gomes,Simone D.; Evarini,Janete A.; Cereda,Marney P.; Coelho,Sílvia R. M.; Coldebella,Anderson.
The cassava leaf, waste generated in the harvest of the roots, is characterized by high content of protein, vitamins and minerals; however, its use is limited due to the high fiber content and antinutritional substances, which can be removed by obtaining protein concentrates. In this context, the objective of this study was to evaluate protein extraction processes, aiming the use of cassava leaves (Manihot esculenta Crantz) as an alternative protein. Four methods were tested: 1) Coagulation of Proteins by Lowering the Temperature, 2) Extraction by Isoelectric Precipitation, 3) Solubilization of Proteins and 4) Fermentation of Filter Leaf Juice. To obtain the concentrates, the use of fresh or dried leaves and extraction in one or two steps were also...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Exploitation; Agricultural waste; Protein extraction.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600015

Impacts of the application of swine wastewater in percolate and in soil cultivated with soybean
Provedor de dados: 70
Autores: Maggi,Cacea F.; Freitas,Paulo S. L. de; Sampaio,Silvio C.; Dieter,Jonathan.
The aim of this study was to evaluate the possible impacts caused in the soil and in the percolate in lysimeters of drainage with application of different rates of swine wastewater (SW) during the cycle of soybean culture and to assess the productivity of it. The experiment was conducted at the Agricultural Engineering Experimental Center of UNIOESTE. The soil was classified as typical Distroferric Red Latosol. There were twenty-four drainage lysimeters in the area in which the soybean was cultivated, cultivar CD 214. Four SW depths (0; 100; 200 and 300 m³ ha-1) were applied to the soil seven days before the sowing in a single application combined with two mineral fertilizations in the sowing (with and without recommended fertilization during sowing), and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lysimeters; Effluent soil pollution.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200007

Desenvolvimento do coeficiente parcial de ergonomia e segurança em tratores agrícolas
Provedor de dados: 70
Autores: Debiasi,Henrique; Schlosser,José F.; Pinheiro,Eder D.
O presente trabalho teve como objetivo criar e aplicar o coeficiente parcial de ergonomia e segurança em tratores agrícolas (COPES). O COPES corresponde a um valor numérico variável de 0 a 100, que expressa a qualidade em termos de ergonomia e segurança dos tratores agrícolas. O referido coeficiente foi desenvolvido e avaliado por meio da verificação da presença e estado de conservação de itens relacionados à ergonomia e segurança, em 175 tratores agrícolas usados, presentes em 114 propriedades amostradas junto às microrregiões gaúchas de Santa Maria, Restinga Seca e Cachoeira do Sul. Os resultados mostraram que o COPES apresentou grande variação entre os tratores amostrados (7,64 a 84,80), sendo a média geral inferior a 35. Isso demonstra que os tratores...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanização agrícola; Ergonomia; Segurança.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300025

IMPORTANCE OF CROP PRODUCTIVITY AND EQUIPMENT LIFETIME IN THE STRATEGIC AND TACTICAL MANAGEMENT OF SUGARCANE HARVESTERS
Provedor de dados: 70
Autores: Banchi,Ângelo D.; Garcia,Angel P.; Albiero,Daniel; Galvão,Cezário B.; Favarin,Luis G. A.
ABSTRACT Recently, Brazilian agriculture and the mechanization process have been improved and developed, particularly in sugarcane cultivation. The developed processes should adopt suitable management practices in terms of the technical, economic, and operational logistical aspects. As a management tool, the present study aimed to measure the impact of the accumulated use of harvesters (life in h) and agricultural productivity (Mg · ha−1) on the harvesting operational capacity (HOC). Mathematical modeling was performed on data obtained from eight sugarcane production units, and equations corresponding to the HOC as a function of the harvester's life and the crop agricultural productivity were developed. The equation that best represented the phenomenon was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Performance indicators; Maintenance management; Harvesting operational capacity; Agricultural mechanization.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500601

Perdas de solo e de água em sistemas de captação in situ no Semi-Árido brasileiro
Provedor de dados: 70
Autores: Brito,Luiza T. L.; Cavalcanti,Nilton B.; Anjos,José B. dos; Silva,Aderaldo S.; Pereira,Lúcio A.
Os sistemas de cultivo utilizados no semi-árido brasileiro apresentam riscos de perda devido à irregularidade das chuvas, devendo-se associá-los a práticas que propiciem maior infiltração e, conseqüentemente, menor erosão, o que pode ser obtido por meio de técnicas de captação de água de chuva in situ. Neste trabalho, teve-se o objetivo de avaliar as perdas de água e de solo em área cultivada com milho (Zea mays L.), submetida a diferentes sistemas de preparo do solo, correspondendo aos tratamentos Guimarães Duque (T1); aração profunda (T2); aração parcial (T3) e sulcos barrados (T4), comparados com o sistema tradicional (T5), que corresponde ao plantio sem preparo do solo. Após cada evento de chuva, a água e o solo escoados foram coletados e medidos. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão; Escoamento; Chuva; Zea mays L.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300011

Modalities for soil preparation and gypsum application in ultisol: stem productivity of sugarcane
Provedor de dados: 70
Autores: Lima,Ronaldo C.; Mello,Luiz M. M. de; Yano,Élcio H.; Silva,José O. R. da; Cesarin,André L.
The study was conducted in an area of expansion of sugarcane at Vale do Paraná factory in Suzanápolis city - São Paulo (SP), in Brazil, in the northwestern region of the State of São Paulo. It was used the sugarcane variety RB92-5345, 1.5m of spacing between rows, in an Ultisol. The study aimed to evaluate the productivity of sugarcane and first ratoon and some soil chemical attributes in function of soil tillage and application or not of gypsum. The experimental design was randomized blocks with six treatments, in a factorial 3x2 and six replicates, the main treatments were soil tillage with three equipments, moldboard plow, chisel plow, and heavy harrow, and two secondary treatments with application of 1 t ha-1of gypsum and no gypsum. After each harvest...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chemical attributes; Mechanization; Gypsum application; Saccharum spp.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600011

Tratamento anaeróbio de águas residuárias do beneficiamento de café por via úmida em reatores UASB em dois estágios
Provedor de dados: 70
Autores: Bruno,Marcelo; Oliveira,Roberto A. de.
Neste trabalho, avaliou-se a eficiência do tratamento de águas residuárias do beneficiamento de café por via úmida em reatores anaeróbios de fluxo ascendente com manta de lodo (UASB), em dois estágios, em escala de bancada, submetidos a tempos de detenção hidráulica (TDH) de 4,0; 5,2 e 6,2 dias e cargas orgânicas volumétricas (COV) de 5,8; 3,0 e 3,6 g DQO total (L d)-1, no primeiro reator (R1), e TDH de 2,0; 2,6 e 3,1 dias e COV de 5,8; 0,5 e 0,4 g DQO total (L d)-1, no segundo reator (R2). Os valores médios de DQO do afluente variaram de 15.440 a 23.040 mg O2 L-1. As eficiências médias de remoção de DQO total e SST foram de 66 a 98% e de 93 a 97%, respectivamente, nos reatores UASB, em dois estágios. O teor médio de metano no biogás variou de 69 a 89%, no...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Digestão anaeróbia; Fenóis; Águas residuárias de café despolpado; Carga orgânica volumétrica.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200017

Start-up of horizontal anaerobic reactors with sludge blanket and fixed bed for wastewater treatment from coffee processing by wet method
Provedor de dados: 70
Autores: Oliveira,Roberto A. de; Bruno,Natani M. N.
In this study it was evaluated the start-up procedures of anaerobic treatment system with three horizontal anaerobic reactors (R1, R2 and R3), installed in series, with volume of 1.2 L each. R1 had sludge blanket, and R2 and R3 had half supporter of bamboo and coconut fiber, respectively. As an affluent, it was synthesized wastewater from mechanical pulping of the coffee fruit by wet method, with a mean value of total chemical oxygen demand (CODtotal) of 16,003 mg L-1. The hydraulic retention time (HRT) in each reactor was 30 h. The volumetric organic loading (VOL) applied in R1 varied from 8.9 to 25.0 g of CODtotal (L d)-1. The mean removal efficiencies of CODtotal varied from 43 to 97% in the treatment system (R1+R2+R3), stabilizing above 80% after 30...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Volumetric organic loading; Bamboo; Methane; Phenols; Reactors in series.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200014

INFLUENCE OF LAND USE CHANGE ON SEDIMENT YIELD: A CASE STUDY OF THE SUB-MIDDLE OF THE SÃO Francisco River Basin
Provedor de dados: 70
Autores: Silva,Vicente De P. R. Da; Silva,Madson T.; Souza,Enio P. De.
ABTSRACT Erosion risk mapping and assessment are important for planning of natural resource management tool. The objective of this study was to simulate different scenarios of land use in the Sub-Middle of the São Francisco River Basin using the Soil and Water Assessment (SWAT) model to analyze the effects of changes in sediment yield, making comparisons with the present land use classification. The scenario analysis was (i) vegetation type characteristic of the semiarid region, (ii) growing corn and (iii) bare soil. For calibration procedure, the first three years of time series from 1993 to 1994 were validated using data from 1995 to 2004. The SWAT model employs the Modified Universal Soil Loss Equation (MUSLE) to compute soil erosion data. The results...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydrologic modeling; Evapotranspiration; Runoff; SWAT model.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601005

CLOACAL AND SURFACE TEMPERATURES OF BROILERS SUBJECT TO THERMAL STRESS
Provedor de dados: 70
Autores: Abreu,Lucas H. P.; Yanagi Junior,Tadayuki; Campos,Alessandro T.; Bahuti,Marcelo; Fassani,Édison J.
ABSTRACT: The cloacal and surface temperatures are important physiological parameters to quantify the thermal comfort of animals, its variations may occur as a function of thermal variables. In this context, the goal of the present study was to evaluate the cloacal (tclo) and surface (tsur) temperatures of Cobb 500® broilers, in the second week of life, subjected to different air dry-bulb temperature (24, 27, 30 and 33 °C) and stress durations (1, 2, 3 and 4 days). The experiment was carried out in four climate-controlled wind tunnels. Air relative humidity and air velocity were set at 60% and 0.2 m s-1, respectively. The tclo and tsur were measured daily through digital thermometer and thermographic camera, respectively. Analysis of variance and Scott...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal environment; Aviculture; Thermal comfort; Thermographic image; Physiologic parameters.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500877

Variação espaço-temporal dos parâmetros para a modelagem estocástica da precipitação pluvial diária no Rio Grande do Sul
Provedor de dados: 70
Autores: Calgaro,Marcelo; Robaina,Adroaldo D.; Peiter,Marcia X.; Bernardon,Tatiane.
O Rio Grande do Sul é um dos maiores produtores de grãos do Brasil, sendo a maioria das culturas conduzida em sistemas não irrigados, tornando-lhes extremamente dependentes das condições climáticas e do regime pluviométrico. Tal fato inspira diversas pesquisas na tentativa de caracterizar o comportamento espacial e temporal das precipitações. Dessa forma, o objetivo do presente trabalho foi estudar a variação espacial e temporal dos parâmetros alfa e beta da função gama para a geração de dados de precipitação pluvial diária no Estado. Os dados de precipitação pluviométrica foram obtidos junto à ANA - Agência Nacional de Águas. A modelagem da precipitação diária foi dividida em ocorrência e quantidade. Realizou-se a estimativa dos parâmetros alfa e beta da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulação; Chuva; Séries históricas.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200003

Climate variations in greenhouse cultivated with gerbera and relationship with external conditions
Provedor de dados: 70
Autores: Andrade Júnior,Aderson S. de; Damasceno,Lisânea M. O.; Dias,Nildo da S.; Gheyi,Hans R.; Guiselini,Cristiane.
Black meshes used in greenhouses provide shade to plants, affecting photosynthesis and presenting certain properties that change the microclimatic conditions in these environments. The objective of this study was to evaluate the variation in climate elements in greenhouse cultivated with gerbera (Gerbera jamesonii, Vr. Rambo) in relation to external conditions and the reference evapotranspiration (ETo) at Teresina, State of Piauí, Brazil. The measurements were obtained from July to October 2007 by an automatic data acquisition system installed inside and outside the greenhouse. The global solar radiation, evapotranspiration, precipitation, temperature, relative humidity, and wind speed were estimated. The results showed that major effect of the shading...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Meteorology; Meteorological elements; Floriculture; Gerbera jamesonii.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500003

Production of a product similar to gelatin from chicken feet collagen
Provedor de dados: 70
Autores: Almeida,Poliana F. de; Calarge,Felipe A.; Santana,José Carlos C.
Chicken feet can be used as an alternative source of collagen for the development of new products. In this sense, the aim of this study was the production of a product similar to gelatin from collagen extracted from chicken feet and the evaluation of sensory quality. The products were produced in two distinct flavors, with grape flavor called GU and pineapple flavor called GA. Subsequently, we compared these formulations with gelatin of a trademark established in the market. We used in the verification of sensory acceptability of products a hedonic scale of 9 points and the availability of consuming the product by 30 untrained tasters. According to the results, all formulations showed good levels of acceptability, indicating the collagen from chicken feet...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chicken feet quality sensory analysis; Utilization of byproduct new product development.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600021

Viabilidade econômica de produção de lenha de eucalipto para secagem de produtos agrícolas
Provedor de dados: 70
Autores: Afonso Júnior,Paulo C.; Oliveira Filho,Delly; Costa,Douglas R.
Este trabalho teve como principal objetivo determinar o custo e a viabilidade de produção de lenha de eucalipto necessária para secagem de produtos agrícolas. As principais considerações técnicas e econômicas foram: a) uso de lenha de eucalipto seca em fornalha de fogo indireto; b) custos referentes à mão-de-obra, materiais, insumos e equipamentos; c) custo de oportunidade e/ou taxa de juros de 10% ao ano; d) preço médio da terra variando de 500,00 a 2.000,00 US$ por ha; e) custo administrativo do reflorestamento de 10% sobre o custo do investimento, e f) período de investimento igual ao ciclo da produção de eucalipto, isto é, 21 anos. Concluiu-se que o investimento no reflorestamento com eucalipto é viável economicamente em terras próprias para lavoura,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energia; Reflorestamento; Secagem.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100004

FUZZY MODELING ON WHEAT PRODUCTIVITY UNDER DIFFERENT DOSES OF SLUDGE AND SEWAGE EFFLUENT
Provedor de dados: 70
Autores: Putti,Fernando F.; Kummer,Ana C. B.; Grassi Filho,Helio; Gabriel Filho,Luís R. A.; Cremasco,Camila P.
ABSTRACT: This study aimed to evaluate the effects of fertilization with composted sewage sludge and irrigation with drinking water (DW) and fertigation with wastewater (WW) in wheat crop using fuzzy rule-based system. The experiment was conducted in the Department of Soil and Environmental Resources, of FCA, UNESP - Botucatu, with factorial 6 × 2, which were applied 6 doses of sewage sludge (0, 50, 100, 150, 200 and 250% of nitrogen recommendation) and two types of effluents (treated water and sewage). In the developing of the system based in fuzzy rules, it was used the Mamdani inference method, where the input variables were sewage sludge doses and water types and the output variables used were the number of tillers, length and number spike per plant;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sustainability; Nitrogen; Mamdani; Fuzzy system.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601103

CHEMICAL CONTROL OF ASIAN SOYBEAN RUST AS A FUNCTION OF CULTIVAR, ROW SPACING AND SPRAY BAR SUPPORT SYSTEMS
Provedor de dados: 70
Autores: Hoffmann,Laercio L.; Roehrig,Rafael; Boller,Walter; Forcelini,Carlos A.
ABSTRACT Product deposition and foliar surface cover are highly impacting factors on the efficiency of foliar fungicides applied to soybean cultivars, due to their low mobility, with side effects on Asian soybean rust (ASR) control. Spray bar support systems, such as the air curtain (Vortex®) and the use of nozzles along the bar (Dropleg®), stand out as an alternative to obtain a better distribution of fungicide throughout the plant. In this study, two spray bar support systems (Vortex® and Dropleg®) were, therefore, evaluated and compared with the conventional spraying method based on the biological efficacy in ASR control. In order to do this, two harvests, with three spacing between rows and two cultivars were employed. Vortex® and Dropleg® spray bar...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plant arrangement; Genetic resistance; Phakopsora pachyrhizi.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400504

ASSEMBLY OF A REMOTELY PILOTED AIRCRAFT OF LOW COST APPLIED TO AGRICULTURE
Provedor de dados: 70
Autores: Cunha,João P. A. R. Da; Sirqueira Neto,Matheus A.
ABSTRACT: The remotely piloted aircraft (RPA) have great applicability in agriculture. Although it is a technology that has been developed for many years, in the field of agriculture it passed unnoticed for a long time. The high cost of acquisition is still a limiting factor for small and medium-sized farmers. In this way, this study had as objective to develop a low cost RPA for agriculture application. In the present study, the development and the assembly of an RPA prototype of a quadcopter type is presented, consisting of four engines and of vertical propulsion, capable of moving without human intervention, that is, autonomous flight, applied to agriculture and low cost investment. In it was boarded a data control and processing system collected from...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Quadcopters; RPA.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601268

ESTIMATION OF RESPIRATORY FREQUENCY AND RECTAL TEMPERATURE ON PIGS IN HEAT STRESS BY FUZZY LOGIC
Provedor de dados: 70
Autores: Oliveira,Rodrigo F. de; Ferreira,Rony A.; Abreu,Lucas H. P.; Yanagi Júnior,Tadayuki; Lourençoni,Dian.
ABSTRACT Physiological parameters such as respiratory frequency and rectal temperature stand out as indicators for heat stress in pigs, however, requiring time and labor for measurements. The possibility of using infrared thermography associated with prediction systems of these physiological variables can help in decision making, allowing greater welfare and productivity of the animals. With this objective, an experiment was carried out with growing pigs submitted to acute and chronic heat stress, working with a thermoneutrality temperature (22° C) and heat stress (34° C). The results were used for the development of a fuzzy model using as input variables: air dry bulb temperature (°C), average surface temperature (°C) and, as output variables: respiratory...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal environment; Fuzzy set theory; Pig breeding farm; Infrared thermography.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400457

Variabilidade espacial e temporal do fósforo, potássio e da produtividade de uma lavoura cafeeira
Provedor de dados: 70
Autores: Ferraz,Gabriel A. E S.; Silva,Fábio M. da; Carvalho,Luis C. C.; Alves,Marcelo de C.; Franco,Bruno C.
A agricultura de precisão surge como uma importante ferramenta para melhorar o gerenciamento da produção cafeeira, mostrando que o conhecimento de determinadas características do solo, associado à resposta de produtividade do cafeeiro, pode facilitar a aplicação localizada e racional dos insumos, com resultados ambientais e econômicos positivos. Desta forma, o presente trabalho objetivou utilizar ferramentas de agricultura de precisão aliadas a ferramentas da geoestatística para avaliar as variáveis fósforo, potássio e produtividade do cafeeiro, em três safras agrícolas, por meio de análises dos semivariogramas e de mapas de isolinhas interpolados por krigagem, e demonstrar que estas ferramentas são de grande valia para o manejo da cultura do café. Este...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Agricultura de precisão; Krigagem; Semivariograma; Café.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100015

Several regulations in gravity table in quality of tobacco seeds
Provedor de dados: 70
Autores: Gadotti,Gizele I.; Baudet,Leopoldo; Villela,Francisco A.
The use of gravity table can result in improved quality of seeds of several species, demonstrating the superiority of the quality attributes of seeds collected in the top positions in relation to the lower positions of the discharge zone of the gravity table. The availability of information on tobacco seeds, particularly on the action of gravity table, has not been addressed in the literature. The present study was to evaluate the influence of different regulations in the gravity table on the quality of tobacco seeds. The terminal edge of the machine of 50 cm width was divided into four parts plus the outlet for stones. The treatments were in the following fractions: original seed (obtained in the feed hopper), heavy seed (at the top), middle high,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nicotiana tabacum; Processing; Vigor; Sanity.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200016

Effect of working pressure at different spray nozzles on drift quantification in wind tunnel
Provedor de dados: 70
Autores: Gandolfo,Marco A.; Carvalho,Fernando K.; Chechetto,Rodolfo G.; Gandolfo,Ulisses D.; Moraes,Eder D. de.
Each year, there is an increase in pesticide consumption and in its importance of use in the large-scale agricultural production, being fundamental the knowledge of application technology to the activity success. The objective of the present study was to evaluate the influence of working pressure on the drift generated by different spray nozzles, assessed in wind tunnel. The treatments were composed of two spray nozzles AXI 110015 and AXI 11002 with pressure levels of 276 and 414 kPa. The spray solution was composed by water and NaCl at 10%. The applications were conducted at wind speed of 2.0 m s-1, being the drift collected at 5.0; 10.0 and 15.0 m away from the spray boom and at heights of 0.2; 0.4; 0.6; 0.8 e 1.0 m from the tunnel floor. To both spray...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Pesticides; Environmental contamination.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100008

Infiltração de água no solo em áreas cultivadas com cana-de-açúcar sob diferentes sistemas de colheita e modelos de ajustes de equações de infiltração
Provedor de dados: 70
Autores: Tomasini,Bruno A.; Vitorino,Antonio C. T.; Garbiate,Marcos V.; Souza,Cristiano M. A. de; A. Sobrinho,Teodorico.
As técnicas de colheita da cultura de cana nem sempre seguem preceitos conservacionistas, fato que pode influenciar atributos físicos do solo com consequente alteração da velocidade de infiltração de água no solo. O trabalho realizado teve como objetivo avaliar o efeito de diferentes sistemas de colheita (manual e mecanizada) da cana-de-açúcar (crua e queimada), sobre as características de infiltração e verificar a adequação de modelos matemáticos para a estimativa da taxa de infiltração de água no solo. Foi utilizado um simulador de chuva portátil calibrado para aplicar uma precipitação de 60 mm h-1. Os testes de infiltração de água no solo foram realizados em três sistemas de colheita: colheita manual de cana queimada, colheita mecanizada de cana crua e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Equação de horton; Sistemas de colheita; Infiltrômetro de aspersão.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600007

Elasticity moduli in round wooden beams of Pinus caribaea
Provedor de dados: 70
Autores: Zangiácomo,André L.; Christoforo,André L.; Lahr,Francisco A. R.
ABSTRACT This research aimed at estimating both longitudinal (E) and shear (G) elasticity moduli of round structural-sized beams made of Pinus caribaea timber, verifying thus the validity of the G = E/ 20 relationship established by the Brazilian standard ABNT NBR 7190: 1997 (Designing of Wooden Structures). We tested twenty pieces of green wood with average length, diameter and conicity of 750 cm, 30 cm and 4%, respectively. Two static bending tests were applied at three points of each piece, being nondestructive and using different distances between supports. In the first trial, the length and diameter relationship (L/ d) was set as being equal to 24; yet in the second test, it was set at 12. The elasticity moduli were estimated by a successive use of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Stiffness; Bending; Beam theory; Least square.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300566

Uniformidade de distribuição do potássio e do nitrogênio em sistema de irrigação por gotejamento
Provedor de dados: 70
Autores: Oliveira,Marcus V. A. M. de; Villas Bôas,Roberto L.
O uso da fertirrigação possibilita a obtenção de bons resultados, todavia é notada a necessidade de trabalhos que venham possibilitar a adoção correta da técnica. Dessa forma ,o presente trabalho buscou comparar a uniformidade de distribuição do potássio e do nitrogênio em sistema de irrigação por gotejamento. A solução de fertilizantes foi injetada durante 25 minutos, sendo recolhidas amostras de solução em diferentes momentos, durante e após ter sido finalizada a operação de injeção, tendo sido especificado o tempo de 35 minutos após o início da operação de injeção da solução de fertilizantes, como tempo-limite para a coleta da última amostra. As amostras coletadas tiveram os teores de potássio (K+) e nitrogênio (NO3- + NH4+) determinados. Com os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertirrigação; Injeção de fertilizantes; Uniformidade de distribuição de fertilizantes.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100010

Variabilidade espacial de atributos físicos de um argissolo vermelho-amarelo sob pastagem e vegetação secundária em regeneração natural
Provedor de dados: 70
Autores: Lima,Julião S. de S.; Sattler,Marcos A.; Passos,Renato R.; Oliveira II,Paulo C.; Souza,Gustavo S. de.
Este trabalho foi realizado com o objetivo de estudar a variabilidade espacial de atributos físicos de um Argissolo Vermelho-Amarelo sob pastagem e vegetação secundária em regeneração natural. Duas áreas foram escolhidas em uma encosta, com a amostragem de solo à profundidade de 0-0,2 m, com os pontos georreferenciados em uma malha regular de 10x10 m, totalizando 64 pontos em cada área. Foram avaliados o volume total de poros, macroporosidade, microporosidade, densidade do solo, resistência do solo à penetração e umidade do solo em cada ponto. Os atributos estudados na área de pastagem apresentam indicador de compactação do solo pelo pisoteio de animais, com estrutura moderada e forte dependência espacial, com exceção da macroporosidade e a resistência à...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manejo do solo; Geoestatística; Semivariograma.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200002

Quantificação das classes de erosão por tipo de uso do solo no município de Franca - SP
Provedor de dados: 70
Autores: Endres,Paula F.; Pissarra,Teresa C. T.; Borges,Maurício J.; Politano,Walter.
Impactos ambientais causados pelas atividades agropecuárias sobre o meio rural podem ser constatados quando são analisadas as paisagens da região. Vários estudos demonstraram que informações da paisagem obtidas a partir de imagens fotográficas são indispensáveis para o diagnóstico do processo erosivo do solo, aspecto indispensável no planejamento conservacionista. Neste trabalho, utilizando-se de técnicas de fotointerpretação, foi realizada a quantificação das classes de erosão acelerada no município de Franca - SP, relacionando-as com os tipos de cobertura vegetal. A coleção de fotografias aéreas empregadas foi produzida pela Base Aerofotogrametria e Projetos S.A., com escala aproximada 1:35.000, em outubro de 1990. Elaboraram-se cartas temáticas do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensoriamento remoto; Erosão; Uso/ocupação do solo.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100022

A COMBINATION OF DISCRETE EVENT SIMULATION AND MULTI-CRITERIA ANALYSIS TO CONFIGURE SUGARCANE DROP AND HOOK DELIVERY SYSTEMS
Provedor de dados: 70
Autores: Faria,Danilo A. F. de; Frazão,Márcia L. da S.; Vieira,José G. V.; Silva,João E. A. R. da; Lemos,Paula H.
ABSTRACT This article explores decision analysis regarding Drop and Hook (D&amp;H) transportation operations at sugarcane mills. By means of a case study, a combination of a discrete event simulation model and multi-attribute utility theory was used to evaluate different configurations for sugarcane delivery systems using internal, external, or no D&amp;H systems. A D&amp;H strategy maximises truck utilisation, as semi-trailers can be handled independently of the traction unit of the trucks, which makes the transport system more agile. For internal D&amp;H systems the semi-trailer detaching/attaching point is located inside the mill site while for external D&amp;H systems it is located outside, before the trucks’ weighbridge. Each configuration requires...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Drop and hook; Multicriteria analysis; Simulation model; Sugarcane; Transport.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200248

HYSTERESIS AND THERMAL INERTIA OF SPHERES OF ALTERNATIVE MATERIALS FOR BLACK GLOBE THERMOMETERS
Provedor de dados: 70
Autores: Sampaio,Carlos A. de P.; Terezo,Rodrigo F.; Vassem Júnior,Ilson; Silva,Leonardo M. da C.; Borges,Luiza K.
ABSTRACT This research was conducted with the objective of evaluating the thermal inertia and hysteresis of the following materials in a wind tunnel: hollow copper sphere with 150.0 mm diameter used as standard in globe thermometers, hollow brass sphere with 75.0 mm diameter, and two hollow plastic spheres with 115.5 and 69.7 mm diameter. The results showed that the thermal inertia and hysteresis for the hollow copper sphere were approximately 24 and 28 min, respectively; these values were bigger than those obtained for the other spheres, implying faster responses of these. While there were no statistical differences in the measurements conducted by globe thermometers which are used to indicate the black globe temperature with the different types of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal comfort; Instrumentation; Thermal properties; Radiant temperature.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500567

Perfis de distribuição volumétrica de pontas XR 11003 e TXVK-4 em diferentes condições de pulverização
Provedor de dados: 70
Autores: Bauer,Fernando C.; Raetano,Carlos G.
Com o objetivo de avaliar a uniformidade da distribuição volumétrica e o efeito da angulação dos bicos na barra em pulverizações, foi conduzido experimento em laboratório, com dez unidades de cada uma das pontas de jato plano XR 11003 e de jato cônico vazio TXVK-4, fabricadas pela Spraying Systems Co. As pontas XR 11003 foram avaliadas, isoladamente, em mesa de prova para bicos construída conforme a Norma ISO 5682-1:1996, a 0,30; 0,40 e 0,50 m de altura, submetidas à pressão de 200 e 300 kPa e posicionadas com ângulos de 30º e 45º no sentido horário e anti-horário e na vertical; as pontas TXVK-4 foram avaliadas nas mesmas alturas, porém a 300 e 400 kPa, e somente na vertical. A distribuição média do volume coletado em cada configuração, das dez unidades de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ponta de pulverização; Coeficiente de variação; Ângulo de pulverização.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200015

MODELING AND TESTING OF AN ICE BANK FOR MILK COOLING AFTER MILKING
Provedor de dados: 70
Autores: Jordan,Rodrigo A.; Cortez,Luís A. B.; Silveira Jr.,Vivaldo; Cavalcanti- Mata,Mário E. R. M.; Oliveira,Fellipe D. de.
ABSTRACT Based on mass and energy balance equations and data collected in specialized bibliographies, it was proposed a methodology for modeling of an ice bank for thermal storage of energy at low temperature to be used in milk cooling. The data obtained by the equations arrangement were used in the design and installation of a real system, which was tested to collect data and to compare it with the estimated. The data obtained in terms of prediction of ice formation, temperature of the ice bank, water and capacity of the selected refrigeration system prove the adequacy of the equations arrangement, showing that it can be used as a tool for sizing solid ice bank in smooth pipe coils, with good approximation.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Milk cooling; Modeling; Thermal storage.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400510

Sentido de pulverização em culturas de soja e feijão com pulverizador de barras
Provedor de dados: 70
Autores: Justino,Altair; Menon,Leandro; Bora,Luciano; Garcia,Luiz C.; Raetano,Carlos G.
O objetivo do experimento foi avaliar o melhor sentido de caminhamento de um pulverizador de barras, montado em três pontos no trator, nas culturas de soja e de feijão. As pulverizações foram orientadas no sentido longitudinal às linhas de semeadura, transversal às linhas de semeadura e no mesmo sentido das linhas de semeadura com os pneus percorrendo locais pré-definidos onde não houve a distribuição de sementes (tramlines). Foram avaliados os componentes de produtividade. Pelos resultados, pode-se observar que não houve diferença significativa quanto aos componentes de produtividade avaliados na cultura da soja quando se variou o sentido da pulverização. Na cultura do feijoeiro, a pulverização no sentido longitudinal apresentou maior produtividade.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Produtividade.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300012

SUGARCANE BASE CUTTING QUALITY USING RECTANGULAR AND CIRCULAR BLADES
Provedor de dados: 70
Autores: Paixão,Carla S. S.; Voltarelli,Murilo A.; Santos,Adão F. dos; Silva,Rouverson P. da.
ABSTRACT Sugarcane mechanized harvesting can lead to serious risks to the longevity of plantations when improperly operated, and may cause damages and disturbances in the remaining ratoons in the field. In this sense, this study aimed to evaluate the damage and disturbance to the sugarcane ratoons by the base cutting quality of two-blade models through statistical process control. The experiment was carried out during the 2015/16 growing season in an agricultural area of the Moreno Mill, located in Cravinhos, São Paulo, Brazil. The sugarcane harvester models A8800 (Machine 1) and BE1035 (Machine 2). The sugarcane variety cultivated in both treatments was SP80-1816. Thirty points were sampled per harvester, with 10-minute intervals between them. Equations...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cutting height; Control charts; Mechanized harvesting; Damages and disturbances; Saccharum spp.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100056

Nova versão do sistema de avaliação de terras - SIAT
Provedor de dados: 70
Autores: Garcia,Gilberto J.; Antonello,Sergio L.; Magalhães,Mônica G. M.
O SIAT é um sistema especialista para Avaliação de Terras derivado do MicroLEIS - Land Evaluation Information System desenvolvido na Espanha. Na primeira versão, as 12 variáveis foram adaptadas e ajustadas para condições tropicais, assim como a estrutura do programa e o banco de dados. Os testes de campo mostraram que os melhores resultados foram obtidos para escalas próximas de 1:100.000. Nesta segunda versão, os intervalos das variáveis foram redefinidos e uma interface de comunicação com o SIG IDRISI foi introduzida, permitindo a troca de dados entre os dois programas. Outra modificação importante foi a adoção de uma equação para calcular a erosividade no lugar de mapa apresentado no Manual do Usuário. Os testes de campo mostraram que o uso do SIAT é...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avaliação de terras; Capacidade de uso; SIG.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200026

SUPPLEMENTATION OF NUTRIENTS FOR TABLE BEETS BY IRRIGATION WITH TREATED DAIRY EFFLUENT
Provedor de dados: 70
Autores: Gomes,Tamara M.; Rossi,Fabrício; Tommaso,Giovana; Ribeiro,Rogers; Kushida,Marta M.; Stablein,Michael James.
ABSTRACT: This study was conducted to evaluate the nutritional status of table beet plants cultivated in a greenhouse irrigated with treated dairy effluent at different irrigation depths. The experimental design used was a randomized block in a 3 x 3 + 1 factorial arrangement with four replications and conducted in a greenhouse. The treatments consisted of three types of water sources and three irrigation depths applied by drip irrigation: anaerobic effluent; anaerobic/aerobic effluent; tap water, and irrigation for replenishment 50; 100 and 150% of the crop evapotranspiration (ETc). All these treatments were applied in combination with 50% of the recommended nitrogen fertilization for the table beet cultivation. A control treatment was irrigated with tap...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water reuse; Beta vulgaris; Anaerobic and aerobic system; Drip; Nutritional status.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601137

CLAY AND PHOSPHORUS LOSSES BY EROSION IN OXISOL WITH SUGARCANE RESIDUES
Provedor de dados: 70
Autores: Paula,Daniela T. De; Martins Filho,Marcílio V.; Farias,Vera L. DA S.; Siqueira,Diego S.
ABSTRACT Considering the importance of nutrients in the soil for the plants development and the soil quality conservation and the quantification relevance of them for proper soil management, the aims of this research were: (i) to quantify the clay loss, adsorbed and soluble P from interrill erosion influenced by the presence of sugarcane residues on the ground surface; (ii) to determine the minimum percentage of residues to be maintained on the soil surface to not enrich the eroded sediment by clay and soluble P (Psed) and adsorbed (Pads). The experimental area is located in Guariba - SP, with soil classified as Red Dystrophic Oxisol. The experiment was designed based on results of previous experiments with residue analysis of variance for 40 plots. These...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Interrill erosion; Simulated rainfall; Vegetation cover.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601063

Ambiente térmico no interior de modelos de galpões avícolas em escala reduzida com ventilação natural e artificial dos telhados
Provedor de dados: 70
Autores: Santos,Pedro A. dos; Yanagi Junior,Tadayuki; Teixeira,Vitor H; Ferreira,Leandro.
O presente trabalho teve o objetivo de avaliar o ambiente térmico no interior de modelos físicos de galpões avícolas construídos em escala reduzida (1:10). O conforto térmico foi avaliado por meio do Índice de Temperatura do Globo Negro e Umidade (ITGU), Carga Térmica de Radiação (CTR) e efetividade das coberturas em reduzir o ITGU em relação à cobertura construída com telhas de alumínio (épsilon). Quatro modelos construídos com telhas cerâmicas e equipados com ventilação natural ou forçada foram comparados a dois modelos construídos com telhas cerâmicas e de alumínio, respectivamente, sem lanternim. Pode-se concluir que as coberturas com câmaras de ventilação artificial (B30CVF) ou natural (B30CVN) proporcionaram melhores ambientes térmicos no interior...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cobertura; Conforto térmico; Avicultura.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300002

Metodologia para avaliação do desempenho de receptor de GPS de uso agrícola em condição cinemática
Provedor de dados: 70
Autores: Machado,Thiago M.; Molin,José P.; Povh,Fabrício P.; Salvi,José V.
São inúmeras as aplicações das tecnologias de Global Navigation Satellite System (GNSS), e o sistema mais utilizado é o Global Positioning System (GPS), desenvolvido pelos Estados Unidos. Em aplicações agrícolas, há a necessidade de posicionamento estático e cinemático, com demandas de distintos níveis de acurácia. No entanto, os usuários carecem de informação quanto ao desempenho cinemático de receptores GNSS, sendo disponibilizados apenas dados de desempenho estático, e por essa razão desenvolveu-se um veículo instrumentado para testar metodologia de avaliação do desempenho de receptores GNSS sob condição cinemática, visando a representar operações agrícolas. Foi utilizada instrumentação para coletar os dados sob variação de velocidade e sentido de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; GPS; Ensaio cinemático.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100013

PERFORMANCE OF CORN SOWING IN FERTILIZATION SYSTEM AND INTERCROPPING
Provedor de dados: 70
Autores: Cortez,Jorge W.; Furlani,Carlos E. A.; Silva,Rouverson P. da; Arcoverde,Sálvio N. S.
ABSTRACT The performance of the tractor-seeder can be influenced by factors related to the seeder, as loads and crop. The aim of the present study was to evaluate the performance of tractor-seeder at sowing in the corn crop in function of the fertilizer systems (at presowing and at sowing) and those intercropping of crops (corn + bean-Stizolobium deeringianum, corn + bean-Cajanus cajan and corn + bean-Dolichos lab lab). The experiment was carried out at FCAV-UNESP with totally randomized delineation, on factorial scheme (2x3) with four repetitions. The use of fertilization during the pre-sowing resulted in greater displacement speed and effective field capacity in the corn sowing operation, without changing the distribution of corn seeds; however, it...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Previous fertilization; Intercropping; Fuel consumption; Agricultural mechanization; Slippage.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200225

Spatial variability of mechanical resistance to penetration evaluated with mobile unit on haplic vertisol cultivated with mango
Provedor de dados: 70
Autores: Cortez,Jorge W.; Lopes,Hélio L.; Coelho,Daniela S.; Arcoverde,Sálvio N. S.
Since the advent of mechanized farming and intensive use of agricultural machinery and implements on the properties, the soil began to receive greater load of machinery traffic, which can cause increased soil compaction. The aim of this study was to evaluate the spatial variability of soil mechanical resistance to penetration (RP) in the layers of 0.00-0.10, 0.10-0.20, 0.20-0.30 and 0.30-0.40m, using geostatistics in an area cultivated with mango in Haplic Vertisol of the northeastern semi-arid, with mobile unit equipped with electronic penetrometer. The RP data was collected in 56 points from an area of 3 ha, and random soil samples were collected to determine the soil moisture and texture. For RP data analysis we used descriptive statistics and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil compaction; Machinery traffic; Agricultural mechanization.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200006

ONE- AND TWO-DIMENSIONAL ECOHYDRAULIC MODELING OF FORMOSO RIVER (MG)
Provedor de dados: 70
Autores: Oliveira,Iara De C. E; Silva,Demetrius D. Da; Guedes,Hugo A. S.; Dergam,Jorge A.; Ribeiro,Celso B. De M.
ABSTRACT The objective of this study was to compare ecohydrological simulations from a one-dimensional model (PHABSIM - Physical Habitat Simulation System) and a two-dimensional model (River2D) in order to indicate a reliable tool that could be used to determine public policies for the sustainable management of the water resources of the FormosoRiver basin(MG). The results from the calibration of hydraulic variables, namely, water depth and velocity, as well as habitat predictions for three fish species of the river were compared. The results showed that River 2D was best suited to simulate ecohydrological features for the studied river stretch. Although PHABSIM presented a better fit of the hydraulic variables at the calibration process, the use of only...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: PHABSIM; River2D; Weighted usable area; Water resources.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601050

GLOBAL SENSITIVITY ANALYSIS METHODS APPLIED TO HYDROLOGIC MODELING WITH THE SAC-SMA MODEL
Provedor de dados: 70
Autores: Uliana,Eduardo M.; Silva,Demetrius D. da; Moreira,Michel C.; Pereira,Donizete dos R.
ABSTRACT This study aimed to use global sensitivity analysis (GSA) methods to evaluate the sensitivity of the SAC-SMA hydrologic model parameters in the estimation of daily flows of the Piracicaba river basin. The study was carried out in three sections of flow monitoring of the Piracicaba river basin, with an area of 5,304.0 km2 and located in the State of Minas Gerais, Brazil. For the global sensitivity analysis of the SAC-SMA model, the Morris and Sobol methods were used. The model parameters showing high sensitivity were UZFWM, which represents the free water depth in the upper zone of the soil and interferes with the subsurface flow and groundwater aquifer recharge; ADIMP, which represents the additional impermeable area of the basin and interferes...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Rain-flow model; Sobol method; Morris method.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100065

DATA MINING TECHNIQUES FOR SEPARATION OF SUMMER CROP BASED ON SATELLITE IMAGES
Provedor de dados: 70
Autores: Becker,Willyan R.; Johann,Jerry A.; Richetti,Jonathan; Silva,Laíza C. DE A.
ABSTRACT: Due to the difficulty in discriminating soybean and corn in mappings obtained by the time series of satellite images, this study aimed to apply the data mining techniques to separate soybean and corn. Pure pixels selection from Landsat-8 were extracted and used to build a standard spectro-temporal EVI profile for both crops. These profiles were obtained with the Timesat software and, further incorporated in the Weka software. Five out of eleven variables of the standard spectro-temporal EVI profile for each crop were found through the decision tree, a data mining technique. These five variables were sufficient to achieve the separation of soybean and corn crops with an accuracy of 96.3% and a kappa index of 0.92.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Corn; EVI; J48; Soybean; Weka.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400750

Automatic and manual spray bar sections control
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Meer,Roderik W. V. D.; Vink,Peter; Justino,Altair; Garcia,Luiz C.
The use of precision farming tools in pesticide application technology can improve the techniques effectiveness during the spraying. Thus, this study aimed to compare automatic and manual systems to interrupt the syrup flow in the spray bar sections when applied in overlapped areas. The sprayings were carried out in eight places in completely randomized design. It was compared the spray consumption and the sprayed area in relation to the total area. The results indicated that in sprays performed with the automatic system there was an average savings of 17.2% of the sprayed volume. The sprayed area using the bar section's automatic control was an average 6.1% lower than the sprayed area with manual control.
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Precision farming and pesticide application technology.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600015

Modelo matemático aplicado à irrigação localizada com microtubos sob regime de escoamento turbulento
Provedor de dados: 70
Autores: Souza,Wanderley de J.; Botrel,Tarlei A.; Almeida,Alexsandro C. dos S.; Correa,Cristina B.
O presente trabalho teve como objetivos, desenvolver dois modelos matemáticos para dimensionamento de microtubos em irrigação localizada, operando sob regime de escoamento turbulento, nos quais foram incluídas as perdas de carga no microtubo, perda de carga localizada e perdas por energia de velocidade na saída do microtubo. Para a determinação da perda de carga localizada, obteve-se, por meio de dados de laboratório, valores de coeficientes K de dissipação de energia na entrada do microtubo. Os modelos foram avaliados com o dimensionamento de uma linha lateral de irrigação e tiveram ótimos desempenhos, tendo em vista que os dados coletados proporcionaram vazão média próxima da vazão de projeto, com coeficiente de determinação acima de 98%, excelente...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Linha lateral; Perda de carga; Hidráulica.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200008

Determination of management zones from normalized and standardized equivalent produtivity maps in the soybean culture
Provedor de dados: 70
Autores: Suszek,Grazieli; Souza,Eduardo G. de; Uribe-Opazo,Miguel A.; Nobrega,Lucia H. P.
Through the site-specific management, the precision agriculture brings new techniques for the agricultural sector, as well as a larger detailing of the used methods and increase of the global efficiency of the system. The objective of this work was to analyze two techniques for definition of management zones using soybean yield maps, in a productive area handled with localized fertilization and other with conventional fertilization. The sampling area has 1.74 ha, with 128 plots with site-specific fertilization and 128 plots with conventional fertilization. The productivity data were normalized by two techniques (normalized and standardized equivalent productivity), being later classified in management zones. It can be concluded that the two methods of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thematic map; Precision agriculture; Geostatistics; Soybean.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500007

Determinação do perfil radial de aspersores a partir de ensaios de distribuição de água em sistemas autopropelidos de irrigação
Provedor de dados: 70
Autores: Prado,Giuliani do; Colombo,Alberto.
Este trabalho apresenta uma rotina computacional, em Visual Basic 6, para determinar o perfil radial de aspersores, mediante ensaios de equipamentos autopropelidos de irrigação. Para a avaliação do programa, foi utilizado o aplicativo computacional SIMULASOFT e dados de ensaios de campo de sistemas autopropelidos de irrigação. As lâminas aplicadas, geradas pelo programa SIMULASOFT, foram para o aspersor PLONA-RL250 (bocal = 20 x 6 mm; pressão = 490 kPa), em deslocamento linear com velocidade de 50 m h-1, e quatro ângulos de giro distintos (180; 270; 330 e 360º). As lâminas aplicadas, observadas nos ensaios de campo, em condições de vento menores que 1,5 m s-1, foram para o aspersor PLONA-RL250, operando na pressão de 392 kPa e sob as condições: i) bocal de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Programa computacional; Lâminas aplicadas; Ensaios de laboratório.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200005

Performance of a diesel engine fueled with a preheated blend of soybean oil and petrodiesel
Provedor de dados: 70
Autores: Delalibera,Hevandro C.; Campolina,Nilson; Weirich Neto,Pedro H.; Ralisch,Ricardo.
Brazil is doing a major effort to find alternatives to diesel oil as combustible. Some study lines are oriented to the development of vegetable oils used as fuel, as a source of getting cheaper and have higher energy density than the converted vegetable oils, and less risk of environmental contamination. The aim of this study was to evaluate the performance, the useful life of the lubricant and some components of a Diesel Cycle engine, with an electronic injection system, in a long-term test operating with a preheated blend (65°C) of 50% (v v-1) of soybean oil in petrodiesel. There was a reduction of the useful life of the injectors which presented failure because of high wear with 264 hours of operation and showed an increase in emissions of particulate...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Electronic injection; Opacity; Lubricant.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600007

Produtividade e rendimento de sementes de pinhão-manso submetido à irrigação e adubação com OMM-Tech
Provedor de dados: 70
Autores: Evangelista,Adão W. P.; Melo,Paulo C. de; Oliveira,Ednaldo L. de; Faria,Manoel A. de.
Com o objetivo de avaliar os efeitos da irrigação e aplicação do fertilizante Organo-Minerais-Marinhos + Biotech® (OMM-Tech) na produtividade e rendimento do pinhão-manso, um experimento foi instalado em Lavras - MG. O delineamento estatístico utilizado foi o de blocos casualizados, com parcelas subdivididas, contendo três repetições. As parcelas receberam tratamentos constituídos por três formas de aplicação do fertilizante OMM-Tech, ou seja: T1 = Testemunha (Sem OMM-Tech); T2 = via solo (120 kg ha-1 de OMM-Tech na forma de pó); T3 = via foliar (OMM-Tech na forma líquida e na concentração de 5%); e T4 = via solo + foliar (60 kg ha-1 de OMM-Tech na forma de pó + OMM-Tech na forma líquida, na concentração de 2,5%). As sub-parcelas receberam os tratamentos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Jatropha curcas L.; Biodiesel; Água.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200011

Biomass allocation and water use efficiency in fertigated sweet pepper
Provedor de dados: 70
Autores: Albuquerque,Francimar da S.; Silva,Ênio F. de F. e; Nunes,Marcus F. F. N.; Souza,Amanda E. R. de.
The use of productivity information and efficiency of water use is important for the economic analysis of production and irrigation management, and also helps the economy of water use, which is essential to plant life. The objective of this study was to evaluate the biomass allocation, the water use efficiency and water content in fruits of sweet pepper cropped under the influence of irrigation blades and potassium doses. The statistic design was a completely randomized factorial scheme (5 x 2) and four replications, with five irrigation blades (80; 90; 100; 110 and 120% of crop evapotranspiration) and two levels of potassium (80 and 120 kg K2O ha-1 ), applied according to phenological phase, through a system of drip irrigation with self-compensated...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation blades; Potassium levels; Drainage lysimeters.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200011

GROWTH OF ORNAMENTAL PEPPER IN COLORED CONTAINERS UNDER PROTECTED ENVIRONMENTS
Provedor de dados: 70
Autores: Costa,Edilson; Alixame,Danieli; Silva,Abimael G. da; Pupim,Rafael de S.; Binotti,Flávio F. da S.
ABSTRACT Ornamental pepper plants produced in containers under protected environments have high added value. We carried out research with an aim to evaluate the growth and development of ornamental pepper in containers of different colors under two protected environments, both with thermal-reflective screens under a polyethylene film: one with 18–22 % shading and the other with 42–50 % in colored containers (brown, blue, black, and red). The treatments formed by a 2 × 4 factorial (environments × container colors) were arranged in a completely random pattern with 4 replications and 5 plants per plot, and a joint analysis of experiments was used to compare environments. The protected environment covered with low-density polyethylene film having 42–50 % of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Capsicum frutescens; Plant ambiance; Pot colors.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500581

MEASUREMENT AND ANALYSIS OF A FIELD AREA BASED ON AN ADAPTIVE KALMAN FILTER
Provedor de dados: 70
Autores: Fang,Susu; Wang,Zengcai; Zhong,Wenjun.
ABSTRACT: This paper proposed the use of an adaptive Kalman filter (AFK) to improve Global Positioning System (GPS) positioning accuracy to measure a tractor operational area. First, we used MATLAB to identify the operation trajectory. Then, we used different colors to show the area of operation. Finally, we used an image-processing method to calculate the effective operational area, actual operational area, and repeat and omission rates. We used these rates to evaluate the tractor efficiency. The experiment indicated that the Kalman filter improved the accuracy of GPS single-point positioning. To test the GPS area-measurement precision, field area measurements were taken. We used GPS to measure standard figures and some irregular figures. The results...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tractor; Kalman filter; Global Positioning System (GPS); Operational area.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500867

Resfriamento rápido de fornos de carbonização
Provedor de dados: 70
Autores: Oliveira Filho,Delly; Teixeira,Carlos A.; Silva,Juarez de S. e; Reis,Hamilton O.; Vorobieff,Cristhian L.
A importância dos recursos naturais renováveis no mundo é crescente. No processo produtivo do carvão vegetal, é possível aumentar a eficiência global de transformação da lenha de eucalipto em carvão vegetal. Em processos industriais, o tempo de resfriamento da massa de carvão varia de 6 a 8 dias, com a utilização do resfriamento natural da massa de carvão, sendo que a temperatura para a abertura dos fornos de carbonização é de cerca de 60 ºC, e a temperatura inicial da massa de carvão em torno de 480 ºC. Sendo assim, foi estudado um sistema de resfriamento de fornos de carbonização utilizando injeção de vapor de água, com o objetivo de reduzir o tempo de resfriamento do carvão. Foram construídos um forno tipo contêiner em escala de laboratório, de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Produção de carvão; Utilização de vapor; Otimização energética.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600004

PERFORMANCE OF FUZZY INFERENCE SYSTEMS TO PREDICT THE SURFACE TEMPERATURE OF BROILER CHICKENS
Provedor de dados: 70
Autores: Bahuti,Marcelo; Abreu,Lucas H. P.; Yanagi Junior,Tadayuki; Lima,Renato R. de; Campos,Alessandro T.
ABSTRACT This study aimed to compare fuzzy systems with different configurations to predict the surface temperature (ts) of broiler chickens subjected to different intensities and durations of thermal challenges in the second week of life. Data on the ts of broiler chickens aged 8 to 11 days were acquired by infrared thermography and subjected to combinations of four dry-bulb temperatures (tdb) (24, 27, 30, and 33 °C) and four durations of thermal challenges (DTC) (1, 2, 3, or 4 days). The input variables of the fuzzy systems were tdb and DTC, and the output variable was ts. The Mamdani inference method involving five defuzzification methods [center of gravity (centroid), bisector of the area (bisector), largest of maximum (lom), middle of maximum (mom),...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pertinence functions; Fuzzy logic; Defuzzification methods; Fuzzy inference methods; Chicks; Infrared thermography.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600813

Sistema de preparo do solo e sua influência na atividade microbiana
Provedor de dados: 70
Autores: Dadalto,Juliana P.; Fernandes,Haroldo C.; Teixeira,Mauri M.; Cecon,Paulo R.; Matos,Antonio T. de.
O sistema de preparo mecanizado do solo influencia diretamente sobre as propriedades físicas e biológicas do solo, além de propiciar ambiente adequado para o estabelecimento das culturas. O preparo do solo pode interferir na atividade microbiológica. Dessa forma, objetivou-se com o presente trabalho avaliar como os sistemas de preparo mecanizado do solo podem afetar sua atividade microbiológica. Os tratamentos foram os seguintes tipos de preparo do solo: plantio direto (PD), plantio convencional (PC) e cultivo mínimo (CM). Todas as análises foram feitas em três instantes: antes do preparo do solo, depois do preparo e 14 dias após o preparo do solo. Os tratamentos foram dispostos no delineamento em blocos casualizados, com quatro blocos. As coletas foram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantio direto; Microrganismos; Carbono orgânico.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300506

A utilização de mapas temáticos no diagnóstico de áreas suscetíveis à contaminação por percolado de aterro sanitário
Provedor de dados: 70
Autores: Rowe,Elmo J.; Cardoso,Décio L.
Atualmente, a preocupação com a proteção de áreas destinadas ao abastecimento público é eminente, pois a disponibilidade de água é cada vez menor. Entre as prováveis fontes de poluição das águas estão os aterros sanitários mal operados, aterros controlados e lixões. Os processos de contaminação no solo ocorrem lentamente e, frequentemente, sem consequências imediatas, porém, em longo prazo, podem ter efeitos sérios e possivelmente irreversíveis. O diagnóstico e a visualização da possível pluma de contaminação, em áreas destinadas à disposição de resíduos, podem ser realizados pela utilização de softwares que utilizam técnicas de interpolação, que transformam dados X, Y, Z, criando mapas temáticos. Com esse objetivo, foram coletadas amostras de solo a 1 e 2...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pluma de contaminação; Solo; Condutividade elétrica.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400017

MATHEMATICAL MODELING FOR DETERMINATION OF THE MAXIMUM MASS TRANSFER CAPACITY OF COWPEA BEANS
Provedor de dados: 70
Autores: Franco Junior,Hélio C.; Morais,Romulo A.; Silva,Warley G. da; Oliveira,Maria O. S.; Martins,Glêndara A. de S.
ABSTRACT Cowpea beans are of great socioeconomic expression for the rural population in North and Northeastern Brazil. This legume is rich in essential nutrients and exhibits great resistance to water stress. However, for grain processing, it is fundamental to study legume behavior during the hydration process. This study aims to evaluate the mass transfer of different cowpea beans via mathematical modeling to determine the viability of hydration for commercialization as a canned product. Physical and chemical analyses of lipids and moisture were performed. The soaking process was performed in a water bath with distilled water at 30, 40, and 50 °C. The mathematical model of Peleg presented satisfactory adjustments, with R2 values ranging between 99.78% and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Leguminous; Peleg model; Hydration; Beans.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200201

MATHEMATICAL MODELING AND HYSTERESIS OF SORPTION ISOTHERMS FOR PADDY RICE GRAINS
Provedor de dados: 70
Autores: Zeymer,Juliana S.; Corrêa,Paulo C.; Oliveira,Gabriel H. H.; Baptestini,Fernanda M.; Campos,Renata C.
ABSTRACT Knowledge on sorption isotherms is important for predicting drying and storage processes of a product. A sorption isotherm can be generated from two processes: desorption and adsorption. The lag between these two curves is called hysteresis. Static method was used to obtain the equilibrium moisture content of paddy rice grains, in different temperature (10, 20, 30, 40 and 50 ± 1°C) and relative humidity (between 11 and 76% ± 2%) conditions. Equilibrium moisture content data were correlated with eight mathematical models and. The Chung Pfost model had the best fit to the experimental data. Desorption and adsorption isotherms, represented by the Chung Pfost model, showed a sigmoidal shape, characteristic of type II curve. Equilibrium moisture...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Adsorption; Desorption; Hygroscopic equilibrium; Relative humidity; Temperature.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400524

Avaliação de tanques de escorva utilizados em substituição à válvula-de-pé em instalações de bombeamento
Provedor de dados: 70
Autores: Betini,Marcos O.; Zanini,José R.; Foratto,Leticia C.; Pereira,Gener T.
A maioria das instalações de abastecimento de água utiliza bombas hidráulicas do tipo turbobombas, requerendo que o interior de sua carcaça e da tubulação de sucção esteja preenchido com água (escorvados) para que a sucção da água possa ser efetivada. O escorvamento das bombas pode ser efetuado instalando-as abaixo do reservatório de captação (bomba afogada). Quando a bomba está acima do reservatório e o escorvamento é manual, é necessário usar válvulas-de-pé, que são suscetíveis ao mau funcionamento, limitando a confiabilidade do sistema, principalmente em caso de automação. Como alternativa à válvula-de-pé, neste trabalho, foram estudados dois tanques escorva, testados no Laboratório de Hidráulica e Irrigação da FCAV/UNESP - Jaboticabal, avaliando-se...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bombas hidráulicas; Bomba não-afogada; Escorvamento.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300007

Métodos probabilístico e determinístico para diagnóstico da necessidade de subsolagem de solos agrícolas
Provedor de dados: 70
Autores: Silva,Gilmar da; Cappelli,Nelson L.; Umezu,Claudio K.
Este trabalho apresenta duas metodologias para avaliar os níveis de resistência mecânica à penetração e auxiliar na tomada de decisão quanto à necessidade de se proceder à operação de subsolagem. A tomada de decisão baseia-se no volume de solo a ser mobilizado em função da resistência mecânica à penetração considerada crítica para o caso. O primeiro método, denominado probabilístico, utiliza-se de técnicas estatísticas para a definição do volume de solo a ser mobilizado. O segundo método, denominado determinístico, utiliza-se do cálculo da porcentagem do volume de solo a ser mobilizado e de sua distribuição espacial. Em ambos, são construídas curvas de porcentagem de pontos experimentais com níveis de resistência mecânica à penetração igual ou superior ao...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compactação do solo; Subsolagem; Resistência mecânica à penetração.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100015

Temperatura do solo afetada pela irrigação e por diferentes coberturas
Provedor de dados: 70
Autores: Ribas,Giovana G.; Streck,Nereu A.; Silva,Stefanía D. da; Rocha,Thiago S. M. da; Langner,Josana A.
RESUMO A irrigação suplementar e a cobertura do solo ("mulching") são práticas de manejo comumente usadas na agricultura. O objetivo deste trabalho foi quantificar a temperatura do solo desnudo com e sem irrigação, e sob diferentes coberturas do solo. Um ensaio de campo foi conduzido em Santa Maria-RS (29o 43' S latitude, 53º 42' W longitude e 95 m de altitude), com seis diferentes áreas: solo desnudo sem e com irrigação, solo com "mulching" de plástico transparente (espessura 100 µm), "mulching" de plástico opaco preto (espessura 110 µm), "mulching" de plástico opaco branco (espessura 150 µm) e cobertura vegetal com palha na dose de 5 t ha-1. A temperatura do solo foi medida a 0,05 m de profundidade, diariamente, às 15h (18 UTC), no período de 10-10-2011...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Propriedades térmicas; "mulching"; Irrigação suplementar.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500817

Estratégias de aeração de milho armazenado: temperatura e teor de água
Provedor de dados: 70
Autores: Nascimento,Vânia R. G.; Queiroz,Marlene R. de.
O objetivo deste trabalho consistiu em avaliar e comparar o desempenho de três diferentes estratégias de aeração de milho armazenado: aeração contínua, aeração noturna e aeração em condições de equilíbrio higroscópico entre os grãos e o ar ambiente. Utilizaram-se grãos de milho com dois níveis de teor de água; 11% e 17%. Realizou-se monitoramento contínuo da temperatura, e amostras de grãos foram retiradas durante os ensaios para análise do teor de água. Observou-se que todas as estratégias de aeração favoreceram a redução da temperatura nos grãos secos (11%) e umidificados (17%). A estratégia de aeração contínua foi a mais eficiente em grãos úmidos, uma vez que evitou aquecimento dos grãos durante o armazenamento. Nenhuma estratégia de aeração manteve a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Armazenagem; Conservação de grãos; Temperatura; Teor de água.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400013

Modeling and simulation of forced-air cooling of strawberries using variable convective coefficient
Provedor de dados: 70
Autores: Siqueira,Álvaro J. H.; Costa,Andréa O. da; Costa Junior,Esly F. da.
In the forced-air cooling process of fruits occurs, besides the convective heat transfer, the mass transfer by evaporation. The energy need in the evaporation is taken from fruit that has its temperature lowered. In this study it has been proposed the use of empirical correlations for calculating the convective heat transfer coefficient as a function of surface temperature of the strawberry during the cooling process. The aim of this variation of the convective coefficient is to compensate the effect of evaporation in the heat transfer process. Linear and exponential correlations are tested, both with two adjustable parameters. The simulations are performed using experimental conditions reported in the literature for the cooling of strawberries. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mathematical modeling; Cooling; Parameters estimation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100017

Irrigation management influence and fertilizer doses with boron on productive performance of cauliflower
Provedor de dados: 70
Autores: Pereira,Michel E. M.; Lima Junior,Joaquim A. de; Souza,Rodrigo O. R. de M.; Gusmão,Sergio A. L. de; Lima,Valdeides M.
ABSTRACT In order to provide scientific information about the irrigated cauliflower production in Northeast of Para, an experiment was installed in the Federal Rural University of Amazonia farm with the Desert hybrid under different water tensions on the ground and boron doses in the municipality of Igarapé-Açu – PA. The experimental design was a randomized block in a 4 x 4 factorial, sixteen treatments with three replications. The treatments consisted of four water tensions on the ground (15, 30, 45 and 60 kPa) as an indicative of the time to irrigate and four boron doses (0, 2, 4 and 6 kg ha-1). The irrigation was performed with drippers and irrigation management with tensiometers. Each plot, 4 m2, consisted of 8 plants located in the spacing of 1.0 m...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brassica oleracea var; Botrytis; Drip irrigation; Tensiometer.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500811

Uso do cilindro infiltrômetro único em diferentes solos
Provedor de dados: 70
Autores: Simões,Welson L.; Figueirêdo,Vladimir B.; Silva,Elio L. da.
O infiltrômetro de anéis concêntricos (IAC) tem sido empregado para a determinação da velocidade de infiltração básica de água no solo (VIB), porém, para sistemas de irrigação por aspersão, a melhor técnica é a que apresenta carga hidráulica zero, como nos simuladores de chuva. O presente trabalho teve o objetivo de avaliar o uso de infiltrômetro de cilindro único (ICU), comparando-o com o IAC e com um simulador de chuva. O experimento foi realizado em dois tipos de solo classificados como Latossolo Vermelho distroférrico e Cambissolo, onde se utilizou um ICU com 0,20 m de diâmetro e 0,50 m de altura. As cargas hidráulicas utilizadas variaram de 0,03 m a 0,30 m com intervalos crescentes de 0,03 m, com três repetições. Utilizou-se de um IAC de 0,30 e 0,90 m...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Infiltrômetro; Infiltração; Irrigação.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200009

Colheita de citros e obtenção de dados para mapeamento da produtividade
Provedor de dados: 70
Autores: Molin,José P.; Mascarin,Leonardo S.
A citricultura é de fundamental importância para a economia brasileira devido a sua expressiva participação na exportação e pela geração de empregos. A colheita manual é atualmente realizada na totalidade das propriedades citrícolas nacionais. A ausência de técnicas para a geração de mapas de produtividade em citros é uma das grandes dificuldades para a implantação da agricultura de precisão, o que justifica empreender técnicas e equipamentos para essa finalidade. Neste trabalho, teve-se o objetivo de ter o correto entendimento dos sistemas de colheita existentes, suas características úteis e limitações. A partir de então, desenvolveu-se e testou-se uma proposta de geração de dados para obtenção de mapas de produtividade sem interferir no processo vigente....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Laranja; Agricultura de precisão; Mapa de produtividade.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100020

CROP MODELING WITH LESS DATA: THE FAO MODEL FOR SOYBEAN YIELD ESTIMATION
Provedor de dados: 70
Autores: Richetti,Jonathan; Johann,Jerry Adriani; Uribe-Opazo,Miguel Angel.
ABSTRACT Crop growth simulation models such as WOFOST and DSSAT are useful, but require several inputs that sometimes are not available, especially in developing areas. In addition, measured data is usually time and labor-intensive. In search of faster and easier methods for soybean estimates, this study presents a lower input requiring methodology for yield estimation. This study combines the FAO-33 yield model with the agro-ecological zone approach for soybean yield estimations using mostly indirect data. Sowing and harvest dates and yield were collected from 74 soybean commercial farms. Agrometeorological data from the European Centre for Medium-Range Weather Forecasts (ECMWF) were used. Fifty farms (66%) were used to calibrate the model and 24 farm...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water balance; Evapotranspiration; Thornthwaite and Mather.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200196

Efeito das dimensões da placa difusora no comportamento hidráulico de um modelo comercial de filtro de areia
Provedor de dados: 70
Autores: Deus,Fábio P. de; Testezlaf,Roberto; Mesquita,Marcio.
O objetivo deste trabalho foi avaliar o efeito da mudança da forma e das dimensões da placa difusora de um filtro de areia comercial sobre a perda de carga gerada pelo equipamento, quando submetido ao escoamento no sentido de filtração, sob as condições de filtro vazio e na presença da camada filtrante. Comparou-se o comportamento hidráulico da placa difusora original do equipamento com placas do tipo plano, com bordas com diferentes dimensões. Os ensaios foram conduzidos em um módulo experimental construído no Laboratório de Hidráulica e Irrigação da FEAGRI/UNICAMP, utilizando quatro combinações de dimensões de placa difusora e para taxas de filtração com valores de 40; 60; 80 e 100 m³ h-1 m-2. Os resultados mostraram que as placas difusoras propostas não...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação localizada; Tratamento da água; Entupimento de emissores.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300012

SPECTRAL VEGETATION INDEXES APPLIED TO NITROGEN SUFFICIENCY INDEX: A STRATEGY WITH POTENTIAL TO INCREASE NITROGEN USE EFFICIENCY ON TOMATO CROP
Provedor de dados: 70
Autores: Oliveira,Thiago F.; Pinto,Francisco A. C.; Silva,Derly J. H.
ABSTRACT The tomato crop is one of the most demanding of nitrogen fertilizers. This element on soil has an elevated mobility that can represent danger to the environment and reduces its efficiency. Therefore, the purpose of this study was to evaluate the methodology for recommending nitrogen fertilizer for tutored tomatoes with a variable rate based on nitrogen sufficiency index. The treatments consisted of a reference plot and five treatments with the nitrogen sufficiency index calculated on spectral indexes NDVI, GNDVI, MCARI, PSSRa and the SPAD value. The productivity was evaluated considering the fruits size and viability. The descriptors of quality, color, soluble solids, total acidity, titratable acidity and flavor were also evaluated. All the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fruit quality; Precision agriculture; Tomato nutrition; Variable rate fertilization.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100118

EMPIRICAL METHODS FOR ESTIMATING REFERENCE SURFACE NET RADIATION FROM SOLAR RADIATION
Provedor de dados: 70
Autores: Flumignan,Danilton L.; Rezende,Maiara K. A.; Comunello,Eder; Fietz,Carlos R.
ABSTRACT Net radiation (Rn) of reference surface is important information that has many applications, but its measurement is rare due to the high cost of the sensor and the complexity involved on the measurement. Therefore, estimate Rn from another variable is desirable, as from solar radiation (Rs); however, standard methods used are complex, making interesting the use of simplified methodologies. Considering these aspects, the present study aimed to set two empirical methods to estimate Rn from Rs for Dourados region, Mato Grosso do Sul, Brazil. One method was based on mathematical modeling (Gauss Method). The other one was a more simplified and practical approach (Practical Method) comprising the determination of fixed monthly conversion factors. It was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Weather station; Gauss Method; Practical Method; Reference evapotranspiration.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100032

INCIDENCE OF FUNGI IN MOMBASA GRASS SEEDS DURING THE STAGES OF THE SEED CONDITIONING PROCESS
Provedor de dados: 70
Autores: Silva,Givanildo Z. da; Martins,Cibele C.; Melo,Lilian F. de; Jeromini,Tatiane S.; Panizzi,Rita de C.
ABSTRACT The objective of this study was to evaluate the effect of the seed conditioning process on the sanitary quality of Panicum maximum ‘Mombasa’ seeds. The seeds were sampled before processing and after exiting the seed blower and sieves (discharge from the top and bottom sieves), first gravity separator (intermediate discharge), seed treatment equipment (dyeing the seeds of the intermediate discharge from the first separator), and second gravity separator (upper, intermediate, and lower discharge). Sanitary analysis was performed by the Blotter Test method with and without surface disinfestation of the seeds, which were incubated at 20 ± 2 °C, with a photoperiod of 12 h, for 7 d. The conditioning process increased the incidence of Fusarium sp. in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Seed pathology; Processing; Seed sanitation; Panicum maximum ‘Mombasa’.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200234

Distribuição longitudinal e germinação de sementes de milho com emprego de tratamento fitossanitário e grafite
Provedor de dados: 70
Autores: Jasper,Roberto; Janszen,Uwe; Jasper,Mônica; Garcia,Luiz C.
Teve-se o objetivo de avaliar as formas de se misturar o lubrificante sólido grafite nas sementes de milho, as dosagens e a influência desse na distribuição longitudinal e na germinação, em sementes sem e com tratamento fitossanitário, em mecanismo dosador com disco perfurado horizontal. Os fatores analisados foram: distribuição longitudinal das sementes (espaçamentos falhos, múltiplos e aceitáveis) e a porcentagem de germinação aos 7 e aos 14 dias após a instalação no germinador. Concluiu-se que o tratamento fitossanitário aumentou os espaçamentos falhos e múltiplos e reduziu os espaçamentos aceitáveis. O emprego de grafite reduziu os espaçamentos falhos e múltiplos e elevou os espaçamentos aceitáveis. A melhor forma de mistura do grafite ocorreu na...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Disco perfurado horizontal; Espaçamentos aceitáveis; Semeadora.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100031

FITTINGS OF ADSORPTION ISOTHERM MODELS AND THERMODYNAMIC PROPERTIES OF URUNDAY SEEDS
Provedor de dados: 70
Autores: Isquierdo,Eder P.; Caldeira,Daniela S. A.; Siqueira,Valdiney C.; Martins,Elton A. S.; Quequeto,Wellytton D.
ABSTRACT This study aimed to obtain and evaluate thermodynamic properties and hygroscopic equilibrium isotherms of urunday seeds as a function of air relative humidity and temperature, as well as identify the best-fitted mathematical models for adsorption phenomenon. A static-gravimetric method was used to obtain hygroscopic equilibrium moisture content. Seeds were placed in airtight containers with different saturated saline solutions for relative humidity control. These were then kept in BOD incubator chambers at 10, 20, 30, and 40 °C. Hygroscopic equilibrium moisture content decreased as temperature increased, for the same water activity. The Sigma-Copace model best-fitted seed adsorption data for equilibrium water activity intervals between 0.1129 and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water activity; Isokinetic; Sorption isotherms; Myracrodruon urundeuva; Relative humidity.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300374

Uso da geoestatística para avaliar a captação automática dos níveis de pressão sonora em instalações de creche para suínos
Provedor de dados: 70
Autores: Borges,Giselle; Miranda,Kesia O. da S.; Rodrigues,Valéria C.; Risi,Natalia.
Este trabalho teve o objetivo de estudar a influência da distribuição de decibelímetros na captação automática dos níveis de pressão sonora, em ambiente de produção intensiva de suínos. O experimento foi conduzido em sala do setor de creche de uma granja comercial de suínos situada no município de Monte Mor, Estado de São Paulo. A sala foi dividida em dez quadrantes idênticos, e os decibelímetros foram instalados no centro geométrico de cada quadrante. Utilizou-se a geoestatística para avaliar a dependência espacial entre os decibelímetros e para predizer os níveis de pressão sonora em locais onde estes não foram instalados. Os dados foram analisados pela correlação entre os decibelímetros e por intermédio da geoestatística, que possibilitou afirmar que...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Níveis de ruídos; Suínos; Vocalização; Metodologia; Decibelímetros.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300002

WATER DEPLETION DEPTH FOR IRRIGATION OF POTATO CULTIVAR ÁGATA
Provedor de dados: 70
Autores: Silva,Edinéia F. da; Jadoski,Sidnei O.; Martinkoski,Lais.
ABSTRACT Potato (Solanum tuberosum L.) cultivation has a high demand for management and treatments during the vegetative cycle in the field. Among these requirements, water management is a limiting factor of tuber productivity and quality. This study aimed to determine the most appropriate soil water depletion depth for irrigation management in potato crops of Ágata cultivar, under the edaphoclimatic conditions of Guarapuava-PR, considering its influence on crop vegetative development. The study was conducted using four water depletion depths in the soil (12, 24, 36, and 48 mm). The different irrigation treatments promoted differences in shoot dry mass, leaf area index (LAI), number of tubers per plant, and productivity. The highest yield was observed for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil water; Potato cultivars; Evapotranspiration.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400434

Microgeneration of electricity with producer gas in dual fuel mode operation
Provedor de dados: 70
Autores: Silva,Marcelo J.; Souza,Samuel N. M. de; Ricieri,Reinaldo P.; Souza,Abel A.; Secco,Deonir.
Among the alternatives to meet the increasing of world demand for energy, the use of biomass as energy source is one of the most promising as it contributes to reducing emissions of carbon dioxide in the atmosphere. Gasification is a technological process of biomass energy production of a gaseous biofuel. The fuel gas has a low calorific value that can be used in Diesel engine in dual mode for power generation in isolated communities. This study aimed to evaluate the reduction in the consumption of oil Diesel an engine generator, using gas from gasification of wood. The engine generator brand used was a BRANCO, with direct injection power of 7.36 kW (10 HP) coupled to an electric generator 5.5 kW. Diesel oil mixed with intake air was injected, as the oil...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gasification; Biomass; Diesel engine generator.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500005

Temperature effect in potassium and nitrate ions in soil transport
Provedor de dados: 70
Autores: Gonçalves,Adriano D. M. A.; Miranda,Jarbas H.; Rossi,Paulo; Sabadin,José F. G.; Kamogawa,Marcos Y.
When doing researches on solute dynamics in porous medium, the knowledge of medium characteristics and percolating liquids, as well as of external factors is very important. An important external factor is temperature and, in this sense, our purpose was determining potassium and nitrate transport parameters for different values of temperature, in miscible displacement experiments. Evaluated parameters were retardation factor (R), diffusion/dispersion coefficient (D) and dispersivity, at ambient temperature (25 up to 28 ºC), 40 ºC and 50 ºC. Salts used were potassium nitrate and potassium chlorate, prepared in a solution made up of 5 ppm nitrate and 2.000 ppm potassium, with Red-Yellow Latosol porous medium. Temperature exhibited a positive influence upon...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Breakthrough curves; Miscible displacement; Computational modeling.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300005

Análise de imagens digitais para a avaliação do comportamento de pintainhos de corte
Provedor de dados: 70
Autores: Cordeiro,Marcelo B.; Tinôco,Ilda F. F.; Filho,Roque M. de Mesquita; Sousa,Fernanda C. de.
Na busca por respostas quanto às condições de bem-estar animal, visou-se a avaliar neste trabalho o comportamento de pintainhos nas duas primeiras semanas de vida, por meio de processamento de imagens digitais. O experimento foi realizado em dois galpões comerciais, utilizados para criação de 15.200 aves de corte por galpão, durante um ciclo produtivo, dotados com fornalha a lenha de aquecimento indireto do ar. Foram instaladas duas câmeras de vídeo por galpão para aquisição de imagens digitais. Uma das câmeras possuía inclinação angular de 45º, e a outra, inclinação angular de 90º em relação ao solo. As imagens foram analisadas para cada condição climática diária e binarizadas, sendo depois processadas por meio de descritor de agrupamento/dispersão e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Comportamento animal; Pintainhos de corte; Processamento de imagens.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300002

Thermal performance and concentration of gases in facilities for pigs in semiarid region from State of Paraiba - Brazil
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Amancio,Daniele; Nascimento,José W. B. do; Gomes,Josivanda P.; Silva,Rafael C.
The study was conducted in a facility for pigs during the nursery and finishing in the town of 'Montadas', in the semiarid of the state of Paraiba, Brazil, in the rainy and dry season, aiming to evaluate the concentration of oxygen, methane, carbon monoxide and ammonia, and the bioclimatic indexes: ambient temperature (AT), relative humidity (RH) and the index of black globe temperature and humidity (IBGTH). These indexes differed significantly (P&gt;0.05) between the periods and times. The AT in the rainy season was in the thermal comfort zone(TCZ) in most of the times in the nursery; for the finishing phase, thermal discomfort occurred; during the dry season, there was thermal comfort in the nursery phase; in the finishing phase the thermal discomfort...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Welfare; Thermal comfort; Gases; Semiarid.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100004

Perdas de solo, matéria orgânica e nutrientes por erosão hídrica em uma vertente coberta com diferentes quantidades de palha de cana-de-açúcar em Guariba - SP
Provedor de dados: 70
Autores: Sousa,Gasparino B.; Martins Filho,Marcílio V.; Matias,Sammy S. R.
A erosão em entressulcos resulta da desagregação causada pelo impacto das gotas de chuva na superfície do solo e pelo transporte superficial das partículas do solo desagregadas, onde se encontram a matéria orgânica e os nutrientes fundamentais para a produção agrícola. O presente trabalho teve como objetivo avaliar as perdas de solo, matéria orgânica e nutrientes em uma vertente localizada em uma área de Latossolo Vermelho-Amarelo distrófico, cultivada com cana-de-açúcar, que é colhida mecanicamente. As parcelas experimentais foram submetidas à ação de uma chuva simulada com intensidade de 60 mm h-1, durante 65 minutos. Foram feitas análises do sedimento erodido para a determinação do volume de solução, das perdas de solo, matéria orgânica e nutrientes....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão em entressulcos; Chuva simulada; Palhada; Latossolo Vermelho.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300008

Evapotranspiration and crop coefficient of drip irrigated watermelon in Piaui coastline, Brazil
Provedor de dados: 70
Autores: Bastos,Edson A.; Silva,Cláudio R.; Rodrigues,Braz H. N.; Andrade Jr.,Aderson S.; Ibiapina,Lívia M. M.
The knowledge of the evapotranspiration (ETc) and crop coefficient (Kc) is fundamental to plan and to manage the irrigation of any crop. The aim of this study was to determine the daily and hourly evapotranspiration of drip irrigated watermelon (Citrullus Lanatus, var. Crimson Sweet) and crop coefficient (Kc) in each crop development phase. The experiment was carried out in an experimental area of 1.27 ha of Embrapa Mid-North, localized in Parnaíba (02°54'S, 41°47'W and 46 m above of sea), State of Piauí, Brazil, from September to November, 2006. Electronic weighing lysimeters of 1.5 m x 1.5 m wide and long and 1.0 m deep were used to obtain the evapotranspiration. The plants were drip irrigated with a lateral row per plant row and drippers spaced 0.5 m...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Citrullus lanatus; Lysimeter; Water consume.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300017

TECHNOLOGICAL QUALITY OF SOYBEAN OIL OBTAINED FROM STORED GRAIN UNDER CONTROLLED ENVIRONMENTAL CONDITIONS
Provedor de dados: 70
Autores: Bischoff,Tábata Z.; Coelho,Silvia R. M.; Schoeninger,Vanderleia; Cassol,FLÁVIA D. R.; Prado,Naimara V. Do; Christ,Divair.
ABSTRACT: Soybean oil has many important components, but for its maintenance it is essential that there is an appropriate storage, temperature, relative humidity and optimum grain moisture content, because the oxidation reactions occur by improper storage, causing product deterioration. The objective of this study was to evaluate the main changes in the quality of soybean crude oil, from grain storage in temperature of 30°C and different relative humidity (59.6%, 67.0% and 76.0%). Soybean grains were packaged in plastic recipients, where saturated salt solutions were added so the grains reached the desired moisture. The analyses of moisture content, lipid, acidity index, color, antioxidant capacity, specific extension by absorption in the ultraviolet...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Extinction specific; Glycine max; Oxidation lipid; Relative humidity.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601145

PERFORMANCE OF DIESEL ENGINE FUELLED WITH FOUR VEGETABLE OILS, PREHEATED AND AT ENGINE WORKING TEMPERATURE
Provedor de dados: 70
Autores: Delalibera,Hevandro C.; Johann,André L.; Figueiredo,Paulo R. A. de; Toledo,Anderson de; Weirich Neto,Pedro H.; Ralisch,Ricardo.
ABSTRACT With the rise of restrictions imposed by law for gases emission, several technologies both for petrodiesel (PD) or diesel engines are been applied, such as the sulfur reduction and the injection electronic command, followed of gases recirculation and/or after-treatment. The utilization of biofuels is considered as an interesting option for pollutants reduction. In this study was evaluated the performance on short duration tests (minor period than the factory indication of the lubricant lifespan) of the Diesel engine fueled with four vegetable oils. With the aim to select the most interesting oils for future evaluations in long duration tests. The analyzed variables were fuel consumption, power relative loss and opacity, for oils of linseed,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Consumption; Brake power; Opacity.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200302

O uso de geotecnologias no planejamento ambiental: o plano diretor municipal de Tambaú - SP
Provedor de dados: 70
Autores: Garcia,Gilberto J.; Pinto,Sergio dos A. F.; Antonello,Sergio L.; Nobre,Mayra F.
A Lei Federal 10.257, de 10 de julho de 2001, regulamentou os artigos 182 e 183 da Constituição Federal de 1988 no que trata da política urbana, especialmente da propriedade, sendo obrigatório para municípios com mais de 20.000 habitantes. Até então, os planos diretores municipais vinham sendo feitos levando em conta apenas as respectivas áreas urbanas, A partir desta lei, tais planos tiveram de levar em conta também as áreas rurais, integrando-as no processo do planejamento municipal sustentado. Analisando-se os planos diretores municipais recentes, elaborados a partir dessas novas diretrizes, nota-se que a maioria ainda enfatiza a área urbana, em detrimento da área rural. O objetivo deste trabalho foi, a partir de um estudo de caso, avaliar e validar...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Análise ambiental; Zoneamento ambiental; Planejamento ambiental; Plano diretor municipal.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600018

Comparação de penetrômetros na avaliação da compactação de latossolos
Provedor de dados: 70
Autores: Beutler,Amauri N.; Centurion,José F.; Silva,Alvaro P.
Diversos penetrômetros são utilizados para avaliar a resistência do solo à penetração em sistemas de uso e manejo, no entanto os valores obtidos com os mesmos divergem. O objetivo deste estudo foi comparar os resultados obtidos com três penetrômetros, em três níveis de compactação. Utilizou-se de um Latossolo Vermelho distrófico (LVd), textura média, e um Latossolo Vermelho eutroférrico (LVef), textura argilosa, cujas amostras foram coletadas na camada de 0-20 cm e compactadas em camadas, em vasos de 25 cm de diâmetro e 20 cm de altura. Determinou-se a resistência do solo à penetração com os penetrômetros de impacto, estático de anel dinamométrico e eletrônico de laboratório. Em solo compactado, o penetrômetro de impacto apresentou valores superiores de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resistência à penetração; Atributos físicos do solo; Conteúdo de água.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100008

Determination of piglets’ rectal temperature and respiratory rate through skin surface temperature under climatic chamber conditions
Provedor de dados: 70
Autores: Mostaço,Gustavo M.; Miranda,Késia O. da S; Condotta,Isabella C. F. da S; Salgado,Douglas D’Alessandro.
ABSTRACT In animal farming, an automatic and precise control of environmental conditions needs information from variables derived from the animals themselves, i.e. they act as biosensors. Rectal temperature (RT) and respiratory rate (RR) are good indicators of thermoregulation in pigs. Since there is a growing concern on animal welfare, the search for alternatives to measure RT has become even more necessary. This research aimed to identify the most adequate body surface areas, on nursery-phase pigs, to take temperature measurements that best represent the correlation of RT and RR. The main experiment was carried out in a climate chamber with five 30-day-old littermate female Landrace x Large White piglets. Temperature conditions inside chamber were varied...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Thermal control; Animal welfare; Temperature sensors; Physiological modelling; Precision livestock farming; Environmental control for swine.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000600979

Atributos físicos e requerimento de potência de uma semeadora-adubadora em um Latossolo sob estados de compactação
Provedor de dados: 70
Autores: Bonini,Andreia K.; Gabriel Filho,Antonio; Secco,Deonir; Souza,Renan F. de; Tavares,Celso.
Este experimento foi desenvolvido em um Latossolo, no Núcleo Experimental de Engenharia Agrícola, localizado em Cascavel - PR, com o objetivo de avaliar os atributos físicos e o esforço tratório de semeadora-adubadora em quatro estados de compactação, e sua influência na população inicial das culturas de soja e milho. O delineamento consistiu em esquema "Split Block", com dois fatores, sendo duas culturas (soja e milho) no primeiro fator e quatro estados de compactação no segundo fator, totalizando oito tratamentos. Os tratamentos foram: T0 - sem compactação adicional; T1 - com uma passada; T3 - com três passadas, e T5 - com cinco passadas de rolo compactador. Avaliaram-se a profundidade do sulco, a velocidade média de deslocamento, a força e a potência...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Densidade do solo; Máquina agrícola; Tração.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100014

MONITORING OF SOYBEAN MECHANICAL HARVESTING AS A FUNCTION OF PLOT SHAPES
Provedor de dados: 70
Autores: Paixão,Carla S. S.; Alcântara,Aline S.; Voltarelli,Murilo A.; Silva,Rouverson P. da; Tavares,Tiago de O.
ABSTRACT: Information on harvester performance is important in the management and optimization of mechanized agricultural systems. In this sense, the aim of this study was to monitor the operation quality of soybean mechanical harvesting in different plot shapes by means of statistical process control. The harvest was carried out in an agricultural area of a farm located in Uberaba, MG, Brazil, with an experimental design based on the assumptions of statistical quality control and 18, 28, and 24 replications for irregular, rectangular, and trapezoidal plots, respectively. The variables and/or quality indicators of harvester performance were forward speed, engine speed, cylinder speed, and concave opening. The lowest variation occurred in the irregular plot...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Grain harvester; Harvester machine performance; Statistical quality control; Glycine max (L.) Merrill.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400689

Decomposition kinetics of gaseous ozone in peanuts
Provedor de dados: 70
Autores: Alencar,Ernandes R. de; Faroni,Lêda R. D.; Martins,Marcio A.; Costa,André R. da; Cecon,Paulo R.
This study was conducted to evaluate the decomposition kinetics of gaseous ozone in peanut grains. This evaluation was made with 1-kg peanut samples, moisture contents being 7.1 and 10.5% wet basis (w.b.), placed in 3-liter glass containers. The peanut grains were ozonated at the concentration of 450 µg L-1, at 25 and 35 ºC, with gas flow rates of 1.0 and 3.0 L min-1. Time of saturation was determined by quantifying the residual concentration of ozone after the gas passed through the grains to constant mass. The decomposition kinetics of ozone was evaluated after the grain mass was ozone-saturated. For the peanut grains whose moisture content was 7.1% (w.b.), at 25 and 35ºC and with flow rates of 1.0 and 3.0 L min-1, the values obtained for time of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Concentration of saturation; Time of saturation; Half-life.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500011

Behavior, performance and physiological parameters of pigs reared in deep bedding
Provedor de dados: 70
Autores: Caldara,Fabiana R.; Rosa,Poliana S. G.; Ferreira,Rony A.; Reis,Nayana M. de O.; Nääs,Irenilza de A.; Paz,Ibiara C. de L. A.; Garcia,Rodrigo G.; Ferreira,Viviane M. O. dos S.
An experiment was conducted to evaluate the behavior, performance and physiological parameters of pigs in different production systems. Twenty four animals in the growth phase were distributed in a randomized block design in three treatments: T1 - concrete floor, T2 - deep bedding with wood shaving, and T3 - deep bedding with coffee husks. The behavioral study was carried out by observing the animal behavior for an uninterrupted period of eight hours throughout seven weeks. The proportions of time spent in each behavior were characterized using the frequency histogram composition. Environmental (IBGTH), physiological (rectal and skin temperature and respiratory rate) and performance (weight gain, feed intake and feed conversion) parameters were measured in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Environment; Animal welfare; Coffee husks; Wood shaving; Swine production.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000100005

Produtividade e composição química do capim-Tifton 85 submetido a diferentes taxas de aplicação do percolado de resíduo sólido urbano
Provedor de dados: 70
Autores: Matos,Antonio T. de; Silva,Denise de F.; Monaco,Paola A. V. Lo; Pereira,Odilon G.
Este trabalho foi realizado com o objetivo de avaliar o efeito da aplicação de diferentes taxas de percolado de resíduo sólido urbano (RSU) na produtividade e na composição química da parte aérea do capim-Tifton 85 (Cynodon spp). O percolado foi aplicado nas taxas de 0 testemunha); 250; 500; 750 e 1.000 kg ha-1 d-1 de DBO5, durante 8 meses. No tratamento-testemunha, não receptor do percolado, aplicou-se água da rede de abastecimento público, sendo a lâmina de aplicação definida com base na Evapotranspiração de Referência (ETo). O experimento foi analisado no esquema de parcelas subdivididas, tendo nas parcelas cinco concentrações de DBO5, e nas subparcelas, os cortes, no delineamento em blocos casualizados, com quatro repetições. Os dados foram submetidos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aterro sanitário; Chorume; Fertirrigação; Forrageira.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100019

Conforto térmico de bovinos da raça nelore a pasto sob diferentes condições de sombreamento e a pleno sol
Provedor de dados: 70
Autores: Navarini,Franciele C.; Klosowski,Elcio S.; Campos,Alessandro T.; Teixeira,Rodrigo de A.; Almeida,Clécio P.
Principalmente em regiões de clima quente, a produção bovina sob condições de pasto pode ser melhorada com o uso de sombra natural para minimizar o estresse por calor. Desse modo, o objetivo do presente estudo foi avaliar o efeito do estresse térmico por meio de índices de conforto térmico na produção bovina sob diferentes condições de sombreamento natural. Este estudo foi conduzido na região oeste do Estado do Paraná, no período de janeiro a fevereiro de 2007. O delineamento experimental foi o inteiramente casualizado, com três tratamentos constituídos de árvores formando pequenos bosques, árvores isoladas e condição não sombreada. A cada um desses tratamentos foi submetido um grupo de dez animais da raça Nelore (repetições). Os valores diários de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bioclimatologia; Conforto térmico; Gado de corte.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400001

BED TEMPERATURE IN COMPOST BARNS TURNED WITH ROTARY HOE AND OFFSET DISC HARROW
Provedor de dados: 70
Autores: Mota,Vania C.; Andrade,Ednilton T. de; Leite,Daniel F.
ABSTRACT The success of confinement for dairy cattle in the compost barn model depends mainly on the management of the bed and consists of its turning. This paper characterises the spatial variability of the bed temperature in the compost barn confinement model, as well as verifying whether there was an effect on efficiency from turning the bed with different agricultural implements. The experiment was conducted during the summer and winter of 2016, with 8 days of collection in each period. Data were analysed with descriptive statistics methods and geostatistical modelling with semivariograms and kriging maps. The results of the t-test at a5% significance level indicated that, after turning the bed with the plough or rotary hoe, the temperature values were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aeration/oxygenation of the bed; Dairy cattle; Confinement; Agricultural implements; Spatial variability.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300280

Freqüência da fertirrigação da bananeira prata-anã com nitrogênio e potássio aplicados por microaspersão
Provedor de dados: 70
Autores: Guerra,Amilton G.; Zanini,José R.; Natale,William; Pavani,Luiz C.
O experimento teve por objetivo avaliar a freqüência de fertirrigações com nitrogênio e potássio aplicadas por microaspersão na cultura da bananeira (Musa sp. AAB), cultivar Prata-Anã, durante dois ciclos de cultivo. O experimento foi conduzido na Área Demonstrativa e Experimental de Irrigação do Departamento de Engenharia Rural da FCAV/UNESP, Jaboticabal - SP. Utilizou-se do delineamento em blocos ao acaso, com parcelas subdivididas e cinco repetições, constituídas por quatro modalidades de aplicação de fertilizantes (adubação via solo, fertirrigação mensal, fertirrigação bimestral e fertirrigação trimestral) e duas doses de nitrogênio e potássio, correspondendo a 100% (dose 1) e 50% (dose 2) da dose recomendada de nutrientes. A fertirrigação mensal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Banana; Musa sp; Irrigação.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100010

Bimodal pore distribution on soils under conservation management system for coffee crop
Provedor de dados: 70
Autores: Carducci,Carla E.; Oliveira,Geraldo C. de; Zeviani,Walmes M.; Lima,Vico M. P.; Serafim,Milson E.
This study aims at detailing bimodal pore distribution by means of water retention curve in an oxidic-gibbsitic Latosol and in a kaolinitic cambisol Latossol under conservation management system of coffee crop. Samples were collected at depths of 20; 40; 80; 120 and 160 cm on coffee trees rows and between rows under oxidic-gibbsitic Latosol (LVd) and kaolinitic cambisol Latossol (LVAd). Water retention curve was determined at matrix potentials (Ψm) -1; -2; -4; -6; -10 kPa obtained from the suction unit; the Ψm of -33; -100; -500; -1,500 kPa were obtained by the Richards extractor, and WP4-T psychrometer was used to determine Ψm -1,500 to -300,000 kPa. The water retention data were adjusted to the double van Genuchten model by nonlinear model procedures of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Psychrometer; Mathematical modeling; Cerrado soils.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200008

Caracterização das instalações avícolas na Mesorregião do Agreste Paraibano
Provedor de dados: 70
Autores: Furtado,Dermeval A.; Tinoco,Ilda F. F.; Nascimento,José W. B. do; Leal,Antonio F.; Azevedo,Marluce A.
Nos últimos anos, as instalações destinadas à produção avícola no Brasil têm-se destacado pelo aumento da densidade de criação que visa a otimizar mão-de-obra, equipamentos, transporte, assistência técnica e, sobretudo, instalações. O objetivo deste trabalho foi realizar pesquisa sobre as principais características tipológicas dos aviários existentes na mesorregião do Agreste do Estado da Paraíba. Observou-se que os aviários são predominantemente concebidos em pequenas dimensões de largura e comprimento, com baixa densidade de alojamento. A grande maioria dos galpões está localizada na direção leste-oeste, com pequena distância entre os aviários, apresentando piso de concreto, cobertura em formato de duas águas, estrutura do telhado em madeira, telhas de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aviários; Bioclimatologia; Construções rurais.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300030

WATER AVAILABILITY AND POTASSIUM DOSES IN CHERRY TOMATO QUALITY
Provedor de dados: 70
Autores: Silva,Tonny J. A. da; Pacheco,Adriano B.; Bonfim-Silva,Edna M.; Duarte,Thiago F.
ABSTRACT The quality of cherry tomato fruits is directly related to the management strategies used in the production system, such as irrigation and fertilization. This study aimed to assess the quality of cherry tomato fruits cultivated under water availability and potassium fertilization. The experiment was carried out in a greenhouse in pots of 12 dm3 of an Oxisol. The experimental design was a randomized block design in a 52 fractional factorial arrangement with five water availabilities in the soil (4, 14, 24, 34, and 44 -kPa), five potassium doses (0, 125, 250, 375, and 500 mg dm−3) and with four blocks. Irrigation was performed with a semi-automated drip irrigation system with soil moisture monitoring by the Diviner 2000® capacitance probe. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil water; Diviner 2000; Lycopersicon esculentum; Mill.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500657

EFFECT OF THERMAL STIMULATION IN EMBRYOS FROM COBB®GENETIC STRAIN UNDER COMMERCIAL SCALE
Provedor de dados: 70
Autores: Flores,Fernanda; Nääs,Irenilza De A.; Garcia,Rodrigo G.
ABSTRACT Studies aimed at producing stronger birds and with better growth performance are being developed involving artificial incubation. To that extent, thermal stimulation by the heat of 1.39 ºC and 1ºC above the standard, and by cold of 36 ºC fixed, were applied in the last week of the embryonic development (day 14 to day 18) to Cobb® strain birds of 33 to 53 weeks age. With the purpose of evaluating the behavior of the embryos facing these temperature stimuli to identify what is the best amplitude, frequency and the most appropriate period to perform temperature variation, obtaining more adapted birds to the field. It has been observed that heat or cold stimulation did not cause embryo mortality and did not affect the hatching and the quality of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hatchability; Incubation; Chick quality; Thermal variation.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200236

VIABILITY OF THE USE OF MINIMUM WATER QUALITY INDICES: A COMPARISON OF METHODS
Provedor de dados: 70
Autores: Oliveira,Amanda R. M. de; Borges,Alisson C.; Matos,Antonio T.; Nascimento,Moysés.
ABSTRACT The achievement of all the water quality parameters that constitute the water quality indices can be a hamper to their use. The objective of this study was to analyze the viability of using minimum indices to monitor water quality, comparing different methods. For this purpose, the Environmental Company of the State of São Paulo database for the year 2016 of the Tietê/Jacaré and the Tietê/Batalha units was used. Four indices present in the literature were compared with the indices currently practiced in the states of São Paulo and Minas Gerais (“standard indices”). For feasibility analysis, the indices were classified by the “standard indices” methods and compared to them. The minimum indices were significantly correlated with the “standard...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water quality index; Bascarán index; Water quality monitoring parameters.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400616

Influência do manejo da irrigação no meloeiro rendilhado cultivado em ambiente protegido
Provedor de dados: 70
Autores: Silva,Tonny J. A.; Machado,Carmello C.; Bonfim-Silva,Edna M.; Coelho,Rubens D.
Visando a avaliar a cultura do melão rendilhado em função do manejo da irrigação, foi realizado um experimento em casa de vegetação com a cultivar Bônus nº 2, na área experimental do Departamento de Engenharia Rural da Escola Superior de Agricultura "Luiz de Queiroz" - ESALQ/USP. Foram avaliados dois sistemas de manejo (tensiômetro e lisímetro de tensão controlada), e dois níveis de fertilidade (presença e ausência de fertilizantes). O lisímetro de tensão controlada é um dispositivo que utiliza cápsula porosa, capaz de fornecer água automaticamente, acoplado a um tubo de Mariotte, que permite realizar leituras de volume de água consumido pela planta. Para os tratamentos com lisímetro de tensão controlada, a porosidade livre de água média (PLA) foi de 15%;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lisímetro; Cápsula porosa; Mariotte.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300018

HYDRAULIC CONDUCTIVITY VARIABILITY IN HORIZONTAL SUBSURFACE FLOW CONSTRUCTED WETLANDS
Provedor de dados: 70
Autores: Baptestini,Gheila C. F.; Matos,Antonio T.; Martinez,Mauro A.; Borges,Alisson C.; Matos,Mateus P.
ABSTRACT Many modifications in hydrodynamic conditions occur inside the bed of a horizontal subsurface flow constructed wetland (HSSF–CW) in operation. Studies on hydraulic conductivity measurement techniques in HSSF–CW are imperative since the monitoring of flow conditions is essential for understanding and controlling its clogging. This study aimed to assess the hydrodynamic behavior in HSSF–CW by means of saturated hydraulic conductivity (Ks) analysis. For this, six HSSF–CW were used: two non-cultivated (control), two cultivated with Tifton 85 (Cynodon spp.), and two cultivated with alligator weed (Alternanthera philoxeroides). Application of swine wastewater (SW) in HSSF–CW started on June 15, 2011, with Ks measurement period between September 9 and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydrodynamic conditions; Clogging; Constructed wetlands; Wastewater treatment.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200333

Estimation of the potential evapotranspiration by a simplified penman method
Provedor de dados: 70
Autores: Villa Nova,Nilson A.; Miranda,Jarbas H. de; Pereira,André B.; Silva,Késia O. da.
The numerous methods for calculating the potential or reference evapotranspiration (ETo or ETP) almost always do for a 24-hour period, including values of climatic parameters throughout the nocturnal period (daily averages). These results have a nil effect on transpiration, constituting the main evaporative demand process in cases of localized irrigation. The aim of the current manuscript was to come up with a model rather simplified for the calculation of diurnal daily ETo. It deals with an alternative approach based on the theoretical background of the Penman method without having to consider values of aerodynamic conductance of latent and sensible heat fluxes, as well as data of wind speed and relative humidity of the air. The comparison between the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Crop water use; Bowen ratio; Energy balance.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300007

Swine manure post-treatment technologies for pathogenic organism inactivation
Provedor de dados: 70
Autores: Bilotta,Patrícia; Kunz,Airton.
Swine manure agricultural use is a common practice in Brazil. Their physic-chemical characteristics favor its use as biofertilizer, but the presence of pathogens may become a risk to human health. This research presents a qualitative study of the main alternatives of pig manure disinfection, analyzing efficiency, advantages and limitations of each procedure. The disinfection studies reported in literature are based on the following treatments: alkaline, thermal, biological, chemical, and physical. The greater efficiencies are in thermal treatment (&gt; 4 log: 60 °C), chemical treatment (3 to 4 log: 30mg Cl- L-1; 3 to 4 log: 40 mg O3 L-1) and physical treatment (3 a 4 log: 220 mJ UV radiation cm-2). The biological treatment (anaerobiosis) also promotes the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chemical treatment; Physical treatment; Effluent reuse; Biosecurity.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200020

Avaliação de áreas potenciais ao cultivo de biomassa para produção de energia e uma contribuição de sensoriamento remoto e sistemas de informações geográficas
Provedor de dados: 70
Autores: Miura,Adalberto K.; Formaggio,Antonio R.; Shimabukuro,Yosio E.; Anjos,Sergio D. dos; Luiz,Alfredo J. B.
A humanidade sempre utilizou a biomassa para fins energéticos, porém com o aumento da demanda, ameaças à segurança energética e os danos para o ambiente e para a saúde decorrentes da utilização dos combustíveis fósseis, a importância desta fonte renovável vem sendo resgatada. Neste cenário, o planejamento agroenergético passa a ser de grande importância para países tropicais como o Brasil, pois permite viabilizar a produção de biomassa para energia onde esta é requerida, de forma sustentável, sem deixar de considerar os aspectos sociais e ambientais. Desta forma, o presente artigo tem por objetivo apresentar importantes questões relacionadas ao planejamento energético regional, como forma de contribuir para soluções e políticas públicas relacionadas à...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agroenergia; Biocombustíveis; SIG; Sensoriamento remoto; Modelagem dinâmico-espacial; Modelo conceitual.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300020

Annual evolution of global, direct and diffuse radiation and fractions in tilted surfaces
Provedor de dados: 70
Autores: Souza,Adilson P. de; Escobedo,João F.; Dal Pai,Alexandre; Gomes,Eduardo N.
It was evaluated the annual evolution of global, direct and diffuse components of incident solar radiation on tilted surfaces to 12.85, 22.85 and 32.85º, facing north, in Botucatu, state of São Paulo, Brazil. The radiometric fractions were obtained for each component of the radiation in the aforementioned surfaces, through the ratio with the global and top of the atmosphere radiations. Seasonality was evaluated based on monthly averages of daily values. The measures occurred between 04/1998 and 07/2001 at 22.85º; 08/2001 and 02/2003 at 12.85º; and from 03/2003 to 12/2007 at 32.85º, with concomitant measures in the horizontal surface (reference). The levels of global and direct radiation on tilted surfaces were lower in summer and higher in the equinoxes...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solar energy; Clearness index; Atmospheric transmissivity; Climatic conditions.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200005

PERFORMANCE OF TIFTON 85 GRASS UNDER FERTIRRIGATION WITH SLAUGHTERHOUSE WASTEWATER
Provedor de dados: 70
Autores: Oliveira,Jacineumo F. de; Rodrigues,Fernando N.; Fia,Ronaldo; Vilela,Hévelyn S.; Mafra,Dayana C. B.
ABSTRACT: The aim of this study was to evaluate the performance of Tifton 85 grass cultivated in soil columns and fertilized with different wastewater doses of swine slaughterhouse. The experiment was conducted in the Environmental Engineering Center and Sanitary of UFLA/MG in PVC columns filled with Dark Red Latosol (Oxisol) and randomly distributed. The treatments applied with nitrogen based load (300 kg ha de N years−1) consisted of four doses of SW and AQT0 control at random. Three cuts were performed, at 60, 90 and 120 days after planting. The highest yields were 10.06, 16.82 and 20.39 t ha−1 in AQT0, AAT4 and AAT3 treatments, respectively. With the increase of nutrients by N rates and root development of Tifton 85 grass, we observed higher...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Productivity; Forage; Nutrients; Disposal; Agroindustrial wastewaters.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400790

Oxisol resistence to penetration in no-till system after sowing
Provedor de dados: 70
Autores: Ros,Vinicius de V; Souza,Cristiano M. A. de; Vitorino,Antonio C. T; Rafull,Leidy Z. L.
If inappropriately conducted, management and sowing practices may compromise the environment and the profitability of the agricultural activity. The aim of this study was to analyze the furrow opener mechanisms action and the level of load applied to soil firming mechanism in no-till, on the Oxisol resistance to penetration during soybean sowing, under three soil moistures. The experiment was arranged in split-split plot design, in which the plots were composed by three soil moistures (23.8; 25.5 and 27.5% b.s.), two furrow opener mechanisms sub-plots (double disks and furrow plough) and the split-split plot of three levels of load applied to soil firming mechanism (12.2; 18.5 and 24.1 kPa), according to randomized blocks design, with three replications....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Furrow opener mechanism; Soil firming mechanism; Soil compaction.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600008

Identificação de ilhas de calor na área urbana de Ilha Solteira - SP através da utilização de geotecnologias
Provedor de dados: 70
Autores: Costa,Douglas F. da; Silva,Hélio R.; Peres,Leonardo de F.
Com a mudança climática prevista para as próximas décadas, os cientistas indicam que uma das consequências será o aumento das temperaturas médias e também o número de dias quentes, o que intensificará o desconforto térmico na população. Assim, esta pesquisa teve por objetivo principal identificar as variações térmicas localizadas na área urbana do município de Ilha Solteira - SP. A metodologia consistiu na aplicação de um algoritmo, utilizando o módulo LEGAL do sistema de informação geográfica SPRING 4.3, que realizou a transformação dos níveis de cinza gerados pelo TM/Landsat-5 em valores de temperatura de superfície. Os resultados mostraram temperaturas de superfície entre 21 ºC e 23 ºC nas áreas que apresentaram maior quantidade de vegetação, como, por...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensoriamento remoto; Landsat-5; Infravermelho termal; Correção atmosférica; Desconforto térmico.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500019

Evolução do uso da terra entre 1996 e 1999 no município de Botucatu-SP
Provedor de dados: 70
Autores: Campos,Sérgio; Silva,Marilda; Piroli,Edson L.; Cardoso,Lincoln G.; Barros,Zacarias X.
Este trabalho teve o objetivo de avaliar a evolução do uso da terra no município de Botucatu - SP, no período de três anos, considerando-se seis tipos de cobertura vegetal (cana-de-açúcar, reflorestamento, floresta nativa, pastagem, cítrus e outros), tendo como base as imagens de satélite Landsat 5, bandas 3; 4 e 5, órbita 220, ponto 76, quadrante A, passagem de 8 de junho de 1999. O Sistema de Informações Geográficas - IDRISI for Windows 3.2, foi utilizado para as análises. Os resultados mostraram que esse programa foi eficiente para auxiliar na identificação e mapeamento das áreas com uso da terra, facilitando o processamento dos dados. As imagens de satélite TM/LANDSAT 5 forneceram um excelente banco de dados para a classificação supervisionada. O...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Imagem de satélite; Geoprocessamento; Sensoriamento remoto.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100024

Demanda energética e eficiência da distribuição de sementes de milho sob variação de velocidade e condição de solo
Provedor de dados: 70
Autores: Mahl,Denise; Gamero,Carlos A.; Benez,Sérgio H.; Furlani,Carlos E. A.; Silva,Antônio R. B.
O trabalho teve o objetivo de avaliar a demanda energética e a eficiência da distribuição de sementes de uma semeadora-adubadora para semeadura direta, submetida à variação de velocidade e condições de solo, na semeadura da cultura do milho. O estudo foi desenvolvido em um Nitossolo Vermelho distrófico, na Fazenda Experimental Lageado, no município de Botucatu - SP. O delineamento experimental foi em blocos casualizados, com oito repetições, combinando-se três velocidades de deslocamento (4,4; 6,1 e 8,1 km h-1) e duas condições de solo (solo manejado sob sistema de plantio direto há cinco anos e solo preparado com escarificador há 18 meses). Avaliaram-se a força de tração, a potência na barra de tração, o consumo de combustível, a capacidade de campo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semeadura direta; Demanda energética; Distribuição de sementes.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100017

Determinação da difusividade efetiva de raiz de chicória
Provedor de dados: 70
Autores: Oliveira,Rafael A. de; Oliveira,Willian P. de; Park,Kil J.
A inulina é um frutooligossacarídeo encontrado em diversos produtos agrícolas, dentre os quais o alho, a banana, a alcachofra de Jerusalém e a raiz de chicória. A inulina é geralmente utilizada em países desenvolvidos, como substituto do açúcar e/ou gordura devido as suas características que a enquadram como alimento funcional e dietético. A raiz de chicória é utilizada como fonte e matéria-prima para a extração comercial de inulina. Os experimentos constituíram-se na secagem das raízes fatiadas em um secador convectivo com fluxo do ar perpendicular, com base em um planejamento fatorial. Pôde-se determinar a difusividade efetiva (variável dependente) para cada uma das combinações das variáveis independentes (temperatura e velocidade do ar), sendo as curvas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Inulina; Secagem; Modelo de Page.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100020

Determination of total accumulated rainfall, global radiation, evapotranspiration and degree-days originated from the ECMWF model to sugar cane crop
Provedor de dados: 70
Autores: Moraes,Rafael A.; Rocha,Jansle V.; Lamparelli,Rubens A. C.
The climate variability between the growth and harvesting of sugar cane is very important because it directly affects yield. The MODIS sensor has characteristics like spatial and temporal resolution that can be applied to monitoring of vegetative vigor variability in the land surface and then, temporal profiles generation. Agro meteorological data from ECMWF model are free and easy to access and have a good representation of reality. In this study, we used the period between sugar cane growth and harvest in the state of Sao Paulo, Brazil, from temporal profiles selecting of NDVI behavior. For each period the precipitation, evapotranspiration, global radiation, length (days) and degree-days were accumulated. The periods were presented in a map format on...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agro meteorological variable; ECMWF; MODIS; Sugar cane.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200013

Agregação de ume nitossolo vermelho distroférrico sob sistemas de plantio direto, preparo convencional e mata nativa
Provedor de dados: 70
Autores: Assis,Renato L. de; Lanças,Kléber P.
O presente estudo teve como objetivo avaliar o efeito do tempo de adoção do sistema plantio direto, comparativamente com área de mata nativa e preparo convencional, utilizando a distribuição de agregados do solo em um Nitossolo Vermelho distroférrico. Os tratamentos foram: mata nativa (MN), preparo convencional (PC), plantio direto com um ano (PD1), plantio direto com quatro anos (PD4), plantio direto com cinco anos (PD5) e plantio direto com 12 anos (PD12). Amostras de agregados foram coletadas aleatoriamente dentro de cada tratamento, nas profundidades de 0-5 e 10-15 cm. Após o peneiramento dos agregados em água, esses foram separados nas classes de agregados de &gt; 2 mm; &lt; 2 mm; 2-1 mm e &lt; 1 mm. O tempo de adoção no sistema plantio direto...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tempo de adoção; Sistemas de manejo; Diâmetro médio geométrico.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100006

ECONOMIC AND ENERGY VIABILITY OF SUNFLOWER IRRIGATED CROP
Provedor de dados: 70
Autores: Gomes,Eder P.; Sanches,Arthur C.; Azevedo,Edéria P. G. de; Geisenhoff,Luciano O.; Jordan,Rodrigo A.
Abstract This study was carried out with the objective of assessing grain yield, economic analysis and energy balance of three sunflower genotypes with and without irrigation. The experiment was installed in the Experimental Farm of the Faculty of Agrarian Sciences of the Federal University of Grande Dourados in the 2011/2012 and 2012/2013 harvests in Dourados-MS, Brazil. The experimental design used was a random complete block design with subdivisions, with and without irrigation (plots), with three genotypes (subplots) and four replications, constituting 24 plots. There were no differences in productivity among the genotypes. The irrigation increased the operational cost of the sunflower crop production, but it did not economically obstruct the activity,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Helianthus annuus L.; Operating cost of production; Energy depreciation; Central pivot.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200180

POSITION ERRORS IN SOWING IN CURVED AND RECTILINEAR ROUTES USING AUTOPILOT
Provedor de dados: 70
Autores: Santos,Adão F. dos; Correa,Lígia N.; Gírio,Lucas A. S.; Paixão,Carla S. S.; Silva,Rouverson P. da.
ABSTRACT The use of automatic routing significantly increases the yield and quality of agricultural operations and reduces the overlap rates between the mechanized set passes during the operation. The objective of this study was to analyse the quality of peanut sowing using automatic routing in two paths, curved and rectilinear, based on the error of parallelism and execution error, through statistical process control. The maps used came from an area of peanut seed production, in the city of Luzitânia, São Paulo, Brazil. The sowing was carried out by the execution of a project elaborated in CAD software that, for its elaboration, was taken into consideration the working width of the seeder-fertilizer, as well as the spacing of the crop. The CenterPoint RTX...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Peanut; GNSS; Parallelism; RTX.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400568

DYNAMIC TRACTION OF A MECHANIZED SET BASED ON TECHNICAL AND OPERATIONAL PARAMETERS
Provedor de dados: 70
Autores: Leite,Daniel M.; Fernandes,Haroldo C.; Teixeira,Mauri M.; Cecon,Paulo R.; Furtado Júnior,Marconi R.
ABSTRACT The objective of this study was to evaluate and model the traction performance parameters of a tractor 4x2 FWD, according to the tractor speed, the internal pressure and the type of tires construction. For each type of tire construction was assembled an experiment in which we evaluated the influence of internal pressures of the front and rear tires and the speed of the mechanical assembly. It was found that the sliding of the diagonal run, presented significant effect in all variables analyzed, since the radial showed no influence of the factors evaluated. The power available in the drawbar was higher when the tractor was equipped for radial tires. The response variables, fuel consumption schedule and specific fuel consumption were more sensitive...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Harrow disc; Instrumentation; Traction performance.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300484

TECHNICAL AND ECONOMIC FEASIBILITY OF USING A VARIABLE-FREQUENCY DRIVE IN MICRO-IRRIGATION SYSTEMS
Provedor de dados: 70
Autores: Pinto,Marinaldo F.; Pereira,Diego J. de S.; Carvalho,Daniel F. de; Alves,Dinara G.; Salvador,Conan A.
ABSTRACT Irrigation is essential for the development of crops in regions with scarcity or irregular rainfall distribution, enabling high productivity. However, the use of water resources and electrical energy leads to a concern with irrigation efficiency. Pressure demand varies during the operations of irrigation systems and the appropriate pressure can be regulated by variable-frequency drives for the power supply of the motor-pump set. This study aimed to analyze the technical and economic feasibility of using a variable-frequency drive to adjust the pressure in subunits of micro-irrigation systems. Laboratory tests were carried out to determine the electrical power consumed in each irrigated subunit for different slopes and the application or not of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pumping system; Energy efficiency; Economic analysis.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100112

FUZZY MODELING OF THE EFFECTS OF IRRIGATION AND WATER SALINITY IN HARVEST POINT OF TOMATO CROP. PART II: APPLICATION AND INTERPRETATION
Provedor de dados: 70
Autores: Viais Neto,Daniel dos S.; Cremasco,Camila P.; Bordin,Deyver; Putti,Fernando F.; Silva Junior,Josué F.; Gabriel Filho,Luís R. A.
ABSTRACT Tomato, the most popular greenery, is characterized by being a demanding crop in water and when in prolonged and severe drought, has limitations in its growth and reduction in productivity. In addition, this vegetable is affected by excess salinity in the water, which causes leaf wilting, apex and leaf edges burn until their death. Such effects generally are studied using statistical analysis, but there are mathematical theories that allow finer adjustments, highlighting among them, the fuzzy logic. The objective of this study was to evaluate the effects on the growth and yield of hybrid tomato from different water tensions in the soil and different salinity doses in the irrigation at 120 days after sowing using fuzzy modeling. It was used data...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuzzy logic; Hydro potential; Drought; Salt stress.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300305

Tamanho de gotas de pontas de pulverização em diferentes condições operacionais por meio da técnica de difração do raio laser
Provedor de dados: 70
Autores: Bueno,Mariana R.; Cunha,João P. A. R. da; Roman,Rodrigo A. A.
O presente trabalho objetivou avaliar o espectro de gotas de pontas de pulverização hidráulicas, submetidas a diferentes pressões e composições de calda, por meio de um analisador de partículas a laser. Em delineamento inteiramente casualizado, avaliaram-se duas pontas de jato plano duplo com indução de ar (AD-IA/D 11002 e AD-IA/D 11004) e duas pontas de jato cônico vazio (MAG - 2 e MAG - 4), em esquema fatorial 3 x 2: três pressões de pulverização (207, 276 e 345 kPa para as pontas de jato plano duplo e 414; 483 e 552 kPa para as pontas de jato cônico); e duas composições de calda (água e água mais o adjuvante fosfatidilcoline + ácido propiônico). A adição do adjuvante reduziu o diâmetro da mediana volumétrica das gotas pulverizadas pelas pontas AD-IA/D...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Espectro de gotas; Tecnologia de aplicação; Adjuvante.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500009

Influence of different systems of minimum ventilation on air quality in broiler houses
Provedor de dados: 70
Autores: Menegali,Irene; Tinôco,Ilda F. F.; Zolnier,Sérgio; Carvalho,Cinara da C. S.; Guimarães,Maria C. de C.
To maintain a competitive development of the Brazilian aviculture, some measures must be taken to enable the identification and reduction of risks to the health of birds, as well as for the physical environment. Therefore, the aim of this study was to evaluate the effectiveness of three different systems of minimum ventilation (positive pressure - SVMP, negative pressure - SVMN and natural ventilation - SVMNat) in the air quality during the first 21 days of life of broiler chicks, during winter. Three points were selected along the length to verify ammonia, carbon monoxide and oxygen concentrations at 3a.m., 9a.m., 3p.m. and 9p.m., by the respiration level of birds and workers. The averages of pollutant gases did not exceed the tolerance levels for the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aviculture; Broiler chicks; Gas concentration; Air renovation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600003

INFLUENCE OF THE PLOTS FORMAT ON THE PERFORMANCE INDEX OF THE SOYBEAN COMBINE HARVESTER
Provedor de dados: 70
Autores: Paixão,Carla S. S.; Voltarelli,Murilo A.; Silva,Rouverson P. Da; Tavares,Tiago De O.; Gírio,Lucas A. Da S.
ABSTRACT: The intensive mechanization during the harvest operation and success of this operation depends on several factors, one of which is the length and format of the plots. The aim of this study was to evaluate the operating performance of a soybean harvester in different geometric plots shape, using as quality indicators performance parameters by means of statistical control tools of process. The experiment was conducted in March 2014 in the city of Uberaba - MG. Operational capacity was evaluated in the mechanical harvesting of soybeans in three plots: irregular, rectangular and trapezoidal. Performance evaluations of soybean harvester were made from the following parameters: displacement speed, engine rotation, cylinder rotation and concave opening....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Control charts; Grain harvester; Quality control; Glycine max (L.) Merrill.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000500961

Rigidez do papelão ondulado: comparação entre resultados experimentais e os obtidos por cálculo analítico
Provedor de dados: 70
Autores: Magalhães,Paulo G.; Figueiredo,Paulo R. de A.; Dedini,Franco G.
Embalagens de papelão ondulado para produtos hortícolas têm como função principal a proteção do produto. O dimensionamento de uma embalagem de papelão requer o conhecimento da rigidez à flexão, que depende dos módulos de elasticidade dos elementos que o constituem. Este trabalho teve por objetivo calcular, a partir da caracterização física do papelão em laboratório, o módulo de elasticidade por diferentes métodos, comparando os resultados com os valores obtidos experimentalmente. Dez corpos de prova de cada um dos papéis selecionados para este estudo foram testados na direção de fabricação e na direção transversal. A resistência à tração dos papéis, capa e miolo, utilizada para calcular a rigidez, foi determinada em máquina universal de ensaios. Para a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Embalagem; Módulo de elasticidade; Rigidez à flexão.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100021

OPERATIONAL AND ENERGY PERFORMANCE OF 250 kW DOUBLE WHEELED VERSUS RUBBER HALF-TRACKED TRACTORS IN THE SOYBEAN SOWING
Provedor de dados: 70
Autores: Neto,Lauro S.; Kmiecik,Leonardo L.; Jasper,Samir P.; Zimmermann,Gabriel G.; Savi,Daniel.
ABSTRACT The technological innovation in agriculture seeks to improve the performance of mechanized assemblies and, currently, rubber half-tracks are a valuable solution for agricultural tractors, combining traction performance and less soil compaction. The objective of the experiment was to evaluate the operational and energy performance of double wheeled versus rubber half-tracked agricultural tractors in the soybean sowing. The experiment was conducted in a strip-plot design with a double factorial arrangement (2×3). The first factor consisted of a tractor with double wheels on the front and rear axles versus a tractor with single wheels on the front axle and rubber half-tracks on the rear axle, while the second factor consisted of three different...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Slippage; Operating speed; Hourly fuel consumption.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500617

Diagnóstico da mecanização em uma região produtora de grãos
Provedor de dados: 70
Autores: Gimenez,Leandro M.; Milan,Marcos.
As máquinas agrícolas, depois da terra, representam o maior investimento para o agricultor, e sua adequação ao tamanho da propriedade é um fator fundamental na redução dos custos. Há, entretanto, no País, carência de informações que permitam a análise e a comparação sobre a eficiência do uso desses equipamentos. Com isso, o objetivo deste trabalho foi avaliar o estado da arte e realizar diagnóstico quanto à posse e uso de sistemas mecanizados em propriedades agrícolas. Para tanto, elaborou-se um questionário que foi aplicado a 139 propriedades de diferentes tamanhos na região dos Campos Gerais, Estado do Paraná, e na região sul do Estado de São Paulo. Essas propriedades foram divididas em estratos de 100-300 ha, 300-600 ha, 600-900 ha e acima de 900 ha. Os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanização agrícola; Tratores; Indicadores.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100015

Influence of the sample area in the variability of losses in the mechanical harvesting of soybeans
Provedor de dados: 70
Autores: Loureiro Júnior,Antônio M.; Silva,Rouverson P. da; Cassia,Marcelo T.; Compagnon,Ariel M.; Voltarelli,Murilo A.
The mechanical harvesting is an important stage in the production process of soybeans and, in this process; the loss of a significant number of grains is common. Despite the existence of mechanisms to monitor these losses, it is still essential to use sampling methods to quantify them. Assuming that the size of the sample area affects the reliability and variability between samples in quantifying losses, this paper aimed to analyze the variability and feasibility of using different sizes of sample area (1, 2 and 3 m²) in quantifying losses in the mechanical harvesting of soybeans. Were sampled 36 sites and the cutting losses, losses by other mechanisms of the combine and total losses were evaluated, as well as the water content in seeds, straw distribution...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Statistical Control Process; Control Charts; Combine.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100009

SPECTRUM AND VELOCITY OF DROPLETS OF SPRAY NOZZLES WITH AND WITHOUT AIR INDUCTION
Provedor de dados: 70
Autores: França,Jorge A. L.; Cunha,João P. A. R. da; Antuniassi,Ulisses R.
ABSTRACT The aim of this study was to evaluate the spectrum and the velocity of droplets produced by nozzles with and without air induction, under different pressures and flow rates. The experiment was conducted in a completely randomized design with five replications, in a factorial 2 x 3 x 3 (two spray nozzles, three flow rates and three operating pressures). The spray nozzles with and without air induction of the Hypro manufacturer (GA and VP) were evaluated, with nominal flow rates of 0.76; 1.14 and 1.51 L min-1 and pressures of 200, 300 and 400 kPa. The spectrum and velocity of the droplets were determined directly, using a Visisize Portable P15 (Oxford Lasers, Imaging Division). The pressure increases further reduction of the VMD and the relative...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spray drift; Droplet size; Application technology of pesticides.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200232

PRODUCTIVITY OF CORN HYBRIDS IN RELATION TO SOWING OVERLAP
Provedor de dados: 70
Autores: Farias,Marcelo S. de; Dagios,Ravel F.; Santi,Antônio L.; Cherubin,Maurício R.
ABSTRACT The automatic control of section shut-off in seed drills minimizes seeding overlap and can reduce productivity losses, especially in responsive crops such as corn. In that context, this study evaluated the effect of sowing overlap on the grain yield and productivity of three corn hybrids. A DB-50 precision seed drill, with 33 rows equipped with a 16-row automatic section control, was used in this experiment. A randomized block design was applied to test three corn hybrids under two sowing conditions (without sowing overlap - WOSO; and with sowing overlap - WSO), with four replications. The analyzed variables were the number of plants per hectare, the number of cobs per hectare, cob length, the number of grains per cob, the thousand grain weight,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays; Precision agriculture; Section control; Plant population.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400489

MULTIVARIATE ANALYSIS OF CHEMICAL AND PHYSICAL ATTRIBUTES OF QUARTZIPSAMMENTS UNDER DIFFERENT AGRICULTURAL USES
Provedor de dados: 70
Autores: Arcoverde,Sálvio N. S.; Cortez,Jorge W.; Olszevski,Nelci; Salviano,Alessandra M.; Giongo,Vanderlise.
ABSTRACT The inadequate agricultural management in the semiarid region of northeastern Brazil, associated with the fragility of most soils, has caused degradation of the quality of this resource. This study aimed to evaluate the quality of Quartzipsamments under different uses through the multivariate analysis of chemical and physical attributes. Five areas were selected: four of them with agricultural use (onion, banana, cassava, and corn) and the other with Caatinga. Soil samples were collected at depths of 0.00–0.10, 0.10–0.20, and 0.20–0.40 m for chemical and physical analyses. The data were submitted to descriptive analysis and then to the multivariate analysis using the principal component analysis (PCA) technique and Ward’s clustering method. PCA...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Principal component; Quality indicator; Soil quality; Sandy soils.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400457

ECONOMIC MANAGEMENT MODEL OF ELECTRICITY GENERATED FROM BIOMASS IN A PIG FARM
Provedor de dados: 70
Autores: Diel,Patrícia Bellé; Casarin,Vanusa A.; Stracke,Marcelo P.; Silva,Deoclécio J. C. da; Santos,Antonio V. Dos; Przyczynski,Renato.
ABSTRACT Faced with the increasing demand for renewable energy, researchers have developed several ways to generate them, such as biogas. Thus, the present study aims to demonstrate the economic viability of electricity generation from biodigesters in a pig farm to contribute to sustainable development by reducing pollution in the environment. Studies focused on biomass derived from pig waste are still scarce. Moreover, one of the motivations of the present study is the fact that Brazil is a major producer and exporter of pig meat, with most of the production taking place in the south and southeast regions. The methodology used is defined as exploratory, descriptive, explanatory, and applied. The scientific procedures were documentary and bibliographic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biodigesters; Renewable energies; Pig farming; Economic management model.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200132

STATISTICAL PROCESS CONTROL IN THE ASSESSMENT OF DRIP IRRIGATION USING WASTEWATER
Provedor de dados: 70
Autores: Acuña Chinchilla,Sisgo R.; Silva,Ênio F. de F. e; Almeida,Ceres D. G. C. de; Silva,Alexsandro O. da; Santos,Patrício R. dos.
ABSTRACT The aim of this study was to evaluate drip irrigation as a process, by monitoring the average flow applied by the emitter using tools of statistical quality control. Four kinds of drippers were selected, two inline labyrinth type and two online where one of the inline emitters was not self-compensating and the other, self-compensating emitter. The system was installed in the field and tested for 85 hours, using three kinds of treated domestic sewage effluents and tap water. The system was under statistical control when the emitters were new, however none of the drippers reaches the manufacturer's specification for average flow. The online drippers showed more dispersion for individual flow measurements and the non-self-compensating inline dripper...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Domestic sewage effluent; Reuse; Emitters; Localized irrigation.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100047

PHYTOREMEDIATION OF FLUORIDE-CONTAMINATED WATER BY Landoltia punctata
Provedor de dados: 70
Autores: Braga,Amanda F.; Borges,Alisson C.; Vaz,Lucas R. L.; Souza,Tamara D. de; Rosa,André P.
ABSTRACT Fluorine is released into the water environment naturally or by anthropogenic activities. Fluorine promotes health benefits at low concentrations, but it promotes adverse effects ranging from fluorosis to carcinogenic problems at high concentrations. Although fluorine removal from environment can occur through processes such as adsorption, reverse osmosis, and electrodialysis, the phytoremediation emerges as an accessible and environmentally friendly treatment. This research aimed to study the phytoremediation potential of Landoltia punctata for treating water contaminated with fluorine ion (fluoride). The central composite rotatable design was used to assess the effect of three variables in the process: pH ranging from 5 to 9; phosphate...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Duckweed; Fluoride; Central composite design; Phytoextraction.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200171

APPLICATION OF OPTICAL METHOD IN MEASURING MECHANICAL VIBRATIONS IN A CANTILEVER BEAM
Provedor de dados: 70
Autores: Silva,Marcos V. G. da; Fabbro,Inácio M. Dal; Lino,Antônio C. L.
ABSTRACT The pertinent literature discloses a family of optical profile measuring techniques highlighting the moiré methods. The Moiré technique is based on the interference of two superimposed optical grids which produce fringe patterns which can be processed to analyze the DYNAMIC MEASUREMENT IN MATERIALS mechanical behavior. The goal of this research is to experimentally determine the mechanical displacement of a slim cantilever beam by means of Moiré technique with Phase Shift. Photomechanical experimental arrangement included a digital camera, a multimedia projector and a PC. The occurrence of oscillations has been adequately analyzed. The results showed data from which useful information can withdraw, being of great importance to support agricultural...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Moiré Technique; Material Mechanical Behavior Analysis; Deformation; Strain; Agricultural Machinery.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100084

Modelo de programação quadrática para análise da movimentação logística e comercialização da soja brasileira
Provedor de dados: 70
Autores: Ojima,Andréa L. R. O.; Yamakami,Akebo.
A proposta deste trabalho é analisar a distribuição logística da soja brasileira aplicando-se modelo de equilíbrio espacial de programação quadrática. O sistema de transporte da soja é um ponto importante na cadeia produtiva, pois a maior parte dos custos dessa commodity é dada pelos custos de transporte. Nesse sentido, a otimização desse segmento é essencial para aumentar a competitividade da soja brasileira no mercado internacional. O complexo soja brasileiro tem aumentado a sua participação nas exportações dos produtos agrícolas nos últimos dez anos, mas os investimentos de outros países faz com que as exportações brasileiras não fiquem focadas apenas no crescimento da produção, mas, sim, na eficiência de toda a cadeia produtiva. Dessa maneira, com a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Transporte de soja; Logística; Programação matemática.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200025

Seleção de sementes de milho durante a simulação da semeadura com disco perfurado horizontal
Provedor de dados: 70
Autores: Jasper,Roberto; Jasper,Mônica; Garcia,Luiz C.
Teve-se o objetivo de verificar a possível seleção de sementes de milho - arredondadas e achatadas - no processo de semeadura com disco perfurado horizontal, bem como as conseqüências na distribuição longitudinal. Os registros dos dados deram-se pela avaliação visual de duas pessoas, com contador manual, no final da esteira carpetada em movimento de 1,54 m s-1, com 4,60 m de perspectiva para avaliação. Assim, um sensor registrava o número de orifícios do disco horizontal que devia passar pelo tubo condutor, e os espaçamentos falhos e múltiplos eram computados por pessoas diferentes. Os espaçamentos aceitáveis foram obtidos pela subtração dos espaçamentos falhos e múltiplos do total contabilizado. A medição do comprimento e espessura das sementes foi...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Distribuição longitudinal; Tamanho da semente.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200011

Compostos orgânicos como substratos na formação de mudas de ipê-amarelo (Tabebuia Chrysotricha (Mart. Ex. Dc.) Standl) irrigadas com água residuária
Provedor de dados: 70
Autores: Muraishi,Reginaldo I.; Galbiatti,João A.; Nobile,Fabio O. de; Barbosa,José C.
A necessidade de estudar a utilização dos resíduos de podas de árvores é de grande importância ambiental para solucionar os problemas de resíduos sólidos existentes nas áreas urbanas junto com os resíduos de lixos domésticos. O estudo destes materiais foi avaliado com o desenvolvimento de mudas de ipê-amarelo (Tabebuia Chrysotricha (Mart. Ex. Dc.) sandl) em diferentes misturas de substratos e tipos de água para irrigação. O experimento foi instalado no Departamento de Engenharia Rural da Faculdade de Ciências Agrárias e Veterinárias - UNESP, Câmpus de Jaboticabal. Foram realizados dois experimentos, avaliados juntamente com delineamento experimental em blocos casualizados, de oito substratos, duas qualidades de águas e quatro repetições, totalizando 64...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Altura de plantas; Diâmetro de caule; Qualidade da água.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600009

REACTION KINETICS OF OZONE GAS IN WHEAT FLOUR
Provedor de dados: 70
Autores: Paes,Juliana L.; Faroni,Lêda R. A.; Martins,Marcio A.; Cecon,Paulo R.; Heleno,Fernanda F.
ABSTRACT The implementation of the ozonation process in the milling industry to control insect pests and improve wheat flour qualities requires understanding the behavior of ozone during ozonation. Therefore, this study aimed to investigate the reaction kinetics of ozone gas in wheat flour. Wheat flour ozonation at concentrations of 0.54, 1.07, 1.61 and 2.14 mg L−1 was used in a prototype consisting of a cylinder and a mixing system with a helical thread. The iodometric titration method was used to quantify the ozone concentration in the air stream. The reaction kinetics were characterized by determining the saturation time and the decomposition kinetics (decay rate and half-life time). With increasing ozone concentration, less time was required to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ozonation; Saturation; Decay rate; Half-life time.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300520

YIELD RESPONSE FACTOR (KY) FOR WINTER CORN CROP IN THE REGION OF DOURADOS, MS, BRAZIL
Provedor de dados: 70
Autores: Silva,Jaqueline A. da; Rezende,Maiara K. A.; Flumignan,Danilton L.
ABSTRACT Plant yield is strongly influenced by the amount of water used by it. In this sense, yield response factor (Ky) allows evaluating the decrease in yield as a function of the evapotranspiration that occurs, which may be an important tool for harvest forecasting. Therefore, this study aimed to determine Ky for winter corn crop grown in the region of Dourados, MS, Brazil. The yield function analysis based on the water factor, which requires actual (Ya) and maximum (Ym) yield data, as well as actual (ETa) and maximum (ETm) evapotranspiration, was used to adjust Ky. Ym was assumed to be 8,820 kg ha−1, while Ya was obtained for each season from the database SIDRA from IBGE. ETm and ETa were estimated by sequential daily water balance, considering four...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Water deficit; Evapotranspiration; Zea mays.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500573

Velocidade de semeadura da soja
Provedor de dados: 70
Autores: Jasper,Roberto; Jasper,Monica; Assumpção,Paulo S. M; Rocil,Jorge; Garcia,Luiz C.
Teve-se o objetivo de estudar a influência da velocidade da semeadura na cultura da soja, com sistemas dosadores de sementes dos tipos disco alveolado horizontal e pneumático. O delineamento experimental adotado foi o em blocos ao acaso, com 05 repetições. As velocidades de semeadura foram de 4; 6; 8; 10 e 12 km h-1. As variáveis avaliadas foram: população de plantas emergidas, distribuição longitudinal e os componentes de rendimento. Aplicou-se a regressão polinomial para os sistemas de disco alveolado horizontal e pneumático, em cada variável. As regressões só foram significativas para o sistema pneumático nos espaçamentos múltiplos e aceitáveis. Os componentes de rendimento da cultura da soja não se alteraram significativamente com o incremento da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Componentes de rendimento; Disco alveolado horizontal e pneumático.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100010

PERFORMANCE OF AIR INDUCTION SPRAY NOZZLE MODELS UNDER DIFFERENT OPERATING CONDITIONS
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; França,Jorge A. L.; Alvarenga,Cleyton B. de; Alves,Guilherme S.; Antuniassi,Ulisses R.
ABSTRACT For the successful application of phytosanitary products, it is essential to understand the spraying process well. The present work aims to evaluate the spectrum and speed of the droplets produced by different spray nozzle models with air induction, working under different operating conditions. The experiment was conducted using an entirely randomized design with five repetitions in a 3 × 3 × 3 factor scheme that incorporates three nozzle models (ADIA, AIXR, and GA), three nominal flows (0.76, 1.14, and 1.51 L min−1), and three operating pressures (200, 300, and 400 kPa). The spectrum and speed of the droplets were determined directly using a real-time droplet analyzer based on high-resolution image analysis. The spray nozzle model interfered with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spray tip; Droplet spectrum; Sprayer; Application technology.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600711

Software para estimativa do custo operacional de máquinas agrícolas - MAQCONTROL
Provedor de dados: 70
Autores: Piacentini,Liane; Souza,Eduardo G. de; Uribe-Opazo,Miguel A.; Nóbrega,Lúcia H. P.; Milan,Marcos.
A seleção e a otimização de sistemas mecanizados são os principais objetivos da mecanização racional. Não é suficiente uma compra adequada do maquinário agrícola se sua utilização não for controlada em aspectos operacionais e financeiros. Neste trabalho, é descrito o desenvolvimento de software para estimativa do custo operacional de máquinas agrícolas (MAQCONTROL), utilizando o ambiente de desenvolvimento Borland Delphi e o banco de dados Firebird. Os custos operacionais foram divididos em fixos e variáveis. Nos custos fixos, foram estimadas as despesas com depreciação, juros, alojamento e seguros. Nos custos variáveis, foi dada ênfase aos custos de manutenção como: óleos lubrificantes, filtros, pneus, graxa, combustível, pequenos reparos e troca de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanização agrícola; Administração rural; Sistema de informação.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300020

FINANCIAL ANALYSIS OF THE INVESTMENT IN PRECISION AGRICULTURE TECHNIQUES ON COTTON CROP
Provedor de dados: 70
Autores: Baio,Fabio H. R.; Silva,Simone P. da; Camolese,Herivelton da S.; Neves,Danilo C.
ABSTRACT: The aim of this study was to evaluate a financial analysis by the use of precision agriculture (PA) techniques on cotton crop. The experiment was carried out in a cotton field of 91 ha and its result compared to another field with similar area, cultivated with the conventional agricultural techniques. The financial analysis was extrapolated to the total farm area of 3,500 ha. All agricultural inputs applied, during the 2013/14 cotton crop season were analyzed, as well as their costs. The use of precision agriculture techniques over the cotton crop reduces production costs in 6.6%, increases the profitability index and operating profit in 3.3% and 7.9% respectively, when compared to conventional agriculture. The fertilizer application in variable...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Economic viability; Crop cost production; Profitability.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400838

INFLUENCE OF FATIGUE ON BENDING OF Pinus caribaea WOOD
Provedor de dados: 70
Autores: Christoforo,André L.; Barbosa,Thaina Q.; Almeida,Diego H. de; Panzera,Tulio H.; Lahr,Francisco A. R.
ABSTRACT This research aimed to evaluate the effect of the number of fatigue cycles (NC, 0 – reference, 450, 4500, 45000, and 90000) for frequencies (Fr) of oscillation equal to 0.5 and 1.0 Hz on the modulus of elasticity (Em) and operating stress (σm) in the static bending of Pinus caribaea wood. Em and σm were determined taking into account three specimens (SPEC) manufactured for reference condition and another three for each of the four NC levels and each Fr level, resulting in 27 SPEC. Sixty experimental determinations were obtained, being the approximate total time of sample exposure to fatigue of 350 hours. The same specimens used to determine Em and σm for the reference condition were also used (via non-destructive tests) to obtain these properties...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fatigue; Pinus caribaea; Static bending; Analysis of variance; Regression models.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200238

Uso de fotografias aéreas coloridas 35 mm na avaliação de produtividade de grãos
Provedor de dados: 70
Autores: Araújo,João C. de; Molin,José P.; Vettorazzi,Carlos A.
Este trabalho foi realizado em duas lavouras monitoradas intensivamente como áreas- piloto de agricultura de precisão. Vários dados estão sendo obtidos como mapeamento de produtividade, levantamentos de propriedades físicas e químicas do solo, pragas, doenças e plantas invasoras, bem como fotografias aéreas coloridas no formato 35 mm. As fotografias receberam orientação por bandeiras georreferenciadas em solo com DGPS para a correção geométrica das imagens e, após selecionadas, foram digitalizadas por meio de scanner. Foram, então, analisados os coeficientes de determinação entre o valor digital das imagens e a produtividade. Os coeficientes de determinação para as duas áreas, em todos os períodos analisados, apresentaram valores baixos, não havendo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Variabilidade espacial; Sensoriamento remoto.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300021

ERRATA
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300613

SOIL ATTRIBUTES AND WHEAT PERFORMANCE IN A GEOREFERENCED SEED PRODUCTION FIELD
Provedor de dados: 70
Autores: Gadotti,Gizele I.; Corrêa,Marciabela F.; Navroski,Renan; Nadal,Ariele P.; Schuch,Luis O. B.
ABSTRACT The aim of this research was to study the linear correlations and spatial distribution between soil attributes and productivity and physiological quality of wheat seeds. Soil samples were collected at georeferenced points in an area of 41 ha with a rectangular grid of 100 × 100 m to determine soil fertility. Grain productivity, number of ears m-2, protein content, and physiological seed quality were assessed. The results were submitted to Pearson's correlation analysis, descriptive statistics, and geostatistics. Phosphorus content presented a high spatial variability, with a coefficient of variation of 97.79%. Protein content, number of ears, and SMP index presented low values of coefficient of variation, indicating their low spatial variability....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Fertility; Seed quality; Triticum aestivum L.; Spatial variability.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400624

ENERGY POTENTIAL OF BIOGAS FROM PIG FARMS IN THE STATE OF MINAS GERAIS, BRAZIL
Provedor de dados: 70
Autores: Sousa,Izabelle de P.; Rosa,André P.; Borges,Alisson C.; Renato,Natália dos S.
ABSTRACT Pig farming stands out as an alternative for decentralized electrical energy production from the use of biogas energy. However, its use is still limited. Thus, this study aimed to estimate and map the biogas production, as well as determine the electric power originated by the use of biogas produced in covered lagoon biodigester from pig farms of different sizes in the state of Minas Gerais, Brazil. The research was based on data provided by the Instituto Mineiro de Agropecuária (IMA). Three forms of electric power were estimated, as follows: (i) total, (ii) current, and (iii) installed. They were estimated from the volume of manure generated at each development stage of the animals. The total electric power corresponded to 31 MW, while the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anaerobic digestion; Covered lagoon biodigester; Energy recovery; Biogas; Pig farming.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300396

Rheological behavior of mixed drink of annona and milk
Provedor de dados: 70
Autores: Duarte,Maria E. M.; Gouveia,Deyzi S.; Mata,Mario E. R. M. C.; Queiroz,Alexandre J. de M.
In this study the rheological behavior in different temperatures (0; 6; 18 e 24 ºC) and physicochemical parameters of integral annona (Annona squamosa) pulp and the annona pulp with milk in different percentages pulp/milk (75g of annona pulp/25g of milk, 50g of annona pulp/50g of milk, 25g of annona pulp/75g of milk) have been availed, in order to verify the effect of temperature and pulp concentration in the rheological behavior of these beverages. To obtain the rheological parameters a concentric cylinder rheometer has been used and the rheograms were analyzed using the Ostwald-de-Wael (power Law) and Herschel-Bulkley models. The physicochemical parameters (sugars, pH, ash, acidity and soluble solids) were determined in order to establish correlations...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fruit; Rheology; Agro-industry; Processing.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200013

Avaliação do desempenho de um sistema automático para controle da fertirrigação do tomateiro cultivado em substrato
Provedor de dados: 70
Autores: Steidle Neto,Antonio J.; Zolnier,Sérgio; Marouelli,Waldir A.; Martinez,Herminia E. P.
Este trabalho teve por objetivo avaliar o desempenho de um sistema de controle automático de fertirrigação para a produção do tomateiro em substrato de areia, comparativamente ao sistema de controle convencional quanto à redução de solução nutritiva. No método de controle automático, os eventos de fertirrigação foram estabelecidos em função das condições meteorológicas do ambiente de cultivo e do estádio de desenvolvimento da cultura. Para isso, o modelo de Penman-Monteith foi utilizado como suporte para a tomada de decisão sobre a frequência adequada para aplicação da solução nutritiva. No sistema de controle convencional, os intervalos entre as fertirrigações permaneceram fixos durante todo o ciclo do tomateiro. Os resultados demonstraram que o sistema...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lycopersicon esculentum; Hidroponia; Solução nutritiva; Automação.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300005

Wear of rotary plows operating in a tropical clay loam soil
Provedor de dados: 70
Autores: González,Hugo; Cappelli,Nelson L.; Toro,Alejandro.
The wear resistance of rotary plows operating in a clay loam soil was studied. The degree of damage caused to the soil and the amount of mass lost by the tools were determined in order to establish correlations between the physical properties of the soil and the wear mechanisms acting on the tribosystem. Field tests were carried out in 12 plots and a randomized experimental design with 4 levels, 3 replicas per level and 2 passes per plot was applied. The levels relate to the tillage implements employed: rotary tiller, rotary power harrow, small motorized rotary tiller and control (unaltered soil). The highest mass losses were measured in rotary tiller and rotary power harrow's tools, while the small motorized rotary tiller's tools showed generally lower...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Abrasive wear; Tribosystems; Rotary plows; Agricultural tool.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400017

Entupimento de tubos gotejadores convencionais com aplicação de cloreto de potássio (branco e vermelho) via duas qualidades de água
Provedor de dados: 70
Autores: Ribeiro,Pabblo A. de A; Coelho,Rubens D; Teixeira,Marconi B.
Neste trabalho, buscou-se avaliar a suscetibilidade de modelos de tubos gotejadores ao entupimento, quando expostos ao uso de cloreto de potássio (branco e vermelho), aplicados via diferentes qualidades de água. O experimento foi realizado no Laboratório de Irrigação do Departamento de Engenharia Rural da Escola Superior de Agricultura "Luiz de Queiroz" ESALQ/USP, por um período de nove meses, analisando o desempenho de oito modelos de tubos gotejadores convencionais, com quatro tratamentos e dez repetições, sendo cada repetição representada por um gotejador. Os tratamentos aplicados foram: (T1-Lg/B) água do lago x cloreto de potássio branco; (T2-Lg/V) água do lago x cloreto de potássio vermelho; (T3-Lb/B) água do laboratório x cloreto de potássio branco,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertirrigação; Uniformidade de distribuição; Irrigação localizada.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200010

ESTIMATION OF THE CHARACTERISTIC VALUE OF WOOD STRENGTH
Provedor de dados: 70
Autores: Christoforo,André L.; Almeida,Andrea de S.; Lanini,Tamiris L. S.; Nogueira,Rodrigo de S.; Lahr,Francisco A. R.
ABSTRACT For safety reasons, wood strength values, essential for structural dimensioning, are calculated based on the characteristic value, which corresponds to the 5% percentile of a given probability distribution model. For small samples, the Brazilian normative document ABNT NBR 7190 establishes an estimator of the characteristic wood strength, which can provide a significantly different result from the characteristic value coming from a suitable model of probability distribution. The main objective of this study was to evaluate the best probability distribution model (normal, lognormal, Weibull, and exponential) and the subsequent calculation of the characteristic value indicated by ABNT NBR 7190 (1997), allowing to evaluate its accuracy, being also...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wood; Compression; Traction; Shear; Probability distribution; Characteristic value.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100127

RESPONSE FROM ANAEROBIC DIGESTION OF LAYING HEN MANURE WITH BIOCHAR ADDITION
Provedor de dados: 70
Autores: Andrade,Willian R.; Ferreira,Cecilia de F. S.; Gates,Richard S.; Borges,Alisson C.; Santos,Tânia M. B. dos.
ABSTRACT This study aimed to assess the anaerobic digestion response of laying hen manure with different inclusion levels of biochar in batch reactors as measured by physicochemical parameters, biogas production and digestate quality. Four levels of biochar inclusions (0, 2.5, 5.0 and 7.5%) were tested with 3 replicates each. Twelve two-liter anaerobic batch reactors were used for 86 days at 35°C. Substrate and digestate of each treatment were assessed for monitored parameters, biogas production and digestate quality. Increased levels (0, 2.5, 5.0 and 7.5%) of biochar were found to gradually reduce total ammonia nitrogen (1794.33, 140.84, 950.81 and 509.32 mg.L-1, respectively). Despite the positive effect of biochar to accelerate initial biogas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogas yield; Total ammonia nitrogen; Volatile solids.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300315

Produção animal e o meio ambiente: uma comparação entre potencial de emissão de metano dos dejetos e a quantidade de alimento produzido
Provedor de dados: 70
Autores: Orrico Júnior,Marco A. P.; Orrico,Ana C. A.; Lucas Júnior,Jorge de.
O objetivo do trabalho foi efetuar a comparação das principais espécies de interesse agropecuário, em relação à eficiência de conversão das dietas em produtos de origem animal (carne ou ovo), produção de resíduo e potencial de emissão de metano, a partir da fermentação dos resíduos. Para isso, foram selecionadas cinco espécies de animais durante a fase de produção: 1) suínos, do nascimento ao abate (peso vivo (PV) final de 90 kg) ; 2) bovinos, do desmame ao abate (PV: 520 kg); 3) caprinos, do desmame ao abate (PV: 30 kg); 4) aves, durante toda a fase de postura (14,7 kg de ovos); 5) frango de corte, do nascimento ao abate (PV: 3,1 kg). Para a estimativa dos parâmetros propostos, foram medidos os dados do desempenho e efetuou-se a biodigestão anaeróbia dos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Conversão alimentar; Coeficiente de resíduo; Resíduos.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200020

SPATIAL VARIABILITY MAPPING OF SUGARCANE QUALITATIVE ATTRIBUTES
Provedor de dados: 70
Autores: Ferraz,Marcos N.; Corrêdo,Lucas de P.; Wei,Marcelo C. Fu; Molin,José P.
ABSTRACT Spatial variability evaluation of qualitative attributes can be used as an excellent strategy to design forms of intervention that result in better crop profitability for some agricultural crops, for example, sugarcane. Based on the assumption that qualitative attributes of sugarcane present spatial variability and their distributions along the stems are uniform in different varieties, this study aimed to evaluate the distributions of the qualitative parameters of different sugarcane varieties and the spatial variability of these attributes in a commercial field. Samples of nine varieties were collected for laboratory quality analysis, and the Brix parameter was analyzed by a digital refractometer. The analysis of variance, the Tukey test, and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharose; Technological quality; Geostatistic.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800109

Modelo de simulação de secagem de produtos agrícolas usando entalpia do ar constante
Provedor de dados: 70
Autores: Dalpasquale,Valdecir A.; Sperandio,Décio.
A simulação matemática de secagem de produtos agrícolas teve seu auge nas décadas de 1960 e 1970, com destaque para os modelos de Thompson e de Michigan. Entretanto, nenhum deles abordou a condição de entalpia constante do ar de secagem durante o processo, limitando-se a conferir se a umidade relativa do ar não excedia 100%. Estudos conduzidos na Universidade Estadual de Maringá permitiram concluir que os balanços de energia e de massa de um processo de secagem estão incluídos no uso da mesma entalpia do ar durante a secagem, ajustando-se, com ela, a umidade absoluta do ar em função da umidade removida do produto. Com essa nova razão da mistura do ar e com a entalpia constante, avalia-se a nova temperatura do ar de secagem na saída da camada e, com essas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulação de secagem; Novo modelo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400016

Influence of stiffness in bolted connections in wooden plane structure of truss type
Provedor de dados: 70
Autores: Christoforo,André L.; Romanholo,Giuliano A.; Panzera,Túlio H.; Borges,Paulo H. R.; Lahr,Francisco A. R.
Trusses are structural systems commonly used in projects, being employed mainly in roof structures, present in most rural buildings. The design of trusses, as well as other structural systems, requires the determination of displacements, strains and stresses. However, the project is developed from an ideal model of calculation, considering free rotation between the elements of a connection. This paper presents a computer program for the analysis of bidimensional wooden trusses with connections formed with two screws per node. The formulation is based on the flexibility method, taking into account the influence of the effect of semi-rigid connections formed by two screws. An example of a structure is presented and analyzed by the program developed here,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Trusses; Semi-rigid connections; Flexibility method; Rural buildings.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500017

Efeito de sistemas de manejo na estabilidade de agregados de um Nitossolo Vermelho
Provedor de dados: 70
Autores: Lacerda,Nilda B.; Zero,Vânia M.; Barilli,Juliana; Moraes,Maria H.; Bicudo,Sílvio J.
Com o objetivo de avaliar o efeito do manejo do solo na estabilidade de agregados de um Nitossolo Vermelho distroférrico, localizado na Fazenda Experimental Lageado da FCA/UNESP, em Botucatu - SP, amostraram-se, em outubro de 2001, três sistemas de manejo de solo: (i) mata (MA), (ii) preparo convencional por 10 anos seguido de semeadura direta por 12 anos (PC/SD) e (iii) preparo convencional por 22 anos (PC), em quatro camadas: 0,0-0,10; 0,10-0,20; 0,20-0,30 e 0,30-0,40 m. O delineamento experimental empregado foi o inteiramente casualizado, com três repetições. As amostragens foram feitas após a cultura do milho (safra 2000-2001). As amostras foram submetidas às análises físicas e químicas, e as médias, comparadas pelo teste de Tukey. O diâmetro médio...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Diâmetro médio ponderado; Índice de estabilidade de agregados; Semeadura direta.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300014

Soursop seedlings: emergence and development under different cultivation environments and substrates – Part I
Provedor de dados: 70
Autores: Costa,Edílson; Sassaqui,Adriano R.; Silva,Anne K. da; Rego,Norton H.; Fina,Bruna G.
ABSTRACT Seedling quality is crucial to obtain vigorous plants in the field. This study aims to evaluate the emergence and development of soursop seedlings in different substrates in protected environments. The experiment was conducted at the Mato Grosso do Sul State University and carried out using five protected environments: greenhouse, greenhouse with thermo-reflective screen, nursery with monofilament screen, nursery with thermo-reflective screen, and nursery with palm thatch. The substrates (S) consisted of cattle manure (M), humus (H), cassava branches (C), and vermiculite (V) as in the following ratios: S1 = H + V (1:3), S2 = H + V (1:1), S3 = H + V (3:1), S4 = H + C (1:3), S5 = H + C (1:1), S6 = H + C (3:1), S7 = M + V (1:3), S8 = M + V (1:1), S9...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Annona muricata; Cattle manure; Cassava branches; Vegetable ambience.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200217

LOW COST FUZZY SYSTEM APPLIED TO THE CONTROL AND SUPERVISION OF THERMAL ENVIRONMENT IN POULTRY FARMS
Provedor de dados: 70
Autores: Alecrim,Paulo D. de; Campos,Alessandro T.; Yanagi Junior,Tadayuki; Ferreira,Jacqueline C.; Trindade,Alander A.
ABSTRACT The aim of this study was to develop an automated fuzzy controller with microcontroller, consisting of hardware and software for the control and supervision of thermal environment in broiler farms. The study has been conducted in two steps: in the first one it was performed a computer analysis through simulation. In the second step it was performed the evaluation of the software and hardware developed by the equipment test in the registration of the thermal environment variables within the facility and activation of the climate control equipment. The experiment was conducted in a poultry house with broilers of Cobb 500 lineage, aged between 1 and 28 days in an experimental farm located in Bambuí - MG. The presented prototype is able to operate in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry environment; Thermal comfort; Fuzzy controller; Ventilation system equipment for broiler houses.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100194

Variabilidade espacial de propriedades físico-hídricas de um nitossolo sob a cultura do feijoeiro irrigado
Provedor de dados: 70
Autores: Guimarães,Rachel M. L.; Gonçalves,Antônio C. A.; Tormena,Cássio A.; Folegatti,Marcos V.; Blainski,Éverton.
Devido à utilização mais intensa de água via irrigação e ao elevado custo que tem sido agregado a este recurso, é necessário que os sistemas de irrigação operem com altos níveis de eficiência. A descrição do padrão espacial de propriedades físico-hídricas do solo pode auxiliar no manejo eficiente da irrigação. Para tanto, técnicas da geoestatística são necessárias. Assim, este trabalho teve como objetivos descrever e avaliar o padrão espacial da porosidade, densidade e armazenamento de água no solo durante um ciclo de secamento, num Nitossolo Vermelho distroférrico cultivado com a cultura do feijoeiro. A área de cultivo foi subdividida em 80 quadrículas, segundo uma malha de 3 por 3 m. Em cada quadrícula, mediu-se o teor de água do solo ao longo do tempo,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Distribuição espacial; Geoestatística; Armazenamento de água no solo; Porosidade do solo; Densidade do solo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400010

STATITIONARY ENGINE PERFORMANCE USING MIXTURE OF SOYBEAN AND CASTOR BEAN BIODIESEL TO DIESEL OIL
Provedor de dados: 70
Autores: Cortez,Jorge W.; Guimarães,Camila C.; dos Santos,Vivianni M. L.
ABSTRACT The use of alternative fuels in diesel engines has been the subject of research that seeks new fuels to expand the energy matrix. The aim of this study was to evaluate the performance of the stationary engine with the use of mixtures of biodiesel from soybean and castor bean added to diesel (S500) in two proportions (25% and 40%), evaluating the torque, effective power observed and specific consumption. The five biodiesel mixtures of soybean (S) and castor bean (C) analyzed were: S100C0, S75C25, S50C50, S25C75 and S0C100, which were added to the diesel in proportions B25 and B40, totaling ten treatments, plus the control with diesel S500 (B7). The stationary engine was subjected to the rotations of 3000, 2700, 2400, 2100, 1800 and 1500 rpm. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agroenergy; Diesel engine; Biodiesel/diesel mixtures; Oleaginous; Engine rotation.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600918

Effects of water deficit in two phenological stages on production of japanese cucumber cultived in greenhouse
Provedor de dados: 70
Autores: Oliveira,Eduardo C.; Carvalho,Jacinto de A.; Silva,Wellington G. da; Rezende,Fátima C.; Almeida,Willian F. de.
The experiment was performed in the experimental area of the Engineering Department Federal University of Lavras, Minas Gerais State, Brazil. It aimed at identifying the adequate irrigation management of the greenhouse-cultivated Japanese cucumber (Cucumis sativus L.). complete randomized design, with four levels of soil water potential (15; 30; 60 e 120 kPa) at two phenological phases (vegetative and reproductive), and 5 replications. Overall, the results showed decrease of yield according to increase of soil water potentials. During the reproductive stage, Japanese cucumber plants were more sensitive to water deficit, resulting in further decrease in yield compared to applied water deficit during the vegetative stage of the culture.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cucumis sativus L.; Greenhouse; Irrigation management.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000400006

Ângulo de giro e espaçamento entre carreadores em sistemas autopropelidos de irrigação com o aspersor Plona-RL400
Provedor de dados: 70
Autores: Prado,Giuliani do; Colombo,Alberto; Biagioni,Priscila F.
Valores determinados em laboratório, de vazão, raio de alcance e do perfil radial de aplicação de água do aspersor canhão PLONA-RL400, foram utilizados em simulações digitais da uniformidade de aplicação de água desse aspersor operando, na ausência de ventos, com diferentes ângulos de giro e espaçamentos entre carreadores, em sistemas autopropelidos de irrigação. Os valores simulados de uniformidade de aplicação de água foram apresentados em três grupos distintos, cada um dos quais representando condições operacionais (bocal e pressão) que determinam a ocorrência da mesma forma geométrica (I, II ou III) do perfil radial adimensional de aplicação de água do aspersor avaliado. Para os perfis do tipo I, II e III, observou-se que espaçamentos de carreadores...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Perfil radial; Simulações digitais; Uniformidade da irrigação.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300003

COMPARISON OF METHODS FOR ESTIMATING REFERENCE EVAPOTRANSPIRATION: AN APPROACH TO THE MANAGEMENT OF WATER RESOURCES WITHIN AN EXPERIMENTAL BASIN IN THE BRAZILIAN CERRADO
Provedor de dados: 70
Autores: Gotardo,Jackeline T.; Rodrigues,Lineu N.; Gomes,Benedito M.
ABSTRACT This study aimed to compare methods for estimating reference evapotranspiration using an experimental basin in the Brazilian Cerrado, for water management purposes. For that, we estimated daily reference evapotranspiration over a certain period (time series between 1982 and 2012) through different empirical methods. These methods consisted of Blaney-Criddle (BC), Hargreaves &amp; Samani (HS), ASCE Penman-Monteith (ASCE- PM), Penman (1948/1963) (PO), Priestley-Taylor (PT), which were all compared to the standard Penman-Monteith FAO-56 (PM-FAO56). Based on statistics, ASCE- PM, P and BC methods should be recommended for cerrado areas, either in rainy or dry seasons. After these, the PT also stood out. Among the less complex methods, based on...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiration; Methods; Penman-Monteith FAO-56.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601016

Desempenho de pontas de pulverização em Brachiaria brizantha cv. MG-4 para controle de ninfas de cigarrinhas das pastagens
Provedor de dados: 70
Autores: Maciel,Cleber D. de G.; Velini,Edivaldo D.; Bernardo,Rodrigo dos S.
O trabalho teve como objetivo estudar o desempenho de pontas de pulverização na deposição da calda inseticida para o controle de ninfas de cigarrinhas das pastagens em Brachiaria brizantha cv. MG-4. Doze tratamentos foram estudados em esquema fatorial 6x2, constituídos pelo contraste de seis pontas de pulverização e pressões de 196 e 392 kPa: TF-VP2 (336 L ha-1 e 467 L ha-1); AI11002-VS (184 L ha-1 e 200 L ha-1); XR11002-VS (200 L ha-1 e 280 L ha-1); TT11002-VP (200 L ha-1 e 280 L ha-1); TJ60-11002VS (208 L ha-1 e 280 L ha-1) e TX-VK4 (72 L ha-1 e 97 L ha-1). Para monitorar a deposição das caldas de pulverização, utilizaram-se os traçadores Azul Brilhante FD&amp;C-1 (0,3% p/v) e Amarelo de Tartrasina FD&amp;C-5 (0,6% p/v). Alvos artificiais, constituídos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pontas de pulverização; Volume de calda; Deposição; Forrageira.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200010

THERMAL EFFICIENCY OF DIFFERENT COVERAGE MATERIALS IN REDUCED MODELS OF ANIMAL HUSBANDRY FACILITIES: A CASE STUDY
Provedor de dados: 70
Autores: Castro,Ariane C. de; Silva,Iran J. O. da; Nazareno,Aérica C.; Nunes,Maria L. A.; Piedade,Sônia M. de S.
ABSTRACT This study aimed to assess different combinations of coverage materials in reduced models of animal husbandry facilities based on thermal comfort indices. It was conducted in an experimental area of the Research Center in Ambience located in São Paulo State, Brazil (22°42′30″ S and 47°38′00″ W). The performance of ceramic and fiber-cement (white painted) tiles was assessed associated with two types of polypropylene commercial linings (lining A and B) installed below the roof, and a thermo-reflective screen (lining C) installed above the fiber-cement roof. Microclimatic assessment of distorted reduced-scale models was performed at 15-minute intervals by registering the air temperature, black globe temperature, relative humidity and air velocity....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambience; Thermal comfort; Tiles; Poultry facility; Linings.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300403

Soursop seedlings: biomasses and biometric relations in different farming environments and substrates – Part II
Provedor de dados: 70
Autores: Costa,Edílson; Sassaqui,Adriano R.; Silva,Anne K. da; Rego,Norton H.; Fina,Bruna G.
ABSTRACT The quality of seedling is critical to obtain vigorous plants in the field. The present study aimed to assess biomasses and biometric relations of soursop seedlings. We used different substrates in protected environments. The experiment was performed at the Universidade Estadual do Mato Grosso do Sul (UFMS) (State University of Mato Grosso do Sul). Five farming environments were developed in greenhouses: one covered with low-density polyethylene film (LDPE), another with with polyethylene and heat-reflective cloth under film under 50% shading in aluminized color, monofilament cloth under 50% shading in black, thermo-reflective cloth under 50% shading in aluminized color, and an environment covered with bacuri coconut straw. Substrates were made of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Annona muricata; Manure; Cassava branches.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200229

Determinação da difusividade e da energia de ativação para feijão macassar (Vigna unguiculata (L.) Walp.), variedade sempre-verde, com base no comportamento da secagem
Provedor de dados: 70
Autores: Silva,Wilton P. da; Mata,Mário E. R. M. C.; Silva,Cleiton D. P. S. e; Guedes,Manoel A.; Lima,Antonio G. B.
Neste artigo, teve-se o objetivo de determinar curvas de secagem em camada fina para grãos de feijão macassar, variedade sempre-verde. Visou-se, também, à determinação da difusividade efetiva da água no interior do produto, bem como a energia de ativação. Para tal, foram utilizadas amostras com 150 g de feijão com teor inicial de água de 37% (bu), nas temperaturas de 40; 50 e 60 ºC. A velocidade do ar do secador convectivo foi mantida em 1,0 m s-1 e, durante todo o processo, os valores médios da temperatura e da umidade relativa do ar ambiente foram, respectivamente, 29 ºC e 58%. A difusividade efetiva da água no produto foi determinada, em cada temperatura, por meio da lei de Fick, pressupondo um modelo esférico para os grãos. Uma expressão para a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelo de Page; Segunda lei de Fick; Teor de água; Grãos esféricos.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200013

Desenvolvimento de plantas de crisântemo cultivadas em vaso em resposta a níveis de condutividade elétrica
Provedor de dados: 70
Autores: Mota,Poliana R. D' Almeida; Bôas,Roberto L. V.; Sousa,Valdemício F. de; Ribeiro,Valdenir Q.
Na floricultura, a competição por mercados é intensa e o diferencial de produtividade consiste no manejo nutricional adequado, por promover grande impacto sobre a qualidade, a produtividade e a longevidade das inflorescências e da planta. O presente trabalho teve o objetivo de avaliar os efeitos de níveis de condutividade elétrica (CE) no desenvolvimento de plantas de crisântemo (Dendranthema grandiflora Tzvelev.) em vaso sob cultivo protegido. O experimento foi conduzido no município de Paranapanema - SP. Usou-se o delineamento experimental de blocos casualizados com quatro repetições e parcelas divididas. As parcelas foram constituídas pelas épocas de amostragem, e as subparcelas, pelos diferentes níveis de CE, determinados na solução aplicada via água...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dendranthema grandiflora; Fertirrigação; Ambiente protegido.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100010

Produtividade do feijoeiro sob diferentes uniformidades de distribuição de água na superfície e na subsuperfície do solo
Provedor de dados: 70
Autores: Frizzone,José A.; Rezende,Roberto; Gonçalves,Antonio C. A.; Helbel Júnior,Celso.
Com o objetivo de comparar a uniformidade de lâminas aplicadas, uniformidade de umidades no solo e produtividade da cultura do feijoeiro, conduziu-se um experimento utilizando a cultivar de feijão IAPAR 57. Foram feitas aplicações de água na superfície do solo, com quatro valores de uniformidades, aplicando-se a mesma lâmina, utilizando-se de quatro espaçamentos entre aspersores: 12 x 12 m; 18 x 18 m; 18 x 24 m, e 24 x 24 m. Foram feitas análises das distribuições dos dados de lâmina aplicada, de umidade do solo e de rendimento de grãos, no espaço. Para isso, foram usadas técnicas de análise exploratória que consistiram principalmente em gráficos tipo "box-plot" simplificados, nos quais são apresentados apenas os valores de mediana, máximo e mínimo das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Análise exploratória; Uniformidade; Phaseolus vulgaris.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300010

Germination and early growth of physic nut submitted to levels of salinity
Provedor de dados: 70
Autores: Lima,Luiz A.; Almeida,Willian F. de; Lima,Pedro L. T.; Oliveira,Eduardo C.; Shock,Clinton C.
Two experiments were conducted to evaluate the effect of salinity on early physic nut plant development. In the first trial, physic nut seeds were exposed to seven levels of salinity (0, 2, 4, 6, 8, 10 and 12dS m-1) with eight repetitions, using a substrate of paper soaked with solutions of CaCl2 and KCl. The treatments were evaluated based on the initial germination, total percentage of germination, and time necessary to germination of 50% of the seeds. Increased salinity reduced the first germination count and delayed the time to 50% germination. From 10dS m-1, there was a reduction in germination percentage. The second trial evaluated the effect of salinity on the growth of physic nut seeds. This trial, carried out inside a greenhouse, with a completely...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Jatropha curcas L.; Seeds; Seedlings; Greenhouse.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600004

Tratamento de esgoto sanitário em sistemas alagados construídos cultivados com lírio-amarelo
Provedor de dados: 70
Autores: Prata,Renata C. C.; Matos,Antonio T. de; Cecon,Paulo R.; Monaco,Paola A. V. Lo; Pimenta,Leonardo A.
Neste artigo, avaliou-se a eficiência de quatro sistemas alagados construídos (SACs) no tratamento de esgoto sanitário após ser submetido a tratamento preliminar e, no caso de alguns SACs, a tratamento primário (tanque séptico). Os SACs foram cultivados com lírio-amarelo (Hemerocallis flava), tendo a brita #0 como meio suporte, e submetidos às taxas de carregamento orgânico (TCO) de esgoto sanitário, em termos de DBO (kg ha-1 d-1), de 44; 98; 230 e 395 kg ha-1 d-1 e tempos de detenção hidráulica (TDH) de 3,9; 2,0; 1,0 e 0,75 dias, respectivamente. Para avaliar a eficiência dos sistemas, foram realizadas, no afluente e no efluente aos SACs, análises de DBO, DQO, SST, N-total, P-total, K e Na durante 6 meses de funcionamento do sistema. Nos SACs, houve...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas wetlands; Plantas ornamentais; Remoção de poluentes; Águas residuárias.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600007

Avaliação da biodegradabilidade anaeróbia de resíduos da bovinocultura e da suinocultura
Provedor de dados: 70
Autores: Moraes,Luciana M.; Paula Júnior,Durval R.
A biodegradabilidade de dejetos da bovinocultura e da suinocultura foi avaliada por meio de metodologia simplificada que permitiu a verificação da aplicabilidade de processos anaeróbios. Os ensaios foram realizados com reatores em batelada, com lodos granulados de três procedências: reator UASB tratando efluente de bovinocultura, reator UASB tratando efluente de suinocultura e reator UASB tratando efluente de abatedouro de aves. Os ensaios (1) - efluente de bovinocultura e lodo de abatedouro de aves não-adaptado; (2) - efluente de suinocultura e lodo de abatedouro de aves não- adaptado; (3) - efluente de bovinocultura e lodo de abatedouro de aves adaptado; (4) - efluente de suinocultura e lodo de abatedouro de aves adaptado; (5) - efluente de bovinocultura...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Processo anaeróbio; Suinocultura; Bovinocultura.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200025

Identification of commercial blocks of outstanding performance of sugarcane using data mining
Provedor de dados: 70
Autores: PELOIA,PAULO R.; RODRIGUES,LUIZ H. A.
ABSTRACT In order to achieve more efficient agricultural production systems, studies relating to the patterns of influence factors on commercial blocks of outstanding performance can be performed to assist management practices. The performance is considered to be the difference between the yield of a given block and the average yield of the homogeneous group that it belongs to. The methods available to identify these outstanding blocks are usually subjective. The aim of this study was to propose an objective and repeatable approach to identify outstanding performance blocks. The proposed approach consisted of performance determination, using regression trees, and the classification of these blocks by k-means clustering. This approach was illustrated using...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Clustering; Regression tree; Yield variability.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500895

Potencialidade do gps de navegação garmin 12 xl utilizando um sistema de baixo custo
Provedor de dados: 70
Autores: Guimarães,Gabriel do N.; Camargo,Paulo de O.
Desde o início do ano 2000, o uso de receptores de navegação aumentou consideravelmente. Muito se deve à desativação da disponibilidade seletiva ocorrida em maio de 2000. Entretanto, esses receptores não registram as observáveis, somente estimam e armazenam as coordenadas, o que impede o pós-processamento dos dados. Baseados nesse aspecto, alguns softwares foram desenvolvidos e estão disponíveis gratuitamente. Eles permitem a gravação das observáveis GPS do receptor, pseudodistâncias (código C/A) e das medidas da fase da onda da portadora. Esses programas são capazes de ler de e registrar em arquivos binários as informações referentes às observáveis GPS e realizar a conversão de formato binário para o formato RINEX. Este trabalho visa a avaliar o receptor...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geodésia; GPS de navegação; Precisão.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200011

Demanda de tração em haste sulcadora na integração lavoura-pecuária com diferentes pressões de pastejo e sua relação com o estado de compactação do solo
Provedor de dados: 70
Autores: Conte,Osmar; Levien,Renato; Trein,Carlos R.; Cepik,Carla T. C.; Debiasi,Henrique.
Conduziu-se um experimento com integração lavoura-pecuária em Latossolo Vermelho distroférrico para avaliar o esforço de tração em hastes sulcadoras de adubo utilizadas em semeadura direta, atuando em diferentes profundidades e intensidades de pastejo, bem como o efeito desse último fator sobre o estado de compactação do solo. Os tratamentos principais foram constituídos pelas alturas da pastagem de inverno (aveia + azevém): 0,10; 0,20; 0,30 e 0,40 m e sem pastejo, obtidas variando-se a carga animal, e os tratamentos secundários foram duas profundidades de atuação da haste sulcadora de adubo: 0,12 e 0,15 m. A massa seca de raízes da pastagem, na camada de 0 a 0,12 m, aumentou com o incremento na intensidade de pastejo. Analisando os valores de resistência...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semeadura direta; Semeadora-adubadora; Mecanismo sulcador.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100016

Produção de alface hidropônica em três ambientes de cultivo
Provedor de dados: 70
Autores: Costa,Edílson; Leal,Paulo A. M.
Propôs-se avaliar a produção hidropônica de alface-crespa, variedade "Vera", em bancadas inclinadas com canais de 100 mm, utilizando a técnica de filme de solução nutritiva, em resposta à aplicação de dióxido de carbono e ao resfriamento evaporativo. Realizaram-se cinco ciclos de cultivo nos períodos de 20-3 a 17-4-2000 (C1); 25-5 a 29-6-2000 (C2); 13-7 a 21-8-2000 (C3); 27-8 a 2-10-2000 (C4) e 12-12-2000 a 10-1-2001 (C5). Avaliaram-se três casas de vegetação, sendo casa de vegetação sem sistema de resfriamento evaporativo do ar e sem injeção aérea de CO2 (A1); casa de vegetação com injeção aérea de CO2 e sem sistema de resfriamento evaporativo do ar (A2), e casa de vegetação com injeção aérea de CO2 e com sistema de resfriamento evaporativo do ar do tipo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Casa de vegetação; CO2; Climatização.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300003

HYBRID SYSTEM SIMULATION TO SUPPLY HEATED AIR TO A SOLAR FOOD DRYER
Provedor de dados: 70
Autores: Rodrigues,Letícia J.; Basso,Diego M.
ABSTRACT The intermittence of solar radiation, due to continuous rainy or cloudy days, is a limitation of simple and small solar dryers. These conditions often make them impossible to use. By including storage systems (thermal accumulation) and/or auxiliary energy sources, drying processes or dehydration can be conducted continuously, even during periods of low insolation. Therefore, the present work simulates and evaluates the thermal and energetic behavior of a hybrid system for heating the air that is directed to the dehydration chamber of a solar food dryer. The software selected for the simulation was TRNSYS. The simulated hybrid system consists of a flat plate solar collector and an arrangement of electrical resistors that guarantee the entry of air,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Electrical resistor arrangement; Flat plate solar collector; Auxiliary heating system; TRNSYS software.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200154

Comparação entre dois tipos de suspensão passiva de barra em condições simuladas de pista de prova normalizada
Provedor de dados: 70
Autores: Pontelli,Cristiano O.; Mucheroni,Mário F.; Balthazar,José M.; Pontes Júnior,Bento R.
Neste trabalho, foram feitas algumas análises sobre o comportamento dinâmico simulado de dois tipos de suspensões passivas das barras dos pulverizadores tracionados. Estas análises foram conduzidas em condições virtuais de pista de prova normalizada ISO 5008, com dois níveis de velocidade de deslocamento do pulverizador (5 km h-1 e 15 km h-1) e em dois perfis de pista existentes na norma (acidentada e suavizada). Foram utilizados nas simulações os softwares MATLAB®; SIMULINK® e Visual Nastran®. Os resultados mostram que a suspensão do tipo trapezoidal teve melhor desempenho em baixas frequências de excitação (w &lt; 0,2 Hz), enquanto a suspensão do tipo pêndulo simples teve melhor desempenho nas demais condições das pistas normalizadas.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Suspensão passiva de barra; Suspensão trapezoidal; Suspensão pendular simples.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400020

SPRAY DRIFT AND CATERPILLAR AND STINK BUG CONTROL FROM AERIAL APPLICATIONS WITH ELECTROSTATIC CHARGE AND ATOMIZER ON SOYBEAN CROP
Provedor de dados: 70
Autores: Cunha,João P. A. R. Da; Barizon,Robson R. M.; Ferracini,Vera L.; Assalin,Marcia R.
ABSTRACT: The use of aerial application with electrostatic charge is an alternative to improve the quality of insecticide applications in soybean crop. The objective of this study was to evaluate the drift and chemical control of the caterpillar and stink bug complex promoted by aerial applications of insecticide in the soybean crop, using electrostatic spray system and rotary atomizers. The insecticide Thiamethoxam + Lambda cyhalothrin was applied with a Cessna 188 Ag Truck agricultural aircraft in two treatments: SPE® electrostatic system, with 54 SPE-5 nozzles and 10 L ha-1 application rate, and Travicar model® 05165 rotary atomizer, with 55° angle blades and application rate of 20 L ha-1. Drift was evaluated through quantification of active ingredient,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural aviation; Application technology; Exodrift; Glycine max.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601163

Sensibility analysis of the pearl model for pesticide leaching in the State of Mato Grosso do Sul, Brazil
Provedor de dados: 70
Autores: Scorza Júnior,Rômulo P.; Silva,João P. da.
For an accurate use of pesticide leaching models it is necessary to assess the sensitivity of input parameters. The aim of this work was to carry out sensitivity analysis of the pesticide leaching model PEARL for contrasting soil types of Dourados river watershed in the state of Mato Grosso do Sul, Brazil. Sensitivity analysis was done by carrying out many simulations with different input parameters and calculating their influence on the output values. The approach used was called one-at-a-time sensitivity analysis, which consists in varying independently input parameters one at a time and keeping all others constant with the standard scenario. Sensitivity analysis was automated using SESAN tool that was linked to the PEARL model. Results have shown that...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Calibration; Pesticide leaching model; Inverse modeling.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500014

CLIMATE CHANGE AND RURAL WORKERS THERMAL COMFORT: HISTORICAL AND FUTURE IMPACTS
Provedor de dados: 70
Autores: Amaro,André L. N.; Yanagi Junior,Tadayuki; Yanagi,Sílvia de N. M.; Ferraz,Gabriel A. E S.; Campos,Alessandro T.
Abstract The aim of the present research was to propose a bioclimatic mapping to classify the thermal comfort and discomfort of rural workers within the state of Minas Gerais, considering historical and future scenarios. Monthly historical series (1976-2014) of minimum, mean and maximum temperature-humidity index (THI), determined through the values of air temperature (minimum, mean and maximum) and relative humidity from 48 weather stations located in the state of Minas Gerais were used to analyze the trends through Mann-Kendall and linear regression assays. The bioclimatic mapping of human comfort, obtained via geostatistical analysis, was developed as a function of the minimum, medium and maximum THI for the historical period (1976-2014) and future...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Human; Biometeorology; Human thermal comfort; THI; Time series.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200173

Avaliação do contato pneu-solo em três modelos de pneus agrícolas
Provedor de dados: 70
Autores: Mazetto,Flávio R.; Lanças,Kléber P.; Nagaoka,Alberto K.; Castro Neto,Pedro; Guerra,Saulo P. S.
Este trabalho teve como objetivo avaliar as áreas de contato, as deformações elásticas dos pneus, a resistência do solo à penetração e os perfis do recalque no solo de três modelos de rodados pneumáticos. O ensaio seguiu um delineamento experimental casualizado, constituído por 12 tratamentos e quatro repetições, nos quais se avaliaram os modelos de pneus de carcaça diagonal, radial e o terceiro de configuração mista, denominado BPAF, inflados com as pressões ideais e submetidos a cargas radiais de 5; 10; 15 e 20 kN, simulando o que ocorre no campo. O ensaio dos pneus agrícolas foi realizado no Núcleo de Ensaio de Máquinas e Pneus Agrícolas - NEMPA, da Faculdade de Ciências Agronômicas - UNESP, Câmpus de Botucatu - SP, em uma prensa hidráulica sobre um...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carga radial; Resistência à penetração; Recalque.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300028

Distribuição da concentração de potássio no solo em lisímetros cultivados com amendoim
Provedor de dados: 70
Autores: Miranda,Jarbas H; Bérgamo,Luís R; Reis,João B. R. da S; Cruciani,Décio E; Duarte,Sergio N.
A aplicação de fertilizantes na agricultura pode provocar uma dinâmica de solutos no solo abaixo da zona radicular, podendo, além de provocar prejuízos econômicos, contaminar águas subterrâneas. O presente trabalho teve como objetivo acompanhar o processo de deslocamento do íon potássio (K+) em lisímetros preenchidos com solo de textura arenosa e cultivado com amendoim (Arachis hypogaea L.), sob diferentes condições de atenuação da densidade de fluxo radiante, como a utilização de filmes plásticos com diferentes espessuras (100 e 150 micras). O deslocamento do íon potássio (K+) foi monitorado por extratores de solução instalados em diferentes profundidades (15 e 25 cm), e o manejo da fertirrigação foi realizado com a utilização de tensiômetros. Concluiu-se...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dinâmica de solutos; Extrator de solução; Fluxo radiante.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200007

Técnicas de mineração de dados para identificação de áreas com cana-de-açúcar em imagens Landsat 5
Provedor de dados: 70
Autores: Nonato,Robson T.; Oliveira,Stanley R. de M.
Neste trabalho, verificou-se a aderência de técnicas de mineração de dados voltadas para problemas de classificação de dados na identificação automatizada de áreas cultivadas com cana-de-açúcar, em imagens do satélite Landsat 5/TM. Para essa verificação, foram estudadas imagens de áreas cultivadas com cana-de-açúcar em três fases fenológicas diferentes. Os pixels foram convertidos em valores de refletância de superfície, nas vizinhanças das cidades de Araras, São Carlos e Araraquara, no Estado de São Paulo. Foram gerados cinco modelos de árvores de decisão binária, induzidos pelo algoritmo C4.5, em que todos produziram taxas de acerto superiores a 90%. A introdução de atributos de textura trouxe ganhos significativos na acurácia do modelo de classificação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mapeamento agrícola; Classificação de imagens; Árvore de decisão; Sensoriamento remoto.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600019

REDUCTION OF SAMPLE SIZE IN THE ANALYSIS OF SPATIAL VARIABILITY OF NONSTATIONARY SOIL CHEMICAL ATTRIBUTES
Provedor de dados: 70
Autores: Maltauro,Tamara C.; Guedes,Luciana P. C.; Uribe-Opazo,Miguel A.
ABSTRACT In the study of spatial variability of soil attributes, it is essential to define a sampling plan with adequate sample size. This study aimed to evaluate, through simulated data, the influence of parameters of the geostatistical model and sampling configuration on the optimization process, and resize and reduce the sample size of a sampling configuration of a commercial area composed of 102 points. For this, an optimization process called genetic algorithm (GA) was used to optimize the efficiency of the geostatistical model estimation based on the Fisher information matrix. The simulated data evidenced that the variation of the nugget effect or practical range did not significantly alter the sample size. GA was efficient in reducing the sample...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fisher information matrix; Genetic algorithm; Geostatistics; Spatial dependence.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800056

Potencial de produção de biogás remanescente nos efluentes de biodigestores abastecidos com dejetos de suínos, com e sem separação da fração sólida, e conduzidos sob diferentes tempos de retenção hidráulica
Provedor de dados: 70
Autores: Orrico Júnior,Marco A. P.; Orrico,Ana C. A.; Lucas Júnior,Jorge de.
O objetivo foi avaliar o potencial poluidor remanescente dos efluentes de biodigestores abastecidos com dejetos de suínos com separação da fração sólida (CSFS) e sem separação da fração sólida (SSFS), e conduzidos sob diferentes tempos de retenção hidráulica (TRH). Os efluentes utilizados eram de biodigestores semicontínuos manejados com TRH de 15; 22; 29 e 36 dias, com e sem separação da fração sólida. Foram utilizados biodigestores batelada, que permaneceram em operação por todo o tempo em que houve produção de biogás (60 dias). Foram avaliadas a produção e a qualidade do biogás, bem como os potenciais de produção por kg de sólidos totais e sólidos voláteis, e as demandas química e bioquímica de oxigênio. Utilizou-se do delineamento inteiramente...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Metano; Sólidos totais; Biodigestão anaeróbia.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400018

Força de tração e volume de solo mobilizado por haste sulcadora em semeadura direta sobre campo nativo, em função do teor de água no solo, profundidade e velocidade de operação
Provedor de dados: 70
Autores: Cepik,Carla T. C.; Trein,Carlos R.; Levien,Renato.
A semeadura direta é um sistema de manejo eficiente em termos de conservação do solo e da água, economia de energia e capacidade operacional dos conjuntos mecanizados. No entanto, em áreas onde existem pecuária e produção de grãos, ou onde o solo é trafegado e trabalhado em condições inadequadas, pode ocorrer compactação do solo nas camadas superficiais. Mesmo compactadas, essas camadas não necessitariam ser descompactadas ou revolvidas, se boa germinação e desenvolvimento da cultura fossem alcançados apenas com a mobilização efetuada pelos sulcadores da semeadora. Os objetivos deste estudo foram determinar a força de tração demandada e o volume de solo mobilizado pelas hastes sulcadoras de adubo, além da patinagem do trator, em diferentes estados de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mobilização do solo; Patinagem; Semeadora-adubadora de precisão.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200018

Greenhouse crisphead lettuce grown with mulching and under different soil water tensions
Provedor de dados: 70
Autores: Geisenhoff,Luciano O; Pereira,Geraldo M; Lima Junior,Joaquim A. de; Silva,Andre L. Pereira da; Aviz,William L. Carrera de.
ABSTRACT Proper irrigation management is important both to enable adequate water supply and to minimize problems with diseases, nutrient leaching and unnecessary water and power wastes. Thus, this study aimed at improving irrigation management in greenhouses. For that reason, we assessed the effect of various water tensions on yield performance of crisphead lettuce, Raider-Plus cv. , grown with mulching. The experiment was conducted in greenhouse at the Federal University of Lavras. Treatments constituted five different soil water tensions, namely 12, 25, 35, 45, and 70 kPa. The results showed that irrigation must be carried out at water soil tension of around 12 kPa to reach satisfying commercial values for both total and commercial yield, 66 and 50 t...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Lactuta sativa; Irrigation management; Protected environment; Soil covering.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100046

Durabilidade de compósito biomassa vegetal-cimento modificado por polímero
Provedor de dados: 70
Autores: Pimentel,Lia L.; Beraldo,Antonio L.; Savastano Júnior,Holmer.
A durabilidade de compósito biomassa vegetal-cimento é um dos fatores mais importantes para a colocação desse material no mercado consumidor. A utilização de polímeros em concreto e argamassa, com o objetivo de melhorar sua durabilidade, é cada vez mais freqüente. Este estudo visou à caracterização de propriedades físicas e mecânicas de compósito biomassa vegetal-cimento modificado com polímeros e a análise da durabilidade desse compósito. Foi testado um polímero de base acrílica em compósitos produzidos com resíduo de Pinus caribaea. Foram realizados ensaios de envelhecimento acelerado, por meio de ciclos de molhamento e secagem, por imersão em água quente e ensaio de envelhecimento natural. As propriedades físicas do compósito avaliadas foram a massa...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compósito fibra vegetal-cimento; Polímeros; MEV.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200002

Anaerobic co-digestion of crude glycerin and starch industry effluent
Provedor de dados: 70
Autores: Larsen,Andrea C.; Gomes,Benedito M.; Gomes,Simone D.; Zenatti,Dilcemara C.; Torres,Douglas G. B.
The Brazil's Biodiesel Production and Use Program introduces biodiesel in the Brazilian energy matrix, bringing along the perspective of a growth of the glycerin offer, co-product generated in the proportion of 10 kg for each 100 L of biodiesel. The aim of this study was to evaluate the addition of crude glycerin in the anaerobic digestion of cassava starch industry effluent (cassava wastewater), in a horizontal semi-continuous flow reactor of one phase in laboratory scale. It was used a reactor with a 8.77 L of useful volume, a medium support for corrugated conduit of polyvinyl chloride (PVC), temperature of 261 ºC, fed with cassava wastewater and glycerin, with hydraulic detention times of 4 and 5 days and increasing volumetric organic load of 3.05;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cassava wastewater; Biodiesel; Biogas; Glycerol.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200013

Formas de mecanização e manejo do solo para a cultura da batata I - características da produção
Provedor de dados: 70
Autores: Jadoski,Sidnei O.; Saito,Larissa R.; Maggi,Marcio F.; Wagner,Marcos V.; Reffatti,Taiã N.
O objetivo da pesquisa foi estudar os efeitos do manejo com diferentes formas de preparo do solo, tipos de resteva e infestação do solo com Trichoderma harzianum sobre a produtividade e as características dos tubérculos da cultura da batata. O experimento foi estruturado em delineamento inteiramente casualizado, em parcelas subsubdivididas, em um esquema fatorial 4 x 5 x 2, com quatro repetições. Foram avaliadas, na parcela, as seguintes formas de preparo do solo: preparo-base (escarificação e sulcamento) - P1; preparo-base mais grade niveladora - P2; preparo-base mais enxada rotativa - P3, e preparo-base mais grade niveladora e enxada rotativa - P4. Na subparcela, utilizaram-se as restevas de aveia, milho, trigo, feijão e uma testemunha sem resteva. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Preparo do solo; Tipos de resteva; Produtividade; Trichoderma harzianum.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500008

Segurança, saúde e ergonomia de trabalhadores em galpões de frangos de corte equipados com diferentes sistemas de abastecimento de ração
Provedor de dados: 70
Autores: Carvalho,Cinara da C. S.; Souza,Cecília de F.; Tinôco,Ilda de F. F.; Vieira,Maria de F. A.; Minette,Luciano J.
O abastecimento de ração nos galpões avícolas pode ser feito de forma manual ou automática, e por demandar esforço acredita-se que o abastecimento manual pode expor o tratador a sobrecarga física. Desta forma, o objetivo deste trabalho foi avaliar os fatores ergonômicos, a postura adotada para a realização das atividades de manejo, bem como a influência na biomecânica dos trabalhadores atuantes em galpões avícolas equipados com comedouro tubular ou automático. Os fatores ergonômicos analisados foram: carga física de trabalho, ambiente térmico, análise postural e biomecânica. Verificou-se que, nos galpões onde o sistema de abastecimento de ração era tubular, os trabalhadores estiveram expostos a maior esforço físico. Baseado no ambiente térmico, o manejo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avicultura; Comedouro; Ergonomia.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300004

Modelo de simulação da temperatura e umidade relativa do ar no interior de estufa plástica
Provedor de dados: 70
Autores: Costa,Edilson; Leal,Paulo A. M.; Carmo Júnior,Ruy R. do.
A simulação dos parâmetros climáticos de temperatura e umidade relativa do ar no interior de uma estufa plástica, por meio do balanço de energia, pode propiciar ao produtor uma ferramenta de auxílio na tomada de decisão. Nesse propósito, realizou-se uma simulação das condições no interior de estufa plástica, em função de parâmetros externos e internos a ela. A simulação revelou uma temperatura no interior da estufa plástica de 23,6 ºC, e os sensores revelaram um valor médio de 24,1 ºC para o período de cultivo da alface. Para a umidade relativa no interior da estufa plástica, o valor simulado foi de 61,6%, e o obtido com o auxílio de sensores foi de 66,0%. Os valores simulados apresentaram-se próximos dos valores obtidos pelos sensores, mostrando que o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Estufa plástica; Umidade relativa do ar; Balanço de energia.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100008

Volumes de calda e pontas de pulverização no controle químico de Spodoptera frugiperda na cultura do sorgo forrageiro
Provedor de dados: 70
Autores: Cunha,João P. A. R. Da; Silva Júnior,Ademilson D. Da.
No manejo de Spodoptera frugiperda na cultura do sorgo, a utilização de inseticida ainda é a principal tática recomendada, contudo este método de controle precisa ser otimizado. O presente trabalho teve como objetivo avaliar o efeito da utilização de três pontas e dois volumes de calda na aplicação de inseticida para o controle químico de Spodoptera frugiperda na cultura do sorgo. O ensaio foi conduzido no delineamento em blocos ao acaso, com quatro repetições, em esquema fatorial (3 x 2) + 1: três tipos de pontas de pulverização (jato cônico vazio, jato plano defletor duplo e jato plano defletor com indução de ar), dois volumes de calda (200 e 130 L ha-1) e um tratamento adicional que não recebeu inseticida. Realizou-se a semeadura direta de uma cultivar...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Bicos de pulverização; Lagarta-do-cartucho; Sorghum bicolor.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400013

Controle estatístico aplicado ao processo de colheita mecanizada de cana-de-açúcar
Provedor de dados: 70
Autores: Silva,Rouverson P. da; Corrêa,Caio F.; Cortez,Jorge W.; Furlani,Carlos E. A.
O avanço da mecanização na colheita da cana-de-açúcar (Saccharum spp.) proporcionou o uso de novas tecnologias e ganho em produtividade para a cultura. O controle da qualidade do processo de colheita da cana-de-açúcar é fundamental para reduzir as perdas. Este trabalho teve o objetivo de avaliar as perdas na colheita mecanizada de cana-de-açúcar, utilizando-as como indicadores de qualidade do processo de colheita. Os dados foram coletados em duas propriedades próximas a Jaboticabal - SP, com a variedade SP80-3280, em 3º e 4º cortes. Caracterizou-se o porte do canavial e, após a colheita, demarcou-se área de 1,5 ha, sendo demarcados 25 pontos, espaçados de 12 x 50 m, quantificando-se as perdas visíveis. Posteriormente, foi aplicado o controle estatístico do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Perdas visíveis; Colhedora de cana-de-açúcar; Controle de qualidade.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200010

Propiedades de adsorción de agua de dos genotipos de arroz rojo
Provedor de dados: 70
Autores: ASCHERI,DIEGO P. R.; BASTOS,SUELY M. C.
A pesar de ser una plaga en el cultivo del arroz blanco, el arroz rojo (Oryza sativa L.) es muy apreciado por su valor nutritivo, sabor, textura y propiedades benéficas. Sus propiedades de adsorción de agua aún no han sido elucidadas, por ese motivo, el objetivo del presente trabajo fue estudiar las propiedades de adsorción de agua de dos genotipos de arroz rojo PB01 y PB05. Fueron utilizados granos de arroz en cáscara con tenor de agua inicial de 2 daga kgms-1 sometidos a proceso de adsorción en 0.113£Aw£0.973 y temperaturas de 30, 50 y 70 °C. Los modelos de Peleg, GAB y Clausius-Clapeyron fueron usados para predecir las variaciones de la humedad de equilibrio en función del tiempo, las isotermas y estabilidad y el calor isostérico de adsorción de agua,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Oryza sativa; Isotermas; Calor isostérico; Estabilidad; Actividad de agua; Cinética de adsorción de agua.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100134

Pontualidade na operação de semeadura e a antecipação da adubação e suas influências na receita líquida da cultura da soja
Provedor de dados: 70
Autores: Matos,Marcos A.; Salvi,José V.; Milan,Marcos.
A cultura da soja tem papel fundamental na economia do País, e estudos sobre os fatores que afetam sua produtividade, apresentam grande importância; um desses fatores está relacionado com a interação entre a época de semeadura e a produtividade da cultura. Os atrasos durante a operação de semeadura resultam em decréscimos na produtividade, e uma das razões para a sua ocorrência é a necessidade de aplicar grandes quantidades de adubo no momento da implantação da cultura. Essas grandes quantidades implicam maior tempo e número de abastecimentos da semeadora, influindo na sua capacidade operacional, sendo uma das alternativas para contornar o problema, antecipar a adubação, realizando-a na cultura anterior. Dessa forma, o objetivo deste trabalho foi avaliar a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanização agrícola; Modelo; Custos.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200018

UMEB - Unidade Móvel para Ensaio da Barra de Tração
Provedor de dados: 70
Autores: Gabriel Filho,Antonio; Lanças,Kléber P.; Guerra,Saulo P.; Paula,Cristiano A.; Monteiro,Leonardo A.
Um equipamento denominado "Unidade Móvel de Ensaio da Barra de Tração - UMEB", foi desenvolvido na FCA/UNESP de Botucatu para realizar ensaios de tratores em solo agrícola. Construída a partir de um reboque ("trailer"), a UMEB foi adaptada para servir como carro dinamométrico instrumentado, utilizado na avaliação do desempenho de tratores submetidos a ensaios na barra de tração. Sua massa total é de 10.500 kg sustentados por um conjunto de seis rodados pneumáticos. Ensaios de campo mostraram que a UMEB proporcionou força de tração acima de 35 kN, mantendo-a constante, em diferentes condições de superfície do solo, mesmo quando a velocidade de deslocamento foi modificada.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Mecanização; Desempenho; Ensaio de tração; Pneu.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400018

Simulação do rendimento e riscos climáticos para o milho safrinha em Londrina - PR, utilizando o modelo CERES-Maize
Provedor de dados: 70
Autores: Cardoso,Célio O.; Faria,Rogério T. de; Folegatti,Marcos V.
Modelos matemáticos possibilitam simular realisticamente o crescimento e o desenvolvimento fenológico de culturas sob ampla gama de condições ambientais e de manejo, a um baixo custo. O objetivo deste trabalho foi investigar os efeitos da época de semeadura no estabelecimento e rendimento do milho safrinha para Londrina - PR, mediante simulações de longo período com o modelo CERES. Os tratamentos consistiram na combinação de 12 épocas de semeadura, uma em cada decêndio, de janeiro a abril, sob dois cenários: sem limitação hídrica (produção potencial) e com limitação hídrica, considerando-se uma cultivar de ciclo precoce, XL-520, durante 24 anos. Os resultados mostraram decréscimos de rendimentos de até 38% da produtividade potencial e de 44% da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelo matemático; Irrigação; Modelagem.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200007

HYDROPHILIC POLYMER CHANGES THE WATER DEMAND IN THE IMPLEMENTATION OF A DWARF CASHEW ORCHARD
Provedor de dados: 70
Autores: Gondim,Rubens S.; Serrano,Luiz A. L.; Maia,Aline de H. N.; Silva,Janderson P. da.
ABSTRACT Important losses of dwarf cashew seedlings during the establishment of orchards in the Brazilian semiarid are related to the relatively short rainy season. This study aimed to evaluate biochar and hydrophilic polymer as soil amendments to increase water retention and reduce plant death in the first year. An experiment was conducted at the Curu Station, Paraipaba, CE, Brazil, using the clone BRS 226. The experimental design consisted of randomized blocks, with amounts of 0.5, 1.0, 2.0, and 4.0 kg of cashew wood biochar and 20, 40, 60, 80 g of hydrophilic polymer applied per pit, as well as a control treatment (no soil amendment). Seedlings were submitted to an irrigation regime to avoid water stress (5 L water seedling−1 when the tensiometer...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anacardium occidentale L.; Climate change; Adaptation; Soil amendment; Biochar.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300344

ELECTROSTATIC SPRAYING EFFECT ON SPRAY DEPOSITION AND POWDERY MILDEW CONTROL IN SOYBEAN
Provedor de dados: 70
Autores: Assunção,Heli H. T. de; Silva,Sérgio M.; Alves,Guilherme S.; Zandonadi,Cesar H. S.; Cunha,João P. A. R. da.
ABSTRACT Electrostatic spray can bring benefits to the pesticide application such as the reduction of application rate and the increase of deposits on targets. Therefore, this study aimed to evaluate the effect of electrostatic spraying using lower application rates and different adjuvants on soybean spray deposition and chemical control of powdery mildew (Microsphaera diffusa Cooke &amp; Peck). The field experiment was conducted in duplicate. A randomized complete block design with four replications in a 2 × 2 × 2 + 1 factorial scheme was used. The factors were two application rates, with and without droplet electrification, two spray solution compositions, and one additional treatment. Deposition on upper and lower leaves, spray loss to the soil, and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application rate; Droplet electrification; Application technology; Microsphaera diffusa.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600721

Aplicação da análise envoltória de dados (AED) na avaliação da eficiência operacional relativa entre usinas de cana-de-açúcar no território brasileiro
Provedor de dados: 70
Autores: Salgado Junior,Alexandre P.; Carlucci,Fabio V.; Novi,Juliana C.
Este estudo tem por objetivo analisar o impacto das variáveis tamanho e localização na eficiência operacional de usinas de cana-de-açúcar no Brasil na safra 2008/2009. Para tanto, realizou-se um estudo de eficiência operacional, por meio da aplicação da Análise Envoltória de Dados (AED), na qual foi possível identificar as usinas mais eficientes dentre um universo de 355 e classificá-las por tamanho e localização. A análise quantitativa sugere que existe maior concentração de usinas classificadas como eficientes e de tamanho grande, localizadas no estado de São Paulo. Objetivando uma análise em profundidade, foi realizado um estudo de múltiplos casos em um grupo de usinas. Conclui-se que a eficiência operacional de usinas de cana-de-açúcar depende da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Usinas de cana-de-açúcar; Análise envoltória de dados (AED); Eficiência operacional.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500003

Produção e pós-colheita de flores de girassóis sob estresse salino em hidroponia de baixo custo
Provedor de dados: 70
Autores: Santos Júnior,José A.; Gheyi,Hans R.; Cavalcante,Antônio R.; Dias,Nildo da S.; Medeiros,Salomão de S.
RESUMO Em face de características relacionadas à infraestrutura, situação edáfica, hídrica e social, peculiares do semiárido brasileiro, é precípua a utilização de sistemas de cultivo alternativos que considerem tais características, inclusive a qualidade da água disponível. Dentro desta lógica, o objetivo do presente trabalho foi avaliar os efeitos do estresse salino sobre as variáveis de produção e pós-colheita de flores de girassóis cultivadas em um sistema hidropônico alternativo de baixo custo. Utilizou-se de delineamento experimental inteiramente casualizado, analisado em esquema fatorial 4 x 3, com três repetições; os tratamentos consistiram na utilização de quatro níveis de salinidade da solução nutritiva (1,7 – testemunha; 4,3; 6,0 e 9,0 dS m-1)...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Floricultura; Salinidade; Agricultura familiar.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000300420

Effects of drying air temperature and grain initial moisture content on soybean quality (Glycine Max (L.) Merrill)
Provedor de dados: 70
Autores: Coradi,Paulo C.; Fernandes,Carlos H. P.; Helmich,Jean C.; Goneli,André L. D.
ABSTRACT This study aimed to evaluate the effect of air-drying temperature and initial moisture content on volume shrinkage, physical quality and oil extraction yield of soybean grains. The grains used in this experiment were harvested at two distinct moisture levels of 19 and 25%. Then, these grains were taken to dryness at three different air temperatures of 75 °C, 90 °C and 105 °C, in a forced circulation convection oven of the air. The results showed a drying time reduction with increasing air temperatures. Regarding volume shrinkage, moisture content reductions influenced grain volume and the Rahman's model was the one that best fit the data. Moreover, the higher the air temperature, the greater the effects on soybean grain shrinkage and physical...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Extraction; Performance; Processing.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500866

Influência da espécie vegetal cultivada nas condições redox de sistemas alagados construídos
Provedor de dados: 70
Autores: Matos,Antonio T. de; Freitas,Wallisson da S.; Brasil,Mozart da S.; Borges,Alisson C.
Em vista da escassez de informações sobre a influência de diferentes macrófitas nas condições ambientais de Sistemas Alagados Construídos (SACs), monitorou-se o potencial redox (Eh) da água residuária da suinocultura (ARS) em tratamento, em 5 SACs, com dimensões de 24,0 m x 1,1 m x 0,70 m. A ARS, previamente tratada em filtros, foi aplicada numa vazão de 0,8 m³ d-1, com tempo de residência aproximado de 4,8 d. Nos SAC1, SAC2 e SAC3 foram plantados, respectivamente, taboa (Typha latifolia L.), alternanthera (Alternanthera philoxeroides (Mart.) Griseb) e capim tifton-85 (Cynodon dactylon Pers.); no SAC4 foi plantado, no primeiro terço do tanque, alternanthera, no segundo terço, taboa e no terceiro terço, capim tifton-85. No SAC5, nada foi plantado....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Macrófitas; Potencial de oxirredução; Suinocultura; Tratamento de águas residuárias; Wetlands.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300015

Incorporação de casca de arroz e de braquiária e seus efeitos nas propriedades físicas e mecânicas de tijolos de solo-cimento
Provedor de dados: 70
Autores: Ferreira,Régis de C.; Gobo,Júlio C. da C.; Cunha,Ananda H. N.
A forma indiscriminada de extração dos recursos naturais e a poluição gerada pelos resíduos promovem impactos sobre o meio ambiente e é motivo de grande preocupação. Visando a oferecer alternativas de destinação de resíduos agrícolas, o presente trabalho estudou composições da mistura de solo-cimento-resíduo agrícola, tendo como objetivo principal determinar os teores máximos de resíduos a serem incorporados sem o comprometimento de suas características mecânicas. Foram utilizados dois tipos de resíduos vegetais (cascas de arroz e de braquiária) e utilizou-se o cimento Portland CP II-F-32 para a composição dos tratamentos. Nas combinações, os teores de cimento e resíduo variaram desde 100% de cimento e 0% de resíduo, até 60% de cimento e 40% de resíduo. Os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resíduos vegetais; Tijolos de terra crua; Resistência à compressão.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100001

Caracterização do microambiente em secção transversal de um galpão do tipo "free-stall" orientado na direção norte-sul
Provedor de dados: 70
Autores: Campos,Alessandro T.; Klosowski,Elcio S.; Santos,Wallacy B. R.; Gasparino,Eliane; Campos,Aloísio T.
O trabalho teve o objetivo de caracterizar o microambiente climático das baias de um galpão de confinamento para gado leiteiro, modelo "free-stall", no sentido transversal da instalação. O "free-stall" é orientado na direção norte-sul, localizado em Marechal Cândido Rondon, região Oeste do Paraná, com capacidade para abrigar 40 vacas em lactação (40 baias). Visando à determinação do Índice de Temperatura do Globo e Umidade (ITGU) e da Carga Térmica de Radiação (CTR), foram instalados quatro globos negros, no centro de baias dispostas no sent ido transversal, dispondo dois globos no lado oeste e dois globos no lado leste (separados pelo corredor de alimentação). Lateralmente ao galpão, no lado leste, havia vegetação a 4 m da instalação, que promovia...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência; Carga térmica de radiação; Gado de leite.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100001

Efeito prolongado de sistemas de preparo do solo com e sem cultivo de soqueira de cana crua em algumas propriedades físicas do solo
Provedor de dados: 70
Autores: Camilotti,Fábio; Andrioli,Itamar; Dias,Fábio L. F.; Casagrande,Ailto A.; Silva,Alysson R. da; Mutton,Miguel A.; Centurion,José F.
Este trabalho foi conduzido em Latossolo Vermelho distrófico típico, sob cultivo de cana crua, com o objetivo de avaliar o efeito prolongado de sistemas de preparo do solo, com e sem cultivo da soqueira, e épocas de amostragem sobre algumas propriedades físicas do solo. O delineamento experimental foi o de blocos ao acaso, em esquema de parcelas subsubdivididas, sendo os tratamentos principais quatro sistemas de preparo do solo: (i) controle da soqueira com duas gradagens, subsolagem e mais uma gradagem de nivelamento; (ii) controle da soqueira com herbicida e uma subsolagem; (iii) controle da soqueira com herbicida; (iv) controle da soqueira com herbicida, aração com arado de aivecas e uma gradagem de nivelamento. Os tratamentos secundários foram: com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Densidade do solo; Porosidade; Saccharum.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100021

Desempenho operacional de um trator agrícola equipado alternadamente com pneus radiais e diagonais
Provedor de dados: 70
Autores: Barbosa,Jackson A.; Vieira,Luciano B.; Dias,Gutemberg P.; Dias Júnior,Moacir de S.
A utilização de pneu radial em tratores agrícolas na década de 1950 resultou em redução das perdas de potência oriundas da resistência ao rolamento e patinagem, com conseqüente melhoria no desenvolvimento da tração. Este trabalho teve como objetivo comparar o desempenho operacional de um trator agrícola equipado alternadamente com pneus radiais e diagonais. A avaliação foi realizada a partir de análises de parâmetros indicadores do desempenho dos referidos pneus sob condições específicas de trabalho. O uso de pneus radiais proporcionou incrementos nos valores de capacidade de tração e potência na barra, diminuição nos valores de consumo específico de combustível e não causou variações no consumo horário de combustível.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pneus agrícolas; Eficiência em tração.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200021

SIMULATION OF DISTANCE BETWEEN FIELD AND REPLENISHMENT PUMP IN MECHANIZED SPRAYING OF SUGARCANE (Saccharum spp.)
Provedor de dados: 70
Autores: Santos,Neisvaldo B. dos.
ABSTRACT Brazil is the world's largest producer of sugarcane destined for mills. Spraying in sugarcane plantations is carried out in extensive cultivation areas and with self-propelled, tractor-driven, and aerial hydraulic equipment. For this, a good positioning of the replenishment pump of agricultural defensives close to the field where the spraying is carried out is necessary. However, it is desirable that the replenishment be carried out at short distances between the field and replenishment pump. This study aimed to assess the impact of the distance between the field and replenishment pump on the operational cost of hydraulic sprayers for sugarcane farming practices. Due to the difficulty in accomplishing the work and meeting the objective under field...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cost; Agricultural mechanization; Computational model; Hydraulic sprayers; Planning and management.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500805

Uso de dois penetrômetros na avaliação da resistência mecânica de um latossolo vermelho distrófico
Provedor de dados: 70
Autores: Roboredo,Delmonte; Maia,João C. de S; Oliveira,Osvaldo J. de; Roque,Cassiano G.
A compactação do solo é um problema que interfere no crescimento radicular e na produção vegetal. O estudo foi realizado na estação experimental do Centro Federal de Educação Tecnológica de Cuiabá (CEFET), município de Santo Antônio do Leverger - MT. O objetivo foi avaliar a resistência mecânica do solo à penetração em um Latossolo Vermelho distrófico, em função de diferentes teores de água, em duas profundidades, utilizando-se de um penetrômetro de velocidade constante e um de impacto, correlacionando-os à densidade do solo. O delineamento experimental utilizado foi em blocos casualizados, com oito tratamentos e cinco repetições, dispostos em esquema de parcelas subdivididas, sendo quatro faixas de umidade nas parcelas: faixa 1 (0,1883 a 0,2354 m³ m-3);...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Penetrometria; Compactação; Umidade; Densidade do solo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200013

Desempenho de um trator agrícola equipado com pneus radiais e diagonais com três níveis de lastros líquidos
Provedor de dados: 70
Autores: Monteiro,Leonardo de A.; Lanças,Kléber P.; Guerra,Saulo P. S.
A utilização correta de pneus em tratores, tanto em relação ao seu tipo quanto à calibração de sua pressão interna, e a lastragem ideal para cada condição de carga são fatores que influem significativamente no desempenho do trator. Esta pesquisa teve como objetivo comparar o desempenho de um trator equipado com pneus radiais e com pneus diagonais, para três condições de lastragem líquida (0%, 40% e 75% de água), em três condições superficiais de um Nitossolo Vermelho distrófico (superfície firme, preparada e com cobertura vegetal de resto de milho) e em três velocidades teóricas de deslocamento (4 km h-1, 5 km h-1 e 7 km h-1), informadas no painel do trator, correspondendo às marchas B1, B2 e C1. O melhor desempenho do trator, equipado com pneu diagonal,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eficiência trativa; Máquinas agrícola; Ensaio de tratores.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300015

Projeto de um cortador de base para colhedora de cana-de-açúcar utilizando otimização matemática
Provedor de dados: 70
Autores: Volpato,Carlos E. S.; Braunbeck,Oscar A.; Oliveira,Carlos A. A. de; Santos,Ariston P.
Um cortador de base representado por um mecanismo de quatro barras foi desenvolvido utilizando-se do programa Autocad. Suas partes constituintes foram pré-dimensionadas em função das características operacionais de uma colhedora de cana-de-açúcar em sistema de cana crua e inteira, colhendo uma linha de cana por passada. A força normal de reação do perfil no ponto de contato foi determinada por meio da análise dinâmica, sendo as equações de equilíbrio dinâmico baseadas nas leis de Newton-Euler. O processo de otimização teve como objetivo minimizar a força normal de reação do solo, submetida a restrições de posição, trajetória, comprimento das barras, constante da mola e da força normal. Implementou-se o Algoritmo de Programação Quadrática Seqüencial - SQP...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mecanismo de quatro barras; Colheita mecânica; Projeto de máquinas.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300022

Operational parameters of soybean seeding in santa fe system
Provedor de dados: 70
Autores: Chioderoli,Carlos A.; Furlani,Carlos E. A.; Aguiar,Aislan O.; Cavichioli,Fábio A.; Cassia,Marcelo T.
The use of no tillage system associated with the crop-livestock integration is an alternate managing that promotes the accumulation of dry matter in the soil, an essential fact to make the system sustainable and profitable. The aim of this study was to evaluate the operational performance of a planter-tractor set on maize straws intercropped with Urochloa, in different seeding modes. The soybean crop was seed on the intercropping of two forage species (Urochloa brizantha and Urochloa ruziziensis) in five cropping systems: MBL (Maize with Urochloa in the maize seeding row, mixed with base fertilizer and deposited at 0.10 m), MBE (Maize with Urochloa seeded between rows at the same day of seeding maize), MBC (Urochloa between rows of maize seeded with the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: No tillage system; Crop-livestock integration; Slip; Operating performance.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500009

Aspectos qualitativos da avaliação de pulverizadores hidráulicos de barra na região de Uberlândia, Minas Gerais
Provedor de dados: 70
Autores: Alvarenga,Cleyton B. de; Cunha,João P. A. R. da.
A inspeção periódica de pulverizadores é uma importante ferramenta para melhorar a tecnologia de aplicação de defensivos. O objetivo deste trabalho foi avaliar o estado de funcionamento de pulverizadores agrícolas na região de Uberlândia - MG, e a metodologia de inspeção para as condições brasileiras. As avaliações foram realizadas em propriedades rurais visitadas aleatoriamente e consistiram em um questionário preenchido pelo operador das máquinas e da inspeção propriamente dita dos pulverizadores. Os itens avaliados foram: existência de vazamentos, mangueiras e conexões, filtros, válvulas antigotejo, pontas de pulverização na barra, proteção de partes móveis, orientação por faixa e monitoramento das condições climáticas. A inspeção mostrou a necessidade...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Aplicação de defensivos; Inspeção de máquinas agrícolas.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300019

Mechanical properties of castor beans subject to different drying temperatures aiming to disrupt the bean coat
Provedor de dados: 70
Autores: Bastos,Adriano C.; Ferraz,Antonio C. De O.
In castor oil extraction process, the bean coat is abrasive to the equipment and releases substances that modify the oil color, reducing its quality. A potential solution would be to run the extraction by compressing only the endosperm. Due to lack of information, the objective of this study was to evaluate the influence of forced air drying at 40, 60, 80 and 100 ºC and farmyard drying, in the mechanical properties of the beans, aiming to break the bean coat. Castor beans were subjected to compression tests, in two perpendicular directions, at a strain rate of 0.6 mm.s-1. Average values of force, deformation energy, strain, all at rupture, and stiffness were used to evaluate the effects of dehydration. It was observed that the heat treatments did not alter...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Conditioning; Threshing; Decortication; Compression.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100011

PEACH PIT CHEMICALLY TREATED BIOMASS AS A BIOSORBENT FOR METFORMIN HYDROCHLORIDE REMOVAL: MODELING AND SORPTION MECHANISMS
Provedor de dados: 70
Autores: Hellmann,Liliane; Schmitz,Ana P. de O.; Módenes,Aparecido N.; Hinterholz,Camila L.; Antoniolli,Camila de A.
ABSTRACT In this work, the potential of peach pit biosorption in the removal of the drug metformin hydrochloride from water is evaluated. Experiments are carried out in a closed batch system to evaluate the effect of the solution pH (2–10), temperature (25, 35 and 45 °C), stirring (100, 150 and 200 rpm) and chemical treatments. During the study, biosorbent characterization, kinetic tests, equilibrium tests and thermodynamic parameter calculations are performed. The operating conditions that show the best results for both the raw biosorbent and the biosorbent submitted to acid, basic and acid followed by basic treatments with removal capacities of 3.17, 10.83, 18.10 and 49.14 mg g−1, respectively, are pH 7, 25 °C and 100 rpm, which result in an equilibrium...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biosorption; Metformin hydrochloride; Peach pit; Kinetic modeling; Equilibrium modeling.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200181

Avaliação de semeadora-adubadora de precisão trabalhando em três sistemas de preparo do solo
Provedor de dados: 70
Autores: Furlani,Carlos E. A.; Lopes,Afonso; Silva,Rouverson P. da.
Avaliou-se uma semeadora-adubadora de precisão com quatro linhas, na cultura do milho (Zea mays L.), trabalhando em Latossolo Vermelho-Escuro eutrófico, A moderado, textura argilosa. As parcelas experimentais foram dispostas em blocos casualizados, com quatro repetições, em esquema fatorial 3 x 3, totalizando 36 observações. Os fatores foram dados pelos sistemas de preparo do solo (convencional, plantio direto e reduzido) e pelas marchas do trator (3ª reduzida alta, 4ª reduzida baixa e 4ª reduzida alta). Foram analisadas as variáveis velocidade de deslocamento, queda de velocidade, força de tração e potência na barra, consumo de combustível, rotação do motor e patinagem média dos rodados do trator. Os resultados mostraram que a operação de semeadura em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Desempenho; Velocidade; Combustível.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200019

Instalação, calibração e funcionamento de um lisímetro de pesagem
Provedor de dados: 70
Autores: Carvalho,Daniel F.; Silva,Leonardo D. B.; Guerra,José G. M.; Cruz,Francisco A.; Souza,Adilson P.
Este trabalho teve como objetivo construir, instalar, calibrar e avaliar a sensibilidade de um lisímetro de pesagem com célula de carga, instalado em Seropédica - RJ, a fim de determinar a evapotranspiração de referência (ETo). O lisímetro, com dimensões de 1,0 m x 1,0 m e 0,7 m de profundidade, foi construído com chapas de aço galvanizado e instalado sobre estrutura metálica montada sobre barras transversais, a fim de concentrar toda a massa do conjunto sobre uma célula de carga localizada no centro do sistema. Após o preenchimento do lisímetro com solo, foi realizada a calibração do mesmo por meio de análise de regressão linear, e toda a área foi plantada com grama-batatais. O conjunto lisimétrico instalado mostrou-se adequado para a estimativa da ETo,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiração; Lisimetria; Célula de carga.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300005

Atributos físicos, químicos e erosão entressulcos sob chuva simulada, em sistemas de plantio direto e convencional
Provedor de dados: 70
Autores: Silva,Cristiane G. da; Alves Sobrinho,Teodorico; Vitorino,Antonio C. T.; Carvalho,Daniel F. de.
Este trabalho teve como objetivo estimar as perdas de solo e água, nos sistemas de plantio direto e convencional, e foi realizado no câmpus experimental da UFMS, em Dourados - MS, em solo classificado como Latossolo Vermelho distroférrico, no período compreendido entre outubro de 2001 e novembro de 2002. As estimativas das perdas de solo e de água foram feitas utilizando-se do infiltrômetro de aspersão InfiAsper/UFMS, regulado para aplicar chuva com intensidade de 60 mm h-1, correspondendo à energia cinética de aproximadamente 820 Jm-2. Foram utilizados os seguintes tratamentos: sucessão milho-pousio; sucessão milho-trigo; sucessão milho-nabo; sucessão milho-ervilhaca; sucessão milho-aveia, os quais foram avaliados nos sistemas de preparo convencional (PC)...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Simulador de chuva; Sucessão de culturas; Perda de solo.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100016

Compostagem e vermicompostagem de dejetos de caprinos: efeito das estações do ano
Provedor de dados: 70
Autores: Amorim,Ana C.; Lucas Júnior,Jorge de; Resende,Kleber T. de.
A caprinocultura brasileira cresceu consideravelmente nos últimos anos, elevando a produção de resíduos, fato que justifica o estudo de práticas de reciclagem, tais como a compostagem e a vermicompostagem, pois, além da agregação de valor com a produção do composto, representa um meio de saneamento na área rural. Para o desenvolvimento deste trabalho, foram utilizados dejetos coletados de caprinos em diferentes faixas etárias, mantidos em sistema de semiconfinamento e com regime alimentar único. O objetivo principal foi avaliar os efeitos das estações do ano sobre os processos de compostagem e vermicompostagem. As reduções na quantidade de matéria seca (MS) foram de 53,7; 53,4; 51,4 e 47,8% para a compostagem e 57,4; 51,0; 41,4 e 53,6% para a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Estações do ano; Leira; Relação C/N.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100007

Regionalização de vazões com base em modelo digital de elevação para a bacia do Rio Paraíba do Sul
Provedor de dados: 70
Autores: Baena,Luiz G. N.; Silva,Demetrius D. da; Pruski,Fernando F.; Calijuri,Maria L.
A regionalização de vazões tem sido realizada com o objetivo de disponibilizar informações hidrológicas em locais sem dados ou com poucas informações disponíveis, porém a determinação das características físicas das bacias de drenagem para cada local de interesse limita consideravelmente a aplicação dos resultados de um estudo convencional de regionalização de vazões. Uma das soluções para esse problema é a automação do processo de delimitação de bacias, utilizando-se de modelo digital de elevação hidrologicamente consistente (MDEHC). O objetivo principal deste trabalho foi a regionalização de vazões máxima, mínima e média de longo período e da curva de permanência para a bacia hidrográfica do Rio Paraíba do Sul, a montante da cidade de Volta Redonda, com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistema de informações geográficas; Bacia hidrográfica; Recursos hídricos.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300013

Distribution of water in sandy soil applied by drip
Provedor de dados: 70
Autores: Gonçalves,Antônio C. A.; Alves,Daniel S.; Marques,Patricia A. A.; Folegatti,Marcos V.; José,Jefferson V.
The search for the use of water with high levels of efficiency has motivated the use of drip irrigation in several agricultural systems. However, for the efficiency be ensured, it is necessary that the water distribution in the soil profile must to be known in more details. As it is a highly variable process, function of the local characteristics, is essential the study of each case. The objective of this research was evaluating the water distribution in the soil profile, from drippers installed in surface and 0.15 m below the soil surface. The experiment was realized in the Technical Center of Irrigation (TCI) of the State University of Maringá - PR. The water monitoring in the soil profile was done with TDR probes installed in a box containing sandy...
Tipo: Info:eu-repo/semantics/other
Palavras-chave: Time Domain Reflectometry; TDR probes; Irrigation.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600013

Eficiência de um hidrociclone de geometria "rietema" para pré-filtragem de água para irrigação
Provedor de dados: 70
Autores: Cruz,Othon C. Da; Zanini,José R.
O hidrociclone é um equipamento amplamente utilizado pela indústria em processos envolvendo separação sólido-líquido, porém ainda pouco utilizado na agricultura irrigada no Brasil. Neste trabalho, avaliou-se o desempenho deste equipamento como pré-filtrante de partículas sólidas, oriundas dos processos erosivos e do assoreamento dos recursos hídricos. Os testes foram realizados com um hidrociclone de geometria "Rietema", possuindo diâmetro de 19,2 cm na parte cilíndrica, operando com vazões variando entre 10 m³ h-1 e 27 m³ h-1. Os materiais particulados usados em suspensão foram: solo franco-argiloso e areia de rio. Os resultados mostraram que a perda de carga máxima média foi de 52 kPa e 47 kPa para as suspensões aquosas de areia e solo, respectivamente....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Separação sólido-líquido; Pré-filtro; Irrigação localizada.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400008

HARVESTING FRUITS USING A MOBILE PLATFORM: A CASE STUDY APPLIED TO CITRUS
Provedor de dados: 70
Autores: Ferreira,Marcos D.; Sanchez,Augusto C.; Braunbeck,Oscar A.; Santos,Eduardo A.
ABSTRACT Harvesting fruits and vegetables has been a challenge. Mobile platforms for harvesting vegetables and fruits have been used, but with some limitations, such as their applicability for a certain time of the year and for a specific crop. A mobile platform was initially developed for harvesting fresh market tomatoes, mainly staked in Brazil. However, after field trials, many problems were identified, such as crop use limitation and machine structure problems. Therefore, the initial project was reformulated to assume different functions, with a retractable and smaller frame and the possibility of adding on other devices, expanding crop harvest and farm use. The concept of a hybrid vehicle with one electric power generator to drive all four wheels with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fruits and vegetables; Harvesting aid; Hybrid vehicle; Multiuse.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200293

Parâmetros solo-máquina em função de doses de resíduos vegetais e profundidades de deposição de adubo em semeadura direta
Provedor de dados: 70
Autores: Kamimura,Karina M.; Levien,Renato; Trein,Carlos R.; Debiasi,Henrique; Conte,Osmar.
O tráfego contínuo e inadequado de máquinas em solos sob semeadura direta tem provocado alterações dos atributos físicos e mecânicos dos solos, influenciando, dessa forma, na produtividade das culturas. O experimento foi conduzido na Estação Experimental Agronômica da Universidade Federal do Rio Grande do Sul, no município de Eldorado do Sul - RS, num Argissolo Vermelho distrófico típico, com o objetivo de quantificar a força de tração e obter informações sobre os atributos físicos do solo, em semeadura direta sobre resíduos de aveia-preta e ervilhaca parcialmente decomposta. O delineamento experimental utilizado foi em blocos casualizados, com parcelas subsubdivididas, sendo, nas parcelas principais, doses de resíduos da cultura de inverno (0; 1,3; 2,6;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Atributos físicos do solo; Força de tração; Tráfego de máquinas.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300010

RETENTION CURVES AND AVAILABLE WATER CAPACITY IN LATOSOLS
Provedor de dados: 70
Autores: Maia,Felipe C. de O.; Bufon,Vinicius B.; Leão,Tairone P.
ABSTRACT Water stored in the soil between field capacity and the permanent wilting point, is known as the available water capacity. Its availability to be effectively used by plants depends on the type of soil and its water retention characteristics. The aim of this work was to compile information about water retention curves in Latosols, and to provide a first approximation of values and most likely amplitudes for water storage and available water capacity of these soils. The database was constituted from information collected from articles, theses, dissertations and other publications. Soil water retention curves, as well as available water, were estimated for the order Latosols, and for the suborders Red Latosol (RL), Red-Yellow Latosol (RYL) and Yellow...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Field capacity; Permanent wilting point; Van Genuchten; Tropical soils.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400546

Formação de mudas de eucalipto com utilização de lixo orgânico e níveis de irrigação calculados por dois métodos
Provedor de dados: 70
Autores: Galbiatti,João A.; Lui,Jandislau J.; Sabonaro,Débora Z.; Bueno,Lara F.; Silva,Vanessa L. da.
O estudo das características e das possibilidades de utilização de Resíduo Sólido Urbano (R.S.U.) e mais especificamente de Resíduo Sólido Orgânico Urbano (R.S.O.U.), no Brasil e no Mundo, ainda não produziu informações que possibilitem conhecimentos suficientes para tomadas de decisões que estão sendo exigidas, em razão do crescente volume de resíduos produzidos e os impactos ao meio ambiente. Este trabalho teve o objetivo de estudar o efeito da irrigação associada ao uso de R.S.O.U. para formação de mudas de eucalipto. A pesquisa foi desenvolvida na UNESP, Câmpus de Jaboticabal - SP, sendo adotado como delineamento estatístico o esquema fatorial inteiramente casualizado. Foram utilizados 11 substratos: dois tipos de solos (um Latossolo Vermelho eutrófico...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eucalipto; Resíduo orgânico; Substrato.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300013

IMPACT OF THE HYDRAULIC LOADING RATE ON THE HYDRODYNAMIC CHARACTERISTICS OF AN ANAEROBIC FIXED BED REACTOR TREATING CATTLE SLAUGHTERHOUSE WASTEWATER
Provedor de dados: 70
Autores: Kreutz,Cristiane; Carvalho,Karina Q. de; Passig,Fernando H.; Belini,Aldria D.; Cordovil,Cláudia S. de C. M. dos S.; Gomes,Simone D.
ABSTRACT The hydrodynamic behavior of an anaerobic fixed bed reactor (AFBR) was evaluated in the treatment of cattle slaughterhouse wastewater. The AFBR was operated at hydraulic retention time (HRT) of 14, 11 and 8 h. Stimulus-response assays were carried out with Eosin Y and the experimental data were adjusted to the single-parameter theoretical models of dispersion and N-continuous stirred tank reactors in series (N-CSTR). The experimental results of the residence time distribution curves showed that at lower flow rate, the reactor showed plug flow behavior with correlation coefficient (r) of 0.88 and number of dispersion of 0.2 for high dispersion (HD). However, at higher and intermediate flow rates, the AFBR behave as a complete mixture flow, (r) of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dead space volume; Hydraulic efficiency; Hydraulic short; Circuiting; Residence; Time distribution.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300403

MODELING OF BASIL ESSENTIAL OIL EXTRACTION WITH VARIABLE DIFFUSION COEFFICIENT
Provedor de dados: 70
Autores: Silveira,Jeniffer C.; Costa,Andréa O. S. da; Costa Junior,Esly F. da.
ABSTRACT: Essential oils are complex mixtures of volatile compounds found at low levels in aromatic plant specific parts. Soluble in organic solvents, these oils are characterized by their fragrance and antimicrobial activity, being widely used in industries. The mathematical modeling of essential oil extraction is a relevant step in the project of industrial plants because it is about achieving optimized operational conditions. A model is available in the literature describing the extraction process of basil essential oil, based on diffusion within the leaf. Parametric equations were tested for the variable diffusion coefficient with the concentration, resulting in a significant improvement in the description process, when compared to papers presented in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Concentration variable diffusion; Parameter estimation; Essential oils.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400717

Distribuição da calda herbicida por pontas de pulverização agrícola utilizadas em áreas de reflorestamento com eucalipto
Provedor de dados: 70
Autores: Ferreira,Marcelo da C.; Di Oliveira,José R. G.; Dal Pietro,Ivan R. P. da S.
O trabalho teve como objetivo avaliar a distribuição de calda por pontas de pulverização hidráulicas para a aplicação de herbicidas em pré-emergência das plantas daninhas, em função do espaçamento na barra utilizada em áreas de reflorestamento com eucalipto. O experimento foi realizado no Laboratório de Ciência das Plantas Daninhas do Departamento de Fitossanidade da UNESP, Câmpus de Jaboticabal. Foram utilizados os modelos com indução de ar AIUB 025, AI 110025, TTI 110015 e DB 12002, considerando o espaçamento de 0,8; 1,0; 1,2 e 1,5 m entre eles. A avaliação da distribuição da calda pulverizada foi realizada em mesa de deposição. Pulverizou-se água com 0,1% do adjuvante não iônico alquilfenol. Os valores observados foram utilizados para a obtenção das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Espaçamento entre pontas; Sobreposição.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200010

DIAGNOSIS AND RECOMMENDATIONS FOR THE BIOCLIMATIC DESIGN OF GRAPE PACKING HOUSES IN HOT AND DRY CLIMATE
Provedor de dados: 70
Autores: Dacanal,Cristiane; Luz,Simone do N.; Turco,Silvia H. N.; Vasconcelos,Osvaldo C. de M.
ABSTRACT The bioclimatic architecture can contribute significantly to moderate thermal environment of agricultural installations, reducing the energy input used in the air conditioning. The present article presents the results of a diagnosis made in packing houses of table grapes, located in a semi - arid region in the Brazilian Northeast. The objective was to verify which strategies of the bioclimatic architecture were applied in the buildings, and also, to propose recommendations for future projects. The methodology consisted of the elaboration of a checklist, from the application of the Mahoney Method and the Brazilian Bioclimatic Zoning, considering Petrolina - PE climate. The checklist was applied in twenty-five packing houses, of three different...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Building design; Building thermal performance; Rural building.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100001

PRODUCTIVE RESPONSES FROM BROILER CHICKENS RAISED IN DIFFERENT COMMERCIAL PRODUCTION SYSTEMS - PART I: FUZZY MODELING
Provedor de dados: 70
Autores: Lourençoni,Dian; Yanagi Junior,Tadayuki; Abreu,Paulo G. de; Campos,Alessandro T.; Yanagi,Silvia de N. M.
ABSTRACT Broiler chickens are classified as homoeothermic animals and require a production environment within well-defined thermal comfort intervals. Therefore, the development of algorithms (mathematical models) to control the environment that can be embedded in microcontrollers becomes necessary. Hence, this work aimed to develop a fuzzy model for predicting the productive performance of broiler chickens as a function of the thermal environment during the various breeding phases. The Mamdani inference and defuzzification methods were used, by means of the gravity center, to develop the fuzzy model. Two hundred and forty-three rules with weighting factors of 1.0 each were elaborated. Three commercial warehouses (conventional system, wind tunnel with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry farming; Productive performance; Artificial intelligence; Fuzzy logic.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100001

Efeito da pressão de trabalho e de modelos de pontas de pulverização sobre a eficiência de herbicida de contato em soja
Provedor de dados: 70
Autores: Boller,Walter; Machry,Marcos.
Nos últimos anos, nas aplicações de herbicidas de contato em pós-emergência, tem-se verificado tendência de redução do volume de calda e a utilização de pontas de pulverização que operam com baixas pressões. Com o objetivo de avaliar pontas de pulverização de jatos planos, das séries Teejet XR, DG, TT e AI, operadas com três níveis de pressão de trabalho, foi conduzido um experimento visando ao controle de picão-preto (Bidens spp.), aplicando-se em pós-emergência da cultura da soja o herbicida de contato bentazon. As pontas de jatos planos das séries Teejet XR 110015, DG 110015 e TT 110015 foram operadas com pressões de 100; 200 e 300 kPa, e a ponta AI 110015, nas pressões de 200; 300 e 400 kPa. Avaliaram-se os níveis de controle das plantas de picão-preto...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Bentazon; Bidens spp.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400015

Evaluation of empirical methods to estimate reference evapotranspiration in Uberaba, State of Minas Gerais, Brazil
Provedor de dados: 70
Autores: Melo,Giovani L. de; Fernandes,André L. T.
Evapotranspiration is the process of water loss of vegetated soil due to evaporation and transpiration, and it may be estimated by various empirical methods. This study had the objective to carry out the evaluation of the performance of the following methods: Blaney-Criddle, Jensen-Haise, Linacre, Solar Radiation, Hargreaves-Samani, Makkink, Thornthwaite, Camargo, Priestley-Taylor and Original Penman in the estimation of the potential evapotranspiration when compared to the Penman-Monteith standard method (FAO56) to the climatic conditions of Uberaba, state of Minas Gerais, Brazil. A set of 21 years monthly data (1990 to 2010) was used, working with the climatic elements: temperature, relative humidity, wind speed and insolation. The empirical methods to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Climatic elements; Empirical equations; FAO Penman-Monteith; Irrigation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500007

Qualidade do corte basal de cana-de-açúcar utilizando-se de três modelos de facas
Provedor de dados: 70
Autores: Voltarelli,Murilo A.; Silva,Rouverson P. da; Cassia,Marcelo T.; Ortiz,Danilo F.; Torres,Luma S.
A colheita mecanizada de cana-de-açúcar é uma tendência crescente e irreversível ao setor canavieiro, devido à sua maior operacionalidade durante os turnos diurno e noturno, em razão das leis ambientais e trabalhistas ligadas a esta operação. Entretanto, o grande desafio deste sistema é a melhoria do mecanismo de corte de base, uma vez que esse mecanismo é capaz de causar elevados índices de danos e abalos nas soqueiras quando associado ao desgaste das facas do mecanismo de corte basal. Diante do exposto, objetivou-se, neste trabalho, avaliar a qualidade do corte basal por meio dos índices de danos e abalos causados às soqueiras, bem como o desgaste de três modelos de facas do mecanismo de corte basal de cana-de-açúcar, em função do tempo de uso. O...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Danos às soqueiras; Controle estatístico de processo; Colheita mecanizada.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300528

IDENTIFICATION OF HOMOGENEOUS RAINFALL ZONES DURING GRAIN CROPS IN PARANÁ, BRAZIL
Provedor de dados: 70
Autores: Lopes,Allan R.; Marcolin,Jonatas; Johann,Jerry A.; Boas,Márcio A. Vilas; Schuelter,Adilson R.
ABSTRACT The aim of this study is to identify homogeneous rainfall zones in the winter and summer 1st and 2nd crops, in the state of Paraná, Brazil. The zones were defined by clustering using the expectation-maximization (EM) algorithm to transform seasonal rainfall series. Monthly average rainfall data collected from 157 weather stations for 20 years (1996 to 2015) were employed. The results show that the number of homogeneous zones varied among growing seasons. The summer crop presented two clusters, with rainfall averages of 1489 and 1925 mm; the second crop presented four clusters, with averages of 1849, 1004, 1454, and 1182 mm; and the winter crop had three clusters, with averages of 969, 1498, and 1171 mm. Clustering was a useful instrument to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Data mining; Clusters; Expectation-maximization; Weka; Soybean; Maize; Wheat.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600707

Influence of urbanization on land surface temperature in Recife city
Provedor de dados: 70
Autores: Santos,Taciana O. dos; Moura,Geber B. de A.; Silva,Bernardo B. da; Oliveira,Leidjane M. M. de; Machado,Celia C. C.
Urbanization has caused significant environmental impacts, replacing natural surfaces by buildings, decreasing green vegetated areas, soil sealing and atmospheric pollution which contribute to increase the land surface temperature in such areas. Thus, this study aimed to analyze the influence of urbanization on land surface temperature (Ts) in Recife city - Pernambuco (PE), in Brazil, using the Thematic Mapper (TM) sensor images from Landsat 5 satellite. To perform the study, images of August 4, 1998 and September 6, 2010 were obtained and processed to generate Ts thematic maps of Recife-PE and of two districts of this city (Curado and Casa Amarela), in order to analyze the transformation dynamics that has occurred in the area. Through the profile produced...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Urban climate; Landsat; Ambient comfort; Thermal infrared.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600016

Análise energética na produção de feno de Cynodon dactylon (L.) Pers
Provedor de dados: 70
Autores: Campos,Alessandro T.; Saglietti,José R. C.; Campos,Aloísio T.; Bueno,Osmar C.
O objetivo do trabalho foi caracterizar o consumo de energia na implantação, condução, fenação e armazenamento, assim como a eficiência energética do Cynodon dactylon (L.) Pers, em sistema intensivo de produção de leite, na região de Coronel Pacheco - MG, sendo utilizados dados coletados pela Embrapa Gado de Leite, em média de sete anos. Para o levantamento dos componentes da matriz, foram utilizados coeficientes energéticos preconizados por autores especializados. A energia direta, relativa aos insumos, teve maior participação que a indireta, sendo os percentuais encontrados de 94,69 e 5,31, respectivamente. O principal consumidor de energia indireta foi o trator, por acionar todos os equipamentos tratorizados, seguido do equipamento de irrigação. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Estruturas e equipamentos; Eficiência energética; Sustentabilidade da agricultura.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000200008

APPLICABILITY OF FINGERPRINTING FOR IDENTIFICATION OF SEDIMENT SOURCES IN A MESOSCALE SEMIARID CATCHMENT
Provedor de dados: 70
Autores: Silva,Eveline M. R. da; Medeiros,Pedro; Araújo,José C. de.
ABSTRACT The study aimed at identifying sediment sources in a mesoscale catchment (933 km2) located in the Brazilian semiarid region. The research explored the potential of using a fingerprinting technique to verify the origin of eroded sediments in a catchment by comparing physical and mineralogical properties of potential sediment sources and sediments deposited in a pond (6 × 103 m3 storage capacity) and a reservoir (20 × 106 m3 storage capacity). The goal was to assess the feasibility of using such material to identify sediment sources in a semiarid environment with a high density of surface reservoirs. Chemical variables were studied by mineralogical analysis using scanning electron microscopy (SEM) and multivariate statistics. The results showed that...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sediment dynamics; Soil physics; Soil mineralogy; Semiarid.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000400553

Análise energética em sistema de produção de suínos com aproveitamento dos desejos como biofertilizante em pastagem
Provedor de dados: 70
Autores: Souza,Cássio V.; Campos,Alessandro T.; Bueno,Osmar C.; Silva,Enilson B.
O objetivo deste trabalho foi estimar a quantidade de energia para a produção de suínos, em ciclo completo, e o balanço energético do sistema com reaproveitamento dos resíduos gerados como biofertilizante, em área de pastagem, utilizando dados médios de cinco ciclos, em granja comercial no município de Diamantina - MG. Quantificou-se o coeficiente energético de cada componente envolvido no processo produtivo de suínos terminados, tratamento dos resíduos e produção de pastagem de Brachiaria decumbens, nas formas de ração, trabalho humano, energia elétrica, máquinas e equipamentos, combustíveis e lubrificantes, instalações, produção de suínos vivos e produção de Brachiaria decumbens. A quantidade média de energia para produzir 1 kg de suíno vivo foi de 53,35...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Suinocultura; Instalações; Tratamento de dejetos; Lagoas de estabilização; Brachiaria decumbens; Energia.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400005

Emerald zoyzia grass development regarding photosynthetically active radiation in different slopes
Provedor de dados: 70
Autores: Coan,Ruchele M.; Turco,José E. P.; Pivetta,Kathia F. L.; Costa,Madson N. da; Mateus,Caroline de M. D'A.
With this study, the objective was to estimate the photosynthetically active radiation (PAR) and to correlate it with the dry matter (MMSPA) of the emerald zoysia (Zoysia japonica Steud.) on surfaces with different expositions and slopes. The research was conducted at the Experimental Watershed of the Agricultural Engineering Department, School of Agriculture and Veterinary Sciences of São Paulo State University (FCAV/UNESP), Brazil, where the surfaces (H, 10 N, 30 N, 50 N, 10 S, 30 S, 50 S, 10 L, 30 L, 50 L, 10 O, 30 O and 50 O) were used. To obtain the global solar radiation, it was installed an automated weather station where the PAR (dependent variable) was obtained by the equation y = a + bx, and the global radiation was independent. To compare means...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zoysia japonica; Slope; Solar radiation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300009

Avaliação de sistema alternativo de automação da irrigação do feijoeiro em casa de vegetação
Provedor de dados: 70
Autores: Queiroz,Tadeu M. de; Carvalho,Jacinto de A.; Rabelo,Giovanni F.; Andrade,Messias J. B.
O presente trabalho teve por objetivo avaliar um controlador alternativo para o manejo automático de sistemas de irrigação com tensiômetros adaptados. Cultivou-se o feijoeiro comum (Phaseolus vulgaris L.) submetido a quatro níveis de déficit hídrico (psi) (15; 30; 45 e 60 kPa) e três métodos de manejo da irrigação (M), sendo dois automatizados, utilizando tensiômetros com vacuômetro de mercúrio (Hg) e tensiômetros com vacuômetro de Bourdon (Vc), ambos adaptados, e o terceiro manejo, convencional, utilizando tensímetro portátil de leitura digital (Ts). Foi avaliado o funcionamento do controlador, a partir do volume de água aplicado e número de acionamentos, a produtividade de grãos e a eficiência de uso da água. Observou-se que tanto o rendimento quanto a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manejo de irrigação; Tensiômetro; Phaseolus vulgaris L.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300008

MODELING OF THE KINETICS OF CRYOGENIC FREEZING OF LIMA BEAN SEEDS AS A FUNCTION OF INITIAL WATER CONTENT
Provedor de dados: 70
Autores: Luciano,Karina M da F.; Mata,Mario E. R. M. Cavalcanti; Fortes,Mauri; Duarte,Maria E. M.
ABSTRACT Cryopreservation is a technique used to preserve genetic material at ultra-low temperatures in cryogenic germplasm banks. In order to enable the cryopreservation of a seed, it is necessary to study its appropriate freezing temperature and its water content, because seeds reach maximum physiological quality with high water contents, and they tolerate drying when they are orthodox seeds, but they may not tolerate cryopreservation. Therefore, the objective of this study was to analyze the influence of initial water content (50 to 10% wet basis) on the kinetic behavior of the lima bean seed at the temperature of −150 °C, in addition to determining changes in its physiological quality (germination and vigor) when cryopreserved (−150 °C) for 30 days...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phaseolus lunatus; Cryogenic; Modeling; Germplasm bank.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300331

Manutenção de tratores agrícolas e condição técnica dos operadores
Provedor de dados: 70
Autores: Reis,Gustavo N. dos; Lopes,Afonso; Furlani,Carlos E. A.; Silva,Rouverson P. da; Grotta,Danilo C. C.; Câmara,Felipe T. da.
A manutenção dos tratores agrícolas pode ser considerada um conjunto de procedimentos que visa a manter o equipamento nas melhores condições de funcionamento, propiciando aumento da vida útil, evitando danos prematuros, eliminando os já observados e concorrendo para maior segurança no trabalho. Essa conduta, apesar de simples, exige atenção e cuidado semelhante ou até maior quando comparado a outro veículo automotor. O presente trabalho teve por objetivo analisar a regularidade e a qualidade da manutenção dos tratores da Fazenda de Ensino, Pesquisa e Produção da UNESP - Jaboticabal, utilizados para os mais variados tipos de trabalho, como aração, gradagem, pulverização e jardinagem, e avaliar a condição técnica dos operadores responsáveis pelas máquinas....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Máquinas agrícolas; Vida útil; Manutenção preventiva.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100031

Uso da termografia infravermelha na análise da termorregulação de cavalo em treinamento
Provedor de dados: 70
Autores: Moura,Daniella J. de; Maia,Ana Paula de A; Vercellino,Rimena do A; Medeiros,Brenda B. L; Sarubbi,Juliana; Griska,Paulo R.
O estresse térmico em equinos aciona mecanismos termorregulatórios, como mudanças no fluxo sanguíneo periférico, para a manutenção da homeostase corporal. A termografia infravermelha permite detectar estas alterações, sendo uma ferramenta útil para avaliar o estresse em animais. Assim, o objetivo deste estudo foi avaliar o uso da termografia infravermelha na termorregulação de equino em condição de treinamento. Foi utilizado um cavalo anglo-árabe, exercitado uma vez ao dia. Foram captadas imagens termográficas da axila, garupa, peito e virilha do cavalo e registrados os parâmetros fisiológicos antes e após exercício e 0; 5 e 10 minutos após o banho, durante 8 dias. A temperatura, a umidade relativa e a velocidade do ar foram monitoradas. A temperatura de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Equinos; Estresse térmico; Parâmetros fisiológicos; Temperatura de superfície.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100003

Uso de redes neurais artificiais na identificação de vocalização de suínos
Provedor de dados: 70
Autores: Nääs,Irenilza de A.; Campos,Leonardo S. L.; Baracho,Marta dos S.; Tolon,Yamilia B.
O bem-estar dos animais tem sido importante tópico de pesquisa na produção animal, principalmente no tocante às formas de sua avaliação. Na avaliação do bem-estar animal, a vocalização mostra-se como ferramenta interessante, por fornecer dados de forma não-invasiva, podendo também ser facilmente automatizada. O presente trabalho teve o objetivo de implementar algoritmo baseado em redes neurais artificiais, capaz de reconhecer vocalizações relacionadas com padrões indicativos de bem-estar. A pesquisa teve duas partes, sendo a primeira o desenvolvimento do algoritmo, e a segunda, sua validação com dados de campo. Registros prévios permitiram o desenvolvimento do algoritmo, a partir de comportamentos observados em porcas alojadas em gaiolas de maternidade. O...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bem-estar animal; Leitões; Análise de sinais.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200001

A NOVEL RAISIN SEGMENTATION ALGORITHM BASED ON DEEP LEARNING AND MORPHOLOGICAL ANALYSIS
Provedor de dados: 70
Autores: Zhao,Yun; Guindo,Mahamed L.; Xu,Xing; Shi,Xiang; Sun,Miao; He,Yong.
ABSTRACT We propose a segmentation algorithm for raisin extraction. The proposed approach consists of the following aspects. Deep learning is used to predict the number of raisins in each connected region, and the shape features such as the roundness, area, X-axis value for the centroid, Y-axis value for the centroid, axis length and perimeter of each region will be used to establish the prediction model. Morphological analysis, based on edge parameters including the polar axis, polar angle and angular velocity, is applied to search for the suitable break points that are useful for identifying the dividing lines between two adjacent raisins. To make our segmentation more accurate, some machine-learning algorithms such as the random forest (RF), support...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Raisin extraction; Segmentation algorithm; Deep learning; Image analysis; Food quality grading.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500639

Índice fuzzy de conforto térmico para frangos de corte
Provedor de dados: 70
Autores: Nascimento,Guilherme R. do; Pereira,Danilo F.; Näas,Irenilza de A.; Rodrigues,Luiz H. A.
A estimativa de conforto térmico na avicultura moderna é importante para que sistemas de climatização possam ser acionados no tempo correto, diminuindo perdas e aumentando rendimentos. Embora a literatura corrente apresente alguns índices de conforto térmico, que são aplicados para essa estimativa, estes são baseados apenas em condições do ambiente térmico e não consideram fatores importantes inerentes aos animais, tais como genética e capacidade de aclimatação, provendo, geralmente, uma estimativa inadequada do conforto térmico das aves. Este trabalho desenvolveu o Índice Fuzzy de Conforto Térmico (IFCT), com o intuito de estimar o conforto térmico de frangos de corte, considerando que o mecanismo usado pelas aves para perda de calor em ambientes fora da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Índice de conforto térmico; Lógica Fuzzy; Termografia infravermelho; Zootecnia de precisão.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200002

Soil water potential during different phenological phases of coffee irrigated by center pivot
Provedor de dados: 70
Autores: Evangelista,Adão W. P.; Lima,Luiz A.; Silva,Antônio C. da; Martins,Carla de P.; Ribeiro,Moisés S.
Irrigation management can be established, considering the soil water potential, as the limiting factor for plant growth, assuming the soil water content between the field capacity and the permanent wilting point as available water for crops. Thus, the aim of this study was to establish the soil water potential interval during four different phenological phases of coffee irrigated by center pivot. The experiment was set at the experimental area of the Engineering Department at the Federal University of Lavras, in Brazil. The coffee variety planted is designated as Rubi, planted 0.8 meters apart, with rows spaced 3.5 meters apart. The treatments corresponded to the water depths applied based on different percentages of Kc and reference evapotranspiration...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigated coffee; Available water; Coffea arabica L.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200006

Periodic inspection of sprayers: diagnostic to the northern of Paraná
Provedor de dados: 70
Autores: Gandolfo,Marco A.; Antuniassi,Ulisses R.; Gandolfo,Ulisses D.; Moraes,Eder D. de; Rodrigues,Eurípedes B.; Adegas,Fernando S.
To optimize the use of pesticides, several countries have carried out periodic inspections in agricultural sprayers. In Brazil, knowing the conditions of this machinery canguide researches and investments in guidelines for its use and maintenance. The objective of this study was to verify the state of sprayer maintenance used in the North of the state of Paraná, in Brazil. Several sprayer items were evaluated, such as: presence, status and scale of the manometer, status of the hose, status of the anti-drip component, presence of leaks, status of the bar, status of the filters, state of the spraying nozzles and errors in the targeted flow rate. Machines were named as approved when there was no failure in any item evaluated. The factor that caused the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Periodic inspection; Sprayer; Quality of application.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200019

Método de avaliação de equipamentos para direcionamento de veículos agrícolas e efeito de sinais de GNSS
Provedor de dados: 70
Autores: Molin,José P; Povh,Fabricio P; Paula,Vanderson R. de; Salvi,José V.
Pesquisas indicam que o uso de novas técnicas no campo da mecanização agrícola, como o tráfego controlado por meio de direcionamento com auxílio de Sistemas de Navegação Global por Satélites (GNSS), pode diminuir as exigências por energia associadas às operações de campo e aumentar a produtividade da mão de obra e da cultura. Alguns autores já utilizaram diferentes metodologias para avaliar erros de paralelismo em sistemas de orientação de veículos, porém não há um procedimento-padrão para medi-los. Sendo assim, o objetivo deste trabalho foi implementar uma planilha eletrônica específica, determinar e comparar a acurácia no paralelismo de dois sistemas distintos de orientação de veículos (uma barra de luz e um piloto automático com atuador de volante) em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sistemas de orientação; Piloto automático; GPS.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100012

Cultivo de flores com o uso de água residuária e suplementação mineral
Provedor de dados: 70
Autores: Medeiros,Salomão de S.; Gheyi,Hans R.; Soares,Frederico A. L.
Este trabalho visa a avaliar o efeito da adubação nitrogenada e potássica na produção de gérbera (Gerbera jamesonni), tipo comercial Rambo, utilizando-se de dois tipos de águas (residuária de origem urbana e de abastecimento) para irrigação. O experimento foi realizado em casa de vegetação, na Universidade Federal de Campina Grande, de outubro de 2006 a janeiro de 2007, abrangendo um ciclo completo de produção. O delineamento experimental utilizado foi o de blocos casualizados, com três repetições, e os tratamentos foram dispostos em esquema fatorial 3 x 4 x 2, em que os fatores estudados foram: níveis crescente de nitrogênio (N1 = 100; N2 = 200 e N3 = 300 mg L-1) e potássio (K1 = 100; K2 = 200; K3 = 300 e K4 = 400 mg L-1) adicionados a uma solução...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reúso; Irrigação; Adubação; Gerbera jamesonni.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600008

SELECTION OF EFFECTIVE SOFTWARE FOR THE ANALYSIS OF THE FRACTIONAL COMPOSITION OF THE CHAOTIC SEED LAYER USING THE EXAMPLE OF OILSEED RADISH
Provedor de dados: 70
Autores: Tsytsiura,Yaroslav.
ABSTRACT This article generalises the peculiarities and efficiency of the use of three software packages, Digimizer image analysis software (v. 4.2), ImageJ2 version 2.0.0-rc-64 and WipFrag 3.3.14.0. These packages were used in studying the fractional composition of oilseed radish seeds for scanning in the mode of single-layer inseparable placement. The generalisation of the main caveats and features of the effective use of each of the software packages is made on the basis of detailed analysis of the features of each of package in the use to the features of the scan and the obtained scanned image The above-mentioned aspects are illustrated in detail and reservations about the options for the effective use of each package are represented. The efficiency...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fractional composition; Image analysis; Oilseed radish; Scanning; Seeds.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000200161

EFFECT OF THE MIST MICRO-SPRAY TIME ON PHOTOSYNTHETIC SPATIAL HETEROGENEITY OF GRAPE CANOPY
Provedor de dados: 70
Autores: Zheng,Ming; Bai,Yungang; Zhang,Jianghui; Liu,Hongbo; Ding,Ping.
ABSTRACT In grape, high temperatures and low humidity prolong midday depression of foliar photosynthesis and dramatically reduce fruit yield. In this study, we explored the effects of various mist micro-spray treatments on grape photosynthesis at a test site in Shanshan County (N, 42.91°; E, 90.30°), Turpan, Xinjiang, China. We tested four different mist micro-spray durations including 1 h (WP1), 2 h (WP2), 3 h (WP3), and 0 h (CK). WP1, WP2, and WP3 affected canopy air temperature and humidity for 5 h, 7 h, and 9 h, respectively. At 12:30, WP1, WP2, and WP3 had the strongest cooling effect and altered temperature by −5.12 °C, −5.09 °C, and −5.17 °C respectively. The relative chlorophyll content was higher in the upper than the lower canopy leaves. There...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Air temperature; Chlorophyll; Photosynthesis; Stomatal conductance; Transpiration rate.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100039

Silting in the dense reservoir network of the Pereira de Miranda catchment
Provedor de dados: 70
Autores: Lira,Daniely; Toledo,Cristian; Mamede,George.
This study aims to analyze the impacts of the reservoir network within Pereira de Miranda - CE catchment (also called Pentecoste) over sediment transport and storage capacity of the system. The survey of the "damming" was carried out using satellite images. We identified 502 erosion units, derived from overlaying maps of the Universal Soil Loss Equation parameters, which allowed the estimation of localized erosion in the basin and identification of areas potentially generating sediment. In order to estimate silting in Pentecoste reservoir, different system structure scenarios were considered. An average erosion rate of 59 t ha-1year-1 was estimated. According to the model, the silting of Pentecoste reservoir may vary from 1.1 to 2.6% per decade, depending...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sediment generation; Sediment retention in reservoirs; Semiarid.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400007

Influência de rotações de culturas nas propriedades físico-hídricas de um Latossolo Vermelho em plantio direto
Provedor de dados: 70
Autores: Cunha,Eurâimi de Q.; Balbino,Luiz C.; Stone,Luís F.; Leandro,Wilson M.; Oliveira,Geraldo C. de.
A adoção do plantio direto, com a inclusão de espécies gramíneas de relação C/N alta, poderá minimizar a degradação estrutural do solo. O objetivo deste trabalho foi avaliar a influência da inclusão da braquiária na rotação de culturas nas propriedades físico-hídricas e no conteúdo de matéria orgânica de um Latossolo Vermelho distrófico em plantio direto. O delineamento experimental foi o de blocos ao acaso, em parcelas subdivididas, com quatro repetições. As parcelas foram compostas por quatro sistemas de rotação, e as subparcelas, por quatro profundidades de amostragem (0-10; 10-20; 20-40, e 40-60 cm). As culturas utilizadas foram: arroz (A); feijão irrigado (F); milho (M); soja (S), e arroz (A+B), milho (M+B) e soja (S+B) consorciados com braquiária. Os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Densidade do solo; Porosidade do solo; Agregação do solo.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400009

STUDY OF THE EFFECTS OF ADJUVANTS ASSOCIATED WITH INSECTICIDES ON THE PHYSICOCHEMICAL PROPERTIES OF THE SPRAY SOLUTION AND CHARACTERIZATION OF DEPOSITS ON WHEAT AND MAIZE LEAVES UNDER SIMULATED RAIN
Provedor de dados: 70
Autores: Melo,Adriano A.; Hunsche,Mauricio; Guedes,Jerson V. C.; Hahn,Lucas; Feltrin,Natalie M.
ABSTRACT The association of adjuvants with phytosanitary products has been tested for several years but is commonly recommended without considering technical and scientific criteria. This study aimed to evaluate the influence of the association of insecticides with different adjuvants on surface tension, contact angle, coverage, hydrogen ionic potential (pH), and the formation of deposits exposed to rain. The insecticides thiamethoxam, imidacloprid, and lambda-cyhalothrin were tested at doses of 75 g ha−1, 150 g ha−1, and 150 g ha−1, respectively, with a spray volume of 200 L ha−1. Break-Thru 240®, Break-Thru 233®, Break-Thru Union®, Oleo FC Agraröl®, and Naturo'il® were added to each of these spray solutions. The results showed that the addition of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Surface tension contact angle potential of hydrogen (pH) coverage; And deposit.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300315

Níveis de déficit hídrico em diferentes estádios fenológicos da cultura da berinjela (Solanum melongena L.)
Provedor de dados: 70
Autores: Carvalho,Jacinto de A.; Santana,Márcio J. de; Pereira,Geraldo M.; Pereira,Joelma R. Durão; Queiroz,Tadeu M. de.
Os efeitos de diferentes níveis de déficit hídrico, aplicados em dois estádios fenológicos da cultura da berinjela, foram avaliados por meio de um experimento conduzido em casa de vegetação, no Departamento de Engenharia, da Universidade Federal de Lavras, em Lavras - MG. Utilizou-se um delineamento experimental inteiramente casualizado em esquema fatorial 2 x 4, sendo duas fases fenológicas (pós-transplante/abertura da gema floral e formação de frutos/colheita) e quatro níveis de déficit hídrico (100; 80; 60 e 40% da evapotranspiração), totalizando oito tratamentos, com seis repetições. Avaliaram-se o diâmetro de caule, altura das plantas e número de folhas em diferentes épocas, produção e número de frutos. Os resultados mostraram que a produção e o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Manejo de água; Irrigação; Estresse hídrico.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200010

Intermitência do sistema de resfriamento adiabático evaporativo por aspersão em instalação para vacas em lactação
Provedor de dados: 70
Autores: Matarazzo,Soraia V.; Silva,Iran J. O. da; Perissinotto,Mauricio; Fernandes,Dérgio A. de A.
Teve-se o objetivo de avaliar o período de intermitência de acionamento do sistema de resfriamento adiabático evaporativo (SRAE) por aspersão na linha de alimentação, em instalação do tipo freestall e sua influência no conforto térmico de vacas em lactação. Foram utilizadas 12 vacas multíparas com produção média de 30 kg de leite por dia. Os tratamentos corresponderam às intermitências de 12; 14 e 16 min, e os dados referentes à temperatura do bulbo seco (TBS), umidade relativa do ar (UR) e temperatura de globo negro (TGN), no interior da instalação e no ambiente externo, foram mensurados ao longo das 24 h durante todo o período experimental. A freqüência respiratória (FR), temperatura retal (TR) e temperatura do pelame (TP) foram medidas às 13; 14; 15 e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência; Vacas em lactação; Conforto térmico.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300001

Spatial influence of physical and chemical parameters on management zone definition in apple orchards
Provedor de dados: 70
Autores: Gebler,Luciano; Grego,Celia R.; Vieira,Abel L.; Kuse,Leonardo da R.
ABSTRACT Precision agriculture adoption in Brazilian apple orchards is still incipient. This study aimed at evaluating the spatial variability of certain soil properties as soil density, soil penetration resistance, electrical conductivity, yield, and fruit quality in an apple orchard through digital mapping, as well as assessing the correlation between these factors by means of geostatistics, establishing management zones. Forty representative points were set within 2.5 hectares of apple orchard, wherein soil samples were collected and analyzed, besides measurements of fruit quality (Brix degree, size or diameter, pulp firmness and color) to generate an overall index quality. We concluded that the fruit quality indexes, when isolated, did not show strong...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Apple trees; Precision fruit-growing; Electrical conductivity in orchards.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601160

Avaliação econômica da elaboração de banana-passa proveniente de cultivo orgânico e convencional
Provedor de dados: 70
Autores: Bittencourt,Jefferson; Queiroz,Marlene R. de; Nebra,Silvia A.
Neste trabalho, foi realizada a avaliação econômica da produção de banana-passa de uma agroindústria localizada no município de Guaraqueçaba - PR. Foi avaliado o processamento da banana-passa convencional e da banana orgânica produzida na região, comparando-se os indicadores de viabilidade econômica. A banana-passa orgânica é exportada para a Europa e a banana-passa convencional é comercializada na região de Curitiba - PR. Ambos os processamentos apresentaram viabilidade econômica positiva, apresentando a banana-passa orgânica os melhores índices (TIR 94%, VPL R$ 486.009,39 e relação benefício-custo de 2,11) do que a banana-passa convencional (TIR 14%, VPL R$ 34.668,00 e relação benefício-custo de 1,17). A banana-passa orgânica apresentou um custo de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agroindústria; Secagem; Viabilidade econômica.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200028

Relations between communication and development of family farmers
Provedor de dados: 70
Autores: Ponchio,Ana Paula S.; Oliveira,Julieta T. A. de.
This research investigates relations between communication and the development of family farmers from the Pontal do Paranapanema region (state of São Paulo), mainly in the municipality of Teodoro Sampaio. Family agriculture in this municipality is represented basically by beneficiaries the Agrarian Reform program. The main hypothesis is that communication contributes positively to the development of those family farmers. Thus, this study aimed to understand communication practices of these farmers and relate them with the development of their families. Quantitative and qualitative research methods were used. Development proxy is understood as the combination between the family living conditions and production. Among the main results, it was found that the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Access to information; Dialogue; Agrarian reform; Pontal do Paranapanema region.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000600022

Root system distribution of sugarcane irrigated with domestic sewage effluent aplication by subsurface drip system
Provedor de dados: 70
Autores: Sousa,Allan C. M. de; Matsura,Edson E.; Elaiuy,Marcelo L. C.; Santos,Leonardo N. S. dos; Montes,Célia R.; Pires,Regina C. de M.
Irrigation with domestic sewage effluent (DSE) has been recommended by subsurface dripping, as it can obtain a high rate of irrigation efficiency and faster use of salts in comparison with other irrigation methods. The study aimed at evaluating the area, the length and the effective depth of the root system of sugarcane irrigated with DSE by subsurface drip system and with different irrigation rates at depths of 0.00-0.20, 0.20-0.40, 0.40-0.60 and 0.60-0.80m. The experiment was carried out in the municipality of Piracicaba, in the state of São Paulo (SP), Brazil, in a sugarcane area irrigated with DSE in a completely randomized blocks set up in furrows, with three replications and four treatments, which are: one area without irrigation (AWI) and three...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Root; Water reuse; Subsurface drip.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400006

Simulação das perdas de água por evaporação e arraste, no aspersor NY-7 (4,6 mm x 4,0 mm), em sistemas de aspersão convencional
Provedor de dados: 70
Autores: Beskow,Samuel; Colombo,Alberto; Ribeiro,Moisés S.; Ferreira,Liamara S.; Rossi,Raitanni.
As perdas de água por evaporação e arraste em sistemas de irrigação por aspersão podem assumir valores consideráveis, reduzindo a eficiência do sistema. Os objetivos do presente trabalho foram avaliar a capacidade preditiva de cinco modelos empíricos para estimar perdas de água por evaporação e arraste em aspersores modelo NY-7 (bocais de 4,6 mm x 4,0 mm), trabalhando sob diferentes condições operacionais e ambientais, e ajustar modelos específicos para o aspersor NY-7. Comparando os resultados medidos em ensaios de campo, com os resultados simulados, foi possível concluir que os cinco modelos empíricos considerados apresentaram pouca ou nenhuma adequação, tanto para os ensaios com um único aspersor (quadrado do erro-médio de 5,27; 20,70; 5,07; 6,95 e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelos empíricos; Eficiência de irrigação; Modelagem matemática.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300004

Fuzzy modeling of broiler performance, raised from 1 to 21 days, subject to heat stress
Provedor de dados: 70
Autores: Abreu,Lucas H. P.; Yanagi Junior,Tadayuki; Fassani,Édison J.; Campos,Alessandro T.; Lourençoni,Dian.
ABSTRACT Given the need to obtain systems to better control broiler production environment, we performed an experiment with broilers from 1 to 21 days, which were submitted to different intensities and air temperature durations in conditioned wind tunnels and the results were used for validation of afuzzy model. The model was developed using as input variables: duration of heat stress (days), dry bulb air temperature (°C) and as output variable: feed intake (g) weight gain (g) and feed conversion (g.g-1). The inference method used was Mamdani, 20 rules have been prepared and the defuzzification technique used was the Center of Gravity. A satisfactory efficiency in determining productive responses is evidenced in the results obtained in the model...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fuzzy logic; Animal environment; Poultry.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000600967

WATER RELATIONS AT THE INITIAL SUGARCANE GROWTH PHASE UNDER VARIABLE WATER DEFICIT
Provedor de dados: 70
Autores: Mauri,Robson; Coelho,Rubens D.; Fraga Junior,Eusímio F.; Barbosa,Fernando Da S.; Leal,Daniel P. V.
ABSTRACT This study aimed to quantify water deficit levels that compromise sugarcane initial growth exposed to different availability soil depths. The experiment was conducted in a greenhouse by using 100-liter capacity asbestos-cement boxes filled with different soil layers simulating depths of 10, 20, 30, and 40 cm. Water deficit levels were represented by accumulated reference evapotranspiration of 0, 40, 80, 120, 160, 200, 240, and 280 mm, which was considered from planting to irrigation return. Soil moisture at field capacity at planting time was sufficient to promote sprouting and emergence regardless the water deficit level that was subsequently exposed. For soil depths of 10 and 20 cm, a 160-mm water deficit level caused total plant death. On the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Sprouting; Saccharum spp.; Growth.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200268

Raw water use charge reduction for the rural sector in the PCJ Watershed
Provedor de dados: 70
Autores: Silva,Rogério T. da; Folegatti,Marcos V.
The deficient environmental preservation on agricultural properties has reflected in great soil losses for erosion and the high rate of sedimentation. Therefore, this work brings the application of software to demonstrate that planters can get benefits by the conservationist practices. The benefits will be obtained from the environment aspect (erosion and sedimentation control), as well as economical aspect (financial incentives). A proposal has been created by the Technical Chamber of Rural Water Use and Conservation (CT-Rural) to estimate the reduction in raw water use charge for the rural water users of the PCJ Watershed - this reduction is being possible since January 2007, at the PCJ Committee. The software develops a simple relationship, so that if...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Software; Conservation practice; Watershed committee; Raw water use charge.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300016

Sensoriamento remoto e geoprocessamento aplicados ao uso da terra em microbacias hidrográficas, Botucatu - SP
Provedor de dados: 70
Autores: Campos,Sérgio; Araújo Júnior,Armindo A.; Barros,Zacarias X.; Cardoso,Lincoln G.; Piroli,Edson L.
O presente trabalho teve como objetivo identificar e quantificar o uso da terra em dez microbacias ocorrentes na bacia do Rio Capivara, município de Botucatu - SP, a partir da estruturação de um banco de dados utilizando o Sistema de Informações Geográficas (SIG) - IDRISI. Os resultados mostram que as classes de uso da terra, "uso agrícola" e "pastagem", foram as mais significativas, pois ocuparam mais da metade da área das microbacias. O alto índice de uso da terra por pastagens, capoeiras, reflorestamento e matas reflete a predominância de solos arenosos com baixa fertilidade. As imagens obtidas do satélite LANDSAT 5 permitiram o mapeamento do uso da terra de maneira rápida, além de fornecer um excelente banco de dados para futuro planejamento e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Imagem de satélite; SIG-IDRISI; Conservação do solo.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200023

Influence of distance, geometry and number of control stations on quality of local geodetic networks for the purpose of georeferencing of rural properties
Provedor de dados: 70
Autores: Rosalen,David Luciano.
The implementation of local geodetic networks for georeferencing of rural properties has become a requirement after publication of the Georeferencing Technical Standard by INCRA. According to this standard, the maximum distance of baselines to GNSS L1 receivers is of 20 km. Besides the length of the baseline, the geometry and the number of geodetic control stations are other factors to be considered in the implementation of geodetic networks. Thus, this research aimed to examine the influence of baseline lengths higher than the regulated limit of 20 km, the geometry and the number of control stations on quality of local geodetic networks for georeferencing, and also to demonstrate the importance of using specific tests to evaluate the solution of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: GNSS baseline Law 10; 267/2001.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200012

ESTIMATION OF THE KINETIC HEAD COEFFICIENT (k) BASED ON THE GEOMETRIC CHARACTERISTICS OF EMITTER PIPES
Provedor de dados: 70
Autores: Flores,José H. N.; Rettore Neto,Osvaldo; Faria,Lessandro C.; Timm,Luís C.
ABSTRACT: The objective of this study was to determine the variability of the head loss as a function of the emitter geometry as well as to develop a relation between local head loss caused by the emitter insertion and geometric characteristics of the emitter pipe, using index of obstruction for dripper pipes with non-coaxial emitters. For this, an experimental bench was developed to control the system and obtain the variables pertinent to the study. From the value of the total head loss in the emitter pipe and the value obtained with calculation of the distributed head loss in the pipe, the difference of these values was local head loss caused by the insertion of the emitter. Total head loss in the emitter pipe and local head loss on the emitter presented...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Non-coaxial emitters; Obstruction index; Trickle irrigation; Head loss.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601091

Longitudinal distribution of bean seeds in horizontal plate meter operating with one or two seed outlets
Provedor de dados: 70
Autores: Teixeira,Sandro S.; Reis,Ângelo V. dos; Machado,Antônio L. T.
This study aimed to evaluate the effect of horizontal plate meter with oblong holes operating with one or two seed outlets at different speeds over the accuracy of longitudinal distribution of common bean seeds (Phaseolus vulgaris L.). The experiment was performed in laboratory using the meter with one and two seed outlet points in relation to ten tangential disk plate speeds (0.03 to 0.30 m s-1). It was used a complete randomized design with four replications, summing up 80 experimental treatments. Tangential speed quantitative factor was estimated through a 2nd order polynomial regression. There was no significant difference in the behavior of the seed meter operating with one or two outlets in the metering of bean seeds in all tested speeds, with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural mechanization; Precision planters; Percentage of single.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300013

A MEASUREMENT SYSTEM BASED ON LiDAR TECHNOLOGY TO CHARACTERIZE THE CANOPY OF SUGARCANE PLANTS
Provedor de dados: 70
Autores: Canata,Tatiana F.; Molin,José P.; Sousa,Rafael V. de.
ABSTRACT Laser sensor applications associated with LiDAR (Light Detection and Ranging) technology on platforms allow the evaluation of crop and forest biomass in a non-invasive way. This study presents the development of a measurement system based on LiDAR technology aimed at the proposed assessment of the height of sugarcane plants during the pre-harvest period. A laser sensor, a GNSS (Global Navigation Satellite System) receiver, and an inertial unit compose the measurement system. The equipment was integrated with a computer for data acquisition and installed on an agricultural tractor platform. The GNSS receiver with a real-time kinematic signal was synchronized to the laser sensor to obtain the point cloud and to the inertial unit to evaluate the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Canopy geometry; Instrumentation; Laser sensor; Remote sensing.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200240

PARAMETERS OF OPERATIONAL PERFORMANCE OF SOIL PREPARATION AND SEMI-MECHANIZED TRANSPLANTATION OF COFFEE SEEDLING
Provedor de dados: 70
Autores: Cunha,João P. B.; Silva,Fabio M. da; Andrade,Ednilton T.; Barros,Murilo M. de.
ABSTRACT In recent years, the coffee has undergone major changes, and in case of transplanting operation, the use of machinery has proved to be a viable alternative to producers. Prior knowledge of the influence of the variables that influence the operational capability of these machines can generate models to estimate precisely these parameters, thus enabling the optimization and management of mechanized operations. One of this tool is the use of the response surface methodology, which allows checking the influence of different independent variables and the response generated to allow a great value. This study aims to verify the use of the response surface method to determine parameters of mechanized operations in coffee plant implantation. The results...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mechanization; Planting seedlings; Coffea Arabica.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600910

Balanço de energia e estimativa da evapotranspiração em culturas irrigadas de maracujazeiro pelo método da razão de Bowen
Provedor de dados: 70
Autores: Silva,Tonny J. A.; Folegatti,Marcos V.; Silva,Cláudio R.; Alves Júnior,José; Bonfim-Silva,Edna M.
A cultura do maracujazeiro-amarelo tem tido grande expansão da área cultivada no Estado de São Paulo e, apesar da importância da irrigação para a cultura, há poucos estudos sobre sua utilização. Este trabalho foi realizado na área experimental de irrigação, na Fazenda Areão, do Departamento de Engenharia Rural, da Escola Superior de Agricultura "Luiz de Queiroz" - ESALQ/USP (Piracicaba - SP). Foram coletados dados de saldo de radiação, fluxo de calor no solo, gradientes de temperatura e pressão de vapor do ar com o objetivo de avaliar a partição da energia disponível e a evapotranspiração em cultivo de maracujazeiros em dois sistemas de plantio (linhas de cultivo norte-sul e leste-oeste). O método da razão de Bowen foi utilizado na determinação dos fluxos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Fluxo de calor latente e sensível; Micrometeorologia.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300008

QUALITY OF CAGAITA POWDER BY FOAM LAYER DRYING METHOD AND DIFFERENT FOAMER AGENTS
Provedor de dados: 70
Autores: Cavalcante,Maisa D.; Belisário,Celso M.; Oliveira,Daniel Emanuel C. de; Maia,Geisa Priscilla A. G.
ABSTRACT One of the factors that hinder the usability of Cerrado fruits is their perishable nature, requiring industrial processing to ensure prolonged shelf life. This study aims to determine the optimal foaming agent for industrial processing of this fruit, and to evaluate the physicochemical characteristics and antioxidant activity of dried cagaita powder (Eugenia dysenterica DC) in foam layers at temperatures of 40, 50, 60, and 70 °C. The effectiveness of three foaming agents at various concentrations were tested, and suitable agents were identified based on a factorial analysis of density, expansion, and stability. The physicochemical characteristics of the powder, along with its vitamin A and C and total carotenoid content and antioxidant activity,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cerrado fruits; Cagaita powder; Bioactive compounds; Antioxidant activity; Vitamin C; Vitamin A; Carotenoids; Foam layer drying.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300381

Avaliação de métodos de estimativa da evapotranspiração horária para alface cultivada em sistema hidropônico em ambiente protegido
Provedor de dados: 70
Autores: Moura,Carlos R. W.; Zolnier,Sérgio; Ribeiro,Aristides; Oliveira,Rubens A. De.
O objetivo deste trabalho foi avaliar a precisão e a exatidão de métodos de estimativa de valores horários de evapotranspiração (ETc) para alface cultivada em sistema hidropônico sob ambiente protegido. Para a determinação dos parâmetros pertinentes aos diferentes métodos de estimativa e sua posterior validação, foram utilizados dois conjuntos de dados experimentais obtidos a partir de medições realizadas nas cultivares Grand Rapids, Regina e Great Lakes. As estimativas de evapotranspiração foram realizadas com os seguintes métodos: Penman-Monteith parametrizado pela FAO, em 1998 (PMF); Penman-Monteith modificado para condições aerodinâmicas características de ambiente protegido (PMAP); Penman-Monteith modificado para ambiente protegido simplificado...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cultivo protegido; Horticultura; Técnica de circulação laminar de nutrientes.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400009

Effect of companion ion on nitrate displacement through transport parameters analysis
Provedor de dados: 70
Autores: SILVA,LÍVIA P. DA; MIRANDA,JARBAS H. DE; OLIVEIRA,LUCIANO A.; JOSÉ,JEFFERSON V.
Nitrate is the main form of nitrogen associated with water contamination; the high mobility of this species in soil justifies the concern regarding nitrogen management in agricultural soils. Therefore, the objective of this research was to assess the effect of companion cation on nitrate displacement, by analyzing nitrate transport parameters through Breakthrough Curves (BTCs) and their settings made by numerical model (STANMOD). The experiment was carried out in the Soil and Water Quality Laboratory of the Department of Biosystems Engineering, "Luiz de Queiroz" College of Agriculture in Piracicaba (SP), Brazil. It was performed using saturated soil columns in steady-state flow condition, in which two different sources of inorganic nitrate Ca(NO3)2 and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Breakthrough curves; Solute dynamics; Leaching.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100051

Desenvolvimento e produtividade da cultura da batata irrigada por gotejamento em dois sistemas de cultivo
Provedor de dados: 70
Autores: Silva,João A.; Pires,Regina C. M.; Sakai,Emilio; Silva,Tonny J. A.; Andrade,José E.; Arruda,Flávio B.; Calheiros,Rinaldo O.
O presente trabalho avalia o desenvolvimento e a produtividade da cultura da batata cv. Monalisa, irrigada por gotejamento, conduzida em parcelas com o plantio tradicional em linhas simples (LS), espaçadas de 0,75 m, e em linhas duplas (LD), com espaçamentos alternados de 0,60 e 0,90 m, dispostos em blocos ao acaso, com oito repetições. O cultivo em LS recebeu uma linha de tubogotejador por linha de plantas, enquanto no cultivo em LD, o tubogotejador foi instalado entre as linhas de menor espaçamento. O plantio da batata foi realizado em 19 de abril de 2005, e a colheita, em 15 de agosto de 2005, em Itobi - SP, sendo a mesma densidade de plantio nos dois tratamentos. A matéria seca da parte aérea e o índice de área foliar não diferiram estatisticamente nos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Manejo da água; Solanum tuberosum L.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300004

REGIONALIZATION OF MAXIMUM AND MINIMUM FLOW IN THE TELES PIRES BASIN, BRAZIL
Provedor de dados: 70
Autores: Lopes,Tárcio R.; Zolin,Cornélio A.; Prado,Giuliani do; Paulino,Janaína; Almeida,Frederico T. de.
ABSTRACT In a watershed there is space and climate variability within its catchment area, causing changes in water qualitative and quantitative characteristics. Thus, the hydrological data collected from a specific basin may be extrapolated to neighboring basins with similar physical characteristics, using techniques of hydrological regionalization. This study developed the flow regionalization in the Teles Pires Basin, using historic series and probabilistic models to verify the data adherence through the regression equations adjustment according to the hydrologically homogeneous regions. The linear and power regression models were tested, employing physical and climatic characteristics and then the best adjustments were selected based on coefficients of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydrological regionalization; Natural flow; Water resources management.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100054

Qualidade da aplicação aérea líquida com uma aeronave agrícola experimental na cultura da soja (Glycine Max L.)
Provedor de dados: 70
Autores: Reis,Elton F. dos; Queiroz,Daniel M. de; Cunha,João P. A. R. da; Alves,Sueli M. F.
Os avanços da tecnologia de aplicação aérea de agroquímicos têm-se dado na direção de redução do volume de calda, o que pode ocasionar má distribuição e consequente deposição irregular. O presente trabalho teve como objetivo avaliar a qualidade da aplicação de calda de pulverização em aplicação aérea, na cultura da soja (Glycine Max L.). Para a aplicação, foi utilizada uma aeronave agrícola experimental, aplicando um volume de calda de 20 L ha-1 . Para a determinação dos volumes depositados nas folhas do terço superior, médio e inferior das plantas de soja, foi utilizado corante alimentício azul brilhante adicionado à calda de pulverização. Estas folhas foram lavadas, e o volume determinado por espectrofotometria. Para a obtenção do espectro de gotas,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Aviação agrícola; Controle estatístico.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500017

Influences of two CO2 concentrations and water availability on bean crop
Provedor de dados: 70
Autores: Silva,João B. L. da; Ferreira,Paulo A.; Pires,Luanna C.; Pereira,Eduardo G.; Carneiro,José E. S.
This study was carried out to determine some physiological and phenological responses of the bean under high [CO2] and drought stress. The experiment was conducted from April to July 2009 in Viçosa, Brazil. The open-top chambers were used to enrich the air with CO2, whereas the drought stress was applied between the flowering and the ripening. The randomized block design was used, with four replicates in the subplots. The following plots were [CO2] at 700ppm (F1) and [CO2] environmental (F2) and the subplots were well watering (S1) and drought stress (S2). The results were subjected to Anova and the Tukey test (P &lt; 0.05). For the treatments F1S1 and F1S2 the photosynthetic rate showed increments of 59% and the transpiration reduction of 12%. The yield,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Photosynthesis; Phaseolus vulgaris L.; Climate changes.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400012

Efeito do lignossulfonato de cálcio e magnésio na resistência mecânica e consumo de energia na fabricação de alimento extrusado para cães
Provedor de dados: 70
Autores: Nascimento,Thiago do; Ferraz,Antonio C. de. O.; Biagi,João D.
Utiliza-se a extrusão termoplástica na produção de alimento animal para obter extrusados que se mantenham íntegros, pois sua desintegração resulta em oneroso reprocessamento. Os objetivos do presente trabalho foram avaliar o efeito da adição de lignossulfonato de cálcio e magnésio, nas concentrações de 0,5; 1,0; 1,5; 2,0 e 4,0%, em massa, em formulação genérica para cães adultos em manutenção, na resistência mecânica do extrusado e medir o consumo de energia elétrica da extrusora, em escala industrial. Não houve diferenças na resistência mecânica do extrusado, quando avaliado através de penetração com ponteira cilíndrica. Porém, utilizando a compressão entre pratos planos rígidos e paralelos, discriminou-se a resistência dos extrusados que continham...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energia elétrica; Extrusão; Ração; Resistência mecânica.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300016

Uso da geotecnologia para caracterizar os cafezais no município de Londrina-PR, em relação à altimetria, declividade e tipo de solo
Provedor de dados: 70
Autores: Trabaquini,Kleber; Miglioranza,Édison; França,Valmir de; Pereira Neto,Osvaldo C.
O sensoriamento remoto e o geoprocessamento são ferramentas importantes no apoio aos levantamentos de dados da agricultura. O estudo teve por objetivo relacionar as variáveis físicas, como altimetria, declividade e tipo de solo com o agrossistema cafeeiro, no município de Londrina-PR, por meio de imagem do sensor Thematic Mapper (TM) do satélite Landsat-5, aliado às técnicas de geoprocessamento. Foi criado um banco de dados com informações de altimetria, declividade e classes de solos, e através de álgebra de mapa, realizado o cruzamento destas informações com a localização das lavouras cafeeiras, a qual foi obtida por meio do classificador digital Bhattacharya aplicado na imagem. A imagem do TM possibilitou o mapeamento de 79% das lavouras cafeeiras e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Café; Geomática; Caracterização ambiental.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600014

INTERACTIONS BETWEEN ADJUVANTS AND THE FUNGICIDE AZOXYSTROBIN+BENZOVINDIFLUPYR IN HYDRAULIC SPRAYING
Provedor de dados: 70
Autores: Landim,Thiago N.; Cunha,João P. A. R. da; Alves,Guilherme S.; Marques,Matheus G.; Silva,Sérgio M.
ABSTRACT Adjuvants are tools to maximize pesticide spray quality. This study aimed to evaluate the interaction effects between adjuvants and the fungicide azoxystrobin + benzovindiflupyr on the physicochemical characteristics, droplet evaporation time, and spray droplet size. The experiment was carried out using a 2×6 factorial scheme, in which the first factor was the absence or presence of the fungicide mixture (water or water + fungicide) and the second factor was the presence of different adjuvants (water and five adjuvants). The parameters evaluated were surface tension, pH, viscosity, electrical conductivity, droplet evaporation time, volume median diameter, percentage of droplets smaller than 100 μm, and relative amplitude of the droplet spectrum....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spray solution additives; Droplet spectrum; Surfactants; Application technology.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000500600

Potencial de redução do consumo de energia elétrica pela utilização de aquecedores solares no Estado de Goiás
Provedor de dados: 70
Autores: Oliveira,Luiz F. C. de; Ferreira,Regis de C.; Almeida,Rogério de A.; Lobato,Engler J. V.; Medeiros,Antônio M. de M.
O presente trabalho analisa a viabilidade técnica da redução do uso de energia elétrica pela substituição dos chuveiros elétricos por aquecedores solares e apresenta uma análise da redução do custo mensal de energia elétrica para os diferentes municípios de Goiás. Por meio do processamento de dados climatológicos e com o auxílio do aplicativo de informações geográficas SPRING®, foram calculados os valores de irradiâncias (MJ m-2 anual-1) e do número de horas anuais de brilho solar sobre a superfície da Terra e no topo da atmosfera, respectivamente, para os municípios do Estado de Goiás. Com base em dados censitários, calcularam-se o consumo médio de energia elétrica mensal por domicílio (kWh mês-1) e o total anual (kWh ano-1). Analisou-se a redução do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Energia elétrica; Energia solar; Eficiência energética.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300002

Management zones using fuzzy clustering based on spatial-temporal variability of soil and corn yield
Provedor de dados: 70
Autores: Rodrigues,Marcos S.; Corá,José E.
Clustering soil and crop data can be used as a basis for the definition of management zones because the data are grouped into clusters based on the similar interaction of these variables. Therefore, the objective of this study was to identify management zones using fuzzy c-means clustering analysis based on the spatial and temporal variability of soil attributes and corn yield. The study site (18 by 250-m in size) was located in Jaboticabal, São Paulo/Brazil. Corn yield was measured in one hundred 4.5 by 10-m cells along four parallel transects (25 observations per transect) over five growing seasons between 2001 and 2010. Soil chemical and physical attributes were measured. SAS procedure MIXED was used to identify which variable(s) most influenced the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Management zone analyst; Precision agriculture; Soil pH; Tropical soils; Zea mays L.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000300470

Efeitos da subsolagem e da adubação verde nas propriedades físicas do solo em pomar de citros
Provedor de dados: 70
Autores: Minatel,Alder L. G.; Andrioli,Itamar; Centurion,José F.; Natale,William.
O presente trabalho teve por objetivo avaliar o efeito da subsolagem e da adubação verde nas propriedades físicas de um Latossolo Vermelho distrófico típico, cultivado com citros (laranjeira Valência). Os tratamentos empregados foram: manejo mecânico das plantas invasoras com roçadora (Testemunha); subsolagem em um lado da planta na entrecopa; subsolagem nos dois lados da planta na entrecopa, e semeadura direta de Crotalaria spectabilis na entrecopa. As propriedades físicas do solo avaliadas foram: porosidade total, macroporosidade, microporosidade, densidade, resistência mecânica à penetração vertical e condutividade hidráulica. Na avaliação efetuada na safra 2001-2002, obtiveram-se os maiores valores de densidade do solo e resistência do solo à...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compactação do solo; Condutividade hidráulica do solo; Manejo do solo.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100010

Failure mode and effect analysis (FMEA) in mechanized harvest of sugarcane billets
Provedor de dados: 70
Autores: Voltarelli,Murilo A.; Paixão,Carla S. S.; Zerbato,Cristiano; Silva,Rouverson P. da; Gazzola,Jonathan.
ABSTRACT The quality control is used for the evaluation of processes and products, and it is important to detect and reduce variability and in operations management can be applied in mechanized harvesting of sugarcane billets. In this sense, this study aimed to identify critical quality indicators and, if necessary, to develop a continuous improvement plan for harvest of sugarcane billets. For the survey and definition of critical quality indicators the FMEA (Failure Mode and Effect Analysis) was applied, after the formation of the quality technical team. Evaluations of the collected variables were through control charts of individual values and the process capability indexes. There are 8 critical quality indicators in the billets harvesting process; the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Quality control; Flowchart; Agricultural mechanization; PDCA; Harvester.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100088

Rotina computacional e equação simplificada para modelar o transporte de sedimentos num Latossolo Vermelho Distrófico
Provedor de dados: 70
Autores: Cerquetani,Gilmar E.; Martins Filho,Marcílio V.
Os objetivos do presente trabalho foram desenvolver rotina computacional para a solução da equação de Yalin e do diagrama de Shields e avaliar uma equação simplificada para modelar a capacidade de transporte de sedimento num Latossolo Vermelho Distrófico que possa ser utilizada no Water Erosion Prediction Project - WEPP, assim como em outros modelos de predição da erosão do solo. A capacidade de transporte de sedimento para o fluxo superficial foi representada como função-potência da tensão cisalhante, a qual revelou ser aproximação da equação de Yalin. Essa equação simplificada pôde ser aplicada em resultados experimentais oriundos de topografia complexa. A equação simplificada demonstrou acuracidade em relação à equação de Yalin, quando calibrada...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão; Modelagem; Equação de Yalin.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200032

Comparação entre métodos de estimativa da evapotranspiração de referência (ETo) em regiões citrícolas paulistas
Provedor de dados: 70
Autores: Palaretti,Luiz F.; Mantovani,Everardo C.; Sediyama,Gilberto C.
As regiões escolhidas para o estudo são importantes no cenário citrícola irrigado, tanto em expansão quanto em atuação. Os dados meteorológicos utilizados para as estimativas são integrantes do banco de dados climáticos do software IRRIPLUS®. Com este software, estimou-se a evapotranspiração de referência (ETo) diária, utilizando as metodologias propostas por Penman-Monteith (EToPM), Hargreaves &amp;amp; Samani (EToHG) e Blaney-Criddle-FAO (EToBC), para o período de um ano. O objetivo deste estudo foi comparar os métodos de estimativa com EToPM, utilizando parâmetros de regressão (β0, β1), coeficiente de determinação (r²), e correlação (r), estimativa do erro-padrão (SEE), índices de concordância (d) e confiança (c). Os resultados indicam tendência de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Consumo de água; Penman-Monteith; Citros.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100005

Efficiency of pneumatic and horizontal perforated disk meter mechanism in corn no-tillage seeders in soil with different mobilization reports
Provedor de dados: 70
Autores: Mahl,Denise; Furlani,Carlos E. A.; Gamero,Carlos A.
This work objectified to evaluate the efficiency of two meter mechanism of corn seeds when submitted to different forward speed and soil management system during the non-tillage seeding. It was used a factorial design in randomized blocks. The factors whose effects were examined were related to the seeders with pneumatic and horizontal disk meter mechanisms for the distribution of the seeds, to the set tractor-seeder forward speeds (4.4; 8.0 and 9.8 km h-1), and to the soil management system considering the corn no-tillage seeding over minimum tillage with chisel plow and the no-tillage system for the seeding of oat culture (Avena strigosa Schreb). It was verified that the forward speed didn't influence the initial and final stands of plants but it...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision of distribution seeds; Forward speed; No-tillage system.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300014

Performance evaluation of hydrocyclone filter for microirrigation
Provedor de dados: 70
Autores: Mailapalli,Damodhara R .; Marques,Patricia A. A.; Thomas,Kochukaleepkal J.
In this study a hydrocyclone filter of 20 cm was selected and its performance was evaluated by studying the variation of discharge, pressure drop, influent concentration, and filtration efficiency with elapsed time of operation. The filter was tested with clean water to determine clean pressure drop and later it was tested with four concentrations of solid suspension, viz. 300; 600; 900 and 1,200 mg L-1. In the concentration of 300 mg L-1, the variation of pressure drop was low. But for the other concentrations of solid suspension, the variation was significant. The maximum pressure drops obtained were 41.19, 45.11, 50.01 and 52.95 kPa at 350, 390, 280 and 190 minutes of elapsed time, respectively. The maximum efficiency of solid suspension was 30.3,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Clogging; Filtration efficiency; Solid suspension.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300006

EFFECT OF ORGANIC LOAD AND ALKALINITY ON DAIRY WASTEWATER BIOMETHANATION
Provedor de dados: 70
Autores: Kispergher,Eduardo M.; D'Aquino,Camila A.; Costa Junior,Luis C. da; Mello,Thiago C. de; Weinschutz,Regina; Mathias,Alvaro L.
ABSTRACT: This study aimed to evaluate the effect of variations in organic load (hydraulic retention times - HRTs: from 2 to 0.5 day) and in alkalinity (NaHCO3 from 4,000 to 1,000 mg.L−1) on methane production. Biomass of sewage sludge was inoculated and stabilized on 1" polypropylene rings. The rings were immersed in the liquid phase (8.41 L) of an upflow anaerobic filter reactor (12.22 L). A solution of 5 g of whole milk powder per liter was used to simulate effluent from the dairy industry. Process effectiveness was measured by chemical oxygen demand reduction, biogas production, and biogas methane content. Biogas production started at a 2-day HRT and synthetic effluent alkalinization with 4,000 mg.L−1 NaHCO3. The best operation condition was at 1-day...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dairy industry; Biofilter; Hydraulic retention time; Alkalinity; Biogas.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400820

SPRAY DEPOSITION ON MAIZE USING AN ELECTROSTATIC SPRAYER
Provedor de dados: 70
Autores: Assunção,Heli H. T. de; Cunha,João P. A. R. da; Silva,Sérgio M.; Alves,Guilherme S.; Lemes,Ernane M.
ABSTRACT It is a well-known fact that the application of pesticides can be improved using an electrostatic spray due to the reduction of the application rate and increase in deposition on plant targets. However, little information exists on the use of such technology in maize crops. Thus, this study is aimed to evaluate the spray deposition on maize resulting from spray application using an electrostatic sprayer in combination with low application rates and different spray compositions. A field experiment was conducted in a randomized block having a 2×2×2 factorial design with two application rates (95 and 52 L ha-1), with or without the spray electrification, and with or without the synthetic adjuvant. The droplet electrification ability, interference of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays; Application rate; Electrified droplet; Spray technology; Spray deposition.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400503

Atrazine bound residues formation and dissipation in subtropical soil under swine wastewater application
Provedor de dados: 70
Autores: Gonçalves,Morgana S.; Sampaio,Silvio C.; Coelho,Silvia R. M.; Suszek,Floriano L.; Cordovil,Claudia M. D. S.
The effects of swine wastewater on atrazine dissipation and formation of bound residues in subtropical clay soil were investigated in this study. The experiment was carried out in laboratory, under room conditions, where samples of Rhodic Hapludox soil received 168.61 mg kg-1 of atrazine and were incubated for 60 days in the following treatments: T1 (sterilized soil + swine wastewater), T2 (sterilized soil + distilled water), T3 (Non sterilized soil + swine wastewater) and T4 (Non sterilized soil + distilled water). The extractable residues and bound residues of atrazine were extracted and analyzed by high performance liquid chromatography. The results showed no effect of swine wastewater on atrazine dissipation. However, the addition of swine wastewater...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Herbicide; Degradation; Sorption; Organic matter.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600017

Efeito de rodas compactadoras submetidas a cargas verticais em profundidades de semeadura sobre o desenvolvimento do milho
Provedor de dados: 70
Autores: Silva,Rouverson P. da; Corá,José E.; Carvalho Filho,Alberto; Lopes,Afonso; Furlani,Carlos E. A.
O sucesso de implantação de uma cultura pode ser garantido por uma semeadura bem realizada, e as rodas compactadoras utilizadas nessa operação devem ser capazes de melhorar o contato solo-semente para promover boa emergência das plântulas. O objetivo deste trabalho foi estudar a influência de três modelos de rodas compactadoras, três profundidades de semeadura e três níveis de carga sobre a roda compactadora na germinação e no desenvolvimento da cultura do milho, em uma pista de ensaios projetada para essa finalidade, no município de Uberaba - MG, em Latossolo Vermelho distrófico, textura média. O delineamento experimental utilizado foi o de parcelas subsubdivididas, com 27 tratamentos e quatro repetições. Os resultados obtidos evidenciaram que a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Canal de solo; Semeadura; Emergência.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200019

Avaliação do desempenho dos modelos de predição da erosão hídrica USLE, RUSLE e WEPP para diferentes condições edafoclimáticas do Brasil
Provedor de dados: 70
Autores: Amorim,Ricardo S. S.; Silva,Demetrius D. da; Pruski,Fernando F.; Matos,Antônio T. de.
Este trabalho teve o objetivo de avaliar o desempenho dos modelos de predição das perdas de solo USLE, RUSLE e WEPP para diferentes condições edafoclimáticas brasileiras. Para alcançar o objetivo proposto, perdas de solo estimadas pelos referidos modelos em nove localidades do Brasil foram comparadas às perdas medidas em parcelas experimentais, por meio do coeficiente de correlação, da raiz do erro quadrático médio (RMSE), do índice de concordância de Willmott, do índice de confiança, do coeficiente de Nash-Sutcliffe e da eficiência dos modelos. As parcelas experimentais adotadas nos estudos de perdas de solo utilizados no presente trabalho apresentavam dimensões (de 38 a 1.875 m²) e tempo de coleta de dados (de 1 a 7 anos) variados. Observou-se diferença...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão; Conservação do solo; Modelagem hidrológica.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600006

Delimitação automática de bacias hidrográficas utilizando dados SRTM
Provedor de dados: 70
Autores: Alves Sobrinho,Teodorico; Oliveira,Paulo T. S.; Rodrigues,Dulce B. B.; Ayres,Fabio M.
A delimitação adequada de bacias hidrográficas é fundamental por ser essa a unidade territorial para fins de planejamento e de gerenciamento dos recursos hídricos. Desse modo, este trabalho teve objetivo de analisar uma metodologia de delimitação automática de bacias hidrográficas. Foram utilizados, para tanto, dados do projeto Shuttle Radar Topographic Mission (SRTM) integrados e processados em Sistema de Informações Geográficas (SIG). Os resultados confirmam valores de área compatíveis aos obtidos com base em cartas topográficas. Assim, a automatização da delimitação de bacias hidrográficas, por meio de dados do SRTM e ambiente SIG, apresenta-se vantajosa em relação ao custo e benefício proporcionado, além de estabelecer a padronização do traçado e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Gestão de recursos hídricos; Bacia hidrográfica; Delimitação automática.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000100005

GEOSTATISTICAL MODELING OF SOYBEAN YIELD AND SOIL CHEMICAL ATTRIBUTES USING SPATIAL BOOTSTRAP
Provedor de dados: 70
Autores: Dalposso,Gustavo H.; Uribe-Opazo,Miguel A.; Johann,Jerry A.; Bastiani,Fernanda De; Galea,Manuel.
ABSTRACT The goal of this study was to use the spatial bootstrap method to model the spatial dependence structure of soybean yield and soil chemical attributes in an agricultural area. The study involved developing confidence intervals in probability plots to determine the probability distributions assumed by the data; determine the empirical distributions of the semivariances and model parameters, allowing to obtain statistics and confidence intervals; and to construct maps for the variables. The quantile-quantile plots indicated that the data follows a normal distribution. The confidence intervals for the semivariances helped to model the spatial dependence structure, and the descriptive statistics of the bootstrap replicates of the model parameters...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Confidence intervals; Quantile-quantile plot; Resampling; Spatial dependence.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300350

Effects of maintenance management procedures in sugarcane mechanic harvesting system equipment
Provedor de dados: 70
Autores: Faria,Luís F. F.; Silva,João E. A. R.
ABSTRACT The aim of this study was to evaluate the effects of modifying the maintenance programming of equipment used in sugarcane mechanical harvesting, by transferring actions that can be planned to periods when machines are inactive due to meal breaks and other working shift transitions stoppages. A simulation model was developed to represent the maintenance procedures of combines, haulouts, and other vehicles used by a harvest team. Scenarios were tested using alternatives for interventions such as refueling, lubrication and harvester blade replacement, enabling strategies to be focused towards better utilization of cutting, loading, and transport (CLT) system equipment. As a result, it was possible to remove one combine and two haulouts, while...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural machinery; Breakdowns; Simulation.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601187

Energy balance in the poultry-shed system and its influence on broiler performance
Provedor de dados: 70
Autores: Silva,Tatiana P. N. da; Pandorfi,Héliton; Guiselini,Cristiane.
ABSTRACT The objective of this study was to determine the energy balance of the poultry-shed system and its effect on broiler performance during the production cycle. The experimental design was completely random with sub-divided blocks. The blocks were composed of five different types of sheds and the sub-blocks of the evaluation times (00:00 h to 23:00 h), allowing an analysis of variance and a comparison between means with the Tukey test. There were no significant differences between the mean values of the exchanges of sensible, latent and total heat between the poultry sheds but the differences for the evaluation times were significant (P&lt;0.05). There was no significant difference between sheds 1 and 4 for broiler productive performance regarding...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Broiler industry; Thermal comfort; Thermography.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400613

COMPARATIVE ASSESSMENT BETWEEN PER-PIXEL AND OBJECT-ORIENTED FOR MAPPING LAND COVER AND USE
Provedor de dados: 70
Autores: Prudente,Victor H. R.; Silva,Bruno B. da; Johann,Jerry A.; Mercante,Erivelto; Oldoni,Lucas V.
ABSTRACT: The traditional per-pixel classification methods consider only spectral information, and may be limited. Object-based classifiers, however, also consider shape and texture, firstly segmenting the image, and then classifying individual objects. Thus, a Geographic Object-Based Image Analysis (GEOBIA) was compared in conjunction with data mining techniques and a traditional per-pixel method. A cut of Landsat-8, bands 2 to 7, orbit/point 223/77, located between the municipalities of Cascavel, Corbélia, Cafelândia and Tupãssi, in the west part of the state of Paraná, from 12/18/2013 was used. In the GEOBIA approach was realized image segmentation, spatial and spectral attribute extraction, and classification using the decision tree supervised...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: GeoDMA; Data mining; Decision tree.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000501015

Efeito do tempo de armazenagem de rações avícolas no dimensionamento de silos
Provedor de dados: 70
Autores: Lopes Neto,José P.; Nascimento,José W. B. do; Silva,Valneide R. da.
Dentre os fatores que afetam o fluxo de produtos sólidos, o tempo de armazenagem destaca-se por favorecer a formação de arcos coesivos. Dessa forma, esta pesquisa teve como objetivo determinar as propriedades de duas rações avícolas, classificá-las quanto à escoabilidade em função do tempo de consolidação e analisar seus efeitos em tremonhas metálicas. Para isso, foram utilizados aparelho de cisalhamento direto "Jenike Shear Cell", bancada de consolidação e duas superfícies de parede. Para o índice de fluxo e diâmetro mínimo do orifício de descarga, adotou-se a metodologia de Jenike. Para o ângulo da tremonha cônica, recorreu-se à metodologia de Enstad. Pode-se afirmar que as duas rações possuem fluxo do tipo fácil, sem variação para os tempos de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Consolidação; Índice de fluxo; Tremonha.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400002

Powder flow criteria for design of vertical silo walls
Provedor de dados: 70
Autores: Lopes Neto,José P.; Nascimento,José W. B. do; Silva,Rafael C.; Costa,Carlos A. da.
For design of vertical silos walls involving the storage of bulk solids to be safe and reliable, it is important knowing the largest possible number of variables such as: flow properties, silo geometry and pattern of flow desired. In order to validate the theories of flow prediction and design of conical hoppers, the flow properties of two bulk solids were determined, the theories of Jenike's flowability and Enstad and Walker for hopper design were analyzed and the results were compared with those experimentally obtained in a reduced model of a semicircular-section silo. Results show that Enstad theory for the hopper design is adequate to occur mass flow inside the silo, and for the sizing of the discharge outlet, the Walker's theory was closer to the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Discharge outlet; Reduced models; Flowability.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300003

Variabilidade local e regional da evapotranspiração estimada pelo algoritmo SEBAL
Provedor de dados: 70
Autores: Moreira,Luis C. J.; Durand,Bruno J.; Teixeira,Adunias dos S.; Andrade,Eunice M.
Em face da importância em conhecer a evapotranspiração (ET) para uso racional da água na irrigação no contexto atual de escassez desse recurso, algoritmos de estimativa da ET a nível regional foram desenvolvidos utilizando-se de ferramentas de sensoriamento remoto. Este estudo objetivou aplicar o algoritmo SEBAL (Surface Energy Balance Algorithms for Land) em três imagens do satélite Landsat 5, do segundo semestre de 2006. As imagens correspondem a áreas irrigadas, floresta nativa densa e a Caatinga do Estado do Ceará (Baixo Acaraú, Chapada do Apodi e Chapada do Araripe). Este algoritmo calcula a evapotranspiração horária a partir do fluxo de calor latente, estimado como resíduo do balanço de energia na superfície. Os valores de ET obtidos nas três regiões...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensoriamento remoto; Balanço de radiação; Landsat.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600015

TRACTOR PERFORMANCE IN SOWING WITH FURROWER CONFIGURATIONS IN AREAS WITH CONTROLLED TRAFFIC OF MACHINES
Provedor de dados: 70
Autores: Bertollo,Gilvan M.; Schlosser,José F.; Bertinatto,Rovian; Martini,Alfran T.; Rüdell,Iury Y. P.
ABSTRACT The controlled traffic of machines is a technique that performs the standardization of machine wheel gauges and width of implements, allowing them to move in predetermined places. The objective of this study was to evaluate the performance of an agricultural tractor, pulling seeder with configurations of furrows, in an area with controlled traffic of machines in various intensities. The study was developed in an agricultural area located in the municipality of Carazinho, RS. The experimental design was 3 × 3 randomized blocks, with traffic conditions (tractor traffic, tractor and harvester traffic, other tractor traffic, harvester and sprayer) and three configurations of furrows (double disk, double disk in the rows without traffic and rod in the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Traction force; Traffic lanes; Engine; Furrower.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500665

Análise numérico-experimental da agitação de calda em reservatórios de pulverizadores agrícolas
Provedor de dados: 70
Autores: Micheli,Gustavo B.; Padilha,Alcides; Scalon,Vicente L.
RESUMO Neste trabalho apresenta-se um estudo numérico-experimental do comportamento da agitação de fluido em reservatórios de pulverizadores agrícolas. Uma adequada agitação da calda de defensivos agrícolas em um reservatório é muito importante para garantir a homogeneidade da pulverização ao longo de toda a cultura. O objetivo do estudo foi avaliar a viabilidade da utilização de um modelo computacional aplicado ao problema de agitação de calda em reservatórios de pulverizadores agrícolas, e assim, auxiliar no projeto dos mesmos, com economia de tempo e custo. Deste modo, resultados de simulações computacionais de fluidodinâmica (CFD) foram comparados a testes experimentais normalizados. Utilizando um modelo monofásico (água), avaliaram-se os perfis de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agitação em reservatórios; Pulverização agrícola; Fluidodinâmica computacional.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601065

Crescimento inicial de duas cultivares de cafeeiro em diferentes regimes hídricos e dosagens de fertirrigação
Provedor de dados: 70
Autores: Rezende,Roberto; Helbel Júnior,Celso; Souza,Renan S. de; Antunes,Fausto M.; Frizzone,José A.
O experimento foi conduzido no Centro Técnico de Irrigação (CTI), Universidade Estadual de Maringá (UEM), tendo como objetivo avaliar os efeitos de diferentes regimes hídricos (irrigado e não irrigado) e fertirrigação, combinados com diferentes doses de adubo para N (15; 30; 45 e 60 g m-1), P (3; 6; 9 e 12 g m-1) e K (15; 30; 45 e 60 g m-1), na fase de crescimento inicial de duas cultivares de café, na região noroeste do Paraná. Foram avaliadas as seguintes variáveis de crescimento da cultura: diâmetro de copa, altura de planta e número de ramos plagiotrópicos totais. Observou-se que a fertirrigação e a irrigação influenciaram no desenvolvimento inicial do cafeeiro, aumentando os valores de todas as variáveis avaliadas. A interação entre regimes hídricos e...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica; Irrigação localizada; Fertirrigação.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000300009

THERMAL INSULATION WITH RECYCLED MATERIAL IN CREEPS FOR PIGLETS
Provedor de dados: 70
Autores: Sartor,Karina; Barros,Juliana de S. G.; Sarubbi,Juliana; Alonso,Jonas B.; Rossi,Luiz A.
ABSTRACT In the swine intensive farming, one of the biggest problems is to meet the thermal requirements of piglets in heated creeps, which demand high consumption of electricity and increase in production costs. The aim of this study was to evaluate the thermal efficiency and the consumption of electric energy in heated and internal insulated creeps, made of recycled material, when compared to creeps without thermal insulation. The treatments were: control (TCON): creep heated through suspended electric resistance, controlled by thermostat; thermal insulation with recycled material (TPK). The experiment was carried out for 21 days. In the treatments, the temperature (°C) and relative humidity (RH) of the air, consumption of electric energy (kWh), specific...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Piglets; Thermal insulation; Thermal efficiency.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600824

Tratamento das águas do processamento dos frutos do cafeeiro em filtro anaeróbio seguido por sistema alagado construído: I - remoção de matéria orgânica
Provedor de dados: 70
Autores: Fia,Ronaldo; Matos,Antonio T. de; Matos,Mateus P. de; Abreu,Edgar C.; Fia,Fatima R. L.
Seis sistemas de tratamento, compostos por três filtros anaeróbios com escoamento descendente, seguidos por seis Sistemas Alagados Construídos (SACs), tiveram suas condições operacionais avaliadas quando utilizados no tratamento da água residuária do processamento dos frutos do cafeeiro (ARC). Os filtros foram confeccionados em PVC (1,5 m de altura e 0,35 m de diâmetro) e preenchidos com brita nº 2. Os SACs foram constituídos por caixas de madeira (1,5 m de comprimento, 0,4 m de altura e 0,5 m de largura), sendo impermeabilizados e preenchidos com brita "zero". A ARC teve o pH corrigido com cal até valores próximos a 7,0, e a concentração de nutrientes alterada, de forma a se obter uma relação DBO/N/P de 100/5/1. Em metade dos SACs foi plantado o azevém...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Filtros anaeróbios; Wetlands construídos; Água residuária agroindustrial; Matéria orgânica; Café.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600019

Efeito de diferentes lâminas de irrigação na cultura do mamão
Provedor de dados: 70
Autores: Santos,Francisco S. S. dos; Viana,Thales V. A.; Azevedo,Benito M. de; Oliveira,Carlos W.; Sousa,Antonio E. C.
O objetivo deste trabalho foi estudar o efeito de diferentes lâminas de irrigação na cultura do mamão (Carica papaya L.), grupo Formosa, variedade 'Tainung Nº 1', nas condições edafoclimáticas do Distrito de Irrigação Jaguaribe Apodi (DIJA), Limoeiro do Norte, Ceará. Para isso, foram aplicados níveis de irrigação correspondentes a 50; 75; 100; 125 e 150% da evaporação do Tanque Classe "A" (ECA). Utilizou-se do delineamento experimental de blocos casualizados, com três repetições e cinco tratamentos. As variáveis analisadas foram massa média do fruto, produtividade e teor de sólidos solúveis totais. Os resultados obtidos demonstraram que a utilização de maiores lâminas de irrigação aumenta a produtividade, entretanto não altera a massa média do fruto e o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carica papaya L.; Tanque Classe "A"; Produtividade; Manejo de irrigação.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400007

Variabilidade espacial do potencial erosivo das chuvas no Estado do Rio de Janeiro
Provedor de dados: 70
Autores: Montebeller,Claudinei A.; Ceddia,Marcos B.; Carvalho,Daniel F. de; Vieira,Sidney R.; Franco,Elenilson M.
Desenvolveu-se este trabalho com o objetivo de analisar a variabilidade espacial da erosividade no Estado do Rio de Janeiro, por meio de análise geoestatística. Os índices de erosividade médios anuais EI30, definidos pelo produto da energia cinética da chuva e sua intensidade máxima em 30 min e KE&gt;25 (definidos como a energia cinética das chuvas com intensidades superiores a 25 mm h-1) foram calculados a partir de dados pluviográficos de 36 estações, enquanto, para outras 57 estações, os mesmos índices foram estimados por meio de equações de regressão, totalizando 93 pontos de amostragem. O modelo matemático ajustado ao semivariograma experimental, para ambos os índices, foi o exponencial. A partir dos parâmetros dos modelos ajustados, foi possível...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Índice de erosividade; Krigagem.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300011

Avaliação de linhas de beneficiamento e impactos de queda na qualidade de caqui "Rama Forte"
Provedor de dados: 70
Autores: Valentini,Silvia R. de T.; Ferreira,Marcos D.; Atarassi,Márcia E.; Benato,Eliane A.
O manuseio inadequado e excessivo de frutas e de hortaliças causa alta incidência de danos físicos e, consequentemente, perdas pós-colheita. O objetivo deste trabalho foi avaliar a magnitude de impacto em linhas de beneficiamento e classificação para caqui "Rama Forte" e determinar, em laboratório, seus limites de impactos. Para a avaliação dos pontos críticos, foi utilizada uma esfera instrumentada de 76 mm de diâmetro (Techmark, Inc., Lansing, EUA), que registrou a magnitude dos impactos em sete equipamentos distintos de quatro unidades de beneficiamento. A determinação de danos físicos foi feita em testes laboratoriais, nos quais a queda dos frutos foi relacionada com a magnitude de impacto, incidência de danos físicos e perdas na qualidade do fruto....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Diospyros kaki L.; Esfera instrumentada; Aceleração (G); Danos físicos.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400014

CHLOROPHYLL FLUORESCENCE OF BASIL PLANTS CULTIVATED IN A HYDROPONIC SYSTEM USING TREATED DOMESTIC WASTEWATER
Provedor de dados: 70
Autores: Gonçalves,Karoline S.; Alves,Lucylia S.; Paz,Vital P. da S.; Bandeira,Samir de S.
ABSTRACT Different techniques have been used to evaluate the energetic characteristics and damage to the photosynthetic apparatus of plants exposed to different stresses, including the measurement of chlorophyll fluorescence. The objective of this study is to evaluate the photosynthetic response by assessing the fluorescence parameters of chlorophyll a in basil (Ocimum basilicum L.) cv. Alfavaca Basilicão cultivated in a hydroponic deep-flow technique system using treated domestic wastewater. The study used a completely randomized block design with a 2 × 2 factorial scheme, in which the factors were the water source used for preparing the nutrient solution (tap water or treated domestic wastewater) and the height (upper and lower) of the platform of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wastewater; Ocimum basilicum L.; Photosynthetic response.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000300288

MICROBIOLOGICAL ACTIVITY DURING THE COMPOSTING OF WASTES FROM BROILER PRODUCTIVE CHAIN
Provedor de dados: 70
Autores: Bernardi,Francieli H.; Costa,Mônica S. S. de M.; Costa,Luiz A. de M.; Damaceno,Felippe M.; Chiarelotto,Maico.
ABSTRACT The quality of the carbon used as bulking agent in the composting process directly affects the dynamics of the waste degradation, which is governed by an active and diversified microbiota. The monitoring of the basal respiration and enzymatic activities during the composting of broiler agro-industrial wastes with different carbon sources as bulking agents was the aim of this study. The microbiological activities were more intense in the thermophilic phase of the process. The dynamics of the enzymatic activities were affected by the different carbon sources used as bulking agent in the composition of the windrows. When the milled sugarcane bagasse was used as carbon source, the windrow presented the highest amount of P in its constitution and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Basal respiration; Alkaline phosphatase; PH; Β-glucosidase; Cellulase; Urease.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000500741

Efficiency of distinct data mining algorithms for classifying stress level in piglets from their vocalization
Provedor de dados: 70
Autores: Cordeiro,Alexandra F. da S.; Nääs,Irenilza de A.; Oliveira,Stanley R. de M.; Violaro,Fabio; Almeida,Andréia C. M. de.
Among the challenges of pig farming in today's competitive market, there is factor of the product traceability that ensures, among many points, animal welfare. Vocalization is a valuable tool to identify situations of stress in pigs, and it can be used in welfare records for traceability. The objective of this work was to identify stress in piglets using vocalization, calling this stress on three levels: no stress, moderate stress, and acute stress. An experiment was conducted on a commercial farm in the municipality of Holambra, São Paulo State , where vocalizations of twenty piglets were recorded during the castration procedure, and separated into two groups: without anesthesia and local anesthesia with lidocaine base. For the recording of acoustic...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vocal expression; Well-being; Level of pain; Pig.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200001

Mapping of use and occupation of the soil and irrigation water quality in the city of Salto do Lontra-Paraná, Brazil
Provedor de dados: 70
Autores: Wrublack,Suzana C.; Mercante,Erivelto; Vilas Boas,Marcio A.
The objective of this study consisted on mapping the use and soil occupation and evaluation of the quality of irrigation water used in Salto do Lontra, in the state of Paraná, Brazil. Images of the satellite SPOT-5 were used to perform the supervised classification of the Maximum Likelihood algorithm - MAXVER, and the water quality parameters analyzed were pH, EC, HCO3-, Cl-, PO4(3-), NO3-, turbidity, temperature and thermotolerant coliforms in two distinct rainfall periods. The water quality data were subjected to statistical analysis by the techniques of PCA and FA, to identify the most relevant variables in assessing the quality of irrigation water. The characterization of soil use and occupation by the classifier MAXVER allowed the identification of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Global Navigation Satellite Systems - GNSS; Geographic Information Systems - GIS; Irrigation.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000500014

Agricultural engineering at UNICAMP: undergraduate student dropout analysis
Provedor de dados: 70
Autores: Testezlaf,Roberto.
Nowadays, dropping out in B.Sc. courses practically occurs in all Universities of the contemporary world. Undergraduate student withdraw could means several losses as, to the student, not to graduate, to the teacher, for not accomplishing his goal as educator, to the university, for not attending its mission, to the society, economic and social losses and also to the family for unfulfilling the dreams. The objective of this research is to present a quantitative study on the dropping out rate in the Agricultural Engineering B.Sc. program (BSAGENG) at State University of Campinas (UNICAMP), seeking to contribute to the understanding of this issue. It has been determined the dropping out rate from 1995 to 2006 based on the university official data, by...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: B.Sc. courses; Higher education; Dropout rate.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000600016

Variabilidad espacial de los modelos de infiltración de Philip y Kostiakov en un suelo Ândico
Provedor de dados: 70
Autores: Rodríguez-Vásquez,Andrés F.; Aristizábal-Castillo,Andrés M.; Camacho-Tamayo,Jesús H.
Conhecer o comportamento da infiltração é de grande utilidade devido a sua aplicação na produção agrícola, pois permite definir a operação de sistemas de irrigação e estudar os efeitos de diferentes práticas de uso do solo. O objetivo do presente estudo foi analisar a variabilidade espacial dos parâmetros do modelo de infiltração de Philip e Kostiakov, assim como a sua relação com a densidade do solo, a densidade das partículas e os teores de areia, de silte e de argila. Os testes de infiltração foram medidos usando dois anéis concêntricos, em uma malha de amostragem retangular de 5 x 8 pontos, em intervalos regulares de 20 m, sob duas condições de umidade do solo. Encontrou-se que a variabilidade do solo e, principalmente, os teores de argila, influem na...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geoestatística; Propriedades hidrofisicas; Atributos do solo.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000100007

Efeito da concentração de coagulantes e do pH da solução na turbidez da água, em recirculação, utilizada no processamento dos frutos do cafeeiro
Provedor de dados: 70
Autores: Matos,Antonio T.; Cabanellas,Cláudia F. G.; Cecon,Paulo R.; Brasil,Mozart S.; Mudado,Cláudio S.
Com o objetivo de determinar a dose e a faixa de pH dos coagulantes sulfato de alumínio (SA), sulfato ferroso clorado (SFC), cloreto férrico (CF) e extrato de semente de moringa (ESM), que proporcionassem maior eficiência na remoção da turbidez na água residuária da despolpa de frutos do cafeeiro (ARDC), após serem efetuadas cinco recirculações, foram conduzidos ensaios de coagulação/floculação utilizando o aparelho "Jar-test". Todos esses coagulantes foram avaliados nas concentrações de 0; 0,5; 1,0; 1,5; 2,0; 2,5 e 3,0 g L-1. No caso da solução preparada com ESM, as doses utilizadas foram: 0; 10; 20; 30; 40; 50 e 60 mL L-1. O pH da solução em teste foi alterado, utilizando-se do hidróxido de sódio (NaOH), na concentração de 0,3 mol L-1, sendo avaliadas as...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Moringa oleifera; Água residuária; Resíduos orgânicos.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300025

ECONOMIC ANALYSIS OF DIFFERENT HYDRAULIC SPRAYERS USED IN SUGARCANE (Saccharum spp.)
Provedor de dados: 70
Autores: Santos,Neisvaldo B. dos.
ABSTRACT Brazil is the largest sugarcane producer worldwide. In mills, sugarcane crops are sprayed with agrochemicals using self-propelled, tractor-driven, and aerial hydraulic sprayers. As sugarcane spraying is regularly performed over extensive areas, the machinery to be used should be planned and dimensioned to ensure timely operations without overloading and at lower costs. Therefore, the current study aimed to analyze the operational and economic performances of different hydraulic sprayers to perform sugarcane crop control. As long as meeting our goal in field conditions would be difficult, we opted to develop a computational model, named as “TratoCana”, using a spreadsheet and programming language. The model was used to assess economic and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultural mechanization; Computer model; Cost; Mill revenue; Planning and management; Sugarcane mill.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200225

LOSS OF WATER AND NUTRIENTS IN DIFFERENT SOIL TILLAGE SYSTEMS SUBJECTED TO NATURAL RAINFALL IN THE STATE OF MATO GROSSO, BRAZIL
Provedor de dados: 70
Autores: Leite,Marcelo H. S.; Couto,Eduardo G.; Amorim,Ricardo S. S.; Scaramuzza,José F.
ABSTRACT The aim of this study was to evaluate the loss of water and nutrients by laminar runoff in different soil tillage systems subjected to natural rainfall. Five experimental plots were established for the cultivation of cotton in the city of Campo Verde - MT, with the following treatments: CTDP = conventional soil tillage and planting of the cotton in the direction of the slope; CTCP = conventional tillage and contour planting; CP = tillage of soil with a disk harrow and a leveling harrow, followed by contour planting; CoP = tillage by two passes of a leveling harrow followed by contour planting; MTCP = minimum tillage with contour planting. The losses of water by laminar runoff in were determined by the stored volume and samples were taken to...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Laminar runoff; Losses of nutrients; Losses of potassium (K); Transports nutrients; Water erosion.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600864

Árvore de decisão para classificação de ocorrências de ferrugem asiática em lavouras comerciais com base em variáveis meteorológicas
Provedor de dados: 70
Autores: Megeto,Guilherme A. S.; Oliveira,Stanley R. de M.; Ponte,Emerson M.del; Meira,Carlos A. A.
A ferrugem asiática é a mais importante doença da soja no Brasil. Apesar de sua epidemiologia ser conhecida, são escassos os estudos sobre os fatores que desencadeiam a doença com base em dados de campo. Este trabalho objetivou modelar a influência de variáveis meteorológicas a partir de um conjunto extenso de dados de ocorrência da ferrugem, por meio da técnica de indução de árvores de decisão. Os modelos foram desenvolvidos com dados de data de ocorrência da doença em quatro safras (2007/08 a 2010/11) e variáveis de temperatura e chuva em diferentes janelas de tempo prévias à data de detecção. Para cada registro de ocorrência, foi gerado um correspondente de "não ocorrência" como sendo o trigésimo dia anterior ao dia da detecção, assumindo-se a presença...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Phakopsora pachyrhizi; Mineração de dados; Previsão de doenças de plantas; Epidemiologia; Sistemas de suporte à decisão; Phakopsora pachyrhizi.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300021

MERCURY IN THE SEDIMENT OF PELOTAS RIVER BASIN, BRAZIL
Provedor de dados: 70
Autores: Remor,Marcelo B.; Sampaio,Silvio C.; Model,Kathleen J.; Falco,Thais D.; Prudente,Victor H. R.
ABSTRACT Many studies have determined the concentration of trace elements in river sediments in Brazil. Notwithstanding, mercury assessments are scarce, especially because of exclusive extraction techniques and expensive analysis techniques. Still, this element is known for its toxicity, persistence, and bioaccumulation, making its presence in the environment an important factor for biota and human health. For this reason, the objective of this study was to determine the mercury concentration in the sediment of the Pelotas River basin, located on the border of the states of Santa Catarina and Rio Grande do Sul. The sediment was collected at eight locations of the Pelotas basin and, after drying, the mercury was quantified by atomic absorption spectrometry...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Heavy metal; Trace element; Multivariate statistics.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100117

DRYING KINETICS OF THE SLICED PULP OF BIOFORTIFIED SWEET POTATO (Ipomoea batatas L.)
Provedor de dados: 70
Autores: Souza,Diene G.; Resende,Osvaldo; Moura,Lígia C. de; Ferreira Junior,Weder N.; Andrade,José W. de S.
ABSTRACT Biofortified sweet potato (Ipomoea batatas) is one of the foods with the highest contributions of carotenoids in the diet, especially provitamin A carotenoids. Thus, this study aimed to analyze the drying kinetics of the biofortified sweet potato pulp using the Akaike (AIC) and Schwarz's Bayesian (BIC) information criteria for model selection, as well as determine the effective diffusion coefficient and activation energy under different drying conditions. The biofortified sweet potatoes were sliced into chips and submitted to drying in an air circulation oven at 1.0 m s−1 at temperatures of 45, 55, 65, and 75 °C until constant mass. The mathematical models Wang and Singh, Verma, Thompson, Page, Newton, Midilli et al., logarithmic, Henderson and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Liquid diffusion; Activation energy; Wang and Singh.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200176

Utilização de lisímetros de pesagem para a determinação dos coeficientes de cultura do meloeiro (Cucumis melo L.) para cultivo em estufa agrícola na região de Araras - SP
Provedor de dados: 70
Autores: Peres,José G.; Marcussi,Leandro; Souza,Claudinei F.; Brugnaro,Caetano.
Esta pesquisa foi conduzida em uma estufa agrícola instalada na área experimental do Centro de Ciências Agrárias da Universidade Federal de São Carlos, localizado em Araras - SP. O solo da área experimental é um Latossolo Vermelho-Escuro, distrófico, de horizonte A moderado e textura argilosa. Os meloeiros estudados foram os híbridos Louis e HD 90. O experimento foi irrigado por gotejamento, e o controle da irrigação, realizado por meio de dois lisímetros de pesagem instalados dentro da estufa. A umidade do solo foi monitorada com uma sonda de TDR e mantida próxima de sua capacidade de campo. As informações climatológicas relevantes ao projeto foram coletadas em estações meteorológicas automáticas, instaladas dentro e fora da estufa. A evapotranspiração de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Melão; Cultivo protegido; Célula de carga.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000300005

INFLUENCE OF ALBUMIN ON GUAVA PULP POWDER OBTAINED BY FOAM-MAT DRYING
Provedor de dados: 70
Autores: Maciel,Roberta M. G.; Afonso,Marcos R. A.; da Costa,José M. C.; Araújo,Tayla M. R.
ABSTRACT Guava is a fruit that stands out for its aroma, intense flavor, vitamins, and minerals. Its availability as a powdered food enhances its commercial applications. This study aimed to evaluate mathematical models for adsorption isotherms and determine the properties and flowability of guava pulp powder obtained by foam-mat drying. The models of GAB, BET, Henderson and Oswin were fitted to determine the isotherms of powders with 4 and 8% albumin, at temperatures of 35°C and 45°C. The powders were evaluated by wall friction angle, flow index, apparent density, and particle microstructure analysis. The best fit to the isotherms was obtained by the GAB model. Wall friction angle ranged from 15.7 to 21.9° and from 13.6 to 20.4° for samples containing 4...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tropical fruit; Food powder; Isotherm.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300388

SPRAY DEPOSITION ON SOYBEAN CROP USING DIFFERENT TRAVEL SPEEDS AND APPLICATION RATES
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Victor,Arthur P.; Sales,Caroline G. R.
ABSTRACT Farmers are seeking pesticide treatments with lower application rates and higher travel speeds. However, this can lead to a poor quality of the application. The aim of this study was to evaluate the spray deposition on soybean crop and the droplet spectra using different application rates and speeds. The experiment was conducted in soybean (R5 stage), M 6410 IPRO variety. Six treatments involving two application rates (80 and 150 L ha-1) and three speeds (10, 15 and 20 km h-1) were evaluated through a self-propelled sprayer. A characterization study of the spray droplets was conducted through the evaluation of water sensitive papers. The spray deposition study was carried out. For this, a marker was added to the application to be detected by...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Glycine max; Sprayer.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100082

INFLUENCE OF GLYPHOSATE CONCENTRATIONS ON SPRAY SOLUTION PHYSICOCHEMICAL CHARACTERISTICS AND DRIFT POTENTIAL
Provedor de dados: 70
Autores: Almeida,Dieimisson P.; Ferreira,Marcelo da C.; Santos,Renata T. da S.; Griesang,Fabiano; Santos,Eduardo de S. dos; Timossi,Paulo C.
ABSTRACT The herbicide glyphosate is sprayed with varying application volumes that result in different concentrations used in the spray solutions. Thus, this study aimed to evaluate the effect of glyphosate concentrations on the potential risk of droplet drift, surface tension of spray solution, and contact angle of droplets on surfaces. Three experiments were conducted in a completely randomized design. Drift potential was evaluated by median volumetric diameter (MVD), percentage volume of droplets with diameter smaller than 100 μm (%V&lt;100 μm), and coefficient of uniformity (Span), with 12 replications. The surface tension of spray solutions and contact angle of droplets were evaluated on Urochloa ruziziensis leaves, paraffin film, and glass, with four...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Surface tension; Contact angle; Droplets; MVD; Congo grass.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100069

PHYSICAL, MECHANICAL AND THERMAL BEHAVIOUR OF ADOBE STABILIZED WITH THE SLUDGE OF WASTEWATER TREATMENT PLANTS
Provedor de dados: 70
Autores: Gandia,Rômulo M.; Gomes,Francisco C.; Corrêa,Andréa A. R.; Rodrigues,Maykmiller C.; Marin,Diego B.
ABSTRACT The need for treated water is essential for life. With the constant increase in population, the most common way to purify surface water is through conventional water treatment plants (WTPs). The high volume of residue (sludge) generated in this process is most often returned to the catchment site, negatively affecting the ecosystem. The sludge of WTPs is similar to soil because it is composed of inorganic solids. Adobe is a construction material made from water and soil without the burning process, so it is considered sustainable, recyclable, and energy-efficient and can be stabilized with various materials. Therefore, the objective of this work is to develop adobes using the sludge of WTPs and to analyse their physical, mechanical and thermal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Wastewater treatment plants; Building materials; Sustainability; Composite materials; Waste in construction.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600684

TEMPORAL VARIATION AND SPATIAL DISTRIBUTION OF RELATIVE INDICES OF LEAF CHLOROPHYLL IN GRAPEVINE cv. CHARDONNAY
Provedor de dados: 70
Autores: Costa,Bruno R. S.; Oldoni,Henrique; Silva,Wendell A.; Martins,Roberto L.; Bassoi,Luís H.
ABSTRACT Variation in the spatial distribution of leaf chlorophyll content associated with the progression of the phenological cycle of crops may occur in cultivated areas as a result of the variability of environmental conditions and of the intrinsic properties of the plants. The objective of the present study was to model the trend in variation and assess the temporal stability of index of chlorophyll a, b, and total chlorophyll (Chla, Chlb, and Chlt, respectively), and to characterize the spatial distribution of Chlt index in grapevine cv. ‘Chardonnay’. The assessments consisted of in situ measurements made with a portable meter in a commercial vineyard located in the municipality of Espírito Santo do Pinhal, state of São Paulo, Brazil, in the period...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Vitis vinifera L.; Photosynthetic pigments; Portable meter.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000800074

PEANUT CULTIVARS SUBMITTED TO IRRIGATION LEVELS AND NITROGEN ADUBATION IN TROPICAL CLIMATE
Provedor de dados: 70
Autores: Barbieri,João D.; Dallacort,Rivanildo; Faria Junior,Cleonir A.; Freitas,Paulo S. L. de; Carvalho,Marco A. C. de.
ABSTRACT: The objective of this study was to define the best irrigation level in a sprinkler system, submitted to nitrogen doses in covering in the municipality of Tangará da Serra - MT, for two cultivars of peanut (Arachis hypogaea L.). The experiment was carried out in the experimental field of the State University of Mato Grosso (UNEMAT), located geographically in latitude 14°39′S; Longitude 57°25′W, at 440 meters of altitude. The climate is classified as tropical humid megathermal (Aw), with annual average rainfall of 1,830 mm and average temperature of the air 24.4°C. The soil is classified as Dystroferric Red Latosol. The experimental design was in randomized blocks where 4 levels (30, 70, 110 and 150% of the reference evapotranspiration, ET0) were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiration; Correlation; Productivity.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601126

Análise de investimento em plataformas colhedoras de milho em espaçamento reduzido: efeito de oscilações da produtividade, do preço do milho e da semente
Provedor de dados: 70
Autores: Dias,Vilnei de O.; Ferri,Diceu J.; Alonço,Airton dos S.; Souza,Renato S. de.
O objetivo deste trabalho foi avaliar a viabilidade econômica do investimento em plataformas colhedoras de milho em espaçamento reduzido quanto a aumentos percentuais de produtividade, do preço do milho e da semente. Para tal, foi confeccionado fluxo de caixa diferencial e, a partir desse, determinaram-se a Taxa Interna de Retorno (TIR) e a Razão Benefício/Custo (B/C) do investimento para as combinações de aumentos de produtividade em diferentes níveis tecnológicos. Fez-se análise de sensibilidade para variações no preço pago pelo produto e nas despesas com sementes para o indicador Valor Presente Líquido (VPL). Foram consideradas áreas de 100 a 300 ha e produtividades de 70; 100; 130 e 160 sc ha-1. Concluiu-se que os acréscimos de produtividade afetam...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Engenharia agrícola; Análise de sensibilidade; Zea mays.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000200008

POTENTIAL DRIFT AND INJURY OF HERBICIDES SPRAYED IN A WIND TUNNEL
Provedor de dados: 70
Autores: Oliveira,Guilherme M. P. de; Gandolfo,Marco A.; Oliveira,Rone B. de; Oliveira,Stella M. P. de; Martins,Vinicius A.
ABSTRACT The possibility of synthetic auxin applications in crops increases the risk of injury to sensitive plants. The aim of this study was to quantify the drift of herbicides sprayed in a wind tunnel and the injury in cotton plants. The experimental design was a completely randomized design with five treatments and four replications. The tested spray solutions were dicamba (0.250 L c.p. ha−1), glyphosate (0.625 L c.p. ha−1), 2,4-D (0.250 L c.p. ha−1), glyphosate + 2,4-D (0.625 L c.p. ha−1 + 0.250 L c.p. ha−1), and glyphosate + dicamba (0.625 L c.p. ha−1 + 0.250 L c.p. ha−1). Drift was quantified in a wind tunnel, collected at distances of 5, 10, and 15 m in relation to the spray tip. Cotton plants were placed in the same wind tunnel and the injury was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dicamba glyphosate herbicide mixture application technology 2; 4-D.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000100075

Modelagem matemática para a descrição do processo de secagem do feijão (Phaseolus vulgaris L.) em camadas delgadas
Provedor de dados: 70
Autores: Corrêa,Paulo C.; Resende,Osvaldo; Martinazzo,Ana P.; Goneli,André L. D.; Botelho,Fernando M.
O objetivo do presente trabalho foi a obtenção e a avaliação das curvas de secagem do feijão (Phaseolus vulgaris L.) e ajustar diferentes modelos matemáticos aos valores experimentais do teor de água para diversas condições do ar. Foram utilizados grãos de feijão colhidos com teor de água de 0,92 (b.s.) e submetidos à secagem até o teor 0,14 (b.s.) sob condições controladas de temperatura (35; 45 e 55 °C) e umidade relativa do ar de secagem de 40 ± 2%. Aos dados experimentais, foram ajustados 12 modelos matemáticos citados na literatura específica e utilizados para a representação do processo de secagem de produtos agrícolas. Pelos resultados obtidos e baseando-se em parâmetros estatísticos, pode-se concluir que metade dos modelos testados representa bem o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Feijão; Modelagem matemática; Teor de água.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300020

Mudanças nas características físico-químicas de um latossolo vermelho-amarelo distrófico após a irrigação com água de reúso na cultura da alface-crespa (Lactuca sativa, L.)
Provedor de dados: 70
Autores: Varallo,Antonio C. T.; Souza,Claudinei F.; Santoro,Bruno de L.
A utilização do efluente de esgoto tratado para poupar os corpos d'água utilizados para irrigação tem sido de grande interesse na agricultura, e o uso não regulamentado desta prática pode acarretar mudanças no comportamento físico-químico do solo. Sua prática tem sido de grande interesse em vista da redução da quantidade de água retirada dos mananciais, preservando-os. Objetivou-se, neste trabalho, a avaliação dos atributos físico-químicos de um Latossolo Vermelho-Amarelo após aplicação de água de reúso. O experimento foi realizado em uma condição de casa de vegetação onde foram cultivados dois ciclos da alface-crespa (Lactuca sativa, L) com dois tratamentos, com três repetições cada: testemunhas (água de abastecimento proveniente de poço) e reúso...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água de reúso; Manejo; Salinidade; Sodicidade.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200007

Comportamento mecânico do solo sob tráfego em dois sistemas de preparo do solo
Provedor de dados: 70
Autores: Terminiello,Antonino M.; Balbuena,Roberto H.; Draghi,Laura M.; Claverie,Jorge A.; Palancar,Telmo C.; Jorajuría,Daniel.
Os solos submetidos a sistemas de produção que não incluem o preparo do solo, estão condicionados, em sua sustentabilidade, a um manejo que priorize o acompanhamento da compactação que o tráfego de máquinas provoca. Foram realizados ensaios de campo com o objetivo de avaliar a reologia de um solo Typic Hapludert, submetido ao tráfego de veículos em dois sistemas de preparo do solo (preparo convencional - LC, e semeadura direta - SD). Os subtratamentos foram quatro intensidades de tráfego (0; 80; 160 e 240 Mg km ha-1). As variáveis experimentais dependentes foram: índice de cone (IC) e densidade aparente a seco (DA). Para 160 e 240 Mg km ha-1, encontraram-se diferenças estatísticas significativas no IC em relação à testemunha. Para o LC, com as maiores...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compactação induzida; Intensidade de tráfego; Semeadura direta.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100018

DROPLET SPECTRA AND SURFACE TENSION OF SPRAY SOLUTIONS BY BIOLOGICAL INSECTICIDE AND ADJUVANTS
Provedor de dados: 70
Autores: Costa,Lilian L.; Silva,Henrique J. P. Soares da; Almeida,Dieimisson P.; Ferreira,Marcelo da C.; Pontes,Nadson de C.
ABSTRACT Biological insecticides can be another pest control method used in integrated pest management; hence there is a demand for scientific information about these products to understand the appropriate application technique. The aim of this study was to evaluate the spray spectra data by different nozzle types using biological insecticide isolated and with adjuvants, as well the surface tension of these spray solutions. For droplet spectra data, a particle size analyzer was used and for surface tension of the spray solution, the method of pendant drop was used. Among the nozzles tested, ADI 11002 provided greater droplets median diameter volume, a lower percentage of droplets with diameters less than 100 μm and also the highest coefficient of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coefficient of uniformity; Volumetric median diameter; Application technology; Tensiometer.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200292

Efeito da irrigação sobre a classificação do café
Provedor de dados: 70
Autores: Custódio,Anselmo A. de P.; Gomes,Natalino M.; Lima,Luiz A.
Foi estudado o efeito da irrigação sobre a classificação do café grão cru, quanto ao tipo, formato do grão e sua granulometria, nas cinco primeiras safras, em lavoura irrigada por pivô- central, aplicando-se cinco lâminas de irrigação em função do balanço entre a evaporação do tanque classe A (ECA) e precipitação (P), além de tratamento-testemunha (não-irrigado). A cultivar plantada foi a Rubi, em março de 1999, no espaçamento de 3,5 m entre linhas e 0,8 m entre plantas. Não foi observado efeito significativo da irrigação sobre os aspectos estudados: tipo (defeitos intrínsecos), formato (grãos chatos e moca) e granulometria dos grãos (peneiras). Contudo, entre as classes de defeito, os grãos verdes e ardidos foram os que apresentaram os maiores percentuais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica L.; Defeitos intrínsecos; Granulometria dos grãos.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400012

ADDITION OF BOILER CHARCOAL WASTE TO COMPOST FOR USE AS SUBSTRATE FOR VEGETABLE SEEDLINGS
Provedor de dados: 70
Autores: Lorin,Higor E. F.; Costa,Mônica S. S. de M.; Chiarelotto,Maico; Santos,Francielly T. dos; Costa,Luiz A. de M.
ABSTRACT The recovery of waste from the broiler production chain (BPC) is consistent with the principles of a circular economy. Besides turning waste into organic compost, its use as substrate for the production of vegetable seedlings further increases its economic value. However, it is necessary to adapt its characteristics to enable its use as substrate. To this end, the addition of boiler remnant charcoal wastes (BCW), another type of waste generated in the BPC, to the organic compost resulting from the composting of BPC waste with different bulking agents (BAs) was studied. The addition of BCW to agro-industrial compost reduced the electrical conductivity (EC) of substrates. Multiple linear regression showed that, of the 13 variables (physical,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Electrical conductivity; Circular economy; Easiness of removal of clod from tray; Seedling quality index; Salinity.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000600753

QUALITY OF SEED DISTRIBUTION AT DIFFERENT SPACES BETWEEN BASE AND INTERMEDIATE BASE
Provedor de dados: 70
Autores: Garcia,Luiz C.; Weirich Neto,Pedro H.; Justino,Altair; Eurich,Joelcio; Souza,Nátali M.
ABSTRACT The aim of this study was to analyze the influence of space between the base and intermediate base on quality of seed distribution with a horizontal seed plate. The experiment was carried out in 2012 at the Laboratory of Agricultural Mechanization of the State University of Ponta Grossa - PR, Brazil, using a sowing simulation device. The experimental design was completely randomized design with four treatments and seven replications. Treatments consisted of spaces (0, 1, 2, and 3 mm) between the base and intermediate base. Replications were defined by 250 spacing between seeds. Corn (Zea mays L.), soybean (Glycine max L. Merrill), and sorghum (Sorghum bicolor Moench) seeds were tested. The analyzed variables were faulty, multiple and acceptable...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Horizontal seed plate; Glycine max; Seeder-fertilizer machine; Sorghum bicolor; Zea mays.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100128

EXPERIMENT OF A SWING SEPARATING SIEVE ON A POTATO DIGGER
Provedor de dados: 70
Autores: Xie,Shengshi; Wang,Chunguang; Deng,Weigang.
ABSTRACT For the purpose of achieving the distribution of the potato-soil mixture and the appropriate parameters of the swing separating sieve, we conducted experiments using the 4SW-170 potato digger. The experiments consisted of two parts. In each part, the experimental factors were crank rotational speed, sieve inclination and machine forward speed. The difference is that the first part involved a single factor test, which selected the coverage of the potato-soil mixture as the evaluation indicator. In contrast, the second part involved an orthogonal test, which selected the obvious rate and damage rate as evaluation indexes. In the first part, it was observed that the coverage of the potato-soil mixture on the separating sieve reduced gradually with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Swing separating sieve; Coverage of potato-soil mixture; Parameter optimization; Experimental studies.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000400548

Estudo granulométrico de grãos de soja normal e transgênico
Provedor de dados: 70
Autores: Milani,Adhemar P.; Bidóia,Vitor S.; Perecin,Dilermando.
Este trabalho foi desenvolvido com o propósito de estudar o comportamento granulométrico de grãos de soja em função da variação do teor de água. A pesquisa foi realizada com seis variedades, sendo duas transgênicas e quatro comuns, com os teores de água de 10%, 12%, 15%, 20% b.s. A granulometria foi determinada utilizando-se de seis subamostras de 120 grãos para cada teor de água, e as suas dimensões (comprimento, largura e espessura) obtidas por meio de paquímetro digital. Os resultados indicaram que cada variedade de soja comportou-se de maneira diferenciada e que as comuns tiveram comportamento granulométrico diferenciado das transgênicas.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Granulometria; Teor de água; Variedades de soja.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400015

Jatropha seed oil content and yield under different irrigation and potassium fertilization levels
Provedor de dados: 70
Autores: Deus,Fábio P. de; Faria,Manoel A. de; Oliveira,Ednaldo L. de; Castro Neto,Pedro.
The aim of this research was to evaluate the effects of different irrigation depths and potassium dosages, of Jatropha seed oil content and yield. The experimental design used was randomized blocks, in split-plots, with four replicates. The treatments were four water depths (plots) and four potassium dosages (subplots) applied through irrigation water. The water depths were applied based on the percentage of accumulated evaporation of a Class A (ECA) tank and of rainfall, as following: L0 = without irrigation, L40, L80 and L120, representing 40, 80 and 120% of the balance, respectively. The potassium dosages were K30, K60, K90 and K120 (30, 60, 90 and 120kg ha-1 of potassium, respectively). The oil extraction of samples was done through chemical extraction...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chemical extraction; Biodiesel; Oilseed; Drip irrigation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600010

Impacto das variáveis ambientais em incubatório de estágio múltiplo de frangos de corte
Provedor de dados: 70
Autores: Baracho,Marta S.; Nääs,Irenilza De A.; Gigli,Ana C. S.
Este trabalho visou a quantificar as características de resposta produtiva de pintos de corte provenientes de duas linhagens comerciais, em incubatório de regime de estágio múltiplo. Para tal, foram monitorados três lotes de ovos férteis em incubatório comercial, verificando o impacto das seguintes variáveis ambientais: temperatura, velocidade do ar, umidade relativa, concentração de dióxido de carbono e presença de fungos. O acompanhamento de pintos provenientes de duas linhagens comerciais distintas (Cobb® e Avian®) foi feito em três lotes, quando também foram coletados dados de perdas. A análise de componentes principais foi empregada para associar as variáveis de ambiente, produção e perdas, observando a magnitude dos vetores. Os resultados mostraram...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avicultura; Incubação; Ambiência.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400001

Solar energy use for water pre-heating in boilers of agro-industries
Provedor de dados: 70
Autores: Celuppi,Rafael; Scapinello,Jaqueline; Andrade,Felipe G. D.; Revello,Jaime H. P.; Magro,Jacir Dal.
Energy consumption in the world has been growing every year. The industrial sector represents 27.32% of the world energy demand. Heating systems that use solar energy may contribute with a percentage of the total energy required by industries. This work aimed to study the use of vacuum solar collectors for water pre-heating in boilers. We used four collectors installed according to NBR 15,569; water flow through the tubes was 0.058 L/s, and temperature in the inlet and outlet pipes was measured. Results showed that instantaneous radiation, and inlet fluid and room temperatures are variables that influence the process, reaching water maximum temperature in the solar collector outlet of 97.9 °C, and efficiency of approximately 65% for most experiments. For...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solar collector; Water heating; Energy efficiency.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300009

Production of tomato seedlings using different substrates and trays in three protected environments
Provedor de dados: 70
Autores: Costa,Edilson; Leal,Paulo A. M.; Benett,Cleiton G. S.; Benett,Katiane S. S.; Salamene,Luiz C. P.
The seedlings production is an essential part for vegetables production. Thus, this study aimed to evaluate the environment, the substrates and the containers in the development of tomato seedlings, cv. Santa crus Kada Gigante, in Aquidauana -MS, Brazil region, from October to November, 2008. Polystyrene trays with 72; 128 and 200 cells, filled with four substrates (soil; Plantmax®; coconut fiber and vermiculite) were tested in three protected environments (greenhouse; screened with Sombrite® and screened with Aluminet®). The experimental design was completely randomized, factorial scheme 3x4 (three trays x four substrates), with four replications, being analyzed individual variance analysis and joint analysis for the environments. The environment with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Solanum lycopersicum; Protected cultivation; Propagation.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500002

Metodologia para cálculo rápido das dimensões de pneus de tratores agrícolas
Provedor de dados: 70
Autores: Márques,Luis.
Os primeiros tratores agrícolas utilizavam como elementos de locomoção rodas metálicas com garras. Diante da impossibilidade de circular por estradas, os danos provocados sobre os caminhos e o recalque em solo desagregado tornaram necessária a busca de outros materiais para os rodados dos tratores. Os rodados pneumáticos, ao se deformarem, adaptam-se melhor às irregularidades do terreno, aumentando a capacidade trativa e a comodidade para o operador. A diminuição da lastragem, substituída por cargas dinâmicas induzidas por transferência de peso, melhora ainda mais o desempenho das rodas no solo, convertendo-as em verdadeiros pontos de apoio. Apesar de toda evolução experimentada pelos rodados, os mesmo oferecem diversas opções técnicas que nem sempre são...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pneus agrícolas; Eficiência em tração; Patinagem.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300019

Multivariate statistical analysis to support the minimum streamflow regionalization
Provedor de dados: 70
Autores: Elesbon,Abrahão A. A.; Silva,Demetrius D. da; Sediyama,Gilberto C.; Guedes,Hugo A. S; Ribeiro,Carlos A. A. S.; Ribeiro,Celso B. de M.
ABSTRACT This study aimed to develop a methodology based on multivariate statistical analysis of principal components and cluster analysis, in order to identify the most representative variables in studies of minimum streamflow regionalization, and to optimize the identification of the hydrologically homogeneous regions for the Doce river basin. Ten variables were used, referring to the river basin climatic and morphometric characteristics. These variables were individualized for each of the 61 gauging stations. Three dependent variables that are indicative of minimum streamflow (Q7,10, Q90 and Q95). And seven independent variables that concern to climatic and morphometric characteristics of the basin (total annual rainfall – Pa; total semiannual rainfall...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Principal component analysis; Cluster analysis; Homogeneous regions.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500838

SPRAY NOZZLES PERFORMANCE IN FUNGICIDES APPLICATIONS FOR ASIAN SOYBEAN RUST CONTROL
Provedor de dados: 70
Autores: Durão,Cléber França; Boller,Walter.
ABSTRACT: The performance of fungicides in controlling Asian soybean rust depends, in part, the spray quality of these products. The market of components to spray offers new types of nozzles which generate droplets with different characteristics. This study aimed to verify whether applications of fungicides with different spray nozzles interfere in soybean rust control. The experiment was conducted in the 2013/2014 harvest. The experimental design was a randomized block with three replications, and compared ten spray nozzles and a control without fungicide application. The applications were made with a backpack sprayer pressurized with CO2, set to apply a spray volume of 150 L ha-1. For the determination of severity four plants per plot were sampled,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycine max; Phakopsora pachyrhizi; Chemical control; Application technology.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000400709

GPS receivers for georeferencing of spatial variability of soil attributes
Provedor de dados: 70
Autores: Rosalen,David L; Rodrigues,Marcos S; Chioderoli,Carlos A; Brandão,Flavia J. C; Siqueira,Diego S.
The characterization of the spatial variability of soil attributes is essential to support agricultural practices in a sustainable manner. The use of geostatistics to characterize spatial variability of these attributes, such as soil resistance to penetration (RP) and gravimetric soil moisture (GM) is now usual practice in precision agriculture. The result of geostatistical analysis is dependent on the sample density and other factors according to the georeferencing methodology used. Thus, this study aimed to compare two methods of georeferencing to characterize the spatial variability of RP and GM as well as the spatial correlation of these variables. Sampling grid of 60 points spaced 20 m was used. For RP measurements, an electronic penetrometer was used...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; GNSS; Compaction; Soil water content.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600013

Características da pulverização em citros em função do volume de calda aplicado com turbopulverizador
Provedor de dados: 70
Autores: Ramos,Hamilton h.; Yanai,Kiyoshi; Corrêa,Ila M.; Bassanezi,Renato B.; Garcia,Luis C.
Este trabalho teve como objetivo avaliar o efeito do volume de calda aplicado por um turbopulverizador sobre a deposição e a cobertura em folhas, ramos e frutos de citros. A pulverização foi realizada com um pulverizador tratorizado Arbus 2000/Valência em pomar de laranja 'Natal', com porte médio de 4,0 m, sendo avaliados seis volumes de calda (50; 70; 85; 100; 150 e 200% do volume-padrão utilizado pelo produtor, de 28 L planta-1). Após a pulverização de plantas uniformes com calda contendo cobre e o traçador fluorescente Poliglow 830 YLSS, amostras foram coletadas em nove setores da planta, sendo a avaliação da deposição feita usando-se análise do íon cobre por espectrofotômetro de absorção atômica, e a da cobertura, por meio de imagens digitalizadas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Deposição; Cobertura; Tecnologia de aplicação.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200009

Shewhart's control charts and process capability ratio applied to a sewage treatment station
Provedor de dados: 70
Autores: Orssatto,Fábio; Vilas Boas,Marcio A.; Nagamine,Ricardo; Uribe-Opazo,Miguel A.
The current study used statistical methods of quality control to evaluate the performance of a sewage treatment station. The concerned station is located in Cascavel city, Paraná State. The evaluated parameters were hydrogenionic potential, settleable solids, total suspended solids, chemical oxygen demand and biochemical oxygen demand in five days. Statistical analysis was performed through Shewhart control charts and process capability ratio. According to Shewhart charts, only the BOD(5.20) variable was under statistical control. Through capability ratios, we observed that except for pH the sewage treatment station is not capable to produce effluents under characteristics that fulfill specifications or standard launching required by environmental...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: STS; Sewage; Process Capability; Shewhart Control Chart.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400016

PREDICTING THE PERFORMANCE PARAMETERS OF CHISEL PLOW USING NEURAL NETWORK MODEL
Provedor de dados: 70
Autores: Marey,Samy; Aboukarima,Abdulwahed; Almajhadi,Yousef.
ABSTRACT This study examines the capability of an artificial neural network (ANN) approach using a backpropagation-learning algorithm to predict performance parameters for a chisel plow at three field sites with differing soils. The draft force, effective field capacity (EFC), fuel consumption rate (FC), overall energy efficiency (OEE), and rate of plowed soil volume (SVR) were predicted at varying plowing speeds, plowing depths, soil moisture contents, soil bulk densities, soil texture indexes, and tractor powers. Collected field data was divided into a training set (for predicting the required parameters) and testing set (for model validation). For the ANN algorithm, the number of hidden layers, neurons, and transfer functions were varied to construct...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Backpropagation-learning algorithm; Draft; Fuel consumption; Overall energy efficiency.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600719

THE ROLE OF CHAR FORMATION IN EQUILIBRIUM MODELING OF GASIFICATION PROCESSES
Provedor de dados: 70
Autores: Ramos,Vinícius F.; Costa Junior,Esly F. da; Costa,Andréa O. S. da.
ABSTRACT This work aims to develop and validate a model based on chemical equilibrium to predict the composition of syngas produced by gasification of woody biomass (sawdust). The model uses Gibbs Energy minimization to evaluate the composition of the system in chemical equilibrium. The results are validated by comparison between experimental data from a gasification experiment and those of other similar models in the literature. The study shows good agreement among experimental results and elucidates the role of solid unburned carbon in such systems, which is present in considerable amount. It can be concluded that equilibrium models can be used to predict carbon conversion in gasification systems.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Char formation; Gasification; Gibbs energy minimization; Modeling.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000200139

Estimación de la evapotranspiración de referencia para dos zonas (Costa Y Región Andina) del Ecuador
Provedor de dados: 70
Autores: Vega,Emil C.; Jara,Jorge C.
Em duas zonas de latitudes similares e com diferentes altitudes, tais como Portoviejo (Região Costa) e Riobamba (Região Andina) no Equador, procurou-se ajustar os modelos de Holdridge (Ho) e Hargreaves-Samani (H-S) e com três modificações (modelos com constantes C HO e KE e KT Diário, Mensal e Anual, respectivamente) com o propósito de estimar a evapotranspiração de referência (ETo), em diferentes níveis das médias móveis do tempo, para o período de três dias. Uma vez ajustados os coeficientes C HO, KE e KT, estimou-se a ETo e foram validados os resultados mediante comparação com as mensurações da ETo, utilizando-se da evaporação do tanque Classe A com seu respectivo coeficiente (ETo Pan). Nos coeficientes C HO (Ho) e KE (H-S), o melhor desempenho foi...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiração de referência (ETo); Altitude; Temperatura; Déficit de pressão de vapor; Hargreaves-Samani.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300006

Corn production for silage intercropped with forage in the farming-cattle breeding integration
Provedor de dados: 70
Autores: Mendonça,Veridiana Z. de; Mello,Luiz M. M. de; Pereira,Francisco C. B. L.; Silva,José O. da R.; Yano,Élcio H.
Corn cropping for silage, due to the plant material exportation, intercropping with forage provides greater ground cover and straw formation for the Direct Planting System (DPS) continuity. The objective of this study was to evaluate corn production for silage in DPS intercropped with four forages (Urochloa brizantha cv. Marandu, U. ruziziensis cv. Ruziziensis, Panicum maximum cv. Tanzânia and P. maximum cv. Áries). We applied three sowing methods (in row together with corn fertilizer; by no-till sowing simultaneously to corn sowing and at V4 corn stage) and corn without intercropping. The experiment was conducted in autumn/ winter of 2010, in Selvíria - MS, in a randomized block design in factorial arrangement (4 x 3 + 1) and 4 replications. For corn, we...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Direct sowing; Interspecific competition; Sowing mode; Mulching.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000400013

Low-flow estimates in regions of extrapolation of the regionalization equations: a new concept
Provedor de dados: 70
Autores: Pruski,Fernando F.; Rodriguez,Renata Del G.; Nunes,Aline A.; Pruski,Pedro L.; Singh,Vijay P.
ABSTRACT Knowledge of natural water availability, which is characterized by low flows, is essential for planning and management of water resources. One of the most widely used hydrological techniques to determine streamflow is regionalization, but the extrapolation of regionalization equations beyond the limits of sample data is not recommended. This paper proposes a new method for reducing overestimation errors associated with the extrapolation of regionalization equations for low flows. The method is based on the use of a threshold value for the maximum specific low flow discharge estimated at the gauging sites that are used in the regionalization. When a specific low flow, which has been estimated using the regionalization equation, exceeds the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water availability; Planning and management of water resources; Water safety.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000500808

Efeitos da temperatura do ar, linhagem e período do dia nas freqüências de ocorrências e tempos de expressão comportamental de matrizes pesadas
Provedor de dados: 70
Autores: Pereira,Danilo F.; Salgado,Douglas D.; Nääs,Irenilza A.; Penha,Nárima L. J.; Bighi,Camila A.
Ajustes de comportamento podem ocorrer rapidamente e a custo menor do que os ajustes fisiológicos. Considerando o comportamento social, é sugestivo que a freqüência e a intensidade de interações agressivas, o total de coesão social e a extensão de vícios sociais possam ser utilizados para avaliação de bem-estar. Esta pesquisa apresenta uma análise das interações entre os fatores experimentais, como temperatura, linhagem e período do dia, nos comportamentos de matrizes pesadas alojadas em câmara climática, buscando evidenciar as diferentes reações das aves submetidas a distintas condições ambientais. Os resultados encontrados mostraram diferenças significativas entre os comportamentos expressos pelas diferentes linhagens, reforçando a necessidade do...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bem-estar animal; Interações; Suporte à tomada de decisão.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000400002

Característica da deposição e distribuição da calda de pulverização na cultura da soja em estádio fenológico V6
Provedor de dados: 70
Autores: Constantin,Jamil; Sales,José G. C.; Maciel,Cleber D. de G.
O trabalho teve como objetivo avaliar a eficácia da deposição da calda de pulverização produzida por diferentes modelos de pontas de pulverização e pressões de trabalho no estádio fenológico V6 da cultura da soja. Oito tratamentos e cinquenta repetições foram estudados em delineamento inteiramente casualizado, em esquema fatorial 4x2, representados por quatro modelos de pontas de pulverização do fabricante Magno® e duas condições de pressão de trabalho (207 e 414 kPa), constituindo os tratamentos: AD 11002 (152 L ha-1 e 208 L ha-1); AD/D 11002 (152 L ha-1 e 208 L ha-1); AD-IA/D 11002 (152 L ha-1 e 208 L ha-1); MAG 2 e MAG 3 (157 L ha-1 e 212 L ha-1). Para monitorar a deposição das caldas de pulverização, utilizou-se dos traçadores Azul Brilhante FD&amp;C-1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Corante; Pontas de pulverização; Glycine max.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300012

Spraying systems and traveling speed in the deposit and spectrum of droplets in cotton plant
Provedor de dados: 70
Autores: Cavalieri,Jhonatan D.; Raetano,Carlos G.; Madureira,Ronaldo P.; Moreira,Lais L. Q.
ABSTRACT Tractor traveling speed can influence the quality of spraying depending on the application technology used. This study aimed to evaluate the droplet spectrum, the deposition and uniformity of spray distribution with different spraying systems and traveling speeds of a self-propelled sprayer in two phenological stages of the cotton plant (B9 and F13). The experimental design was randomized blocks and treatments were three spraying techniques: common flat spray tips; tilted flat jet with air induction, at 120 L ha-1; and rotary atomizer disk, 20 L ha-1, combined with four traveling speeds: 12, 15, 18 and 25 km h-1, with four replications. Spraying deposition was evaluated for both leaf surfaces from the cotton plant apex and base (stage B9) and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Application technology; Rotary atomizer disk; Rotating nozzle; Gossypium hirsutum L.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601042

Material embodiment and energy flows as efficiency indicators of soybean (Glycine max) production in Brazil
Provedor de dados: 70
Autores: Romanelli,Thiago L.; Nardi,Hudson de S.; Saad,Filipe A.
As the requirement for agriculture to be environmentally suitable there is a necessity to adopt indicators and methodologies approaching sustainability. In Brazil, biodiesel addition into diesel is mandatory and soybean oil is its main source. The material embodiment determines the convergence of inputs into the crop. Moreover, the material flows are necessary for any environmental analysis. This study evaluated distinct production scenarios, and also conventional versus GMO crops, through the material embodiment and energy analysis. GMO crops demanded less indirectly applied inputs. The energy balance showed linearity with yield, whereas for EROI, the increases in input and yield were not affected.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Production systems; GMO; Environmental management; Energy balance; EROI.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200006

Segurança das condições de trabalho de tratorista em aplicações de herbicidas em soja e amendoim e eficiência de equipamentos de proteção individual
Provedor de dados: 70
Autores: Cristóforo,Adriano B.; Machado Neto,Joaquim G.
Teve-se o objetivo de avaliar a eficiência de um conjunto de equipamentos de proteção individual no controle das exposições proporcionadas ao tratorista aplicando herbicidas nas culturas de soja e de amendoim com o pulverizador de barra e a segurança dessas condições de trabalho. Os pulverizadores utilizados foram os convencionais empregados nas duas culturas para as aplicações de herbicidas em pré-plantio incorporado (ppi), em pré-emergência (pré) e em pós-emergência inicial (pós), com volumes de 200 L ha-1, e 150 L ha-1 apenas na aplicação em pós, na cultura de soja. As exposições sem EPIs foram de 102,77 mL de calda por dia nas aplicações em ppi, 39,62 em pré e 47,14 em pós-emergência. A eficiência dos EPIs no controle das exposições dérmicas foi de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Herbicidas; Soja; Amendoim; Risco de intoxicação.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000200001

Broilers'toes asymmetry and walking ability assessment
Provedor de dados: 70
Autores: Nääs,Irenilza de A.; Baracho,Marta dos S.; Salgado,Douglas D.; Sonoda,Lilia T.; Carvalho,Victor R. C.; Moura,Daniella J. de; Paz,Ibiara C. L. A.
Brazilian poultry production nowadays occupies important position in world's economy due to its technological advancement, which associated to the development of genetic strains of high growth may cause deviation in the growth rate and harm production. Morphological asymmetry has been pointed as an indicator of welfare, as maintained the pattern that leads to balance, the broiler chicken would have its normal locomotion characteristics, freely reaching water and feed. Thus, the objective of this research was to verify the possibility of using morphological asymmetry for evaluating walking ability of broiler chicken. The research was done in the Technology Center, at UNICAMP. The experiment was made using biomechanics analysis and following, the toes were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Animal welfare; Biomechanics; Morphological asymmetry.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000400004

USE OF RESIDUES FROM THE CELLULOSE INDUSTRY AND SUGARCANE BAGASSE IN PARTICLEBOARDS
Provedor de dados: 70
Autores: da Silva,Sérgio A. M.; Minillo,Larissa Q.; Aquino,Vinícius B. de M.; Lahr,Francisco A. R.; Christoforo,André L.
ABSTRACT The use of alternative materials such as lignocellulosic residues in the production of particleboards has increased considering that these residues are produced in large volumes and often do not have an appropriate destination. This research studied the use of residues from cellulose industries, sugarcane bagasse, and castor oil-based polyurethane resin in the production of wooden panels and evaluated the influence of using these residues on the physical and mechanical properties of the panels. The products were manufactured according to the Brazilian standard ABNT NBR 14810 and the requirements of the panels were evaluated based on national and international standards. All treatments partially met the regulatory requirements. The addition of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Industrial residues; Eucalyptus; Sugarcane bagasse; Particleboards; Castor oil-based resin.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100107

Numerical evaluation of the modulus of longitudinal elasticity in structural round timber elements of the Eucalyptus genus
Provedor de dados: 70
Autores: Christoforo,André L.; Panzera,Túlio H.; Batista,Fabiano B.; Borges,Paulo H. R.; Lahr,Francisco A. R.
Currently, the standards that deal with the determination of the properties of rigidity and strength for structural round timber elements do not take in consideration in their calculations and mathematical models the influence of the existing irregularities in the geometry of these elements. This study has as objective to determine the effective value of the modulus of longitudinal elasticity for structural round timber pieces of the Eucalyptus citriodora genus by a technique of optimization allied to the Inverse Analysis Method, to the Finite Element Method and the Least Square Method.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Round timber; Finite Element Method; Least Square Method.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500018

EXCEL ADD-IN TO MODEL THE SOIL COMPRESSION CURVE
Provedor de dados: 70
Autores: Gubiani,Paulo I.; Reinert,Dalvan J.; Reichert,José M.; Goulart,Rafael Z.; Fontanela,Eracilda.
ABSTRACT Soil compression curve (CC) provides parameters to identify soil load-bearing capacity and susceptibility to compaction. An Excel add-in (ACC) incorporating graphical procedures for mathematical models for soil CC description and calculation of parameters was developed. By using the ACC, soil CC can be described by means of the Casagrande method, mathematically operationalized with the van Genuchten equation, with or without restrictions on its parameters, and by Dias Junior and Pierce method in its original form and also modified using the void ratio rather than soil bulk density. The ACC uses a single Excel spreadsheet for input and output data, in addition to a graphical interface and a tool for exporting editable charts. Compared to SAS...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Compressibility; Precompression stress; Load-bearing capacity.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300603

Desenvolvimento e produtividade do maracujazeiro-amarelo irrigado sob diferentes lâminas de irrigação em ambiente protegido e natural
Provedor de dados: 70
Autores: Carvalho,Jacinto de A.; Koetz,Marcio; Sousa,Alexandre M. G. de; Souza,Kleber J. de.
A irrigação é uma prática que, além de aumentar a produtividade, pode proporcionar a obtenção de um produto com melhor qualidade. O cultivo do maracujazeiro em ambiente protegido não é uma atividade comum, sendo necessária a pesquisa sob esta condição, especialmente sobre a irrigação. Este trabalho foi conduzido com o objetivo de avaliar o efeito das diferentes tensões de água no solo sobre o comportamento da cultura em ambiente protegido e natural, na região de Lavras - MG. O experimento foi instalado em ambiente protegido e natural na área experimental da Engenharia -UFLA, com delineamento em blocos casualizados e quatro repetições. Os tratamentos foram constituídos de quatro tensões de água no solo, preestabelecidas em 15; 30; 45 e 60 kPa, à...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Manejo de irrigação; Ambiente protegido; Passiflora edulis Sims f. flavicarpa Deg.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000500009

HIGH PRECISION WEIGHING LYSIMETERS FOR EVAPOTRANSPIRATION MEASUREMENTS OF SUGARCANE PRE-SPROUTED PLANTLETS
Provedor de dados: 70
Autores: Libardi,Luís G. P.; Faria,Rogério T. de; Dalri,Alexandre B.; Rolim,Glauco de S.; Palaretti,Luiz F.
Abstract Sugarcane pre-sprouted plantlets (PSP) production system is an innovative method to enhance crop multiplication rate. Determination of crop evapotranspiration (ETc) is crucial for water requirement identification throughout the plant cycle for irrigation management. ETc can be satisfactorily measured by weighing lysimeters. The objective of the study was to construct and calibrate three low-cost weighing lysimeters to measure ETc of PSP. The built lysimeters had 0.6909 m2 area (1179 mm × 586 mm), with 400 mm depth supported by 3 load cells. Lysimeters calibration showed excellent precision measurements, due to high linear correlation (R2 = 1.0000) between electric signal and equivalent mass, high accuracy, confirmed by mean absolute error between...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation; Water balance; Water requirement.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000200208

Tamanho amostral para ensaios de mecanismos dosadores de sementes de milho em esteira carpetada
Provedor de dados: 70
Autores: Dias,Vilnei de O.; Alonço,Airton dos S.; Carpes,Dauto P.; Veit,André A.; Souza,Lucas B. de.
Devido à grande diversidade de tamanhos amostrais empregados em avaliações de desempenho de mecanismos dosadores de sementes, o objetivo deste trabalho foi determinar o tamanho de amostra para experimentos em laboratório, com dosadores de sementes tipo disco alveolado horizontal e pneumático, e estudar o efeito dos tratamentos na regularidade de distribuição de sementes da cultura do milho. Para isso, foi conduzido experimento em condições de laboratório, conforme a norma ISO 7256/1. Os tratamentos compreenderam a combinação de quatro mecanismos dosadores (dois pneumáticos e dois de disco alveolado horizontal), com três velocidades de semeadura, de 0,7; 1,4 e 2,1 m s-1. Foram utilizados os métodos de determinação do tamanho de amostra, intensidade de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Semeadoras de precisão; Espaçamentos aceitáveis; Bootstrap.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000500021

AGRONOMIC PERFORMANCE OF RADISH GENOTYPES UNDER DIFFERENT IRRIGATION DEPTHS
Provedor de dados: 70
Autores: Cunha,Fernando F. da; Souza,Ivan P. de; Campos,Washington de O.; Andrade Júnior,Valter C. de; Magalhães,Thiago A.
ABSTRACT In radish production, the choice of proper genotypes and irrigation regime is of great importance to achieve success. In light of this, the current study aimed to evaluate the agronomic performance of a few radish genotypes under different irrigation strategies. The plants were grown in the city of Unaí - MG, in Brazil, under field conditions, and during two cycles, one of 40 days (from February 28 to April 8, 2015) and other of 51 days (from May 9 to June 28, 2015). The experimental design was a randomized block design in a split-plot arrangement with four replications. The treatments consisted of four irrigation strategies (50, 75, 100, and 125% of crop evapotranspiration - ETc) applied by a dripping irrigation system, while subplots consisted...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Horticulture; Irrigation management; Raphanus sativus.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162019000200182

WATER-RETAINING POLYMER MITIGATES THE WATER DEFICIT IN Schinus terebinthifolia: PHOTOSYNTHETIC METABOLISM AND INITIAL GROWTH
Provedor de dados: 70
Autores: Beltramin,Francisco A.; Silva,Willian C.; Santos,Cleberton C.; Scalon,Silvana de P. Q.; Vieira,Maria do C.
ABSTRACT The use of water-retaining polymer (hydrogel) can mitigate the damage to the photosynthetic apparatus and increase the robustness of young plants under water deficit conditions. Thus, the aim of this study was to evaluate the effect of water-retaining polymer on the morphophysiological aspects of Schinus terebinthifolia Raddi submitted to water deficit. The studied water regimes were characterized by three plant irrigation management: 1) control: irrigated daily, 2) stress: water deficit (irrigation suspension) and 3) stress + hydrogel: water deficit + water-retaining polymer. The plants were submitted to irrigation suspension until photosynthesis approached zero [1st P0], followed by resumption of irrigation (REI) for 15 days. After REI, until...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brazilian pink pepper; Cerrado biome; Hydrogel; Physiological plasticity.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600684

Integrating professional education, research and extensionin irrigated agriculture technology centers
Provedor de dados: 70
Autores: Rosa,Jadir A.
With the objective to stimulate the use of irrigation and the electric energy fee reduction during night time program granted by the 2004 Federal law, the Government of the state of Paraná, Brazil launched the Night Irrigation Program - NPI. Beyond this discount, the farmer that adheres to NPI will get additional benefits, as completion of the electric grid without cost, subsidized financing of equipment, technical assistance, support with environmental farm compliance, and the possibility of replacing the entire pump energy matrix. As part of the NPI strategy of action, installation of learning centers for irrigation technology was planned in agricultural schools, thus contributing both to improve technical professional training in agriculture, and for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Family farming; Water use; Electric energy; Vocational training.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600018

Movimento de nitrato proveniente de água residuária em colunas de solos
Provedor de dados: 70
Autores: Gomes,Eliane R. S.; Sampaio,Silvio C.; Corrêa,Marcus M.; Vilas Boas,Márcio A.; Alves,Luis F. A.; Sobrinho,Teodorico A.
O presente trabalho foi realizado visando à avaliação do movimento do nitrato (N-NO-3) proveniente de águas residuárias de frigorífico, em colunas de solo. No experimento, foram utilizados dois tipos de solo, um de textura argilosa e outro de textura arenosa, ambos corrigidos com calcário, quatro colunas de PVC, de 500 mm de comprimento e 75 mm de diâmetro. Após saturação com CaCl2 0,01 M, foi mantida na parte superior de cada coluna, por meio de frasco de Mariotte, uma lâmina de 100 mm da água residuária, que permitiu uma lâmina total de infiltração correspondente a 2,5 vezes o volume total de poros de cada coluna avaliada. Foi coletado, para cada coluna, um total de 100 amostras do efluente percolado, sendo analisadas 20 amostras com intervalo de cinco...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poluição do solo; Dinâmica de soluto; Lixiviação de sais.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300008

Estimation of evaporation in the Banabuiú dam, in the state of Ceará, Brazil, by different combined methods, derived from the Penman equation
Provedor de dados: 70
Autores: Leão,Raimundo A. de O.; Soares,Antônio A.; Teixeira,Adunias dos S.; Silva,Demetrius D. Da.
The state of Ceará, Brazil, has 75% of its area covered by Brazilian semiarid, with its peculiar features. In this state, the dams are constituted in water structure of strategic importance, ensuring, both in time and space, the development and supply of water to population. However, construction of reservoirs results in various impacts that should be carefully observed when deciding on their implementation. One of the impacts identified as negative is the increased evaporation, which constitutes a major component of water balance in reservoirs, especially in arid regions. Several methods for estimating evaporation have been proposed over time, many of them deriving from the Penman equation. This study evaluated six different methods for estimating...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dams; Semiarid; Hydrologycal modelling; Water balance.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000100014

Trickle irrigation: effects on papaya crop
Provedor de dados: 70
Autores: Carvalho,Gian C.; Coelho,Eugênio F.; Silva,Afrânio dos S. A. M. da; Pamponet,Arthur J. M.
The objective of this study was to evaluate growth and yield of papaya cv. Sunrise solo under trickle irrigation system configurations. A random block design was used with six treatments and four replications. Treatments were: T1- a 32 L h-1 micro sprinkler; T2 - a 43 L h-1 micro sprinkler and T3 - a 60 L h-1 micro sprinkler for four plants; T4 - Drip system with four emitters per plant on one lateral line per crop row; T5 - Drip system with eight emitters per plant on two laterals line per crop row; T6 - Drip system with four emitters per plant on one lateral line distributed as pig tail. The dripper flow rate was 4 L h-1and they were apart each other 0.50 m. Crop growth variables were measured every two weeks. Production variables were evaluated during...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carica Papaya L; Yield; Trickle irrigation systems.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200005

Fragment size of corn silage according to the dry matter and forage harvester adjustments
Provedor de dados: 70
Autores: Weirich Neto,Pedro H.; Garbuio,Paulo W.; Souza,Nátali M. de; Delalibera,Hevandro C.; Leitão,Khetlen.
In Brazil, the best results in milk production are found in the state of Paraná. Such results are reached through genetic selection of the animals and management of their diets, in which whole plant corn silage is widely used. Aiming the silage quality, it was evaluated the influence of dry matter content of the corn culture as forage and the harvester adjustments on the fragment size of whole plant corn silage. The fragment size of two corn hybrids silage (SPEED and 2B688) was evaluated using a 5x3 factorial, with 4 repetitions. The first factor was the harvest time of the plants (105, 108, 112, 118, and 123 days after sowing (DAS)), which determines the forage dry matter (DM) content. The second factor was the harvester adjustments (2, 6.5 and 11mm of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ensilage; Whole plant silage; Harvest time.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400016

Teores de macronutrientes em folhas de bananeira CV. Pacovan Apodi, sob lâminas de irrigação e doses de potássio
Provedor de dados: 70
Autores: Barroso,Andréia de A. F.; Viana,Thales V. de A.; Marinho,Albanise B.; Costa,Solerne C.; Azevedo,Benito M. de.
Por meio da análise química da folha, é possível avaliar o estado nutricional da planta, em que os resultados obtidos são comparados a padrões (correlação entre a concentração do nutriente nas folhas e o desenvolvimento da cultura). Objetivou-se, com este trabalho, avaliar as concentrações de macronutrientes nas folhas de bananeira sob lâminas de irrigação e doses de potássio na chapada do Apodi, Ceará. Utilizou-se o delineamento experimental em blocos casualizados, com arranjo em parcelas subdivididas, com três repetições. Foram empregadas cinco lâminas de irrigação (na parcela): 50%, 75%, 100%, 125% e 150% da ETc do lisímetro e quatro doses de potássio (na subparcela): 0%, 60%, 140% e 200% de K2O (recomendada pela análise do solo). As variáveis...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Musa spp; Análise foliar; Manejo da irrigação.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300013

Viabilidade econômica do investimento em plataformas de colhedoras de milho em espaçamento reduzido
Provedor de dados: 70
Autores: Dias,Vilnei de O.; Souza,Renato S. de; Alonço,Airton dos S.
Com o objetivo de avaliar a relação custo/benefício da adoção de espaçamento reduzido na cultura do milho em relação à aquisição de uma plataforma específica para a colheita mecanizada de grãos, foi realizado um estudo considerando as diferentes variáveis que interferem no investimento. Para tal, foi confeccionado um fluxo de caixa diferencial. Foram calculados com base no fluxo de caixa os indicadores de viabilidade econômica Valor Presente Líquido (VPL), Período de Retorno do Capital (PRC) e Taxa Interna de Retorno (TIR). Fez-se, ainda, a análise de sensibilidade sobre o VPL para variações no aumento da produtividade. Os VPLs encontrados ficaram entre R$ -32.157,00 e R$ 484.022,00. O PRC variou de 1,74 a 17,13 anos, e a TIR de -0,70 a 55,04%. A...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Custos de produção; Colheita mecanizada; Zea mays.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000300015

KINETICS OF MASS LOSS OF ARABICA COFFEE DURING ROASTING PROCESS
Provedor de dados: 70
Autores: VARGAS-ELÍAS,GUILLERMO A.; CORRÊA,PAULO C.; SOUZA,NATÁLIA R. DE; BAPTESTINI,FERNANDA M.; MELO,EVANDRO DE C.
ABSTRACT Roasting is one of the most complex coffee processing steps due to simultaneous transfers of heat and mass. During this process, beans lose mass because of fast physical and chemical changes that will set color and flavor of the commercial coffee beverage. Therefore, we aimed at assessing the kinetics of mass loss in commercially roasted coffee beans according to heating throughout the processing. For that, we used samples of 350-g Arabica coffee processed grains with water content of 0.1217 kga kg-1, in addition to a continuous roaster with firing gas. The roaster had initial temperatures of 285, 325, 345 and 380 °C, decreasing during the process up to 255, 285, 305 and 335 °C respectively. Mass loss was calculated by the difference between grain...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica; Mass decrease; Roasting degree; Roasting temperature; Non-isothermal roasting.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200300

Preventive diagnosis of dairy cow lameness
Provedor de dados: 70
Autores: Mollo Neto,Mario; Nääs,Irenilza de A.; Carvalho,Victor C. de; Conceição,Antonio H. Q.
This research aimed to develop a Fuzzy inference based on expert system to help preventing lameness in dairy cattle. Hoof length, nutritional parameters and floor material properties (roughness) were used to build the Fuzzy inference system. The expert system architecture was defined using Unified Modelling Language (UML). Data were collected in a commercial dairy herd using two different subgroups (H1 and H2), in order to validate the Fuzzy inference functions. The numbers of True Positive (TP), False Positive (FP), True Negative (TN), and False Negative (FN) responses were used to build the classifier system up, after an established gold standard comparison. A Lesion Incidence Possibility (LIP) developed function indicates the chances of a cow becoming...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Decision-making support; Expert system; Fuzzy inference.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300020

DIRECT CONNECTION PHOTOVOLTAIC SYSTEM IN MULTI-MOTOR APPLICATION FOR THE RURAL SECTOR
Provedor de dados: 70
Autores: Queiroz,André O.; Brito,Alaan U.
ABSTRACT Photovoltaic pumping systems equipped with variable speed drive have been consolidated as an alternative for water supply in rural locations where energy services are unavailable. Such systems are of the direct connection type and, therefore, it is likely that their operation occurs in two situations: when energy is available and when the reservoir is full or the available energy is insufficient for pumping water. Thus, this study aimed to evaluate the shared use of a photovoltaic pumping system equipped with a variable speed drive and the motor load of the agricultural equipment (cassava grater). The tests were performed in the laboratory and subsequently in the field, where data of the grated cassava production was collected in periods when the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Photovoltaic pumping system with variable speed drive; Agricultural equipment; Cassava processing (Manihot esculenta Crantz).
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000300303

Variabilidade espacial de atributos do solo antes e após calagem e fosfatagem em doses variadas na cultura de cana-de-açúcar
Provedor de dados: 70
Autores: Corá,José E.; Beraldo,José M. G.
Avaliou-se a distribuição espacial de atributos do solo por meio de mapas de isolinhas elaborados a partir da variabilidade espacial dos atributos expressa no semivariograma e por meio de interpolação linear, antes e após a aplicação de doses variadas de calcário e fertilizante fosfatado na cultura de cana-de-açúcar. Foram coletadas amostras de solo na intensidade de uma amostra por hectare, na profundidade de 0-0,20 m, em três talhões comerciais de cana-de-açúcar. Os mapas de isolinhas elaborados por meio da krigagem, levando-se em consideração a existência de dependência espacial de atributos do solo, expressa no semivariograma, apresentaram maior precisão e diferentes padrões de ocorrência da distribuição espacial dos atributos, comparados àqueles...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Manejo do solo; Geoestatística.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200005

AGRICULTURAL MACHINERY AND IMPLEMENTS DESIGN PROCESS: GUIDELINES FOR SMALL AND MID-SIZED BUSINESSES
Provedor de dados: 70
Autores: Bergamo,Renato L.; Romano,Leonardo N.
ABSTRACT This study aims at presenting the process of machine design and agricultural implements by means of a reference model, formulated with the purpose of explaining the development activities of new products, serving as a guideline to coach human resources and to assist in formalizing the process in small and medium-sized businesses (SMB), i.e. up to 500 employees. The methodology used included the process modeling, carried out from case studies in the SMB, and the study of reference models in literature. The modeling formalism used was based on the IDEF0 standard, which identifies the dimensions required for the model detailing: input information; activities; tasks; knowledge domains; mechanisms; controls and information produced. These dimensions...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Product development process; Reference model; Prototypes.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100206

Quality of papaya hybrid grown under different irrigation depths
Provedor de dados: 70
Autores: Silva,Mônica S. da; Melo,Alberto S. de; Pedroza,Juarez P.; Gomes,Josivanda P.; M. Júnior,Sebastião de Oliveira.
Irrigation is a practice widely used in fruit production in the Brazilian Northeast region, including in the papaya crop in order to increase their productivity. For the purpose of knowing the productive potential of papaya hybrid irrigated, an experiment was carried out in order to evaluate the performance of a papaya hybrid under different irrigations depths. Four irrigation depths (50, 75, 100 and 125% of ETo) were tested and the reference evapotranspiration was calculated by the Penman-Monteith model. The hybrid papaya used was UENF/Caliman 01, which was planted in single rows, spaced 4 x 2m from each other, and irrigated by dripping. The experimental design in randomized blocks was used with six replications and three plants per plot. The following...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carica papaya L.; Irrigation; Water consumption; Fruit production.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400025

SPATIAL VARIABILITY OF IRRIGATED COMMON BEAN YIELD CORRELATED WITH THE FERTILITY OF A SANDY SOIL
Provedor de dados: 70
Autores: Oliveira,Job T. de; Roque,Cassiano G.; Teodoro,Paulo; Montanari,Rafael.
ABSTRACT The common bean is widely cultivated in Brazil. In the 2016–2017 growing season, an experiment was carried out in a Typic Quartzipsamment (or Neossolo Quartzarênico) soil in the municipality of Cassilândia, MS, Brazil, with the aim of characterizing specific aspects of soil management, using a linear and spatial correlation between the irrigated yield of common beans and the chemical properties of the soil. Soil samples were collected from layers at depths 0.00–0.10 and 0.10–0.20 m, within a grid of 117 georeferenced points. A data analysis was carried out using statistical and geostatistical techniques. A multiple regression analysis showed that about 31% of the grain yield variability of the irrigated common bean crop could be attributed to the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Geostatistics; Soil management; Irrigation; (Phaseolus vulgaris L.).
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000500645

ERRATUM
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400561

Evapotranspiração de referência com base na radiação solar global estimada pelo método de Bristow-Campbell
Provedor de dados: 70
Autores: Conceição,Marco A. F.
A quantidade de água a ser aplicada em sistemas de irrigação é normalmente calculada com base na evapotranspiração de referência (ETo) da região. Vários métodos podem ser empregados para o cálculo de ETo, sendo o de Hargreaves um dos mais adotados. Esse método utiliza valores estimados da radiação solar global (Rs) com base na diferença entre as temperaturas máxima (Tmáx) e mínima (Tmín) do ar. Entretanto, a Rs pode ser calculada por outros métodos, como o de Bristow-Campbell, que também se baseia na diferença entre Tmáx e Tmín. No presente trabalho, foram estimados valores diários da ETo pelo método de Hargreaves, em Jales - SP, com e sem o uso da equação de Bristow-Campbell para cálculo de Rs. Esses valores foram comparados aos obtidos pelo método de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hargreaves; Penman-Monteith; Irrigação.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000400006

KALE SEEDLINGS PRODUCTION IN DIFFERENT SUBSTRATES, CELL VOLUMES AND PROTECTED ENVIRONMENTS
Provedor de dados: 70
Autores: Costa,Edilson; Curi,Thayla M. R. de C.; Figueiredo,Thiago; Binotti,Flávio F. da S.; Cardoso,Eliana D.
ABSTRACT The kale is a brassica, this vegetable presents importance on nutritional and economic patterns. The present study aimed to evaluate the effect of different substrates, trays and protected environment in the formation of kale seedlings. The experiment was conducted in two greenhouses located at the State University of Mato Grosso do Sul - MS. The first environment consisted of an agricultural greenhouse with polyethylene film cover, while the second was an agricultural nursery with monofilament screen and mesh to offer 50% of shading. In each protected environment were used 72 and 128 cells tray and six different compositions of substrates with organic material based on cassava branches (CB) and cattle manure (CM): 1) 100% CM; 2) 20% CM + 80% CB;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Brassica oleracea var acephala; Cassava branches; Cattle manure; Greenhouse; Multi cells.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100046

Força requerida para o desprendimento de frutos de tomate industrial em diferentes estádios de maturação
Provedor de dados: 70
Autores: REIS,ELTON F. DOS; HOLTZ,VANDOIR; COUTO,RÓDNEY F.; VASCONCELOS,LUIS H. C.; CAMPOS,ANDRÉ J. DE.
A colheita do tomate destinado ao processamento, atualmente, é feita com colhedoras automotrizes; para isso, são necessários estudos que viabilizem a melhoria destas colhedoras, reduzindo assim perdas no campo. Este trabalho teve como objetivo quantificar a força necessária para o desprendimento do fruto de tomate de seu pedúnculo em diferentes estágios de maturação. O experimento foi realizado na Fazenda Madeira, no Município de Gameleira de Goiás-GO, e no Laboratório de Engenharia Agrícola da Universidade Estadual de Goiás. Nas condições de campo, os frutos foram retirados avaliando-se a força de tração no sentido axial do pedúnculo ao fruto e, em laboratório, nos sentidos axial e transversal. O trabalho foi realizado no delineamento experimental...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Colheita mecanizada; Tomate industrial; Solanum lycopersicum.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000200293

Production of natural aroma by yeast in wastewater of cassava starch industry
Provedor de dados: 70
Autores: Oliveira,Simone M. M.; Gomes,Simone D.; Sene,Luciane; Christ,Divair; Piechontcoski,Julia.
ABSTRACT 2-Phenylethanol (PE) is an aromatic alcohol with a characteristic odor of roses, widely used in food industry to modify certain aroma compositions in formulations with fruit, jam, pudding, and chewing gums, and also in cosmetic and fragrance industry. This compound occurs naturally in low concentrations in some essential oils from flowers and plants. An alternative to plants extraction are biotechnological processes. This study evaluated 2-phenylethanol’s production in cultivation of Saccharomyces cerevisiae in cassava wastewater originated from starch industry. The substrate was supplemented with glucose and L-phenylalanine in order to obtain higher 2-phenylethanol concentrations and better efficiency in glucose/2-phenylethanol conversion. It was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: 2-phenylethanol; Flavor; Aerobic cultivation.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400721

Análise comparativa de sensores de velocidade de deslocamento em função da superfície
Provedor de dados: 70
Autores: Molin,José P.; Souza,Adriano B. M.; Fontana,Gustavo; Nagumo,Gustavo K.
Um dos fatores que influencia diretamente no desempenho de sistemas mecanizados é a velocidade de deslocamento pela sua importância no planejamento e na execução das operações agrícolas. O objetivo deste trabalho foi avaliar a acurácia de quatro sensores de velocidade, em condições de superfície asfáltica, solo com cobertura vegetal, aclives e declives, acelerações e desacelerações, submetidos a velocidades representativas para aplicações agrícolas. Foram ensaiados dois modelos comerciais de sensores de radar, um sensor de GPS e um sensor óptico. Foram identificadas diferenças significativas para as situações de solo com cobertura vegetal, acelerações e desacelerações. Para a superfície asfáltica, em situação de velocidade constante, os sensores avaliados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sensor; GPS; Radar.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300023

Qualidade do ar, ambiente térmico e desempenho de suínos criados em creches com dimensões diferentes
Provedor de dados: 70
Autores: Campos,Josiane A.; Tinôco,Ilda de F. F.; Baêta,Fernando da C.; Cecon,Paulo R.; Mauri,Aldo L.
Em uma suinocultura, a fase de creche é considerada crítica, na qual o animal fica exposto às condições ambientais do recinto onde está alojado, sem a proteção da matriz e inserido em um meio social coletivo e desconhecido. Essa fase requer ambiente térmico mais aquecido e, por isso, em período de inverno, os abrigos são mantidos mais fechados, o que pode ser agravante em termos de renovação do ar. Este trabalho teve como objetivo avaliar duas creches de dimensões diferentes, em período de inverno, levando-se em consideração o ambiente térmico, a qualidade do ar e o desempenho dos animais alojados nessas instalações. Foram utilizadas duas creches com dimensões diferentes (I e II), ambas sem nenhum tipo de aquecimento. Foram feitas medições de concentrações...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ambiência animal; Conforto térmico; Instalação suinícola.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000300001

Rolo destorroador após a semeadura do trigo
Provedor de dados: 70
Autores: Garcia,Luiz C.; Morgado,Carlos B.; Dyck,Rogério; Jasper,Roberto; Fornari,Allison J.
Teve-se o objetivo de verificar a influência do rolo destorroador utilizado após a semeadura do trigo, sobre palhada de milho, em duas unidades de produção agrícola. As variáveis analisadas foram: população de plantas 15 dias após a emergência, população de plantas com espigas, grãos por espiga, massa de 1.000 grãos, produtividade e viabilidade econômica da operação. A significativa elevação da população de plantas emergidas com o emprego do rolo destorroador não refletiu nos componentes de produção. Portanto, não se recomenda sua utilização nas condições experimentais.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Plantio direto; Componentes de produção; Palhada de milho.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200019

Distribución espacial de la rugosidad en parcelas agrícolas en Provincia de Buenos Aires - Argentina
Provedor de dados: 70
Autores: Salgado,Héctor.
O uso de imagens SAR para estimar e monitorar a umidade superficial do solo requer que se considere outros fatores que influenciam na retrodifusão do sinal-radar, entre os quais a rugosidade da cobertura da superfície à escala de centímetro é muito importante. Há diversos métodos para determinar a rugosidade, mas muitos são caros ou de operação de campo complexa. Neste trabalho, é apresentado um método versátil e econômico que usa máquina fotográfica e tela quadrada. Cada fotografia é processada numericamente obtendo a altura RMS, como parâmetro da rugosidade da cobertura. Por meio de técnicas geoestatísticas de krigagem é estimada a distribuição espacial da rugosidade. São mostradas experiências em áreas com cobertura de trigo, localizadas na área...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Rugosidade superficial; Microtopografia; Rugosímetro.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000200030

Características físicas e mecânicas de misturas de solo, cimento e cinzas de bagaço de cana-de-açúcar
Provedor de dados: 70
Autores: Valenciano,Martha Del C. Mesa; Freire,Wesley J.
Este trabalho teve por finalidade analisar algumas características de misturas de solo, cimento e cinzas de bagaço de cana-de-açúcar para sua possível utilização na fabricação de materiais alternativos de construção. Para tal, amostras de cinzas de bagaço de cana-de-açúcar foram submetidas a um tratamento prévio que consistia de peneiramento e moagem, antes de serem incorporadas às misturas de solo e cimento. Diferentes combinações de cimento-cinzas foram estudadas, determinando-se, para cada uma delas, a consistência normal e a resistência à compressão simples, aos 7 e 28 dias. Posteriormente, corpos-de-prova moldados com tais misturas de solo-cimento-cinzas foram submetidos a ensaios de compactação, compressão simples e absorção de água. Os resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Resíduo agroindustrial; Cinzas de bagaço de cana-de-açúcar; Resistência à compressão simples.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300001

ECONOMIC AND FINANCIAL VIABILITY OF DIGESTER USE IN CATTLE CONFINEMENT FOR BEEF
Provedor de dados: 70
Autores: Montoro,Stela B.; Santos,David F. L.; Lucas Junior,Jorge de.
ABSTRACT This research analyzes the economic and financial feasibility of implementing a biodigester for confinement of beef cattle on a farm located in the State of São Paulo, through the approach of discounted cash flow. The anaerobic digestion technology arouses interest, due to its advantages with the generation of electricity and the pollution reduction of water resources, soil and air, from the biogas and bio-fertilizer production, high value-added products to cattle raising. It was verified that the treatment system of cattle manure with biodigesters generate biogas and fertilizer as revenue, with free cash flows that enable a return on investment in 3.8 years and return an IRR 26.40% and an MIRR of 10.69%; all above than the minimum rate of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biogas; Biofertilizer; Cattle; Discounted cash flow.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000200353

Perdas de solo e nutrientes por erosão num Argissolo com resíduos vegetais de cana-de-açúcar
Provedor de dados: 70
Autores: Martins Filho,Marcílio V.; Liccioti,Thiago T.; Pereira,Gener T.; Marques Júnior,José; Sanchez,Rodrigo B.
O presente trabalho teve como objetivo determinar as perdas de solo, matéria orgânica (MO) e nutrientes (P, K, Ca e Mg) por erosão, em área cultivada com cana-de-açúcar, cuja palhada é mantida sobre a superfície do solo, localizada em Catanduva - SP, sob um Argissolo Vermelho--Amarelo. Em parcelas experimentais, com 0 (CS0), 50 (CS50) e 100% (CS100) de cobertura sobre a superfície do solo, aplicou-se chuva simulada com intensidade de 60 mm h-1, durante 65 minutos. Análises do sedimento erodido indicaram taxas de enriquecimento da seguinte ordem: 2,7 a 1,9 (MO), 3,8 a 2,7 (P), 1,3 a 1,7 (K), 3,9 a 3,6 (Ca) e 2,9 a 2,6 (Mg) vezes em relação ao solo original para CS0 e CS50, respectivamente. A CS50 propiciou controle significativo da erosão de 69%, mas não...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Processo erosivo; Simulação de chuva; Cobertura do solo.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162009000100002

Soil penetration resistance in a rhodic eutrudox affected by machinery traffic and soil water content
Provedor de dados: 70
Autores: Moraes,Moacir T. de; Debiasi,Henrique; Franchini,Julio C.; Silva,Vanderlei R. da.
Soil compaction caused by machinery traffic reduces crop yields. This study aimed to evaluate the effects of intensive traffic, and the soil water content, on the soil penetration resistance (PR) of a Rhodic Eutrudox (Distroferric Red Latosol, Brazilian Classification), managed under no-tillage (NT). The experiment consisted of six treatments: NT with recent chiseling, NT without additional compaction, and NT with additional compaction by 4, 8, 10 and 20 passes of a harvester with a weight of 100 kN (70 kN on the front axle). Undisturbed soil samples were collected at 5.5-10.5 cm and 13.5-18.5 cm depth to quantify the soil bulk density (BD). The PR was assessed in four periods, using an impact penetrometer, inserted in the soil to a depth of 46 cm. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil layers with mechanical impedance; No-tillage; Soil compaction; Soil consistency; Soil profile.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000400014

Weather variables, water balance, growth, and agro industrial yield of sugarcane
Provedor de dados: 70
Autores: TEODORO,IÊDO; DANTAS NETO,JOSÉ; HOLANDA,LUCAS A. DE; SAMPAIO NETO,GIVALDO D.; SOUZA,JOSÉ L. DE; BARBOSA,GERALDO V. DE S.; LYRA,GUILHERME B.
The objective of this study was to evaluate the meteorological variables, water deficiency, growth, and agro-industrial yield of sugarcane varieties: RB72454, RB863129, RB867515, RB92579, RB93509, RB931003, RB951541, and RB971755, in rainfed crop in two harvests in the Rio Largo-AL region. The meteorological variables were obtained in an automatic station and water balance was done by Thornthwaite &amp; Mather method. During the study period, the air temperature ranged from 16.6 to 35.9 ºC. In the first production cycle rained 1,806 mm and the crop evapotranspiration was 1,775 mm. In the second cycle, the rainfall totaled 1,632 mm and the crop evapotranspiration was 1,290 mm. The average water excess of two production cycles was 689 mm and the water...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Air temperature; Rain; Evapotranspiration; Canopy height.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000100076

EFFECTS OF SOIL WATER AVAILABILITY AND ORGANIC MATTER CONTENT ON FRUIT YIELD AND SEED OIL CONTENT OF CASTOR BEAN1
Provedor de dados: 70
Autores: Lacerda,Rogério D. de; Almeida,Larissa C.; Guerra,Hugo O. C.; Silva,José E. B. da.
ABSTRACT The objective of this study was to assess the sensitivity of the castor bean cultivar “BRS 188 Paraguaçu” to available soil water for plants and soil organic matter content based on their effects on fruit yield and seed oil content. A 2 × 4 factorial experiment was conducted from October 2008 to March 2009 under field conditions using randomized complete block design; two soil organic matter contents (5.0 and 25.0 g·kg−1) and four available soil water levels for plants at the irrigation time (70, 80, 90, and 100% of the total available soil water) with three replicates were tested. On each experimental unit measuring 100 m2, 50 plants were cultivated with a spacing of 2 m × 1 m (24 useful and 26 border plants). Analysis of variance (F test) was...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: “BRS 188 Paraguaçu”; Ricinus communis L.; Irrigation; Biodiesel.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000600703

Avaliação de perdas invisíveis na colheita mecanizada em dois fluxos de massa de cana-de-açúcar
Provedor de dados: 70
Autores: Neves,Jorge L. M.; Magalhães,Paulo S. G.; Moraes,Edson E.; Araújo,Fausto V. M.
Neste trabalho, analisou-se o comportamento da colhedora de cana-de-açúcar picada frente a dois fluxos de alimentação de matéria-prima, mensurando-se as perdas invisíveis, impossíveis de serem quantificadas diretamente no campo, a eficiência de limpeza da colhedora e a velocidade do ar na saída dos extratores. Os ensaios foram realizados sob condições controladas no Centro de Tecnologia Copersucar, em janeiro de 2000. Os resultados apontaram que o fluxo de massa de cana que alimenta a colhedora, na faixa avaliada, não tem influência nas magnitudes das perdas invisíveis totais de cana e na eficiência de limpeza da matéria-prima. A velocidade média do ar na saída do extrator primário foi de 12,0 m s-1, e no extrator secundário, de 9,2 m s-1, com coeficiente...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Colhedora de cana picada; Perdas na colheita; Fluxo de ar.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000300016

Desempenho da cultura da rúcula cultivada em época de verão em túneis baixos de polietileno perfurado
Provedor de dados: 70
Autores: Pereira,Edilaine R.; Silva,Iran J. O.; Moura,Daniella J.; Piedade,Sonia M. S.
O túnel baixo é um tipo de ambiente protegido utilizado, principalmente, em cultivo de espécies de pequeno porte, como alface, morango, pimentão, rúcula e pepino. Por serem estruturas de menor porte, apresentam menor custo de instalação em relação ao túnel alto. A presença de material plástico em sua cobertura proporciona um ganho térmico durante o dia, facilitando o crescimento das plantas, protegendo as culturas do impacto da chuva, dos ventos frios e das temperaturas mínimas. Esta pesquisa teve o objetivo de avaliar o efeito de filme de polietileno com diferentes intensidades de perfurações (0; 5; 10; 15 e 20%), no microclima em túneis baixos e no desenvolvimento da cultura da rúcula (Eruca vesicaria sativa (Mill) Thell) em época de verão. Os resultados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Eruca vesicaria sativa (Mill) Thell; Microclima; Plasticultura.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000200006

Efeito das condições ambientais no nível de ruído emitido por leitões
Provedor de dados: 70
Autores: Silva-Miranda,Kesia O. da; Borges,Giselle; Menegale,Vinícius L. de C.; Silva,Iran Jose O. da.
Objetivou-se, com este trabalho, avaliar a influência das variáveis ambientais nos níveis de ruídos emitidos por suínos e quantificar as faixas em dB comparativamente às condições de conforto térmico estabelecidas pela literatura. O experimento foi conduzido em câmara climática, onde foram alojados cinco leitões em fase de creche, submetidos à variação na temperatura ambiente de 20°C a 38°C e umidade relativa de 50% a 80%. Decibelímetros foram instalados para o registro dos níveis de ruídos e sensores dataloggers para os dados de temperatura e umidade relativa. O nível de atividade foi utilizado para quantificar a movimentação dos animais por intermédio de análise de imagens. Análises de correlação e regressão foram aplicadas nos dados para análise...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ruído animal; Vocalização; Temperatura; Decibelímetro.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000300003

Water requirement and yield of fig trees under different drip irrigation management
Provedor de dados: 70
Autores: Andrade,Irineu P. de S.; Carvalho,Daniel F. de; Almeida,Wilk S. de; Silva,Jonathas B. Gonçalves; Silva,Leonardo D. B. da.
This work aimed to study the effect of drip irrigation management on growth and yield of the 'Roxo de Valinhos' fig tree (Ficus carica L.), at three years old, and to determine crop coefficients (Kc) and its water requirement (ETc) under Baixada Fluminense climate and soil conditions, state of Rio de Janeiro, Brazil. The study was carried out in the experimental area of SIPA (Sistema Integrado de Produção Agroecológica) in Seropédica, Rio de Janeiro State, from July 2011 to May 2012. The experimental area was divided in two blocks, named B1 (sandy clay loam texture) and B2 (loamy sand texture). In each block, irrigation frequencies (IF) of two (T1) and four days (T2) were evaluated, as well as the irrigation absence (T3). Irrigation management and water...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Crop coefficient; Ficus carica L.; TDR; Irrigation frequency; Water balance.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000100003

Evapotranspiração do capim Tanzânia obtida pelo método de razão de Bowen e lisímetro de pesagem
Provedor de dados: 70
Autores: Silva,Leonardo D. B. da; Folegatti,Marcos V.; Villa Nova,Nilson A.
A irrigação de pastagens no Brasil apresentou crescimento acentuado nos últimos anos. No entanto, em função da ausência de pesquisas sobre a aplicação de água em pastagens, o manejo da irrigação não vem sendo realizado de maneira racional. Com o objetivo de contribuir para suprir a carência de informações, neste trabalho, comparou-se a evapotranspiração do capim Tanzânia estimada pelo método de razão de Bowen com a medida por lisímetro de pesagem. O experimento foi conduzido em Piracicaba - SP, entre os dias 21 de julho de 2000 e 15 de julho de 2001. Por meio de um lisímetro de pesagem e um sistema automático de razão de Bowen, foram obtidos valores de evapotranspiração do capim Tanzânia (ETc). A evapotranspiração média do capim Tanzânia foi de 4,13 mm...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Panicum maximum; Balanço de energia; Pastagem irrigada.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300016

Transport of broilers: load microclimate during Brazilian summer
Provedor de dados: 70
Autores: Barbosa Filho,José A. D.; Queiroz,Marília L. V.; Brasil,Daniel de F.; Vieira,Frederico M. C.; Silva,Iran J. O.
The objective of this study was to characterize the microclimatic profile of broiler transport trucks under commercial conditions, in the summer, by continuous monitoring of environmental variables (temperature and air relative humidity). Three loads were monitored from farm to slaughterhouse, considering factors such as distance and day periods (morning, afternoon, and night). To obtain the profile of the environmental variables during journey, data loggers, that determined the microclimate to which birds were submitted, were installed in the trucks; data loggers also allowed visualization of the Enthalpy Comfort Index (ECI) so that load regions could be classified according to heat comfort limits for 6-week old poultries. Temperature, relative humidity,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poultry farming; Animal welfare; Pre-slaughter operations; Heat stress.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000300003

Resistência mecânica do solo e força de tração em hastes sulcadoras de semeadoras-adubadoras em sistema de integração lavoura-pecuária
Provedor de dados: 70
Autores: Conte,Osmar; Levien,Renato; Trein,Carlor R.; Mazurana,Michael; Debiasi,Henrique.
A integração lavoura-pecuária, realizada mediante a implantação de pastagens no inverno e a semeadura de milho ou soja no verão, constitui-se numa alternativa para a diversificação de atividades e ampliação dos lucros. Animais em pastejo, principalmente em áreas agrícolas manejadas sob semeadura direta, podem resultar na compactação adicional do solo, diagnosticada geralmente pelo aumento de resistência do solo à penetração (RP). Com o objetivo de avaliar a correlação entre RP e força de tração (FT) medida em hastes sulcadoras de semeadoras-adubadoras, nos anos de 2004 e 2005, foi conduzido um experimento em São Miguel das Missões - RS, em Latossolo Vermelho (0.540 kg kg-1 de argila). Os tratamentos consistiram em quatro intensidades de pastejo, que...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Compactação do solo; Semeadura direta; Pastejo.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400013

Produção, qualidade dos frutos e estado nutricional da laranja valência sob fertirrigação e adubação convencional
Provedor de dados: 70
Autores: Duenhas,Luiza H.; Villas Bôas,Roberto L.; Souza,Cláudio M. P.; Oliveira,Marcus V. A. M.; Dalri,Alexandre B.
O objetivo deste trabalho foi comparar os efeitos de doses de nitrogênio, fósforo e potássio aplicadas via água de irrigação em comparação à aplicação convencional de fertilizantes, com irrigação e sem irrigação. O experimento foi conduzido em um pomar de laranja 'Valência' (Citrus sinensis Osbeck) localizado em Pratânia - SP, durante três anos consecutivos, e analisados os dados do último ano de observação. As diferentes formas de aplicação dos fertilizantes e a redução das doses fornecidas via água de irrigação não resultaram em diferenças significativas sobre o número médio de frutos e produtividade. Também não foram constatadas diferenças estatísticas dos tratamentos sobre a qualidade do suco e o estado nutricional das plantas, com exceção do teor de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigação; Citrus sinensis; Nutrição de plantas.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100017

Perdas de solo e caracterização física e micromorfológica de crostas formadas em solos sob chuva simulada
Provedor de dados: 70
Autores: Brandão,Viviane dos S.; Silva,Demétrius D. da; Ruiz,Hugo A.; Pruski,Fernando F.; Schaefer,Carlos E. G. R.; Martinez,Mauro A.; Silva,Eduardo O.
Devido aos prejuízos provocados pela erosão sobre sistemas agrários e urbanos, foi desenvolvido este artigo para que se possa estabelecer relação entre a erosão e o selamento formado pelo impacto das gotas de chuva. Para avaliar as perdas de solo e as características físicas e micromorfólogicas das crostas desenvolvidas pelo impacto das gotas de água, foi realizado experimento, utilizando simulador de chuvas, num esquema fatorial 5 x 6, sendo cinco solos (Argissolo Vermelho, Argissolo Vermelho-Amarelo, Latossolo Vermelho-Amarelo, Neossolo Flúvico e Neossolo Quartzarênico) e seis energias cinéticas de chuva simulada (0; 525; 1.051; 2.102; 3.153 e 4.204 J m-2), com três repetições. As perdas de solo foram determinadas por amostragem do volume total de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Selamento; Escoamento superficial; Energia cinética da chuva.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162007000100006

AXENIC CULTIVATION OF Pleurotus ostreatus var. Florida IN SUPPLEMENTED SUGARCANE BAGASSE BRIQUETTES
Provedor de dados: 70
Autores: Magalhães,Anderson C.; Moreira,Bruno R. de A.; Zied,Diego C.
ABSTRACT Articles on the applicability of briquetting to the production of mushrooms are rare. Therefore, this research provides the scientific community and, mainly, producers, unpublished technical information regarding the productive yield of oyster mushroom cultivated in sugarcane bagasse briquettes supplemented with bioproducts of cereals. In 30 days of axenic cultivation, 6 tons-force briquettes with 80% humidity resulted in higher productivity (30.4%), and generated the lowest physical volume of exhausted compound (44.8%), thus, overcoming the technical performance of the other briquetting matrices tested, and even of methods traditionally used for the preparation of substrate for P. ostreatus cultivation on a commercial scale. The conclusion is,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Briquetting; Bioconversion; Edible mushrooms; Productivity.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600835

Soil sampling intensity and spatial distribution pattern of soils attributes and corn yield in no-tillage system
Provedor de dados: 70
Autores: Rodrigues,Marcos S.; Corá,José E.; Fernandes,Carolina.
Taking into account that the sampling intensity of soil attributes is a determining factor for applying of concepts of precision agriculture, this study aims to determine the spatial distribution pattern of soil attributes and corn yield at four soil sampling intensities and verify how sampling intensity affects cause-effect relationship between soil attributes and corn yield. A 100-referenced point sample grid was imposed on the experimental site. Thus, each sampling cell encompassed an area of 45 m² and was composed of five 10-m long crop rows, where referenced points were considered the center of the cell. Samples were taken from at 0 to 0.1 m and 0.1 to 0.2 m depths. Soil chemical attributes and clay content were evaluated. Sampling intensities were...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Geostatistics; Precision agriculture; Zea mays.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000500005

Influência da vazão de água sobre o rendimento de um coletor solar plano construído em termoplástico
Provedor de dados: 70
Autores: Jordan,Rodrigo A.; Seye,Omar; Motomiya,Anamari V. de A.
Resumo Avaliou-se o rendimento térmico de um coletor solar plano construído em termoplástico, em condições reais de operação, registrando as temperaturas de entrada e de saída de água na placa, mediante quatro distintas vazões mássicas de água: 0,026 kg s-1; 0,04 kg s-1; 0,054 kg s-1; e 0,068 kg s-1. Os ensaios foram realizados no Laboratório de Termodinâmica e Energia da Faculdade de Engenharia Agrícola da Unicamp. Com base nos valores de temperatura da água na entrada e na saída das placas, foram calculados os valores de potência térmica [W m-2]. O maior valor médio diário de potência térmica (753 W m-2) foi obtido para a vazão de 0,054 kg s-1. Para a maior vazão (0,068 kg s-1), o valor de potência térmica foi similar ao obtido para a vazão de 0,04 kg...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aquecimento solar; Rendimento térmico; Coletor solar plano; Vazão de água.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400665

Redundant variables and the quality of management zones
Provedor de dados: 70
Autores: Ricardo,Sobjak; Souza,Eduardo G. de; Bazzi,Claudio L.; Uribe-Opazo,Miguel A.; Betzek,Nelson M.
ABSTRACT Precision agriculture (PA) allows farmers to identify and address variations in an agriculture field. Management zones (MZs) make PA more feasible and economical. The most important method for defining MZs is a fuzzy C-means algorithm, but selecting the variable for use as the input layer in the fuzzy process is problematic. BAZZI et al. (2013) used Moran’s bivariate spatial autocorrelation statistic to identify variables that are spatially correlated with yield while employing spatial autocorrelation. BAZZI et al. (2013) proposed that all redundant variables be eliminated and that the remaining variables would be considered appropriate on the MZ generation process. Thus, the objective of this work, a study case, was to test the hypothesis that...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Precision agriculture; Spatial correlation; Relative efficiency.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100078

Modelo para o dimensionamento e a locação de sistemas de terraceamento em nível
Provedor de dados: 70
Autores: Griebeler,Nori P.; Pruski,Fernando F.; Teixeira,Alessandro F.; Silva,Demetrius D. da.
A erosão hídrica é um dos principais causadores da degradação das terras agrícolas, provocando expressivos prejuízos à sociedade. Em virtude desses danos, torna-se fundamental o desenvolvimento de técnicas que permitam o aumento da eficiência das práticas para a conservação do solo. Com esse objetivo, desenvolveu-se um modelo para o dimensionamento e a locação de sistemas de terraceamento em nível, utilizando modelos digitais de elevação do terreno gerados em sistemas de informações geográficas (SIG). A fim de possibilitar a aplicação do modelo desenvolvido, elaborou-se um software que permite a realização das interações necessárias para o dimensionamento do sistema. Os resultados obtidos mostram que o modelo oferece a vantagem de permitir o...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Erosão hídrica; Conservação do solo e água; Planejamento integrado.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000300015

ANAEROBIC DIGESTION STABILITY TEST BY SHEWHART CONTROL CHART
Provedor de dados: 70
Autores: Alcantara,Michael S.; Grisotti,Geovane; Tavares,Maria H. F.; Gomes,Simone D.
ABSTRACT The anaerobic digestion (AD) operation complexity raise the importance of stability testing to verify whether the operating conditions are under control and whether the process is working as required. The current method of verifying process stability is by a range of the ratio between volatile fatty acidity and total alkalinity (VFA/ TA) within which stable conditions are brought about; these rates vary with the content of organic material. A few indicators as pH or constant biogas production are also used. Therefore, the aim of this study was to propose the use of Shewhart control chart for individual measures as a stability test for AD, as well as to demonstrate its use in poultry litter AD. The method showed to be advantageous since it...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Process monitoring; Statistical process control; Waste treatment.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000300618

Establishment of anammox process in sludge samples collected from swine wastewater treatment system
Provedor de dados: 70
Autores: Casagrande,Caroline G; Kunz,Airton; Soares,Hugo M; Prá,Marina C. de; Schierholt Neto,Guilherme F.
The high load of nitrogen present in swine wastewater is one of the biggest management challenges of the activity. The Anammox process emerges as a good alternative for biological removal of nitrogen. This study aims to acclimate sludge collected from swine effluent treatment systems to establish the Anammox process. Two sludge samples were collected at Embrapa Swine and Poultry, Concordia - SC, Brazil, one from the bottom of an inactive anaerobic pond (inoculum A) and another from an aeration tank (inoculum B). Both were acclimated until the depletion of NO3-N, being subsequently inoculated in two reactors (Reactor A - Inoculum A and Reactor B - Inoculum B). The Reactor A showed activity after 110 days of operation, while the Reactor B needed 170 days....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrogen removal; Swine wastewater; Anammox process.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000600014

Codigestão anaeróbia de dejetos de suínos e níveis de inclusão de óleo de descarte
Provedor de dados: 70
Autores: Orrico,Ana C. A.; Sunada,Natália da S; Lucas Junior,Jorge de; Orrico Junior,Marco A. P; Schwingel,Alice W.
RESUMO A codigestão dos dejetos de suínos e dos resíduos lipídicos vem sendo amplamente explorada, com melhorias na degradação dos substratos em digestão e, consequentemente, dos rendimentos de biogás. Assim, foram avaliados os desempenhos de biodigestores abastecidos com dejetos de suínos e crescentes níveis de óleo de descarte, por meio das produções e potenciais de produção de biogás, reduções dos teores de sólidos totais (ST), sólidos voláteis (SV) e da demanda química de oxigênio (DQO). Para o desenvolvimento do ensaio de codigestão, foram preparados substratos compostos por dejetos de suínos, óleo de descarte (nas proporções de 0; 2; 4; 6; 8; 10 e 12% de óleo em relação aos teores de ST do substrato), água para diluição destes resíduos e inóculo,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Biodigestor; Suinocultura; Sólidos totais; Sólidos voláteis.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000400657

SPACIAL ILLUMINANCES VARIABILITY AND ENERGY CONSUMPTION IN AVIARIES FOR LAYING HENS EQUIPED WITH COMPACT FLUORESCENT LAMPS AND LIGHT EMITTING DIODE
Provedor de dados: 70
Autores: Ribeiro,Priscilla A. P.; Yanagi Junior,Tadayuki; Oliveira,Daniela D. de; Ferraz,Gabriel A. E. S.; Lourençoni,Dian.
ABSTRACT The spatial illuminance distribution interferes in the commercial production of eggs and electric energy consumption, being considered the second major source of costs in the production chain. Therefore, in this study the objective was to evaluate the spatial distribution of the illuminance level and electric energy consumption in two commercial aviaries for egg production. The first aviary was equipped with compact fluorescent lamps (CFL) and the second, with light-emitting diode (LED) lamps. The illuminances in the aviaries were analyzed using descriptive statistics and their spatial distribution through geostatistics. It was found that the aviary equipped with CFL showed better uniformity in the illuminances distribution and better results in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Electric energy; Geostatistics; Artificial illumination; Aviary.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000600962

Performance of UASB reactors in two stages under different HRT and OLR treating residual waters of swine farming
Provedor de dados: 70
Autores: Urbinati,Estevão; Duda,Rose M.; Oliveira,Roberto A. de.
In this study it was evaluated the effects of hydraulic retention time (HRT) and Organic Loading Rate (OLR) on the performance of UASB (Upflow Anaerobic Sludge Blanket) reactors in two stages treating residual waters of swine farming. The system consisted of two UASB reactors in pilot scale, installed in series, with volumes of 908 and 188 L, for the first and second stages (R1 and R2), respectively. The HRT applied in the system of anaerobic treatment in two stages (R1 + R2) was of 19.3, 29.0 and 57.9 h. The OLR applied in the R1 ranged from 5.5 to 40.1 kg CODtotal (m³ d)-1. The average removal efficiencies of chemical oxygen demand (COD) and total suspended solids (TSS) ranged, respectively, from 66.3 to 88.2% and 62.5 to 89.3% in the R1, and from 85.5...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Anaerobic digestion; Swine excrements; Methane gas; UASB reactors in series; Two stage treatments.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200015

Análise econômica de milho convencional e transgênico em dois sistemas de preparos de solo
Provedor de dados: 70
Autores: Silva,Paulo R. A.; Correia,Tiago P. da S; Sousa,Saulo F. G.; Millani,Thais M.
RESUMO O milho é um produto de grande importância na agricultura, em função de sua ampla utilização e das formas de produção. Tendo em vista esses cenários, o trabalho teve como objetivo a análise econômica do sistema de produção de milho utilizando diferentes híbridos de milho e preparos de solo. O estudo foi realizado na Fazenda Experimental Lageado, pertencente à Faculdade de Ciências Agronômicas/UNESP de Botucatu-SP. Foram analisados dois híbridos em dois tipos de sistemas de preparo do solo, sendo milho convencional e milho transgênico, em preparo convencional e cultivo mínimo. Para os diferentes tipos de cultivo, foram utilizados os mesmos tratores, implementos e adubação, sendo os seguintes parâmetros analisados: custos operacionais, custos de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Custo operacional; Produtividade; Biotecnologia.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162015000601032

Validação do modelo ClimaBR em relação ao número de dias chuvosos e à precipitação total diária
Provedor de dados: 70
Autores: Zanetti,Sidney S.; Oliveira,Vicente de P. S. de; Pruski,Fernando F.
Este trabalho foi realizado com o objetivo de validar o modelo ClimaBR no que se refere à geração de séries sintéticas de precipitação total diária em diferentes localidades brasileiras. Para tanto, foram geradas séries sintéticas de precipitação para 12 localidades, escolhidas de forma distribuída, para que todas as diferentes regiões de precipitação homogênea do País fossem contempladas. A partir das séries pluviométricas, disponíveis nas estações meteorológicas das localidades selecionadas, o ClimaBR foi utilizado para gerar as séries sintéticas de precipitação, sendo gerada uma série de 100 anos para cada localidade. A qualidade dos resultados foi analisada comparando-se o ajuste entre os valores observados e os gerados pelo ClimaBR, por meio de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chuva; Simulação de dados climáticos; Séries sintéticas.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162006000100011

TIME SERIES TRENDS OF STREAMFLOW AND RAINFALL IN THE SANTO ANTÔNIO RIVER BASIN, BRAZIL
Provedor de dados: 70
Autores: Ferreira,Fernanda L. V.; Rodrigues,Lineu N.; Silva,Demetrius D. da; Teixeira,David B. de S.; Almeida,Laura T. de.
ABSTRACT Detecting trends in streamflow and rainfall series can have great significance for proper water resource management. Thus, the objective of this study was to analyze the trends of historical streamflow and rainfall series using nonparametric statistical tests. A historical series of pluviometric and fluviometric gauges, which belong to the hydrometeorological network of the Brazilian Water National Agency in the Santo Antônio River Basin, Brazil, from 1985 to 2014 were used. By applying statistical tests, it was found that the time series are independent and random, and from the total 24 rainfall gauges evaluated, 12 presented nonstationary behavior, exhibiting mostly decreasing trends. Based on the six fluviometric gauges used for the annual...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Stationarity; Run test; Mann Kendall test; Pettitt test.
Ano: 2021
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100047

Compartimentação fisiográfica para análise ambiental do potencial erosivo a partir das propriedades da rede de drenagem
Provedor de dados: 70
Autores: Nascimento,Paulo S. R.; Garcia,Gilberto J.
O presente trabalho teve como objetivo compartimentar a sub-bacia do Baixo Rio Piracicaba - SP, em unidades homogêneas quanto à potencialidade à erosão visando a subsidiar o gerenciamento ambiental. A importância desta pesquisa concentra-se no intenso desenvolvimento dos processos erosivos na área em foco e na sua importância socioeconômica em níveis estadual e nacional. O procedimento adotado para atingir o objetivo foi a análise da rede de drenagem e dos lineamentos obtidos pelas imagens TM/Landsat-5. O resultado obtido foi a divisão da área em quatro compartimentos quanto à potencialidade à erosão: muito alta, alta, média e baixa. Concluiu-se que a área estudada é heterogênea, com regiões sujeitas a diferentes intensidades de processos erosivos e que a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zonas homólogas; Lineamento; Imagem TM/Landsat-5.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162005000100026

Modelo aplicado à dinâmica da água e do potássio no solo sob irrigação por gotejamento: análise de sensibilidade
Provedor de dados: 70
Autores: Rivera,René N.C.; Miranda,Jarbas H.; Duarte,Sérgio N.; Botrel,Tarlei A.
A compreensão do transporte simultâneo da água e de solutos, a partir de uma fonte pontual, permite desenvolver estratégias eficientes na fertirrigação, sendo importante no dimensionamento, na operação e no manejo de sistemas de irrigação localizada. O presente trabalho teve como objetivo apresentar a análise de sensibilidade de um modelo matemático, desenvolvido para simular o deslocamento simultâneo de água e de potássio na irrigação por gotejamento. A análise de sensibilidade foi realizada com respeito às variações individuais da condutividade hidráulica do solo saturado, umidade inicial e saturada do solo, dispersividade, fator de retardamento e vazão do emissor. Os resultados obtidos revelaram que o modelo matemático, com relação à distribuição de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Deslocamento miscível; Dinâmica de solutos; Modelagem computacional.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000300006

Climate risk in maize crop in the northeastern of Brazil based on climate change scenarios
Provedor de dados: 70
Autores: Silva,Vicente de P. R. da; Campos,João H. B. da C.; Silva,Madson T.
This study evaluates the impacts of climate change on the agricultural zoning of climatic risk in maize crop cultivated in the Northeastern of Brazil, based on the Intergovernmental Panel on Climate Change (IPCC) reports. The water balance model, combined with geospatial technologies, was used to identify areas of the study region where the crops could suffer yield restrictions due to climate change. The data used in the study were the time series of rainfall with at least 30 years of daily data, crop coefficients, potential evapotranspiration and duration of the crop cycle. The scenarios of the increasing of air temperature used in the simulations were of 1.5ºC, 3ºC and 5ºC. The sowing date of maize crop from January to March appears to be less affected...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Global warming; Water balance; Rainfall; Agricultural zoning.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600019

Viabilidade técnica e econômica da produção de ervilha (Pisum sativum L.) cultivada sob diferentes lâminas de irrigação
Provedor de dados: 70
Autores: Oliveira,Eduardo C.; Carvalho,Jacinto de A.; Rezende,Fátima C.; Freitas,Wellington A. de.
Realizou-se, com o presente trabalho, uma avaliação técnica e econômica da produção de ervilha (Pisum satiums L.) em função de lâminas de irrigação. O experimento foi instalado em casa de vegetação, com delineamento inteiramente casualizado (DIC), com cinco tratamentos de reposição de água no solo (50; 75; 100; 125 e 150% da capacidade de campo) e quatro repetições. O momento de irrigar foi definido quando a tensão média da água no solo, obtida nos tensiômetros instalados na parcela com 100% de reposição de água, atingiu 15 kPa. Concluiu-se que a produção da cultura e o número de vagens por planta foram afetados pelo déficit e pelo excesso hídrico aplicados pelos tratamentos. A máxima produtividade obtida foi igual a 4.197 kg ha-1 com a aplicação de 188,4...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pisum sativum L.; Casa de vegetação; Lâmina ótima econômica.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000200012

INFLUENCE OF DRAINAGE METHODS ON SOYBEAN DEVELOPMENT IN LOWLANDS
Provedor de dados: 70
Autores: Rosso,Ricardo B.; Peiter,Marcia X.; Robaina,Adroaldo D.; Ben,Luis H. Bahú; Mezzomo,Wellington.
ABSTRACT The need for crop rotation and profitability in lowland areas are the two main reasons for the introduction of soybean cultivation in the state of Rio Grande do Sul, Brazil. These areas have poor natural drainage, which impedes proper soybean growth. In this sense, this study aimed to assess the efficiency of using broad base ridges in comparison to the surface drainage for soybean cultivation in lowlands. The study was conducted during the 2014/2015 and 2015/2016 growing seasons in São João do Polêsine, RS, Brazil. The assessed drainage methods were the use of broad base ridges with different width dimensions (22.5, 15.0, and 7.5 m) and surface drainage. The results showed that the shoot dry matter and leaf area index have similar behavior. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Ridge; Glycine max; Lowland.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000100045

ERRATA
Provedor de dados: 70
Tipo: Info:eu-repo/semantics/other
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400738

Alterações microclimáticas causadas pelo uso de tela plástica
Provedor de dados: 70
Autores: Pezzopane,José E. M.; Oliveira,Paulo C. de; Reis,Edvaldo F. dos; Lima,Julião S. de S.
Com o objetivo de caracterizar as alterações microclimáticas provocadas pelo uso de tela plástica na agricultura, foi desenvolvido um experimento com alface, em área de cultivo agrícola, em Alegre - ES (latitude 20º45’S, longitude 41º28’W e altitude 150 m), no período de setembro a dezembro de 1996. Foram utilizados sombreamentos de 0; 30; 50, e 70%, segundo especificação comercial. Os resultados mostraram que a tela com especificação comercial de 50% de sombreamento provocou uma atenuação média de 41% na radiação solar global, ocorrendo, no entanto, uma flutuação significativa ao longo do dia em função do movimento aparente do sol. A cobertura com a tela plástica não provocou alterações significativas da temperatura e umidade relativa do ar. Em relação à...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Microclima; Tela plástica; Sombreamento.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000100002

UNCERTAINTY ANALYSIS OF A WEB-BASED DATA ACQUISITION SYSTEM FOR POULTRY MANAGEMENT WITH SENSOR NETWORKS
Provedor de dados: 70
Autores: Yu,Ligen; Teng,Guanghui; Riskowski,Gerald L.; Xu,Xuzhang; Guo,Wenzhong.
ABSTRACT This paper presents a web-based data acquisition system developed by the LabVIEW software program for environment monitoring for poultry management. The measurement error and uncertainty analysis should be conducted accurately to maximize the reliability of this system. An algorithm was proposed for the uncertainty analysis to estimate the sensor networks, with the calibration and validation processes fulfilling the standards of the Guide to the Expression of Uncertainty in Measurement. For the different environmental sensors, the values of the uncertainties were calculated by the methods of type A and B evaluation through a case study. Environmental parameters including air temperature, relative humidity, and CO2 concentration of a compartment...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Uncertainty analysis; Sensor networks; Data acquisition; Measurement; Poultry management.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000600857

Mapeamento das formas do relevo para estimativa de custos de fertilização em cana-de-açúcar
Provedor de dados: 70
Autores: Sanchez,Rodrigo B.; Marques Júnior,José; Pereira,Gener T.; Baracat Neto,Jorge; Siqueira,Diego S.; Souza,Zigomar M. de.
A modelagem matemática associada ao conhecimento da variabilidade dos atributos do solo e mapeamento das formas do relevo pode auxiliar no manejo da fertilidade do solo em usinas sucroalcooleiras. O presente trabalho teve como objetivo avaliar o uso da geoestatística e da modelagem matemática na estimativa de custos de fertilização, em diferentes formas do relevo. Em uma área de 200 ha, foram identificadas duas formas de relevo, uma côncava e outra convexa, sendo os solos coletados nos pontos de cruzamento de uma malha, com intervalos regulares de 50 m, perfazendo um total de 623 pontos. As amostras foram submetidas a análises químicas, e, posteriormente, os dados foram avaliados por meio da estatística descritiva, geoestatística e modelagem matemática. Os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zonas de manejo específico; Taxa variada; Agricultura de precisão.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000200008

Modelagem matemática para seleção de conjuntos mecanizados agrícolas pelo menor custo operacional
Provedor de dados: 70
Autores: Baio,Fábio H. R.; Rodrigues,Andrew D.; Santos,Gilson S. dos; Silva,Simone P. da.
A seleção de uma máquina agrícola pode tornar-se uma tarefa árdua, pois há diversas variáveis que devem ser consideradas. A escolha do equipamento mais adequado para uma propriedade agrícola é uma das etapas mais importantes do processo produtivo. O objetivo deste trabalho foi desenvolver um modelo de computador por programação linear em plataforma web para seleção automatizada de conjuntos mecanizados agrícolas, baseados no menor custo operacional. O programa, desenvolvido em linguagem ASP.NET, pode ser acessado gratuitamente pela Internet (http://www.maquinas.ufms.br). O usuário pode selecionar um conjunto mecanizado agrícola dentro de uma vasta lista de opções que contém suas especificações técnicas ou deixar que o programa lhe retorne automaticamente a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Modelagem computacional; Programação linear; Seleção de máquinas.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200018

Efeito de pontas de pulverização no controle químico da ferrugem da soja
Provedor de dados: 70
Autores: Cunha,João P. A. R. da; Moura,Eudes A. C.; Silva Júnior,Jair L. da; Zago,Flávio A.; Juliatti,Fernando C.
O controle químico eficiente da ferrugem asiática da soja depende da correta seleção da ponta de pulverização. Este trabalho teve o objetivo de avaliar o efeito da utilização de diferentes pontas de pulverização na aplicação de fungicida para o controle da ferrugem da soja. O ensaio foi conduzido no delineamento em blocos ao acaso, com quatro repetições, em esquema fatorial (4 x 2) + 1: quatro tipos de ponta de pulverização (jato plano defletor duplo, jato plano duplo com pré-orifício e jato cônico vazio com e sem indução de ar), dois volumes de aplicação (150 e 200 L ha-1) e um tratamento adicional que não recebeu fungicida. Realizou-se a semeadura direta da cultivar de soja M-SOY 8008 (ciclo precoce), avaliando-se, após a aplicação do fungicida...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tecnologia de aplicação; Glycine max L.; Phakopsora pachyrhizi.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000200009

Efeito da aplicação de água residuária da lavagem dos frutos de café sobre as propriedades químicas do solo
Provedor de dados: 70
Autores: Silva,George B; Rolim,Mário M; Pedrosa,Elvira M. R; Bebé,Felizarda V; Silva,Enio F. F.
O objetivo deste trabalho foi avaliar as alterações químicas de solos tratados com água residuária de café (ARC). O experimento foi conduzido em colunas de PVC, onde foram avaliadas quatro doses de ARC (0; 174; 522 e 870 t ha-1), em dois Argissolos Amarelos subdivididos em quatro camadas, para dois períodos de incubação (30 e 60 dias). O delineamento experimental foi o inteiramente casualizado, em arranjo fatorial, e as variáveis analisadas foram cálcio, magnésio, potássio, sódio, pH e condutividade elétrica do extrato da pasta saturada. As doses de ARC alteraram as propriedades químicas dos solos nos dois períodos de incubação estudados, aumentando os teores de Ca++, Na+ e, principalmente, K+ nos dois solos. A dose de aplicação de 174 t ha-1 de ARC elevou...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reúso; Qualidade ambiental; Coffea sp.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000100016

Qualidade de sementes de soja em função do horário de colheita e do sistema de trilha de fluxo radial e axial
Provedor de dados: 70
Autores: Marcondes,Maria C; Miglioranza,Édison; Fonseca,Inês C. de B.
O trabalho objetivou avaliar dois tipos de colhedoras, de fluxo radial e axial, em relação à qualidade física e fisiológica de sementes de duas cultivares de soja, BRS 184 e BRS 133, colhidas em dois horários, às 10 e 18 horas. A colhedora de fluxo radial trabalhou a 5,0 km h-1 , com o cilindro batedor a 750 rotações por minuto (rpm). A colhedora de fluxo axial trabalhou a 8,0 km h-1, e rotor com 650 rpm. Para a avaliação da qualidade física e fisiológica das sementes, foram realizados testes de germinação, envelhecimento acelerado, tetrazólio, dano mecânico (hipoclorito), umidade de campo e laboratório, sementes quebradas (bandinha) e pureza. A colheita realizada às 18 horas, com grau de umidade menor que 12%, ocasionou maiores danos mecânicos nas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glycine max; Qualidade; Desempenho de colhedora.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162010000200014

Sistema de monitoramento de perdas visíveis de cana-de-açúcar em colhedora de cana picada
Provedor de dados: 70
Autores: Neves,Jorge L. M.; Magalhães,Paulo S. G.; Ota,Walter M.
A área de cana colhida mecanicamente tem crescido, sobretudo em regiões com relevo até 12% de declividade, principalmente por ser essa uma forma de viabilizar a colheita de cana-de-açúcar crua a um custo competitivo. A adoção desse sistema introduz certos inconvenientes, tais como: aumento dos índices de matéria estranha na carga, o que, por sua vez, implica a redução da qualidade tecnológica da matéria-prima fornecida para moagem, e perdas de colmos e/ou frações no campo. A tentativa de reduzir tais índices, por meio do aumento da velocidade de saída de ar dos extratores das colhedoras, pode aumentar as perdas de matéria-prima em níveis inaceitáveis economicamente. Este trabalho avaliou o nível de perdas visíveis de lascas de cana, por meio do extrator...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cana crua; Colheita; Mecanização.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162004000300030

Evaluation of thermorregulatory capacity of dairy buffaloes using infrared thermography
Provedor de dados: 70
Autores: Sevegnani,Kelly B; Fernandes,Danielle P. B; Silva,Silvia H. Modenese-Gorla da.
ABSTRACT The objective of this study was to evaluate the thermoregulatory response of dairy buffaloes in pre-milking and post-milking. To identify animal thermoregulatory capacity, skin surface temperatures were taken by an infrared thermometer (SST), a thermographic camera (MTBP) as well as respiratory rate records (RR). Black Globe and Humidity Index (BGHI), radiating thermal load (RTL) and enthalpy (H) were used to characterize the thermal environment. Artificial Neural Networks analyzed those indices as well as animal physiological data, using a single layer trained with the least mean square (LMS) algorithm. The results indicated that pre-milking and post-milking environments reached BGHI, RR, SST and MTBP values above thermal neutrality zone for...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Buffalo; Heat stress; Respiratory rate; Surface temperature.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000100001

Enhancing the analytical capacity for biogas development in Brazil: assessment of an original measurement system for low biogas flow rates out of agricultural biomass residues
Provedor de dados: 70
Autores: Konrad,Odorico; Bezama,Alberto B.; Prade,Thomas; Backes,Gladis M.; Oechsner,Hans.
ABSTRACT This study presents a comparison of two systems for measuring low-flow biogas production rates. Grass silage was used as substrate in the experiment. Measurements were made by using (a) manual readings and (b) an automated system. The automated system proved to be efficient as it allowed readings of the biogas flow rates in real time. Results were stored in a computerized system with a safe access interface to download the recorded data at any desired moment. Furthermore, the systems also minimized the error rate in comparison to the manual method.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Automation; Biogas; Biogas meter; Biogas volume.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000500792

Chironomus gr. decorus (Diptera: Chironomidae) e outros insetos aquáticos de um açude temporário do semi-árido paraibano, Brasil
Provedor de dados: 71
Autores: Abílio,Francisco José Pegado; Fonseca-Gessner,Alaíde A.; Watanabe,Takako; Leite,Romualdo Lunguinho.
Com o objetivo de estudar a composição da fauna de Chironomidae e de outros insetos aquáticos do açude temporário Soledade, Soledade-PB (07º 02' S e 36º 22' W), coletas qualitativas foram realizadas em dois períodos: agosto de 1995, período em que o açude tinha um bom volume d'água e em março de 1999, após o completo dessecamento do açude por um período de 3 anos. Utilizou-se para isso um pegador manual com malha de 0,50 mm. As amostras coletadas foram fixadas em formol a 10%, a triagem através de bandejas iluminadas e a identificação através de estereomicroscópio. Apenas uma espécie de Chironomidae foi registrada, Chironomus gr. decorus, a qual contribuiu com 28,09% para o total da fauna de insetos aquáticos no mês de agosto/95 e foi a única espécie a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chironomidae; Chironomus gr. decorus; Semi-arido; Açude temporário.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200007

Ciclo biológico de Rhodnius robustus Larrousse, 1927 alimentado con sangre humana en condiciones de laboratorio
Provedor de dados: 71
Autores: Aldana,Elis; Zamora,Ezequiel; Lizano,Eliécer.
El propósito del presente trabajo es el estudio del ciclo biológico de R. robustus alimentado con sangre humana. Los triatominos procedían de una colonia fundada con ejemplares capturados en Caño Tigre, estado Mérida, Venezuela. Los insectos fueron alimentados a través de membrana de látex en un alimentador artificial a 37ºC con sangre humana con citrato de sodio como anticoagulante. Se observó una fecundidad de 13,9 huevos/hembra/semana, fertilidad 78,32 %, el ciclo biológico desde huevo a adulto se completó en aproximadamente 70 días. Los resultados muestran que R. robustus es capaz de reproducirse exitosamente al ser alimentada con sangre humana, lo cual contribuye a su potencialidad como especie domiciliaria y transmisora de la Enfermedad de Chagas.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Triatominae; Eficacia biológica; Comportamento; Rhodnius robustus.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100004

Jocélia Grazia
Provedor de dados: 71
Autores: Jurberg,Claudia.
Tipo: Info:eu-repo/semantics/other
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100001

Ocorrência de Dentocarpus silvai silvai Dusbabek &amp;amp; Cruz, 1966 (Acari: Chirodiscidae) em duas espécies de molossídeos (Mammalia: Chiroptera) no estado do Rio de Janeiro, Brasil
Provedor de dados: 71
Autores: Fonseca,Marcelo A.; Valim,Michel P.; Botão-Miranda,Raphael A.; Gitti,Clayton B.; Amorim,Marinete; Serra-Freire,Nicolau M.
Occurence of Dentocarpus silvai silvai, Dusbabek &amp;amp; Cruz, 1966 (Acari: Chirodiscidae) on two molossids (Mammalia: Chiroptera) species in Rio de Janeiro state, Brazil - In 2001 mites from three bats were collected, Molossus ater at Silva Jardim municipality and from Molossus molossus at Rio de Janeiro municipality, both in the Rio de Janeiro state. The mites where identified as Dentocarpus silvai silvai (Acari: Chirodiscidae), this being the first report of this mite species in Brazil.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Molossidae; Molossus ater; Chirodiscidae; Dentocarpus silvai silvai.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100010

Fauna de Chironomidae e outros insetos aquáticos de açudes do semi-árido paraibano, Brasil
Provedor de dados: 71
Autores: Abílio,Francisco José Pegado; Fonseca-Gessner,Alaíde A.; Watanabe,Takako; Leite,Romualdo Lunguinho.
Com o objetivo de estudar a fauna de Chironomidae e outros insetos aquáticos dos açudes São Mamede - SM (06º 55' S e 37º 06' W) e São Gonçalo - SG (06º 50' S e 38º 19' W), do semi-árido paraibano, coletas qualitativas foram realizadas em agosto e dezembro/95 (período seco) e julho/96 (após o pico máximo de chuvas da região). Foram feitos arrastos junto a vegetação da margem, utilizou-se para isso um pegador manual com 0,50 mm de abertura de malha. Registrou-se a participação de 15 taxa, dos quais Chironomus gr. decorus foi à espécie de Chironomidae dominante e freqüente nos dois açudes, contribuindo com uma abundância máxima de 81,82% em SG (dezembro/1995). Já no mês de julho/1996, constatou-se também a ocorrência de Goeldichironomus gr. pictus (1,45% em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Insetos aquáticos; Chironomidae; Chironomus gr. decorus; Semi-arido.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200009

Aspectos exocoriales de huevos de Triatoma patagonica Del Ponte, 1929 por microscopía electrónica de barrido
Provedor de dados: 71
Autores: Visciarelli,Elena; Ferrero,Adriana; Costamagna,Sixto Raúl.
Se estudiaron por microscopía electrónica de barrido (SEM) los patrones geométricos de las células de huevos de Triatoma patagonica Del Ponte, 1929, especie considerada vector activo de la enfermedad de Chagas. Se seleccionaron huevos de edad conocida: 5 días, 14 días y eclosionados, según sus características morfológicas y se registraron imágenes del exocorion en las zonas cefálica (opérculo), caudal y media. Los resultados obtenidos mostraron que los huevos de T. patagonica presentan en sus zonas cefálica y caudal, células con forma de hexágonos, pentágonos y cuadriláteros y en la media principalmente hexágonos. Se observó que los patrones geométricos de las distintas partes del huevo no cambian durante el desarrollo embrionario.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Triatoma patagonica; Ultraestructura; Enfermedad de Chagas; Triatominae; Huevos.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400007

Chironomidae (Diptera) em substratos artificiais num pequeno reservatório: Represa do Monjolinho, São Carlos, São Paulo, Brasil
Provedor de dados: 71
Autores: Correia,Leny Célia da Silva; Trivinho-Strixino,Susana.
O presente estudo teve como objetivo verificar possíveis diferenças taxonômicas e funcionais entre as assembléias de Chironomidae que colonizam substratos orgânicos e inorgânicos estruturalmente distintos. Substratos poliméricos (isopor e tela de náilon), minerais (pedra de argila expandida e areia grossa) e orgânicos vegetais (detritos de Scirpus cubensis e Cabomba piauhyensis; detritos de madeira), contidos em sacos de náilon, foram submersos na Represa do Monjolinho. Estes, após 30 dias, foram retirados, lavados em peneira de malha de 0,21 mm e os organismos retidos identificados sob microscópios estereoscópicos e/ou óptico. A análise de 3432 larvas indicou a presença de 17 unidades taxonômicas das quais Goeldichironomus neopictus foi predominante, com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chironomidae; Substratos artificiais; Goeldichironomus neopictus; Estrutura taxonomica; Guildas de alimentação.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200010

Sobre a ocorrência de Philornis angustifrons e P. deceptiva (Diptera, Muscidae) em ninhos de Suiriri affinis e S. islerorum (aves, tyrannidae), no cerrado do Distrito Federal, Brasil
Provedor de dados: 71
Autores: Higgins,Barbara Fernandes; Lopes,Leonardo Esteves; Santana,Fernando Henrique de Assis; Couri,Márcia Souto; Pujol-Luz,José Roberto.
The first report of Philornis angustifrons and P. deceptiva infesting nests of Suiriri affinis and S. islerorum in area of Distrito Federal's savanna is presented. It is known that larvae of these species have a strict relationship of parasitism with birds. The pupae were collected after the abandonment of the nests and the flies emerged in a period of about 13 days.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Parasitism; Savanna; First record.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100012

Ocorrência de Oryzaephilus surinamensis Linnaeus, 1758 (Coleoptera:Ccujidae) e Necrobia rufipes De Geer, 1775 (Coleoptera:Cleridae) infestando rações de animais domésticos
Provedor de dados: 71
Autores: Gredilha,Rodrigo; Saavedra,Priscilla Ribeiro; Guerim,Luciana; Lima,Aurino Florêncio de; Serra-Freire,Nicolau Maués.
Verificou-se a ocorrência de insetos associados a rações industriais para cães e gatos. Coletas simultâneas de péletes foram realizadas após a abertura dos sacos embalados na indústria e distribuídos para comercialização, no período de maio à novembro de 2003. Foram selecionadas para análise, seis diferentes tipos do total das marcas disponíveis para a venda no comércio da cidade do Rio de Janeiro. Registrou-se a incidência dos besouros Necrobia rufipes e Oryzaephilus surinamensis.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coleoptera; Necrobia rufipes; Oryzaephilus surinamensis; Ração animal.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100007

A associação de Philopota sp. Wiedemann (Diptera, Acroceridae) com flores do Gervão-Azul, Stachytarphetta cayenensis (Verbenaceae) na Ilha da Marambaia, Rio de Janeiro, Brasil
Provedor de dados: 71
Autores: Luz,José Roberto Pujol.
The acrocerids (small headed-flies) form a small group of flies, which are difficult to find and observe. They are rare in collections. Their larvae are heteromorphic parasitoids of many families of spiders and their imagoes show a great deal of morphological variation. Little is known about the biology and systematics of this group in the Neotropical region, especially the Philopotinae. Most studies are based on species from Europe and North America. The Philopotinae occurs througout the world, and are characterized by the strongly developed postpronota, which form a shield dorsally in front of the scutum. Fifty specimens of Philopota sp. were collected from branches of Stachytarphetta cayenensis (Verbenaceae) in the Ilha da Marambaia (23º 04' S - 43º 53'...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Philopotinae; Verbenaceae; Atlantic Rain Forest; Hill-topping; Brazil.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400010

Tres citas nuevas del género Ischnoptera Burmeister, 1838 (Blattellinae, Blattellidae, Blattaria) para Uruguay
Provedor de dados: 71
Autores: del C. Valverde,Alejandra; Crespo,Francisco A.
The number of species of the genus Ischnoptera reported from Uruguay is doubled, increasing its number to 6. Ischnoptera argentina Hebard, 1921; I. bilunata Saussure, 1869; and I. litostylata Hebard, 1921 are reported for the first time. The available information on the species distribution is mapped.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Blattaria; Ischnoptera; Cockroaches; Distribution.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100014

Aspectos atuais da distribuição geográfica de Anopheles (Kerteszia) cruzii Dyar &amp;amp; Knab, 1908 no estado do Espírito Santo, Brasil
Provedor de dados: 71
Autores: Rezende,Helder Ricas; Cerutti Junior,Crispim; Santos,Claudiney Biral dos.
Anopheles cruzii was registered in Espírito Santo state both in 1957 and 1968. Our study provides additional evidence of its presence, including municipalities that were non mentioned before. Anopheles captures undertaken between 1998 and 2003 pointed out a distribution restricted to the forested outskirts of the mountains in the highland area of the state. Its epidemiological role is suggested by the simultaneous presence of malaria cases in the same municipalities.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Anopheles cruzii; Malaria; Geographical distribution; Espírito Santo; Brazil.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100011

Insetos aquáticos do açude São José dos Cordeiros (semi-árido paraibano) com ênfase em Chironomidae
Provedor de dados: 71
Autores: Brito-Junior,Luciano de; Abílio,Francisco José Pegado; Watanabe,Takako.
Com o objetivo de estudar a composição da fauna de Chironomidae e outros insetos aquáticos do açude São José dos Cordeiros (07º 23'S e 36º 49'W), semi-árido paraibano, coletas qualitativas bimestrais foram realizadas durante o período de julho/1998 a julho/1999. Utilizou-se para isso um pegador manual com 0,50 mm de abertura de malha. Os arrastos foram feitos junto a vegetação da margem e as amostras fixadas em formol a 10 %. Para a triagem do material utilizou-se bandejas iluminadas e a identificação dos organismos foi feita através de estereomicroscópio. Foram determinadas algumas variáveis físicas e químicas da água para correlacionar com os dados biológicos. Aedokritus foi o gênero de Chironomidae dominante e freqüente no sedimento do açude,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chironomidae; Aedokritus sp; Insetos aquáticos; Semi-arido.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200002

Descrição de Brontostoma doughertyae sp. nov. e estudo morfológico comparativo com B. rubrum (Amyot &amp;amp; Serville, 1843) (Hemiptera: Heteroptera: Reduviidae: Ectrichodiinae)
Provedor de dados: 71
Autores: Gil-Santana,Hélcio R.; Lopes,Catarina M.; Marques,Oton Meira; Jurberg,José.
Brontostoma doughertyae sp. nov. (Hemiptera-Heteroptera: Reduviidae: Ectrichodiinae), proveniente dos Estados do Espírito Santo e Bahia, Brasil, é descrita com base em exemplares machos. Apresenta-se uma análise comparativa entre as estruturas fálicas de Brontostoma rubrum (Amyot &amp;amp; Serville, 1843) e B. doughertyae sp. nov.. Observou-se que três estruturas se destacam como diagnósticos: o processo do gonoporo (PrG); o suporte do falosoma (SPh) e o falosoma (Ph). Uma chave para as espécies brasileiras de Brontostoma é apresentada.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Morfologia comparada; Estruturas fálicas; Lista das espécies; Sinonímia; Brontostoma.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100006

First record of Aedes aegypti (L.) (Diptera: Culicidae) infected by the parasite Ascogregarina culicis (Ross) (Apicomplexa: Lecudinidae) in Argentina
Provedor de dados: 71
Autores: Dellapé,Mariana E.; Marti,Gerardo A.; Tranchida,María C.; García,Juan J.
In a survey for parasites and pathogens of Aedes aegypti conducted in La Plata, Argentina, an aseptate gregarine was found parasitizing larvae, pupae and adults of this mosquito species. This gregarine species was identified as Ascogregarina culicis based on the morphology and size of gamonts, gametocysts and oocysts. It is the first record of gregarine infections in culicids from Argentina.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Gregarine; Ascogregarina culicis; Aedes aegypti.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100009

Atração de mosquitos (Diptera: Culicidae) por lâmpadas incandescentes e fluorescentes
Provedor de dados: 71
Autores: Barghini,Alessandro; Urbinatti,Paulo Roberto; Natal,Delsio.
Programas de eletrificação rural em áreas isoladas, implantados com base em instalações fotovoltaicas e tradicionais, introduziriam um novo fator antrópico, que levantam suspeitas de associação à transmissão de doenças por culicídeos. Para testar atratividade de mosquitos por diferentes tipos de lâmpadas, foram utilizadas duas armadilhas tipo New Jersey, uma com lâmpada incandescente de 40 watts, e a outra, provida de bulbo fluorescente, compacta e com reator eletrônico de cor de igual intensidade luminosa, de 9 watts, com luz de temperatura de 6.200 K. Essas armadilhas operaram em duas áreas, em tempo e locais padronizados, totalizando 11 coletas, no período de janeiro a abril de 2002. Os resultados mostram que a lâmpada fluorescente atraiu 1,3 vezes mais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Culicidae; Impactos; Eletrificação rural.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400005

Colonização do "litter" de Eleocharis sellowiana kunth. (Cyperaceae) por larvas de Chironomidae (Diptera) em um brejo no litoral do Estado do Rio de Janeiro
Provedor de dados: 71
Autores: Nessimian,Jorge Luiz; Henriques-de-Oliveira,Ana Lucia.
Foram observados os processos de colonização do "litter" de Eleocharis sellowiana (Cyperaceae), macrófita dominante no Brejo-canal de Itaipuaçú, Maricá, RJ, pela fauna de macroinvertebrados aquáticos. Realizou-se um experimento no período de abril a junho de 1996, depositando-se no corpo d'água, 25 amostras de mesmo peso (50 g de peso úmido) de folhas. Foram realizadas 5 retiradas de 5 amostras em um período de 70 dias. Insetos representaram 51% do total de macroinvertebrados colonizadores sendo Chironomidae (Diptera) o principal táxon com 58%, totalizando 2347 indivíduos. Dentre os Chironomidae, Chironomini (Chironominae) constituiu o grupo mais abundante com 63,1%, seguido de Tanypodinae com 34,3%. Tanytarsini (Chironominae) apresentou participação...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Chironomidae; Larvas; Colonização; Macrófitas; Brejos.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200003

Rodolfo Ubaldo Carcavallo (« 1931 † 2004)
Provedor de dados: 71
Autores: Jurberg,José.
Tipo: Info:eu-repo/semantics/article
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400001

Composição e distribuição dos macroinvertebrados em diferentes substratos de fundo de um riacho no Município de Itatinga, São Paulo, Brasil
Provedor de dados: 71
Autores: Kikuchi,Regina Mayumi; Uieda,Virgínia Sanches.
O padrão de distribuição de organismos aquáticos é resultado da interação entre o hábito, as condições físicas, que compreendem o hábitat (substrato, fluxo, turbulência) e a disponibilidade alimentar. O presente trabalho teve como objetivo conhecer a composição e compreender o padrão de distribuição das comunidades animais de um riacho tropical. As coletas foram realizadas em um afluente da Bacia do Paranapanema, localizado no município de Itatinga, São Paulo. Quando analisada a ocorrência em diferentes tipos de substrato de fundo - vegetal, rochoso e arenoso - encontramos uma maior densidade no substrato rochoso e maior riqueza no substrato vegetal. Nos três substratos, os invertebrados da classe Insecta, e principalmente a ordem Diptera, predominaram em...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Macroinvertebrados; Ambiente lótico; Distribuição; Substrato; Ordenação.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200006

A peridomestic population of the tsetse fly Glossina palpalis palpalis Robineau-Desvoidy, 1830 (Diptera: Glossinidae) at Kontagora town, Niger state, Nigeria
Provedor de dados: 71
Autores: Ahmed,A. B.
The present article considers some aspects of a peridomestic population of the tsetse fly Glossina palpalis palpalis Robineau-Desvoidy, 1830 in Kontagora, Nigeria. This situation characterizes an abnormal behaviour of the vector, and it is of significant epidemiological importance. Data on the ecology of this species were collected in 1995 and 1999. The results indicated that the species exists during both dry and wet seasons; approximately 30.0% of the catches were gorged with blood giving a MHS of 2.4, indicating a well-nourished population. Dissection of inseminated pars indicated pregnancy rates of approximately 30.0% and 70.0% in the dry and wet seasons and the presence of all 4 stages of pregnancy, suggesting that breeding occurs at both seasons....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Glossina palpalis palpalis; Peridomestic behaviour; Trypanosoma brucei; Kontagora; Nigeria.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400004

Why are the subfamily relationships of Triatominae (Hemiptera: Reduviidae) important?
Provedor de dados: 71
Autores: Schaefer,Carl W.
Why are the subfamily relationships of Triatominae (Hemiptera: Reduviidae) important?-This question is really two: Is Triatominae a phylogenetically valid monophyletic subfamily; and, if it is, to what other reduviid subfamilies is it most closely related? If the answer to the first question is Yes, then what one knows about one member of Triatominae may be true for other members; if the answer is No, then no such prediction can be made. Because many members of Triatominae are of medical importance, such predictions are vitally (literally) important. For the same reason, knowledge of the subfamily relatives of medically important triatomines is important: For here too predictions about one related member can be based on knowledge of others. These points...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Harpactocorinae; Linshcosteus; Phylogeny; Peiratinae; Reduviinae.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100002

Níveis de enzootia por ectoparasitos em amostras de rolinha [Columbina talpacoti (Temminck, 1810)] no Rio de Janeiro, Brasil
Provedor de dados: 71
Autores: Valim,Michel P.; Serra-Freire,Roger T.; Fonseca,Marcelo A.; Serra-Freire,Nicolau M.
O primeiro inquérito sobre a fauna de ectoparasitos em rolinha (Columbina talpacoti) é feito no Brasil. As espécies de ectoparasitos encontrados foram: Microlynchia pussila (Speiser, 1902) (Diptera); Columbicola passerinae (Wilson, 1941) and Physconelloides eurysema (Carriker, 1903) (Phthiraptera: Ischnocera); Hohorstiella passerinae Hill &amp;amp; Tull, 1978 (Phthiraptera: Amblycera) and Byersalges talpacoti (Cerný, 1972), Diplaegidia columbigallinae (Cerný, 1972), Nanolichus sp. and Pterophagus lomatus Gaud &amp;amp; Barré, 1992 (Acari: Acaridida), sendo B. talpacoti a espécie de maior prevalência.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Columbina talpacoti; Ectoparasitos; Malófagos; Ácaros de pena; Rio de Janeiro.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400003

Descrição de genitálias de Neoblattella Shelford, 1911 com chave para identificação e considerações sobre o gênero (Blattaria, Blattellidae)
Provedor de dados: 71
Autores: Lopes,Sonia Maria; Oliveira,Edivar Heeren de.
Neste trabalho sete espécies de Neoblattella Shelford, 1911 são estudadas e descritas, pela primeira vez, as genitálias do macho e da fêmea. Com base nesse estudo são reunidas em quatro grupos, com a finalidade de estabelecer relação entre elas e elucidar problemas taxonômicos.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Neoblattella; Blattaria; Blattellidae; Genitália; Taxonomia.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400006

Flebotomíneos de municípios do norte do estado do Paraná, sul do Brasil
Provedor de dados: 71
Autores: Membrive,Norberto Assis; Rodrigues,Gesse; Membrive,Umberto; Monteiro,Wuelton Marcelo; Neitzke,Herintha Coeto; Lonardoni,Maria Valdrinez Campana; Silveira,Thaís Gomes Verzignassi; Teodoro,Ueslei.
This work reports the results of sandfly collections in several places, during 2001 and 2002, in Bom Sucesso, Jardim Alegre, Kaloré, Londrina and Sabáudia municipalities, North of the State. The sandflies catches were performed with Shannon and Falcão traps in domiciliary areas, domestic animal shelters, barns and in the forest. A total of 4,019 specimens of 8 species were captured. Nyssomyia whitmani predominates in all of the municipalities. The species Migonemyia migonei, Nyssomyia neivai and N. whitmani may be involved in the epidemiology of American Tegumentary Leishmaniasis in this state.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: American Tegumentary Leishmaniasis; Nyssomyia whitmani; Insect vectors; Sandflies.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400009

Occurrence of chironomid larvae living inside fallen-fruits in Atlantic Forest streams, Brasil
Provedor de dados: 71
Autores: Roque,Fabio de Oliveira; Siqueira,Tadeu; Trivinho-Strixino,Susana.
Occurrence of chironomid larvae living inside fallen-fruits in Atlantic Forest streams, Brazil - The Chironomidae larvae explore a wide variety of habitats and kinds of food. In this study we reported the use of fallen-fruits by chironomid larvae in low order streams in the Brazilian Atlantic Forest. We found chironomid larvae mining fruit tissue of 12 tree species. Seven morphospecies of Endotribelos were identified, including the species E. albatum and E. grodhaus found for the first time in Brazil. Our results suggest that larvae of Endotribelos are the commonest insect group living inside fallen-fruits in streams.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Feeding behavior; Endotribelos; Diptera; Neotropical region.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200011

Maruins (Ceratopogonidae: Diptera) do estuário do Rio Pará e do litoral do Estado do Pará, Brasil
Provedor de dados: 71
Autores: Trindade,Rosimeire Lopes da; Gorayeb,Inocêncio de Sousa.
O presente trabalho teve como objetivo fazer o levantamento das espécies de ceratopogonídeos hematófagos (maruins) em áreas costeiras do Estado do Pará. Foram amostrados dois pontos, um no litoral (Praia do Crispim/Marapanim) e outro no estuário do rio Pará (Outeiro/Belém). As coletas foram feitas mensalmente em 2003 de abril a outubro em Outeiro e nos meses de junho, julho, setembro e outubro em Marapanim. Foram utilizados os métodos de isca humana e armadilha tipo CDC. Foram coletados 4003 exemplares de maruins distribuídos em 18 espécies de Culicoides Latreille e uma de Leptoconops Skuse, sendo L. brasiliensis (Lutz) a única espécie comum aos dois pontos de coleta. As duas espécies mais abundantes coletadas em Outeiro foram C. batesi Wirth &amp;amp;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Insecta; Diptera; Ceratopogonidae; Amazônia; Zona costeira.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100005

Chironomidae (Diptera) do Rio Ribeira (divisa dos Estados de São Paulo e Paraná) numa avaliação ambiental faunística
Provedor de dados: 71
Autores: Trivinho-Strixino,Susana; Strixino,Giovanni.
Durante um programa de caracterização limnológica, foi avaliado um trecho do Rio Ribeira, contido na área de influência do futuro reservatório da UHE Tijuco Alto, através da comunidade macrobentônica. Em 4 campanhas de coleta, no período de XII/95 a IX/96, foram colhidas amostras de sedimento em 5 pontos do rio compreendidos entre o Córrego das Criminosas e o município de Eldorado, ambos no estado de São Paulo. Os dados faunísticos analisados (composição taxonômica, participação relativa de cada táxon, índices comunitários e bióticos) permitiram estabelecer a seguinte avaliação preliminar: 1- Das 15 famílias de macroinvertebrados assinaladas, Chironomidae (Diptera) e Elmidae (Coleoptera) foram as mais representativas, contribuindo, respectivamente, com...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Diptera; Chironomidae; River macroinvertebrates; Faunist river evaluation; Biotic index.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200008

Malófagos (Heptapsogastridae) de Tinamiformes (aves) encontrados em um novo hospedeiro [Crypturellus obsoletus (Temminck, 1815)] em Petrópolis, Rio de Janeiro, Brasil
Provedor de dados: 71
Autores: Valim,Michel P.; Becker,Cristiane Maciel; Serra-Freire,Nicolau M.
This paper reports the encounter of five lice species on a specimen of tinamou in Petrópolis city, Rio de Janeiro state. These only two of them, Strongylocotes complantus and Kelloggia ribeiroi, had been previously told in this host species. The others species (Megapeostus petersi; Heptapsogaster mandibularis; Discocorpus microgenitalis) were reported at first time on this bird species.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Tinamous lice; Crytpurellus obsoletus; Phthiraptera; Heptapsogastridae; Brazil.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100013

Elio Corseuil
Provedor de dados: 71
Autores: Jurberg,Claudia.
Tipo: Info:eu-repo/semantics/article
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400002

Sebastião José de Oliveira (*1918 †2005)
Provedor de dados: 71
Autores: Messias,Maria Conceição.
Tipo: Info:eu-repo/semantics/report
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200001

Registro de Gracilinanus agilis (Marsupialia, Didelphidae) parasitado por Metacuterebra apicalis (Diptera, Cuterebridae) no cerrado de Brasília, Distrito Federal, Brasil
Provedor de dados: 71
Autores: Pujol-Luz,José Roberto; Mendonça,André Faria; Henriques,Raimundo.
The first report of infection caused by maggots of the botfly Metacuterebra apicalis (Guérin-Méneville) on miceopossums Gracilinanus agilis (Burmeister) is presented. The examined individuals collected in the cerrado vegetation in Brasilia, DF, Brazil, showed infections in ventral area of the body, around genital organs. Two botflies (male and female) emerged in a period of 29 to 31 days.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Parasitism; Myiasis; Cuterebridae; Marsupialia; Cerrado.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812004000400008

Espécie nova de Aglaopteryx Hebard, 1917 (Blattellidae, Pseudophyllodromiinae) coletada em ninhos de vespas (Hymenoptera, Sphecidae) no estado do Amazonas, Brasil
Provedor de dados: 71
Autores: Lopes,Sonia Maria; Oliveira,Edivar Heeren de.
Aglaopteryx sacrificata sp. nov. é descrita com base em caracteres morfológicos da genitália do macho. A espécie foi coletada em ninhos de vespas solitárias da família Sphecidae, no estado do Amazonas, Brasil.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aglaopteryx sp. nov.; Blattaria; Amazonas; Taxonomia.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100008

A new species of Oukuriella Epler, 1986 (Insecta, Diptera, Chironomidae, Chironominae) from São Paulo State , Brazil
Provedor de dados: 71
Autores: Trivinho-Strixino,Susana; Messias,Maria Conceição.
The immature and adult stages of a new species of the genus Oukuriella Epler, 1986 from the Southeast of Brazil are described. The larvae, reared in laboratory to obtain adults, were obtained from submerged wood collected in a reservoir situated in the Jataí Ecological Station (Luiz Antônio, SP). According to Messias et al. (2000) the genus is composed of three species group. The adults of this new species congregate morphological characteristics of the Oukuriella - second group, which is characterised by wings without markings, abdominal tergites with setal tufts and gonostylus broad, 1,5x longer than gonocoxite, but is distinguished by different thoracic and abdominal pigmentation. This is the first description of female for the Oukuriella second group....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Região neotropical; Brazil; Chironomidae; Chironomini; Oukuriella.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200012

Dinâmica da emergência de Parachironomus supparilis Edwards, 1931 (Diptera, Chironomidae) da fitofauna de Cabomba piauhyensis Gardney, 1844
Provedor de dados: 71
Autores: Sonoda,Kathia C.; Trivinho-Strixino,Susana; Strixino,Giovanni.
Parachironomus supparilis é uma espécie neotropical de larga ocorrência em toda a América do Sul. Embora o gênero tenha recebido detalhada revisão taxonômica, escassos têm sido os trabalhos de cunho ecológico, principalmente aqueles referentes à dinâmica numérica e aos padrões de emergência. Com o objetivo de analisar a dinâmica fenológica dessa espécie, característica da fauna fitófila de diferentes macrófitas aquáticas de ambientes lênticos, foi estabelecido um programa mensal de coletas de Cabomba piauhyensis (Sonoda, 1999) (Nymphaeaceae) em uma lagoa marginal (Lagoa do Infernão) do Rio Mogi-Guaçu, localizada na Estação Ecológica de Jataí (Luiz Antônio, SP). Volumes pré-fixados da macrófita foram coletados mensalmente e mantidos em laboratório, onde...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Dinâmica fenológica; Nymphaeaceae; Parachironomus; Lagoa do Infernão.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200004

Observações preliminares sobre a atratividade por diferentes cores em Calliphoridae (Diptera), Niterói, RJ, Brasil
Provedor de dados: 71
Autores: Fraga,Mariana Borges; d'Almeida,José Mario.
This research aimed to evaluate the influence of colours on the collecting of Calliphoridae flies. The methodology was based on colour traps (green, black, yellow, red, blue and white), baited with fish rotten (sardine). Green, black and red colours were the most attractive to the blowflies. It were collected 3549 flies, belonging to nine species. The most frequent were Chrysomya megacephala (Fabricius, 1794) (74,86%) and Lucilia eximia (Wiedemann, 1819) (14,06%).
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Blowflies; Calliphoridae; Colour traps.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100015

Sobre uma nova espécie neotrópica do gênero Larsia Fittkau, 1962 (Diptera: Chironomidae: Tanypodinae)
Provedor de dados: 71
Autores: Serpa-Filho,Arlindo.
Este trabalho apresenta a descrição de uma nova do gênero Larsia Fittkau, 1962 (Diptera: Chironomidae: Tanypodinae). O gênero até o momento está representado por 23 espécies no mundo. Na região Neotrópica, segundo Spies &amp;amp; Reiss (1996) já foram assinaladas quatro espécies, sendo três na Guatemala, L. fittkaui Sublette &amp;amp; Sasa, 1994, L. planensis Johannsen, 1946, L. reissi Sublette &amp;amp; Sasa, 1994 e uma na Argentina, L. pallescens Edwards, 1931. A espécie nova foi coletada no Estado do Rio de Janeiro, procedente de Araras, município Petrópolis, RJ, sendo o primeiro registro do gênero no Brasil. Os exemplares testemunhos estão depositados na Coleção Entomológica do Instituto Oswaldo Cruz.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Tanypodinae; Larsia; Espécie nova; Rio de Janeiro; Brasil.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200013

Miíases humanas por Cochliomyia Hominivorax (Coquerel, 1858) (Diptera, Calliphoridae) em hospitais públicos na cidade do Recife, Pernambuco, Brasil
Provedor de dados: 71
Autores: Nascimento,Edleuza Maria Ferreira do; Oliveira,Jaqueline Bianque de; Paes,Maria José; Lobo,Andrea de Paula; Silva,Ana Lúcia Andrade da; Santos Júnior,Edivaldo Rosas dos; Leal,Jefferson Luis Figueiredo; Moya-Borja,Gonzalo Efraim.
A ocorrência de miíases humanas causadas pelas larvas de Cochliomyia hominivorax foi registrada pela primeira vez em Recife, Estado de Pernambuco, Brasil. No período de novembro de 1999 a outubro de 2002 foram registrados, em três hospitais da rede pública, 24 casos de miíases em pacientes de ambos os sexos, com idade variando de 08 a 93 anos. As miíases diagnosticadas foram classificadas em cutâneas, orais, anais, auriculares e oculares, sendo os membros inferiores acometidos com maior freqüência (10/24) (41,7%). Em todos os casos, as miíases se desenvolveram em lesões pré-existentes, resultantes de: escoriações de natureza variada (10/24) (41,7%); lesões de origem não identificada (05/24) (20,8%); doenças do sistema circulatório (03/24) (12,5%);...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Miíase humana; Cochliomyia hominivorax; Calliphoridae; Pernambuco.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000100003

Fauna de Chironomidae (Diptera) associada à Salvinia sp. e Myriophyllum sp. num reservatório do córrego do espraiado, São Carlos, São Paulo, Brasil
Provedor de dados: 71
Autores: Dornfeld,Carolina Buso; Fonseca-Gessner,Alaide A.
A presença de vegetação num ecossistema aquático é mais uma aréa disponível para a colonização. Vários estudos têm demonstrado uma relação positiva entre a presença de macrófitas e a abundância e a diversidade de Chironomidae. As variáveis ambientais e as larvas de Chironomidae associadas com as macrófitas Salvinia sp. e Myriophyllum sp. foram estudadas num reservatório com pequenas dimensões no estado de São Paulo, Brasil. Em Salvinia os grupos predominantes foram Tanytarsus, Monopelopia e Labrundinia, entretanto Cricotopus e Tanytarsus alternaram a dominância em Myriophyllum. Alem disso, discutiu-se a estrutura dos grupos funcionais de alimentação associados a essas macrófitas.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Macrofitas; Diversidade; Abundância.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0328-03812005000200005

Número Completo jul./set. 2019.‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬ (PDF com Capa e Artigos)
Provedor de dados: 194
Autores: Rural, Extensão.
Número Completo jul./set. 2019.‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬‬ (PDF com Capa e Artigos)
Tipo: Info:eu-repo/semantics/article
Ano: 2020
URL: http://periodicos.ufsm.br/extensaorural/article/view/42352

Controle de custos na produção do gado de corte: um estudo de caso em uma propriedade rural de Santa Catarina
Provedor de dados: 194
Autores: Domenico, Daniela Di; Magro, Cristian Bau Dal; Zanin, Antonio; Martini, Raphael.
O estudo teve como objetivo relacionar e analisar os custos na atividade da pecuária de corte em uma propriedade rural do Oeste Catarinense. A pesquisa se classifica quanto aos objetivos como exploratória, quanto aos procedimentos como documental, e quanto a abordagem do problema de caráter quantitativo. Os controles da contabilidade rural e da contabilidade de custos, quando implantados têm como meta auxiliar o empresário rural na tomada de decisão, obtendo um real controle de suas entradas, gastos e custos, envolvidos na atividade da pecuária, tendo, assim, maior controle e gestão da atividade. Os resultados apontaram que com o uso dos controles fornecidos pela contabilidade rural e contabilidade de custos, é possível que o proprietário rural obtenha a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Contabilidade Rural; Atividade Pecuária; Controle de custos.
Ano: 2015
URL: http://periodicos.ufsm.br/extensaorural/article/view/11326

CONFORMAÇÕES REGIONAIS DO DESENVOLVIMENTO RURAL E DA AGRICULTURA FAMILIAR: desigualdade e diversidade da geografia econômica do Rio Grande do Sul
Provedor de dados: 194
Autores: Conterato, Marcelo Antonio; Schneider, Sergio.
O objetivo deste trabalho é, a partir da construção de um Índice deDesenvolvimento Rural (IDR) e de uma tipologia da agricultura familiar,analisar a relação existente entre a dimensão espacial do desenvolvimentoe a intensidade e o formato da diversidade da agricultura familiar em trêsregiões gaúchas. Desenvolvido a partir de dados secundários dasmicrorregiões de Caxias do Sul, Missões e Frederico Westphalen, o IDRpermitiu estabelecer um olhar multidisciplinar sobre o desenvolvimento ruraldas respectivas regiões. Por sua vez, a partir de municípios representativosdestas microrregiões (Veranópolis, Salvador das Missões e Três Palmeiras,respectivamente) foi possível descortinar e diversidade da agriculturafamiliar. Somente a partir disso constatou-se a...
Tipo: Info:eu-repo/semantics/article
Ano: 2010
URL: http://periodicos.ufsm.br/extensaorural/article/view/5509

A percepção de compradores sobre a qualidade da carne suína in natura no mercado varejista de Campo Grande (MS)
Provedor de dados: 194
Autores: Souza, Celso Correia de; Gabriel, Rafael; Reis Neto, José Fransisco dos; Frainer, Daniel Massen.
Este estudo teve como objetivo avaliar a percepção de compradores sobre a qualidade da carne suína in natura no mercado varejista de Campo Grande (MS). Uma amostra aleatória de 400 indivíduos da cidade foi investigada, em lugares perto de pontos de venda de carne suína fresca. Foram realizadas estatísticas univariadas, bivariadas e multivariadas concluindo que 76,75% da população consumiam carne suína fresca. Destes, 49% consumiram pelo menos uma vez por semana. O preço não influenciava a frequência de consumo de carne suína, mas a facilidade de preparação, principalmente, em relação às mulheres que têm pouco tempo para fazer as refeições em casa. Além disso, oferecendo uma maior variedade de cortes poderia trazer um aumento na frequência de consumo desta...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Carne gorda; Comportamento do consumidor; Risco à saúde; Saúde animal.
Ano: 2016
URL: http://periodicos.ufsm.br/extensaorural/article/view/21488

Agricultura familiar e a permanência no campo: a experiência de um projeto realizado e a percepção dos jovens sobre o município de Santa Terezinha (Santa Catarina)
Provedor de dados: 194
Autores: Staloch, Rubens; Rocha, Isa de Oliveira.
A agricultura familiar, no contexto brasileiro, começa a ser discutida a partir da década de 1990. Nas três últimas décadas deixou de ser percebida como sinônimo de atraso e decadência para ser compreendida como fator chave para o desenvolvimento regional e ao alcance dos Objetivos do Desenvolvimento Sustentável da Organização das Nações Unidas. O presente trabalho surge com o objetivo de estruturar uma relação entre desenvolvimento sustentável, agricultura familiar e a percepção de jovens que vivem nas áreas rurais do município de Santa Terezinha, localizado na região do Alto Vale do Itajaí (Santa Catarina), considerando o cenário constituído de não permanência no campo. A metodologia para a elaboração deste texto tomou por base a pesquisa exploratória,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura familiar; Desenvolvimento sustentável; Jovem no campo; Santa Terezinha (SC).
Ano: 2019
URL: http://periodicos.ufsm.br/extensaorural/article/view/36130

AVALIAÇÃO ECONÔMICA DO CONTROLE PREVENTIVO DAS PRAGAS INICIAIS DO FUMO
Provedor de dados: 194
Autores: Link, Dionisio; Leal, Rodolpho Saenger.
A avaliação econômica do controle preventivo das pragas iniciais da culturado fumo foi realizada com a instalação de cinco ensaios, na região fumageira, na safra 2000/01. As doses registradas dos inseticidas testados, Imidacloprido +Ciflutrina, Imidacloprido e Tiametoxam resultaram em maior retorno econômico. As subdoses testadas apresentaram valores reduzidos de retorno econômico. Independente da forma de aplicação, as doses registradas garantem melhor controle e maiores rendimentos.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Controle químico; Nicotinóides; Forma de aplicação; Rendimento.
Ano: 2003
URL: http://periodicos.ufsm.br/extensaorural/article/view/5547

Dinâmica demográfica da população rural: um estudo de caso na microrregião e município de Frederico Westphalen/RS
Provedor de dados: 194
Autores: Boscardin, Mariele; Spanevello, Rosani Marisa.
O presente estudo tem como objetivo traçar um panorama das principais características sociodemográﬁcas da população rural da microrregião e especialmente do município de Frederico Westphalen, norte do estado do Rio Grande do Sul, bem como discutir as implicações destas características para o meio rural local, com base nos dados do IBGE. De modo geral, a análise aponta que a região não foge ao padrão nacional e estadual no que tange às mudanças demográficas, caracterizada especialmente pela redução da população jovem e acréscimo na população idosa. Estas características não apenas confirmam mudanças na estrutura etária populacional, mas também revelam a emergência de “novas dinâmicas” do meio rural, demonstrando que muitos agricultores podem estar exercendo...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Envelhecimento; Estrutura etária; Migração.
Ano: 2019
URL: http://periodicos.ufsm.br/extensaorural/article/view/34946

MOVIMENTOS CAMPONESES E QUESTÕES AMBIENTAIS: POSITIVAÇÃO DA AGRICULTURA CAMPONESA?
Provedor de dados: 194
Autores: Picolotto, Everton Lazzaretti; Piccin, Marcos Botton.
Os movimentos camponeses estão passando por mudanças em seu repertório de pautas e em seu formato de organização. Com a entrada de pautas ambientais no repertório de lutas (preservação ambiental, defesa da biodiversidade, do conhecimento tradicional e das culturas locais) e atransnacionalização da organização camponesa através da constituição da Via Campesina, os movimentos camponeses estão se tornado agentes centrais da contemporaneidade. O objetivo deste artigo é analisar como as questões ambientais têm reconfigurado o repertório de pautas dos movimentos camponeses. Para atingir esse objetivo, parte-se de um referencial teórico da sociologia ambiental; analisa-se como as questões ambientais estão sendo assimiladas pelos movimentos camponeses; ecomo estas...
Tipo: Info:eu-repo/semantics/article
Ano: 2008
URL: http://periodicos.ufsm.br/extensaorural/article/view/5500

O projeto profissional do jovem no contexto da Escola Família Agrícola de Santa Cruz do Sul
Provedor de dados: 194
Autores: Pozzebon, Adair; Charão-Marques, Flávia.
Este artigo descreve e analisa o processo de elaboração e desenvolvimento do Projeto Profissional do Jovem – PPJ na Escola Família Agrícola de Santa Cruz do Sul - EFASC no âmbito de um processo formativo baseado na pedagogia da alternância. Os argumentos desenvolvidos têm por base pesquisa quanti-qualitativa realizada junto a estudantes e educadores entre 2014 e 2015. Os resultados indicam que o PPJ é o principal meio para discutir, refletir e organizar possibilidades concretas de inserção sócio-profissional dos estudantes, contribuindo significativamente para fortalecer o vínculo identitario do jovem com o meio onde vive e ampliando a percepção das oportunidades de diversificação e geração de renda. No entanto, identifica-se a necessidade de fortalecer...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura familiar; Educação do campo; Juventude rural; Pedagogia da alternância.
Ano: 2016
URL: http://periodicos.ufsm.br/extensaorural/article/view/20335

Viabilidade econômica da suinocultura no sistema wean to finish em São José do Rio Pardo - SP
Provedor de dados: 194
Autores: Evangelista, Mariane Zabotto; Pereira, Rafaela.
Este trabalho analisou a viabilidade econômica da produção Wean to Finish de suínos em São José do Rio Pardo nas produções independente e integrada. Foram levantados os custos fixos e variáveis anuais de manejo e manutenção de instalações, despesas administrativas e fiscais e custos da construção hipotética de uma instalação de 1.000 m2 em uma propriedade com granjas já em funcionamento. O plantel projetado foi de 1.000 animais por lote, sendo produzidos dois lotes anuais. Foram construídos dois fluxos de caixa, um para produção independente e outro para produção integrada, ambos para o período de 21 anos. O valor presente líquido (VPL) apresentou viabilidade apenas para a produção integrada, com R$ 634.055,44 de lucro. A taxa interna de retorno (TIR) para...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Custos de produção; Produção integrada; Suínos.
Ano: 2020
URL: http://periodicos.ufsm.br/extensaorural/article/view/35482

Saber tradicional etnobotânico na comunidade Quilombola do Cedro no Sudoeste de Goiás
Provedor de dados: 194
Autores: Silva, Jesiel Souza.
Os quilombos são os maiores símbolos de resistência frente ao sistema escravocrata que perdurou no território brasileiro por muitos anos. Espalhadas por todo o território brasileiro, essas comunidades criaram estratégicas de sobrevivência frente ao modelo fundiário concentrador e conservador. Nesse contexto, a comunidade do Cedro, no sudoeste de Goiás, é uma comunidade constituída de descendentes de escravos e que se reconhecem como portadores de uma identidade baseada na mesma origem e em uma cultura comum distinta dos demais grupos circunvizinhos. Este artigo é fruto de uma pesquisa empírica e tem como objetivo analisar a importância do conhecimento tradicional na sustentabilidade da comunidade como fator de fortalecimento no processo produtivo,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Quilombolas; Etnobotânica; Resistência; Conhecimento tradicional.
Ano: 2019
URL: http://periodicos.ufsm.br/extensaorural/article/view/34928

Indicadores da modernização agrícola do Estado de Mato Grosso
Provedor de dados: 194
Autores: Beckmann, Elizangela; Santana, Antônio Cordeiro de.
A modernização da produção agrícola de Mato Grosso resultou das combinações entre insumos químicos, máquinas e equipamentos mecânicos e biotecnologia com as variáveis relacionadas à educação, assistência técnica, inovações na organização e gestão da atividade. Assim, para destacar o estado na produção agrícola foram identificados e analisados os fatores que determinam a modernização da agricultura e apresentada sua configuração nos municípios por meio de um Índice de Modernização Agrícola Municipal. Para tanto, utilizou-se a Análise Fatorial para extrair os fatores e hierarquizar os municípios de acordo com o nível de modernização. Foram identificados cinco fatores responsáveis pela modernização agrícola de Mato Grosso e, dentre estes, a agricultura de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura; Análise fatorial; Índice de modernização.
Ano: 2017
URL: http://periodicos.ufsm.br/extensaorural/article/view/22992

PERDA DE RENDA EM COMUNIDADES PESQUEIRAS NA REGIÃO CARBONÍFERA DO RIO GRANDE DO SUL: COMO A ECONOMIA DOS RECURSOS NATURAIS A EXPLICA
Provedor de dados: 194
Autores: Denardin, Valdir Frigo; Mattuela, Juvir Luiz.
Disponivel em anexo.
Tipo: Info:eu-repo/semantics/article
Ano: 1998
URL: http://periodicos.ufsm.br/extensaorural/article/view/6139

AVICULTURA DE CORTE NO RIO GRANDE DO SUL: um olhar da nova economia institucional sobre a produção da Agrosul Agroavícola – São Sebastião do Caí/RS - POULTRY IN RIO GRANDE DO SUL: a look at the new institutional economics on production of Agrosul Agroavíc
Provedor de dados: 194
Autores: Sopeña, Mauro Barcellos; Ramos, Fernando de Souza.
O presente artigo está baseado em pesquisa de estágio profissional realizada em 2011, na Agrosul Agroavícola Industrial, empresa situada no município de São Sebastião do Caí, Rio Grande do Sul. O estudo foi desenvolvido em diferentes setores produtivos da avicultura de corte e pôde verificar in loco aspectos da estrutura produtiva do setor. A observação direta dos processos e das transações da empresa permitiu que, a partir de uma abordagem institucional, se determinasse com mais clareza que arranjos produtivos são criados naquele setor. Em sentido amplo, a agroavícola opera em meio a uma cadeia produtiva importante, com baixos custos de transação. A verticalização está fortemente presente em muitas operações da firma e não se verifica comportamento...
Tipo: Info:eu-repo/semantics/article
Ano: 2011
URL: http://periodicos.ufsm.br/extensaorural/article/view/5573

Os estudos de extensão pesqueira nos Programas de Pós-Graduação em Extensão Rural
Provedor de dados: 194
Autores: Sousa, Diego Neves de.
http://dx.doi.org/10.5902/231817969092A trajetória histórica da extensão pesqueira foi semelhante a da extensão rural ocorrida no país, sendo conduzida ao mesmo tratamento de intervenção metodológica, bem como pautada por políticas públicas descontínuas. O objetivo deste artigo é mapear os estudos de extensão pesqueira encontrados nos Programas de Pós-graduação em Extensão Rural. Para isso, foram pesquisadas as dissertações defendidas no período de 1986 a 2014 nos três mestrados em Extensão Rural existentes no país. Entre os resultados, considerou-se que os estudos voltados às questões da extensão pesqueira são escassos e pouco explorados pela academia e instituições de pesquisa e extensão. A carência de dados técnicos, econômicos, sociais e ambientais...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Extensão pesqueira; Extensão rural; ATEPA.
Ano: 2014
URL: http://periodicos.ufsm.br/extensaorural/article/view/9092

O PROCESSO DE COLONIZAÇÃO DA TERRA E DO CONHECIMENTO NA AMAZÔNIA
Provedor de dados: 194
Autores: Scalabrin, Rosemeri; Aragão, Ana Lucia Assunção.
Este artigo discute o modelo de desenvolvimento implementado na Amazônia brasileira e o que ele causou no meio rural paraense, buscando identificar a presença da visão ocidental inculcada no processo de colonização da terra e do conhecimento na região mesorregião Sudeste do Pará/Amazônia, bem como, compreender o papel de iniciativas contra-hegemônicas construídas pelos movimentos sociais do campo e pela Universidade como resultado de um processo dialógico. A pesquisa demonstrou que se faz fundamental o acesso, pelas populações do campo, às políticas públicas, em especial a educacional em que se possibilite a inter-relação de conhecimentos com vistas a construção de solução dos complexos problemas do campo.
Tipo: Info:eu-repo/semantics/article
Ano: 2013
URL: http://periodicos.ufsm.br/extensaorural/article/view/8569

AS REPRESENTAÇÕES DO TRABALHO NO TURISMO RURAL PARA AS MULHERES DA REGIÃO DOS CAMPOS DE CIMA DA SERRA -RS
Provedor de dados: 194
Autores: Lunardi, Raquel; Almeida, Joaquim Anécio de Jesus.
As mudanças ocorridas no meio rural brasileiro, a partir da década de setenta, proporcionaram o desenvolvimento de atividades não-agrícolas nas propriedades e, conseqüentemente, o aumento da participação da mulher nessa nova realidade. Uma das principais atividades que surgiram no espaço rural foi o turismo. Este trabalho tem como  objetivo estudar o papel da mulher no desenvolvimento da atividade turísticano meio rural. Para isso, foram observadas mulheres empreendedoras em oito pousadas-fazenda no meio rural na região dos Campos de Cima  da Serra, estado do Rio Grande do Sul. Os municípios estudados foram: Bom Jesus, Cambará do Sul e São José dos Ausentes. Para analisar com maior precisão o trabalho dessas mulheres foram realizadas entrevistas norteadas...
Tipo: Info:eu-repo/semantics/article
Ano: 2008
URL: http://periodicos.ufsm.br/extensaorural/article/view/5498

Diagnosis of extractivism, processing and marketing of products from butia plantations in Rio Grande do Sul (Brazil)
Provedor de dados: 194
Autores: Ambrosini, Larissa Bueno; Roldan, Bruna Bresolin; Bremm, Carolina; Kroeff, Denise Reif.
Brazil is home to 37 genera of palm trees that participate in the ecologicalbalance of different biomes. In the southern region there is a genus of palm tree, Butia spp., which has eight species, and is threatened with extinction. Butiá extractivism, through management that allows its rational exploration, can be an alternative to encourage its preservation. The aim of this article is to present a diagnosis of the extraction of butia plant in the state of Rio Grande do Sul, providing systematized data about this reality. The first stage of the research consisted of a survey on thenumber of properties that have areas of butia groves throughout the state, through Emater-RS. Based on these data, it was possible to define a statistically representative sample,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Butia spp; Frutas nativas; Sustentabilidade ambiental; Butia spp; Environmental conservation; Environmental sustainability; Native fruits.
Ano: 2022
URL: http://periodicos.ufsm.br/extensaorural/article/view/68706