Data/hora: 21/05/2024 02:11:04

Provedor de dados: 	5	
País: 	France	
Título: 	Modelling mud transport in a macrotidal estuary	
Autores: 	Le Hir, Pierre; Bassoullet, Philippe; L'Yavanc, Jacky.	
Data: 	1988	
Ano: 	1988	
Palavras-chave: 	Dynamique des sédiments cohésifs; Estuaire Morlaix; Tassement des vases; Modèle mathématique; Érosion; Dépôt; Cohesive sediment dynamics; Estuary; Erosion; Deposition; SoiT consolidation; Mathematical modelling.	
Resumo: 	In order to determine the fate of the fine particles and adsorbed contaminants in·a short macrotidal èstuary, a mathematical modelling system for cohesive suspended mater transport and bottom evolution, including a new consolidation algorithm, is developed. An analysis of successive erosion, transport and deposi~ion processes due to tidal forcing is given and comparisons with field data are provided. A description of mean-term bottom variations has been attempted and is partially validated by differential soundings.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	https://archimer.ifremer.fr/doc/00682/79379/81909.pdf

https://archimer.ifremer.fr/doc/00682/79379/	
Formato: 	application/pdf	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use