Data/hora: 19/05/2024 11:25:25

Provedor de dados: | 58
País: | Brazil
Título: | Continuous ethanol production using immobilized yeast cells entrapped in loofa-reinforced alginate carriers
Autores: | Bangrak,Phoowit; Limtong,Savitree; Phisalaphong,Muenduen.
Data: | 2011-06-01
Ano: | 2011
Palavras-chave: | Ethanol; Loofa; Alginate; Immobilization; Continuous.
Resumo: | A culture of Saccharomyces cerevisiae M30 entrapped in loofa-reinforced alginate was used for continuous ethanol fermentation in a packed-bed reactor with initial sugar concentrations of 200-248 g/L. Maximum ethanol productivity of 11.5 g/(L·h) was obtained at an ethanol concentration of 57.4 g/L, an initial sugar concentration of 220 g/L and a dilution rate (D) of 0.2 h-1. However, a maximum ethanol concentration of 82.1 g/L (productivity of 9.0 g/(L·h)) was obtained at a D of 0.11 h-1. Ethanol productivity in the continuous culture was 6-8-fold higher than that in the batch culture. Due to the developed carrier's high biocompatibility, high porosity, and good mechanical strength, advantages such as cell regeneration, reusability, altered mechanical strength, and high capacity to trap active cells in the reactor were achieved in this study. The immobilized cell reactor was successfully operated for 30 days without any loss in ethanol productivity. The average conversion yield was 0.43-0.45 throughout the entire operation, with an immobilization yield of 47.5%. The final total cell concentration in the reactor was 37.3 g/L (17.7 g/L immobilized cells and 19.6 g/L suspended cells). The concentration of suspended cells in the effluent was 0.8 g/L.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1517-83822011000200032
Editor: | Sociedade Brasileira de Microbiologia
Relação: | 10.1590/S1517-83822011000200032
Formato: | text/html
Fonte: | Brazilian Journal of Microbiology  v.42 n.2 2011
Fonte: | info:eu-repo/semantics/openAccess