Data/hora: 03/06/2024 03:39:10

Provedor de dados: 	5	
País: 	France	
Título: 	Structure and properties of fibres from sea-grass (Zostera marina)	
Autores: 	Davies, Peter; Morvan, C; Sire, O; Baley, C.	
Data: 	2007-07	
Ano: 	2007	
Palavras-chave: 	Xylan; Tension; Mechanical behaviour; IR spectroscopy; Sea grass; Fibre.	
Resumo: 	This paper presents results from a study of fibres extracted from Zostera marina eel-grass collected from the Baltic coast. This species of sea-grass is shown to contain small diameter (around 5 mu m) fibres composed of similar to 57% cellulose, similar to 38% of non-cellulosic polysaccharides (mainly xylan) and similar to 5% of residual matter so-called Klason lignin. This composition is quite different to that of commonly used terrestrial fibres. Single fibre stiffness values up to 28 GPa were measured. This stiffness combined with a low density could provide an attractive reinforcement for composite materials, and may be particularly suitable for use in bio-degradable structures.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/2007/publication-2607.pdf

DOI:10.1007/s10853-006-0546-1	
Editor: 	Springer	
Relação: 	http://archimer.ifremer.fr/doc/00000/2607/	
Formato: 	application/pdf	
Fonte: 	Journal of Materials Science (0022-2461) (Springer), 2007-07 , Vol. 42 , N. 13 , P. 4850-4857	
Fonte: 	2007 Springer