Data/hora: 12/06/2024 13:55:00

Provedor de dados: 	5	
País: 	France	
Título: 	Ocean doppler anomaly and ocean surface current from Sentinel 1 tops mode	
Autores: 	Johnsen, Harald; Nilsen, Vegard; Engen, Geir; Mouche, Alexis; Collard, Fabrice.	
Data: 	2016	
Ano: 	2016	
Palavras-chave: 	Doppler effect; Sea surface; Sea measurements; Ocean temperature; Surface treatment; Antennas.	
Resumo: 	Processing and analysis of Doppler information from Sentinel 1A Interferometric Wide (IW) and Extra Wide (EW) modes are performed for assessing the capabilities of mapping ocean surface current field. Data from Agulhas (South-Africa) and Norwegian Coast are used in combination with numerical models, higher-order satellite products, and Lagrangian drifters. Results show strong Doppler signal and dynamics from coastal areas caused by a mixture of surface current and wind/wave induced drifts at a spatial resolution of around 2 km2 in IW mode and 4km2 in EW mode. Doppler values of up to 70 Hz are observed, corresponding to a surface drift velocity of 3.5 m/s. The Sentinel 1 retrieved surface current component is in reasonable agreement with the circulation models and drifter measurements. Surface current values up to 1.5 m/s are observed in the central Agulhas current, with a standard deviation of around 0.39 m/s with respect to Lagrangian drifters.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00356/46713/46589.pdf

http://archimer.ifremer.fr/doc/00356/46713/	
Editor: 	Geoscience and Remote Sensing Symposium (IGARSS), 2016 IEEE International. 10-15 July 2016.pp. 3993 - 3996	
Formato: 	application/pdf	
Fonte: 	2016 IEEE

info:eu-repo/semantics/openAccess

restricted use