Data/hora: 07/06/2024 08:15:59

Provedor de dados: | 52
País: | Brazil
Título: | A Mathematical Model for the Removal of Organic Mater in Stabilization Ponds
Autores: | Medri,Waldir; Medri,Vandir.
Data: | 2002-03-01
Ano: | 2002
Palavras-chave: | Stabilization ponds; Mathematical model; Optimization.
Resumo: | This work presents an application to systemize the construction of ponds systems for treatment of domestic sewage. It consisted of two anaerobic ponds operated in parallel during May/97 to April/99. These were connected in series with a chicaned facultative pond. The treatment system was controlled with samples collected from the crude sewage (compound sample), in the affluents and effluents of the ponds and along the flux of the anaerobic and facultative ponds. The following parameters were analyzed: pH, Biochemical Oxygen Demand, Chemical Oxygen Demand, Total Solids, Sedimentable Solids, Total Coliforms, Oxygen Consumed in Acid Medium (OCAM) and temperature.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-89132002000100014
Editor: | Instituto de Tecnologia do Paraná - Tecpar
Relação: | 10.1590/S1516-89132002000100014
Formato: | text/html
Fonte: | Brazilian Archives of Biology and Technology  v.45 n.1 2002
Fonte: | info:eu-repo/semantics/openAccess