Data/hora: 02/06/2024 07:28:32

Provedor de dados: 	63	
País: 	Brazil	
Título: 	A rapid method for measuring soil water content in the field with a areometer	
Autores: 	Calbo,Adonai Gimenez.	
Data: 	2002-12-01	
Ano: 	2002	
Palavras-chave: 	Hydrostatic balance; Irrigation moment; Pycnometer; Soil humidity.	
Resumo: 	The availability of a rapid method to evaluate the soil water content (U) can be an important tool to determine the moment to irrigate. The soil areometer consists of an elongated hydrostatic balance with a weighing pan, a graduated neck, a float and a pynometric flask. In this work an areometer was adapted to rapidly measure soil water content without the need of drying the soil. The expression U = (M A - M AD)/(M M -M A) was used to calculate the soil water content. In this equation M M is the mass to level the areometer with the pycnometric flask filled with water, M A the mass to level the areometer with a mass M M of soil in the pycnometer, the volume being completed with water, and similarly M AD the mass added to the pan to level the areometer with a mass M M of dried soil in the pycnometric flask. The convenience of this method is that the values M M and M AD are known. Consequently, the decision on irrigation can be made after a measurement that takes, about, ten minutes. The procedure involves only stirring the soil with water for at least 2 minutes to remove the adhered air. The soil water content data obtained with the areometric method were similar to those obtained weighing the soil before and after drying to constant weight, in an oven at 105º C.	
Tipo: 	Info:eu-repo/semantics/report	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162002000400029	
Editor: 	São Paulo - Escola Superior de Agricultura "Luiz de Queiroz"	
Relação: 	10.1590/S0103-90162002000400029	
Formato: 	text/html	
Fonte: 	Scientia Agricola  v.59 n.4 2002	
Fonte: 	info:eu-repo/semantics/openAccess