Data/hora: 10/06/2024 15:09:06

Provedor de dados: | 70
País: | Brazil
Título: | SUGARCANE BASE CUTTING QUALITY USING RECTANGULAR AND CIRCULAR BLADES
Autores: | Paixão,Carla S. S.; Voltarelli,Murilo A.; Santos,Adão F. dos; Silva,Rouverson P. da.
Data: | 2021-02-01
Ano: | 2021
Palavras-chave: | Cutting height; Control charts; Mechanized harvesting; Damages and disturbances; Saccharum spp.
Resumo: | ABSTRACT Sugarcane mechanized harvesting can lead to serious risks to the longevity of plantations when improperly operated, and may cause damages and disturbances in the remaining ratoons in the field. In this sense, this study aimed to evaluate the damage and disturbance to the sugarcane ratoons by the base cutting quality of two-blade models through statistical process control. The experiment was carried out during the 2015/16 growing season in an agricultural area of the Moreno Mill, located in Cravinhos, São Paulo, Brazil. The sugarcane harvester models A8800 (Machine 1) and BE1035 (Machine 2). The sugarcane variety cultivated in both treatments was SP80-1816. Thirty points were sampled per harvester, with 10-minute intervals between them. Equations were used to calculate the indices, which were then evaluated through descriptive analysis and statistical process control. Machine 2 presented process instability for the index of damages, with lower data variability. On the other hand, Machine 1 presented instability during the process due to the quality indicator and index of disturbance, but with a lower operation variability.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162021000100056
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/1809-4430-eng.agric.v41n1p56-61/2021
Formato: | text/html
Fonte: | Engenharia Agrícola  v.41 n.1 2021
Fonte: | info:eu-repo/semantics/openAccess