Data/hora: 03/06/2024 11:21:27

Provedor de dados: 	91	
País: 	Brazil	
Título: 	A CFD approach to assess the effects of different opening combinations in poultry houses	
Autores: 	Saraz,Jairo A. O.; Rocha,Keller S. O.; Damasceno,Flavio A.; Tinoco,Ilda F. F.; Osorio,Robinson; Tobón,Julio C. A.	
Data: 	2017-12-01	
Ano: 	2017	
Palavras-chave: 	Natural ventilation; Ammonia concentration; Computational simulation.	
Resumo: 	ABSTRACT The aim of this study was to use computational fluids dynamics (CFD) to evaluate hygiene and comfort conditions in function of temperature level and ammonia (NH3) concentration during the night in commercial poultry houses used in Brazil and countries with tropical and subtropical climates. Four models with different curtain heights and different air inlet and outlet positions were used, adopting the open building typology without thermal insulation. The validated CFD model did not present statistical differences from the experimental data, making it possible to use this model to predict the behavior in the four proposed cases. This model can be used to improve the internal conditions of the poultry facilities during the night and could be an important tool to reduce energy consumption and generate better conditions for animal production of chicks over 21 days old.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017001200852	
Editor: 	Departamento de Engenharia Agrícola  - UFCG	
Relação: 	10.1590/1807-1929/agriambi.v21n12p852-857	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Engenharia Agrícola e Ambiental  v.21 n.12 2017	
Fonte: 	info:eu-repo/semantics/openAccess