Consulta: creatorFacets:"Leymarie, Edouard"
Registros recuperados: 17
Data/hora: 03/06/2024 04:27:46

WP2 : Développer la nouvelle génération des flotteurs Argo
Provedor de dados: 5
Autores: Le Reste, Serge; Andre, Xavier; Dutreuil, Vincent; Leymarie, Edouard.
Tipo: Text
Ano: 2016
URL: http://archimer.ifremer.fr/doc/00317/42856/42271.pdf

Arctic mid-winter phytoplankton growth revealed by autonomous profilers
Provedor de dados: 5
Autores: Randelhoff, Achim; Lacour, Léo; Marec, Claudie; Leymarie, Edouard; Lagunas, José; Xing, Xiaogang; Darnis, Gérald; Penkerc’h, Christophe; Sampei, Makoto; Fortier, Louis; D’ortenzio, Fabrizio; Claustre, Hervé; Babin, Marcel.
It is widely believed that during winter and spring, Arctic marine phytoplankton cannot grow until sea ice and snow cover start melting and transmit sufficient irradiance, but there is little observational evidence for that paradigm. To explore the life of phytoplankton during and after the polar night, we used robotic ice-avoiding profiling floats to measure ocean optics and phytoplankton characteristics continuously through two annual cycles in Baffin Bay, an Arctic sea that is covered by ice for 7 months a year. We demonstrate that net phytoplankton growth occurred even under 100% ice cover as early as February and that it resulted at least partly from photosynthesis. This highlights the adaptation of Arctic phytoplankton to extreme low-light...
Tipo: Text
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00652/76416/77468.pdf

Assessing the Variability in the Relationship Between the Particulate Backscattering Coefficient and the Chlorophyll a Concentration From a Global Biogeochemical-Argo Database
Provedor de dados: 5
Autores: Barbieux, Marie; Uitz, Julia; Bricaud, Annick; Organelli, Emanuele; Poteau, Antoine; Schmechtig, Catherine; Gentili, Bernard; Obolensky, Grigor; Leymarie, Edouard; Penkerc'H, Christophe; D'Ortenzio, Fabrizio; Claustre, Herve.
Characterizing phytoplankton distribution and dynamics in the world's open oceans requires in situ observations over a broad range of space and time scales. In addition to temperature/salinity measurements, Biogeochemical-Argo (BGC-Argo) profiling floats are capable of autonomously observing at high-frequency bio-optical properties such as the chlorophyll fluorescence, a proxy of the chlorophyll a concentration (Chla), the particulate backscattering coefficient (b(bp)), a proxy of the stock of particulate organic carbon, and the light available for photosynthesis. We analyzed an unprecedented BGC-Argo database of more than 8,500 multivariable profiles collected in various oceanic conditions, from subpolar waters to subtropical gyres. Our objective is to...
Tipo: Text
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00673/78495/80780.pdf

Underwater Radiance Distributions Measured with Miniaturized Multispectral Radiance Cameras
Provedor de dados: 5
Autores: Antoine, David; Morel, Abdré; Leymarie, Edouard; Houyou, Amel; Gentili, Bernard; Victori, Stephane; Buis, Jean-pierre; Buis, Nicolas; Meunier, Sylvain; Canini, Marius; Crozel, Didier; Fougnie, Bertrand; Henry, Patrice.
Miniaturized radiance cameras measuring underwater multispectral radiances in all directions at high-radiometric accuracy (CE600) are presented. The camera design is described, as well as the main steps of its optical and radiometric characterization and calibration. The results show the excellent optical quality of the specifically designed fish-eye objective. They also show the low noise and excellent linearity of the complementary metal oxide semiconductor (CMOS) detector array that is used. Initial results obtained in various oceanic environments demonstrate the potential of this instrument to provide new measurements of the underwater radiance distribution from the sea surface to dimly lit layers at depth. Excellent agreement is obtained between nadir...
Tipo: Text
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00185/29659/28027.pdf

Hydrography and biogeochemistry dedicated to the Mediterranean BGC-Argo network during a cruise with RV Tethys 2 in May 2015
Provedor de dados: 5
Autores: Taillandier, Vincent; Wagener, Thibaut; D'Ortenzio, Fabrizio; Mayot, Nicolas; Legoff, Herve; Ras, Josephine; Coppola, Laurent; Pasqueron De Fommervault, Orens; Schmechtig, Catherine; Diamond, Emilie; Bittig, Henry; Lefevre, Dominique; Leymarie, Edouard; Poteau, Antoine; Prieur, Louis.
We report on data from an oceanographic cruise, covering western, central and eastern parts of the Mediterranean Sea, on the French research vessel Tethys 2 in May 2015. This cruise was fully dedicated to the maintenance and the metrological verification of a biogeochemical observing system based on a fleet of BGC-Argo floats. During the cruise, a comprehensive data set of parameters sensed by the autonomous network was collected. The measurements include ocean currents, seawater salinity and temperature, and concentrations of inorganic nutrients, dissolved oxygen and chlorophyll pigments. The analytical protocols and data processing methods are detailed, together with a first assessment of the calibration state for all the sensors deployed during the...
Tipo: Text
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00677/78943/81333.pdf

Two databases derived from BGC-Argo float measurements for marine biogeochemical and bio-optical applications
Provedor de dados: 5
Autores: Organelli, Emanuele; Barbieux, Marie; Claustre, Herve; Schmechtig, Catherine; Poteau, Antoine; Bricaud, Annick; Boss, Emmanuel; Briggs, Nathan; Dall'Olmo, Giorgio; D'Ortenzio, Fabrizio; Leymarie, Edouard; Mangin, Antoine; Obolensky, Grigor; Penkerc'H, Christophe; Prieur, Louis; Roesler, Collin; Serra, Romain; Uitz, Julia; Xing, Xiaogang.
Since 2012, an array of 105 Biogeochemical-Argo (BGC-Argo) floats has been deployed across the world's oceans to assist in filling observational gaps that are required for characterizing open-ocean environments. Profiles of biogeochemical (chlorophyll and dissolved organic matter) and optical (single-wavelength particulate optical backscattering, downward irradiance at three wavelengths, and photosynthetically available radiation) variables are collected in the upper 1000 m every 1 to 10 days. The database of 9837 vertical profiles collected up to January 2016 is presented and its spatial and temporal coverage is discussed. Each variable is quality controlled with specifically developed procedures and its time series is quality-assessed to identify issues...
Tipo: Text
Ano: 2017
URL: https://archimer.ifremer.fr/doc/00662/77389/79010.pdf

Development and validation of the new ProvBioII float
Provedor de dados: 5
Autores: Leymarie, Edouard; Poteau, Antoine; Andre, Xavier; Besson, F; Brault, Patrice; Claustre, Herve; David, Arnaud; D'Ortenzio, Fabrizio; Dufour, A; Lavigne, Heloise; Le Reste, Serge; Le Traon, Pierre-yves; Migon, Christophe; Nogre, David; Obolensky, G; Penkerc'H, C; Sagot, Jerome; Schaeffer, Christophe; Schmechtig, C; Taillandier, V.
In the last ten years, a productive collaboration has grown between the Laboratoire d’Océanographie de Villefranche (LOV), NKE and IFREMER to implement biogeochemical sensors on profiling floats. A first project (2003) was dedicated to the design of the so-called ProvBio floats (models A and B) that consisted of a PROVOR-CTS3 float instrumented with three new optical sensors: a Wetlabs transmissometer (C-Rover), a 3-wavelength Satlantic radiometer (OCR-503) and an “ECO3” Wetlabs sensor, measuring chlorophyll-a fluorescence, colored dissolved organic matter and particle backscattering coefficients (see First Success of ProvBio floats, Coriolis Letter n°5). Then, the integration of biogeochemical sensors continued in the framework of ProNuts project (2009,...
Tipo: Text
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00219/32989/31438.pdf

WP2 : Développer la nouvelle génération des flotteurs Argo (2015)
Provedor de dados: 5
Autores: Le Reste, Serge; Andre, Xavier; Dutreuil, Vincent; Leymarie, Edouard.
Tipo: Text
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00280/39080/37644.pdf

Sea-ice detection for autonomous underwater vehicles and oceanographic lagrangian platforms by continuous-wave laser polarimetry
Provedor de dados: 5
Autores: Lagunas, Jose; Marec, Claudie; Leymarie, Edouard; Penkerc'H, Christophe; Rehm, Eric; Desaulniers, Pierre; Brousseau, Denis; Larochelle, Patrick; Roy, Gilles; Fournier, Georges; Thibault, Simon; Babin, Marcel.
The use of Lagrangian platforms and of Autonomous Underwater Vehicles (AUVs) in oceanography has increased rapidly over the last decade along with the development of improved biological and chemical sensors. These vehicles provide new spatial and temporal scales for observational studies of the ocean. They offer a broad range of deployment and recovery capabilities that reduce the need of large research vessels. This is especially true for ice-covered Arctic ocean where surface navigation is only possible during the summer period. Moreover, safe underwater navigation in icy waters requires the capability of detecting sea ice on the surface (ice sheets). AUVs navigating in such conditions risk collisions, RF communication shadowing, and being trapped by ice...
Tipo: Text
Palavras-chave: Lidar; Polarization; Sea-ice; AUV; Argo; Arctic; Amundsen; Marine robotics.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00475/58665/61166.pdf

Biogeochemical Argo: The Test Case of the NAOS Mediterranean Array
Provedor de dados: 5
Autores: D’ortenzio, Fabrizio; Taillandier, Vincent; Claustre, Hervé; Prieur, Louis Marie; Leymarie, Edouard; Mignot, Alexandre; Poteau, Antoine; Penkerc’h, Christophe; Schmechtig, Catherine Marie.
The necessity of wide, global-scale observing systems for marine biogeochemistry emerged dramatically in the last decade. A global network based on Biogeochemical (BGC) Argo floats is considered to be one of the most promising approaches for reaching this goal. As a first step, pilot studies were encouraged to test the feasibility of a global BGC-Argo array, to consolidate the methods and practices under development, and to set up the array’s characteristics. A pilot study in The Mediterranean Sea—deemed a suitable candidate for a test case because it combines a relatively large diversity of oceanic BGC conditions in a reduced open-ocean basin—was consequently approved as a part of the “Novel Argo ocean Observing System” (NAOS) project, a French national...
Tipo: Text
Palavras-chave: BGC-Argo floats; Mediterranean; Bioregions; Ocean color; Physical biological interactions.
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00618/73031/72145.pdf

Autonomously profiling the nitrate concentrations in the ocean : the Pronuts project
Provedor de dados: 5
Autores: D'Ortenzio, Fabrizio; Le Reste, Serge; Lavigne, Heloise; Besson, F.; Claustre, H.; Coppola, Laurent; Dufour, A.; Dutreuil, Vincent; Laes, Agathe; Leymarie, Edouard; Malarde, Damien; Mangin, A.; Migon, Christophe; Morin, P.; Poteau, A.; Prieur, L.; Raimbault, P.; Testor, Pierre.
Tipo: Text
Ano: 2012
URL: http://archimer.ifremer.fr/doc/00114/22555/20243.pdf

Green Edge ice camp campaigns: understanding the processes controlling the under-ice Arctic phytoplankton spring bloom
Provedor de dados: 5
Autores: Massicotte, Philippe; Amiraux, Rémi; Amyot, Marie-pier; Archambault, Philippe; Ardyna, Mathieu; Arnaud, Laurent; Artigue, Lise; Aubry, Cyril; Ayotte, Pierre; Bécu, Guislain; Bélanger, Simon; Benner, Ronald; Bittig, Henry C; Bricaud, Annick; Brossier, Eric; Bruyant, Flavienne; Chauvaud, Laurent; Christiansen-stowe, Debra; Claustre, Hervé; Cornet-barthaux, Véronique; Coupel, Pierre; Cox, Christine; Delaforge, Aurélie; Dezutter, Thibault; Dimier, Céline; Dominé, Florent; Dufour, Francis; Dufresne, Christiane; Dumont, Dany; Ehn, Jens; Else, Brent; Ferland, Joannie; Forget, Marie-hélène; Fortier, Louis; Gali, Marti; Galindo, Virginie; Gallinari, Morgane; Garcia, Nicole; Gerikas-ribeiro, Catherine; Gourdal, Margaux; Gourvil, Priscilla; Goyens, Clemence; Grondin, Pierre-luc; Guillot, Pascal; Guilmette, Caroline; Houssais, Marie-noëlle; Joux, Fabien; Lacour, Léo; Lacour, Thomas; Lafond, Augustin; Lagunas, José; Lalande, Catherine; Laliberté, Julien; Lambert-girard, Simon; Larivière, Jade; Lavaud, Johann; Lebaron, Anita; Leblanc, Karine; Le Gall, Florence; Legras, Justine; Lemire, Mélanie; Levasseur, Maurice; Leymarie, Edouard; Leynaert, Aude; Lopes Dos Santos, Adriana; Lourenço, Antonio; Mah, David; Marec, Claudie; Marie, Dominique; Martin, Nicolas; Marty, Constance; Marty, Sabine; Massé, Guillaume; Matsuoka, Atsushi; Matthes, Lisa; Moriceau, Brivaela; Muller, Pierre-emmanuel; Mundy, Christopher-john; Neukermans, Griet; Oziel, Laurent; Panagiotopoulos, Christos; Pangazi, Jean-jacques; Picard, Ghislain; Picheral, Marc; Pinczon Du Sel, France; Pogorzelec, Nicole; Probert, Ian; Queguiner, Bernard; Raimbault, Patrick; Ras, Joséphine; Rehm, Eric; Reimer, Erin; Rontani, Jean-françois; Rysgaard, Soren; Saint-béat, Blanche; Sampei, Makoto; Sansoulet, Julie; Schmidt, Sabine; Sempere, Richard; Sevigny, Caroline; Shen, Yuan; Tragin, Margot; Tremblay, Jean-eric; Vaulot, Daniel; Verin, Gauthier; Vivier, Frédéric; Vladoiu, Anda; Whitehead, Jeremy; Babin, Marcel.
The Green Edge initiative was developed to investigate the processes controlling the primary productivity and the fate of organic matter produced during the Arctic phytoplankton spring bloom (PSB) and to determine its role in the ecosystem. Two field campaigns were conducted in 2015 and 2016 at an ice camp located on landfast sea ice southeast of Qikiqtarjuaq Island in Baffin Bay (67.4797N, 63.7895W). During both expeditions, a large suite of physical, chemical and biological variables was measured beneath a consolidated sea ice cover from the surface to the bottom at 360 m depth to better understand the factors driving the PSB. Key variables such as temperature, salinity, radiance, irradiance, nutrient concentrations, chlorophyll-a concentration,...
Tipo: Text
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00598/71000/69266.pdf

Preparing the New Phase of Argo: Scientific Achievements of the NAOS Project
Provedor de dados: 5
Autores: Le Traon, Pierre-yves; D'Ortenzio, Fabrizio; Babin, Marcel; Leymarie, Edouard; Marec, Claudie; Pouliquen, Sylvie; Thierry, Virginie; Cabanes, Cecile; Claustre, Hervé; Desbruyeres, Damien; Lacour, Leo; Lagunas, Jose-luis; Maze, Guillaume; Mercier, Herle; Penkerc'H, Christophe; Poffa, Noe; Poteau, Antoine; Prieur, Louis; Racape, Virginie; Randelhoff, Achim; Rehm, Eric; Schmechtig, Catherine Marie; Taillandier, Vincent; Wagener, Thibaut; Xing, Xiaogang.
Argo, the international array of profiling floats, is a major component of the global ocean and climate observing system. In 2010, the NAOS (Novel Argo Observing System) project was selected as part of the French “Investissements d’Avenir” Equipex program. The objectives of NAOS were to consolidate the French contribution to Argo’s core mission (global temperature and salinity measurements down to 2000 m), and also to develop the future generation of French Argo profiling floats and prepare the next phase of the Argo program with an extension to the deep ocean (Deep Argo), biogeochemistry (BGC-Argo) and polar seas. This paper summarizes how NAOS has met its objectives. The project significantly boosted France’s contribution to Argo’s core mission by...
Tipo: Text
Palavras-chave: Profiling floats; Deep ocean; Biogeochemistry; Mediterranean Sea; Arctic; Atlantic; Argo.
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00654/76584/77729.pdf

A BGC-Argo Guide: Planning, Deployment, Data Handling and Usage
Provedor de dados: 5
Autores: Bittig, Henry C.; Maurer, Tanya L.; Plant, Joshua N.; Schmechtig, Catherine; Wong, Annie P. S.; Claustre, Hervé; Trull, Thomas W.; Udaya Bhaskar, T. V. S.; Boss, Emmanuel; Dall’olmo, Giorgio; Organelli, Emanuele; Poteau, Antoine; Johnson, Kenneth S.; Hanstein, Craig; Leymarie, Edouard; Le Reste, Serge; Riser, Stephen C.; Rupan, A. Rick; Taillandier, Vincent; Thierry, Virginie; Xing, Xiaogang.
The Biogeochemical-Argo program (BGC-Argo) is a new profiling-float-based, ocean wide, and distributed ocean monitoring program which is tightly linked to, and has benefited significantly from, the Argo program. The community has recommended for BGC-Argo to measure six additional properties in addition to pressure, temperature and salinity measured by Argo, to include oxygen, pH, nitrate, downwelling light, chlorophyll fluorescence and the optical backscattering coefficient. The purpose of this addition is to enable the monitoring of ocean biogeochemistry and health, and in particular, monitor major processes such as ocean deoxygenation, acidification and warming and their effect on phytoplankton, the main source of energy of marine ecosystems. Here we...
Tipo: Text
Palavras-chave: Ocean observation; Ocean biogeochemical cycles; Sensors; Carbon cycle; Ocean optics; Best practices; Argo.
Ano: 2019
URL: https://archimer.ifremer.fr/doc/00512/62344/66607.pdf

ROSACE: A Proposed European Design for the Copernicus Ocean Colour System Vicarious Calibration Infrastructure
Provedor de dados: 5
Autores: Antoine, David; Vellucci, Vincenzo; Banks, Andrew C.; Bardey, Philippe; Bretagnon, Marine; Bruniquel, Véronique; Deru, Alexis; Hembise Fanton D’andon, Odile; Lerebourg, Christophe; Mangin, Antoine; Crozel, Didier; Victori, Stéphane; Kalampokis, Alkiviadis; Karageorgis, Aristomenis P.; Petihakis, George; Psarra, Stella; Golbol, Melek; Leymarie, Edouard; Bialek, Agnieszka; Fox, Nigel; Hunt, Samuel; Kuusk, Joel; Laizans, Kaspars; Kanakidou, Maria.
The European Copernicus programme ensures long-term delivery of high-quality, global satellite ocean colour radiometry (OCR) observations from its Sentinel-3 (S3) satellite series carrying the ocean and land colour instrument (OLCI). In particular, the S3/OLCI provides marine water leaving reflectance and derived products to the Copernicus marine environment monitoring service, CMEMS, for which data quality is of paramount importance. This is why OCR system vicarious calibration (OC-SVC), which allows uncertainties of these products to stay within required specifications, is crucial. The European organisation for the exploitation of meteorological satellites (EUMETSAT) operates the S3/OLCI marine ground segment, and envisions having an SVC infrastructure...
Tipo: Text
Palavras-chave: Satellite ocean colour; System vicarious calibration; Fiducial reference measurements; Radiometry; SI-traceability; Uncertainty budget; Mediterranean Sea; BOUSSOLE; MSEA.
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00629/74136/73601.pdf

Preparing the New Phase of Argo: Technological Developments on Profiling Floats in the NAOS Project
Provedor de dados: 5
Autores: André, Xavier; Le Traon, Pierre-yves; Le Reste, Serge; Dutreuil, Vincent; Leymarie, Edouard; Malardé, Damien; Marec, Claudie; Sagot, Jérôme; Amice, Martin; Babin, Marcel; Claustre, Hervé; David, Arnaud; D’ortenzio, Fabrizio; Kolodziejczyk, Nicolas; Lagunas, José Luis; Le Menn, Marc; Moreau, Bertrand; Nogré, David; Penkerc’h, Christophe; Poteau, Antoine; Renaut, Corentin; Schaeffer, Christophe; Taillandier, Vincent; Thierry, Virginie.
The international array of profiling floats known as Argo is a major component of the global ocean- and climate-observing system. In 2010, the NAOS (Novel Argo Observing System) project was selected as part of France’s Equipex “Investissement d’Avenir” program. The objectives of NAOS were to consolidate the French contribution to the Argo core mission (global temperature and salinity measurements down to 2,000 m) as well as to develop the future generation of French Argo profiling floats and prepare the next phase of the Argo program with an extension to the deep ocean (Deep-Argo), biogeochemistry (BGC-Argo) and polar seas. This paper summarizes the main technological advances and at-sea validations carried out as part of NAOS: development of a deep (4,000...
Tipo: Text
Palavras-chave: Ocean; Argo; Global observing system; Profiling float; Deep; Biogeochemistry; Under-ice; Float technology.
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00658/77029/78314.pdf

ProVal: A New Autonomous Profiling Float for High Quality Radiometric Measurements
Provedor de dados: 5
Autores: Leymarie, Edouard; Penkerc'H, Christophe; Vellucci, Vincenzo; Lerebourg, Christophe; Antoine, David; Boss, Emmanuel; Lewis, Marion R.; D'Ortenzio, Fabrizio; Claustre, Herve.
An efficient system to produce in situ high quality radiometric measurements is compulsory to rigorously perform the vicarious calibration of satellite sensors dedicated to Ocean Color Radiometry (OCR) and to validate their derived products. This requirement is especially needed during the early stages of an OCR satellite activity or for remote areas poorly covered by oceanographic cruises with possible bio-optical anomalies. Taking advantage of Argo's profiling float technology, we present a new autonomous profiling float dedicated to in situ radiometric measurements. The float is based on the Provor CTS5 (manufacturer NKE) with an added novel two protruding arm design allowing for sensor redundancies, shading mitigation and near-surface data. Equipped...
Tipo: Text
Palavras-chave: Autonomous profiling floats; Remote sensing reflectance; Ocean color; Validation; System vicarious calibration; Austral ocean; Mediterranean Sea; Radiometric measurement.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00585/69694/67579.pdf