Data/hora: 09/06/2024 13:30:10

Provedor de dados: 	111	
País: 	China	
Título: 	Experimental modeling of orange settling depth in water	
Autores: 	kheiralipour, Kamran; Kakaee, Mehdi; Nouri, Behzad.	
Data: 	2015-06-23	
Ano: 	2015	
Palavras-chave: 	Orange; Experimental Modeling; Settling Depth; Sorting; Physical Characteristics.	
Resumo: 	Settling depth of orange fruits and vegetables with the density lower than the density of water is an important hydrodynamic property important in hydraulic sorting and transporting. In this research, settling depth of orange fruit with regular shapes was experimentally modeled. The considered parameters in multivariate modeling were fruit characteristics, density, mass and volume, and dropping height of the fruits. The characteristics were determined by standard methods. The settling depth was determined by a water column and a digital camera. The models were obtained in MATLAB software. The best model was based on the density, volume and dropping height with coefficient of determination (R2) and mean squire error (MSE) of 0.89 and 4.67×10-7, respectively.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.cigrjournal.org/index.php/Ejounral/article/view/3184	
Editor: 	International Commission of Agricultural and Biosystems Engineering	
Relação: 	http://www.cigrjournal.org/index.php/Ejounral/article/view/3184/2118	
Formato: 	application/pdf	
Fonte: 	Agricultural Engineering International: CIGR Journal; Vol 17, No 2 (2015): CIGR Journal

1682-1130