Data/hora: 16/06/2024 17:41:41

Provedor de dados: | Agricultural Engineering International : The CIGR e-journal
País: | China
Título: | Effect of Roofing Material Type on Microclimate in the Sheep Buildings
Autores: | hatem, mohamed hashem.
Data: | 2015-04-26
Ano: | 2015
Palavras-chave: | Sheep housing; Roofing material; Microclimate; Building in hot climate; Temperature – humidity index (THI).
Resumo: | A study  was conducted on description of  the  sheep houses ( materials, location, orientation ,……etc) and its  effect on  microenvironment in  two  housing ( concrete roofing material, Iron sheet  roofing  material ) in  Giza , Egypt. In order to select the appropriate type of housing that provides the best inside climate throughout making adjustment in housing. During the experimental period, maximum temperature was recorded under Iron sheet and lowest temperature as in Concrete. The maximum protection from high temperature was given in concrete than in Iron sheet. Adjustment of temperature and relative humidity through the day   was successful under concrete than Iron sheet.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/3169
Editor: | International Commission of Agricultural and Biosystems Engineering
Relação: | http://www.cigrjournal.org/index.php/Ejounral/article/view/3169/2047
Formato: | application/pdf

Fonte:

Agricultural Engineering International: CIGR Journal; 2015: Special Issue: 18th World Congress of CIGR

1682-1130