Data/hora: 03/06/2024 16:22:58

Provedor de dados: | 111
País: | China
Título: | Evaluation the mechanical harvesting efficiency of olive with the application of fruit loosening spray
Autores: | Khdair, Adnan I.; Abu-Rumman, Ghaida; Khdair, Sawsan.
Data: | 2019-01-25
Ano: | 2019
Palavras-chave: | Olive Mechanical Harvesting; Abscission; Harvest productivity; Removal efficiency; Fruit detachment force.
Resumo: | Abstract: Olive is harvested mainly by hand in the Mediterranean. This resulted in steady rising of harvesting cost due to shortage of skilled labors at harvesting time. Operation cost might be reduced and harvesting processes will be carried out on time if mechanical harvesters are used. In 2015 an experiment was performed to study the effects of mechanical harvester and use of loosening agent on harvesting productivity and efficiency. The experiment was conducted using randomized complete block with two regional olive varieties Nabali Rosie and Nabali. Harvesting productivity by hand (hand picking), pneumatic comb and branch shaker machines were evaluated. Ethrel abscission chemical was used two weeks before harvesting as an abscission and loosening agent at three concentration levels: 0, 1500 and 3000 ppm. The results showed that harvesting techniques and Ethrel amount had significant effects on yield productivity at α = 0.01. The harvesting productivity increased by two and four times compared to traditional method (hand harvesting) using pneumatic comb and branch shaker machines, respectively. The fruit detachment force (FDF) was also significantly affected by abscission dosage at α = 0.01. It was reduced from 9.35 N to 5.65 N for Nabali Rosie at ethrel level of 1500 ppm. This reduction in FDF as result of abscission application increased the removal percentage and harvesting production of olives. The percentages of injured fruits and detached leaves were acceptable with less than 10% and 12%, respectively.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/4743
Editor: | International Commission of Agricultural and Biosystems Engineering
Relação: | http://www.cigrjournal.org/index.php/Ejounral/article/view/4743/2882
Formato: | application/pdf

Fonte:

Agricultural Engineering International: CIGR Journal; Vol 20, No 4 (2018): CIGR Journal; 69-75

1682-1130

Fonte: | Copyright (c) 2019 Agricultural Engineering International: CIGR Journal