Data/hora: 16/06/2024 06:55:14

Provedor de dados: | 14
País: | Brazil
Título: | Malt bagasse: Alkaline pretreatment and enzymatic hydrolysis to release glucose from malt bagasse.
Autores: | RODRIGUES, D. de S.
Data: | 2021-07-23
Ano: | 2021
Palavras-chave: | Alkaline pretreatment; Lignocellulosic; Malt; Bagasse; Glucose; Hydrolysis; Biomass; Renewable resources.
Resumo: | Alkaline pretreatment process followed by enzymatic hydrolysis for release of glucose from malt bagasse. The alkaline pretreatment promotes biomass delignification, exposing the cellulose fibers, making them accessible to enzymatic action. A maximum conversion of cellulose into glucose (74%) was achieved when sodium hydroxide was used at a concentration of 4% (w/v).
Tipo: | Folders
Idioma: | Inglês

Identificador:

Brasília, DF: Embrapa Agroenergy, 2021.

http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/1133093

Relação: | (Embrapa Agroenergy. Technology Showcase. Chemistry of Renewables).

Formato:

PDF: il. color.

2 p.

Fonte: | openAccess