Data/hora: 09/06/2024 13:53:07

Provedor de dados: | Organic Eprints
País: | Germany
Título: | Demonstration of Plough Dethatchers
Autores: | Alföldi, Thomas.
Data: | 2014
Ano: | 2014
Palavras-chave: | Production systems; Buildings and machinery.
Resumo: | The crop to be incorporated was a frost susceptible green manure that spontaneously grassed and looked like an old ley. The ground was very dry.   The film shows the following plow dethatchers at work:    • Bugnot 52 Rapidlab  • Mini-8 OVLAC  • Escudero Adero  • Kverneland Ecomat  • Traditional Operating plow    Under wet conditions, the shallow tillage without soil-turning (= with crow's feet dethatchers for example) does not provide an absolutely clean soil. It’s the same with a superficial and complete reversal of a ley.   One strategy would be to till soil superficially (= 3 - 4 cm for example) with crow's feet or cultivator blades to dry vegetation, then moving a disc harrow plow, which, even without causing complete reversal would leave behind a "clean" field. But this strategy has yet to be tested and demonstrated.
Tipo: | Practice tool
Idioma: | Francês

Identificador:

http://orgprints.org/31169/1/video.php_y%3Dhttps_%252F%252Fwww.youtube.com%252Fwatch_list%3DUUCoC0X8wJIEkpNkxYPYHEAQ%26v%3DQzWHC9TfS1w

{Tool}   Demonstration of Plough Dethatchers.  [Démonstration de charrues déchaumeuses.]         Creator(s): Alföldi, Thomas.  Issuing Organisation(s): Research Institute of Organic Agriculture FiBL.  OK-Net Arable Tool Description. (2014)

Relação: | http://orgprints.org/31169/
Formato: | video/mpeg