Data/hora: 09/06/2024 14:43:50

Provedor de dados: | Organic Eprints
País: | Germany
Título: | Ley Destruction with Shallow Ploughing or Cultivators
Autores: | Alföldi, Thomas; Wüthrich, Bertrand.
Data: | 2016
Ano: | 2016
Palavras-chave: | Pasture and forage crops; Production systems; Soil tillage.
Resumo: | To plough a ley at a maximum depth of 10 cm is a major challenge.  The video shows how different machines succeed in handling the issue. The following machines are presented:  01:08 WecoDyn (Bärtschi Hüswil)  02:10 Kerner Komet (Alphatec)  3:23 Vario Digger (PL Agri - Service)  04:25 Treffler TG 300 (GVS agricultural)  05:22 Carré Penterra (Grunderco)  06:08 Einböck Taifun (Aebi Suisse)  06:52 Skim plough Ovlac (Aebi Suisse)  07:28 Standard Plough Kverneland (Agriott)  The choice of a machine for a specific farm is highly dependent on the prevailing soil conditions, the weed pressure and its crop rotation and should be carefully considered.    The Video is available in German https://www.youtube.com/watch?v=McZU2lTYfyI and in French https://www.youtube.com/watch?v=5nG_hB8F7j4
Tipo: | Practice tool
Idioma: | Alemão

Identificador:

http://orgprints.org/30994/1/video.php_y%3Dhttps_%252F%252Fwww.youtube.com%252Fwatch_v%3DMcZU2lTYfyI

http://orgprints.org/30994/2/video.php_y%3Dhttps_%252F%252Fwww.youtube.com%252Fwatch_v%3D5nG_hB8F7j4

http://orgprints.org/30994/3/video.php_y%3Dhttps_%252F%252Fwww.youtube.com%252Fwatch_v%3DMcZU2lTYfyI

{Tool}   Ley Destruction with Shallow Ploughing or Cultivators.  [Kunstwiesenumbruch bei reduzierter Bodenbearbeitung.]         Creator(s): Alföldi, Thomas and Wüthrich, Bertrand.  Issuing Organisation(s): Research Institute of Organic Agriculture FiBL.  OK-Net Arable video. (2016)

Relação: | http://orgprints.org/30994/

Formato:

video/mpeg

video/mpeg

video/mpeg