Data/hora: 03/06/2024 02:35:27

Provedor de dados: | 25
País: | Brazil
Título: | O emprego do Geoprocessamento na Análise Espacial da Bacia Hidrográfica do Córrego Guariroba, Campo Grande – MS
Autores: | Yamaciro, Raony Moreira Gomes.
Data: | 2007-10-25
Ano: | 2007
Palavras-chave: | Geoprocessing; Bacia Hidrográfica; Digital Terrain Model.
Resumo: | The present study aimed to use Geoprocessing techniques applied to basin management. The study area was the Guariroba microbasin in Campo Grande city - MS. Using the Digital Terrain Model, from EMBRAPA website, topographical data were extracted in Arcgis environment, a TIN grade was generated and from its, a hypsometric map and a three-dimensional declivity map. The land use/cover was also mapped, using a CBERS image and the MAXVER algorithm in ERDAS environment. The Guariroba basin presents low levels of declivity, with fragments of native vegetation and high degree of degradation, distributed in 24 % of the total of the area of the basin.
Tipo: | Article
Idioma: | Português

Identificador:

1982-1751

http://hdl.handle.net/2315/89

Relação: | 1/2007

Formato:

381389 bytes

application/pdf