Data/hora: 05/06/2024 04:09:00

Provedor de dados: 	27	
País: 	Belgium	
Título: 	New developments in the high density flow-through culturing of brine shrimp &lt;i&gt;Artemia&lt;/i&gt;	
Autores: 	Lavens, P.; Baert, P.; De Meulemeester, A.; Van Ballaer, E.; Sorgeloos, P.	
Data: 	1985	
Ano: 	1985	
Palavras-chave: 	Aquaculture systems; Brine shrimp culture; Recirculating systems; Artemia.	
Resumo: 	A closed culture system for the high density culturing of &lt;i&gt;Artemia spp.&lt;/i&gt; in 300-liter tanks using a new formula of artificial seawater and micronized waste products from agricultural crops as food is described. Culture conditions are greatly improved by applying a new filter technique and an electronic transparency meter which controls food distributions automatically. A total volume of 6,000 liters of culture water recirculated over a rotating biological contactor, a cross-flow sieve and a plate separator at a flow rate of 3000 liters per hour.Production yields obtained with this culture system, when extrapolated to a 1 m³ tank, indicate that 50 g of brine shrimp cysts can be converted into 20 kg of fresh (wet dry) pre-adult &lt;i&gt;Artemia&lt;/i&gt; in 14 days. These results are comparable to those reported earlier with open flow- through conditions.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.vliz.be/nl/open-marien-archief?module=ref&refid=3232	
Fonte: 	%3Ci%3EJ.+World+Aquacult.+Soc.+16%3C%2Fi%3E%3A+498-507	
Fonte: 	info:eu-repo/semantics/restrictedAccess