Data/hora: 16/06/2024 06:53:35

Provedor de dados: | 32
País: | Mexico
Título: | Índice de salinidad de la red hidrográfica del estado de Morelos, México
Autores: | Ramírez García, Jazmin.
Data: | 2012-09-09
Ano: | 2009
Palavras-chave: | Calidad del agua; Riego; Eutrofización; Sodicidad; RAS; PSI; Maestría; Hidrociencias; Quality of the water; Watering; Eutrophication; Sodicity; SAR; ESP.
Resumo: | En la Red Hidrográfica del estado de Morelos el agua ocupa un lugar primordial, su disponibilidad y riqueza ha constituido un elemento de soporte básico para el desarrollo económico. Alrededor de 63000 hectáreas son irrigadas en Morelos y dado que las actividades agropecuarias, industriales y recreacionales compiten por este recurso, se hace necesario conocer las características químicas de las aguas y los efectos adversos sobre los terrenos en donde se aplican. Los objetivos de este trabajo fueron determinar las concentraciones iónicas del sistema y establecer índices para conocer el efecto sobre las propiedades físicas de los suelos. Se colectaron muestras de agua en 66 estaciones durante julio de 2007 y 78 en mayo de 2008 (primer y segundo muestreo respectivamente). Las mediciones comprendieron; cationes, aniones, pH, conductividad eléctrica (CE), residuo seco evaporado y calcinado (RSE y RSC), presión osmótica (PO), fosfatos, boro y las diferentes modificaciones de la relación de adsorción de sodio (RAS), las cuales fueron, RAS original, RASaj y RASo. La conductividad eléctrica de las aguas en los orígenes fue de 107 a 186 µS cm-1 y de 300 a 3447 µS cm-1 cuando reciben afluentes de manantiales y aguas urbano-industriales, siendo aguas de salinidad media a muy altamente salinas. La concentración de calcio, magnesio, sodio, bicarbonatos, sulfatos, fosfatos y boro fueron de 0.36 a 16.33 mmolc L-1, 0.28 a 14.22 mmolc L-1, 0.15 a 9.02 mmolc L-1, 0.58 a 12.55 mmolc L-1, 0.02 a 28.04 mmolc L-1,  0.004 a 5.0 mg L-1 y 0.0 a 3.6 mg L-1, respectivamente. La variación del RAS original fue de 0.10 a 3.96, RASaj de 0.19 a 6.87 y RASo de 0.15 a 4.46, indicando que son aguas de bajo contenido de sodio. Los valores de pH variaron de 6.79 a 8.42. Con los resultados obtenidos se hace evidente que la salinidad de las aguas de la red hidrográfica se debe principalmente a la dilución de materiales calcáreos, depósitos evaporiticos y contaminación antropogénica._________The system hydrographic of state of Morelos, the water has a very important place, it is readiness and wealth have constituted a basic element for the economic development, due to the agricultural, industrial activities and leisure activities compete for this resource. Around 6300 ha are irrigated in Morelos, that makes necessary to know the chemical characteristics of the waters and the adverse effects on the soil where they are applied. The objectives of this work were to determine the ionic concentration of the system and know indexes about the effect on the physical properties of the soil. Water sample were collected from 66 stations in July 2007 and 78 on May 2008 (first and second sampling respectively). The measurements were cations, anions, pH, electrical conductivity (EC), dry residues evaporated and burned (RSE and RSC), osmotic pressure (OP), phosphates, boron and the sodium absorption ratio (SAR) with their respective modifications that were SAR, SARaj, SARo. Electrical conductivity at the sources of the water was of 107 to 186 µS cm-1 and when these received the flowing of spring source and urban industrial their values were from 300 to 3447 µS cm-1, these waters were of the half salinity to high salinity. The calcium concentration, magnesium, sodium, bicarbonates, sulfates, phosphates and boron were from 0.36 to 16.33 mmolc L-1, 0.28 to14.22 mmolc L-1, 0.15 to 9.02 mmolc L-1, 0.58 to 12.55 mmolc L-1, 0.02 to 28.04 mmolc L-1, 0.004 a 5.0 mg L-1 and 0.0 to 3.6 mg L-1, respectively. The range of the SAR was from 0.10 to 3.96, SARaj was from 0.19 to 6.87 and SARo was from 0.15 to 4.46, indicating that is water with low sodium concentration. The pH values were ranging from 6.79 to 8.42. The conclusion of this work is clear; the salinity of the hydrographic system is due to the dilution of calcareous materials, deposits evaporites and contribution anthropogenic.
Tipo: | Tesis
Idioma: | Espanhol
Identificador: | http://hdl.handle.net/10521/1621