Data/hora: 02/06/2024 02:13:25

Provedor de dados: | Depósito Institucional Abierto de Documentos Digitales del Colegio de Postgraduados (COLPOS DIGITAL )
País: | Mexico
Título: | Calidad de aguas naturales y residuales en el sistema hidrográfico Valle del Mezquital, Hidalgo México.
Autores: | Barrios Castillo, Isaac Mateo.
Data: | 2014-04-28
Ano: | 2014
Palavras-chave: | Salinidad; Sodicidad; RAS; PSI; CSR; Salinity; Sodicity; SAR; ESP; RSC; Hidrociencias; Maestría.
Resumo: | Actualmente se ha usado prácticamente toda el agua disponible para satisfacer los requerimientos de los diferentes cultivos que se explotan en la agricultura bajo riego. Cada vez más se utilizan hasta el límite las aguas superficiales y subterráneas de la más variada composición química y concentración de sales. En México, se riegan aproximadamente 180,000 ha en diferentes lugares del Valle del Mezquital con aguas residuales urbano-industriales que derivan de la zona metropolitana del Valle de México, prácticamente sin ningún tratamiento. En esta investigación se analizan los efectos de los elementos inorgánicos que afectan la calidad del agua de riego residual urbano-industrial de la red hidrográfica Valle del Mezquital, Hidalgo. Se analizan los problemas de salinidad y sodicidad de estas aguas. La concentración total electrolítica de estas aguas varió de la siguiente manera: 135-4612 μ S cm-1. Altos niveles de sodio intercambiable propician la dispersión de las arcillas y afectan la infiltración del agua en los suelos. Los efectos de la sodicidad se evalúan con la relación de adsorción de sodio (RAS). Para ello se evaluaron las siguientes formulaciones RASor, RASaj y RASº. Se calcularon las sales hipotéticas en estas aguas y la composición salina resultó ser la siguiente: NaCl&gt;NaHCO3&gt;Mg (HCO3)2&gt;Ca (HCO3)2&gt;MgSO4. Estas aguas son: sódico-clorhídrico-bicarbonatadas. _______________  NATURAL AND RESIDUAL WATER QUALITY IN THE HIDROGRAPHIC SYSTEM VALLE DEL MEZQUITAL, HIDALGO, MÉXICO. ABSTRACT: Nowadays, practically any available water is being used to satisfy the moisture requirements of the different crops that are actively being grown under irrigation conditions. Surface and underground waters are ever more being used to exhaustion, regardless of their varied chemical composition or concentration of salts. In Mexico, approximately 180 000 ha in different places in the Valle del Mezquital are being irrigated with urban-industrial residual waters from the metropolitan zone of the Valle de México, with practically no treatment. In the present research work are analyzed and discussed the effects of the inorganic elements that affect the quality of the urban-industrial residual waters used for irrigation in the Valle del Mezquital, Hidalgo. Problems of salinity and sodicity in these waters are analyzed. The total electrolytic concentration of these waters varied as follows: 135-4612 μ S cm-1. High levels of exchangeable sodium favor the dispersion of clays and affect water infiltration into the soil. The effects of sodicity are evaluated with the sodium adsorption ratio (SAR). To do this, the following formulas were evaluated: SARor, SARaj, and SARº. Hypothetical salts were evaluated for these waters, and the saline composition turned out to be: NaCl&gt;NaHCO3&gt;Mg (HCO3)2&gt;Ca (HCO3)2&gt;MgSO4. The waters are: sodic-chlorhydric-bicarbonated.
Idioma: | Espanhol
Identificador: | http://hdl.handle.net/10521/2281